ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:53:58.342 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:53:58.347 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:53:58.348 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:53:58.350 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:53:58.352 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:53:58.354 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:53:58.361 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:53:58.368 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:53:58.371 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 08:53:58.377 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:53:59.578 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:53:59.580 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:54:01.673 |  | ←RRC BCCH SIB |  |  |
14 | 08:54:01.678 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:54:01.693 |  | ←RRC BCCH SIB |  |  |
16 | 08:54:01.713 |  | ←RRC BCCH SIB |  |  |
17 | 08:54:01.758 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:55:41.352 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:55:41.352 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:55:41.352 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:55:41.352 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:55:41.413 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:55:41.413 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:55:41.413 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:55:41.413 |  |  |  | →NAS EMM Attach request |  |
26 | 08:55:41.413 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:55:41.413 |  |  |  | NAS K-asme 7b03164382b1804c0021131a49294a97... |  |
28 | 08:55:41.413 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:55:41.414 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:55:41.414 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:55:41.415 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:55:41.485 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:55:41.485 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:55:41.485 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:55:41.485 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:55:41.485 |  |  |  | NAS UE auth OK |  |
37 | 08:55:41.485 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 08:55:41.485 |  |  |  | NAS K-nas-int 476253b71dcec92d0f143da090c53... |  |
39 | 08:55:41.485 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:55:41.486 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:55:41.486 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:55:41.487 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:55:41.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 08:55:41.525 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:55:41.525 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 08:55:41.525 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:55:41.525 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:55:41.526 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 08:55:41.526 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:55:41.527 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 08:55:41.573 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 08:55:41.573 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:55:41.573 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 08:55:41.573 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:55:41.573 |  |  |  | NAS K-enb ae1db9f1ffb6bdbbe7ddab248371c7f59... |  |
56 | 08:55:41.573 |  |  |  | NAS ← EMM Attach accept |  |
57 | 08:55:41.574 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:55:41.574 |  |  | RRC K-enb ae1db9f1ffb6bdbbe7ddab248371c7f59... |  |  |
59 | 08:55:41.574 |  |  | RRC rrc-cip efee669cb144ae69e7036e3d1234261... |  |  |
60 | 08:55:41.574 |  |  | RRC rrc-int 600aacaf1b6e6eb4b604dfd411e32b7... |  |  |
61 | 08:55:41.574 |  |  | RRC up-cip e46da1326236ee21d57b0854b282fc7d... |  |  |
62 | 08:55:41.574 |  |  | RRC up-int 3ef4b13d71dfb269f994c24c0febd0d5... |  |  |
63 | 08:55:41.575 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:55:41.605 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:55:41.605 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:55:41.605 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:55:41.605 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:55:41.655 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:55:41.655 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:55:41.655 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 08:55:41.655 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:55:41.655 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 08:55:41.685 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:55:41.685 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:55:41.725 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 08:55:41.725 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:55:41.725 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 08:55:41.725 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:55:41.725 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:55:41.726 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 08:55:41.726 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:55:41.727 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 08:55:46.939 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:55:46.940 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:55:47.322 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:55:47.322 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:55:47.322 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:55:47.322 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:55:47.365 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:55:47.365 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:55:47.365 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:55:47.365 |  |  |  | →NAS EMM Service request |  |
93 | 08:55:47.365 |  |  |  | NAS K-enb 572ae0f9e9c77ffeea249b7ed654df6ec... |  |
94 | 08:55:47.366 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 08:55:47.366 |  |  | RRC K-enb 572ae0f9e9c77ffeea249b7ed654df6ec... |  |  |
96 | 08:55:47.366 |  |  | RRC rrc-cip 2eadd93cf2a2c673f7b048f5372e897... |  |  |
97 | 08:55:47.366 |  |  | RRC rrc-int 41050fa51c258ad01897a38c3677652... |  |  |
98 | 08:55:47.366 |  |  | RRC up-cip 649aeaae3211abcbdafdcac7feefbace... |  |  |
99 | 08:55:47.366 |  |  | RRC up-int 14c9c05d326c4119e643fb5002a595a7... |  |  |
100 | 08:55:47.367 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:55:47.405 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:55:47.405 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:55:47.405 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:55:47.405 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:55:47.445 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:55:47.445 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:56:06.845 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:56:06.849 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:56:06.885 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:56:06.973 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:56:06.977 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:56:06.982 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:56:07.005 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:56:07.133 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 08:56:07.137 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 08:56:07.138 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
117 | 08:56:07.149 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
118 | 08:56:07.165 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 08:56:07.173 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 08:56:07.177 |  | ←enobeB PCAP frame← TCP |  |  |
121 | 08:56:07.189 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 08:56:07.195 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 08:56:07.204 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
124 | 08:56:07.205 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 08:56:07.213 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
126 | 08:56:07.245 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 08:56:07.285 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 08:56:09.045 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 08:56:09.049 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 08:56:09.085 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 08:56:09.093 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
132 | 08:56:09.102 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 08:56:09.125 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 08:56:09.501 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 08:56:09.504 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 08:56:09.505 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 08:56:09.517 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
138 | 08:56:09.525 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 08:56:09.533 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 08:56:09.541 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 08:56:09.551 |  |  |  |  | →HTTP GET | IDMS-Endpoint
142 | 08:56:09.556 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
143 | 08:56:09.567 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 08:56:09.568 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 08:56:09.569 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 08:56:09.605 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 08:56:14.373 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 08:56:14.381 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 08:56:14.391 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 08:56:14.393 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 08:56:14.404 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
152 | 08:56:14.405 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 08:56:14.406 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
154 | 08:56:14.445 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 08:56:14.448 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 08:56:14.460 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
157 | 08:56:14.485 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 08:56:15.285 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:56:15.290 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 08:56:15.325 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 08:56:15.413 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 08:56:15.418 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 08:56:15.445 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 08:56:15.613 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 08:56:15.618 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 08:56:15.629 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
167 | 08:56:15.645 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 08:56:15.653 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
169 | 08:56:15.657 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 08:56:15.669 |  |  |  |  | →HTTP POST | IDMS-Endpoint
171 | 08:56:15.685 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
172 | 08:56:15.693 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
173 | 08:56:15.695 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
174 | 08:56:15.765 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 08:56:16.005 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 08:56:16.009 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 08:56:16.045 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 08:56:16.053 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 08:56:16.057 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 08:56:16.060 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 08:56:16.085 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 08:56:16.093 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 08:56:16.097 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 08:56:16.098 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 08:56:16.109 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
186 | 08:56:16.133 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
187 | 08:56:16.137 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 08:56:16.150 |  |  |  |  | →HTTP POST | HTTP-Proxy
189 | 08:56:16.173 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
190 | 08:56:16.174 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
191 | 08:56:16.182 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
192 | 08:56:16.205 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 08:56:16.245 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 08:56:16.249 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 08:56:16.285 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 08:56:16.293 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
197 | 08:56:16.297 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 08:56:16.300 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
199 | 08:56:16.325 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 08:56:16.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 08:56:16.337 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 08:56:16.349 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
203 | 08:56:16.373 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 08:56:16.377 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 08:56:16.390 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 08:56:16.447 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
207 | 08:56:16.457 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 08:56:16.457 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 08:56:16.485 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 08:56:16.533 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
211 | 08:56:16.551 |  |  |  |  | →SIP REGISTER | P-CSCF
212 | 08:56:16.574 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
213 | 08:56:16.601 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
214 | 08:56:16.605 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
215 | 08:56:16.605 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
216 | 08:56:16.615 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
217 | 08:56:17.253 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
218 | 08:56:17.272 |  |  |  |  | →SIP REGISTER | P-CSCF
219 | 08:56:17.274 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
220 | 08:56:17.284 |  |  |  |  | ←SIP 200 OK | P-CSCF
221 | 08:56:17.617 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
222 | 08:56:17.667 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 08:56:17.678 |  |  |  |  | ←SIP 200 OK | P-CSCF
224 | 08:56:17.678 |  |  |  |  | MIKEY | Media-Server
225 | 08:56:17.881 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49054;transp... |  |  |
226 | 08:56:17.883 |  |  |  |  | XML→ | Media-Server
227 | 08:56:17.884 |  |  |  |  | XML→ | Media-Server
228 | 08:56:17.888 |  |  |  |  | ←XML | Media-Server
229 | 08:56:17.891 |  |  |  |  | ←SIP NOTIFY | P-CSCF
230 | 08:56:17.948 |  |  |  |  | →SIP 200 OK | P-CSCF
231 | 08:56:18.089 |  | ←enobeB PCAP frame← TCP |  |  |
232 | 08:56:18.125 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 08:56:18.133 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 08:56:18.137 |  | ←enobeB PCAP frame← TCP |  |  |
235 | 08:56:18.140 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
236 | 08:56:18.165 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 08:56:18.213 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 08:56:18.216 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 08:56:18.217 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
240 | 08:56:18.228 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
241 | 08:56:18.293 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
242 | 08:56:18.297 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 08:56:18.309 |  |  |  |  | →HTTP GET | HTTP-Proxy
244 | 08:56:18.318 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
245 | 08:56:18.319 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:691: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
246 | 08:56:18.327 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
247 | 08:56:18.365 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 08:56:18.405 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 08:56:18.408 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 08:56:18.413 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 08:56:18.417 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 08:56:18.419 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
253 | 08:56:18.445 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 08:56:18.605 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 08:56:18.609 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 08:56:18.645 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 08:56:18.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 08:56:18.657 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 08:56:18.660 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
260 | 08:56:18.685 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 08:56:18.773 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
262 | 08:56:18.777 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 08:56:18.805 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 08:56:18.813 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
265 | 08:56:18.817 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 08:56:18.850 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
267 | 08:56:18.852 |  |  |  |  | →HTTP GET | HTTP-Proxy
268 | 08:56:18.867 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:696: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
269 | 08:56:18.900 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
270 | 08:56:18.901 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 08:56:18.902 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
272 | 08:56:18.908 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
273 | 08:56:18.925 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 08:56:18.933 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 08:56:18.965 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
276 | 08:56:18.969 |  | ←enobeB PCAP frame← TCP |  |  |
277 | 08:56:18.973 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 08:56:18.977 |  | ←enobeB PCAP frame← TCP |  |  |
279 | 08:56:18.980 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
280 | 08:56:18.981 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 08:56:19.612 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
282 | 08:56:19.613 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
283 | 08:56:19.624 |  |  |  |  | ←SIP 200 OK | P-CSCF
284 | 08:56:19.624 |  |  |  |  | MIKEY | Media-Server
285 | 08:56:19.688 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 08:56:19.733 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
287 | 08:56:19.736 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 08:56:19.737 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
289 | 08:56:19.765 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 08:56:19.813 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 08:56:19.813 |  |  |  |  | XML→ | Media-Server
292 | 08:56:19.813 |  |  |  |  | XML→ | Media-Server
293 | 08:56:19.817 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
294 | 08:56:19.817 |  |  |  |  | ←XML | Media-Server
295 | 08:56:19.818 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49054;transp... |  |  |
296 | 08:56:19.828 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
297 | 08:56:19.829 |  |  |  |  | ←SIP NOTIFY | P-CSCF
298 | 08:56:19.845 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 08:56:19.864 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 08:56:19.874 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 08:56:19.875 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
302 | 08:56:19.876 |  |  |  |  | →SIP 200 OK | P-CSCF
303 | 08:56:19.876 |  |  |  |  | →HTTP GET | HTTP-Proxy
304 | 08:56:19.878 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:701: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
305 | 08:56:19.884 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
306 | 08:56:19.933 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 08:56:19.937 |  | ←enobeB PCAP frame← TCP |  |  |
308 | 08:56:19.948 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
309 | 08:56:19.965 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:56:19.973 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 08:56:19.977 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 08:56:20.005 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 08:56:20.013 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
314 | 08:56:20.017 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 08:56:20.020 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
316 | 08:56:20.045 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 08:56:20.101 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
318 | 08:56:20.105 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 08:56:20.117 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
320 | 08:56:20.125 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 08:56:20.133 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
322 | 08:56:20.137 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 08:56:20.149 |  |  |  |  | →HTTP GET | HTTP-Proxy
324 | 08:56:20.161 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:706: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
325 | 08:56:20.183 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
326 | 08:56:20.190 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
327 | 08:56:20.205 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 08:56:20.213 | →enobeB PCAP frame→ TCP |  |  |  |
329 | 08:56:20.245 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
330 | 08:56:20.249 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 08:56:20.253 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 08:56:20.257 |  | ←enobeB PCAP frame← TCP |  |  |
333 | 08:56:20.260 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
334 | 08:56:20.285 | →enobeB PCAP frame→ TCP |  |  |  |
335 | 08:56:20.539 |  |  |  |  | →SIP PUBLISH | P-CSCF
336 | 08:56:20.583 |  |  |  |  | MIKEY | Media-Server
337 | 08:56:20.607 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
338 | 08:56:20.776 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
339 | 08:56:20.779 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
340 | 08:56:20.783 |  |  |  |  | XML→ | Media-Server
341 | 08:56:20.786 |  |  |  |  | ←SIP 200 OK | P-CSCF
342 | 08:56:20.789 |  |  |  |  | ←SIP 200 OK | P-CSCF
343 | 08:56:20.790 |  |  |  |  | MIKEY | Media-Server
344 | 08:56:20.978 |  |  |  |  | XML→ | Media-Server
345 | 08:56:20.979 |  |  |  |  | XML→ | Media-Server
346 | 08:56:21.007 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49054;transp... |  |  |
347 | 08:56:21.012 |  |  |  |  | MIKEY | Media-Server
348 | 08:56:21.013 |  |  |  |  | ←XML | Media-Server
349 | 08:56:21.017 |  |  |  |  | ←SIP NOTIFY | P-CSCF
350 | 08:56:21.068 |  |  |  |  | →SIP 200 OK | P-CSCF
351 | 08:56:21.071 |  |  |  |  | ←XML | Media-Server
352 | 08:56:21.072 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
353 | 08:56:21.082 |  |  |  |  | ←SIP MESSAGE | P-CSCF
354 | 08:56:21.973 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
355 | 08:56:21.989 |  |  |  |  | →SIP 200 OK | P-CSCF
356 | 08:56:23.999 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
357 | 08:56:24.044 |  | ←RRC DCCH RRC Connection Release |  |  |
358 | 08:56:24.045 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
359 | 08:56:24.078 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
360 | 08:56:24.182 |  |  |  |  | ←XML | Media-Server
361 | 08:56:24.185 |  |  |  |  | ←SIP NOTIFY | P-CSCF
362 | 08:56:25.072 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
363 | 08:56:25.072 |  | →RRC CCCH RRC Connection Request |  |  |
364 | 08:56:25.072 |  | ←RRC CCCH RRC Connection Setup |  |  |
365 | 08:56:25.072 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
366 | 08:56:25.125 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
367 | 08:56:25.125 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
368 | 08:56:25.125 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
369 | 08:56:25.125 |  |  |  | →NAS EMM Service request |  |
370 | 08:56:25.125 |  |  |  | NAS K-enb 960e5d20517f661e86c91c4e92f1082af... |  |
371 | 08:56:25.126 |  | ←RRC DCCH Security Mode Command |  |  |
372 | 08:56:25.126 |  |  | RRC K-enb 960e5d20517f661e86c91c4e92f1082af... |  |  |
373 | 08:56:25.126 |  |  | RRC rrc-cip 36fa63adac7e399c2e6ca25a286fa8c... |  |  |
374 | 08:56:25.126 |  |  | RRC rrc-int 520df8606272b08280f4987772ff990... |  |  |
375 | 08:56:25.126 |  |  | RRC up-cip 474651b0e9cda1e895d851f9282d4484... |  |  |
376 | 08:56:25.126 |  |  | RRC up-int 42f485e9436bc1cf1df4c72f0dfe76ba... |  |  |
377 | 08:56:25.127 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
378 | 08:56:25.165 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
379 | 08:56:25.165 |  | →RRC DCCH Security Mode Complete |  |  |
380 | 08:56:25.165 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
381 | 08:56:25.165 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
382 | 08:56:25.205 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
383 | 08:56:25.205 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
384 | 08:56:25.207 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49054;transp... |  |  |
385 | 08:56:25.252 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
386 | 08:56:25.252 |  | ←RRC PCCH Paging |  |  |
387 | 08:56:25.253 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
388 | 08:56:25.272 |  |  |  |  | →SIP 200 OK | P-CSCF
389 | 08:56:25.285 | →enobeB PCAP frame→ TCP |  |  |  |
390 | 08:56:25.289 |  | ←enobeB PCAP frame← TCP |  |  |
391 | 08:56:25.325 | →enobeB PCAP frame→ TCP |  |  |  |
392 | 08:56:25.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
393 | 08:56:25.337 |  | ←enobeB PCAP frame← TCP |  |  |
394 | 08:56:25.340 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
395 | 08:56:25.365 | →enobeB PCAP frame→ TCP |  |  |  |
396 | 08:56:25.453 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
397 | 08:56:25.457 |  | ←enobeB PCAP frame← TCP |  |  |
398 | 08:56:25.458 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
399 | 08:56:25.469 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
400 | 08:56:25.485 | →enobeB PCAP frame→ TCP |  |  |  |
401 | 08:56:25.493 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
402 | 08:56:25.497 |  | ←enobeB PCAP frame← TCP |  |  |
403 | 08:56:25.509 |  |  |  |  | →HTTP GET | HTTP-Proxy
404 | 08:56:25.522 |  |  |  |  | ←XML | Media-Server
405 | 08:56:25.539 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
406 | 08:56:25.540 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
407 | 08:56:25.544 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49054;transp... |  |  |
408 | 08:56:25.547 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
409 | 08:56:25.553 |  |  |  |  | ←SIP NOTIFY | P-CSCF
410 | 08:56:25.565 | →enobeB PCAP frame→ TCP |  |  |  |
411 | 08:56:25.573 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
412 | 08:56:25.589 |  |  |  |  | →SIP 200 OK | P-CSCF
413 | 08:56:25.593 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:900: Test-Body Step 1
414 | 08:56:25.594 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
415 | 08:56:25.594 |  |  |  |  | MMICmd: Make the MCPTT User requesting the establishment of an MCPTT On-demand pre-arranged broadcast group call for the selected MCPTT temporary group GROUP D as a member of the MCPTT broadcast group GROUP A, with explicit floor control
416 | 08:56:25.594 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:903: Test-Body Step 2
417 | 08:56:25.605 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
418 | 08:56:25.609 |  | ←enobeB PCAP frame← TCP |  |  |
419 | 08:56:25.613 | →enobeB PCAP frame→ TCP |  |  |  |
420 | 08:56:25.616 |  | ←enobeB PCAP frame← TCP |  |  |
421 | 08:56:25.620 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
422 | 08:56:25.645 | →enobeB PCAP frame→ TCP |  |  |  |
423 | 08:56:39.293 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
424 | 08:56:39.294 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
425 | 08:56:39.321 |  |  |  |  | →SIP INVITE | P-CSCF
426 | 08:56:39.353 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
427 | 08:56:39.355 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
428 | 08:56:39.358 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 45CC6FFADB1FF997426737C29D2C3925, Master Salt: 38E2D1E026B0A3C05045C6D6, MKI: 2632398F
429 | 08:56:39.358 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
430 | 08:56:39.362 |  |  |  |  | XML→ | Media-Server
431 | 08:56:39.362 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
432 | 08:56:39.363 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:910: Step 2 Verdict: Pass
433 | 08:56:39.364 |  |  |  |  | ←SIP 100 Trying | P-CSCF
434 | 08:56:39.366 |  |  |  |  | ←SIP 200 OK | P-CSCF
435 | 08:56:39.976 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
436 | 08:56:39.976 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
437 | 08:56:39.976 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
438 | 08:56:39.977 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
439 | 08:56:40.045 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
440 | 08:56:40.045 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
441 | 08:56:40.045 |  | →RRC DCCH UL Information Transfer |  |  |
442 | 08:56:40.045 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
443 | 08:56:40.045 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
444 | 08:56:40.123 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
445 | 08:56:40.253 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
446 | 08:56:40.270 |  |  |  |  | →SIP ACK | P-CSCF
447 | 08:56:40.271 |  | ←enobeB PCAP frame← |  |  |
448 | 08:56:40.282 |  |  |  |  | ←Floor Taken | Media-Server
449 | 08:56:40.325 | →enobeB PCAP frame→ |  |  |  |
450 | 08:56:40.340 |  |  |  |  | Floor ACK→ | Media-Server
451 | 08:56:40.341 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:49054;transport... |  |  |
452 | 08:56:40.343 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
453 | 08:56:40.343 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:920: Test-Body Step 6
454 | 08:56:40.351 |  |  |  |  | ←SIP BYE | P-CSCF
455 | 08:56:40.373 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
456 | 08:56:40.389 |  |  |  |  | →SIP 200 OK | P-CSCF
457 | 08:56:40.965 | →enobeB PCAP frame→ |  |  |  |
458 | 08:56:42.397 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
459 | 08:56:42.398 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
460 | 08:56:42.398 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
461 | 08:56:42.399 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
462 | 08:56:42.399 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
463 | 08:56:42.445 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
464 | 08:56:42.445 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
465 | 08:56:42.445 |  | →RRC DCCH UL Information Transfer |  |  |
466 | 08:56:42.445 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
467 | 08:56:42.445 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
468 | 08:56:42.593 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
469 | 08:56:42.594 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
470 | 08:56:42.637 |  | ←RRC DCCH RRC Connection Release |  |  |
471 | 08:56:42.638 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
472 | 08:56:42.660 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
473 | 08:56:42.662 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
474 | 08:56:42.665 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
475 | 08:56:43.413 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.