MSG #34 2021-12-17 08:55:41.485

NAS

     EMM: Authentication response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x1 (Integrity protected)
    Auth code = 0xc315186b
    Sequence number = 0x06
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x53 (Authentication response)
    Authentication response parameter:
      Length = 8
      Data = 4a 81 71 b6 bd 9c 1d c7