ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 11:53:38.995 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 11:53:38.997 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 11:53:38.998 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 11:53:39.000 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 11:53:39.000 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 11:53:39.001 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 11:53:39.003 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 11:53:39.004 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 11:53:39.005 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 11:53:39.006 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 11:53:40.209 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 11:53:40.211 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 11:53:41.629 |  | ←RRC BCCH SIB1 |  |  |
14 | 11:53:41.704 |  | ←RRC BCCH SIB |  |  |
15 | 11:53:41.709 |  | ←RRC BCCH SIB1 |  |  |
16 | 11:53:41.724 |  | ←RRC BCCH SIB |  |  |
17 | 11:53:41.744 |  | ←RRC BCCH SIB |  |  |
18 | 11:55:15.303 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 11:55:15.303 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 11:55:15.303 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 11:55:15.303 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 11:55:15.364 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 11:55:15.364 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 11:55:15.364 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 11:55:15.364 |  |  |  | →NAS EMM Attach request |  |
26 | 11:55:15.364 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 11:55:15.364 |  |  |  | NAS K-asme 80d454913c2171c50446dd6142453f4a... |  |
28 | 11:55:15.364 |  |  |  | NAS ← EMM Authentication request |  |
29 | 11:55:15.365 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 11:55:15.365 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 11:55:15.366 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 11:55:15.436 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 11:55:15.436 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 11:55:15.436 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 11:55:15.436 |  |  |  | →NAS EMM Authentication response |  |
36 | 11:55:15.436 |  |  |  | NAS UE auth OK |  |
37 | 11:55:15.436 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 11:55:15.436 |  |  |  | NAS K-nas-int 480f50aae2c0c21d380e51a123eae... |  |
39 | 11:55:15.436 |  |  |  | NAS ← EMM Security mode command |  |
40 | 11:55:15.437 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 11:55:15.437 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 11:55:15.438 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 11:55:15.476 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 11:55:15.476 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 11:55:15.476 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 11:55:15.476 |  |  |  | →NAS EMM Security mode complete |  |
47 | 11:55:15.476 |  |  |  | NAS ← ESM ESM information request |  |
48 | 11:55:15.477 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 11:55:15.477 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 11:55:15.478 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 11:55:15.524 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 11:55:15.524 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 11:55:15.524 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 11:55:15.524 |  |  |  | →NAS ESM ESM information response |  |
55 | 11:55:15.524 |  |  |  | NAS K-enb 5bd7c631d78dbac3cdd6ba0db3a68c81b... |  |
56 | 11:55:15.524 |  |  |  | NAS ← EMM Attach accept |  |
57 | 11:55:15.525 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 11:55:15.525 |  |  | RRC K-enb 5bd7c631d78dbac3cdd6ba0db3a68c81b... |  |  |
59 | 11:55:15.525 |  |  | RRC rrc-cip 8d1d3f1c8cd8f21753d65fdf4312edc... |  |  |
60 | 11:55:15.525 |  |  | RRC rrc-int 861a62a0eabd4cfda6fb4143f567123... |  |  |
61 | 11:55:15.525 |  |  | RRC up-cip c5378e6222d9b02fcf9b0aee5a9904f3... |  |  |
62 | 11:55:15.525 |  |  | RRC up-int 71409088a0b950deb2eeb27c068e6b10... |  |  |
63 | 11:55:15.526 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 11:55:15.556 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 11:55:15.556 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 11:55:15.556 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 11:55:15.556 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 11:55:15.606 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 11:55:15.606 |  | →RRC DCCH UE Capability Information |  |  |
70 | 11:55:15.606 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 11:55:15.606 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 11:55:15.606 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 11:55:15.636 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 11:55:15.636 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 11:55:15.676 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 11:55:15.676 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 11:55:15.676 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 11:55:15.676 |  |  |  | →NAS EMM Attach complete |  |
79 | 11:55:15.676 |  |  |  | NAS ← EMM EMM information |  |
80 | 11:55:15.677 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 11:55:15.677 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 11:55:15.678 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 11:55:22.596 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 11:55:22.597 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 11:55:24.433 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 11:55:24.433 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 11:55:24.433 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 11:55:24.433 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 11:55:24.476 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 11:55:24.476 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 11:55:24.476 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 11:55:24.476 |  |  |  | →NAS EMM Service request |  |
93 | 11:55:24.476 |  |  |  | NAS K-enb a27561a5aecb1211688c775cdf669ba5f... |  |
94 | 11:55:24.477 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 11:55:24.477 |  |  | RRC K-enb a27561a5aecb1211688c775cdf669ba5f... |  |  |
96 | 11:55:24.477 |  |  | RRC rrc-cip c49e59f3e2e5798c770441a6214c1f5... |  |  |
97 | 11:55:24.477 |  |  | RRC rrc-int 2d76d071e8091a5f07b54329ec2bb55... |  |  |
98 | 11:55:24.477 |  |  | RRC up-cip 2354824b28f7edc8c1a109ed45a271df... |  |  |
99 | 11:55:24.477 |  |  | RRC up-int c8d3f10564ab223c3f26130926cc067c... |  |  |
100 | 11:55:24.478 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 11:55:24.516 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 11:55:24.516 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 11:55:24.516 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 11:55:24.516 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 11:55:24.556 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 11:55:24.556 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 11:55:39.356 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 11:55:39.360 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 11:55:39.396 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 11:55:39.524 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 11:55:39.528 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 11:55:39.533 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 11:55:39.556 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 11:55:39.684 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 11:55:39.687 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
116 | 11:55:39.688 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
117 | 11:55:39.716 | →enobeB PCAP frame→ TCP |  |  |  |
118 | 11:55:39.764 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
119 | 11:55:39.767 |  | ←enobeB PCAP frame← TCP |  |  |
120 | 11:55:39.767 |  |  |  |  | →HTTP GET | HTTP-Proxy
121 | 11:55:39.773 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 11:55:39.792 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
123 | 11:55:39.796 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 11:55:39.836 | →enobeB PCAP frame→ TCP |  |  |  |
125 | 11:55:41.676 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 11:55:41.696 |  | ←enobeB PCAP frame← TCP |  |  |
127 | 11:55:41.716 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 11:55:41.724 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
129 | 11:55:41.727 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 11:55:41.733 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
131 | 11:55:41.756 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 11:55:42.084 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 11:55:42.087 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 11:55:42.089 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 11:55:42.116 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 11:55:42.124 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
137 | 11:55:42.128 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 11:55:42.129 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 11:55:42.145 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
140 | 11:55:42.146 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
141 | 11:55:42.147 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 11:55:42.148 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 11:55:42.196 | →enobeB PCAP frame→ TCP |  |  |  |
144 | 11:55:46.844 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
145 | 11:55:46.848 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 11:55:46.849 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 11:55:46.862 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
148 | 11:55:46.865 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
149 | 11:55:46.865 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 11:55:46.876 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 11:55:46.916 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 11:55:46.918 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
153 | 11:55:46.920 |  | ←enobeB PCAP frame← TCP |  |  |
154 | 11:55:46.956 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 11:55:47.676 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 11:55:47.679 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 11:55:47.716 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 11:55:47.764 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
159 | 11:55:47.768 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 11:55:47.770 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 11:55:47.796 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 11:55:47.884 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 11:55:47.886 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
164 | 11:55:47.888 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 11:55:47.916 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 11:55:47.924 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 11:55:47.928 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 11:55:47.928 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 11:55:47.958 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
170 | 11:55:47.961 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
171 | 11:55:47.964 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
172 | 11:55:48.036 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 11:55:48.276 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 11:55:48.280 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 11:55:48.316 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 11:55:48.324 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
177 | 11:55:48.328 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 11:55:48.333 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
179 | 11:55:48.356 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 11:55:48.404 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 11:55:48.407 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
182 | 11:55:48.408 |  | ←enobeB PCAP frame← TCP |  |  |
183 | 11:55:48.409 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
184 | 11:55:48.444 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
185 | 11:55:48.448 |  |  |  |  | →HTTP POST | HTTP-Proxy
186 | 11:55:48.449 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 11:55:48.472 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
188 | 11:55:48.480 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
189 | 11:55:48.484 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
190 | 11:55:48.516 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 11:55:48.556 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 11:55:48.560 |  | ←enobeB PCAP frame← TCP |  |  |
193 | 11:55:48.596 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 11:55:48.604 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
195 | 11:55:48.608 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 11:55:48.611 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
197 | 11:55:48.636 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 11:55:48.644 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 11:55:48.647 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
200 | 11:55:48.648 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 11:55:48.649 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 11:55:48.684 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
203 | 11:55:48.688 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 11:55:48.688 |  |  |  |  | →HTTP POST | HTTP-Proxy
205 | 11:55:48.751 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
206 | 11:55:48.751 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
207 | 11:55:48.753 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
208 | 11:55:48.796 | →enobeB PCAP frame→ TCP |  |  |  |
209 | 11:55:48.844 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
210 | 11:55:48.849 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 11:55:48.873 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
212 | 11:55:48.902 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
213 | 11:55:48.904 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
214 | 11:55:48.910 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
215 | 11:55:48.912 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
216 | 11:55:49.684 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
217 | 11:55:49.690 |  |  |  |  | →SIP REGISTER | P-CSCF
218 | 11:55:49.715 |  |  |  |  | ←SIP 200 OK | P-CSCF
219 | 11:55:49.717 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
220 | 11:55:50.075 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
221 | 11:55:50.138 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 11:55:50.138 |  |  |  |  | MIKEY | Media-Server
223 | 11:55:50.140 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
224 | 11:55:50.346 |  |  |  |  | XML→ | Media-Server
225 | 11:55:50.347 |  |  |  |  | XML→ | Media-Server
226 | 11:55:50.351 |  |  |  |  | ←XML | Media-Server
227 | 11:55:50.355 |  |  |  |  | ←SIP NOTIFY | P-CSCF
228 | 11:55:50.357 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42587;transp... |  |  |
229 | 11:55:50.415 |  |  |  |  | →SIP 200 OK | P-CSCF
230 | 11:55:50.600 |  | ←enobeB PCAP frame← TCP |  |  |
231 | 11:55:50.644 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 11:55:50.648 |  | ←enobeB PCAP frame← TCP |  |  |
233 | 11:55:50.652 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
234 | 11:55:50.676 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 11:55:50.764 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 11:55:50.767 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
237 | 11:55:50.768 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
238 | 11:55:50.796 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 11:55:50.816 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 11:55:50.816 |  |  |  |  | →HTTP GET | HTTP-Proxy
241 | 11:55:50.825 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:722: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
242 | 11:55:50.834 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
243 | 11:55:50.837 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
244 | 11:55:50.878 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
245 | 11:55:50.880 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 11:55:50.888 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 11:55:51.036 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 11:55:51.040 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 11:55:51.076 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 11:55:51.084 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
251 | 11:55:51.087 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 11:55:51.091 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
253 | 11:55:51.116 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 11:55:51.164 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
255 | 11:55:51.167 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 11:55:51.167 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
257 | 11:55:51.169 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
258 | 11:55:51.204 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
259 | 11:55:51.207 |  |  |  |  | →HTTP GET | HTTP-Proxy
260 | 11:55:51.208 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 11:55:51.218 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:727: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
262 | 11:55:51.268 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
263 | 11:55:51.276 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
264 | 11:55:51.277 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 11:55:51.278 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
266 | 11:55:51.316 | →enobeB PCAP frame→ TCP |  |  |  |
267 | 11:55:51.324 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 11:55:51.332 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 11:55:51.340 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 11:55:51.342 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
271 | 11:55:51.343 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 11:55:51.344 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 11:55:51.396 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 11:55:52.036 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
275 | 11:55:52.082 |  |  |  |  | ←SIP 200 OK | P-CSCF
276 | 11:55:52.083 |  |  |  |  | MIKEY | Media-Server
277 | 11:55:52.084 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
278 | 11:55:52.119 |  | ←enobeB PCAP frame← TCP |  |  |
279 | 11:55:52.164 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
280 | 11:55:52.168 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 11:55:52.169 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
282 | 11:55:52.196 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 11:55:52.284 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
284 | 11:55:52.284 |  |  |  |  | XML→ | Media-Server
285 | 11:55:52.285 |  |  |  |  | XML→ | Media-Server
286 | 11:55:52.285 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
287 | 11:55:52.287 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
288 | 11:55:52.289 |  |  |  |  | ←XML | Media-Server
289 | 11:55:52.292 |  |  |  |  | ←SIP NOTIFY | P-CSCF
290 | 11:55:52.295 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42587;transp... |  |  |
291 | 11:55:52.316 | →enobeB PCAP frame→ TCP |  |  |  |
292 | 11:55:52.334 |  |  |  |  | →SIP 200 OK | P-CSCF
293 | 11:55:52.334 |  |  |  |  | →HTTP GET | HTTP-Proxy
294 | 11:55:52.336 |  | ←enobeB PCAP frame← TCP |  |  |
295 | 11:55:52.337 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:732: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
296 | 11:55:52.343 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
297 | 11:55:52.347 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
298 | 11:55:52.404 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 11:55:52.406 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
300 | 11:55:52.408 |  | ←enobeB PCAP frame← TCP |  |  |
301 | 11:55:52.436 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 11:55:52.476 | →enobeB PCAP frame→ TCP |  |  |  |
303 | 11:55:52.480 |  | ←enobeB PCAP frame← TCP |  |  |
304 | 11:55:52.516 | →enobeB PCAP frame→ TCP |  |  |  |
305 | 11:55:52.524 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
306 | 11:55:52.528 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 11:55:52.531 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
308 | 11:55:52.556 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 11:55:52.644 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
310 | 11:55:52.647 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
311 | 11:55:52.648 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
312 | 11:55:52.676 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 11:55:52.684 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
314 | 11:55:52.687 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 11:55:52.687 |  |  |  |  | →HTTP GET | HTTP-Proxy
316 | 11:55:52.698 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:737: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
317 | 11:55:52.730 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
318 | 11:55:52.736 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 11:55:52.737 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
320 | 11:55:52.756 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 11:55:52.764 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 11:55:52.836 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
323 | 11:55:52.838 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
324 | 11:55:52.840 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 11:55:52.844 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 11:55:52.848 |  | ←enobeB PCAP frame← TCP |  |  |
327 | 11:55:52.876 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 11:55:52.996 |  |  |  |  | →SIP PUBLISH | P-CSCF
329 | 11:55:53.039 |  |  |  |  | MIKEY | Media-Server
330 | 11:55:53.065 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
331 | 11:55:53.245 |  |  |  |  | XML→ | Media-Server
332 | 11:55:53.249 |  |  |  |  | ←SIP 200 OK | P-CSCF
333 | 11:55:53.251 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
334 | 11:55:53.252 |  |  |  |  | ←SIP 200 OK | P-CSCF
335 | 11:55:53.253 |  |  |  |  | MIKEY | Media-Server
336 | 11:55:53.255 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
337 | 11:55:53.447 |  |  |  |  | XML→ | Media-Server
338 | 11:55:53.448 |  |  |  |  | XML→ | Media-Server
339 | 11:55:53.483 |  |  |  |  | MIKEY | Media-Server
340 | 11:55:53.483 |  |  |  |  | ←XML | Media-Server
341 | 11:55:53.488 |  |  |  |  | ←SIP NOTIFY | P-CSCF
342 | 11:55:53.491 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42587;transp... |  |  |
343 | 11:55:53.526 |  |  |  |  | →SIP 200 OK | P-CSCF
344 | 11:55:53.529 |  |  |  |  | ←XML | Media-Server
345 | 11:55:53.536 |  |  |  |  | ←SIP MESSAGE | P-CSCF
346 | 11:55:53.539 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
347 | 11:55:54.407 |  |  |  |  | →SIP 200 OK | P-CSCF
348 | 11:55:56.417 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
349 | 11:55:56.465 |  | ←RRC DCCH RRC Connection Release |  |  |
350 | 11:55:56.466 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
351 | 11:55:56.486 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
352 | 11:55:56.487 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1212: Test-Body Step 1
353 | 11:55:56.489 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
354 | 11:55:56.489 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request the establishment of an MCPTT locally initiated ambient listening call
355 | 11:55:56.490 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1215: Test-Body Step 2
356 | 11:55:57.713 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
357 | 11:55:57.713 |  | →RRC CCCH RRC Connection Request |  |  |
358 | 11:55:57.713 |  | ←RRC CCCH RRC Connection Setup |  |  |
359 | 11:55:57.713 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
360 | 11:55:57.756 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
361 | 11:55:57.756 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
362 | 11:55:57.756 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
363 | 11:55:57.756 |  |  |  | →NAS EMM Service request |  |
364 | 11:55:57.756 |  |  |  | NAS K-enb 3d5b449db03b092591a6a0e1cfa9c5b05... |  |
365 | 11:55:57.757 |  | ←RRC DCCH Security Mode Command |  |  |
366 | 11:55:57.757 |  |  | RRC K-enb 3d5b449db03b092591a6a0e1cfa9c5b05... |  |  |
367 | 11:55:57.757 |  |  | RRC rrc-cip 7d927f6c61378efee62c461a2e730f0... |  |  |
368 | 11:55:57.757 |  |  | RRC rrc-int 514c523461543af13b15a3577b183ff... |  |  |
369 | 11:55:57.757 |  |  | RRC up-cip 7a3c09f72c808eb4b321d19dfea15112... |  |  |
370 | 11:55:57.757 |  |  | RRC up-int b91cff81fff736fd775e348bfc646828... |  |  |
371 | 11:55:57.758 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
372 | 11:55:57.796 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
373 | 11:55:57.796 |  | →RRC DCCH Security Mode Complete |  |  |
374 | 11:55:57.796 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
375 | 11:55:57.796 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
376 | 11:55:57.836 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
377 | 11:55:57.836 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
378 | 11:56:03.124 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
379 | 11:56:03.125 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
380 | 11:56:03.212 |  |  |  |  | →SIP INVITE | P-CSCF
381 | 11:56:03.261 |  |  |  |  | MIKEY | Media-Server
382 | 11:56:03.469 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: CABC66C768C089203A044FB4852D65C3, Master Salt: DE9F8C8EB778275B94F856B8, MKI: 27AEA98D
383 | 11:56:03.469 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
384 | 11:56:03.472 |  |  |  |  | XML→ | Media-Server
385 | 11:56:03.474 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
386 | 11:56:03.474 |  |  |  |  | XML→ | Media-Server
387 | 11:56:03.477 |  |  |  |  | ←SIP 100 Trying | P-CSCF
388 | 11:56:03.479 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
389 | 11:56:03.479 |  |  |  |  | ←SIP 200 OK | P-CSCF
390 | 11:56:03.482 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
391 | 11:56:04.110 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
392 | 11:56:04.111 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
393 | 11:56:04.111 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
394 | 11:56:04.112 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
395 | 11:56:04.156 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
396 | 11:56:04.156 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
397 | 11:56:04.156 |  | →RRC DCCH UL Information Transfer |  |  |
398 | 11:56:04.156 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
399 | 11:56:04.156 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
400 | 11:56:04.240 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
401 | 11:56:04.524 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
402 | 11:56:04.528 |  |  |  |  | →SIP ACK | P-CSCF
403 | 11:56:04.537 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1217: Step 2 Verdict: Pass
404 | 11:56:04.538 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1221: Test-Body Step 7
405 | 11:56:04.538 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1230: Test-Body Step 9 - 10
406 | 11:56:04.642 |  |  |  |  | MMICmd: Release call (hang up the call)
407 | 11:56:05.076 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
408 | 11:56:05.116 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
409 | 11:56:05.124 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
410 | 11:56:05.132 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
411 | 11:56:05.156 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
412 | 11:56:07.295 |  |  |  |  | →SIP BYE | P-CSCF
413 | 11:56:07.303 |  |  |  |  | ←SIP 200 OK | P-CSCF
414 | 11:56:07.306 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
415 | 11:56:07.316 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
416 | 11:56:07.320 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
417 | 11:56:07.556 | →enobeB PCAP frame→ |  |  |  |
418 | 11:56:09.305 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
419 | 11:56:09.328 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
420 | 11:56:09.329 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
421 | 11:56:09.329 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
422 | 11:56:09.330 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
423 | 11:56:09.356 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
424 | 11:56:09.356 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
425 | 11:56:09.356 |  | →RRC DCCH UL Information Transfer |  |  |
426 | 11:56:09.356 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
427 | 11:56:09.356 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
428 | 11:56:09.447 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
429 | 11:56:09.448 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
430 | 11:56:09.494 |  | ←RRC DCCH RRC Connection Release |  |  |
431 | 11:56:09.495 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
432 | 11:56:09.520 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
433 | 11:56:09.521 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1232: Step 10 Verdict: Pass
434 | 11:56:09.521 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1236: Test-Body Step 13
435 | 11:56:09.523 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
436 | 11:56:09.523 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request the establishment of an MCPTT locally initiated ambient listening call
437 | 11:56:09.524 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1239: Test-Body Step 14
438 | 11:56:15.603 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
439 | 11:56:15.603 |  | →RRC CCCH RRC Connection Request |  |  |
440 | 11:56:15.603 |  | ←RRC CCCH RRC Connection Setup |  |  |
441 | 11:56:15.603 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
442 | 11:56:15.636 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
443 | 11:56:15.636 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
444 | 11:56:15.636 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
445 | 11:56:15.636 |  |  |  | →NAS EMM Service request |  |
446 | 11:56:15.636 |  |  |  | NAS K-enb 59bc05c1bd2cbfb6e9fd4a64e3bf8f160... |  |
447 | 11:56:15.637 |  | ←RRC DCCH Security Mode Command |  |  |
448 | 11:56:15.637 |  |  | RRC K-enb 59bc05c1bd2cbfb6e9fd4a64e3bf8f160... |  |  |
449 | 11:56:15.637 |  |  | RRC rrc-cip dea7d06e3616a354015a5d5d6c3b495... |  |  |
450 | 11:56:15.637 |  |  | RRC rrc-int db6444f1fa567a12f3eae182ffc6f27... |  |  |
451 | 11:56:15.637 |  |  | RRC up-cip d5c663afe909c260fa8b06569e84eca3... |  |  |
452 | 11:56:15.637 |  |  | RRC up-int 7dfa5d88f4b25741932da0339249abd2... |  |  |
453 | 11:56:15.638 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
454 | 11:56:15.676 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
455 | 11:56:15.676 |  | →RRC DCCH Security Mode Complete |  |  |
456 | 11:56:15.676 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
457 | 11:56:15.676 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
458 | 11:56:15.716 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
459 | 11:56:15.716 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
460 | 11:56:15.724 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
461 | 11:56:15.725 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
462 | 11:56:15.733 |  |  |  |  | →SIP INVITE | P-CSCF
463 | 11:56:15.748 |  |  |  |  | MIKEY | Media-Server
464 | 11:56:15.953 |  |  |  |  | XML→ | Media-Server
465 | 11:56:15.954 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
466 | 11:56:15.954 |  |  |  |  | XML→ | Media-Server
467 | 11:56:15.957 |  |  |  |  | ←SIP 100 Trying | P-CSCF
468 | 11:56:15.959 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
469 | 11:56:15.959 |  |  |  |  | ←SIP 200 OK | P-CSCF
470 | 11:56:15.961 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
471 | 11:56:16.602 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
472 | 11:56:16.603 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
473 | 11:56:16.603 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
474 | 11:56:16.604 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
475 | 11:56:16.636 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
476 | 11:56:16.636 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
477 | 11:56:16.636 |  | →RRC DCCH UL Information Transfer |  |  |
478 | 11:56:16.636 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
479 | 11:56:16.636 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
480 | 11:56:16.742 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
481 | 11:56:16.764 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
482 | 11:56:16.768 |  |  |  |  | →SIP ACK | P-CSCF
483 | 11:56:16.777 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1241: Step 14 Verdict: Pass
484 | 11:56:16.777 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1243: Test-Body Step 15 - 18
485 | 11:56:16.777 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1245: Test-Body Step 19
486 | 11:56:16.778 |  |  |  |  | ←XML | Media-Server
487 | 11:56:16.810 |  |  |  |  | ←SIP BYE | P-CSCF
488 | 11:56:16.815 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:42587;transport... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
489 | 11:56:16.844 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
490 | 11:56:16.847 |  |  |  |  | →SIP 200 OK | P-CSCF
491 | 11:56:17.196 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
492 | 11:56:17.200 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
493 | 11:56:17.396 | →enobeB PCAP frame→ |  |  |  |
494 | 11:56:18.855 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
495 | 11:56:18.877 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
496 | 11:56:18.878 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
497 | 11:56:18.878 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
498 | 11:56:18.879 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
499 | 11:56:18.916 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
500 | 11:56:18.916 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
501 | 11:56:18.916 |  | →RRC DCCH UL Information Transfer |  |  |
502 | 11:56:18.916 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
503 | 11:56:18.916 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
504 | 11:56:18.995 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
505 | 11:56:18.996 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
506 | 11:56:19.044 |  | ←RRC DCCH RRC Connection Release |  |  |
507 | 11:56:19.045 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
508 | 11:56:19.064 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
509 | 11:56:19.065 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1247: Step 19 Verdict: Pass
510 | 11:56:19.066 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
511 | 11:56:19.069 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
512 | 11:56:19.816 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.