MSG #51 2022-01-05 11:55:15.524

    enobeB PCAP frame

    {
      "layers": {
        "frame": {
          "frame.encap_type": "45",
          "frame.time": "Jan  5, 2022 11:55:15.524227000 CET",
          "frame.offset_shift": "0.000000000",
          "frame.time_epoch": "1641380115.524227000",
          "frame.time_delta": "0.005019000",
          "frame.time_delta_displayed": "0.045950000",
          "frame.time_relative": "93.855008000",
          "frame.number": "8235",
          "frame.len": "76",
          "frame.cap_len": "76",
          "frame.marked": "0",
          "frame.ignored": "0",
          "frame.protocols": "user_dlt:mac-lte-framed:mac-lte:rlc-lte:pdcp-lte:lte_rrc:nas-eps:chap:chap:ipcp"
        },
        "user_dlt": "DLT: 147, Payload: mac-lte-framed (mac-lte-framed)",
        "mac-lte": {
          "mac-lte.context": "",
          "mac-lte.context_tree": {
            "mac-lte.radio-type": "1",
            "mac-lte.direction": "0",
            "mac-lte.ueid": "1677",
            "mac-lte.sfn": "165",
            "mac-lte.subframe": "6",
            "mac-lte.rnti": "1737",
            "mac-lte.rnti-type": "3",
            "mac-lte.is-predefined-frame": "0",
            "mac-lte.length": "51",
            "mac-lte.ul-grant-size": "51",
            "mac-lte.crc-status": "1",
            "mac-lte.carrier-id": "0",
            "mac-lte.ul-tti-count": "1"
          },
          "mac-lte.ul-phy": "",
          "mac-lte.ul-phy_tree": {
            "mac-lte.ul-phy.modulation-type": "4",
            "mac-lte.ul-phy.tbs-index": "19",
            "mac-lte.ul-phy.resource-block-length": "1",
            "mac-lte.ul-phy.resource-block-start": "7",
            "mac-lte.ul-phy.harq-id": "0",
            "mac-lte.ul-phy.ndi": "1"
          },
          "mac-lte.ulsch.header": "",
          "mac-lte.ulsch.header_tree": {
            "mac-lte.sch.subheader": "",
            "mac-lte.sch.subheader_tree": {
              "mac-lte.sch.reserved": "0x00000000",
              "mac-lte.sch.format2": "0",
              "mac-lte.sch.extended": "0x00000000",
              "mac-lte.ulsch.lcid": "0x0000001f"
            }
          },
          "mac-lte.control.bsr": "",
          "mac-lte.control.bsr_tree": {
            "mac-lte.control.bsr.buffer-size-0": "0",
            "mac-lte.control.bsr.buffer-size-1": "0",
            "mac-lte.control.bsr.buffer-size-2": "0",
            "mac-lte.control.bsr.buffer-size-3": "0"
          },
          "mac-lte.sch.header-only": "0",
          "mac-lte.sch.sdu": "b0:05:00:00:00:10:60:c0:00:00:00:00:01:a0:00:00:60:00:01:40:00:00:a0:00:02:20:00:00:00:00:00",
          "rlc-lte": {
            "rlc-lte.context": "",
            "rlc-lte.context_tree": {
              "rlc-lte.direction": "0",
              "rlc-lte.mode": "4",
              "rlc-lte.ueid": "1677",
              "rlc-lte.channel-type": "4",
              "rlc-lte.channel-id": "1",
              "rlc-lte.pdu-length": "31",
              "rlc-lte.am-seqnum-length": "10"
            },
            "rlc-lte.am": "",
            "rlc-lte.am.header": "",
            "rlc-lte.am.header_tree": {
              "rlc-lte.am.frame-type": "0x00000001",
              "rlc-lte.am.rf": "0x00000000",
              "rlc-lte.am.p": "0x00000001",
              "rlc-lte.am.fi": "0x00000002",
              "rlc-lte.am.fixed.e": "0x00000000",
              "rlc-lte.am.fixed.sn": "5"
            },
            "rlc-lte.sequence-analysis": "",
            "rlc-lte.sequence-analysis_tree": {
              "rlc-lte.sequence-analysis.previous-frame": "8233",
              "rlc-lte.sequence-analysis.ok": "1"
            },
            "rlc-lte.am.data": "00:00:00:10:60:c0:00:00:00:00:01:a0:00:00:60:00:01:40:00:00:a0:00:02:20:00:00:00:00:00",
            "rlc-lte.reassembly-info": "",
            "rlc-lte.reassembly-info_tree": {
              "rlc-lte.reassembly-info.number-of-segments": "2",
              "rlc-lte.reassembly-info.total-length": "125",
              "rlc-lte.reassembly-info.segment": {
                "rlc-lte.reassembly-info.segment.sn": "5",
                "rlc-lte.reassembly-info.segment.frame": "8235",
                "rlc-lte.reassembly-info.segment.length": "29"
              }
            },
            "pdcp-lte": {
              "pdcp-lte.configuration": "",
              "pdcp-lte.configuration_tree": {
                "pdcp-lte.direction": "0",
                "pdcp-lte.plane": "1",
                "pdcp-lte.ueid": "1677",
                "pdcp-lte.channel-type": "1",
                "pdcp-lte.channel-id": "1",
                "pdcp-lte.rohc.compression": "0"
              },
              "pdcp-lte.reserved": "0",
              "pdcp-lte.seq-num": "3",
              "pdcp-lte.sequence-analysis": "",
              "pdcp-lte.sequence-analysis_tree": {
                "pdcp-lte.sequence-analysis.previous-frame": "8222",
                "pdcp-lte.sequence-analysis.expected-sn": "3",
                "pdcp-lte.sequence-analysis.ok": "1"
              },
              "lte_rrc": {
                "lte_rrc": "LTE Radio Resource Control (RRC) protocol",
                "lte-rrc.UL_DCCH_Message_element": {
                  "per.choice_index": "0",
                  "lte-rrc.message": "0",
                  "lte-rrc.message_tree": {
                    "per.choice_index": "9",
                    "lte-rrc.c1": "9",
                    "lte-rrc.c1_tree": {
                      "lte-rrc.ulInformationTransfer_element": {
                        "per.choice_index": "0",
                        "lte-rrc.criticalExtensions": "0",
                        "lte-rrc.criticalExtensions_tree": {
                          "per.choice_index": "0",
                          "lte-rrc.c1": "0",
                          "lte-rrc.c1_tree": {
                            "lte-rrc.ulInformationTransfer_r8_element": {
                              "per.optional_field_bit": "0",
                              "per.choice_index": "0",
                              "lte-rrc.dedicatedInfoType": "0",
                              "lte-rrc.dedicatedInfoType_tree": {
                                "per.octet_string_length": "117",
                                "lte-rrc.dedicatedInfoNAS": "27:e6:80:7b:05:01:02:01:da:28:13:12:4d:43:53:54:61:61:73:74:69:6e:67:44:65:66:61:75:6c:74:27:55:80:c2:23:16:01:00:00:16:10:24:b7:e8:e8:24:b7:e8:e8:24:b7:e8:e8:24:b7:e8:e8:2a:c2:23:16:02:00:00:16:10:44:b8:c1:f0:b4:39:da:9b:4b:83:fd:42:b9:cb:c0:a7:2a:80:21:10:01:00:00:10:81:06:00:00:00:00:83:06:00:00:00:00:00:0d:00:00:03:00:00:0a:00:00:05:00:00:11:00",
                                "lte-rrc.dedicatedInfoNAS_tree": {
                                  "nas-eps": {
                                    "nas_eps.security_header_type": "2",
                                    "gsm_a.L3_protocol_discriminator": "0x00000002",
                                    "nas_eps.msg_auth_code": "0xe6807b05",
                                    "nas_eps.seq_no": "1",
                                    "nas_eps.bearer_id": "0",
                                    "nas_eps.esm.proc_trans_id": "1",
                                    "nas_eps.nas_msg_esm_type": "218",
                                    "Access Point Name": {
                                      "gsm_a.gm.elem_id": "0x00000028",
                                      "gsm_a.len": "19",
                                      "gsm_a.gm.sm.apn": "MCSTaastingDefault"
                                    },
                                    "Protocol Configuration Options": {
                                      "gsm_a.gm.elem_id": "0x00000027",
                                      "gsm_a.len": "85",
                                      "gsm_a.gm.sm.link_dir": "0",
                                      "gsm_a.gm.sm.ext": "1",
                                      "gsm_a.gm.configuration_protocol": "0",
                                      "gsm_a.gm.sm.pco_pid": "0x00000011",
                                      "gsm_a.gm.sm.pco_pid_tree": {
                                        "gsm_a.gm.sm.pco.length": "0x00000000"
                                      }
                                    }
                                  }
                                }
                              }
                            }
                          }
                        }
                      }
                    }
                  }
                }
              },
              "pdcp-lte.mac": "0x00000000"
            }
          },
          "mac-lte.padding-data": "00:00:00:00:00:00:00:00:00:00:00:00:00",
          "mac-lte.padding-length": "13"
        },
        "mac-lte.ulsch": "",
        "_ws.lua.fake": "",
        "_ws.col.Info": "ULInformationTransfer, ESM information response",
        "_ws.col.Protocol": "LTE RRC UL_DCCH/NAS-EPS"
      }
    }