#######################################################################

# Anritsu Generated PICS/PIXIT file

#

# Changes Applied: 3GPP_TS_34.123-3_AND_NR_n78_AND_TestSequence-688728358_AND_NR_n78_AND_TestSequence-688728358

#######################################################################

pc_1xCSfallback,                             BOOLEAN,       false   #-- @desc  Support of 1xCS fallback

pc_1xRTT,                                    BOOLEAN,       false   #-- @desc  UE supports CDMA2000 1xRTT band class

pc_4Layer_spatial_mux_tm3_tm4,               BOOLEAN,       TRUE    #-- @desc  Support of 4 layer spatial multiplexing with transmission mode 3 and transmission mode 4

pc_5GCN,                                     BOOLEAN,       TRUE    #-- @desc  UE supports 5GS Core

pc_5GCN_N3AN,                                BOOLEAN,       false   #-- @desc  UE supports 5GS Core over non-3GPP Access Network

pc_5GC_NSSAA,                                BOOLEAN,       false   #-- @desc  Support of network slice-specific authentication and authorization

pc_5GC_NSSAA_EAP_AKA_Prime,                  BOOLEAN,       false   #-- @desc  Support of EAP-AKA as EAP method for network slice-specific authentication and authorization

pc_5GC_RACS,                                 BOOLEAN,       false   #-- @desc  Support of RACS

pc_5GC_RACS_Manufacturer_URCID,              BOOLEAN,       false   #-- @desc  UE support of Manufacturer assigned radio capability ID

pc_A5_4_CS,                                  BOOLEAN,       TRUE    #-- @desc  Support of A54

pc_APN_Default_Configuration,                ENUM-APN_DefaultConfiguration_Type,internet #-- @desc  The DNNAPN configuration specified in TS 38.508-1 [2] Table 4.8.4-1 which is to be used for the default DNNAPN.

pc_APN_ID_IMS,                               CHARSTRING,    ims     #-- @desc  APNDNN ID of type IMS

pc_APN_ID_Internet,                          CHARSTRING,    ABCDE   #-- @desc  APNDNN ID of type Internet

pc_APN_ID_MIOT,                              CHARSTRING,    MIOT    #-- @desc  APNDNN ID of type MIOT

pc_APN_ID_URLLC,                             CHARSTRING,    URLLC   #-- @desc  APNDNN ID of type URLLC

pc_APN_ID_V2X,                               CHARSTRING,    V2X     #-- @desc  APNDNN ID of type V2X

pc_APN_RateControl,                          BOOLEAN,       false   #-- @desc  The UE supports APN rate control

pc_A_BDS,                                    BOOLEAN,       TRUE    #-- @desc Support for A-BDS

pc_A_GLONASS,                                BOOLEAN,       TRUE    #-- @desc Support for A-GLONASS

pc_A_GPS_ADR,                                BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Gps

pc_A_GPS_ADR_ENH,                            BOOLEAN,       false   #-- @desc Support of ADR enhancements for Gps

pc_A_GPS_HA,                                 BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Gps

pc_A_GPS_L1C,                                BOOLEAN,       false   #-- @desc Support of A-GPS L1C signal

pc_A_GPS_L1C_A,                              BOOLEAN,       TRUE    #-- @desc Support for A-GPS L1C/A

pc_A_GPS_L1C_A_MGPS,                         BOOLEAN,       TRUE    #-- @desc Support for A-GPS L1C/A and Modernized GPS

pc_A_GPS_L2C,                                BOOLEAN,       false   #-- @desc Support of A-GPS L2C signal

pc_A_GPS_L5,                                 BOOLEAN,       TRUE    #-- @desc Support of A-GPS L5 signal

pc_A_GPS_VelocityMeas,                       BOOLEAN,       TRUE    #-- @desc Support of Velocity measurement reporting for Gps

pc_A_Galileo,                                BOOLEAN,       TRUE    #-- @desc Support for A-Galileo

pc_A_QZSS,                                   BOOLEAN,       false   #-- @desc Support of A-QZSS

pc_A_SBAS,                                   BOOLEAN,       false   #-- @desc Support of A-SBAS

pc_Additional_PDU_establishment,             BOOLEAN,       TRUE    #-- @desc  ExpectedNoOfPDUSessionsAtRegistration + 1

pc_Allowed_CSG_list,                         BOOLEAN,       TRUE    #-- @desc  Support of Allowed CSG list

pc_Attach,                                   BOOLEAN,       false   #-- @desc  Support EPS attach (with or without pre-configuration)

pc_AttachWithIMSI,                           BOOLEAN,       false   #-- @desc  Support of Attach With IMSI

pc_AttachWithPDN,                            BOOLEAN,       TRUE    #-- @desc  Support of EMM-REGISTERED with PDN

pc_AttachWithoutPDN,                         BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED without PDN

pc_Auto_Attach_after_TAU_Reject,             BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) after the TAU Reject

pc_Auto_PDN_Connectivity,                    BOOLEAN,       TRUE    #-- @desc  Support of automatic PDN Connectivity in EUTRAN

pc_AutomaticAttachSwitchON,                  BOOLEAN,       TRUE    #-- @desc  Support of automatic PS attach procedure at switch on.

pc_Automatic_EPS_Re_Attach,                  BOOLEAN,       TRUE    #-- @desc  Support of automatic re-activation of the EPS bearer(s)

pc_Automatic_Re_Attach,                      BOOLEAN,       TRUE    #-- @desc  Support of automatic re-activation of the EPS bearer(s) during Network Initiated Detach with detach type set to re-attach required

pc_Autonomous_search_function_nr_CAG,        BOOLEAN,       false   #-- @desc  Support of autonomous search function to detect CAG cells on serving and non-serving frequencies

pc_Available_PLMNs_AcT_Ind,                  BOOLEAN,       false   #-- @desc  Support of AccessTechnology indication in available PLMNs list

pc_B41_UE_PC2,                               BOOLEAN,       TRUE    #-- @desc  Support of TDD Band 41 Power class 2 operation

pc_BDS,                                      BOOLEAN,       false   #-- @desc Support for BDS

pc_BDS_ADR,                                  BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for BDS

pc_BDS_ADR_ENH,                              BOOLEAN,       false   #-- @desc Support of ADR enhancements for BDS

pc_BDS_B1C,                                  BOOLEAN,       false   #-- @desc  Support for A-BDS B1C

pc_BDS_B1I,                                  BOOLEAN,       TRUE    #-- @desc Support for A-BDS B1I

pc_BDS_DiffCorr,                             BOOLEAN,       false   #-- @desc Bbds-DifferentialCorrectionsSupport for B1I

pc_BDS_GridMod,                              BOOLEAN,       false   #-- @desc Bbds-GridModelSupport

pc_BDS_HA,                                   BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for BDS

pc_BDS_VelocityMeas,                         BOOLEAN,       TRUE    #-- @desc Support of Velocity measurement reporting for BDS

pc_BSRVCC,                                   BOOLEAN,       TRUE    #-- @desc  UE indicates g.3gpp.ps2cs-srvcc-orig-pre-alerting media feature tag in INVITE request

pc_Background,                               BOOLEAN,       TRUE    #-- @desc  UE Supports Background QoS class

pc_Band10_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 10

pc_Band11_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 11

pc_Band12_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 12

pc_Band13_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 13

pc_Band14_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 14

pc_Band19_Supp,                              BOOLEAN,       TRUE    #-- @desc  TRUE if UE supports Frequency Band 19

pc_Band1_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 1

pc_Band20_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 20

pc_Band21_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 21

pc_Band22_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 22

pc_Band25_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 25

pc_Band26_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 26

pc_Band2_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 2

pc_Band32_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 32

pc_Band3_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 3

pc_Band4_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 4

pc_Band5_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 5

pc_Band6_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 6

pc_Band7_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 7

pc_Band8_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 8

pc_Band9_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 9

pc_Bds_DiffCorr_B1C,                         BOOLEAN,       false   #-- @desc Bds-DifferentialCorrectionsSupport for B1C

pc_BidirecVoiceOverIMS,                      BOOLEAN,       TRUE    #-- @desc  UE capable of initiating a bidirectional voice session over IMS

pc_Bluetooth,                                BOOLEAN,       false   #-- @desc Support for UE-Assisted Bluetooth

pc_CAG,                                      BOOLEAN,       false   #-- @desc  Support of Closed Access Group

pc_CE_Measurements,                          BOOLEAN,       TRUE    #-- @desc  Support of intra-frequency RSRQ measurements and inter-frequency RSRP and RSRQ measurements in RRC_CONNECTED

pc_CEmodeA,                                  BOOLEAN,       false   #-- @desc  Support of CE mode A

pc_CEmodeB,                                  BOOLEAN,       false   #-- @desc  Support of CE mode B

pc_CMAS_Message,                             BOOLEAN,       TRUE    #-- @desc  Support of CMAS message

pc_CMAS_NR,                                  BOOLEAN,       TRUE    #-- @desc  Support of CMAS message on NR

pc_CRS_Interference_Handling,                BOOLEAN,       false   #-- @desc  Support of CRS interference handling

pc_CS,                                       BOOLEAN,       TRUE    #-- @desc  UE supports CS domain services

pc_CSI_RS_DS_Meas,                           BOOLEAN,       TRUE    #-- @desc  Support of CSI-RS based discovery signals measurement

pc_CS_Em_Call_in_1xRTT,                      BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in 1xRTT

pc_CS_Em_Call_in_GERAN,                      BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in GERAN

pc_CS_Em_Call_in_UTRA,                       BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in UTRA

pc_CS_Fallback,                              BOOLEAN,       TRUE    #-- @desc  The UE supports CS fallback for voice calls. If true pc_CS and at least one of pc_FDD pc_TDD_HCR pc_TDD_LCR pc_TDD_VHCR or pc_UMTS_GSM is also true.

pc_CS_MO_LR_CSFallback,                      BOOLEAN,       TRUE    #-- @desc Support for CS-MO-LR with CS Fallback for a position estimate

pc_CS_PS_data_centric,                       BOOLEAN,       false   #-- @desc  Support of CSPS mode 2

pc_CS_PS_voice_centric,                      BOOLEAN,       TRUE    #-- @desc  Support of configuring the UE to voice centric

pc_Category_M1_voice,                        BOOLEAN,       false   #-- @desc  Support for GSMA PRD NG.108 "IMS Profile for Voice and SMS for UE Category M1"

pc_Combined_Attach,                          BOOLEAN,       TRUE    #-- @desc  Support combined EPSIMSI attach (with or without pre-configuration)

pc_CommunicationHold_DuringEmergencyCall,    BOOLEAN,       false   #-- @desc  UE supports Communication Hold during emergency call

pc_Concatenated_SMS_IP_MO,                   BOOLEAN,       TRUE    #-- @desc  Concatenated SM-over-IP sender

pc_Concatenated_SMS_IP_MT,                   BOOLEAN,       TRUE    #-- @desc  Concatenated SM-over-IP receiver

pc_Control_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of Control Plane CIoT

pc_DC_SCG_DRB,                               BOOLEAN,       false   #-- @desc  Support of DC SCG DRB

pc_DC_Split_DRB,                             BOOLEAN,       false   #-- @desc  Support of DC Split DRB

pc_DL_256QAM,                                BOOLEAN,       TRUE    #-- @desc  Support of downlink 256 QAM

pc_DL_AoD_periodicalReporting_UEA,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode

pc_DL_AoD_periodicalReporting_UEB,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode

pc_DL_AoD_periodicalReporting_standalone,    BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode

pc_DL_CA_2Carriers,                          BOOLEAN,       TRUE    #-- @desc  DL CA with 2 carriers

pc_DL_CA_3Carriers,                          BOOLEAN,       TRUE    #-- @desc  DL CA with 3 carriers

pc_DL_NR_CA_3CC,                             BOOLEAN,       false   #-- @desc  DL NR CA with 3 carriers

pc_DL_PRS_RSRP_MeasFR1,                      BOOLEAN,       TRUE    #-- @desc  Support of DL-PRS-RSRP-MeasFR1

pc_DL_PRS_RSRP_MeasFR2,                      BOOLEAN,       false   #-- @desc  Support of DL-PRS-RSRP-MeasFR2

pc_DL_TDOA_additionalPathsReport,            BOOLEAN,       false   #-- @desc  Support of additionalPathsReport

pc_DL_TDOA_periodicalReporting_UEA,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode

pc_DL_TDOA_periodicalReporting_UEB,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode

pc_DL_TDOA_periodicalReporting_standalone,   BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode

pc_DL_interBand_CaBwClassComb_AA,            BOOLEAN,       TRUE    #-- @desc  DL Inter-band contiguous CA BW class A-A

pc_DL_intraBand_ContCaBWclassB,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class B

pc_DL_intraBand_ContCaBWclassC,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class C

pc_DL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       TRUE    #-- @desc  Support of DL intra-band non-contiguous CA BW Class Combination A-A

pc_DRX_Adaptation,                           BOOLEAN,       false   #-- @desc  Supports DRX adaptation

pc_DSMIPv6,                                  BOOLEAN,       false   #-- @desc  Support of Mobility management based on Dual-Stack Mobile IPv6

pc_DaylightSavingTime,                       BOOLEAN,       TRUE    #-- @desc  UE storesupdates the daylight saving time when receives information

pc_DualRM_Coding,                            BOOLEAN,       TRUE    #-- @desc  Dual RM Coding

pc_EAB,                                      BOOLEAN,       TRUE    #-- @desc  Support of Extended Access Barring

pc_EAB_override,                             BOOLEAN,       TRUE    #-- @desc  Support of Extended Access Barring Override

pc_ECID,                                     BOOLEAN,       TRUE    #-- @desc Support of UE assisted ECID

pc_ECID_Rsrp,                                BOOLEAN,       TRUE    #-- @desc Support fo RSRP

pc_ECID_Rsrq,                                BOOLEAN,       TRUE    #-- @desc Support of RSRQ

pc_ECID_UeRxTx,                              BOOLEAN,       TRUE    #-- @desc Support of UE Rx-Tx Time Difference

pc_ECID_idleStateForMeasurements,            BOOLEAN,       false   #-- @desc Support of idleStateForMeasurements

pc_ECID_periodicalReporting,                 BOOLEAN,       false   #-- @desc Support of periodicalReporting

pc_ECID_triggeredReporting,                  BOOLEAN,       false   #-- @desc Support of triggeredReporting

pc_ECID_ueRxTxSupTDD,                        BOOLEAN,       TRUE    #-- @desc Support of ueRxTxSupTDD

pc_EDCH_UE_Category_FDD,                     INTEGER,       6       #-- @desc  FDD E-DCH physical layer categories

pc_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  LCR TDD E-DCH physical layer categories

pc_EDTM,                                     BOOLEAN,       false   #-- @desc  Support for EDTM

pc_EMM_Information,                          BOOLEAN,       TRUE    #-- @desc  Support of EMM Information message

pc_EN_DC,                                    BOOLEAN,       TRUE    #-- @desc  EN-DC (Option 3)

pc_EPC_MO_LR_RequestAssistanceData,          BOOLEAN,       TRUE    #-- @desc Support of EPC-MO-LR request for assistance data

pc_EPC_MO_LR_RequestPositionEstimate,        BOOLEAN,       TRUE    #-- @desc Support of EPC-MO-LR request for a position estimate

pc_EPC_RACS,                                 BOOLEAN,       false   #-- @desc  Support of RACS

pc_EPS_IMS_EmergencyCall,                    BOOLEAN,       false   #-- @desc  Support of MS emergency call in EPS

pc_EPS_IMS_eCall_Capable,                    BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services over EPS

pc_EPS_IMS_eCall_Only,                       BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services over EPS

pc_EPS_Services_Disable,                     BOOLEAN,       TRUE    #-- @desc  Support of disabling of EPS services

pc_EPS_fallback,                             BOOLEAN,       TRUE    #-- @desc  Support of EPS fallback

pc_ESM_MO_Bearer_Allocation,                 BOOLEAN,       TRUE    #-- @desc  Support of ESM UE requested bearer resource allocation procedure

pc_ESM_MO_Bearer_Modification,               BOOLEAN,       TRUE    #-- @desc  Support of ESM UE requested bearer resource modification procedure

pc_ESM_Notification,                         BOOLEAN,       TRUE    #-- @desc  Support of ESM Notification procedure

pc_ESM_UE_Modification_NW_TFT,               BOOLEAN,       TRUE    #-- @desc  Support for UE requested modification of network allocated TFTs

pc_ETWS_NR,                                  BOOLEAN,       TRUE    #-- @desc  Support of ETWS message on NR

pc_ETWS_message,                             BOOLEAN,       TRUE    #-- @desc  Support of ETWS message

pc_E_UTRAN_2_GERAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support for inter-RAT PS handover from E_UTRAN to GERAN

pc_E_UTRA_WLAN_offload,                      BOOLEAN,       TRUE    #-- @desc  Support Offload tofrom WLAN and supports S2b

pc_EarlyMedia,                               BOOLEAN,       TRUE    #-- @desc  UE supports early media

pc_EmergSpeech,                              BOOLEAN,       TRUE    #-- @desc  Emergency Call

pc_EmergencyService_fallback,                BOOLEAN,       TRUE    #-- @desc  Support of emergency services fallback

pc_Enable_Disable_SMSoverIMS,                BOOLEAN,       TRUE    #-- @desc  UE supports enablingdisabling SMS over IMS

pc_Enhanced_1xCSfallback,                    BOOLEAN,       false   #-- @desc  Support of Enhanced 1xCS fallback

pc_FDD,                                      BOOLEAN,       TRUE    #-- @desc  UE supports UTRA band as defined in TS 25.101

pc_FDD_TypeB_HalfDuplex,                     BOOLEAN,       false   #-- @desc  Support of Type B Half duplex FDD operation

pc_FDDtoTDD_Handover,                        BOOLEAN,       TRUE    #-- @desc  Support Handover between FDD and TDD

pc_FDPCH,                                    BOOLEAN,       TRUE    #-- @desc  Full support of F-DPCH

pc_FR1toFR2_Handover,                        BOOLEAN,       TRUE    #-- @desc  Support Handover between FR1 and FR2

pc_Fast_First_HPPLMN_Search,                 BOOLEAN,       TRUE    #-- @desc  Support of Fast First Higher Piority PLMN search

pc_FeatrGrp_101_F,                           BOOLEAN,       TRUE    #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_101_T,                           BOOLEAN,       TRUE    #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_102_F,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_102_T,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_103_F,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_103_T,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_104_F,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_104_T,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_105_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_105_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_106_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_106_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_107_F,                           BOOLEAN,       TRUE    #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_107_T,                           BOOLEAN,       TRUE    #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_108_F,                           BOOLEAN,       TRUE    #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_108_T,                           BOOLEAN,       TRUE    #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_109_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_109_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_10_F,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_10_T,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_110_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_110_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_111_F,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_111_T,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_112_F,                           BOOLEAN,       TRUE    #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_112_T,                           BOOLEAN,       TRUE    #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_113_F,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_113_T,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_114_F,                           BOOLEAN,       TRUE    #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_114_T,                           BOOLEAN,       TRUE    #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_115_F,                           BOOLEAN,       TRUE    #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_115_T,                           BOOLEAN,       TRUE    #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_116_F,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_116_T,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_11_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_11_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_12_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_12_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_13_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_13_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_14_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_14_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_15_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_15_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_16_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_16_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_17_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_17_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_18_F,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_18_T,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_19_F,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_19_T,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_1_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_1_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_20_F,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_20_T,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_21_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_21_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_22_F,                            BOOLEAN,       TRUE    #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_22_T,                            BOOLEAN,       TRUE    #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_F,                            BOOLEAN,       TRUE    #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_T,                            BOOLEAN,       TRUE    #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_F,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_T,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_26_F,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_26_T,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_27_F,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_27_T,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_28_F,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling

pc_FeatrGrp_28_T,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling

pc_FeatrGrp_29_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_29_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_2_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_2_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_30_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_30_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_31_F,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_31_T,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_33_F,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for UTRAN including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to reportStrongestCellsForSON

pc_FeatrGrp_33_T,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for UTRAN including:

pc_FeatrGrp_34_F,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_34_T,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_35_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_35_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_36_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:

pc_FeatrGrp_36_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to portStrongestCellsForSON

pc_FeatrGrp_37_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_37_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_38_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_38_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_F,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_T,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_3_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_3_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_40_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_40_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_41_F,                            BOOLEAN,       TRUE    #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_41_T,                            BOOLEAN,       TRUE    #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_42_F,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments)

pc_FeatrGrp_42_T,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments)

pc_FeatrGrp_4_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_4_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_5_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_5_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_6_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_6_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_7_F,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM

pc_FeatrGrp_7_T,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM

pc_FeatrGrp_8_F,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_8_T,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_9_F,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FeatrGrp_9_T,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FixedBroadband,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Broadband

pc_FlexibleStartPRB_PDSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PDSCH

pc_FlexibleStartPRB_PUSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PUSCH

pc_FlightPathPlan,                           BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement

pc_FullNameNetwork,                          BOOLEAN,       TRUE    #-- @desc  Support of storage of the network full name

pc_GALILEO,                                  BOOLEAN,       false   #-- @desc Support for Galileo

pc_GALILEO_ADR,                              BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Galileo

pc_GALILEO_ADR_ENH,                          BOOLEAN,       false   #-- @desc Support of ADR enhancements for Galileo

pc_GALILEO_E1,                               BOOLEAN,       TRUE    #-- @desc Support of E1 signal in Galileo

pc_GALILEO_E5a,                              BOOLEAN,       false   #-- @desc Support of E5a signal in Galileo

pc_GALILEO_E5aE5b,                           BOOLEAN,       false   #-- @desc Support of E5a+E5b signal in Galileo

pc_GALILEO_E5b,                              BOOLEAN,       false   #-- @desc Support of E5b signal in Galileo

pc_GALILEO_E6,                               BOOLEAN,       false   #-- @desc Support of E6 signal in Galileo

pc_GALILEO_HA,                               BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Galileo

pc_GALILEO_VelocityMeas,                     BOOLEAN,       TRUE    #-- @desc Support of Velocity measurement reporting for Galileo

pc_GERAN,                                    BOOLEAN,       TRUE    #-- @desc  UE Supports GSM andor GPRS

pc_GERAN_2_E_UTRAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support of GERAN to E-UTRAN PS Handover

pc_GERAN_2_E_UTRAN_meas,                     BOOLEAN,       TRUE    #-- @desc  Supports Neighbour Cell measurements and Network controlled & autonomous cell reselection to E-UTRAN

pc_GERAN_2_E_UTRAN_measreporting_CCN,        BOOLEAN,       TRUE    #-- @desc  Supports CCN towards E-UTRAN E-UTRAN Neighbour cell measurement reporting and Network controlled cell reselection to E-UTRAN

pc_GLONASS,                                  BOOLEAN,       TRUE    #-- @desc Support for GLONASS

pc_GLONASS_ADR,                              BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Glonass

pc_GLONASS_ADR_ENH,                          BOOLEAN,       false   #-- @desc Support of ADR enhancements for Glonass

pc_GLONASS_G1,                               BOOLEAN,       TRUE    #-- @desc Support of G1 signal in Glonass

pc_GLONASS_G2,                               BOOLEAN,       false   #-- @desc Support of G2 signal in Glonass

pc_GLONASS_G3,                               BOOLEAN,       false   #-- @desc Support of G3 signal in Glonass

pc_GLONASS_HA,                               BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Glonass

pc_GLONASS_VelocityMeas,                     BOOLEAN,       TRUE    #-- @desc Support of Velocity measurement reporting for Glonass

pc_GNSS_AA,                                  BOOLEAN,       TRUE    #-- @desc Support of GNSS Acquisition Assistance

pc_GNSS_AcquAssistSup_BDS,                   BOOLEAN,       TRUE    #-- @desc Gnss-AcquisitionAssistanceSupport for BDS

pc_GNSS_AcquAssistSup_Galileo,               BOOLEAN,       TRUE    #-- @desc Gnss-AcquisitionAssistanceSupport for Galileo

pc_GNSS_AcquAssistSup_Glonass,               BOOLEAN,       TRUE    #-- @desc Gnss-AcquisitionAssistanceSupport for GLONASS

pc_GNSS_AcquAssistSup_Gps,                   BOOLEAN,       TRUE    #-- @desc Gnss-AcquisitionAssistanceSupport for GPS

pc_GNSS_AcquAssistSup_Qzss,                  BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for QZSS

pc_GNSS_AcquAssistSup_Sbas,                  BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for SBAS

pc_GNSS_AcquAssist_BDS_B1C,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1C

pc_GNSS_AcquAssist_BDS_B1I,                  BOOLEAN,       TRUE    #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1I

pc_GNSS_AcquAssist_GPS_L1CA,                 BOOLEAN,       TRUE    #-- @desc Support of GNSS-AcquisitionAssistance for GPS L1 C/A

pc_GNSS_AcquAssist_GPS_L5,                   BOOLEAN,       TRUE    #-- @desc Support of GNSS-AcquisitionAssistance for GPS L5

pc_GNSS_AcquAssist_Galileo_E1,               BOOLEAN,       TRUE    #-- @desc Support of GNSS-AcquisitionAssistance for Galileo E1

pc_GNSS_AcquAssist_Galileo_E5A,              BOOLEAN,       false   #-- @desc Support of GNSS-AcquisitionAssistance for Galileo E5A

pc_GNSS_AlmanacSup_BDS,                      BOOLEAN,       TRUE    #-- @desc Gnss-AlmanacSupport for BDS (Model-7)

pc_GNSS_AlmanacSup_Galileo,                  BOOLEAN,       TRUE    #-- @desc Gnss-AlmanacSupport for Galileo (Model-1)

pc_GNSS_AlmanacSup_Glonass,                  BOOLEAN,       TRUE    #-- @desc Gnss-AlmanacSupport for GLONASS (Model-5)

pc_GNSS_AlmanacSup_Gps,                      BOOLEAN,       TRUE    #-- @desc Gnss-AlmanacSupport for GPS (Model-2)

pc_GNSS_AlmanacSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for QZSS (Model-2)

pc_GNSS_AlmanacSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for SBAS (Model-6)

pc_GNSS_AuxInfoSup_BDS,                      BOOLEAN,       TRUE    #-- @desc Gnss-AuxiliaryInformationSupport for BDS

pc_GNSS_AuxInfoSup_Galileo,                  BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for Galileo

pc_GNSS_AuxInfoSup_Glonass,                  BOOLEAN,       TRUE    #-- @desc Gnss-AuxiliaryInformationSupport for GLONASS

pc_GNSS_AuxInfoSup_Gps,                      BOOLEAN,       TRUE    #-- @desc Gnss-AuxiliaryInformationSupport for GPS

pc_GNSS_AuxInfoSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for QZSS

pc_GNSS_AuxInfoSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for SBAS

pc_GNSS_DGNSS_Sup_BDS,                       BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for BDS B1I

pc_GNSS_DGNSS_Sup_Bds_B1C,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for BDS B1C

pc_GNSS_DGNSS_Sup_Galileo,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for Galileo E1

pc_GNSS_DGNSS_Sup_Galileo_E5A,               BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for Galileo E5A

pc_GNSS_DGNSS_Sup_Glonass,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GLONASS

pc_GNSS_DGNSS_Sup_Gps,                       BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GPS L1 C/A

pc_GNSS_DGNSS_Sup_Gps_L5,                    BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GPS L5

pc_GNSS_DGNSS_Sup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for QZSS

pc_GNSS_DGNSS_Sup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for SBAS

pc_GNSS_DataBitsSup_BDS,                     BOOLEAN,       TRUE    #-- @desc Gnss-DataBitAssistanceSupport for BDS

pc_GNSS_DataBitsSup_Galileo,                 BOOLEAN,       TRUE    #-- @desc Gnss-DataBitAssistanceSupport for Galileo

pc_GNSS_DataBitsSup_Glonass,                 BOOLEAN,       TRUE    #-- @desc Gnss-DataBitAssistanceSupport for GLONASS

pc_GNSS_DataBitsSup_Gps,                     BOOLEAN,       TRUE    #-- @desc Gnss-DataBitAssistanceSupport for GPS

pc_GNSS_DataBitsSup_Qzss,                    BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for QZSS

pc_GNSS_DataBitsSup_Sbas,                    BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for SBAS

pc_GNSS_EOPSup,                              BOOLEAN,       TRUE    #-- @desc Gnss-EarthOrientationParametersSupport (Common Assistance Data)

pc_GNSS_EllipArc,                            BOOLEAN,       false   #-- @desc Ellipsoid Arc Support

pc_GNSS_EllipPoint,                          BOOLEAN,       TRUE    #-- @desc Ellipsoid Point Support

pc_GNSS_EllipPointAlt,                       BOOLEAN,       TRUE    #-- @desc Ellipsoid Point With Altitude Support

pc_GNSS_EllipPointAltUncertEllip,            BOOLEAN,       TRUE    #-- @desc Ellipsoid Point With Altitude And Uncertainty Ellipsoid Support

pc_GNSS_EllipPointUncertCircle,              BOOLEAN,       TRUE    #-- @desc Ellipsoid Point With Uncertainty Circle Support

pc_GNSS_EllipPointUncertEllip,               BOOLEAN,       TRUE    #-- @desc Ellipsoid Point With Uncertainty Ellipse Support

pc_GNSS_FTA,                                 BOOLEAN,       false   #-- @desc Support of GNSS Fine Time Assistance

pc_GNSS_FTA_UEA,                             BOOLEAN,       false   #-- @desc Support of UE Fine Time Assistance measurements for UE-assisted Assisted-GNSS

pc_GNSS_FTA_UEB,                             BOOLEAN,       false   #-- @desc Support of UE Fine Time Assistance measurements for UE-based Assisted-GNSS

pc_GNSS_HA_EllipPointAltUncertEllip,         BOOLEAN,       false   #-- @desc High Accuracy Ellipsoid Point With Altitude And Uncertainty Ellipsoid-r15

pc_GNSS_HA_EllipPointUncertCircle,           BOOLEAN,       false   #-- @desc High Accuracy Ellipsoid Point With Uncertainty Ellipse-r15

pc_GNSS_HVVel,                               BOOLEAN,       false   #-- @desc Horizontal With Vertical Velocity Support

pc_GNSS_HVVelUncert,                         BOOLEAN,       TRUE    #-- @desc Horizontal With Vertical Velocity And Uncertainty Support

pc_GNSS_HVel,                                BOOLEAN,       false   #-- @desc Horizontal Velocity Support

pc_GNSS_HVelUncert,                          BOOLEAN,       false   #-- @desc Horizontal Velocity With Uncertainty Support

pc_GNSS_IonoModSup,                          BOOLEAN,       TRUE    #-- @desc Gnss-IonosphericModelSupport (Common Assistance Data)

pc_GNSS_NavModSup_BDS,                       BOOLEAN,       TRUE    #-- @desc Gnss-NavigationModelSupport for BDS (Model-6)

pc_GNSS_NavModSup_Galileo,                   BOOLEAN,       TRUE    #-- @desc Gnss-NavigationModelSupport for Galileo (Model-1)

pc_GNSS_NavModSup_Glonass,                   BOOLEAN,       TRUE    #-- @desc Gnss-NavigationModelSupport for GLONASS (Model-4)

pc_GNSS_NavModSup_Gps,                       BOOLEAN,       TRUE    #-- @desc Gnss-NavigationModelSupport for GPS (Model-2)

pc_GNSS_NavModSup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for QZSS (Model-2)

pc_GNSS_NavModSup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for SBAS (Model-5)

pc_GNSS_Polygon,                             BOOLEAN,       false   #-- @desc Polygon Support

pc_GNSS_RTISup_BDS,                          BOOLEAN,       TRUE    #-- @desc Gnss-RealTimeIntegritySupport for BDS

pc_GNSS_RTISup_Galileo,                      BOOLEAN,       TRUE    #-- @desc Gnss-RealTimeIntegritySupport for Galileo

pc_GNSS_RTISup_Glonass,                      BOOLEAN,       TRUE    #-- @desc Gnss-RealTimeIntegritySupport for GLONASS

pc_GNSS_RTISup_Gps,                          BOOLEAN,       TRUE    #-- @desc Gnss-RealTimeIntegritySupport for GPS

pc_GNSS_RTISup_Qzss,                         BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for QZSS

pc_GNSS_RTISup_Sbas,                         BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for SBAS

pc_GNSS_RTK_AuxStationInfo,                  BOOLEAN,       false   #-- @desc Gnss-RTK-AuxiliaryStationDataSupport-r15 (Common assistance data)

pc_GNSS_RTK_BiasInfo_Glonass,                BOOLEAN,       false   #-- @desc Glo-RTK-BiasInformationSupport-r15

pc_GNSS_RTK_FKP_Gradients_Bds,               BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for BDS

pc_GNSS_RTK_FKP_Gradients_Galileo,           BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for Galileo

pc_GNSS_RTK_FKP_Gradients_Glonass,           BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for GLONASS

pc_GNSS_RTK_FKP_Gradients_Gps,               BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for GPS

pc_GNSS_RTK_MAC_CorrectionDifferences_Bds,   BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for BDS

pc_GNSS_RTK_MAC_CorrectionDifferences_Galileo,BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for Galileo

pc_GNSS_RTK_MAC_CorrectionDifferences_Glonass,BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GLONASS

pc_GNSS_RTK_MAC_CorrectionDifferences_Gps,   BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GPS

pc_GNSS_RTK_OBS_Bds,                         BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for BDS B1I

pc_GNSS_RTK_OBS_Bds_B1C,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for BDS B1C

pc_GNSS_RTK_OBS_Galileo,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for Galileo

pc_GNSS_RTK_OBS_Galileo_E5A,                 BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for Galileo E5A

pc_GNSS_RTK_OBS_Glonass,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GLONASS

pc_GNSS_RTK_OBS_Gps,                         BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GPS L1 C/A

pc_GNSS_RTK_OBS_Gps_L5,                      BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GPS L5

pc_GNSS_RTK_RefStationInfo,                  BOOLEAN,       false   #-- @desc Gnss-RTK-ReferenceStationInfoSupport-r15 (Common assistance data)

pc_GNSS_RTK_Residuals_Bds,                   BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for BDS

pc_GNSS_RTK_Residuals_Galileo,               BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for Galileo

pc_GNSS_RTK_Residuals_Glonass,               BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for GLONASS

pc_GNSS_RTK_Residuals_Gps,                   BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for GPS

pc_GNSS_RTK_SSR_ClockCorrections_Bds,        BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for BDS

pc_GNSS_RTK_SSR_ClockCorrections_Galileo,    BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for Galileo

pc_GNSS_RTK_SSR_ClockCorrections_Glonass,    BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for GLONASS

pc_GNSS_RTK_SSR_ClockCorrections_Gps,        BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for GPS

pc_GNSS_RTK_SSR_CodeBias_Bds,                BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for BDS B1I

pc_GNSS_RTK_SSR_CodeBias_Bds_B1C,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for BDS B1C

pc_GNSS_RTK_SSR_CodeBias_Galileo,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for Galileo E1

pc_GNSS_RTK_SSR_CodeBias_Galileo_E5A,        BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for Galileo E5A

pc_GNSS_RTK_SSR_CodeBias_Glonass,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GLONASS

pc_GNSS_RTK_SSR_CodeBias_Gps,                BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GPS

pc_GNSS_RTK_SSR_CodeBias_Gps_L5,             BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GPS L5

pc_GNSS_RTK_SSR_OrbitCorrections_Bds,        BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for BDS

pc_GNSS_RTK_SSR_OrbitCorrections_Galileo,    BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for Galileo

pc_GNSS_RTK_SSR_OrbitCorrections_Glonass,    BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for GLONASS

pc_GNSS_RTK_SSR_OrbitCorrections_Gps,        BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for GPS

pc_GNSS_RefLocSup,                           BOOLEAN,       TRUE    #-- @desc Gnss-ReferenceLocationSupport (Common Assistance Data)

pc_GNSS_RefTimeSup,                          BOOLEAN,       TRUE    #-- @desc Gnss-ReferenceTimeSupport (Common Assistance Data)

pc_GNSS_SSR_GridCorrSupp_Bds,                BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for BDS

pc_GNSS_SSR_GridCorrSupp_Galileo,            BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for Galileo

pc_GNSS_SSR_GridCorrSupp_Glonass,            BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for GLONASS

pc_GNSS_SSR_GridCorrSupp_Gps,                BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for GPS

pc_GNSS_SSR_GridCorrSupp_Qzss,               BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for QZSS

pc_GNSS_SSR_PhaseBias_Bds_B1C,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for BDS B1C

pc_GNSS_SSR_PhaseBias_Bds_B1I,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for BDS B1I

pc_GNSS_SSR_PhaseBias_Galileo_E1,            BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for Galileo E1

pc_GNSS_SSR_PhaseBias_Galileo_E5A,           BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for Galileo E5A

pc_GNSS_SSR_PhaseBias_Glonass,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GLONASS

pc_GNSS_SSR_PhaseBias_Gps_L1CA,              BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GPS L1 C/A

pc_GNSS_SSR_PhaseBias_Gps_L5,                BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GPS L5

pc_GNSS_SSR_PhaseBias_Qzss,                  BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for QZSS

pc_GNSS_SSR_STEC_CorrSupp_Bds,               BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for BDS

pc_GNSS_SSR_STEC_CorrSupp_Galileo,           BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for Galileo

pc_GNSS_SSR_STEC_CorrSupp_Glonass,           BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for GLONASS

pc_GNSS_SSR_STEC_CorrSupp_Gps,               BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for GPS

pc_GNSS_SSR_STEC_CorrSupp_Qzss,              BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for QZSS

pc_GNSS_SSR_URA_Bds,                         BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for BDS

pc_GNSS_SSR_URA_Galileo,                     BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for Galileo

pc_GNSS_SSR_URA_Glonass,                     BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for GLONASS

pc_GNSS_SSR_URA_Gps,                         BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for GPS

pc_GNSS_SSR_URA_Qzss,                        BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for QZSS

pc_GNSS_TimeModSup_BDS,                      BOOLEAN,       TRUE    #-- @desc Gnss-TimeModelsSupport for BDS

pc_GNSS_TimeModSup_Galileo,                  BOOLEAN,       TRUE    #-- @desc Gnss-TimeModelsSupport for Galileo

pc_GNSS_TimeModSup_Glonass,                  BOOLEAN,       TRUE    #-- @desc Gnss-TimeModelsSupport for GLONASS

pc_GNSS_TimeModSup_Gps,                      BOOLEAN,       TRUE    #-- @desc Gnss-TimeModelsSupport for GPS

pc_GNSS_TimeModSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for QZSS

pc_GNSS_TimeModSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for SBAS

pc_GNSS_UTCModSup_BDS,                       BOOLEAN,       TRUE    #-- @desc Gnss-UTC-ModelSupport for BDS (Model-5)

pc_GNSS_UTCModSup_Galileo,                   BOOLEAN,       TRUE    #-- @desc Gnss-UTC-ModelSupport for Galileo (Model-1)

pc_GNSS_UTCModSup_Glonass,                   BOOLEAN,       TRUE    #-- @desc Gnss-UTC-ModelSupport for GLONASS (Model-3)

pc_GNSS_UTCModSup_Gps,                       BOOLEAN,       TRUE    #-- @desc Gnss-UTC-ModelSupport for GPS (Model-1)

pc_GNSS_UTCModSup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for QZSS (Model-1)

pc_GNSS_UTCModSup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for SBAS (Model-4)

pc_GNSS_location_r16,                        BOOLEAN,       TRUE    #-- @desc  UE is equipped with a GNSS or A-GNSS receiver that may be used to provide detailed location information along with SON or MDT related measurements in RRC_CONNECTED RRC_IDLE and RRC_INACTIVE.

pc_HO_from_UTRA_to_eFDD,                     BOOLEAN,       TRUE    #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (FDD)

pc_HO_from_UTRA_to_eTDD,                     BOOLEAN,       TRUE    #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (TDD)

pc_HRPD,                                     BOOLEAN,       false   #-- @desc  UE supports CDMA2000 HRPD band class

pc_HSDPA_FDD,                                BOOLEAN,       TRUE    #-- @desc  UE Supports HSDPA - FDD

pc_HSDPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - TDD

pc_HSDSCH_UE_Category_FDD,                   INTEGER,       10      #-- @desc  FDD HS-DSCH physical layer categories

pc_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  LCR TDD HS-DSCH physical layer categories

pc_HSUPA_FDD,                                BOOLEAN,       TRUE    #-- @desc  UE Supports HSUPA - FDD

pc_HSUPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - TDD

pc_Highspeed_Enh_Prach,                      BOOLEAN,       TRUE    #-- @desc  Support high speed enhancement for random access preambles generated from restricted set type B in high speed scenario as specifed in TS 36.211

pc_HttpDigestAuthentication,                 BOOLEAN,       false   #-- @desc  HTTP Digest XCAP Authentication

pc_HttpGBAAuthentication,                    BOOLEAN,       TRUE    #-- @desc  GBA XCAP Authentication

pc_IMS,                                      BOOLEAN,       false   #-- @desc  Support of IMS

pc_IMSI_Detach,                              BOOLEAN,       TRUE    #-- @desc  Support of detach for non-EPS services

pc_IMS_5GS,                                  BOOLEAN,       false   #-- @desc  Support of IMS

pc_IMS_APN_default,                          BOOLEAN,       TRUE    #-- @desc  Configured with IMS APN as default APN

pc_IMS_Audio_FeatureTag,                     BOOLEAN,       TRUE    #-- @desc  UE supports audio media feature tag

pc_IMS_CS_PS_SRVCC,                          BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC

pc_IMS_CS_PS_SRVCCAlert,                     BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC in alerting state

pc_IMS_CS_PS_SRVCCMidCall,                   BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC and the MSC server assisted mid-call feature

pc_IMS_Deregistration,                       BOOLEAN,       TRUE    #-- @desc  UE has the method that supports IMS deregistration

pc_IMS_Disable_Preconditions,                BOOLEAN,       TRUE    #-- @desc  UE supports disabling preconditions

pc_IMS_E2ae,                                 BOOLEAN,       false   #-- @desc  UE supports end-to-access-edge media security using SDES

pc_IMS_EmergencyCall,                        BOOLEAN,       false   #-- @desc  UE supports IMS emergency services

pc_IMS_ExplicitConsultativeTransfer,         BOOLEAN,       TRUE    #-- @desc  Explicit Communication Transfer - consultative transfer

pc_IMS_GIBA_Sec,                             BOOLEAN,       false   #-- @desc  UE supports GIBA security only

pc_IMS_GRUUsInSIP,                           BOOLEAN,       false   #-- @desc  UE supports obtaining and using GRUUs in the Session Initiation Protocol (SIP)

pc_IMS_Geolocation,                          BOOLEAN,       false   #-- @desc  UE is capable of obtaining location information

pc_IMS_SRVCCAlert,                           BOOLEAN,       TRUE    #-- @desc  UE indicates g.3gpp.srvcc-alerting media feature tag in INVITE request or 180 response

pc_IMS_Sec,                                  BOOLEAN,       TRUE    #-- @desc  UE supports full IMS security

pc_IMS_Session_Timer,                        BOOLEAN,       TRUE    #-- @desc  UE supports Session Timer

pc_IMS_Session_Timer_own_benefit,            BOOLEAN,       TRUE    #-- @desc  UE uses Session Timer for its benefit alone

pc_IMS_Session_Timer_reINVITE,               BOOLEAN,       false   #-- @desc  UE supports usage of re-INVITE for session refresh

pc_IMS_TWS,                                  BOOLEAN,       TRUE    #-- @desc  Three way session

pc_IMS_Video_FeatureTag,                     BOOLEAN,       TRUE    #-- @desc  UE indicates video media feature tag in REGISTER and INVITE request

pc_IMS_after_EmReg_rejection,                BOOLEAN,       TRUE    #-- @desc  UE reattempts IMS emergency service without registration after rejection of emergency registration

pc_IMS_emergency_call,                       BOOLEAN,       false   #-- @desc  Support of MS emergency call

pc_IP_Ping,                                  BOOLEAN,       false   #-- @desc  Support of ICMP or ICMP IPv6

pc_IPv4,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv4 (used IMS PICS as currently not defined in LTE)

pc_IPv4_Link_MTU_Parameter,                  BOOLEAN,       TRUE    #-- @desc  UE supports IPv4 Link MTU parameter

pc_IPv6,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv6 (used IMS PICS as currently not defined in LTE)

pc_ISR,                                      BOOLEAN,       TRUE    #-- @desc  Support of ISR

pc_ImmConnect,                               BOOLEAN,       false   #-- @desc  Immediate connection supported for all circuit switched basic services

pc_IndicateSigcomp,                          BOOLEAN,       false   #-- @desc  Indicate the willingness to receive the responses and requests compressed from initial REGISTER onwards by using the "comp=sigcomp" parameter

pc_InitiateP_CSCFDiscovery_viaDHCPv4,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv4

pc_InitiateP_CSCFDiscovery_viaDHCPv6,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv6

pc_InitiateP_CSCFDiscovery_viaPCO,           BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via PCO

pc_InitiateSession,                          BOOLEAN,       TRUE    #-- @desc  Initiating a session

pc_InitiatesDedicatedPDPContext,             BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate Dedicated PDP Context

pc_InterBand_CA_BetweenFR1_FR2,              BOOLEAN,       TRUE    #-- @desc  Inter-Band CA between FR1 and FR2

pc_InterBand_CA_WithinFR1,                   BOOLEAN,       TRUE    #-- @desc  Inter-Band CA within FR1

pc_InterBand_CA_WithinFR2,                   BOOLEAN,       false   #-- @desc  Inter-Band CA within FR2

pc_InterBand_ENDC_IncludingFR1_FR2,          BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including both FR1 and FR2

pc_InterBand_ENDC_IncludingFR2,              BOOLEAN,       TRUE    #-- @desc  Inter-Band EN-DC including FR2

pc_InterBand_ENDC_WithinFR1,                 BOOLEAN,       TRUE    #-- @desc  Inter-Band EN-DC within FR1

pc_InterBand_NRDC_BetweenFR1_FR2,            BOOLEAN,       TRUE    #-- @desc  Inter-Band EN-DC bewtween FR1 and FR2

pc_InterFreq_ProximityIndication,            BOOLEAN,       TRUE    #-- @desc  Support of Inter Frequency Proximity Indication

pc_InterFreq_RSTD_WithGaps,                  BOOLEAN,       TRUE    #-- @desc Support of inter-frequency RSTD measurements that require measurement gaps

pc_InterFreq_RSTD_withGaps,                  BOOLEAN,       TRUE    #-- @desc Support of inter-frequency RSTD measurements that require measurement gaps

pc_InterRAT_DL_CompressedModeRequired,       BOOLEAN,       TRUE    #-- @desc  UE supports DL DPCH compressed mode

pc_InterRAT_UL_CompressedModeRequired,       BOOLEAN,       TRUE    #-- @desc  UE supports UL DPCH compressed mode

pc_Interactive,                              BOOLEAN,       TRUE    #-- @desc  UE Supports Interactive QoS class

pc_IntraBand_Contiguous_CA_WithinFR1,        BOOLEAN,       TRUE    #-- @desc  Intra-Band Contiguous CA within FR1

pc_IntraBand_Contiguous_CA_WithinFR2,        BOOLEAN,       TRUE    #-- @desc  Intra-Band Contiguous CA within FR2

pc_IntraBand_Contiguous_ENDC,                BOOLEAN,       TRUE    #-- @desc  Intra-Band Contiguous EN-DC

pc_IntraBand_NonContiguous_CA_WithinFR1,     BOOLEAN,       TRUE    #-- @desc  Intra-Band Non-contiguous CA within FR1

pc_IntraBand_NonContiguous_CA_WithinFR2,     BOOLEAN,       TRUE    #-- @desc  Intra-Band Non-contiguous CA within FR2

pc_IntraBand_NonContiguous_ENDC,             BOOLEAN,       TRUE    #-- @desc  Intra-Band Non-Contiguous EN-DC

pc_IntraFreqA3_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of eventA3 for intra-frequency neighbouring cells in normal coverage and CE Mode A

pc_IntraFreqHO_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of intra-frequency handover to target cell in normal coverage and CE Mode A

pc_IntraFreq_ProximityIndication,            BOOLEAN,       TRUE    #-- @desc  Support of Intra Frequency Proximity Indication

pc_KeepEpsBearerParametersAfterNormalDetach, BOOLEAN,       TRUE    #-- @desc  If the UE supports this then the next ATTACH after DETACH shall be done using AT command AT+CGATT=1.

pc_LAP,                                      BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication.

pc_LAP_override,                             BOOLEAN,       false   #-- @desc  Support of Low Access Prioirty Override

pc_LPP,                                      BOOLEAN,       TRUE    #-- @desc LTE Positioning Protocol (LPP)

pc_LPP_MsgSegmentation,                      BOOLEAN,       false   #-- @desc Support of LPP message segmentation

pc_LPP_SendingACK_ProvideCapabilities,       BOOLEAN,       TRUE    #-- @desc Support of sending of acknowledgement request in LPP Provide Capabilities message

pc_LTE_UL_Segmentation,                      BOOLEAN,       false   #-- @desc  Support of RRC message Segmentation in the UL

pc_LocalTimeZone,                            BOOLEAN,       TRUE    #-- @desc  Support of storage of the local time zone

pc_LoggedMeasurementsIdle,                   BOOLEAN,       TRUE    #-- @desc  Support of logged measurements in RRC_IDLE

pc_MBS_AcquisitionAssist,                    BOOLEAN,       false   #-- @desc Support of mbs-AcquisitionAssistance

pc_MBS_AlmanacAssist,                        BOOLEAN,       false   #-- @desc Support of mbs-AlmanacAssistance

pc_MGPS,                                     BOOLEAN,       false   #-- @desc Support for Modernized GPS

pc_MO_PDU_Session_Modification,              BOOLEAN,       TRUE    #-- @desc  Support of UE requested PDU session modification

pc_MTSI_ACR,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Anonymous Communication Rejection

pc_MTSI_CommDivert,                          BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Communication Diversion

pc_MTSI_CommHold,                            BOOLEAN,       TRUE    #-- @desc  Communication Hold

pc_MTSI_CommWaiting,                         BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Communication Waiting

pc_MTSI_Conference,                          BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Conference

pc_MTSI_Incoming_CB,                         BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Incoming Communication Barring

pc_MTSI_MessageWait,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Message Waiting Indication

pc_MTSI_OIP,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Originating Identification Presentation

pc_MTSI_OIR,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Originating Identification Restriction

pc_MTSI_OIR_C,                               BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Originating Identification Restriction - Configuration

pc_MTSI_Outgoing_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Outgoing Communication Barring

pc_MTSI_Speech,                              BOOLEAN,       TRUE    #-- @desc  MTSI media - Speech

pc_MTSI_Speech_AMRWB,                        BOOLEAN,       TRUE    #-- @desc  MTSI media - Speech AMR wideband

pc_MTSI_Speech_EVS,                          BOOLEAN,       TRUE    #-- @desc  MTSI media - Speech EVS

pc_MTSI_TIP,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Terminating Identification Presentation

pc_MTSI_TIR,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Terminating Identification Restriction

pc_MTSI_TIR_C,                               BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Terminating Identification Restriction - Configuration

pc_MTSI_Video,                               BOOLEAN,       TRUE    #-- @desc   MTSI media - Video

pc_MT_LR,                                    BOOLEAN,       TRUE    #-- @desc Support of Mobile Terminated location request

pc_MT_LR_loc_notif,                          BOOLEAN,       TRUE    #-- @desc Support of EPC-MT-LR Location Notification

pc_Manual_CSG_Selection,                     BOOLEAN,       TRUE    #-- @desc  Support of Manual CSG selection

pc_MinimumPeriodicSearchTimer,               BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer

pc_More_Than_128_CAbandComb,                 BOOLEAN,       TRUE    #-- @desc  Support of more than 128 CA Band Combinations

pc_Multi_RTT,                                BOOLEAN,       TRUE    #-- @desc  Support for UE-Assisted Multi-RTT

pc_Multi_RTT_additionalPathsReport,          BOOLEAN,       false   #-- @desc  Support of additionalPathsReport

pc_Multi_RTT_periodicalReporting,            BOOLEAN,       false   #-- @desc  Support of periodicalReporting

pc_MultimediaTelephonyService,               BOOLEAN,       TRUE    #-- @desc  Multimedia telephony service participant

pc_Multiple_Cells_Meas_Ext,                  BOOLEAN,       false   #-- @desc  Support of measurement reporting triggered based on a number of cells

pc_Multiple_PDN,                             BOOLEAN,       TRUE    #-- @desc  Support for multiple PDN connections

pc_NB_User_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of User Plane CIoT in NB-S1 mode

pc_NE_DC,                                    BOOLEAN,       false   #-- @desc  NE-DC (Option 4)

pc_NG102_Call_Combined_Registration_EUTRA,   BOOLEAN,       TRUE    #-- @desc  Voice call after combined Registration E-UTRA

pc_NG102_Call_Combined_Registration_WLAN,    BOOLEAN,       TRUE    #-- @desc  Voice call after combined Registration WLAN

pc_NG102_Combined_Registration_EUTRA,        BOOLEAN,       TRUE    #-- @desc  Combined Registration E-UTRA

pc_NG102_Combined_Registration_WLAN,         BOOLEAN,       TRUE    #-- @desc  Combined Registration WLAN

pc_NG102_Dual_Registration_EUTRA,            BOOLEAN,       false   #-- @desc  Dual Registration E-UTRA

pc_NG114_v1_0,                               BOOLEAN,       TRUE    #-- @desc  Version 1.0 as of 07 August 2020

pc_NG114_v1_0_EVS_A1,                        BOOLEAN,       false   #-- @desc  EVS Configuration A1

pc_NG114_v1_0_EVS_B0,                        BOOLEAN,       false   #-- @desc  EVS Configuration B0

pc_NG114_v1_0_audio,                         BOOLEAN,       TRUE    #-- @desc  audio feature tag

pc_NG114_v1_0_default_config_evs_br,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBr

pc_NG114_v1_0_default_config_evs_bw,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBw

pc_NG114_v1_0_default_config_voice_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for voice exempt

pc_NG114_v1_0_final_SDP_offer,               BOOLEAN,       TRUE    #-- @desc  final codec selection

pc_NG114_v1_0_first_SDP_answer,              BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to initial SDP offer

pc_NG114_v1_0_forking,                       BOOLEAN,       false   #-- @desc  Forking behavior

pc_NG114_v1_0_initial_SDP_offer,             BOOLEAN,       TRUE    #-- @desc  Codecs and attributes in initial SDP offer

pc_NG114_v1_0_mmtel,                         BOOLEAN,       TRUE    #-- @desc  mmtel ICSI value

pc_NG114_v1_0_second_SDP_answer,             BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to second SDP offer

pc_NG114_v1_0_video,                         BOOLEAN,       TRUE    #-- @desc  video feature tag

pc_NG114_v2_0,                               BOOLEAN,       false   #-- @desc  Version 2.0 as of 07 August 2021

pc_NG114_v2_0_default_config_video_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for video exempt

pc_NGEN_DC,                                  BOOLEAN,       false   #-- @desc  NE-DC (Option 7)

pc_NG_RAN_EUTRA,                             BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA (Option 5)

pc_NG_RAN_NR,                                BOOLEAN,       TRUE    #-- @desc  NG-RAN NR (Option 2)

pc_NGeFDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA FDD (Option 5)

pc_NGeTDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA TDD (Option 5)

pc_NMO_I_Behaviour,                          BOOLEAN,       false   #-- @desc  Support of the extended NMO I system information

pc_NR_5GC_EmergencyService_fallback,         BOOLEAN,       TRUE    #-- @desc  Support of emergency services fallback in NR connected to 5GCN

pc_NR_5GC_EmergencyServices,                 BOOLEAN,       false   #-- @desc  Support of emergency services in NR connected to 5GCN

pc_NR_ECID,                                  BOOLEAN,       TRUE    #-- @desc  Support for UE-Assisted NR E-CID

pc_NR_ECID_CSIRsrp,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRP

pc_NR_ECID_CSIRsrq,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRQ

pc_NR_ECID_SSRsrp,                           BOOLEAN,       TRUE    #-- @desc  Support of SS RSRP

pc_NR_ECID_SSRsrq,                           BOOLEAN,       TRUE    #-- @desc  Support of SS RSRQ

pc_NR_ECID_periodicalReporting,              BOOLEAN,       false   #-- @desc  Support of periodicalReporting

pc_NR_ECID_triggeredReporting,               BOOLEAN,       false   #-- @desc  Support of triggeredReporting

pc_NR_RRC_Release_With_Deprioritisation,     BOOLEAN,       TRUE    #-- @desc  Support of  RRC connection release with deprioritisation

pc_NR_UL_SRS_Capability,                     BOOLEAN,       false   #-- @desc  Support for NR UL-SRS-Capability

pc_NR_UL_Segmentation,                       BOOLEAN,       TRUE    #-- @desc  Support of RRC message Segmentation in the UL

pc_NR_ehc_r16,                               BOOLEAN,       false   #-- @desc  Support EHC (Ethernet header compression)

pc_Navic_DGNSS_Sup,                          BOOLEAN,       false   #-- @desc Navic-DifferentialCorrectionsSupport-r16 for

pc_Navic_GridModelSupp,                      BOOLEAN,       false   #-- @desc Navic-GridModelSupport-r16

pc_No_USIM_TestExecution,                    BOOLEAN,       TRUE    #-- @desc  Support of test execution with no USIM

pc_NonIP_Link_MTU_Parameter,                 BOOLEAN,       false   #-- @desc  UE supports Non-IP Link MTU parameter

pc_OMA_LPPe,                                 BOOLEAN,       TRUE    #-- @desc Support for OMA LPPe

pc_OTDOA,                                    BOOLEAN,       TRUE    #-- @desc Support of UE assisted OTDOA

pc_OTDOA_additionalNeighbourCellInfoList,    BOOLEAN,       false   #-- @desc Support of additionalNeighbourCellInfoList

pc_OTDOA_additionalPathsReport,              BOOLEAN,       false   #-- @desc Support of additionalPathsReport

pc_OTDOA_additional_prs_config,              BOOLEAN,       false   #-- @desc Support of additional-prs-config

pc_OTDOA_densePrsConfig,                     BOOLEAN,       false   #-- @desc Support of densePrsConfig

pc_OTDOA_idleStateForMeasurements,           BOOLEAN,       false   #-- @desc Support of idleStateForMeasurements

pc_OTDOA_interFreqRSTDmeasurement,           BOOLEAN,       TRUE    #-- @desc Support of interFreqRSTDmeasurement

pc_OTDOA_interRAT_RSTDmeasurement,           BOOLEAN,       false   #-- @desc Support of interRAT-RSTDmeasurement

pc_OTDOA_maxSupportedPrsBandwidth,           BOOLEAN,       false   #-- @desc Support of maxSupportedPrsBandwidth

pc_OTDOA_maxSupportedPrsBandwidth_r14,       ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsBandwidth_r14,n6      #-- @desc  maxSupportedPrsBandwidth

pc_OTDOA_maxSupportedPrsConfigs,             BOOLEAN,       false   #-- @desc Support of maxSupportedPrsConfigs

pc_OTDOA_maxSupportedPrsConfigs_r14,         ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsConfigs_r14,c2      #-- @desc  maxSupportedPrsConfigs

pc_OTDOA_motionMeasurements,                 BOOLEAN,       false   #-- @desc Support of motionMeasurements

pc_OTDOA_multiPrbNprs,                       BOOLEAN,       false   #-- @desc Support of multiPrbNprs

pc_OTDOA_numberOfRXantennas,                 BOOLEAN,       false   #-- @desc Support of numberOfRXantennas

pc_OTDOA_numberOfRXantennas_r14,             ENUM-OTDOA_ProvideCapabilities.numberOfRXantennas_r14,rx1     #-- @desc  Support of numberOfRXantennas

pc_OTDOA_periodicalReporting,                BOOLEAN,       false   #-- @desc Support of periodicalReporting

pc_OTDOA_prsFrequencyHopping,                BOOLEAN,       false   #-- @desc Support of prsFrequencyHopping

pc_OTDOA_prsOccGroup,                        BOOLEAN,       false   #-- @desc Support of prsOccGroup

pc_OTDOA_prs_based_tbs,                      BOOLEAN,       false   #-- @desc Support of prs-based-tbs

pc_OTDOA_prs_id,                             BOOLEAN,       false   #-- @desc Support of prs-id

pc_OTDOA_tp_separation_via_muting,           BOOLEAN,       false   #-- @desc Support of tp-separation-via-muting

pc_P2X_UE,                                   BOOLEAN,       false   #-- @desc  Support of V2X communicatin as Pedestrian UE

pc_PDCP_Delay_r16,                           BOOLEAN,       TRUE    #-- @desc  UE supports UL PDCP Packet Average Delay measurement and reporting in RRC_CONNECTED state

pc_PDCP_PktDelay,                            BOOLEAN,       TRUE    #-- @desc  Support for PDCP Packet Delay per QCI

pc_PLMN_EF_LRPLMNSI_Automatic_Mode_Exception,BOOLEAN,       TRUE    #-- @desc  Support of Automatic Mode EF_LRPLMSI PLMN Selection Expression

pc_PLMN_Manual_Mode_Exception,               BOOLEAN,       TRUE    #-- @desc  Support of Manual Mode PLMN Selection Expression

pc_PPI_Support,                              BOOLEAN,       TRUE    #-- @desc  Support of Power Preference Indication

pc_PRS_ProcessingSymbolsInEveryTms,          ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSymbolsInEveryTms_r16,n8      #-- @desc  PRS-ProcessingSymbolsInEveryTms for at least one NR band

pc_PS,                                       BOOLEAN,       TRUE    #-- @desc  Packet Switched

pc_PS_data_centric,                          BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS data centric

pc_PS_data_off,                              BOOLEAN,       false   #-- @desc  UE supports PS data off

pc_PS_voice_centric,                         BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS voice centric

pc_PUSCH_Ehn_MMTEL,                          BOOLEAN,       false   #-- @desc  Support of PUSCH enhancement for MMTEL voice and video enhancements mode

pc_PWS_UpperLayer,                           BOOLEAN,       TRUE    #-- @desc  Presence of PWS upper layer for functions like duplicate definition

pc_P_CSCFDiscovery_viaDHCPv4,                BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF discovery via DHCPv4

pc_P_CSCFDiscovery_viaDHCPv6,                BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF discovery via DHCPv6

pc_P_CSCFDiscovery_viaPCO,                   BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF Discovery via PCO

pc_ParamGpsAssisData,                        BOOLEAN,       TRUE    #-- @desc Support of MO-LR request for assistance data

pc_ParamPosEstimate,                         BOOLEAN,       TRUE    #-- @desc Support of MO-LR request for a position estimate

pc_Preconditions,                            BOOLEAN,       TRUE    #-- @desc  Integration of resource management and SIP? (use of preconditions)

pc_ProvideDST_inUse,                         BOOLEAN,       TRUE    #-- @desc  UE supports a mechanism to provide daylight saving time

pc_Provide_IMS_APN,                          BOOLEAN,       false   #-- @desc  Configured to provide IMS APN during initial attach

pc_Provide_IMS_as_second_APN,                BOOLEAN,       false   #-- @desc  Configured to provide IMS APN as the 2nd PDN connection

pc_Provide_Internet_as_second_APN,           BOOLEAN,       false   #-- @desc  Configured to provide Internet APN as the 2nd PDN connection

pc_QZSS_ADR,                                 BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Qzss

pc_QZSS_ADR_ENH,                             BOOLEAN,       false   #-- @desc Support of ADR enhancements for Qzss

pc_QZSS_HA,                                  BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Qzss

pc_QZSS_QZS_L1,                              BOOLEAN,       false   #-- @desc Support of QZS-L1 signal in QZSS

pc_QZSS_QZS_L1C,                             BOOLEAN,       false   #-- @desc Support of QZS-L1C signal in QZSS

pc_QZSS_QZS_L2C,                             BOOLEAN,       false   #-- @desc Support of QZS-L2C signal in QZSS

pc_QZSS_QZS_L5,                              BOOLEAN,       false   #-- @desc Support of QZS-L5 signal in QZSS

pc_QZSS_VelocityMeas,                        BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Qzss

pc_RLF_ReportForInterRAT_MRO,                BOOLEAN,       TRUE    #-- @desc  Support of Radio Link Failure Report for InterRAT MRO

pc_ROHC_profile0x0001,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0001

pc_ROHC_profile0x0002,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0002

pc_ROHC_profile0x0003,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0003

pc_ROHC_profile0x0004,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0004

pc_ROHC_profile0x0006,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0006

pc_ROHC_profile0x0101,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0101

pc_ROHC_profile0x0102,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0102

pc_ROHC_profile0x0103,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0103

pc_ROHC_profile0x0104,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0104

pc_RSRP_MeasFR1,                             BOOLEAN,       TRUE    #-- @desc  Support of RSRP-MeasFR1

pc_RSRP_MeasFR2,                             BOOLEAN,       false   #-- @desc  Support of RSRP-MeasFR2

pc_RS_SINR_MeasEUTRA,                        BOOLEAN,       TRUE    #-- @desc  Support of E-UTRA RS-SINR measurements

pc_Rach_Report,                              BOOLEAN,       TRUE    #-- @desc  Support of delivery of rachReport upon request from the network

pc_Re_Attach_AfterDetachColl,                BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach

pc_RequestIPv4HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv4 address of the Home Agent during Attach procedure

pc_RequestIPv6HAAddress_DuringAttach,        BOOLEAN,       TRUE    #-- @desc  Support for being configured to request the IPv6 address of the Home Agent during Attach procedure

pc_SBAS_ADR,                                 BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Sbas

pc_SBAS_ADR_ENH,                             BOOLEAN,       false   #-- @desc Support of ADR enhancements for Sbas

pc_SBAS_HA,                                  BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Sbas

pc_SBAS_VelocityMeas,                        BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Sbas

pc_SCPTM,                                    BOOLEAN,       false   #-- @desc  The UE supports SC-PTM

pc_SFTD_MeasNR_Cell_FDD,                     BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR neighbour cell in FDD

pc_SFTD_MeasNR_Cell_TDD,                     BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR neighbour cell in TDD

pc_SFTD_MeasNR_Neigh_FDD,                    BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR neighbour cell in FDD

pc_SFTD_MeasNR_Neigh_TDD,                    BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR neighbour cell in TDD

pc_SFTD_MeasPSCell_MRDC_FDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR PSCell

pc_SFTD_MeasPSCell_MRDC_TDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR PSCell

pc_SFTD_MeasPSCell_NRDC_FDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR PSCell in FDD

pc_SFTD_MeasPSCell_NRDC_TDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR PSCell in TDD

pc_SIP_Based_UserConfiguration,              BOOLEAN,       TRUE    #-- @desc  SIP based user configuration

pc_SIP_Digest,                               BOOLEAN,       false   #-- @desc  SIP Digest without TLS

pc_SI_Neighbour_UMTS_Autonomous_Gaps,        BOOLEAN,       TRUE    #-- @desc  Upon configuration of si-RequestForHO by the network supports acquistion of relevant information from a neighbouring UMTS cell by reading the SI of the neighbouring cell using autonomous gaps and reporting

pc_SI_Neighbour_interFreq_Autonomous_Gaps,   BOOLEAN,       TRUE    #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intrer-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting

pc_SI_Neighbour_intraFreq_Autonomous_Gaps,   BOOLEAN,       TRUE    #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intra-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting

pc_SMS_IP_MO,                                BOOLEAN,       TRUE    #-- @desc  UE supports SM-over-IP sender

pc_SMS_IP_MT,                                BOOLEAN,       TRUE    #-- @desc  UE supports SM-over-IP receiver

pc_SMS_SGs,                                  BOOLEAN,       TRUE    #-- @desc  The UE supports SMS over SGs and is configured for SMS over SGs.  If true at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. If it is set to true pc_combined_attach shall be set to true

pc_SMS_SGs_MO,                               BOOLEAN,       TRUE    #-- @desc  Support of Short Message Service (SMS) MO over SGs

pc_SMS_SGs_MT,                               BOOLEAN,       TRUE    #-- @desc  Support of Short Message Service (SMS) MT over SGs

pc_SMS_SGs_Multi_MO,                         BOOLEAN,       TRUE    #-- @desc  Support of sending concatenated multiple short message over SGs

pc_SM_PDU_DN_RequestContainer,               BOOLEAN,       false   #-- @desc  The UE includes the SM PDU DN request container IE in the PDU Session Establishment Request message

pc_SNPN,                                     BOOLEAN,       false   #-- @desc  Support of Stand-alone Non-Public Network

pc_SOR_ACKNotReqLocalRel,                    BOOLEAN,       false   #-- @desc  Support of UE local release when the security check is successful but SOR Transparent container indicates ACK has been NOT requested

pc_SRS_switching,                            BOOLEAN,       false   #-- @desc  Support of SRS switching between a band pair

pc_SRVCC_GERAN_UTRAN,                        BOOLEAN,       TRUE    #-- @desc  Support for SRVCC from E-UTRAN to GERANUTRAN

pc_Semi_Persistence_Scheduling,              BOOLEAN,       TRUE    #-- @desc  Support of semi persistance scheduling

pc_Sens,                                     BOOLEAN,       false   #-- @desc Support for UE-Assisted Sensor

pc_Set_UE_Cap_Info_NR,                       BOOLEAN,       false   #-- @desc  Support of test function SET UL MESSAGE for using a preconfigured UE capability container over NR

pc_ShortNameNetwork,                         BOOLEAN,       false   #-- @desc  Support of storage of the network short name

pc_Speech,                                   BOOLEAN,       TRUE    #-- @desc  UE supports Speech

pc_Squal_based_CellReselection_between_E_UTRAN_and_GERAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to E-UTRAN from GERAN

pc_Squal_based_CellReselection_to_E_UTRAN_from_UTRAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to E-UTRAN from UTRAN

pc_Squal_based_CellReselection_to_UTRAN_from_E_UTRAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to UTRAN from E-UTRAN

pc_StandaloneGNSS_Location,                  BOOLEAN,       TRUE    #-- @desc  Support of standalone GNSS receiver to provide detailed location information in RRC measurement report and logged measurements in RRC_IDLE

pc_Streaming,                                BOOLEAN,       TRUE    #-- @desc  UE Supports Streaming QoS class

pc_SupportOpModeA,                           BOOLEAN,       TRUE    #-- @desc  UE supports Operation Mode A

pc_SwitchOnOff,                              BOOLEAN,       TRUE    #-- @desc  switch onoff supported

pc_T3412Extended,                            BOOLEAN,       TRUE    #-- @desc  Support of T3412 extended value IE

pc_TAU_connected_in_IMS,                     BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TAU_idle_in_IMS,                          BOOLEAN,       TRUE    #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TDD_HCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_LCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_SpecialSubframe,                      BOOLEAN,       TRUE    #-- @desc  Support of TDD special subframe

pc_TDD_VHCR,                                 BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_band_UE_PC2,                          BOOLEAN,       TRUE    #-- @desc  Support of TDD Bands 38 40 41 and 42 Power class 2 operation

pc_TTI_Bundling,                             BOOLEAN,       TRUE    #-- @desc  Support of TTI Bundling

pc_TestModeforCSGproximity,                  BOOLEAN,       false   #-- @desc  Support of UE radio bearer test mode for CSG proximity testing

pc_TransferEmergencyPDUN1toS1noN26,          BOOLEAN,       TRUE    #-- @desc  Support of Emergency PDU session transfer from N1 mode to S1 mode when network does not support N26 interface

pc_TransferEmergencyPDUS1toN1noN26,          BOOLEAN,       TRUE    #-- @desc  Support of Emergency PDN connection transfer from S1 mode to N1 mode when network does not support N26 interface

pc_UDC,                                      BOOLEAN,       false   #-- @desc  Support of the uplink data compression operation

pc_UDC_SIP,                                  BOOLEAN,       false   #-- @desc  Support of UL data compression with SIP static dictionary

pc_UEA_AGNSS,                                BOOLEAN,       TRUE    #-- @desc Support of UE assisted Assisted-GNSS

pc_UEA_A_GANSS,                              BOOLEAN,       TRUE    #-- @desc Support of UE-Assisted A-GANSS

pc_UEA_DL_AoD,                               BOOLEAN,       TRUE    #-- @desc  Support for UE-Assisted DL-AoD

pc_UEA_DL_TDOA,                              BOOLEAN,       TRUE    #-- @desc  Support for UE-Assisted DL-TDOA

pc_UEA_MBS,                                  BOOLEAN,       false   #-- @desc Support for UE-Assisted MBS

pc_UEB_AGNSS,                                BOOLEAN,       TRUE    #-- @desc Support of UE based Assisted-GNSS

pc_UEB_A_GANSS,                              BOOLEAN,       TRUE    #-- @desc Support of UE-Based A-GANSS

pc_UEB_DL_AoD,                               BOOLEAN,       false   #-- @desc  Support for UE-Based DL-AoD

pc_UEB_DL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Based DL-TDOA

pc_UEB_MBS,                                  BOOLEAN,       false   #-- @desc Support for UE-Based MBS

pc_UEB_Sens,                                 BOOLEAN,       false   #-- @desc Support for UE-Based Sensor

pc_UEB_WLAN,                                 BOOLEAN,       false   #-- @desc Support for UE-Based WLAN

pc_UE_NoRegIMS_IMSVoPS_0,                    BOOLEAN,       TRUE    #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to '0'

pc_UE_NoReqIMS_IMSVoPS_0,                    BOOLEAN,       TRUE    #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to 0

pc_UE_supports_user_initiated_PDN_disconnect,BOOLEAN,       TRUE    #-- @desc  UE supports user initiated PDN disconnect

pc_UL_256QAM,                                BOOLEAN,       TRUE    #-- @desc  Support of uplink 256 QAM

pc_UL_64QAM,                                 BOOLEAN,       TRUE    #-- @desc  Support of uplink 64 QAM

pc_UL_CA,                                    BOOLEAN,       TRUE    #-- @desc  Support of UL CA

pc_UL_CA_2Carriers,                          BOOLEAN,       TRUE    #-- @desc  UL CA with 2 carriers

pc_UL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 3 carriers

pc_UL_CoMP,                                  BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation

pc_UL_IntraBand_ContCaBWclassB,              BOOLEAN,       TRUE    #-- @desc  UL Intra-band contiguous CA BW class B

pc_UL_IntraBand_ContCaBWclassC,              BOOLEAN,       TRUE    #-- @desc  UL Intra-band contiguous CA BW class C

pc_UL_MIMO,                                  BOOLEAN,       false   #-- @desc  Support of UL MIMO

pc_UL_NR_CA_2CC,                             BOOLEAN,       TRUE    #-- @desc  UL NR CA with 2 carriers

pc_UL_NR_CA_3CC,                             BOOLEAN,       false   #-- @desc  UL NR CA with 3 carriers

pc_UL_SupportedInAllBandsInCAComb,           BOOLEAN,       TRUE    #-- @desc  UL (Pcell) supported in each band of Inter-band CA combination under test

pc_UL_interBand_CaAA,                        BOOLEAN,       TRUE    #-- @desc  Support of UL inter-band CA _ A-A

pc_UL_interBand_CaBwClassComb_AA,            BOOLEAN,       TRUE    #-- @desc  UL Inter-band contiguous CA BW class A-A

pc_UL_intraBand_contCaTypeB,                 BOOLEAN,       TRUE    #-- @desc  UL Intra-band contiguous CA Type B

pc_UL_intraBand_contCaTypeC,                 BOOLEAN,       TRUE    #-- @desc  UL Intra-band contiguous CA Type C

pc_UL_intraBand_nonContCaAA,                 BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA _ A-A

pc_UL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       TRUE    #-- @desc  Support of UL intra-band non-contiguous CA BW Class Combination A-A

pc_UMI_ProcNeeded_DuringCSFB,                BOOLEAN,       TRUE    #-- @desc  Requiring UMI proceeding to paging response

pc_USIM_Removal,                             BOOLEAN,       TRUE    #-- @desc  USIM removable without power down supported

pc_USSI,                                     BOOLEAN,       TRUE    #-- @desc  USSI

pc_UTRA,                                     BOOLEAN,       TRUE    #-- @desc  UE supports UTRA

pc_UTRAN_ANR,                                BOOLEAN,       false   #-- @desc  Support of UTRAN ANR

pc_UTRAN_ProximityIndication,                BOOLEAN,       TRUE    #-- @desc  Support of UTRAN Proximity Indication

pc_UTRA_CompressedModeRequired,              BOOLEAN,       TRUE    #-- @desc  Support of Compressed Mode

pc_UTRA_FeatrGrp_1,                          BOOLEAN,       TRUE    #-- @desc  Support of UTRA CELL_PCH and URA_PCH to RRC_IDLE cell reselection

pc_UTRA_FeatrGrp_2,                          BOOLEAN,       TRUE    #-- @desc  Support of EUTRAN measurements and reporting in connected mode

pc_UTRA_FeatrGrp_3,                          BOOLEAN,       TRUE    #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for high priority layers

pc_UTRA_FeatrGrp_4,                          BOOLEAN,       TRUE    #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for all layers

pc_UeAssistedAgps,                           BOOLEAN,       TRUE    #-- @desc  Support of UE assisted Network Assisted GPS L1 CA

pc_UeBasedAgps,                              BOOLEAN,       TRUE    #-- @desc  Support of UE based Network Assisted GPS L1 CA

pc_UniversalAndLocalTimeZone,                BOOLEAN,       TRUE    #-- @desc  Support of storage of the universal time and local time zone

pc_UpdateUE_LocationInformation,             BOOLEAN,       TRUE    #-- @desc  Update UE Location Information

pc_Use_QCI_66,                               BOOLEAN,       TRUE    #-- @desc  The UE supports a bearer with QCI 66

pc_Use_SMS_over_IP,                          BOOLEAN,       TRUE    #-- @desc  The UE is configured to use SMS over IP

pc_UserInitiatedPLMN_Reselection,            BOOLEAN,       TRUE    #-- @desc  Support user initiated PLMN reselection in automatic mode

pc_UserInitiated_SNPN_Reselection,           BOOLEAN,       false   #-- @desc  Support of autonomous search function to detect CAG cells on serving and non-serving frequencies

pc_User_Plane_CIoT_Optimisation,             BOOLEAN,       false   #-- @desc  Support of User Plane CIoT

pc_VideoCodecH264CBP,                        BOOLEAN,       TRUE    #-- @desc  MTSI media - Video codec H.264 CBP Level 1.2

pc_VideoCodecH264CBPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CBP Level 3.1

pc_VideoCodecH264CHPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CHP Level 3.1

pc_VideoCodecH265Lv31,                       BOOLEAN,       false   #-- @desc  Reference: 34.229-2 Table A.1511

pc_VoLTE,                                    BOOLEAN,       TRUE    #-- @desc  Support of VoLTE in GSMA PRD IR.92: "IMS profile for Voice and SMS"

pc_WLAN,                                     BOOLEAN,       false   #-- @desc Support for UE-Assisted WLAN

pc_WLAN_APId,                                BOOLEAN,       false   #-- @desc Support of wlan-AP-Identifier

pc_WLAN_APLocinfo,                           BOOLEAN,       false   #-- @desc Support of wlan-AP-Location

pc_WLAN_IMS_EmergencyCall,                   BOOLEAN,       false   #-- @desc  UE supports IMS emergency call over WLAN

pc_WLAN_Meas_Imm_MDT,                        BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in Immediate MDT

pc_WLAN_Meas_logged_MDT,                     BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in logged MDT

pc_WLAN_XCAP_without_PDN,                    BOOLEAN,       false   #-- @desc  If PICS is true Wi-Fi access without PDN connection applies.  Otherwise EPC-integrated WLAN applies

pc_WLAN_voice,                               BOOLEAN,       false   #-- @desc  Support for IR.51

pc_XCAP_UsernameIsConfiguredInUE,            BOOLEAN,       TRUE    #-- @desc  UE indicated OMA-TS-XDM_MO-V1_1-20080627-A.doc section 5.2.8 "Node: <X>AAUTHNAME" is configured

pc_XCAP_XUIisDefaultPublicUserId,            BOOLEAN,       TRUE    #-- @desc  UE uses the default public user id received in P-Associated-URI header in 200 OK for REGISTER as XCAP User Identity (XUI)

pc_XCAP_only_APN,                            BOOLEAN,       TRUE    #-- @desc  Configured with an APN for XCAP only usage

pc_XCAP_over_Internet_APN,                   BOOLEAN,       TRUE    #-- @desc  Configured to use Internet APN for XCAP signalling

pc_ZUC,                                      BOOLEAN,       TRUE    #-- @desc  Support of ZUC algorithm

pc_am_WithShortSN,                           BOOLEAN,       TRUE    #-- @desc  Support RLC AM with 12 bit length of RLC sequence number

pc_as_ReflectiveQoS,                         BOOLEAN,       TRUE    #-- @desc  Support of reflective QoS

pc_barometer_r16,                            BOOLEAN,       false   #-- @desc  UE supports uncompensated barometric pressure measurement reporting upon request from the network.

pc_bwp_SameNumerology_upto2,                 BOOLEAN,       TRUE    #-- @desc  Support of BWP adaptation (up to 2 BWPs) with the same numerology

pc_bwp_SameNumerology_upto4,                 BOOLEAN,       TRUE    #-- @desc  Support of BWP adaptation (up to 4 BWPs) with the same numerology

pc_bwp_SwitchingDelay_Type1,                 BOOLEAN,       TRUE    #-- @desc  Supports DCI and timer based active BWP switching delay type1

pc_bwp_SwitchingDelay_Type2,                 BOOLEAN,       TRUE    #-- @desc  Supports DCI and timer based active BWP switching delay type2

pc_bwp_WithoutRestriction,                   BOOLEAN,       false   #-- @desc  Support of BWP operation without bandwidth restriction

pc_ce_HARQ_AckBundling,                      BOOLEAN,       TRUE    #-- @desc  Support of HARQ-ACK bundling

pc_ce_PUSCH_NB_MaxTBS,                       BOOLEAN,       false   #-- @desc  Support of ce-PUSCH-NB-MaxTBS-r14

pc_condHandoverFailure_r16,                  BOOLEAN,       TRUE    #-- @desc  Support conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover

pc_condHandoverTwoTriggerEvents_r16,         BOOLEAN,       TRUE    #-- @desc  Support 2 trigger events for same execution condition of conditional handover

pc_condHandover_r16,                         BOOLEAN,       TRUE    #-- @desc  Support conditional handover

pc_condPSCellChange_r16,                     BOOLEAN,       false   #-- @desc  Support conditional PSCell change

pc_configuredUL_GrantType1,                  BOOLEAN,       TRUE    #-- @desc  Support Type 1 PUSCH transmissions with configured grant

pc_configuredUL_GrantType2,                  BOOLEAN,       TRUE    #-- @desc  Support Type 2 PUSCH transmissions with configured grant

pc_csi_RSRP_AndRSRQ_MeasWithSSB,             BOOLEAN,       false   #-- @desc  Support CSI-RSRP and CSI-RSRQ measurement where CSI-RS resource is configured with an associated SSPBCH

pc_csi_RSRP_AndRSRQ_MeasWithoutSSB,          BOOLEAN,       false   #-- @desc  Support CSI-RSRP and CSI-RSRQ measurement where CSI-RS resource is configured without an associated SSPBCH

pc_csi_RS_CFRA_ForHO,                        BOOLEAN,       false   #-- @desc  Support handover using a contention free random access on PRACH resources that are associated with CSI-RS resources of the target cell

pc_dataInactMon,                             BOOLEAN,       false   #-- @desc  Support of data inactivity monitoring

pc_data_centric,                             BOOLEAN,       false   #-- @desc  Support of UEs usage setting as data centric

pc_dci_DL_PriorityIndicator_r16,             BOOLEAN,       false   #-- @desc  Supports the priority indicator field configured in DCI formats 1_1 and 1_2 in a BWP when configured to monitor both DCI formats 1_1 and 1_2 in the BWP.

pc_dci_Format1_2And0_2_r16,                  BOOLEAN,       false   #-- @desc  Support monitoring DCI format 1_2 for DL scheduling and monitoring DCI format 0_2 for UL scheduling

pc_dci_UL_PriorityIndicator_r16,             BOOLEAN,       false   #-- @desc  Supports the priority indicator field configured in DCI formats 0_1 and 0_2 in a BWP when configured to monitor both DCI formats 0_1 and 0_2 in the BWP

pc_dl_PRS_BufferType,                        ENUM-PRS_ProcessingCapabilityPerBand_r16.dl_PRS_BufferType_r16,type1   #-- @desc  dl-PRS-BufferType for at least one NR band

pc_dl_RSTD_MeasurementPerPairOfTRP_FR1,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR1

pc_dl_RSTD_MeasurementPerPairOfTRP_FR2,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR2

pc_downlinkSPS,                              BOOLEAN,       TRUE    #-- @desc  Support PDSCH reception based on semi-persistent scheduling

pc_downlink_LAA,                             BOOLEAN,       TRUE    #-- @desc  Supports downlink LAA operation

pc_durationOfPRS_ProcessingSymbols,          ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSysmbols_r16,nDot125 #-- @desc  durationOfPRS-ProcessingSymbols for at least one NR band

pc_dynamicPowerSharing,                      BOOLEAN,       TRUE    #-- @desc  UE supports 5GS Core

pc_dynamicSwitchRA_Type0_1_PDSCH,            BOOLEAN,       TRUE    #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PDSCH

pc_dynamicSwitchRA_Type0_1_PUSCH,            BOOLEAN,       TRUE    #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PUSCH

pc_dynamicSwitch_SUL,                        BOOLEAN,       TRUE    #-- @desc  Support supplemental uplink with dynamic switch (DCI based selection of PUSCH carrier)

pc_eAttachWithIMSI,                          BOOLEAN,       TRUE    #-- @desc  Support of Attach With IMSI

pc_eBand10_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 10

pc_eBand11_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 11

pc_eBand12_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 12

pc_eBand13_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 13

pc_eBand14_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 14

pc_eBand17_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 17

pc_eBand18_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 18

pc_eBand19_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 19

pc_eBand1_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 1

pc_eBand20_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 20

pc_eBand21_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 21

pc_eBand22_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 22

pc_eBand23_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 23

pc_eBand24_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 24

pc_eBand25_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 25

pc_eBand26_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 26

pc_eBand27_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 27

pc_eBand28_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 28

pc_eBand29_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 29

pc_eBand2_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 2

pc_eBand30_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 30

pc_eBand31_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 31

pc_eBand32_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 32

pc_eBand33_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 33

pc_eBand34_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 34

pc_eBand35_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 35

pc_eBand36_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 36

pc_eBand37_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 37

pc_eBand38_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 38

pc_eBand39_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 39

pc_eBand3_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 3

pc_eBand40_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 40

pc_eBand41_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 41

pc_eBand42_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 42

pc_eBand43_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 43

pc_eBand44_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 44

pc_eBand45_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 45

pc_eBand46_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 46

pc_eBand47_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 47

pc_eBand48_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 48

pc_eBand4_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 4

pc_eBand53_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 53

pc_eBand5_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 5

pc_eBand65_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 65

pc_eBand66_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 66

pc_eBand68_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 68

pc_eBand69_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 69

pc_eBand6_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 6

pc_eBand70_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 70

pc_eBand71_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 71

pc_eBand72_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 72

pc_eBand73_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 73

pc_eBand74_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 74

pc_eBand7_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 7

pc_eBand85_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 85

pc_eBand87_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 87

pc_eBand88_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 88

pc_eBand8_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 8

pc_eBand9_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 9

pc_eCall_Test_Call,                          BOOLEAN,       false   #-- @desc  Capability to trigger a Test eCall

pc_eCall_automatic_Initiated,                BOOLEAN,       false   #-- @desc  Capability to initiate Automatic eCall

pc_eCall_manual_Initiated,                   BOOLEAN,       false   #-- @desc  Capability to initiate a Manual eCall

pc_eFDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA FDD

pc_eFDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA FDD bands

pc_eHARQ_Pattern_for_TTI_bundling,           BOOLEAN,       TRUE    #-- @desc  Support of enhanced HARQ pattern for TTI bundling operation for FDD

pc_eIMTA_TDD,                                BOOLEAN,       false   #-- @desc  Support of TDD ULDL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD Pcell

pc_eMBMS,                                    BOOLEAN,       TRUE    #-- @desc  Support of eMBMS

pc_eMBMS_SC,                                 BOOLEAN,       TRUE    #-- @desc  Support of eMBMS service continuity

pc_eMinimumPeriodicSearchTimer,              BOOLEAN,       TRUE    #-- @desc  Support of Minimum Periodic Search Timer

pc_ePDCCH,                                   BOOLEAN,       false   #-- @desc  Support of ePDCCH

pc_ePSM,                                     BOOLEAN,       false   #-- @desc  Support of Power Saving Mode (in EUTRA)

pc_eRedirectionUTRA,                         BOOLEAN,       TRUE    #-- @desc  Support of use of the UTRA system information provided by RRCConnectionRelease upon redirection

pc_eTDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA TDD

pc_eTDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA TDD bands

pc_eWLAN,                                    BOOLEAN,       false   #-- @desc  WLAN

pc_edrx,                                     BOOLEAN,       false   #-- @desc  Support of extended DRX

pc_eutra_CGI_Reporting,                      BOOLEAN,       TRUE    #-- @desc  Support acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the EN-DC is not configured.

pc_eutra_EPC_HO_ToNR_FDD_FR1_r15,            BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover to NR FR1 FDD from EUTRA connected to EPC

pc_eutra_EPC_HO_ToNR_TDD_FR1_r15,            BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover to NR FR1 TDD from EUTRA connected to EPC

pc_eutra_EPC_HO_ToNR_TDD_FR2_r15,            BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover to NR FR2 TDD from EUTRA connected to EPC

pc_eventA_MeasAndReport,                     BOOLEAN,       TRUE    #-- @desc  Support NR measurements and events A triggered reporting

pc_eventB_MeasAndReport,                     BOOLEAN,       TRUE    #-- @desc  Support inter-RAT EUTRA measurements and events B triggered reporting

pc_extendedLongDRX,                          BOOLEAN,       false   #-- @desc  Support of extended Long DRX cycle

pc_fixed_broadband_XCAP,                     BOOLEAN,       false   #-- @desc  The UE uses XCAP in fixed broadband access

pc_freqBandPriorityAdjustment,               BOOLEAN,       TRUE    #-- @desc  Support of prioritization of the frequency bands in multiBandInfoList over the band in freqBandIndicator as defined by freqBandIndicatorPriority-r12

pc_gnss_heightMeas,                          BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement

pc_gp10_en_dc,                               BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 10 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp10_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 10 configured by NR RRC

pc_gp11_en_dc,                               BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 1 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp11_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 11 configured by NR RRC

pc_gp12_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 12 configured by NR RRC

pc_gp15_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 15 configured by NR RRC

pc_gp16_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 16 configured by NR RRC

pc_gp17_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 17 configured by NR RRC

pc_gp18_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 18 configured by NR RRC

pc_gp19_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 19 configured by NR RRC

pc_gp20_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 20 configured by NR RRC

pc_gp21_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 21 configured by NR RRC

pc_gp22_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 22 configured by NR RRC

pc_gp23_nr,                                  BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 23 configured by NR RRC

pc_gp2_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 2 configured by NR RRC

pc_gp3_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 3 configured by NR RRC

pc_gp4_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 4 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp4_nr,                                   BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 4 configured by NR RRC

pc_gp5_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 5 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp5_nr,                                   BOOLEAN,       TRUE    #-- @desc  Support measurement gap pattern 5 configured by NR RRC

pc_gp6_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 6 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp6_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 6 configured by NR RRC

pc_gp7_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 7 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp7_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 7 configured by NR RRC

pc_gp8_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 8 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp8_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 8 configured by NR RRC

pc_gp9_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 9 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC

pc_gp9_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 9 configured by NR RRC

pc_handoverInterF,                           BOOLEAN,       TRUE    #-- @desc  Support inter-frequency Handover from the corresponding duplex mode or from the corresponding frequency range

pc_heightMeas,                               BOOLEAN,       false   #-- @desc  Support of height-based measurement reporting

pc_immMeasWLAN_r16,                          BOOLEAN,       false   #-- @desc  UE supports WLAN measurements in RRC_CONNECTED state

pc_inactiveState,                            BOOLEAN,       TRUE    #-- @desc  Support of RRC_INACTIVE as specified in TS 38.331

pc_independentGapConfig,                     BOOLEAN,       TRUE    #-- @desc  Support two independent measurement gap configurations for FR1 and FR2

pc_interFreqDAPS_r16,                        BOOLEAN,       TRUE    #-- @desc  Support inter-frequency DAPS handover

pc_interRAT_EUTRA_Handover,                  BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover to EUTRA connected to EPC

pc_interRAT_NR_ToENDC,                       BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover from NR to EN-DC

pc_interRAT_eLTE_Handover,                   BOOLEAN,       TRUE    #-- @desc  Support inter-RAT Handover to EUTRA connected to 5GC

pc_interleavingVRB_ToPRB_PDSCH,              BOOLEAN,       TRUE    #-- @desc  Support receiving PDSCH with interleved VRB-to-PRB mapping

pc_intraAndInterF_MeasAndReport,             BOOLEAN,       TRUE    #-- @desc  Support NR intra-freq and inter-freq measurements and at least periodical reporting

pc_intraFreqDAPS_r16,                        BOOLEAN,       TRUE    #-- @desc  Support intra-frequency DAPS handover

pc_intraFreq_CE_NeedForGaps,                 BOOLEAN,       false   #-- @desc  Require intra-frequency measurement gaps for operating in CE Mode A or CE Mode B

pc_lch_ToGrantPriorityRestriction_r16,       BOOLEAN,       false   #-- @desc  Supports restricting data transmission from a given LCH to a configured (sub-) set of dynamic grant priority levels

pc_loggedMeasWLAN_r16,                       BOOLEAN,       false   #-- @desc  Support of WLAN measurements in RRC_IDLE and RRC_INACTIVE state

pc_loggedMeasurements_r16,                   BOOLEAN,       false   #-- @desc  UE supports logged measurements in RRC_IDLE and RRC_INACTIVE. A UE that supports logged measurements shall support both periodical logging and event-triggered logging. The memory size of MDT logged   measurements is 64KB.

pc_logicalChannelSR_DelayTimer,              BOOLEAN,       TRUE    #-- @desc  Supports the logicalChannelSR-DelayTimer

pc_longDRX_Cycle,                            BOOLEAN,       TRUE    #-- @desc  Support long DRX cycle

pc_maxDL_PRS_RSRP_MeasurementFR1,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR1

pc_maxDL_PRS_RSRP_MeasurementFR2,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR2

pc_maxNrOfDL_PRS_ResourceSetPerTrpPerFrequencyLayer,INTEGER,       1       #-- @desc  maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr1,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr1_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr1

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr2,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr2_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr2

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_Only_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-Only

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr2_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr2_Only_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr2-Only

pc_maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer,ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer for at least one NR band

pc_maxNrOfDL_PRS_ResourcesPerResourceSet,    ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerResourceSet_r16,n1      #-- @desc  maxNrOfDL-PRS-ResourcesPerResourceSet for at least one NR band

pc_maxNrOfPosLayer,                          INTEGER,       1       #-- @desc  maxNrOfPosLayer

pc_maxNrOfRx_TX_MeasFR1,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR1

pc_maxNrOfRx_TX_MeasFR2,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR2

pc_maxNrOfTRP_AcrossFreqs,                   ENUM-NR_DL_PRS_ResourcesCapability_r16.maxNrOfTRP_AcrossFreqs_r16,n4      #-- @desc  maxNrOfTRP-AcrossFreqs

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS120,ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs120_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 120kHz SCS for at least one NR band

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS15, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs15_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 15kHz SCS for at least one NR band

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS30, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs30_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 30kHz SCS for at least one NR band

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS60, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs60_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 60kHz SCS for at least one NR band

pc_maxNumberAP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberAP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberAP-SRS-PosResourcesPerBWP

pc_maxNumberMIMO_LayersPDSCH,                BOOLEAN,       TRUE    #-- @desc  UEs supporting 5GS and The maximum number of spatial multiplexing layer(s) supported by the UE for DL reception. For single CC standalone NR it is mandatory with capability signaling to support at least 4 MIMO layers in the bands where 4Rx is specified as mandatory for the given UE and at least 2 MIMO layers in FR2. If absent the UE doesn't support MIMO on this carrier

pc_maxNumberPathLossEstimatePerServing,      ENUM-OLPC_SRS_Pos_r16.maxNumberPathLossEstimatePerServing_r16,n1      #-- @desc  maxNumberPathLossEstimatePerServing for at least one NR band

pc_maxNumberPeriodicSRS_PosResourcesPerBWP,  ENUM-SRS_PosResourcesPerBand_r16.maxNumberPeriodicSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberPeriodicSRS-PosResourcesPerBWP

pc_maxNumberSP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSP-SRS-PosResourcesPerBWP

pc_maxNumberSRS_PosPathLossEstimateAllServingCells,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosPathLossEstimateAllServingCells_r16,n1      #-- @desc  maxNumberSRS-PosPathLossEstimateAllServingCells

pc_maxNumberSRS_PosResourceSetsPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourceSetsPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourceSetsPerBWP

pc_maxNumberSRS_PosResourcesPerBWP,          ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourcesPerBWP

pc_maxNumberSRS_PosSpatialRelationsAllServingCell,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosSpatialRelationsAllServingCells_r16,n0      #-- @desc  maxNumberSRS-PosSpatialRelationsAllServingCells

pc_maxNumberSearchSpaces,                    BOOLEAN,       TRUE    #-- @desc  UE supports maxNumberSearchSpaces

pc_maxSupportedFreqLayers,                   INTEGER,       1       #-- @desc  maxSupportedFreqLayers-r16

pc_multipleTimingAdvance,                    BOOLEAN,       TRUE    #-- @desc  Support of multiple timing advances

pc_multipleUplinkSPS,                        BOOLEAN,       false   #-- @desc  Support of multiple uplink SPS and reporting SPS assistance information

pc_nas_ReflectiveQoS,                        BOOLEAN,       TRUE    #-- @desc  Support of NAS reflective QoS

pc_noOf_PDNsNewConnection,                   INTEGER,       0       #-- @desc  Number of UE requested PDN connection establishments after ATTACH in a new signaling connection

pc_noOf_PDNsSameConnection,                  INTEGER,       0       #-- @desc  Number of UE requested PDN connection establishments after ATTACH during the same signaling connection

pc_noOf_PDUs,                                INTEGER,       1       #-- @desc  Number of UE requested PDU session establishments after REGISTRATION

pc_noOf_PDUsNewConnection,                   INTEGER,       1       #-- @desc  Number of UE-requested PDU session establishments after REGISTRATION in a new signaling connection

pc_noOf_PDUsSameConnection,                  INTEGER,       0       #-- @desc  Number of UE requested PDU session establishments after REGISTRATION during the same signaling connection

pc_nrBand12_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 12

pc_nrBand14_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 14

pc_nrBand18_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 18

pc_nrBand1_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 1

pc_nrBand20_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 20

pc_nrBand24_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 24

pc_nrBand257_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 257

pc_nrBand258_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 258

pc_nrBand259_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 259

pc_nrBand25_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 25

pc_nrBand260_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 260

pc_nrBand261_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 261

pc_nrBand26_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 26

pc_nrBand28_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 28

pc_nrBand29_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 29

pc_nrBand2_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 2

pc_nrBand30_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 30

pc_nrBand34_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 34

pc_nrBand38_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 38

pc_nrBand39_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 39

pc_nrBand3_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 3

pc_nrBand40_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 40

pc_nrBand41_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 41

pc_nrBand46_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 46

pc_nrBand48_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 48

pc_nrBand50_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 50

pc_nrBand51_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 51

pc_nrBand53_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 53

pc_nrBand5_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 5

pc_nrBand65_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 65

pc_nrBand66_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 66

pc_nrBand70_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 70

pc_nrBand71_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 70

pc_nrBand74_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 74

pc_nrBand75_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 75

pc_nrBand76_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 76

pc_nrBand77_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 77

pc_nrBand78_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 78

pc_nrBand79_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 79

pc_nrBand7_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 7

pc_nrBand80_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 80

pc_nrBand81_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 81

pc_nrBand82_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 82

pc_nrBand83_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 83

pc_nrBand84_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 84

pc_nrBand86_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 86

pc_nrBand89_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 89

pc_nrBand8_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 8

pc_nrBand90_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 90

pc_nrBand91_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 91

pc_nrBand92_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 92

pc_nrBand93_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 93

pc_nrBand94_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 94

pc_nrBand95_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 95

pc_nrBand96_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 96

pc_nrBand97_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 97

pc_nrBand99_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 99

pc_nrFDD,                                    BOOLEAN,       TRUE    #-- @desc  NR FDD (Option 2)

pc_nrFDD_MultiBand,                          BOOLEAN,       TRUE    #-- @desc  Support of multiple NR FDD bands

pc_nrFR1,                                    BOOLEAN,       TRUE    #-- @desc  Support of frequency range FR1

pc_nrFR2,                                    BOOLEAN,       TRUE    #-- @desc  Support of frequency range FR2

pc_nrMIMO_CB_PUSCH,                          BOOLEAN,       TRUE    #-- @desc  Supports more than one MIMO layer at the UE for PUSCH transmission with codebook precoding

pc_nrMIMO_NonCB_PUSCH,                       BOOLEAN,       false   #-- @desc  Supports more than one MIMO layer at the UE for PUSCH transmission with non-codebook precoding

pc_nrSDL,                                    BOOLEAN,       false   #-- @desc  Support of NR SDL

pc_nrSDL_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR SDL bands

pc_nrSUL,                                    BOOLEAN,       false   #-- @desc  Support of NR SUL

pc_nrSUL_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR SUL bands

pc_nrTDD,                                    BOOLEAN,       TRUE    #-- @desc  NR TDD (Option 2)

pc_nrTDD_MultiBand,                          BOOLEAN,       TRUE    #-- @desc  Support of multiple NR TDD bands

pc_nr_CGI_Reporting,                         BOOLEAN,       TRUE    #-- @desc  Support acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when EN-DC is not configured

pc_nr_CGI_Reporting_NPN_r16,                 BOOLEAN,       false   #-- @desc  Support of acquisition of CGI related information from a neighbouring intra-frequency or inter-frequency NPN CAG cell

pc_olpc_SRS_PosBasedOnPRS_Neigh,             BOOLEAN,       TRUE    #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Neigh for at least one NR band

pc_olpc_SRS_PosBasedOnPRS_Serving,           BOOLEAN,       TRUE    #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Serving for at least one NR band

pc_olpc_SRS_PosBasedOnSSB_Neigh,             BOOLEAN,       TRUE    #-- @desc  Support of olpc-SRS-PosBasedOnSSB-Neigh for at least one NR band

pc_orientation_r16,                          BOOLEAN,       false   #-- @desc  UE supports orientation information reporting upon request from the network.

pc_outOfOrderDelivery,                       BOOLEAN,       TRUE    #-- @desc  Supports Out of order delivery of data to upper layers by PDCP

pc_pdcp_DuplicationMCG_OrSCG_DRB,            BOOLEAN,       TRUE    #-- @desc  Support CA-based PDCP duplication over MCG or SCG DRB

pc_pdcp_DuplicationMoreThanTwoRLC_r16,       BOOLEAN,       false   #-- @desc  Support PDCP duplication with more than two RLC entities

pc_pdcp_DuplicationSplitDRB,                 BOOLEAN,       TRUE    #-- @desc  Support PDCP duplication with more than two RLC entities

pc_pdcp_DuplicationSplitSRB,                 BOOLEAN,       TRUE    #-- @desc  Support PDCP duplication over split SRB12

pc_pdsch_256QAM_FR1,                         BOOLEAN,       TRUE    #-- @desc  Support 256QAM for PDSCH for FR1

pc_pdsch_256QAM_FR2,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PDSCH for FR2

pc_pdsch_Mapping_TypeA,                      BOOLEAN,       TRUE    #-- @desc  support receiving PDSCH using PDSCH mapping type A with less than seven symbols

pc_pdsch_Mapping_TypeB,                      BOOLEAN,       TRUE    #-- @desc  support receiving PDSCH using PDSCH mapping type B with less than seven symbols

pc_pdsch_RepetitionMultiSlots,               BOOLEAN,       TRUE    #-- @desc  Support PDSCH Reception when configured with higher layer parameter aggregationFactorDL>1

pc_periodicEUTRA_MeasAndReport,              BOOLEAN,       false   #-- @desc  Supports periodic EUTRA measurement and reporting.

pc_prs_FromServNeighCellAsQCL,               BOOLEAN,       false   #-- @desc  Support of prs-FromServNeighCellAsQCL for at least one NR band

pc_pusch_256QAM_FR1,                         BOOLEAN,       TRUE    #-- @desc  Support 256QAM for PUSCH for FR1

pc_pusch_256QAM_FR2,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PUSCH for at least one NR FR2 band

pc_pusch_RepetitionMultiSlots,               BOOLEAN,       TRUE    #-- @desc  Supports transmitting PUSCH scheduled by DCI format 0_0 or 0_1 when configured with higher layer parameter aggregationFactorUL > 1

pc_qci1Indication_inRLF,                     BOOLEAN,       TRUE    #-- @desc  Support of QCI1 indication in Radio Link Failure Report

pc_qoe_MTSI_MeasReport,                      BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for MTSI Service

pc_qoe_MeasReport,                           BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for Streaming Service

pc_ra_Type0_PUSCH,                           BOOLEAN,       TRUE    #-- @desc  Support resource allocation Type 0 for PUSCH

pc_rachReport_r16,                           BOOLEAN,       false   #-- @desc  Support of rachReport

pc_recommendedBitRate,                       BOOLEAN,       false   #-- @desc  Supports the bit rate recommendation message from the gNB to the UE as specified in TS 38.321

pc_recommendedBitRateQuery,                  BOOLEAN,       false   #-- @desc  Supports the bit rate recommendation query message from the UE to the gNB as specified in TS 38.321

pc_reducedCP_Latency,                        BOOLEAN,       false   #-- @desc  Support reduced control plane latency as defined in TS 38.331

pc_releasePreference_r16,                    BOOLEAN,       false   #-- @desc  Support of release preference assistance information

pc_reqFreqBands,                             BOOLEAN,       TRUE    #-- @desc  Support of reception of requested Frequency Bands

pc_rssiAndChannelOccupancyReporting,         BOOLEAN,       TRUE    #-- @desc  Supports measurement and reporting for RSSI and channel occupancy

pc_scalingFactor0dot75,                      BOOLEAN,       TRUE    #-- @desc  Support scaling factor 0.75 is applied to the band in the max data rate calculation

pc_scptm_NonServingCell,                     BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on a cell that may be additionally configured as an Scell

pc_scptm_SCell,                              BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on configured SCell

pc_shortDRX_Cycle,                           BOOLEAN,       TRUE    #-- @desc  Support short DRX cycle

pc_shortSN,                                  BOOLEAN,       TRUE    #-- @desc  Support 12 bit length of PDCP sequence number

pc_shortSPS_intervalFDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in FDD mode

pc_shortSPS_intervalTDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in TDD mode

pc_simulLTE_NR_PRS,                          BOOLEAN,       false   #-- @desc  Support of simulLTE-NR-PRS

pc_simul_NR_DL_AoD_DL_TDOA,                  BOOLEAN,       TRUE    #-- @desc  Support of simul-NR-DL-AoD-DL-TDOA for at least one NR band

pc_simul_NR_DL_AoD_Multi_RTT,                BOOLEAN,       TRUE    #-- @desc  Support of simul-NR-DL-AoD-Multi-RTT for at least one NR band

pc_skipUplinkDynamic,                        BOOLEAN,       false   #-- @desc  Support of skipping UL transmissions if no data is available

pc_skipUplinkSPS,                            BOOLEAN,       false   #-- @desc  Support of skipping SPS UL transmissions if no data is available

pc_skipUplinkTxDynamic,                      BOOLEAN,       false   #-- @desc  Support skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission

pc_sms_over_NAS,                             BOOLEAN,       TRUE    #-- @desc  Support of SMS over NAS

pc_spatialBundlingHARQ_ACK,                  BOOLEAN,       TRUE    #-- @desc  Supports spatial bundling of HARQ-ACK bits carried on PUCCH or PUSCH per PUCCH group.  With spatial bundling 2 HARQ-ACK bits for a DL MIMO data is bundled into a single bit by logical AND operation

pc_spatialRelation_SRS_PosBasedOnCSI_RS_Serving,BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnCSI-RS-Serving for at least one NR band

pc_spatialRelation_SRS_PosBasedOnPRS_Neigh,  BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Neigh for at least one NR band

pc_spatialRelation_SRS_PosBasedOnPRS_Serving,BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Serving for at least one NR band

pc_spatialRelation_SRS_PosBasedOnSRS,        BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnSRS for at least one NR band

pc_spatialRelation_SRS_PosBasedOnSSB_Neigh,  BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Neigh for at least one NR band

pc_spatialRelation_SRS_PosBasedOnSSB_Serving,BOOLEAN,       TRUE    #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Serving for at least one NR band

pc_speed_r16,                                BOOLEAN,       false   #-- @desc  UE supports speed information reporting upon request from the network.

pc_splitDRB_withUL_Both_MCG_SCG,             BOOLEAN,       TRUE    #-- @desc  Support UL transmission via both MCG path and SCG path for the split DRB

pc_splitSRB_WithOneUL_Path,                  BOOLEAN,       TRUE    #-- @desc  Support UL transmission via either MCG path or SCG path for the split SRB

pc_srb3,                                     BOOLEAN,       TRUE    #-- @desc  Support direct SRB between the SN and the UE

pc_srs_AssocPRS_MultiLayersFR1,              BOOLEAN,       TRUE    #-- @desc  Support of srs-AssocPRS-MultiLayersFR1

pc_srs_AssocPRS_MultiLayersFR2,              BOOLEAN,       false   #-- @desc  Support of srs-AssocPRS-MultiLayersFR2

pc_ss_CCH_Interference_Handling,             BOOLEAN,       false   #-- @desc  Support of Synchronisation signal and common channel interference handling

pc_ss_SINR_Meas,                             BOOLEAN,       TRUE    #-- @desc  Support SS-SINR measurements

pc_ss_rsrp_SINR,                             BOOLEAN,       false   #-- @desc UE supports rsrp SINR

pc_ssb_FromNeighCellAsQCL,                   BOOLEAN,       false   #-- @desc  Support of ssb-FromNeighCellAsQCL for at least one NR band

pc_supportedBandwidthPRS_FR1,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr1,mhz5    #-- @desc  supportedBandwidthPRS in FR1 for at least one NR band

pc_supportedBandwidthPRS_FR2,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr2,mhz50   #-- @desc  supportedBandwidthPRS in FR2 for at least one NR band

pc_tdd_FDD_CA_FDD_PCell,                     BOOLEAN,       TRUE    #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the second bit setting to 1

pc_tdd_FDD_CA_TDD_PCell,                     BOOLEAN,       TRUE    #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the first bit setting to 1

pc_twoStepScheduling_uplink_LAA,             BOOLEAN,       false   #-- @desc  Supports two step uplink scheduling using PUSCH trigger A and PUSCH trigger B

pc_ue_CategoryDL_0,                          BOOLEAN,       false   #-- @desc  UE Category DL 0

pc_ue_CategoryDL_10,                         BOOLEAN,       false   #-- @desc  UE Category DL 10

pc_ue_CategoryDL_11,                         BOOLEAN,       false   #-- @desc  UE Category DL 11

pc_ue_CategoryDL_12,                         BOOLEAN,       TRUE    #-- @desc  UE Category DL 12

pc_ue_CategoryDL_13,                         BOOLEAN,       false   #-- @desc  UE Category DL 13

pc_ue_CategoryDL_14,                         BOOLEAN,       false   #-- @desc  UE Category DL 14

pc_ue_CategoryDL_15,                         BOOLEAN,       false   #-- @desc  UE Category DL 15

pc_ue_CategoryDL_16,                         BOOLEAN,       TRUE    #-- @desc  UE Category DL 16

pc_ue_CategoryDL_17,                         BOOLEAN,       false   #-- @desc  UE Category DL 17

pc_ue_CategoryDL_18,                         BOOLEAN,       TRUE    #-- @desc  UE Category DL 18

pc_ue_CategoryDL_19,                         BOOLEAN,       false   #-- @desc  UE Category DL 19

pc_ue_CategoryDL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category UL 1bis and Category 1 UE

pc_ue_CategoryDL_20,                         BOOLEAN,       false   #-- @desc  UE Category DL 20

pc_ue_CategoryDL_21,                         BOOLEAN,       false   #-- @desc  UE Category DL 21

pc_ue_CategoryDL_22,                         BOOLEAN,       false   #-- @desc  UE Category DL 22

pc_ue_CategoryDL_23,                         BOOLEAN,       false   #-- @desc  UE Category DL 23

pc_ue_CategoryDL_24,                         BOOLEAN,       false   #-- @desc  UE Category DL 24

pc_ue_CategoryDL_25,                         BOOLEAN,       false   #-- @desc  UE Category DL 25

pc_ue_CategoryDL_26,                         BOOLEAN,       false   #-- @desc  UE Category DL 26

pc_ue_CategoryDL_4,                          BOOLEAN,       false   #-- @desc  UE Category DL 4

pc_ue_CategoryDL_6,                          BOOLEAN,       false   #-- @desc  UE Category DL 6

pc_ue_CategoryDL_7,                          BOOLEAN,       false   #-- @desc  UE Category DL 7

pc_ue_CategoryDL_9,                          BOOLEAN,       false   #-- @desc  UE Category DL 9

pc_ue_CategoryDL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M0

pc_ue_CategoryDL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M2

pc_ue_CategoryUL_0,                          BOOLEAN,       false   #-- @desc  UE Category UL 0

pc_ue_CategoryUL_13,                         BOOLEAN,       TRUE    #-- @desc  UE Category UL 13

pc_ue_CategoryUL_14,                         BOOLEAN,       false   #-- @desc  UE Category UL 14

pc_ue_CategoryUL_15,                         BOOLEAN,       false   #-- @desc  UE Category UL 15

pc_ue_CategoryUL_16,                         BOOLEAN,       false   #-- @desc  UE Category UL 16

pc_ue_CategoryUL_17,                         BOOLEAN,       false   #-- @desc  UE Category UL 17

pc_ue_CategoryUL_18,                         BOOLEAN,       TRUE    #-- @desc  UE Category UL 18

pc_ue_CategoryUL_19,                         BOOLEAN,       false   #-- @desc  UE Category UL 19

pc_ue_CategoryUL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category DL 1bis

pc_ue_CategoryUL_20,                         BOOLEAN,       false   #-- @desc  UE Category UL 20

pc_ue_CategoryUL_21,                         BOOLEAN,       false   #-- @desc  UE Category UL 21

pc_ue_CategoryUL_22,                         BOOLEAN,       false   #-- @desc  UE Category UL 22

pc_ue_CategoryUL_23,                         BOOLEAN,       false   #-- @desc  UE Category UL 23

pc_ue_CategoryUL_24,                         BOOLEAN,       false   #-- @desc  UE Category UL 24

pc_ue_CategoryUL_25,                         BOOLEAN,       false   #-- @desc  UE Category UL 25

pc_ue_CategoryUL_26,                         BOOLEAN,       false   #-- @desc  UE Category UL 26

pc_ue_CategoryUL_3,                          BOOLEAN,       false   #-- @desc  UE Category UL 3

pc_ue_CategoryUL_5,                          BOOLEAN,       false   #-- @desc  UE Category UL 5

pc_ue_CategoryUL_7,                          BOOLEAN,       false   #-- @desc  UE Category UL 7

pc_ue_CategoryUL_8,                          BOOLEAN,       false   #-- @desc  UE Category UL 8

pc_ue_CategoryUL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M1

pc_ue_CategoryUL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M2

pc_ue_Category_1,                            BOOLEAN,       false   #-- @desc  UE Category 1

pc_ue_Category_10,                           BOOLEAN,       TRUE    #-- @desc  UE Category 10

pc_ue_Category_11,                           BOOLEAN,       false   #-- @desc  UE Category 11

pc_ue_Category_12,                           BOOLEAN,       TRUE    #-- @desc  UE Category 12

pc_ue_Category_2,                            BOOLEAN,       false   #-- @desc  UE Category 2

pc_ue_Category_3,                            BOOLEAN,       false   #-- @desc  UE Category 3

pc_ue_Category_4,                            BOOLEAN,       TRUE    #-- @desc  UE Category 4

pc_ue_Category_5,                            BOOLEAN,       false   #-- @desc  UE Category 5

pc_ue_Category_6,                            BOOLEAN,       false   #-- @desc  UE Category 6

pc_ue_Category_7,                            BOOLEAN,       TRUE    #-- @desc  UE Category 7

pc_ue_Category_8,                            BOOLEAN,       false   #-- @desc  UE Category 8

pc_ue_Category_9,                            BOOLEAN,       false   #-- @desc  UE Category 9

pc_um_WithLongSN,                            BOOLEAN,       TRUE    #-- @desc  Support RLC UM with 12 bit length of RLC sequence number

pc_um_WithShortSN,                           BOOLEAN,       TRUE    #-- @desc  Support RLC UM with 6 bit length of RLC sequence number

pc_uplink_LAA,                               BOOLEAN,       false   #-- @desc  Supports uplink LAA operation

pc_v2xPartialSensing,                        BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using UE autonomous resource selection mode with partial sensing

pc_voiceFallbackIndication,                  BOOLEAN,       TRUE    #-- @desc  Support of voiceFallbackIndication

pc_voiceOverNR,                              BOOLEAN,       false   #-- @desc  Support IMS voice over NR

pc_voice_PS_1_CS_2,                          BOOLEAN,       TRUE    #-- @desc  Configured voice domain preference

pc_wakeUpSignal,                             BOOLEAN,       false   #-- @desc  Support of Wake Up Signal

px_AccessPointName,                          OCTETSTRING,   08696E7465726E6574 #-- @desc  Access Point Name

px_AquireGNSS_MaxTime,                       INTEGER,       60      #-- @desc  The maximume time (in seconds) taken for the UE to acquire GNSS and derive UTC time (and normally position) and then start to transit or receive as appropriate

px_AttachTypeTested,                         ENUM-EUTRA_ATTACH_TESTED_Type,COMBINED_ATTACH #-- @desc  Attach Type to be tested if UE supports both pc_Attach and pc_Combined_Attach

px_AuthAMF,                                  BITSTRING,     1001000100010001 #-- @desc  Authentication Management Field (16 bits). The value shall be different from '1111 1111 1111 111'B (AMFresynch).

px_AuthK,                                    BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  Authentication Key

px_BcapDataCompression,                      BITSTRING,     0       #-- @desc  Data compression supported (used in the Bearer Capability).Default value: Default IMSI

px_BcapFNUR,                                 BITSTRING,     00001   #-- @desc  Fixed Network User rate supported: 00001B: FNUR 9.6 kbits 00010B: FNUR 14.4 kbits 00011B: FNUR 19.2 kbits 00100B: FNUR 28.8 kbits 00101B: FNUR 38.4 kbits 00110B: FNUR 48.0 kbits 00111B: FNUR 56.0 kbits 01000B: FNUR 64.0 kbits 01001B: FNUR 33.6 kbits 01010B: FNUR 32.0 kbits.

px_CipherAlg,                                BITSTRING,     010     #-- Anritsu TTCN CR required px_CipherAlg type @desc  NAS Ciphering Algorithm Default value: (GEA2)

px_CipherKey,                                BITSTRING,     0101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher Key

px_CipherKey128,                             BITSTRING,     01011110010010101011001101011000100100010011011101011101001010100101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher key (128 bits) to be used e.g. for A54 and GEA4

px_DelayBeforeIntraCellHO,                   INTEGER,       300     #-- @desc  Temporary PIXIT used to define the delay before an intra cell handover

px_DigestPasswordForXCAP,                    CHARSTRING,    XCAP-Password #-- @desc  XCAP password

px_ENDC_BandCombination,                     ENUM-ENDC_BandCombination_Type,DC_3A_n78A #-- @desc  Band combination for EN-DC test cases

px_ENDC_CA_BandCombination,                  ENUM-ENDC_CA_BandCombination_Type,DC_1A_n28A_n78A #-- @desc  EN-DC CA Band Combination

px_ENDC_SecondaryBandCombination,            ENUM-ENDC_BandCombination_Type,DC_3A_n41A #-- @desc  Secondary band combination for EN-DC test cases

px_EUTRA_CA_BandCombination,                 ENUM-CA_BandCombination_Type,CA_1C   #-- @desc  CA band combination applied in CA test cases

px_EUTRA_DC_BandCombination,                 ENUM-DC_BandCombination_Type,DC_1A_3A #-- @desc  DC band combination applied in DC test cases

px_EllipsoidPointWithAltitude,               OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value to be provided in Update UE location information (see 36.509 cl 6.12)

px_EmergencyCallNumber,                      CHARSTRING,    112     #-- @desc  Emergency Number used by UE to initiate an emergency call

px_FDD_OperationBand,                        INTEGER,       1       #-- @desc  The operation band under test as defined in 34.108 clause 5.1.1. Value 1 means Band 1 2 means Band 2 etc.This pixit shall be set in synchronisation with the values that are being set to 6 other Pixits viz: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid

px_FRESH,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  no default value can be proposed

px_GPRS_CipheringAlgorithm,                  ENUM-GPRS_CipheringAlgorithm_Type,gea2    #-- @desc  NAS Ciphering Algorithm Default value: (GEA2)

px_GeoInfo,                                  OCTETSTRING,   9032B9D66360B600323C3C006544 #-- @desc Geographical information to be sent as Location Estimate in FACILITY message from the System Simulator.

px_GnssScenario2012,                         BOOLEAN,       false   #-- @desc  Usage of GNSS scenarios with date in 2012 from 3GPP TS 37.571-5

px_HorizontalVelocity,                       OCTETSTRING,   123456  #-- @desc  Horizontal Velocity to be provided in Update UE location information (see 36.509 cl 6.12)

px_IMEISV_Def,                               HEXSTRING,     3586880000001578 #-- @desc  Default IMEISV value.  No default can be proposed as this is a manufacturer defined value

px_IMEI_Def,                                 HEXSTRING,     358688000000158 #-- @desc  Default IMEI value transmitted by UE.  Digit 15 shall be set as a Spare Digit i.e. shall be set to '0' (see TS 23.003)

px_IMSI_Def,                                 HEXSTRING,     001010000000333 #-- @desc  Default IMSI

px_IMS_AssociatedTelUri,                     CHARSTRING,    tel:+4989364072 #-- @desc  Set as record 3 in EFIMPU as defined in TS 34.229-1[5]

px_IMS_CalleeContactUri,                     CHARSTRING,    sip:12345@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeContactUri2,                    CHARSTRING,    sip:User-C-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeUri,                            CHARSTRING,    sip:12345@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CalleeUri2,                           CHARSTRING,    sip:67890@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CiphAlgo_Def,                         ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ciphering Algorithm

px_IMS_HomeDomainName,                       CHARSTRING,    test.3gpp.com #-- @desc  Home Domain Name.

px_IMS_HomeDomainName_Refreshed,             CHARSTRING,    refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_IPSecAlgorithm,                       ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Integrity Algorithm

px_IMS_MessageAccountIdentity,               CHARSTRING,    testaccountidentity #-- @desc  message accout identity configured at the UE as used for subscription to message-summary event package

px_IMS_Private_UserId,                       CHARSTRING,    001010123456789@test.3gpp.com #-- @desc  Private User Identity.When usingan ISIM this is set to the same value as EFIMPI.When ISIM is not used just USIM the private user identity is derived from px_IMSI.

px_IMS_Private_UserId_Refreshed,             CHARSTRING,    privateuser@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity1,                  CHARSTRING,    sip:001010123456789@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  Public User Identity. It is set to the same value as the first record in EFIMPU.

px_IMS_PublicUserIdentity1_Refreshed,        CHARSTRING,    sip:PublicId1@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity2,                  CHARSTRING,    sip:+11234567890@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the second record in EFIMPU.

px_IMS_PublicUserIdentity3,                  CHARSTRING,    sip:user@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the third record in EFIMPU.

px_IMS_SPI_ValidValueList_PDN1,              CHARSTRING,    256,258,264,266 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN1; each value shall be greater than or equal to 256

px_IMS_SPI_ValidValueList_PDN2,              CHARSTRING,    260,262,268,270 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN2; each value shall be greater than or equal to 256

px_IP_MTU_Size,                              INTEGER,       1300    #-- @desc  MTU size. This value is specific to the SS.

px_IPv4_Address,                             CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address

px_IPv4_Address1_NW,                         CHARSTRING,    192.168.0.3 #-- @desc  IPv4 Gateway Address in PDN1

px_IPv4_Address1_RemoteUE,                   CHARSTRING,    192.168.0.6 #-- @desc  IPv4 Address of remote UE connected to PDN1

px_IPv4_Address1_UE,                         CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address connected to PDN1

px_IPv4_Address2,                            CHARSTRING,    192.168.1.2 #-- @desc  2nd IPv4 Address @sic R5s110011 sic@

px_IPv4_Address2_NW,                         CHARSTRING,    192.168.1.4 #-- @desc  IPv4 Gateway Address in PDN2

px_IPv4_Address2_RemoteUE,                   CHARSTRING,    192.168.1.6 #-- @desc  IPv4 Address of remote UE connected to PDN2

px_IPv4_Address2_UE,                         CHARSTRING,    192.168.1.2 #-- @desc  IPv4 Address connected to PDN2

px_IPv4_Address2a_UE,                        CHARSTRING,    192.168.1.3 #-- @desc  IPv4 Address connected to PDN2a

px_IPv4_Address3_NW,                         CHARSTRING,    192.168.1.8 #-- @desc  IPv4 Gateway Address in PDN3

px_IPv4_Address3_RemoteUE,                   CHARSTRING,    192.168.1.9 #-- @desc  IPv4 Address of remote UE connected to PDN3

px_IPv4_Address3_UE,                         CHARSTRING,    192.168.1.7 #-- @desc  IPv4 Address connected to PDN3

px_IPv4_Address4_NW,                         CHARSTRING,    192.168.2.1 #-- @desc  IPv4 Gateway Address in PDN4

px_IPv4_Address4_UE,                         CHARSTRING,    192.168.2.2 #-- @desc  IPv4 Address connected to PDN4

px_IPv4_Address5_NW,                         CHARSTRING,    192.168.2.3 #-- @desc  IPv4 Gateway Address in PDN5

px_IPv4_Address5_UE,                         CHARSTRING,    192.168.2.4 #-- @desc  IPv4 Address connected to PDN5

px_IPv4_Address6_NW,                         CHARSTRING,    192.168.2.5 #-- @desc  IPv4 Gateway Address in PDN6

px_IPv4_Address6_UE,                         CHARSTRING,    192.168.2.6 #-- @desc  IPv4 Address connected to PDN6

px_IPv4_Address_HomeAgent,                   CHARSTRING,    192.168.0.5 #-- @desc  IPv4 Home Address Agent

px_IPv4_Address_Other,                       CHARSTRING,    192.168.0.8 #-- @desc  Other IPv4 Address

px_IPv6_Address,                             CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address

px_IPv6_Address1_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 Gateway Address in PDN1

px_IPv6_Address1_RemoteUE,                   CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN1

px_IPv6_Address1_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address in PDN1

px_IPv6_Address2,                            CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  2nd IPv6 Address  @sic R5s110011 sic@

px_IPv6_Address2_NW,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:4444 #-- @desc  IPv6 Gateway Address in PDN2

px_IPv6_Address2_RemoteUE,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN2

px_IPv6_Address2_UE,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  IPv6 Address in PDN2

px_IPv6_Address2a_UE,                        CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Address in PDN2a

px_IPv6_Address3_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:8888 #-- @desc  IPv6 Gateway Address in PDN3

px_IPv6_Address3_RemoteUE,                   CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:9999 #-- @desc  IPv6 Address of remote UE in PDN3

px_IPv6_Address3_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:7777 #-- @desc  IPv6 Address in PDN3

px_IPv6_Address4_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:1111 #-- @desc  IPv6 Gateway Address in PDN4

px_IPv6_Address4_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:2222 #-- @desc  IPv6 Address in PDN4

px_IPv6_Address5_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:3333 #-- @desc  IPv6 Gateway Address in PDN5

px_IPv6_Address5_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:4444 #-- @desc  IPv6 Address in PDN5

px_IPv6_Address6_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:5555 #-- @desc  IPv6 Gateway Address in PDN6

px_IPv6_Address6_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:6666 #-- @desc  IPv6 Address in PDN6

px_IPv6_Address_BSF,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 BSF address

px_IPv6_Address_HomeAgent,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Home Address Agent

px_IPv6_Address_Other,                       CHARSTRING,    1111:2222:3333:4444:5555:5555:6666:8888 #-- @desc  Other IPv6 Address

px_LcsClientAddressDigits,                   CHARSTRING,    123456  #-- @desc LCS Client external address Digits

px_LcsClientAddressNPI,                      BITSTRING,     0001    #-- @desc LCS Client external address NPI

px_LcsClientAddressTOA,                      BITSTRING,     1001    #-- @desc LCS Client external address TOA

px_LcsClientName,                            CHARSTRING,    OPERATOR #-- @desc LCS Client name

px_MFBI_BandChannelBandwidth,                ENUM-Dl_Bandwidth_Type,n25     #-- @desc  MFBI E-UTRAN Channel Bandwidth

px_MFBI_FrequencyBand,                       INTEGER,       26      #-- @desc  a supported E-UTRA MFBI frequency band

px_MFBI_UTRAN_FrequencyBand,                 INTEGER,       26      #-- @desc  A supported UTRAN MFBI frequency band.

px_MS_ClsmkESIND,                            BITSTRING,     0       #-- @desc  Default Early Sending Indication

px_MS_ClsmkRevLvl,                           BITSTRING,     10      #-- @desc  Default Revision Level

px_MobileDataOn,                             BOOLEAN,       true    #-- @desc  Specifies whether mobile data associated with Internet PDN is enabled on the DUT

px_NAS_5GC_AuthenticationType,               ENUM-NAS_5GC_AKA_Type,AKA_5G  #-- @desc  NAS 5GC Authentication type

px_NAS_5GC_CipheringAlgorithm,               BITSTRING,     0010    #-- @desc  NAS 5GC Ciphering Algorithm

px_NAS_5GC_IntegrityAlgorithm,               BITSTRING,     0010    #-- @desc  NAS 5GC Integrity Algorithm

px_NAS_5GC_XRES_Length,                      INTEGER,       16      #-- @desc  NAS 5GC XRES length in octets used in Authentication

px_NAS_CipheringAlgorithm,                   BITSTRING,     001     #-- @desc  NAS Ciphering Algorithm (eea1)

px_NAS_IntegrityProtAlgorithm,               BITSTRING,     001     #-- @desc  NAS Integrity Algorithm (eia1)

px_NEDC_BandCombination,                     ENUM-NEDC_BandCombination_Type,DC_n28A_3A #-- @desc  NE-DC Band Combination

px_NR_CA_BandCombination,                    ENUM-NR_CA_BandCombination_Type,CA_n3A_n77A #-- @desc  NR CA Band Combination

px_NR_CipheringAlgorithm,                    ENUM-CipheringAlgorithm,nea2    #-- @desc  Ciphering Algorithm

px_NR_DC_BandCombination,                    ENUM-NR_DC_BandCombination_Type,DC_n78A_n257A #-- @desc  NR CA Band Combination

px_NR_DC_CA_BandCombination,                 ENUM-NR_DC_CA_BandCombination_Type,DC_n78A_n257G #-- @desc  NR DC CA Band Combination

px_NR_IntegrityProtAlgorithm,                ENUM-IntegrityProtAlgorithm,nia2    #-- @desc  Integrity Algorithm

px_NR_OverlappingNotSupportedBand_MFBI,      INTEGER,       77      #-- @desc  A not supported NR band that is overlapping with a supported band (px_NR_PrimaryBand). Applied to MFBI test case scenario.

px_NR_PrimaryBand,                           INTEGER,       78      #-- @desc  NR primary band

px_NR_PrimaryBandDeltaNRf1,                  INTEGER,       1       #-- @desc  delta frequency in dB for NR primary band test frequency NRf1

px_NR_PrimaryBandDeltaNRf2,                  INTEGER,       0       #-- @desc  delta frequency in dB for NR primary band test frequency NRf2

px_NR_PrimaryBandDeltaNRf3,                  INTEGER,       0       #-- @desc  delta frequency in dB for NR primary band test frequency NRf3

px_NR_PrimaryBandDeltaNRf4,                  INTEGER,       0       #-- @desc  delta frequency in dB for NR primary band test frequency NRf4

px_NR_PrimaryBandDeltas_DeltaNRf1,           INTEGER,       1       #-- @desc  ?(f) in dB for NR primary band test frequencies NRf1, NRf2, NRf3 and NRf4

px_NR_SecondaryBand,                         INTEGER,       41      #-- @desc  NR secondary band

px_NR_SecondaryBandDeltaNRf1,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf1

px_NR_SecondaryBandDeltaNRf2,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf2

px_NR_SecondaryBandDeltaNRf3,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf3

px_NR_SecondaryBandDeltaNRf4,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf4

px_NR_SidelinkBand,                          INTEGER,       47      #-- @desc  NR sidelink band

px_NoTDD_LCR_onLTE,                          BOOLEAN,       false   #-- @desc  Only applicable to UE supporting (at least) LTE and LCR TDD.  If set to true the UE is configured not to report support of LCR TDD (IE utraTDD128 in UECapabilityInformation) when being camped on an LTE cell with no detectable LCR TDD cell in the environment.

px_OverlappingNotSupportedFrequencyBand_MFBI,INTEGER,       27      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band

px_OverlappingSupportedFrequencyBand_MFBI,   INTEGER,       26      #-- @desc  a supported E-UTRA frequency band overlapping withpx_OverlappingNotSupportedFrequencyBand_MFBI applied to MFBI enhancement test case scenario.

px_PTMSI_Def,                                OCTETSTRING,   C2345678 #-- @desc  Default PTMSI

px_PTMSI_SigDef,                             OCTETSTRING,   AB1234  #-- @desc  Default PTMSI signature (3 octets 3GPP 24.008   10.5.5.8).

px_PWS_CB_DataCodingScheme,                  BITSTRING,     1010    #-- @desc  CMAS or ETWS data coding scheme of the alphabetcodingand the applied language (see TS 23.401)

px_PWS_CB_DataPage1,                         CHARSTRING,    warning1 #-- @desc  ETWS or CMAS Page 1 warning data message

px_PWS_CB_DataPage2,                         CHARSTRING,    warning2 #-- @desc  ETWS or CMAS Page 2 warning data message

px_PWS_CB_DataPage3,                         CHARSTRING,    warning3 #-- @desc  CMAS or ETWS Page 3 warning data message

px_PWS_CB_DataPage4,                         CHARSTRING,    warning4 #-- @desc  CMAS or ETWS Page 4 warning data message

px_RATComb_Tested,                           ENUM-RATComb_Tested_Type,EUTRA_UTRA #-- @desc  This parameter represents the network RAT capabilitypreference and indicates which if any is supported RAT combination is to be tested

px_RRC_CipheringAlgorithm,                   CHARSTRING,    eea1    #-- @desc  Ciphering Algorithm

px_RRC_CipheringAlgorithm_r12,               ENUM-CipheringAlgorithm_r12,eea2    #-- @desc  Ciphering Algorithm

px_RRC_IntegrityProtAlgorithm,               ENUM-IntegrityProtAlgorithm_Type,eia2    #-- @desc  Integrity Algorithm

px_RRC_PS_ServTested,                        ENUM-RRC_ServTested,ps_Interactive #-- @desc  PS Service to be tested

px_Release_check_in_eMBMS_TCs,               BOOLEAN,       true    #-- Anritsu TTCN WA for release check in MBMS

px_ReportUTRA_RAT,                           ENUM-ReportUTRA_RAT_Type,both    #-- @desc  Specifies which UTRA RATs a UE reports on

px_ResetStoredInfo,                          BOOLEAN,       false   #-- @desc Support of RESETUEPOSITIONINGSTOREDINFORMATION command as defined in 3GPP TS 34.109 cl. 6.10

px_SMSTransport_CP_CIoT,                     BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise the SMS service as transport mechanism for user data for Control Plane CIoT Optimisation

px_SMS_ChkMsgReceived,                       BOOLEAN,       true    #-- @desc  Whether the operator can check an MT Short Message received

px_SMS_IndexOffset,                          INTEGER,       1       #-- @desc  Memory location index at UE for SMS storage used in +CMSS command

px_SMS_MsgFrmt,                              CHARSTRING,    1       #-- @desc  SMS message format <mode> (see TS 27.005 cl.3.2.). NOTE: Default value is for text mode. Change value to 0 to execute tests with PDU mode

px_SMS_PrefMem1,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 1 <mem1> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem2,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 2 <mem2> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem3,                             CHARSTRING,    MT      #-- @desc  SMS Preferred Memory 3 <mem3> of TS 27.005 [31] clause 3.2.2

px_SMS_SMSC_InternationalNumber,             CHARSTRING,    112233445566778 #-- @desc  international number of the SMSC:

px_SMS_Service,                              CHARSTRING,    1       #-- @desc  SMS Service <service> of TS 27.005 [31] clause 3.2.1

px_SPI_pc,                                   INTEGER,       5000    #-- Anritsu TTCN WA for SPI

px_SPI_ps,                                   INTEGER,       1000    #-- Anritsu TTCN WA for SPI

px_SRNC_Id,                                  BITSTRING,     1       #-- @desc  SRNC Id

px_SRNTI,                                    BITSTRING,     1       #-- @desc  S RNTI

px_SinglePLMN_Tested,                        ENUM-SinglePLMN_TestedType,MultiPLMN #-- @desc  This parameter represents the network capabilitypreference to support multi PLMNs on the same test Band and indicates the preference of multi PLMNs or single PLMN test environment. This PIXIT shall be set to SinglePLMN when only one frequency is defined for the test band

px_StartStop,                                BOOLEAN,       TRUE    #-- Anritsu TTCN WA for Automation EnableDisable

px_StartString,                              CHARSTRING,    StartTest: #-- Anritsu TTCN WA for Automation Starting test cases string e.g.: StartTest:TC_7_1_2_1

px_StopString,                               CHARSTRING,    EndTest: #-- Anritsu TTCN WA for Automation Stopping test cases string e.g.: StopTest:Passed

px_TDD_OperationBandCharstring,              CHARSTRING,    a       #-- @desc  Applicable for TDD. The operation band under test as defined in 34.108 clause 5.1.2

px_TMSI_Def,                                 OCTETSTRING,   11223344 #-- @desc  Default TMSI

px_TestLoopModeB_Delay,                      OCTETSTRING,   5A      #-- @desc  This parameter represents the IP PDU delay to be used for UE test loop mode B intest cases where long delay may be needed e.g. because of user interaction.

px_UARFCN_D_High,                            INTEGER,       10837   #-- @desc  High Range downlink UARFCN value

px_UARFCN_D_Low,                             INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value

px_UARFCN_D_Mid,                             INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value

px_UARFCN_High_TDD,                          INTEGER,       9596    #-- @desc  High Range downlink UARFCN value for LCR TDD

px_UARFCN_Low_TDD,                           INTEGER,       9504    #-- @desc  Low Range downlink UARFCN value for LCR TDD

px_UARFCN_Mid_TDD,                           INTEGER,       9550    #-- @desc  Mid Range downlink UARFCN value for LCR TDD

px_UE_CS_PS_UsageSetting_Tested,             ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CSPS mode is under test @sic R5s120274 sic@

px_UE_PS_UsageSetting_Tested,                ENUM-PS_MODE,  VOICE_CENTRIC #-- @desc  specifies which PS mode is under test @sic R5s120274 sic@

px_UEwithISIM,                               BOOLEAN,       FALSE   #-- @desc  true - UE has ISIM; false - UE has USIM only

px_UTRAN_CipheringAlgorithm,                 ENUM-CipheringAlgorithm_r7,uea2    #-- @desc  UTRAN Ciphering algorithm

px_UTRAN_ModeUnderTest,                      ENUM-UTRAN_FDD_TDD_Type,UTRAN_FDD #-- @desc  specifies which radio access technology is being tested in UTRAN

px_UTRAN_OverlappingNotSupportedFrequencyBandMFBI,INTEGER,       27      #-- @desc  A not supported UTRAN frequency band that is overlapping with a supported MFBI band (px_MFBI_UTRAN_FrequencyBand). This pixit shall be set also in accordance with the values of the 3 Pixits: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid.

px_UeLcsNotification,                        INTEGER,       20      #-- @desc Value for UE LCS Notification timeout timer (in seconds)

px_WLANBand,                                 ENUM-WLAN_Band_Type,Band2_4Ghz #-- @desc  WLAN ISM Band

px_WLAN_BeaconRSSI,                          INTEGER,       78      #-- @desc  Beacon RSSI value for IMS over WLAN test cases

px_WLAN_NetworkAddrIPv4,                     CHARSTRING,    192.168.3.1 #-- @desc  IPv4 WLAN Network Address

px_WLAN_NetworkAddrIPv6,                     CHARSTRING,    1111:2222:3333:4444:5555:6666:3333:2222 #-- @desc  IPv6 WLAN Network Address

px_WLAN_PDN1_ToOffload,                      BOOLEAN,       true    #-- @desc  If set to true the first PDN connection is offloaded to WLAN. If set to false the second PDN connection is offloaded to WLAN.

px_WLAN_RulesToBeTested,                     CHARSTRING,    ANDSF_Rules #-- @desc  Rules to be tested in WLAN test cases

px_WLAN_UE_AddrIPv4,                         CHARSTRING,    1.1.1.30 #-- @desc  IPv4 WLAN UE Address

px_WLAN_UE_AddrIPv6,                         CHARSTRING,    1111:1111:1111:1111:1111:1111:1111:2222 #-- @desc  IPv6 WLAN UE Address

px_XCAP_RootUri,                             CHARSTRING,    /XCAP.3gpp.org #-- @desc  XCAP Root URI

px_XCAP_TargetUri,                           CHARSTRING,    sip:user@domain.com #-- @desc  Target (SIP or TEL URI) where to forward to

px_XCAP_Username,                            CHARSTRING,    0       #-- @desc  username to be used for HTTP authentication in case of pc_XCAP_UsernameIsConfiguredInUE==true

px_eAuthRAND,                                BITSTRING,     10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111 #-- @desc  Random Challenge

px_eJapanMCC_Band6,                          HEXSTRING,     442     #-- @desc  Japan MCC code to be used for Band 6. The same value will be used for E-UTRAN and Inter-RAT cells. Type is different to that defined in 34.123-3.

px_eMaxNumberROHC_ContextSessions,           ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions @sic R5s130329 sic@

px_ePDG_Ipsec_CipheringAlgorithm,            ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ipsec Ciphering Algorithm used in ePDG

px_ePDG_Ipsec_IntegrityAlgorithm,            ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Ipsec Integrity Algorithm used in ePDG

px_ePDG_OperatorProvisionedFQDN,             CHARSTRING,    en.test.org #-- @desc  domain name of the ePDG to be considered to assign the IP addresses of the ePDG in responses to DNS queries

px_ePrimaryBandChannelBandwidth,             ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_ePrimaryFrequencyBand

px_ePrimaryFrequencyBand,                    INTEGER,       3       #-- @desc  E-UTRAN primary frequency band

px_eSecondaryBandChannelBandwidth,           ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_eSecondaryFrequencyBand

px_eSecondaryFrequencyBand,                  INTEGER,       1       #-- @desc  E-UTRAN secondary frequency band

px_eTDDsubframeConfig,                       ENUM-TDD_SubframeAssignment_Type,sa1     #-- @desc  TDD uplink-downlink subframe configuration

px_nPrimaryFrequencyBand,                    INTEGER,       78      #-- @desc  NR primary frequency band

px_nonSMSTransport_CP_CIoT,                  BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise non-SMS services as transport mechanism for user data for Control Plane CIoT Optimisation

