ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:45:10.799 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:45:10.803 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:45:10.804 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:45:10.805 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:45:10.805 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:45:10.806 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:45:10.808 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:45:10.809 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:45:10.810 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8081 configured!
10 | 08:45:10.811 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:45:12.014 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:45:12.016 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:45:14.063 |  | ←RRC BCCH SIB1 |  |  |
14 | 08:45:14.138 |  | ←RRC BCCH SIB |  |  |
15 | 08:45:14.143 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:45:14.158 |  | ←RRC BCCH SIB |  |  |
17 | 08:45:14.178 |  | ←RRC BCCH SIB |  |  |
18 | 08:46:51.147 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:46:51.147 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:46:51.147 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:46:51.147 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:46:51.198 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:46:51.198 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:46:51.198 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:46:51.198 |  |  |  | →NAS EMM Attach request |  |
26 | 08:46:51.198 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:46:51.198 |  |  |  | NAS K-asme 27c0efd092e8e7cc2979619b5a943f01... |  |
28 | 08:46:51.198 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:46:51.199 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:46:51.199 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:46:51.200 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:46:51.270 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:46:51.270 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:46:51.270 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:46:51.270 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:46:51.270 |  |  |  | NAS UE auth OK |  |
37 | 08:46:51.270 |  |  |  | NAS K-nas-cip a34eeba5119f386fd085bcbbc28fb... |  |
38 | 08:46:51.270 |  |  |  | NAS K-nas-int 28fe9f8e8979ca0fff23a48d42901... |  |
39 | 08:46:51.270 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:46:51.271 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:46:51.271 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:46:51.272 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:46:51.310 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 08:46:51.310 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:46:51.310 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
46 | 08:46:51.310 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:46:51.310 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:46:51.311 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0xe2) |  |  |
49 | 08:46:51.311 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:46:51.312 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 08:46:51.358 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 08:46:51.358 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:46:51.358 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
54 | 08:46:51.358 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:46:51.358 |  |  |  | NAS ← EMM Attach accept |  |
56 | 08:46:51.358 |  |  |  | NAS K-enb d4319024a3bf0e7239d9f644ccaee8891... |  |
57 | 08:46:51.359 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:46:51.359 |  |  | RRC K-enb d4319024a3bf0e7239d9f644ccaee8891... |  |  |
59 | 08:46:51.359 |  |  | RRC rrc-cip b5930d5ad7acf3ff4c9ee0d15c9ba64... |  |  |
60 | 08:46:51.359 |  |  | RRC rrc-int 83a367f7f66afe552b73a640584c683... |  |  |
61 | 08:46:51.359 |  |  | RRC up-cip 288ae354d7c4ad3185ffb4c03d7e2294... |  |  |
62 | 08:46:51.359 |  |  | RRC up-int 0bc0f808bd8b9ccd150f6d9c05516c77... |  |  |
63 | 08:46:51.360 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:46:51.390 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:46:51.390 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:46:51.390 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:46:51.390 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:46:51.447 |  | →RRC DCCH UE Capability Information |  |  |
69 | 08:46:51.448 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
70 | 08:46:51.448 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
71 | 08:46:51.448 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
72 | 08:46:51.470 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
73 | 08:46:51.510 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
74 | 08:46:51.510 |  | →RRC DCCH UL Information Transfer |  |  |
75 | 08:46:51.510 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
76 | 08:46:51.510 |  |  |  | →NAS EMM Attach complete |  |
77 | 08:46:51.510 |  |  |  | NAS ← EMM EMM information |  |
78 | 08:46:51.511 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0xab) |  |  |
79 | 08:46:51.511 |  | ←RRC DCCH DL Information Transfer |  |  |
80 | 08:46:51.512 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
81 | 08:46:54.431 |  | ←RRC DCCH RRC Connection Release |  |  |
82 | 08:46:54.432 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
83 | 08:46:58.277 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
84 | 08:46:58.277 |  | →RRC CCCH RRC Connection Request |  |  |
85 | 08:46:58.277 |  | ←RRC CCCH RRC Connection Setup |  |  |
86 | 08:46:58.277 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
87 | 08:46:58.310 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
88 | 08:46:58.310 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
89 | 08:46:58.310 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
90 | 08:46:58.310 |  |  |  | →NAS EMM Service request |  |
91 | 08:46:58.310 |  |  |  | NAS K-enb aa7539f02e8ae8bda389882024ce4f40e... |  |
92 | 08:46:58.311 |  |  | RRC K-enb aa7539f02e8ae8bda389882024ce4f40e... |  |  |
93 | 08:46:58.312 |  |  | RRC rrc-cip bc15910c8aa9d543125fcd53249ea1c... |  |  |
94 | 08:46:58.312 |  |  | RRC rrc-int 2ba61586bf209fa3556cadc29caef5a... |  |  |
95 | 08:46:58.312 |  |  | RRC up-cip f253f81e6e45e8f0850424b788141818... |  |  |
96 | 08:46:58.312 |  |  | RRC up-int 39b95b927bac66b4ffd02be3667671fc... |  |  |
97 | 08:46:58.312 |  | ←RRC DCCH Security Mode Command |  |  |
98 | 08:46:58.312 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
99 | 08:46:58.350 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
100 | 08:46:58.350 |  | →RRC DCCH Security Mode Complete |  |  |
101 | 08:46:58.350 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
102 | 08:46:58.350 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
103 | 08:46:58.390 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
104 | 08:46:58.390 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
105 | 08:47:30.990 | →enobeB PCAP frame→ TCP |  |  |  |
106 | 08:47:30.993 |  | ←enobeB PCAP frame← TCP |  |  |
107 | 08:47:31.030 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:47:31.078 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
109 | 08:47:31.081 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 08:47:31.086 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
111 | 08:47:31.110 | →enobeB PCAP frame→ TCP |  |  |  |
112 | 08:47:31.195 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
113 | 08:47:31.198 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
114 | 08:47:31.201 |  | ←enobeB PCAP frame← TCP |  |  |
115 | 08:47:31.202 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 08:47:31.230 | →enobeB PCAP frame→ TCP |  |  |  |
117 | 08:47:31.235 |  |  |  |  | →HTTP GET | HTTP-Proxy
118 | 08:47:31.238 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
119 | 08:47:31.241 |  | ←enobeB PCAP frame← TCP |  |  |
120 | 08:47:31.242 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:323: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
121 | 08:47:31.267 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
122 | 08:47:31.277 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
123 | 08:47:31.278 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 08:47:33.313 |  | ←enobeB PCAP frame← TCP |  |  |
125 | 08:47:33.350 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 08:47:33.358 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
127 | 08:47:33.361 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 08:47:33.365 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
129 | 08:47:33.874 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
130 | 08:47:33.881 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
131 | 08:47:33.914 |  |  |  |  | →HTTP GET | IDMS-Endpoint
132 | 08:47:33.918 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 08:47:33.920 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
134 | 08:47:33.921 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 08:47:33.923 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:561: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
136 | 08:47:33.924 |  |  |  |  | MMICmd: Please provide user credentials: username and password
137 | 08:47:33.927 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
138 | 08:47:33.990 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 08:47:39.005 |  |  |  |  | →HTTP POST | IDMS-Endpoint
140 | 08:47:39.010 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 08:47:39.017 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
142 | 08:47:39.020 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:566: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
143 | 08:47:39.025 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
144 | 08:47:39.081 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
145 | 08:47:39.089 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 08:47:39.593 |  | ←enobeB PCAP frame← TCP |  |  |
147 | 08:47:39.638 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
148 | 08:47:39.641 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 08:47:39.644 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
150 | 08:47:39.670 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 08:47:39.802 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
152 | 08:47:39.809 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
153 | 08:47:39.835 |  |  |  |  | →HTTP POST | IDMS-Endpoint
154 | 08:47:39.841 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 08:47:39.857 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:571: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
156 | 08:47:39.859 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
157 | 08:47:39.868 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
158 | 08:47:40.310 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:47:40.313 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 08:47:40.350 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 08:47:40.358 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 08:47:40.360 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 08:47:40.361 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 08:47:40.390 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 08:47:40.442 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
166 | 08:47:40.449 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 08:47:40.475 |  |  |  |  | →HTTP POST | HTTP-Proxy
168 | 08:47:40.478 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 08:47:40.481 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 08:47:40.489 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
171 | 08:47:40.490 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:591: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
172 | 08:47:40.497 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
173 | 08:47:40.553 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 08:47:40.598 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
175 | 08:47:40.601 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 08:47:40.604 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
177 | 08:47:40.630 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 08:47:40.638 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 08:47:40.641 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 08:47:41.090 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
181 | 08:47:41.097 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 08:47:41.156 |  |  |  |  | →HTTP POST | HTTP-Proxy
183 | 08:47:41.158 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
184 | 08:47:41.161 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 08:47:41.219 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
186 | 08:47:41.219 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:595: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
187 | 08:47:41.227 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 08:47:41.228 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
189 | 08:47:41.270 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 08:47:41.310 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 08:47:41.356 |  |  |  |  | →SIP REGISTER | P-CSCF
192 | 08:47:41.358 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
193 | 08:47:41.379 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
194 | 08:47:41.403 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
195 | 08:47:41.404 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
196 | 08:47:41.410 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
197 | 08:47:41.417 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
198 | 08:47:42.117 |  |  |  |  | →SIP REGISTER | P-CSCF
199 | 08:47:42.118 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
200 | 08:47:42.144 |  |  |  |  | ←SIP 200 OK | P-CSCF
201 | 08:47:42.152 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
202 | 08:47:42.558 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
203 | 08:47:42.559 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
204 | 08:47:42.560 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
205 | 08:47:42.570 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
206 | 08:47:42.616 |  |  |  |  | ←SIP 200 OK | P-CSCF
207 | 08:47:42.617 |  |  |  |  | MIKEY | Media-Server
208 | 08:47:42.624 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
209 | 08:47:42.830 |  |  |  |  | XML→ | Media-Server
210 | 08:47:42.831 |  |  |  |  | XML→ | Media-Server
211 | 08:47:42.835 |  |  |  |  | ←XML | Media-Server
212 | 08:47:42.838 |  |  |  |  | ←SIP NOTIFY | P-CSCF
213 | 08:47:42.846 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40638;transp... |  |  |
214 | 08:47:42.874 |  |  |  |  | →SIP 200 OK | P-CSCF
215 | 08:47:42.878 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
216 | 08:47:43.070 | →enobeB PCAP frame→ TCP |  |  |  |
217 | 08:47:43.073 |  | ←enobeB PCAP frame← TCP |  |  |
218 | 08:47:43.110 | →enobeB PCAP frame→ TCP |  |  |  |
219 | 08:47:43.118 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
220 | 08:47:43.121 |  | ←enobeB PCAP frame← TCP |  |  |
221 | 08:47:43.123 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
222 | 08:47:43.150 | →enobeB PCAP frame→ TCP |  |  |  |
223 | 08:47:43.234 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
224 | 08:47:43.238 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
225 | 08:47:43.241 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
226 | 08:47:43.270 | →enobeB PCAP frame→ TCP |  |  |  |
227 | 08:47:43.275 |  |  |  |  | →HTTP GET | HTTP-Proxy
228 | 08:47:43.278 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
229 | 08:47:43.281 |  | ←enobeB PCAP frame← TCP |  |  |
230 | 08:47:43.282 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:731: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
231 | 08:47:43.290 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
232 | 08:47:43.299 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
233 | 08:47:43.350 | →enobeB PCAP frame→ TCP |  |  |  |
234 | 08:47:43.386 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
235 | 08:47:43.390 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 08:47:43.393 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 08:47:43.430 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 08:47:43.590 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 08:47:43.593 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 08:47:43.630 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 08:47:43.638 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
242 | 08:47:43.641 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 08:47:43.644 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
244 | 08:47:43.670 | →enobeB PCAP frame→ TCP |  |  |  |
245 | 08:47:43.714 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
246 | 08:47:43.718 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
247 | 08:47:43.721 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
248 | 08:47:43.750 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 08:47:43.755 |  |  |  |  | →HTTP GET | HTTP-Proxy
250 | 08:47:43.758 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
251 | 08:47:43.761 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 08:47:43.766 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:736: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
253 | 08:47:43.808 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
254 | 08:47:43.818 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
255 | 08:47:43.819 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 08:47:43.820 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
257 | 08:47:43.870 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 08:47:43.874 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
259 | 08:47:43.878 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
260 | 08:47:43.881 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 08:47:43.910 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 08:47:44.598 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
263 | 08:47:44.599 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
264 | 08:47:44.600 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
265 | 08:47:44.601 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
266 | 08:47:44.609 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
267 | 08:47:44.663 |  |  |  |  | ←SIP 200 OK | P-CSCF
268 | 08:47:44.664 |  |  |  |  | MIKEY | Media-Server
269 | 08:47:44.671 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
270 | 08:47:44.710 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 08:47:44.712 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 08:47:44.750 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 08:47:44.758 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
274 | 08:47:44.761 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
275 | 08:47:44.790 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 08:47:44.873 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
277 | 08:47:44.875 |  |  |  |  | XML→ | Media-Server
278 | 08:47:44.876 |  |  |  |  | XML→ | Media-Server
279 | 08:47:44.878 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
280 | 08:47:44.878 |  |  |  |  | ←XML | Media-Server
281 | 08:47:44.881 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
282 | 08:47:44.881 |  |  |  |  | ←SIP NOTIFY | P-CSCF
283 | 08:47:44.889 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40638;transp... |  |  |
284 | 08:47:44.910 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 08:47:44.914 |  |  |  |  | →HTTP GET | HTTP-Proxy
286 | 08:47:44.914 |  |  |  |  | →SIP 200 OK | P-CSCF
287 | 08:47:44.916 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:741: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
288 | 08:47:44.918 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
289 | 08:47:44.919 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
290 | 08:47:44.921 |  | ←enobeB PCAP frame← TCP |  |  |
291 | 08:47:44.922 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
292 | 08:47:44.930 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 08:47:44.931 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
294 | 08:47:44.950 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 08:47:44.986 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
296 | 08:47:44.990 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
297 | 08:47:44.993 |  | ←enobeB PCAP frame← TCP |  |  |
298 | 08:47:44.998 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 08:47:45.001 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 08:47:45.030 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 08:47:45.033 |  | ←enobeB PCAP frame← TCP |  |  |
302 | 08:47:45.070 | →enobeB PCAP frame→ TCP |  |  |  |
303 | 08:47:45.078 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
304 | 08:47:45.081 |  | ←enobeB PCAP frame← TCP |  |  |
305 | 08:47:45.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
306 | 08:47:45.110 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 08:47:45.234 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
308 | 08:47:45.238 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
309 | 08:47:45.241 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
310 | 08:47:45.270 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 08:47:45.275 |  |  |  |  | →HTTP GET | HTTP-Proxy
312 | 08:47:45.278 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
313 | 08:47:45.281 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 08:47:45.284 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:746: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
315 | 08:47:45.310 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
316 | 08:47:45.320 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
317 | 08:47:45.321 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
318 | 08:47:45.350 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 08:47:45.354 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
320 | 08:47:45.358 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 08:47:45.361 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 08:47:45.390 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 08:47:45.678 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
324 | 08:47:45.679 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
325 | 08:47:45.680 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
326 | 08:47:45.681 |  |  |  |  | →SIP PUBLISH | P-CSCF
327 | 08:47:45.708 |  |  |  |  | MIKEY | Media-Server
328 | 08:47:45.798 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
329 | 08:47:45.798 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
330 | 08:47:45.799 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
331 | 08:47:45.800 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
332 | 08:47:45.919 |  |  |  |  | XML→ | Media-Server
333 | 08:47:45.922 |  |  |  |  | ←SIP 200 OK | P-CSCF
334 | 08:47:45.926 |  |  |  |  | ←SIP 200 OK | P-CSCF
335 | 08:47:45.926 |  |  |  |  | MIKEY | Media-Server
336 | 08:47:45.930 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
337 | 08:47:45.933 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
338 | 08:47:46.126 |  |  |  |  | XML→ | Media-Server
339 | 08:47:46.127 |  |  |  |  | XML→ | Media-Server
341 | 08:47:46.164 |  |  |  |  | ←XML | Media-Server
342 | 08:47:46.169 |  |  |  |  | ←SIP NOTIFY | P-CSCF
343 | 08:47:46.177 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40638;transp... |  |  |
344 | 08:47:46.234 |  |  |  |  | →SIP 200 OK | P-CSCF
345 | 08:47:46.238 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
346 | 08:47:46.239 |  |  |  |  | ←XML | Media-Server
347 | 08:47:46.255 |  |  |  |  | ←SIP MESSAGE | P-CSCF
348 | 08:47:46.264 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
349 | 08:47:46.265 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
350 | 08:47:47.195 |  |  |  |  | →SIP 200 OK | P-CSCF
351 | 08:47:47.198 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
352 | 08:47:49.203 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
353 | 08:47:49.270 |  | ←RRC DCCH RRC Connection Release |  |  |
354 | 08:47:49.271 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
355 | 08:47:49.279 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
356 | 08:47:49.283 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
357 | 08:47:49.283 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
358 | 08:47:58.367 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
359 | 08:47:58.367 |  | →RRC CCCH RRC Connection Request |  |  |
360 | 08:47:58.367 |  | ←RRC CCCH RRC Connection Setup |  |  |
361 | 08:47:58.367 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
362 | 08:47:58.438 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
363 | 08:47:58.438 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
364 | 08:47:58.438 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
365 | 08:47:58.438 |  |  |  | →NAS EMM Service request |  |
366 | 08:47:58.439 |  |  | RRC K-enb 65ca862763d4c77c5ad4756a7a6e049d7... |  |  |
367 | 08:47:58.439 |  |  |  | NAS K-enb 65ca862763d4c77c5ad4756a7a6e049d7... |  |
368 | 08:47:58.440 |  |  | RRC rrc-cip b0f84609d1ba08a5119af7a38fca6b5... |  |  |
369 | 08:47:58.440 |  |  | RRC rrc-int 8a303d481ceb12671173838c1d742ed... |  |  |
370 | 08:47:58.440 |  |  | RRC up-cip 02ee59637ef7c31a699a567b0e73a5a0... |  |  |
371 | 08:47:58.440 |  |  | RRC up-int d69f5ed07d4473aaea5417da03075d8b... |  |  |
372 | 08:47:58.440 |  | ←RRC DCCH Security Mode Command |  |  |
373 | 08:47:58.440 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
374 | 08:47:58.470 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
375 | 08:47:58.470 |  | →RRC DCCH Security Mode Complete |  |  |
376 | 08:47:58.470 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
377 | 08:47:58.470 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
378 | 08:47:58.510 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
379 | 08:47:58.510 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
380 | 08:47:58.518 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
381 | 08:47:58.518 |  |  |  |  | →SIP INVITE | P-CSCF
382 | 08:47:58.547 |  |  |  |  | ←SIP 100 Trying | P-CSCF
383 | 08:47:58.551 |  |  |  |  | ←SIP 200 OK | P-CSCF
384 | 08:47:58.553 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
385 | 08:47:58.555 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
386 | 08:47:58.559 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
387 | 08:47:59.195 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
388 | 08:47:59.196 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
389 | 08:47:59.196 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
390 | 08:47:59.197 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
391 | 08:47:59.230 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
392 | 08:47:59.230 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
393 | 08:47:59.230 |  | →RRC DCCH UL Information Transfer |  |  |
394 | 08:47:59.230 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
395 | 08:47:59.230 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
396 | 08:47:59.321 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
397 | 08:47:59.394 |  |  |  |  | →SIP ACK | P-CSCF
398 | 08:47:59.398 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
399 | 08:48:01.397 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
400 | 08:48:01.447 |  | ←RRC DCCH RRC Connection Release |  |  |
401 | 08:48:01.447 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
402 | 08:48:01.466 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
403 | 08:48:01.467 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1224: Test-Body Step 1
404 | 08:48:01.470 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
405 | 08:48:01.470 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT broadcast group call using a pre-established session, automatic commencement mode, with Floor Default Control
406 | 08:48:01.471 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1227: Test-Body Step 2
407 | 08:48:10.297 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
408 | 08:48:10.297 |  | →RRC CCCH RRC Connection Request |  |  |
409 | 08:48:10.297 |  | ←RRC CCCH RRC Connection Setup |  |  |
410 | 08:48:10.297 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
411 | 08:48:10.350 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
412 | 08:48:10.350 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
413 | 08:48:10.350 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
414 | 08:48:10.350 |  |  |  | →NAS EMM Service request |  |
415 | 08:48:10.350 |  |  |  | NAS K-enb 229f0b58731b9eae8aae420a6c50d2bc2... |  |
416 | 08:48:10.351 |  |  | RRC K-enb 229f0b58731b9eae8aae420a6c50d2bc2... |  |  |
417 | 08:48:10.352 |  |  | RRC rrc-cip faa72574f094a249121a91edb104564... |  |  |
418 | 08:48:10.352 |  |  | RRC rrc-int 8f9fa8037b624db60fb9d69bef818fc... |  |  |
419 | 08:48:10.352 |  |  | RRC up-cip aaa7b04219981604c501a545c6968205... |  |  |
420 | 08:48:10.352 |  |  | RRC up-int 07543e1a35a01c1973b7b10e0a8a988c... |  |  |
421 | 08:48:10.352 |  | ←RRC DCCH Security Mode Command |  |  |
422 | 08:48:10.352 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
423 | 08:48:10.390 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
424 | 08:48:10.390 |  | →RRC DCCH Security Mode Complete |  |  |
425 | 08:48:10.390 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
426 | 08:48:10.390 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
427 | 08:48:10.430 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
428 | 08:48:10.430 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
429 | 08:48:10.438 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
430 | 08:48:10.439 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
431 | 08:48:10.440 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
432 | 08:48:10.441 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
433 | 08:48:10.442 | →enobeB PCAP frame→ SIP over IPSEC: REFER sip:sessionB@cf.mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml SRTP frame: |  |  |  |
434 | 08:48:10.445 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
435 | 08:48:10.460 |  |  |  |  | →SIP REFER | P-CSCF
436 | 08:48:10.470 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 08:48:10.518 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
438 | 08:48:10.526 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
439 | 08:48:10.534 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
440 | 08:48:10.543 |  |  |  |  | XML→ | Media-Server
441 | 08:48:10.550 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
442 | 08:48:10.551 |  |  |  |  | XML→ | Media-Server
443 | 08:48:10.555 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: D3E233F762D56E1D788CD781B49DBF80, Master Salt: 5BE0FEC34B0160D537974EB4, MKI: 272B5372
444 | 08:48:10.555 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
445 | 08:48:10.557 |  |  |  |  | ←SIP 200 OK | P-CSCF
446 | 08:48:10.557 |  |  |  |  | ←Connect | Media-Server
447 | 08:48:10.564 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
448 | 08:48:10.590 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
449 | 08:48:10.594 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
450 | 08:48:10.595 |  |  |  |  | Verdict PASS: MCPTT_MediaControl_Procedures.ttcn:442: PreestablishedSessionAcknowledge Verdict: Pass
451 | 08:48:10.595 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1231: Step 2 Verdict: Pass
452 | 08:48:10.596 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1235: Test-Body Step 6
453 | 08:48:10.596 |  |  |  |  | MMICmd: Make the MCPTT User leave the MCPTT session
454 | 08:48:10.597 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1238: Test-Body Step 7
455 | 08:48:10.598 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
456 | 08:48:10.606 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
457 | 08:48:10.630 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
458 | 08:48:10.670 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
459 | 08:48:13.557 |  |  |  |  | →SIP REFER | P-CSCF
460 | 08:48:13.578 |  |  |  |  | ←SIP 200 OK | P-CSCF
461 | 08:48:13.586 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
462 | 08:48:13.598 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
463 | 08:48:13.601 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
464 | 08:48:13.638 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
465 | 08:48:13.641 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
466 | 08:48:13.646 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
467 | 08:48:15.576 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
468 | 08:48:15.626 |  | ←RRC DCCH RRC Connection Release |  |  |
469 | 08:48:15.627 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
470 | 08:48:15.630 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
471 | 08:48:15.635 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
472 | 08:48:15.637 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
473 | 08:48:15.638 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
474 | 08:48:15.639 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
475 | 08:48:15.648 |  |  |  |  | ←SIP BYE | P-CSCF
476 | 08:48:15.727 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
477 | 08:48:15.727 |  | →RRC CCCH RRC Connection Request |  |  |
478 | 08:48:15.727 |  | ←RRC CCCH RRC Connection Setup |  |  |
479 | 08:48:15.727 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
480 | 08:48:15.750 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
481 | 08:48:15.750 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
482 | 08:48:15.750 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
483 | 08:48:15.750 |  |  |  | →NAS EMM Service request |  |
484 | 08:48:15.750 |  |  |  | NAS K-enb 247f18df64cbb5c564bc99804f6a61b70... |  |
485 | 08:48:15.751 |  |  | RRC K-enb 247f18df64cbb5c564bc99804f6a61b70... |  |  |
486 | 08:48:15.752 |  |  | RRC rrc-cip ed3bef5e2f766c91c7c76756c140220... |  |  |
487 | 08:48:15.752 |  |  | RRC rrc-int 180d880660fd928762075ad43b6e635... |  |  |
488 | 08:48:15.752 |  |  | RRC up-cip 905b9af46c8445d72725694fb09a7558... |  |  |
489 | 08:48:15.752 |  |  | RRC up-int d3a9ad7d11c02eb6136d6d9d70f96df4... |  |  |
490 | 08:48:15.752 |  | ←RRC DCCH Security Mode Command |  |  |
491 | 08:48:15.752 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
492 | 08:48:15.790 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
493 | 08:48:15.790 |  | →RRC DCCH Security Mode Complete |  |  |
494 | 08:48:15.790 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
495 | 08:48:15.790 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
496 | 08:48:15.797 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
497 | 08:48:15.797 |  | ←RRC PCCH Paging |  |  |
498 | 08:48:15.830 | →enobeB PCAP frame→ SRTP frame: RRCConnectionReconfigurationComplete [76-bytes] ... |  |  |  |
499 | 08:48:15.830 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
500 | 08:48:15.832 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |
501 | 08:48:15.833 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
502 | 08:48:15.838 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
503 | 08:48:15.841 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
504 | 08:48:15.875 |  |  |  |  | →SIP 200 OK | P-CSCF
505 | 08:48:15.878 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
506 | 08:48:15.882 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
507 | 08:48:16.110 | →enobeB PCAP frame→ |  |  |  |
508 | 08:48:17.883 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
509 | 08:48:17.906 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
510 | 08:48:17.906 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
511 | 08:48:17.906 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
512 | 08:48:17.907 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
513 | 08:48:17.950 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
514 | 08:48:17.950 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
515 | 08:48:17.950 |  | →RRC DCCH UL Information Transfer |  |  |
516 | 08:48:17.950 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
517 | 08:48:17.950 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
518 | 08:48:18.022 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
519 | 08:48:18.024 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
520 | 08:48:18.082 |  | ←RRC DCCH RRC Connection Release |  |  |
521 | 08:48:18.083 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
522 | 08:48:18.101 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
523 | 08:48:18.102 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
524 | 08:48:18.104 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
525 | 08:48:18.853 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.