MSG #312 2022-08-09 09:04:08.364

HTTP 200 OK message at 09:04:08.364

    HTTP/1.1 200 OK
    Content-Type: application/vnd.3gpp.mcptt-service-config+xml
    Cache-Control: no-store
    Pragma: no-cache
    Content-Length: 5865

    <mcpttsc:service-configuration-info-Type xmlns:mcpttsc='urn:3gpp:ns:mcpttServiceConfig:1.0'>
     <mcpttsc:service-configuration-params domain='mcstaasting.com'>
      <mcpttsc:common>
       <mcpttsc:min-length-alias>2</mcpttsc:min-length-alias>
       <mcpttsc:broadcast-group>
        <mcpttsc:num-levels-group-hierarchy>1</mcpttsc:num-levels-group-hierarchy>
        <mcpttsc:num-levels-user-hierarchy>1</mcpttsc:num-levels-user-hierarchy>
       </mcpttsc:broadcast-group>
      </mcpttsc:common>
      <mcpttsc:on-network>
       <mcpttsc:emergency-call>
        <mcpttsc:private-cancel-timeout>PT30M</mcpttsc:private-cancel-timeout>
        <mcpttsc:group-time-limit>PT20M</mcpttsc:group-time-limit>
       </mcpttsc:emergency-call>
       <mcpttsc:private-call>
        <mcpttsc:hang-time>PT30S</mcpttsc:hang-time>
        <mcpttsc:max-duration-with-floor-control>PT30S</mcpttsc:max-duration-with-floor-control>
        <mcpttsc:max-duration-without-floor-control>PT20M</mcpttsc:max-duration-without-floor-control>
       </mcpttsc:private-call>
       <mcpttsc:num-levels-priority-hierarchy>10</mcpttsc:num-levels-priority-hierarchy>
       <mcpttsc:transmit-time>
        <mcpttsc:time-limit>PT30S</mcpttsc:time-limit>
        <mcpttsc:time-warning>PT20M</mcpttsc:time-warning>
       </mcpttsc:transmit-time>
       <mcpttsc:hang-time-warning>PT20M</mcpttsc:hang-time-warning>
       <mcpttsc:floor-control-queue>
        <mcpttsc:depth>5</mcpttsc:depth>
        <mcpttsc:max-user-request-time>PT20M</mcpttsc:max-user-request-time>
       </mcpttsc:floor-control-queue>
       <mcpttsc:fc-timers-counters>
        <mcpttsc:T1-end-of-rtp-media>PT4S</mcpttsc:T1-end-of-rtp-media>
        <mcpttsc:T3-stop-talking-grace>PT3S</mcpttsc:T3-stop-talking-grace>
        <mcpttsc:T7-floor-idle>PT2S</mcpttsc:T7-floor-idle>
        <mcpttsc:T8-floor-revoke>PT1S</mcpttsc:T8-floor-revoke>
        <mcpttsc:T11-end-of-RTP-dual>PT4S</mcpttsc:T11-end-of-RTP-dual>
        <mcpttsc:T12-stop-talking-dual>PT30S</mcpttsc:T12-stop-talking-dual>
        <mcpttsc:T15-conversation>PT30S</mcpttsc:T15-conversation>
        <mcpttsc:T16-map-group-to-bearer>PT0.5S</mcpttsc:T16-map-group-to-bearer>
        <mcpttsc:T17-unmap-group-to-bearer>PT0.5S</mcpttsc:T17-unmap-group-to-bearer>
        <mcpttsc:T20-floor-granted>PT1S</mcpttsc:T20-floor-granted>
        <mcpttsc:T55-connect>PT2S</mcpttsc:T55-connect>
        <mcpttsc:T56-disconnect>PT2S</mcpttsc:T56-disconnect>
        <mcpttsc:C7-floor-idle>10</mcpttsc:C7-floor-idle>
        <mcpttsc:C17-unmap-group-to-bearer>3</mcpttsc:C17-unmap-group-to-bearer>
        <mcpttsc:C20-floor-granted>3</mcpttsc:C20-floor-granted>
        <mcpttsc:C55-connect>3</mcpttsc:C55-connect>
        <mcpttsc:C56-disconnect>3</mcpttsc:C56-disconnect>
       </mcpttsc:fc-timers-counters>
       <mcpttsc:signalling-protection>
        <mcpttsc:confidentiality-protection>true</mcpttsc:confidentiality-protection>
        <mcpttsc:integrity-protection>true</mcpttsc:integrity-protection>
       </mcpttsc:signalling-protection>
       <mcpttsc:protection-between-mcptt-servers>
        <mcpttsc:allow-signalling-protection>true</mcpttsc:allow-signalling-protection>
        <mcpttsc:allow-floor-control-protection>true</mcpttsc:allow-floor-control-protection>
       </mcpttsc:protection-between-mcptt-servers>
       <mcpttsc:emergency-resource-priority>
        <mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
        <mcpttsc:resource-priority-priority>8</mcpttsc:resource-priority-priority>
       </mcpttsc:emergency-resource-priority>
       <mcpttsc:imminent-peril-resource-priority>
        <mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
        <mcpttsc:resource-priority-priority>5</mcpttsc:resource-priority-priority>
       </mcpttsc:imminent-peril-resource-priority>
       <mcpttsc:normal-resource-priority>
        <mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
        <mcpttsc:resource-priority-priority>1</mcpttsc:resource-priority-priority>
       </mcpttsc:normal-resource-priority>
       <mcpttsc:anyExt>
        <mcpttsc:functional-alias-list xmlns:mcpttsc='urn:3gpp:ns:mcpttServiceConfig:1.0'>
     <mcpttsc:functional-alias-entry>
      <mcpttsc:functional-alias>mcptt-fa-a-id@mcstaasting.com</mcpttsc:functional-alias>
      <mcpttsc:max-simultaneous-activations>1</mcpttsc:max-simultaneous-activations>
      <mcpttsc:allow-takeover>true</mcpttsc:allow-takeover>
      <mcpttsc:mcptt-user-list>
       <mcpttsc:entry>
        <mcpttsc:uri-entry>sip:mcptt-userA-id@mcstaasting.com</mcpttsc:uri-entry>
       </mcpttsc:entry>
      </mcpttsc:mcptt-user-list>
     </mcpttsc:functional-alias-entry>
    </mcpttsc:functional-alias-list>

       </mcpttsc:anyExt>
      </mcpttsc:on-network>
      <mcpttsc:off-network>
       <mcpttsc:emergency-call>
        <mcpttsc:private-cancel-timeout>PT5S</mcpttsc:private-cancel-timeout>
        <mcpttsc:group-time-limit>PT5S</mcpttsc:group-time-limit>
       </mcpttsc:emergency-call>
       <mcpttsc:private-call>
        <mcpttsc:hang-time>PT5S</mcpttsc:hang-time>
        <mcpttsc:max-duration-with-floor-control>PT60S</mcpttsc:max-duration-with-floor-control>
       </mcpttsc:private-call>
       <mcpttsc:num-levels-priority-hierarchy>4</mcpttsc:num-levels-priority-hierarchy>
       <mcpttsc:transmit-time>
        <mcpttsc:time-limit>PT60S</mcpttsc:time-limit>
        <mcpttsc:time-warning>PT50S</mcpttsc:time-warning>
       </mcpttsc:transmit-time>
       <mcpttsc:hang-time-warning>PT4S</mcpttsc:hang-time-warning>
       <mcpttsc:default-prose-per-packet-priority>
        <mcpttsc:mcptt-private-call-signalling>1</mcpttsc:mcptt-private-call-signalling>
        <mcpttsc:mcptt-private-call-media>1</mcpttsc:mcptt-private-call-media>
        <mcpttsc:mcptt-emergency-private-call-signalling>8</mcpttsc:mcptt-emergency-private-call-signalling>
        <mcpttsc:mcptt-emergency-private-call-media>8</mcpttsc:mcptt-emergency-private-call-media>
       </mcpttsc:default-prose-per-packet-priority>
       <mcpttsc:allow-log-metadata>true</mcpttsc:allow-log-metadata>
      </mcpttsc:off-network>
     </mcpttsc:service-configuration-params>
    </mcpttsc:service-configuration-info-Type>