ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 09:01:46.661 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 09:01:46.663 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 09:01:46.664 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 09:01:46.665 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 09:01:46.666 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 09:01:46.666 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 09:01:46.668 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 09:01:46.669 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 09:01:46.670 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8081 configured!
10 | 09:01:46.672 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 09:01:47.873 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 09:01:47.874 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 09:01:50.619 |  | ←RRC BCCH SIB |  |  |
14 | 09:01:50.624 |  | ←RRC BCCH SIB1 |  |  |
15 | 09:01:50.639 |  | ←RRC BCCH SIB |  |  |
16 | 09:01:50.659 |  | ←RRC BCCH SIB |  |  |
17 | 09:01:50.704 |  | ←RRC BCCH SIB1 |  |  |
18 | 09:03:24.128 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 09:03:24.128 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 09:03:24.128 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 09:03:24.128 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 09:03:24.159 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 09:03:24.159 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 09:03:24.159 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 09:03:24.159 |  |  |  | →NAS EMM Attach request |  |
26 | 09:03:24.159 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 09:03:24.159 |  |  |  | NAS K-asme eb3310d520cfe04c542f24ea442b5d3f... |  |
28 | 09:03:24.159 |  |  |  | NAS ← EMM Authentication request |  |
29 | 09:03:24.160 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 09:03:24.160 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 09:03:24.161 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 09:03:24.231 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 09:03:24.231 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 09:03:24.231 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 09:03:24.231 |  |  |  | →NAS EMM Authentication response |  |
36 | 09:03:24.231 |  |  |  | NAS UE auth OK |  |
37 | 09:03:24.231 |  |  |  | NAS K-nas-cip 43070abb0cad3d86af4c7a2544a25... |  |
38 | 09:03:24.231 |  |  |  | NAS K-nas-int 762814495efbfbcefa6c0f9533af3... |  |
39 | 09:03:24.231 |  |  |  | NAS ← EMM Security mode command |  |
40 | 09:03:24.232 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 09:03:24.232 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 09:03:24.233 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 09:03:24.241 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 09:03:24.271 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 09:03:24.271 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 09:03:24.271 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
47 | 09:03:24.271 |  |  |  | →NAS EMM Security mode complete |  |
48 | 09:03:24.271 |  |  |  | NAS ← ESM ESM information request |  |
49 | 09:03:24.272 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
50 | 09:03:24.272 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 09:03:24.273 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 09:03:24.319 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 09:03:24.319 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 09:03:24.319 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
55 | 09:03:24.319 |  |  |  | →NAS ESM ESM information response |  |
56 | 09:03:24.319 |  |  |  | NAS ← EMM Attach accept |  |
57 | 09:03:24.319 |  |  |  | NAS K-enb 80f2a59aac77bdeeb0518089e0ddcacb9... |  |
58 | 09:03:24.320 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 09:03:24.320 |  |  | RRC K-enb 80f2a59aac77bdeeb0518089e0ddcacb9... |  |  |
60 | 09:03:24.320 |  |  | RRC rrc-cip 2f2fd50ac08350d82ccc82950cccad2... |  |  |
61 | 09:03:24.320 |  |  | RRC rrc-int 0e5d97337249b0ee514028bb16a92e4... |  |  |
62 | 09:03:24.320 |  |  | RRC up-cip 29b1487b05a027c7fb895f043e31702e... |  |  |
63 | 09:03:24.320 |  |  | RRC up-int 2edf2c89b3c992bcc28520f8021a3039... |  |  |
64 | 09:03:24.321 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 09:03:24.351 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 09:03:24.351 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 09:03:24.351 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 09:03:24.351 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 09:03:24.401 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 09:03:24.401 |  | →RRC DCCH UE Capability Information |  |  |
71 | 09:03:24.402 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
72 | 09:03:24.402 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 09:03:24.402 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 09:03:24.439 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 09:03:24.471 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 09:03:24.471 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 09:03:24.471 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
78 | 09:03:24.471 |  |  |  | →NAS EMM Attach complete |  |
79 | 09:03:24.471 |  |  |  | NAS ← EMM EMM information |  |
80 | 09:03:24.472 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
81 | 09:03:24.472 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 09:03:24.473 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 09:03:30.316 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 09:03:30.317 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 09:03:30.668 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 09:03:30.668 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 09:03:30.668 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 09:03:30.668 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 09:03:30.719 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 09:03:30.719 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 09:03:30.719 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 09:03:30.719 |  |  |  | →NAS EMM Service request |  |
93 | 09:03:30.719 |  |  |  | NAS K-enb c7de3cded260a7065bbed949b08c390fd... |  |
94 | 09:03:30.720 |  |  | RRC K-enb c7de3cded260a7065bbed949b08c390fd... |  |  |
95 | 09:03:30.721 |  |  | RRC rrc-cip 64a362b6a5df20f718db1ba50a7b07f... |  |  |
96 | 09:03:30.721 |  |  | RRC rrc-int 3699439044f3902454b7fcffafde906... |  |  |
97 | 09:03:30.721 |  |  | RRC up-cip b6d1709abcafae6244934da1e4ee0706... |  |  |
98 | 09:03:30.721 |  |  | RRC up-int f3f65861006bfefd3e529ffc1509668c... |  |  |
99 | 09:03:30.721 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 09:03:30.721 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 09:03:30.751 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 09:03:30.751 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 09:03:30.751 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 09:03:30.751 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 09:03:30.791 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] ... |  |  |  |
106 | 09:03:30.791 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 09:03:54.954 |  | ←enobeB PCAP frame← TCP |  |  |
108 | 09:03:54.991 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 09:03:55.079 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
110 | 09:03:55.082 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 09:03:55.084 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
112 | 09:03:55.111 | →enobeB PCAP frame→ TCP |  |  |  |
113 | 09:03:55.315 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
114 | 09:03:55.319 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 09:03:55.322 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 09:03:55.351 | →enobeB PCAP frame→ TCP |  |  |  |
117 | 09:03:55.355 |  |  |  |  | →HTTP GET | HTTP-Proxy
118 | 09:03:55.359 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
119 | 09:03:55.362 |  | ←enobeB PCAP frame← TCP |  |  |
120 | 09:03:55.362 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:323: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
121 | 09:03:55.384 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
122 | 09:03:55.394 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
123 | 09:03:55.395 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 09:03:55.431 | →enobeB PCAP frame→ TCP |  |  |  |
125 | 09:03:55.439 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 09:03:57.474 |  | ←enobeB PCAP frame← TCP |  |  |
127 | 09:03:57.519 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
128 | 09:03:57.521 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 09:03:57.527 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
130 | 09:03:57.551 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 09:03:57.835 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
132 | 09:03:57.839 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 09:03:57.842 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 09:03:57.844 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 09:03:57.871 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 09:03:57.877 |  |  |  |  | →HTTP GET | IDMS-Endpoint
137 | 09:03:57.879 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
138 | 09:03:57.882 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 09:03:57.893 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
140 | 09:03:57.894 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:561: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
141 | 09:03:57.896 |  |  |  |  | MMICmd: Please provide user credentials: username and password
142 | 09:03:57.901 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
143 | 09:04:03.195 |  |  |  |  | →HTTP POST | IDMS-Endpoint
144 | 09:04:03.198 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
145 | 09:04:03.199 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 09:04:03.202 |  | ←enobeB PCAP frame← TCP |  |  |
147 | 09:04:03.202 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:566: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
148 | 09:04:03.205 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
149 | 09:04:03.231 | →enobeB PCAP frame→ TCP |  |  |  |
150 | 09:04:03.235 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
151 | 09:04:03.239 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 09:04:03.242 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 09:04:03.271 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 09:04:03.751 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 09:04:03.754 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 09:04:03.791 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 09:04:03.799 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
158 | 09:04:03.802 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
159 | 09:04:03.831 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 09:04:03.914 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
161 | 09:04:03.919 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 09:04:03.922 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 09:04:03.951 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 09:04:03.955 |  |  |  |  | →HTTP POST | IDMS-Endpoint
165 | 09:04:03.959 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
166 | 09:04:03.960 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
167 | 09:04:03.962 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 09:04:03.963 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:571: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
169 | 09:04:03.968 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
170 | 09:04:04.031 | →enobeB PCAP frame→ TCP |  |  |  |
171 | 09:04:04.391 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 09:04:04.394 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 09:04:04.431 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 09:04:04.439 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
175 | 09:04:04.442 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 09:04:04.446 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
177 | 09:04:04.471 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 09:04:04.476 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
179 | 09:04:04.479 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 09:04:04.482 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 09:04:04.483 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 09:04:04.517 |  |  |  |  | →HTTP POST | HTTP-Proxy
183 | 09:04:04.519 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
184 | 09:04:04.522 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 09:04:04.541 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:591: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
186 | 09:04:04.548 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
187 | 09:04:04.557 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
188 | 09:04:04.591 | →enobeB PCAP frame→ TCP |  |  |  |
189 | 09:04:04.631 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 09:04:04.634 |  | ←enobeB PCAP frame← TCP |  |  |
191 | 09:04:04.671 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 09:04:04.679 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
193 | 09:04:04.682 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 09:04:04.685 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
195 | 09:04:04.711 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 09:04:04.755 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
197 | 09:04:04.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
198 | 09:04:04.762 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 09:04:04.763 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
200 | 09:04:04.798 |  |  |  |  | →HTTP POST | HTTP-Proxy
201 | 09:04:04.799 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
202 | 09:04:04.800 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
203 | 09:04:04.802 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 09:04:04.803 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 09:04:04.860 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
206 | 09:04:04.860 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:595: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
207 | 09:04:04.868 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
208 | 09:04:04.869 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
209 | 09:04:04.911 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 09:04:04.951 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 09:04:04.958 |  |  |  |  | →SIP REGISTER | P-CSCF
212 | 09:04:04.959 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
213 | 09:04:04.981 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
214 | 09:04:05.011 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
215 | 09:04:05.013 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
216 | 09:04:05.019 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
217 | 09:04:05.027 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
218 | 09:04:05.758 |  |  |  |  | →SIP REGISTER | P-CSCF
219 | 09:04:05.759 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
220 | 09:04:05.784 |  |  |  |  | ←SIP 200 OK | P-CSCF
221 | 09:04:05.792 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
222 | 09:04:06.159 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 09:04:06.160 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 09:04:06.169 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
225 | 09:04:06.225 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 09:04:06.226 |  |  |  |  | MIKEY | Media-Server
227 | 09:04:06.233 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
228 | 09:04:06.440 |  |  |  |  | XML→ | Media-Server
229 | 09:04:06.441 |  |  |  |  | XML→ | Media-Server
230 | 09:04:06.444 |  |  |  |  | ←XML | Media-Server
231 | 09:04:06.448 |  |  |  |  | ←SIP NOTIFY | P-CSCF
232 | 09:04:06.456 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37835;transp... |  |  |
233 | 09:04:06.516 |  |  |  |  | →SIP 200 OK | P-CSCF
234 | 09:04:06.519 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
235 | 09:04:06.671 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 09:04:06.674 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 09:04:06.711 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 09:04:06.719 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 09:04:06.722 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 09:04:06.725 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 09:04:06.751 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 09:04:06.835 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
243 | 09:04:06.839 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
244 | 09:04:06.842 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
245 | 09:04:06.871 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 09:04:06.876 |  |  |  |  | →HTTP GET | HTTP-Proxy
247 | 09:04:06.879 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
248 | 09:04:06.882 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 09:04:06.884 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:731: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
250 | 09:04:06.892 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
251 | 09:04:06.900 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
252 | 09:04:06.947 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
253 | 09:04:06.951 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
254 | 09:04:06.954 |  | ←enobeB PCAP frame← TCP |  |  |
255 | 09:04:06.959 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 09:04:06.962 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 09:04:06.991 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 09:04:07.111 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 09:04:07.114 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 09:04:07.151 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 09:04:07.159 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
262 | 09:04:07.162 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 09:04:07.165 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
264 | 09:04:07.191 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 09:04:07.243 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
266 | 09:04:07.250 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 09:04:07.251 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
268 | 09:04:07.276 |  |  |  |  | →HTTP GET | HTTP-Proxy
269 | 09:04:07.282 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 09:04:07.288 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:736: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
271 | 09:04:07.335 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
272 | 09:04:07.349 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
273 | 09:04:07.350 |  | ←enobeB PCAP frame← TCP |  |  |
274 | 09:04:07.351 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 09:04:07.352 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
276 | 09:04:07.391 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 09:04:07.399 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 09:04:07.403 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
279 | 09:04:07.407 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 09:04:07.410 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 09:04:07.411 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 09:04:07.431 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 09:04:08.039 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
284 | 09:04:08.040 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
285 | 09:04:08.041 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
286 | 09:04:08.042 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
287 | 09:04:08.043 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
288 | 09:04:08.051 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
289 | 09:04:08.107 |  |  |  |  | ←SIP 200 OK | P-CSCF
290 | 09:04:08.107 |  |  |  |  | MIKEY | Media-Server
291 | 09:04:08.115 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
292 | 09:04:08.151 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 09:04:08.154 |  | ←enobeB PCAP frame← TCP |  |  |
294 | 09:04:08.191 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 09:04:08.199 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 09:04:08.202 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
297 | 09:04:08.231 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 09:04:08.314 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
299 | 09:04:08.319 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
300 | 09:04:08.319 |  |  |  |  | XML→ | Media-Server
301 | 09:04:08.320 |  |  |  |  | XML→ | Media-Server
302 | 09:04:08.322 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
303 | 09:04:08.323 |  |  |  |  | ←XML | Media-Server
304 | 09:04:08.326 |  |  |  |  | ←SIP NOTIFY | P-CSCF
305 | 09:04:08.334 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37835;transp... |  |  |
306 | 09:04:08.351 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 09:04:08.355 |  |  |  |  | →SIP 200 OK | P-CSCF
308 | 09:04:08.355 |  |  |  |  | →HTTP GET | HTTP-Proxy
309 | 09:04:08.357 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:741: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
310 | 09:04:08.359 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
311 | 09:04:08.362 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 09:04:08.364 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
313 | 09:04:08.372 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
314 | 09:04:08.373 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
315 | 09:04:08.431 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 09:04:08.435 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
317 | 09:04:08.439 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
318 | 09:04:08.442 |  | ←enobeB PCAP frame← TCP |  |  |
319 | 09:04:08.471 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 09:04:08.591 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 09:04:08.594 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 09:04:08.631 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 09:04:08.639 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
324 | 09:04:08.642 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 09:04:08.645 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
326 | 09:04:08.671 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 09:04:08.755 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
328 | 09:04:08.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
329 | 09:04:08.762 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 09:04:08.763 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
331 | 09:04:08.791 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 09:04:08.795 |  |  |  |  | →HTTP GET | HTTP-Proxy
333 | 09:04:08.799 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
334 | 09:04:08.802 |  | ←enobeB PCAP frame← TCP |  |  |
335 | 09:04:08.805 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:746: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
336 | 09:04:08.833 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
337 | 09:04:08.844 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
338 | 09:04:08.845 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
339 | 09:04:08.871 | →enobeB PCAP frame→ TCP |  |  |  |
340 | 09:04:08.911 | →enobeB PCAP frame→ TCP |  |  |  |
341 | 09:04:08.915 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
342 | 09:04:08.919 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
343 | 09:04:08.922 |  | ←enobeB PCAP frame← TCP |  |  |
344 | 09:04:08.951 | →enobeB PCAP frame→ TCP |  |  |  |
345 | 09:04:09.079 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
346 | 09:04:09.080 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
347 | 09:04:09.081 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
348 | 09:04:09.082 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
349 | 09:04:09.090 |  |  |  |  | →SIP PUBLISH | P-CSCF
350 | 09:04:09.137 |  |  |  |  | MIKEY | Media-Server
351 | 09:04:09.169 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
352 | 09:04:09.169 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
353 | 09:04:09.170 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
354 | 09:04:09.363 |  |  |  |  | XML→ | Media-Server
355 | 09:04:09.367 |  |  |  |  | ←SIP 200 OK | P-CSCF
356 | 09:04:09.370 |  |  |  |  | ←SIP 200 OK | P-CSCF
357 | 09:04:09.370 |  |  |  |  | MIKEY | Media-Server
358 | 09:04:09.374 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
359 | 09:04:09.378 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
360 | 09:04:09.571 |  |  |  |  | XML→ | Media-Server
361 | 09:04:09.572 |  |  |  |  | XML→ | Media-Server
363 | 09:04:09.607 |  |  |  |  | ←XML | Media-Server
364 | 09:04:09.612 |  |  |  |  | ←SIP NOTIFY | P-CSCF
365 | 09:04:09.621 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37835;transp... |  |  |
366 | 09:04:09.676 |  |  |  |  | →SIP 200 OK | P-CSCF
367 | 09:04:09.679 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
368 | 09:04:09.687 |  |  |  |  | ←XML | Media-Server
369 | 09:04:09.694 |  |  |  |  | ←SIP MESSAGE | P-CSCF
370 | 09:04:09.703 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
371 | 09:04:09.704 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
372 | 09:04:10.516 |  |  |  |  | →SIP 200 OK | P-CSCF
373 | 09:04:10.519 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
374 | 09:04:12.524 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
375 | 09:04:12.584 |  | ←RRC DCCH RRC Connection Release |  |  |
376 | 09:04:12.585 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
377 | 09:04:12.602 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
378 | 09:04:12.604 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1337: Test-Body Step 1
379 | 09:04:12.605 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
380 | 09:04:12.606 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT on-demand pre-arranged group call using Group A, automatic commencement mode, with implicit floor control
381 | 09:04:12.607 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1340: Test-Body Step 2
382 | 09:04:15.138 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
383 | 09:04:15.138 |  | →RRC CCCH RRC Connection Request |  |  |
384 | 09:04:15.138 |  | ←RRC CCCH RRC Connection Setup |  |  |
385 | 09:04:15.138 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
386 | 09:04:15.191 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
387 | 09:04:15.191 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
388 | 09:04:15.191 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
389 | 09:04:15.191 |  |  |  | →NAS EMM Service request |  |
390 | 09:04:15.191 |  |  |  | NAS K-enb 053723c60e93496f4aa5b91521f373d2a... |  |
391 | 09:04:15.192 |  |  | RRC K-enb 053723c60e93496f4aa5b91521f373d2a... |  |  |
392 | 09:04:15.193 |  |  | RRC rrc-cip 8be7036e15185441f1c8b6999cb5500... |  |  |
393 | 09:04:15.193 |  |  | RRC rrc-int e9c83f0ec5b38106fd1dd14b07a245a... |  |  |
394 | 09:04:15.193 |  |  | RRC up-cip 7dc467268263a9f5ff3033c0d1f8091c... |  |  |
395 | 09:04:15.193 |  |  | RRC up-int 2e1de1905193994314b42b9d6137e57b... |  |  |
396 | 09:04:15.193 |  | ←RRC DCCH Security Mode Command |  |  |
397 | 09:04:15.193 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
398 | 09:04:15.231 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
399 | 09:04:15.231 |  | →RRC DCCH Security Mode Complete |  |  |
400 | 09:04:15.231 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
401 | 09:04:15.231 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
402 | 09:04:15.279 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
403 | 09:04:15.288 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
404 | 09:04:15.288 |  |  |  |  | →SIP INVITE | P-CSCF
405 | 09:04:15.289 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
406 | 09:04:15.304 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: DD38CA444C8825D8F80CCB8C1FE41E84, Master Salt: 2F2063099A6F13B698E2B701, MKI: 25F6E13B
407 | 09:04:15.304 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
408 | 09:04:15.308 |  |  |  |  | XML→ | Media-Server
409 | 09:04:15.309 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
410 | 09:04:15.310 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl_MCPTT_MCVideo.ttcn:998: INVITE Verdict: Pass
411 | 09:04:15.311 |  |  |  |  | ←SIP 100 Trying | P-CSCF
412 | 09:04:15.315 |  |  |  |  | ←SIP 200 OK | P-CSCF
413 | 09:04:15.319 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
414 | 09:04:15.322 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
415 | 09:04:15.963 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
416 | 09:04:15.963 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
417 | 09:04:15.963 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
418 | 09:04:15.964 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
419 | 09:04:15.991 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
420 | 09:04:15.991 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
421 | 09:04:15.991 |  | →RRC DCCH UL Information Transfer |  |  |
422 | 09:04:15.991 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
423 | 09:04:15.991 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
424 | 09:04:16.088 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
425 | 09:04:16.196 |  |  |  |  | →SIP ACK | P-CSCF
426 | 09:04:16.199 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
427 | 09:04:16.205 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl_MCPTT_MCVideo.ttcn:1001: ACK Verdict: Pass
428 | 09:04:16.206 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1342: Step 2 Verdict: Pass
429 | 09:04:16.206 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1344: Test-Body Step 3
430 | 09:04:16.209 |  |  |  |  | ←Floor Granted | Media-Server
431 | 09:04:16.217 |  | ←enobeB PCAP frame← |  |  |
432 | 09:04:16.751 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
433 | 09:04:16.767 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 09:04:16.775 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
435 | 09:04:16.791 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
436 | 09:04:16.831 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 09:04:16.957 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1347: Test-Body Step 4
438 | 09:04:16.958 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1350: Test-Body Step 5
439 | 09:04:16.961 |  |  |  |  | ←Floor Taken | Media-Server
440 | 09:04:16.969 |  | ←enobeB PCAP frame← |  |  |
441 | 09:04:16.999 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
442 | 09:04:17.031 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
443 | 09:04:17.039 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
444 | 09:04:17.047 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
445 | 09:04:17.079 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
446 | 09:04:17.708 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1353: Test-Body Step 6
447 | 09:04:17.709 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1356: Test-Body Step 7
448 | 09:04:17.712 |  |  |  |  | ←Release MultiTalker | Media-Server
449 | 09:04:17.720 |  | ←enobeB PCAP frame← |  |  |
450 | 09:04:17.721 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
451 | 09:04:17.751 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
452 | 09:04:17.754 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
453 | 09:04:17.767 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
454 | 09:04:17.770 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
455 | 09:04:18.564 |  |  |  |  | MMICmd: Release call (hang up the call)
456 | 09:04:20.237 |  |  |  |  | →SIP BYE | P-CSCF
457 | 09:04:20.257 |  |  |  |  | ←SIP 200 OK | P-CSCF
458 | 09:04:20.265 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
459 | 09:04:20.791 | →enobeB PCAP frame→ |  |  |  |
460 | 09:04:22.255 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
461 | 09:04:22.267 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
462 | 09:04:22.267 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
463 | 09:04:22.267 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
464 | 09:04:22.268 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
465 | 09:04:22.311 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
466 | 09:04:22.311 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
467 | 09:04:22.311 |  | →RRC DCCH UL Information Transfer |  |  |
468 | 09:04:22.311 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
469 | 09:04:22.311 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
470 | 09:04:22.384 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
471 | 09:04:22.386 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
472 | 09:04:22.435 |  | ←RRC DCCH RRC Connection Release |  |  |
473 | 09:04:22.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
474 | 09:04:22.453 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
475 | 09:04:22.454 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1361: Step 9 Verdict: Pass
476 | 09:04:22.456 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
477 | 09:04:22.458 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
478 | 09:04:23.205 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.