ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:42:52.279 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:42:52.281 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:42:52.281 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:42:52.283 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:42:52.283 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:42:52.284 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:42:52.286 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:42:52.287 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:42:52.288 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8081 configured!
10 | 13:42:52.290 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:42:53.498 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:42:53.500 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:43:20.070 |  | ←RRC BCCH SIB |  |  |
14 | 13:43:20.075 |  | ←RRC BCCH SIB1 |  |  |
15 | 13:43:20.155 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:43:20.230 |  | ←RRC BCCH SIB |  |  |
17 | 13:43:20.235 |  | ←RRC BCCH SIB1 |  |  |
18 | 13:44:22.789 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:44:22.789 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:44:22.789 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:44:22.789 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:44:22.850 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:44:22.850 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:44:22.850 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:44:22.850 |  |  |  | →NAS EMM Attach request |  |
26 | 13:44:22.850 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:44:22.850 |  |  |  | NAS K-asme 74216c5f2f2c0dc18139b46af6b7c7bd... |  |
28 | 13:44:22.850 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:44:22.851 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:44:22.851 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:44:22.852 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:44:22.922 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:44:22.922 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:44:22.922 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:44:22.922 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:44:22.922 |  |  |  | NAS UE auth OK |  |
37 | 13:44:22.922 |  |  |  | NAS K-nas-cip cfaf82b61e2f54d0735ef2a47df5d... |  |
38 | 13:44:22.922 |  |  |  | NAS K-nas-int b64ec0b32535fb433b17a4815ac8c... |  |
39 | 13:44:22.922 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:44:22.923 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:44:22.923 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:44:22.924 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:44:22.962 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:44:22.962 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:44:22.962 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x7) |  |  |
46 | 13:44:22.962 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:44:22.962 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:44:22.963 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
49 | 13:44:22.963 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:44:22.964 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:44:22.972 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 13:44:23.010 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 13:44:23.010 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 13:44:23.010 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5e) |  |  |
55 | 13:44:23.010 |  |  |  | →NAS ESM ESM information response |  |
56 | 13:44:23.010 |  |  |  | NAS ← EMM Attach accept |  |
57 | 13:44:23.010 |  |  |  | NAS K-enb 294890acecfdd2472103e4df11de44a75... |  |
58 | 13:44:23.011 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 13:44:23.011 |  |  | RRC K-enb 294890acecfdd2472103e4df11de44a75... |  |  |
60 | 13:44:23.011 |  |  | RRC rrc-cip 03db835ac23bdf5f08873f65fcd991d... |  |  |
61 | 13:44:23.011 |  |  | RRC rrc-int b5b414574e2a37c4ba020669a7d333a... |  |  |
62 | 13:44:23.011 |  |  | RRC up-cip 0db12e3b794784b6a360f46c22847acc... |  |  |
63 | 13:44:23.011 |  |  | RRC up-int 10526c15a1e2ece25a37a257a4477a9b... |  |  |
64 | 13:44:23.012 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 13:44:23.042 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 13:44:23.042 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 13:44:23.042 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 13:44:23.042 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 13:44:23.092 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 13:44:23.092 |  | →RRC DCCH UE Capability Information |  |  |
71 | 13:44:23.092 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5e) |  |  |
72 | 13:44:23.092 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 13:44:23.092 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 13:44:23.122 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 13:44:23.122 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 13:44:23.162 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 13:44:23.162 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 13:44:23.162 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
79 | 13:44:23.162 |  |  |  | →NAS EMM Attach complete |  |
80 | 13:44:23.162 |  |  |  | NAS ← EMM EMM information |  |
81 | 13:44:23.163 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0x79) |  |  |
82 | 13:44:23.163 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 13:44:23.164 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer |  |  |
84 | 13:44:26.008 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 13:44:26.009 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 13:44:29.099 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 13:44:29.099 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 13:44:29.099 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 13:44:29.099 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 13:44:29.122 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 13:44:29.122 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 13:44:29.122 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 13:44:29.122 |  |  |  | →NAS EMM Service request |  |
94 | 13:44:29.122 |  |  |  | NAS K-enb eb0152e43ae50e17dc4407626f189c6bc... |  |
95 | 13:44:29.123 |  | ←RRC DCCH Security Mode Command |  |  |
96 | 13:44:29.123 |  |  | RRC K-enb eb0152e43ae50e17dc4407626f189c6bc... |  |  |
97 | 13:44:29.123 |  |  | RRC rrc-cip 407775a3476b9b41d6e2e69d898f56e... |  |  |
98 | 13:44:29.123 |  |  | RRC rrc-int 8aaf738fb188c6a3113adcfd977a796... |  |  |
99 | 13:44:29.123 |  |  | RRC up-cip 2550a7d25e5faf302a1a92cb7bf588ba... |  |  |
100 | 13:44:29.123 |  |  | RRC up-int ba61cd13c83d61d32cd1c2f84b88842a... |  |  |
101 | 13:44:29.124 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 13:44:29.162 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 13:44:29.162 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 13:44:29.162 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 13:44:29.162 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 13:44:29.202 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 13:44:29.202 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 13:45:03.242 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 13:45:03.245 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 13:45:03.282 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 13:45:03.330 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 13:45:03.333 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 13:45:03.335 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 13:45:03.362 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 13:45:03.490 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:45:03.493 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:45:03.493 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
118 | 13:45:03.494 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 13:45:03.522 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 13:45:03.570 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:45:03.572 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 13:45:03.573 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 13:45:03.579 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:323: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 13:45:03.597 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 13:45:03.601 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
126 | 13:45:03.602 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 13:45:03.642 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 13:45:03.682 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:45:05.802 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 13:45:05.805 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:45:05.842 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 13:45:05.850 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 13:45:05.853 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 13:45:05.858 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 13:45:05.882 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 13:45:06.210 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 13:45:06.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
138 | 13:45:06.213 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 13:45:06.218 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
140 | 13:45:06.242 | →enobeB PCAP frame→ TCP |  |  |  |
141 | 13:45:06.290 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
142 | 13:45:06.293 |  | ←enobeB PCAP frame← TCP |  |  |
143 | 13:45:06.293 |  |  |  |  | →HTTP GET | IDMS-Endpoint
144 | 13:45:06.309 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
145 | 13:45:06.310 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:561: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
146 | 13:45:06.311 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
147 | 13:45:06.311 |  |  |  |  | MMICmd: Please provide user credentials: username and password
148 | 13:45:06.402 | →enobeB PCAP frame→ TCP |  |  |  |
149 | 13:45:11.610 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
150 | 13:45:11.613 |  | ←enobeB PCAP frame← TCP |  |  |
151 | 13:45:11.614 |  |  |  |  | →HTTP POST | IDMS-Endpoint
152 | 13:45:11.622 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
153 | 13:45:11.623 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
154 | 13:45:11.626 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:566: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
155 | 13:45:11.642 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:45:11.650 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:45:11.652 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
158 | 13:45:11.653 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 13:45:11.682 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 13:45:12.162 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 13:45:12.165 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 13:45:12.202 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 13:45:12.250 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
164 | 13:45:12.253 |  | ←enobeB PCAP frame← TCP |  |  |
165 | 13:45:12.254 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 13:45:12.282 | →enobeB PCAP frame→ TCP |  |  |  |
167 | 13:45:12.379 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
168 | 13:45:12.381 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
169 | 13:45:12.490 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 13:45:12.491 |  |  |  |  | →HTTP POST | IDMS-Endpoint
171 | 13:45:12.493 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 13:45:12.499 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 13:45:12.502 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
174 | 13:45:12.502 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:571: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 13:45:12.522 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 13:45:12.882 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 13:45:12.885 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 13:45:12.922 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 13:45:12.930 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 13:45:12.933 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 13:45:12.936 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 13:45:12.962 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 13:45:13.010 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 13:45:13.013 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:45:13.013 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
186 | 13:45:13.014 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
187 | 13:45:13.050 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
188 | 13:45:13.051 |  |  |  |  | →HTTP POST | HTTP-Proxy
189 | 13:45:13.052 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 13:45:13.058 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 13:45:13.060 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
192 | 13:45:13.061 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
193 | 13:45:13.061 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:591: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
194 | 13:45:13.125 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:45:13.170 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 13:45:13.173 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 13:45:13.176 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 13:45:13.202 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 13:45:13.210 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 13:45:13.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
201 | 13:45:13.213 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 13:45:13.214 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 13:45:13.250 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 13:45:13.253 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 13:45:13.254 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 13:45:13.283 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
207 | 13:45:13.284 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:595: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
208 | 13:45:13.285 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
209 | 13:45:13.286 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
210 | 13:45:13.322 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 13:45:13.362 | →enobeB PCAP frame→ TCP |  |  |  |
212 | 13:45:13.410 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
213 | 13:45:13.414 |  |  |  |  | →SIP REGISTER | P-CSCF
214 | 13:45:13.437 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
215 | 13:45:13.463 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
216 | 13:45:13.464 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
217 | 13:45:13.470 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
218 | 13:45:13.472 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
219 | 13:45:14.170 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
220 | 13:45:14.175 |  |  |  |  | →SIP REGISTER | P-CSCF
221 | 13:45:14.198 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 13:45:14.201 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 13:45:14.530 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
224 | 13:45:14.531 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
225 | 13:45:14.532 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
226 | 13:45:14.540 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
227 | 13:45:14.552 |  |  |  |  | ←SIP 200 OK | P-CSCF
228 | 13:45:14.552 |  |  |  |  | MIKEY | Media-Server
229 | 13:45:14.554 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
230 | 13:45:14.746 |  |  |  |  | XML→ | Media-Server
231 | 13:45:14.748 |  |  |  |  | XML→ | Media-Server
232 | 13:45:14.751 |  |  |  |  | ←XML | Media-Server
233 | 13:45:14.754 |  |  |  |  | ←SIP NOTIFY | P-CSCF
234 | 13:45:14.756 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43081;transp... |  |  |
235 | 13:45:14.810 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
236 | 13:45:14.813 |  |  |  |  | →SIP 200 OK | P-CSCF
237 | 13:45:15.002 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 13:45:15.005 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 13:45:15.042 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:45:15.050 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 13:45:15.053 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 13:45:15.056 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 13:45:15.133 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 13:45:15.133 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
245 | 13:45:15.134 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 13:45:15.210 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 13:45:15.213 |  | ←enobeB PCAP frame← TCP |  |  |
248 | 13:45:15.213 |  |  |  |  | →HTTP GET | HTTP-Proxy
249 | 13:45:15.222 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:731: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.ue-config/users/sip:mcdata-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcdataue-configuration.xml
250 | 13:45:15.237 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
251 | 13:45:15.241 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
252 | 13:45:15.282 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 13:45:15.290 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 13:45:15.291 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
255 | 13:45:15.293 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 13:45:15.322 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 13:45:15.642 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 13:45:15.645 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 13:45:15.682 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 13:45:15.690 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 13:45:15.693 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 13:45:15.696 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 13:45:15.722 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 13:45:15.770 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 13:45:15.772 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
266 | 13:45:15.773 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
267 | 13:45:15.802 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 13:45:15.810 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcdat... |  |  |  |
269 | 13:45:15.811 |  |  |  |  | →HTTP GET | HTTP-Proxy
270 | 13:45:15.813 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 13:45:15.813 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:736: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.user-profile/users/sip:mcdata-userA-id@mcstaasting.com/mcdatauser-profile-49.xml
272 | 13:45:15.820 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
273 | 13:45:15.822 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
274 | 13:45:15.823 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
275 | 13:45:15.842 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 13:45:15.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
277 | 13:45:15.884 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
278 | 13:45:15.885 |  | ←enobeB PCAP frame← TCP |  |  |
279 | 13:45:15.890 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 13:45:15.893 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 13:45:15.922 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 13:45:16.610 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
283 | 13:45:16.611 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
284 | 13:45:16.619 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
285 | 13:45:16.631 |  |  |  |  | ←SIP 200 OK | P-CSCF
286 | 13:45:16.631 |  |  |  |  | MIKEY | Media-Server
287 | 13:45:16.633 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
288 | 13:45:16.642 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 13:45:16.645 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 13:45:16.682 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 13:45:16.690 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
292 | 13:45:16.693 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 13:45:16.811 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
294 | 13:45:16.813 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
295 | 13:45:16.820 |  |  |  |  | XML→ | Media-Server
296 | 13:45:16.821 |  |  |  |  | XML→ | Media-Server
297 | 13:45:16.824 |  |  |  |  | ←XML | Media-Server
298 | 13:45:16.826 |  |  |  |  | ←SIP NOTIFY | P-CSCF
299 | 13:45:16.828 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43081;transp... |  |  |
300 | 13:45:16.850 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 13:45:16.851 |  |  |  |  | →HTTP GET | HTTP-Proxy
302 | 13:45:16.853 |  | ←enobeB PCAP frame← TCP |  |  |
303 | 13:45:16.853 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:741: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.service-config/global/service-config.xml
304 | 13:45:16.855 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
305 | 13:45:16.857 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
306 | 13:45:16.858 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
307 | 13:45:16.875 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
308 | 13:45:16.877 |  |  |  |  | →SIP 200 OK | P-CSCF
309 | 13:45:16.922 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 13:45:16.924 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
311 | 13:45:16.925 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 13:45:16.931 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 13:45:16.934 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 13:45:16.962 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 13:45:17.002 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 13:45:17.005 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 13:45:17.042 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 13:45:17.050 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
319 | 13:45:17.053 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 13:45:17.056 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
321 | 13:45:17.082 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 13:45:17.130 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
323 | 13:45:17.133 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 13:45:17.133 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
325 | 13:45:17.135 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
326 | 13:45:17.170 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
327 | 13:45:17.173 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 13:45:17.173 |  |  |  |  | →HTTP GET | HTTP-Proxy
329 | 13:45:17.182 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:746: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
330 | 13:45:17.201 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
331 | 13:45:17.204 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
332 | 13:45:17.205 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
333 | 13:45:17.242 | →enobeB PCAP frame→ TCP |  |  |  |
334 | 13:45:17.250 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
335 | 13:45:17.251 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
336 | 13:45:17.253 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 13:45:17.282 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 13:45:17.290 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
339 | 13:45:17.291 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
340 | 13:45:17.292 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcdata-server-A@mcstaasting.com SIP/2.... SIP over IPSEC: PUBLISH sip:mcdata-server-A@mcstaasting.com SIP/2.... |  |  |  |
341 | 13:45:17.304 |  |  |  |  | →SIP PUBLISH | P-CSCF
342 | 13:45:17.348 |  |  |  |  | MIKEY | Media-Server
343 | 13:45:17.450 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
344 | 13:45:17.451 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
345 | 13:45:17.452 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
346 | 13:45:17.455 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
347 | 13:45:17.555 |  |  |  |  | XML→ | Media-Server
348 | 13:45:17.558 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 13:45:17.560 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
350 | 13:45:17.562 |  |  |  |  | ←SIP 200 OK | P-CSCF
351 | 13:45:17.562 |  |  |  |  | MIKEY | Media-Server
352 | 13:45:17.564 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
353 | 13:45:17.752 |  |  |  |  | XML→ | Media-Server
354 | 13:45:17.753 |  |  |  |  | XML→ | Media-Server
355 | 13:45:17.755 |  |  |  |  | Protected MCData Message | -
356 | 13:45:17.786 |  |  |  |  | ←XML | Media-Server
357 | 13:45:17.791 |  |  |  |  | ←SIP NOTIFY | P-CSCF
358 | 13:45:17.794 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43081;transp... |  |  |
359 | 13:45:17.850 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
360 | 13:45:17.852 |  |  |  |  | →SIP 200 OK | P-CSCF
361 | 13:45:17.856 |  |  |  |  | ←XML | Media-Server
362 | 13:45:17.869 |  |  |  |  | ←SIP MESSAGE | P-CSCF
363 | 13:45:17.873 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
364 | 13:45:17.874 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
365 | 13:45:17.875 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
366 | 13:45:18.650 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
367 | 13:45:18.653 |  |  |  |  | →SIP 200 OK | P-CSCF
368 | 13:45:20.662 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
369 | 13:45:20.715 |  | ←RRC DCCH RRC Connection Release |  |  |
370 | 13:45:20.716 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
371 | 13:45:20.736 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
372 | 13:45:20.737 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:348: Test-Body Step 1
373 | 13:45:20.739 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
374 | 13:45:20.739 |  |  |  |  | MMICmd: Make the MCDATA User request to send a group standalone SDS message with disposition request "DELIVERY"
375 | 13:45:20.740 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:351: Test-Body Step 2 - 2B
376 | 13:45:26.049 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
377 | 13:45:26.049 |  | →RRC CCCH RRC Connection Request |  |  |
378 | 13:45:26.049 |  | ←RRC CCCH RRC Connection Setup |  |  |
379 | 13:45:26.049 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
380 | 13:45:26.082 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
381 | 13:45:26.082 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
382 | 13:45:26.082 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
383 | 13:45:26.082 |  |  |  | →NAS EMM Service request |  |
384 | 13:45:26.082 |  |  |  | NAS K-enb 8f7113c28662fc9ee6592536e2d15fc9e... |  |
385 | 13:45:26.083 |  | ←RRC DCCH Security Mode Command |  |  |
386 | 13:45:26.083 |  |  | RRC K-enb 8f7113c28662fc9ee6592536e2d15fc9e... |  |  |
387 | 13:45:26.083 |  |  | RRC rrc-cip 36763c9037d8c3228fc4ab608532c89... |  |  |
388 | 13:45:26.083 |  |  | RRC rrc-int 80518fdcd325903f7072991696587ac... |  |  |
389 | 13:45:26.083 |  |  | RRC up-cip 419c08c9be3bf4ac38ab0e2334625e6f... |  |  |
390 | 13:45:26.083 |  |  | RRC up-int 3a39e66d15b3a85ce65d0f718cf7cd83... |  |  |
391 | 13:45:26.084 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
392 | 13:45:26.122 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
393 | 13:45:26.122 |  | →RRC DCCH Security Mode Complete |  |  |
394 | 13:45:26.122 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
395 | 13:45:26.122 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
396 | 13:45:26.162 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
397 | 13:45:26.162 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
398 | 13:45:26.170 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
399 | 13:45:26.171 | →enobeB PCAP frame→ SIP over IPSEC: MESSAGE sip:mcdata-server-A@mcstaasting.com SIP/2.... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
400 | 13:45:26.173 |  |  |  |  | →SIP MESSAGE | P-CSCF
401 | 13:45:26.179 |  |  |  |  | ←SIP 202 Accepted | P-CSCF
402 | 13:45:26.180 |  |  |  |  | XML→ | Media-Server
403 | 13:45:26.181 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 202 Accepted |  |  |
404 | 13:45:26.181 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:732: MIME part application/vnd.3gpp.mcdata-signalling 410062F248D400000000000180C8C9FFA78044C000000000000000002872E73D780038023000D79B0E39F3F922F625A8E87FC6E2CA834B22832D007BCCE72BABE111D2E9C7557671B3D0CE9BE7F07A93C7B3672EFD5158BC627A03
405 | 13:45:26.182 |  |  |  |  | Protected MCData Message | -
406 | 13:45:26.182 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:617: Decrypted payload: 01000019548D8006FA1D72D94FC3828C751C38255E37598C239D7CCC4DBBB842FA6F05641B8081
407 | 13:45:26.182 |  |  |  |  | MCData Message | -
408 | 13:45:26.182 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:732: MIME part application/vnd.3gpp.mcdata-payload 430062F248D4000000000001FCCD1DA53EFDBDC85E37596B102BA828000000407800230252E2E5F783F6C0F560A59D3DF2E9E7596E00070A4F9F38969CE7407B1492D1FD6887
409 | 13:45:26.182 |  |  |  |  | Protected MCData Message | -
410 | 13:45:26.182 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:617: Decrypted payload: 030178000D0154657374204D657373616765
411 | 13:45:26.182 |  |  |  |  | MCData Message | -
412 | 13:45:26.182 |  |  |  |  | Verdict PASS: MCData_SDS_MCX_IMS.ttcn:354: Step 2 Verdict: Pass
413 | 13:45:26.182 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:358: Test-Body Step 4
414 | 13:45:26.183 |  |  |  |  | ←XML | Media-Server
415 | 13:45:26.185 |  |  |  |  | MCData Message | -
416 | 13:45:26.185 |  |  |  |  | Protected MCData Message | -
417 | 13:45:26.189 |  |  |  |  | ←SIP MESSAGE | P-CSCF
418 | 13:45:26.192 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
419 | 13:45:26.193 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcdata-signalling |  |  |
420 | 13:45:26.290 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
421 | 13:45:26.293 |  |  |  |  | →SIP 200 OK | P-CSCF
422 | 13:45:26.300 |  |  |  |  | Verdict PASS: MCData_SDS_MCX_IMS.ttcn:362: Step 4 Verdict: Pass
423 | 13:45:28.302 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
424 | 13:45:28.346 |  | ←RRC DCCH RRC Connection Release |  |  |
425 | 13:45:28.347 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
426 | 13:45:28.370 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
427 | 13:45:28.371 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:368: Test-Body Step 6
428 | 13:45:29.122 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
429 | 13:45:29.124 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
430 | 13:45:29.872 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.