MSG #76 2022-08-09 13:44:23.162

    enobeB PCAP frame

    {
      "layers": {
        "frame": {
          "frame.encap_type": "45",
          "frame.time": "Aug  9, 2022 13:44:23.162399000 CEST",
          "frame.offset_shift": "0.000000000",
          "frame.time_epoch": "1660045463.162399000",
          "frame.time_delta": "0.007083000",
          "frame.time_delta_displayed": "0.040132000",
          "frame.time_relative": "63.047173000",
          "frame.number": "5550",
          "frame.len": "130",
          "frame.cap_len": "130",
          "frame.marked": "0",
          "frame.ignored": "0",
          "frame.protocols": "user_dlt:mac-lte-framed:mac-lte:rlc-lte:pdcp-lte:lte_rrc:nas-eps"
        },
        "user_dlt": "DLT: 147, Payload: mac-lte-framed (mac-lte-framed)",
        "mac-lte": {
          "mac-lte.context": "",
          "mac-lte.context_tree": {
            "mac-lte.radio-type": "1",
            "mac-lte.direction": "0",
            "mac-lte.ueid": "797",
            "mac-lte.sfn": "628",
            "mac-lte.subframe": "8",
            "mac-lte.rnti": "857",
            "mac-lte.rnti-type": "3",
            "mac-lte.is-predefined-frame": "0",
            "mac-lte.length": "105",
            "mac-lte.ul-grant-size": "105",
            "mac-lte.crc-status": "1",
            "mac-lte.carrier-id": "0",
            "mac-lte.ul-tti-count": "1"
          },
          "mac-lte.ul-phy": "",
          "mac-lte.ul-phy_tree": {
            "mac-lte.ul-phy.modulation-type": "4",
            "mac-lte.ul-phy.tbs-index": "19",
            "mac-lte.ul-phy.resource-block-length": "2",
            "mac-lte.ul-phy.resource-block-start": "91",
            "mac-lte.ul-phy.harq-id": "0",
            "mac-lte.ul-phy.ndi": "0"
          },
          "mac-lte.ulsch.header": "",
          "mac-lte.ulsch.header_tree": {
            "mac-lte.sch.subheader": "",
            "mac-lte.sch.subheader_tree": {
              "mac-lte.sch.reserved": "0x00",
              "mac-lte.sch.format2": "0",
              "mac-lte.sch.extended": "0x00",
              "mac-lte.ulsch.lcid": "0x1f"
            }
          },
          "mac-lte.control.bsr": "",
          "mac-lte.control.bsr_tree": {
            "mac-lte.control.bsr.lcg-id": "0",
            "mac-lte.control.bsr.buffer-size": "0"
          },
          "mac-lte.sch.header-only": "0",
          "mac-lte.sch.sdu": "a0:00:00:16:bc:47:51:97:14:c7:09:58:cd:35:e6:69:25:9a:9c:23:b4:e3:d9",
          "rlc-lte": {
            "rlc-lte.context": "",
            "rlc-lte.context_tree": {
              "rlc-lte.direction": "0",
              "rlc-lte.mode": "4",
              "rlc-lte.ueid": "797",
              "rlc-lte.channel-type": "4",
              "rlc-lte.channel-id": "2",
              "rlc-lte.pdu-length": "23",
              "rlc-lte.am-seqnum-length": "10"
            },
            "rlc-lte.am": "",
            "rlc-lte.am.header": "",
            "rlc-lte.am.header_tree": {
              "rlc-lte.am.frame-type": "0x01",
              "rlc-lte.am.rf": "0x00",
              "rlc-lte.am.p": "0x01",
              "rlc-lte.am.fi": "0x00",
              "rlc-lte.am.fixed.e": "0x00",
              "rlc-lte.am.fixed.sn": "0"
            },
            "rlc-lte.sequence-analysis": "",
            "rlc-lte.sequence-analysis_tree": {
              "rlc-lte.sequence-analysis.ok": "1"
            },
            "rlc-lte.am.data": "00:16:bc:47:51:97:14:c7:09:58:cd:35:e6:69:25:9a:9c:23:b4:e3:d9",
            "pdcp-lte": {
              "pdcp-lte.configuration": "",
              "pdcp-lte.configuration_tree": {
                "pdcp-lte.direction": "0",
                "pdcp-lte.plane": "1",
                "pdcp-lte.ueid": "797",
                "pdcp-lte.channel-type": "1",
                "pdcp-lte.channel-id": "2",
                "pdcp-lte.rohc.compression": "0"
              },
              "pdcp-lte.security-config": "",
              "pdcp-lte.security-config_tree": {
                "pdcp-lte.security-config.setup-frame": "5528",
                "pdcp-lte.security-config.ciphering": "2",
                "pdcp-lte.security-config.integrity": "2",
                "pdcp-lte.security-config.bearer": "1",
                "pdcp-lte.security-config.direction": "0",
                "pdcp-lte.security-config.count": "0",
                "pdcp-lte.security-config.cipher-key": "03db835ac23bdf5f08873f65fcd991d0",
                "pdcp-lte.security-config.integrity-key": "b5b414574e2a37c4ba020669a7d333a5"
              },
              "pdcp-lte.reserved": "0",
              "pdcp-lte.seq-num": "0",
              "pdcp-lte.sequence-analysis": "",
              "pdcp-lte.sequence-analysis_tree": {
                "pdcp-lte.sequence-analysis.expected-sn": "0",
                "pdcp-lte.sequence-analysis.ok": "1"
              },
              "lte_rrc": {
                "lte_rrc": "LTE Radio Resource Control (RRC) protocol",
                "lte-rrc.UL_DCCH_Message_element": {
                  "per.choice_index": "0",
                  "lte-rrc.uL_DCCH_Message.message": "0",
                  "lte-rrc.uL_DCCH_Message.message_tree": {
                    "per.choice_index": "9",
                    "lte-rrc.c1": "9",
                    "lte-rrc.c1_tree": {
                      "lte-rrc.ulInformationTransfer_element": {
                        "per.choice_index": "0",
                        "lte-rrc.criticalExtensions": "0",
                        "lte-rrc.criticalExtensions_tree": {
                          "per.choice_index": "0",
                          "lte-rrc.c1": "0",
                          "lte-rrc.c1_tree": {
                            "lte-rrc.ulInformationTransfer_r8_element": {
                              "per.optional_field_bit": "0",
                              "per.choice_index": "0",
                              "lte-rrc.dedicatedInfoType": "0",
                              "lte-rrc.dedicatedInfoType_tree": {
                                "per.octet_string_length": "13",
                                "lte-rrc.dedicatedInfoNAS": "27:88:93:6e:dd:02:9a:aa:18:f8:23:f8:8f",
                                "lte-rrc.dedicatedInfoNAS_tree": {
                                  "nas-eps": {
                                    "nas_eps.security_header_type": "2",
                                    "gsm_a.L3_protocol_discriminator": "0x07",
                                    "nas_eps.msg_auth_code": "0x88936edd",
                                    "nas_eps.seq_no": "2",
                                    "nas_eps.ciphered_msg": "9a:aa:18:f8:23:f8:8f"
                                  }
                                }
                              }
                            }
                          }
                        }
                      }
                    }
                  }
                }
              },
              "pdcp-lte.mac": "0x4c9b7f50"
            }
          },
          "mac-lte.padding-data": "00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00",
          "mac-lte.padding-length": "77"
        },
        "mac-lte.ulsch": "",
        "_ws.lua.fake": "",
        "nas_eea2": {
          "nas-eps": {
            "nas_eps.security_header_type": "0",
            "gsm_a.L3_protocol_discriminator": "0x07",
            "nas_eps.msg_auth_code": "0x88936edd",
            "nas_eps.seq_no": "2",
            "nas_eps.nas_msg_emm_type": "0x43",
            "ESM message container": {
              "gsm_a.len": "3",
              "nas_eps.emm.esm_msg_cont": "52:00:c2",
              "nas_eps.emm.esm_msg_cont_tree": {
                "nas_eps.bearer_id": "5",
                "gsm_a.L3_protocol_discriminator": "0x02",
                "nas_eps.esm.proc_trans_id": "0",
                "nas_eps.nas_msg_esm_type": "0xc2"
              }
            }
          }
        },
        "_ws.col.Info": "ULInformationTransfer, Ciphered message",
        "_ws.col.Protocol": "LTE RRC UL_DCCH/NAS-EPS/NAS-EPS"
      }
    }