MSG #55 2023-06-16 16:40:04.567
NAS

     ESM: ESM information response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x195f8de8
    Sequence number = 0x01
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 0
    Procedure transaction identity = 6
    Message type = 0xda (ESM information response)
    Access point name = "MCSTaaStingDefault"