MSG #28 2023-06-16 16:40:04.415
NAS

     EMM: Authentication request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xf60f334b
    Sequence number = 0x06
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x52 (Authentication request)
    NAS key set identifier:
      TSC = 0
      NAS key set identifier = 2
    Authentication parameter RAND:
      Data = ac ea e1 7b 7b f2 42 76 de ee 6c 85 ed 6c f7 f6
    Authentication parameter AUTN:
      Length = 16
      Data = b5 53 5f 5d c3 36 90 01 d1 58 f2 83 7d 43 b2 55