ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 16:39:51.483 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 16:39:51.484 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 16:39:51.485 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 16:39:51.486 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 16:39:51.487 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 16:39:51.487 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:829: IMS UDP port 192.168.16.111:5060 configured
7 | 16:39:51.489 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:779: IMS TCP port 192.168.16.111:5060 configured!
8 | 16:39:51.491 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:800: Http Proxy (CMS, KMS, GMS) at port 192.168.16.111:8100 configured!
9 | 16:39:51.492 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:811: IdM port 192.168.16.111:8080 configured!
10 | 16:39:51.494 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 16:39:52.694 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 16:39:52.697 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 16:39:56.560 |  | ←RRC BCCH SIB1 |  |  |
14 | 16:39:56.635 |  | ←RRC BCCH SIB |  |  |
15 | 16:39:56.640 |  | ←RRC BCCH SIB1 |  |  |
16 | 16:39:56.655 |  | ←RRC BCCH SIB |  |  |
17 | 16:39:56.675 |  | ←RRC BCCH SIB |  |  |
18 | 16:40:04.363 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 16:40:04.363 |  | →RRC CCCH RRC connection request |  |  |
20 | 16:40:04.363 |  | ←RRC CCCH RRC connection setup |  |  |
21 | 16:40:04.363 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 16:40:04.415 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 16:40:04.415 |  | →RRC DCCH RRC connection setup complete |  |  |
24 | 16:40:04.415 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 16:40:04.415 |  |  |  | →NAS EMM Attach request |  |
26 | 16:40:04.415 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 16:40:04.415 |  |  |  | NAS K-asme c39b3dedd8106253d382c8ac296e307f... |  |
28 | 16:40:04.415 |  |  |  | NAS ← EMM Authentication request |  |
29 | 16:40:04.416 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
30 | 16:40:04.416 |  | ←RRC DCCH DL information transfer |  |  |
31 | 16:40:04.417 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
32 | 16:40:04.487 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer |  |  |  |
33 | 16:40:04.487 |  | →RRC DCCH UL information transfer |  |  |
34 | 16:40:04.487 |  | [EMBEDDED NAS IN PREV RRC] ESM Unknown message (type=0xec) |  |  |
35 | 16:40:04.487 |  |  |  | →NAS EMM Authentication response |  |
36 | 16:40:04.487 |  |  |  | NAS UE auth OK |  |
37 | 16:40:04.487 |  |  |  | NAS 3GPP ctx tx_nas_count=0 rx_nas_count=16... |  |
38 | 16:40:04.487 |  |  |  | NAS K-nas-cip e71eff4c73ebf3b27139887fa524c... |  |
39 | 16:40:04.487 |  |  |  | NAS K-nas-int fed57fef20c2d64a66c3455ad1b1d... |  |
40 | 16:40:04.487 |  |  |  | NAS ← EMM Security mode command |  |
41 | 16:40:04.488 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
42 | 16:40:04.488 |  | ←RRC DCCH DL information transfer |  |  |
43 | 16:40:04.489 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 16:40:04.527 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 16:40:04.527 |  | →RRC DCCH UL information transfer |  |  |
46 | 16:40:04.527 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
47 | 16:40:04.527 |  |  |  | →NAS EMM Security mode complete |  |
48 | 16:40:04.527 |  |  |  | NAS ← ESM ESM information request |  |
49 | 16:40:04.528 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
50 | 16:40:04.528 |  | ←RRC DCCH DL information transfer |  |  |
51 | 16:40:04.529 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 16:40:04.567 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 16:40:04.567 |  | →RRC DCCH UL information transfer |  |  |
54 | 16:40:04.567 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
55 | 16:40:04.567 |  |  |  | →NAS ESM ESM information response |  |
56 | 16:40:04.567 |  |  |  | NAS ← EMM Attach accept |  |
57 | 16:40:04.567 |  |  |  | NAS K-enb 7b2fcf374b4c8d764887814cdd41c74c7... |  |
58 | 16:40:04.567 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
59 | 16:40:04.568 |  | ←RRC DCCH Security mode command |  |  |
60 | 16:40:04.568 |  |  | RRC K-enb 7b2fcf374b4c8d764887814cdd41c74c7... |  |  |
61 | 16:40:04.568 |  |  | RRC rrc-cip 385c5136f0e2b35a3b60c13525e3bef... |  |  |
62 | 16:40:04.568 |  |  | RRC rrc-int a02bf2653f069a8f94c02b02de324bb... |  |  |
63 | 16:40:04.568 |  |  | RRC up-cip 5ee3b1703d91d2766370c6c7a6b09179... |  |  |
64 | 16:40:04.568 |  |  | RRC up-int 84b6ccb3f78121ee82d696dc160dad04... |  |  |
65 | 16:40:04.569 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 16:40:04.607 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 16:40:04.607 |  | →RRC DCCH Security mode complete |  |  |
68 | 16:40:04.607 |  | ←RRC DCCH UE capability enquiry |  |  |
69 | 16:40:04.607 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 16:40:04.655 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 16:40:04.655 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
72 | 16:40:04.655 |  | →RRC DCCH UE capability information |  |  |
73 | 16:40:04.655 |  |  | RRC EUTRA band combinations |  |  |
74 | 16:40:04.655 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
75 | 16:40:04.655 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
76 | 16:40:04.687 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
77 | 16:40:04.687 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
78 | 16:40:04.727 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM data transport[Malformed Packet] |  |  |  |
79 | 16:40:04.727 |  | →RRC DCCH UL information transfer |  |  |
80 | 16:40:04.727 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM data transport |  |  |
81 | 16:40:04.727 |  |  |  | →NAS EMM Attach complete |  |
82 | 16:40:04.727 |  |  |  | NAS ← EMM EMM information |  |
83 | 16:40:04.728 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
84 | 16:40:04.728 |  | ←RRC DCCH DL information transfer |  |  |
85 | 16:40:04.729 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
86 | 16:40:09.664 |  | ←RRC DCCH RRC connection release |  |  |
87 | 16:40:09.665 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
88 | 16:40:20.953 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
89 | 16:40:20.953 |  | →RRC CCCH RRC connection request |  |  |
90 | 16:40:20.953 |  | ←RRC CCCH RRC connection setup |  |  |
91 | 16:40:20.953 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
92 | 16:40:21.007 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
93 | 16:40:21.007 |  | →RRC DCCH RRC connection setup complete |  |  |
94 | 16:40:21.007 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
95 | 16:40:21.007 |  |  |  | →NAS EMM Service request |  |
96 | 16:40:21.007 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
97 | 16:40:21.007 |  |  |  | NAS K-enb 466b187678c7780e7508ec0c1a3651b46... |  |
98 | 16:40:21.007 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
99 | 16:40:21.008 |  |  | RRC K-enb 466b187678c7780e7508ec0c1a3651b46... |  |  |
100 | 16:40:21.008 |  |  | RRC EUTRA band combinations |  |  |
101 | 16:40:21.008 |  |  | RRC rrc-cip 68f725893b5da4892a0dc1d9b44e248... |  |  |
102 | 16:40:21.008 |  |  | RRC rrc-int 24ba28143b841133333873deee50b1b... |  |  |
103 | 16:40:21.008 |  |  | RRC up-cip cc8d7a8223bbb44070e9d89267226079... |  |  |
104 | 16:40:21.008 |  |  | RRC up-int 4162f4954e5c0635e12cdf533ea3f797... |  |  |
105 | 16:40:21.008 |  | ←RRC DCCH Security mode command |  |  |
106 | 16:40:21.009 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
107 | 16:40:21.047 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
108 | 16:40:21.047 |  | →RRC DCCH Security mode complete |  |  |
109 | 16:40:21.047 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
110 | 16:40:21.047 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
111 | 16:40:21.087 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
112 | 16:40:21.087 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
113 | 16:40:21.089 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 16:40:21.127 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 16:40:21.135 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 16:40:21.137 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 16:40:21.145 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 16:40:21.167 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 16:40:21.207 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
120 | 16:40:21.211 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
121 | 16:40:21.215 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 16)
122 | 16:40:21.247 | →enobeB PCAP frame→ TCP |  |  |  |
123 | 16:40:21.255 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
124 | 16:40:21.261 |  |  |  |  | →HTTP GET | HTTP-Proxy
125 | 16:40:21.267 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:349: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
126 | 16:40:21.277 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 16:40:21.278 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
128 | 16:40:21.327 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 16:40:22.007 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 16:40:22.009 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 16:40:22.047 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 16:40:22.055 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 16:40:22.057 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 16:40:22.060 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 16:40:22.087 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 16:40:22.207 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 16:40:22.210 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 16:40:22.213 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
139 | 16:40:22.247 | →enobeB PCAP frame→ TCP |  |  |  |
140 | 16:40:22.255 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
141 | 16:40:22.257 |  | ←enobeB PCAP frame← TCP |  |  |
142 | 16:40:22.260 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
143 | 16:40:22.260 |  |  |  |  | →HTTP GET | IDMS-Endpoint
144 | 16:40:22.262 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
145 | 16:40:22.267 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:602: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
146 | 16:40:22.267 |  |  |  |  | MMICmd: Please provide user credentials: username and password
147 | 16:40:22.327 | →enobeB PCAP frame→ TCP |  |  |  |
148 | 16:40:29.185 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 16:40:29.191 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 16:40:29.195 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 16:40:29.197 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
152 | 16:40:29.201 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:607: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 16:40:29.209 |  | ←enobeB PCAP frame← TCP |  |  |
154 | 16:40:29.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:698: IdM port - Client closed the connection (id 18)
155 | 16:40:29.407 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 16:40:29.409 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 16:40:29.447 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 16:40:29.455 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
159 | 16:40:29.457 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 16:40:29.459 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 16:40:29.487 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 16:40:29.527 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 16:40:29.529 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 16:40:29.532 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
165 | 16:40:29.575 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
166 | 16:40:29.580 |  |  |  |  | →HTTP POST | IDMS-Endpoint
167 | 16:40:29.582 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
168 | 16:40:29.585 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
169 | 16:40:29.589 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:612: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
170 | 16:40:29.647 | →enobeB PCAP frame→ TCP |  |  |  |
171 | 16:40:29.727 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 16:40:29.729 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 16:40:29.767 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 16:40:29.775 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
175 | 16:40:29.777 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 16:40:29.778 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
177 | 16:40:29.807 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 16:40:29.815 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 16:40:29.817 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 16:40:29.821 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 19)
181 | 16:40:29.865 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 16:40:29.871 |  |  |  |  | →HTTP POST | HTTP-Proxy
183 | 16:40:29.891 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
184 | 16:40:29.891 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:631: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
185 | 16:40:29.892 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
186 | 16:40:29.929 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 16:40:29.975 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
188 | 16:40:29.977 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 16:40:29.979 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
190 | 16:40:30.007 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 16:40:30.015 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
192 | 16:40:30.018 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
193 | 16:40:30.021 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 20)
194 | 16:40:30.065 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 16:40:30.069 |  |  |  |  | →HTTP POST | HTTP-Proxy
196 | 16:40:30.102 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
197 | 16:40:30.105 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
198 | 16:40:30.107 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:634: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
199 | 16:40:30.175 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
200 | 16:40:30.181 |  |  |  |  | →SIP REGISTER | P-CSCF
201 | 16:40:30.187 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:838: IMS UDP_s port 192.168.16.111:5062 configured
202 | 16:40:30.204 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:789: IMS TCP_s port 192.168.16.111:5062 configured!
203 | 16:40:30.205 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
204 | 16:40:30.205 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:847: IMS UDP_c port 192.168.16.111:5061 configured
205 | 16:40:30.207 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
206 | 16:40:30.313 |  |  |  |  | →SIP REGISTER | P-CSCF
207 | 16:40:30.333 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
208 | 16:40:30.335 |  |  |  |  | ←SIP 200 OK | P-CSCF
209 | 16:40:30.610 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
210 | 16:40:30.640 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
211 | 16:40:30.643 |  |  |  |  | ←SIP 200 OK | P-CSCF
212 | 16:40:30.647 |  |  |  |  | MIKEY | Media-Server
213 | 16:40:30.939 |  |  |  |  | XML→ | Media-Server
214 | 16:40:30.944 |  |  |  |  | ←XML | Media-Server
215 | 16:40:30.945 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... |  |  |
216 | 16:40:30.947 |  |  |  |  | ←SIP NOTIFY | P-CSCF
217 | 16:40:30.981 |  |  |  |  | →SIP 200 OK | P-CSCF
218 | 16:40:31.049 |  | ←enobeB PCAP frame← TCP |  |  |
219 | 16:40:31.087 | →enobeB PCAP frame→ TCP |  |  |  |
220 | 16:40:31.095 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
221 | 16:40:31.097 |  | ←enobeB PCAP frame← TCP |  |  |
222 | 16:40:31.102 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
223 | 16:40:31.127 | →enobeB PCAP frame→ TCP |  |  |  |
224 | 16:40:31.167 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
225 | 16:40:31.170 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
226 | 16:40:31.174 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
227 | 16:40:31.215 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
228 | 16:40:31.222 |  |  |  |  | →HTTP GET | HTTP-Proxy
229 | 16:40:31.228 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:815: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
230 | 16:40:31.233 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
231 | 16:40:31.234 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
232 | 16:40:31.247 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
233 | 16:40:31.287 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 16:40:31.289 |  | ←enobeB PCAP frame← TCP |  |  |
235 | 16:40:31.293 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
236 | 16:40:31.327 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 16:40:31.367 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 16:40:31.369 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 16:40:31.407 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 16:40:31.415 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 16:40:31.417 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 16:40:31.427 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 16:40:31.447 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 16:40:31.487 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 16:40:31.490 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 16:40:31.494 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
247 | 16:40:31.535 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
248 | 16:40:31.543 |  |  |  |  | →HTTP GET | HTTP-Proxy
249 | 16:40:31.550 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:820: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
250 | 16:40:31.561 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
251 | 16:40:31.562 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
252 | 16:40:31.562 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
253 | 16:40:31.607 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 16:40:31.615 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 16:40:31.647 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 16:40:31.649 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 16:40:31.650 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 16:40:31.653 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
259 | 16:40:31.687 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 16:40:32.090 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
261 | 16:40:32.120 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
262 | 16:40:32.122 |  |  |  |  | ←SIP 200 OK | P-CSCF
263 | 16:40:32.125 |  |  |  |  | MIKEY | Media-Server
264 | 16:40:32.129 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 16:40:32.175 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
266 | 16:40:32.177 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 16:40:32.178 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
268 | 16:40:32.207 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 16:40:32.247 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 16:40:32.249 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
271 | 16:40:32.252 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
272 | 16:40:32.295 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 16:40:32.300 |  |  |  |  | →HTTP GET | HTTP-Proxy
274 | 16:40:32.301 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:825: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
275 | 16:40:32.303 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
276 | 16:40:32.304 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
277 | 16:40:32.327 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 16:40:32.367 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 16:40:32.369 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 16:40:32.372 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
281 | 16:40:32.407 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 16:40:32.434 |  |  |  |  | XML→ | Media-Server
283 | 16:40:32.439 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... |  |  |
284 | 16:40:32.439 |  |  |  |  | ←XML | Media-Server
285 | 16:40:32.441 |  |  |  |  | ←SIP NOTIFY | P-CSCF
286 | 16:40:32.495 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
287 | 16:40:32.501 |  |  |  |  | →SIP 200 OK | P-CSCF
288 | 16:40:32.713 |  | ←enobeB PCAP frame← TCP |  |  |
289 | 16:40:32.718 |  |  |  |  | →SIP PUBLISH | P-CSCF
290 | 16:40:32.726 |  |  |  |  | MIKEY | Media-Server
291 | 16:40:32.777 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 16:40:32.778 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 16:40:32.847 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
294 | 16:40:32.849 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
295 | 16:40:32.852 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
296 | 16:40:32.895 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
297 | 16:40:32.900 |  |  |  |  | →HTTP GET | HTTP-Proxy
298 | 16:40:32.902 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:830: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
299 | 16:40:32.903 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
300 | 16:40:32.904 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
301 | 16:40:32.927 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 16:40:32.967 | →enobeB PCAP frame→ TCP |  |  |  |
303 | 16:40:32.969 |  | ←enobeB PCAP frame← TCP |  |  |
304 | 16:40:32.972 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
305 | 16:40:33.007 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 16:40:33.020 |  |  |  |  | XML→ | Media-Server
307 | 16:40:33.021 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
308 | 16:40:33.023 |  |  |  |  | ←SIP 200 OK | P-CSCF
309 | 16:40:33.081 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
310 | 16:40:33.090 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
311 | 16:40:33.092 |  |  |  |  | ←SIP 200 OK | P-CSCF
312 | 16:40:33.096 |  |  |  |  | MIKEY | Media-Server
313 | 16:40:33.390 |  |  |  |  | XML→ | Media-Server
314 | 16:40:33.393 |  |  |  |  | Protected MCData Message | -
315 | 16:40:33.440 |  |  |  |  | ←XML | Media-Server
316 | 16:40:33.441 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... |  |  |
317 | 16:40:33.443 |  |  |  |  | ←SIP NOTIFY | P-CSCF
318 | 16:40:33.501 |  |  |  |  | →SIP 200 OK | P-CSCF
319 | 16:40:33.508 |  |  |  |  | ←XML | Media-Server
320 | 16:40:33.528 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
321 | 16:40:33.530 |  |  |  |  | ←SIP MESSAGE | P-CSCF
322 | 16:40:33.862 |  |  |  |  | →SIP 200 OK | P-CSCF
323 | 16:40:35.869 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
324 | 16:40:35.908 |  | ←RRC DCCH RRC connection release |  |  |
325 | 16:40:35.909 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
326 | 16:40:35.923 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
327 | 16:40:35.924 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:464: Test-Body Step 1
328 | 16:40:35.925 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request to determine the current status of a functional alias and later notification of status changes of a functional alias
329 | 16:40:35.927 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
330 | 16:41:08.563 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
331 | 16:41:08.563 |  | →RRC CCCH RRC connection request |  |  |
332 | 16:41:08.563 |  | ←RRC CCCH RRC connection setup |  |  |
333 | 16:41:08.563 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
334 | 16:41:08.607 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
335 | 16:41:08.607 |  | →RRC DCCH RRC connection setup complete |  |  |
336 | 16:41:08.607 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
337 | 16:41:08.607 |  |  |  | →NAS EMM Service request |  |
338 | 16:41:08.607 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
339 | 16:41:08.607 |  |  |  | NAS K-enb 5e9006fb7bb252e5623564b07449869b0... |  |
340 | 16:41:08.607 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
341 | 16:41:08.608 |  |  | RRC K-enb 5e9006fb7bb252e5623564b07449869b0... |  |  |
342 | 16:41:08.608 |  |  | RRC EUTRA band combinations |  |  |
343 | 16:41:08.608 |  |  | RRC rrc-cip ee6d5dd2f2ed3a096c7d125ec553df2... |  |  |
344 | 16:41:08.608 |  |  | RRC rrc-int ace1f02296dc49f56f92423bd5dc769... |  |  |
345 | 16:41:08.608 |  |  | RRC up-cip 214da8782fb56ef112601ee24892bfa3... |  |  |
346 | 16:41:08.608 |  |  | RRC up-int ada5db5daafa4d15c7c24a7903244e30... |  |  |
347 | 16:41:08.608 |  | ←RRC DCCH Security mode command |  |  |
348 | 16:41:08.609 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
349 | 16:41:08.647 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
350 | 16:41:08.647 |  | →RRC DCCH Security mode complete |  |  |
351 | 16:41:08.647 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
352 | 16:41:08.647 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
353 | 16:41:08.687 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
354 | 16:41:08.687 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
355 | 16:41:08.710 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
356 | 16:41:08.713 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
357 | 16:41:08.715 |  |  |  |  | ←SIP 200 OK | P-CSCF
358 | 16:41:08.717 |  |  |  |  | XML→ | Media-Server
359 | 16:41:08.718 |  |  |  |  | ←XML | Media-Server
360 | 16:41:08.720 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
361 | 16:41:08.722 |  |  |  |  | ←SIP NOTIFY | P-CSCF
362 | 16:41:08.780 |  |  |  |  | →SIP 200 OK | P-CSCF
363 | 16:41:10.783 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
364 | 16:41:10.811 |  | ←RRC DCCH RRC connection release |  |  |
365 | 16:41:10.812 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
366 | 16:41:10.826 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
367 | 16:41:10.826 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:466: Step 1 Verdict: Pass
368 | 16:41:10.827 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:468: Test-Body Step 2
369 | 16:41:10.828 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request to change the status of a functional alias to 'activated'
370 | 16:41:10.828 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
371 | 16:41:13.793 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
372 | 16:41:13.793 |  | →RRC CCCH RRC connection request |  |  |
373 | 16:41:13.793 |  | ←RRC CCCH RRC connection setup |  |  |
374 | 16:41:13.793 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
375 | 16:41:13.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
376 | 16:41:13.847 |  | →RRC DCCH RRC connection setup complete |  |  |
377 | 16:41:13.847 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
378 | 16:41:13.847 |  |  |  | →NAS EMM Service request |  |
379 | 16:41:13.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
380 | 16:41:13.847 |  |  |  | NAS K-enb cdf00f142db6a70622e4bafc9e6ee193d... |  |
381 | 16:41:13.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
382 | 16:41:13.848 |  |  | RRC K-enb cdf00f142db6a70622e4bafc9e6ee193d... |  |  |
383 | 16:41:13.848 |  |  | RRC EUTRA band combinations |  |  |
384 | 16:41:13.848 |  |  | RRC rrc-cip 7a27bb5b2b1394f13c4c101b006864e... |  |  |
385 | 16:41:13.848 |  |  | RRC rrc-int afe58fa98e0d75b10fa6febe4a4198b... |  |  |
386 | 16:41:13.848 |  |  | RRC up-cip 92797cd2ab92750220f9ee9df0f8b4e5... |  |  |
387 | 16:41:13.848 |  |  | RRC up-int bdfdf31e24f26114bdc82884c2b7c313... |  |  |
388 | 16:41:13.848 |  | ←RRC DCCH Security mode command |  |  |
389 | 16:41:13.849 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
390 | 16:41:13.887 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
391 | 16:41:13.887 |  | →RRC DCCH Security mode complete |  |  |
392 | 16:41:13.887 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
393 | 16:41:13.887 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
394 | 16:41:13.927 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
395 | 16:41:13.927 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
396 | 16:41:13.958 |  |  |  |  | →SIP PUBLISH | P-CSCF
397 | 16:41:13.965 |  |  |  |  | XML→ | Media-Server
398 | 16:41:13.967 |  |  |  |  | XML→ | Media-Server
399 | 16:41:13.968 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
400 | 16:41:13.970 |  |  |  |  | ←XML | Media-Server
401 | 16:41:13.970 |  |  |  |  | ←SIP 200 OK | P-CSCF
402 | 16:41:13.972 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
403 | 16:41:13.974 |  |  |  |  | ←SIP NOTIFY | P-CSCF
404 | 16:41:14.022 |  |  |  |  | →SIP 200 OK | P-CSCF
405 | 16:41:16.027 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
406 | 16:41:16.054 |  | ←RRC DCCH RRC connection release |  |  |
407 | 16:41:16.055 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
408 | 16:41:16.069 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
409 | 16:41:16.069 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:470: Step 2 Verdict: Pass
410 | 16:41:16.070 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:472: Test-Body Step 3 - 3E
411 | 16:41:16.070 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request status change of a functional alias to 'not activated'
412 | 16:41:16.072 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
413 | 16:41:19.753 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
414 | 16:41:19.753 |  | →RRC CCCH RRC connection request |  |  |
415 | 16:41:19.753 |  | ←RRC CCCH RRC connection setup |  |  |
416 | 16:41:19.753 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
417 | 16:41:19.807 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
418 | 16:41:19.807 |  | →RRC DCCH RRC connection setup complete |  |  |
419 | 16:41:19.807 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
420 | 16:41:19.807 |  |  |  | →NAS EMM Service request |  |
421 | 16:41:19.807 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
422 | 16:41:19.807 |  |  |  | NAS K-enb a6fb92b3afb1bfe60d78e70f9e7b3ba52... |  |
423 | 16:41:19.807 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
424 | 16:41:19.808 |  |  | RRC K-enb a6fb92b3afb1bfe60d78e70f9e7b3ba52... |  |  |
425 | 16:41:19.808 |  |  | RRC EUTRA band combinations |  |  |
426 | 16:41:19.808 |  |  | RRC rrc-cip aa4d50944ca598bdf37164be56bfbd8... |  |  |
427 | 16:41:19.808 |  |  | RRC rrc-int a36abf3576a26996cbd76750852302e... |  |  |
428 | 16:41:19.808 |  |  | RRC up-cip 139c39f89027a30d3c5cb438bb72681a... |  |  |
429 | 16:41:19.808 |  |  | RRC up-int 860223271c6039a95824ec49765817fe... |  |  |
430 | 16:41:19.808 |  | ←RRC DCCH Security mode command |  |  |
431 | 16:41:19.809 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
432 | 16:41:19.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
433 | 16:41:19.847 |  | →RRC DCCH Security mode complete |  |  |
434 | 16:41:19.847 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
435 | 16:41:19.847 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
436 | 16:41:19.887 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
437 | 16:41:19.887 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
438 | 16:41:19.918 |  |  |  |  | →SIP PUBLISH | P-CSCF
439 | 16:41:19.925 |  |  |  |  | XML→ | Media-Server
440 | 16:41:19.927 |  |  |  |  | XML→ | Media-Server
441 | 16:41:19.928 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
442 | 16:41:19.931 |  |  |  |  | ←XML | Media-Server
443 | 16:41:19.931 |  |  |  |  | ←SIP 200 OK | P-CSCF
444 | 16:41:19.932 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48327;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
445 | 16:41:19.934 |  |  |  |  | ←SIP NOTIFY | P-CSCF
446 | 16:41:19.980 |  |  |  |  | →SIP 200 OK | P-CSCF
447 | 16:41:21.983 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
448 | 16:41:22.012 |  | ←RRC DCCH RRC connection release |  |  |
449 | 16:41:22.013 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
450 | 16:41:22.026 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
451 | 16:41:22.027 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:474: Step 3 - 3E Verdict: Pass
452 | 16:41:22.028 |  |  |  |  | MMICmd: Make the UE (MCPTT client) de-subscribe from functional alias status change notifications
453 | 16:41:22.028 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
454 | 16:41:28.793 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
455 | 16:41:28.793 |  | →RRC CCCH RRC connection request |  |  |
456 | 16:41:28.793 |  | ←RRC CCCH RRC connection setup |  |  |
457 | 16:41:28.793 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
458 | 16:41:28.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
459 | 16:41:28.847 |  | →RRC DCCH RRC connection setup complete |  |  |
460 | 16:41:28.847 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
461 | 16:41:28.847 |  |  |  | →NAS EMM Service request |  |
462 | 16:41:28.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
463 | 16:41:28.847 |  |  |  | NAS K-enb 0a96cb2e0a9e1a2c932c94a4109c03cae... |  |
464 | 16:41:28.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
465 | 16:41:28.848 |  |  | RRC K-enb 0a96cb2e0a9e1a2c932c94a4109c03cae... |  |  |
466 | 16:41:28.848 |  |  | RRC EUTRA band combinations |  |  |
467 | 16:41:28.848 |  |  | RRC rrc-cip 63a377482b96dc8966239857abb6627... |  |  |
468 | 16:41:28.848 |  |  | RRC rrc-int 24317fe2f009a6445360e03857ae2ea... |  |  |
469 | 16:41:28.848 |  |  | RRC up-cip 7808f393cdc4bf2a01c7d39d56694998... |  |  |
470 | 16:41:28.848 |  |  | RRC up-int 93cbd3febd6b26a70dbf8e890a42f8da... |  |  |
471 | 16:41:28.848 |  | ←RRC DCCH Security mode command |  |  |
472 | 16:41:28.849 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
473 | 16:41:28.887 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
474 | 16:41:28.887 |  | →RRC DCCH Security mode complete |  |  |
475 | 16:41:28.887 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
476 | 16:41:28.887 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
477 | 16:41:28.927 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
478 | 16:41:28.927 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
479 | 16:41:28.950 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
480 | 16:41:28.952 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
481 | 16:41:28.955 |  |  |  |  | ←SIP 200 OK | P-CSCF
482 | 16:41:28.957 |  |  |  |  | XML→ | Media-Server
483 | 16:41:30.960 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
484 | 16:41:30.988 |  | ←RRC DCCH RRC connection release |  |  |
485 | 16:41:30.989 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
486 | 16:41:31.004 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
487 | 16:41:31.005 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:477: Step 4 - 7 Verdict: Pass
488 | 16:41:31.006 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
489 | 16:41:31.006 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
490 | 16:41:31.756 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.