MSG #80 2023-06-16 16:40:04.727

NAS

     ESM: ESM data transport
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x8e9424b8
    Sequence number = 0x02
    Protocol discriminator = 0x2 (EPS Session Management)
    Error while parsing message (message_type = 0xeb)
    Remaining bytes:
      92 78 eb a7 4b 19 94