MSG #477 2023-06-16 16:31:58.841
NAS

     ESM: Deactivate EPS bearer context request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xde2ba0bf
    Sequence number = 0x05
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xcd (Deactivate EPS bearer context request)
    ESM cause = 0x24 (Regular deactivation)
    Protocol configuration options:
      Ext = 1
      Configuration protocol = 0
      Protocol ID = 0x0011 (Network support of Local address in TFT indicator)
      Data =