ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 16:29:59.098 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 16:29:59.099 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 16:29:59.100 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 16:29:59.104 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 16:29:59.106 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 16:29:59.107 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:829: IMS UDP port 192.168.16.111:5060 configured
7 | 16:29:59.111 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:779: IMS TCP port 192.168.16.111:5060 configured!
8 | 16:29:59.114 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:800: Http Proxy (CMS, KMS, GMS) at port 192.168.16.111:8100 configured!
9 | 16:29:59.115 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:811: IdM port 192.168.16.111:8080 configured!
10 | 16:29:59.119 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 16:30:00.320 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 16:30:00.323 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 16:30:13.115 |  | ←RRC BCCH SIB |  |  |
14 | 16:30:13.120 |  | ←RRC BCCH SIB1 |  |  |
15 | 16:30:13.200 |  | ←RRC BCCH SIB1 |  |  |
16 | 16:30:13.275 |  | ←RRC BCCH SIB |  |  |
17 | 16:30:13.280 |  | ←RRC BCCH SIB1 |  |  |
18 | 16:30:20.683 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 16:30:20.683 |  | →RRC CCCH RRC connection request |  |  |
20 | 16:30:20.683 |  | ←RRC CCCH RRC connection setup |  |  |
21 | 16:30:20.683 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 16:30:20.735 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 16:30:20.735 |  | →RRC DCCH RRC connection setup complete |  |  |
24 | 16:30:20.735 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 16:30:20.735 |  |  |  | →NAS EMM Attach request |  |
26 | 16:30:20.735 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 16:30:20.735 |  |  |  | NAS K-asme b5b30371d648e21a8f42fe35bc98bb5e... |  |
28 | 16:30:20.735 |  |  |  | NAS ← EMM Authentication request |  |
29 | 16:30:20.736 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
30 | 16:30:20.736 |  | ←RRC DCCH DL information transfer |  |  |
31 | 16:30:20.737 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
32 | 16:30:20.807 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
33 | 16:30:20.807 |  | →RRC DCCH UL information transfer |  |  |
34 | 16:30:20.807 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
35 | 16:30:20.807 |  |  |  | →NAS EMM Authentication response |  |
36 | 16:30:20.807 |  |  |  | NAS UE auth OK |  |
37 | 16:30:20.807 |  |  |  | NAS 3GPP ctx tx_nas_count=0 rx_nas_count=16... |  |
38 | 16:30:20.807 |  |  |  | NAS K-nas-cip 652f87967ad94aa52d508f78a2c22... |  |
39 | 16:30:20.807 |  |  |  | NAS K-nas-int 0bce27a452c0fa0c0f9f274f1d3c0... |  |
40 | 16:30:20.807 |  |  |  | NAS ← EMM Security mode command |  |
41 | 16:30:20.808 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
42 | 16:30:20.808 |  | ←RRC DCCH DL information transfer |  |  |
43 | 16:30:20.809 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 16:30:20.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 16:30:20.847 |  | →RRC DCCH UL information transfer |  |  |
46 | 16:30:20.847 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
47 | 16:30:20.847 |  |  |  | →NAS EMM Security mode complete |  |
48 | 16:30:20.847 |  |  |  | NAS ← ESM ESM information request |  |
49 | 16:30:20.848 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
50 | 16:30:20.848 |  | ←RRC DCCH DL information transfer |  |  |
51 | 16:30:20.849 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 16:30:20.887 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 16:30:20.887 |  | →RRC DCCH UL information transfer |  |  |
54 | 16:30:20.887 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
55 | 16:30:20.887 |  |  |  | →NAS ESM ESM information response |  |
56 | 16:30:20.887 |  |  |  | NAS ← EMM Attach accept |  |
57 | 16:30:20.887 |  |  |  | NAS K-enb 60c8389bbad48b99f2883395571800044... |  |
58 | 16:30:20.887 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
59 | 16:30:20.888 |  | ←RRC DCCH Security mode command |  |  |
60 | 16:30:20.888 |  |  | RRC K-enb 60c8389bbad48b99f2883395571800044... |  |  |
61 | 16:30:20.888 |  |  | RRC rrc-cip 2e0a7dbbe7e33140221c33118757c29... |  |  |
62 | 16:30:20.888 |  |  | RRC rrc-int 81cb4c111fb2bc3cf69aa6ca98cc9ad... |  |  |
63 | 16:30:20.888 |  |  | RRC up-cip 311dc5cf549f21f25d9800d658f5a4d0... |  |  |
64 | 16:30:20.888 |  |  | RRC up-int ca929fb8d45d3db89257d2c6f6793911... |  |  |
65 | 16:30:20.889 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 16:30:20.927 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 16:30:20.927 |  | →RRC DCCH Security mode complete |  |  |
68 | 16:30:20.927 |  | ←RRC DCCH UE capability enquiry |  |  |
69 | 16:30:20.927 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 16:30:20.975 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 16:30:20.975 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
72 | 16:30:20.975 |  | →RRC DCCH UE capability information |  |  |
73 | 16:30:20.975 |  |  | RRC EUTRA band combinations |  |  |
74 | 16:30:20.975 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
75 | 16:30:20.975 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
76 | 16:30:21.007 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
77 | 16:30:21.007 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
78 | 16:30:21.047 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
79 | 16:30:21.047 |  | →RRC DCCH UL information transfer |  |  |
80 | 16:30:21.047 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xf) |  |  |
81 | 16:30:21.047 |  |  |  | →NAS EMM Attach complete |  |
82 | 16:30:21.047 |  |  |  | NAS ← EMM EMM information |  |
83 | 16:30:21.048 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
84 | 16:30:21.048 |  | ←RRC DCCH DL information transfer |  |  |
85 | 16:30:21.049 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
86 | 16:30:27.337 |  | ←RRC DCCH RRC connection release |  |  |
87 | 16:30:27.338 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
88 | 16:30:35.383 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
89 | 16:30:35.383 |  | →RRC CCCH RRC connection request |  |  |
90 | 16:30:35.383 |  | ←RRC CCCH RRC connection setup |  |  |
91 | 16:30:35.383 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
92 | 16:30:35.407 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
93 | 16:30:35.407 |  | →RRC DCCH RRC connection setup complete |  |  |
94 | 16:30:35.407 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
95 | 16:30:35.407 |  |  |  | →NAS EMM Service request |  |
96 | 16:30:35.407 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
97 | 16:30:35.407 |  |  |  | NAS K-enb 670163dc27947fa9f48dee4d6c5701dec... |  |
98 | 16:30:35.407 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
99 | 16:30:35.408 |  |  | RRC K-enb 670163dc27947fa9f48dee4d6c5701dec... |  |  |
100 | 16:30:35.408 |  |  | RRC EUTRA band combinations |  |  |
101 | 16:30:35.408 |  |  | RRC rrc-cip 4e7b19c2919f4e0b46e4900fc083b7e... |  |  |
102 | 16:30:35.408 |  |  | RRC rrc-int 9f3d4078536d2f5a4d5a422ff3c6e3d... |  |  |
103 | 16:30:35.408 |  |  | RRC up-cip ab33d417aeb042e283ccecc8ce0c7985... |  |  |
104 | 16:30:35.408 |  |  | RRC up-int 9ebfeb8f569ea91215818e5f2383f8a2... |  |  |
105 | 16:30:35.408 |  | ←RRC DCCH Security mode command |  |  |
106 | 16:30:35.409 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
107 | 16:30:35.447 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
108 | 16:30:35.447 |  | →RRC DCCH Security mode complete |  |  |
109 | 16:30:35.447 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
110 | 16:30:35.447 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
111 | 16:30:35.487 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
112 | 16:30:35.487 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
113 | 16:30:35.489 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 16:30:35.527 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 16:30:35.535 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 16:30:35.537 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 16:30:35.548 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 16:30:35.567 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 16:30:35.607 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
120 | 16:30:35.610 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
121 | 16:30:35.614 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 16)
122 | 16:30:35.647 | →enobeB PCAP frame→ TCP |  |  |  |
123 | 16:30:35.655 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
124 | 16:30:35.662 |  |  |  |  | →HTTP GET | HTTP-Proxy
125 | 16:30:35.670 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:349: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
126 | 16:30:35.676 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 16:30:35.677 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
128 | 16:30:35.727 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 16:30:36.407 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 16:30:36.409 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 16:30:36.447 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 16:30:36.455 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 16:30:36.457 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 16:30:36.461 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 16:30:36.487 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 16:30:36.647 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 16:30:36.649 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 16:30:36.652 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
139 | 16:30:36.687 | →enobeB PCAP frame→ TCP |  |  |  |
140 | 16:30:36.705 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 16:30:36.708 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 16:30:36.708 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 16:30:36.711 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 16:30:36.715 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:602: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 16:30:36.715 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 16:30:42.855 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 16:30:42.857 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 16:30:42.861 |  |  |  |  | →HTTP POST | IDMS-Endpoint
149 | 16:30:42.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
150 | 16:30:42.865 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 16:30:42.869 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:607: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
152 | 16:30:42.887 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 16:30:42.889 |  | ←enobeB PCAP frame← TCP |  |  |
154 | 16:30:42.892 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:698: IdM port - Client closed the connection (id 18)
155 | 16:30:42.927 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 16:30:43.087 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 16:30:43.089 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 16:30:43.127 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 16:30:43.135 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
160 | 16:30:43.137 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 16:30:43.139 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 16:30:43.167 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 16:30:43.207 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
164 | 16:30:43.209 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 16:30:43.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
166 | 16:30:43.255 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 16:30:43.260 |  |  |  |  | →HTTP POST | IDMS-Endpoint
168 | 16:30:43.262 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
169 | 16:30:43.264 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
170 | 16:30:43.268 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:612: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
171 | 16:30:43.327 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 16:30:43.407 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 16:30:43.409 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 16:30:43.447 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 16:30:43.455 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
176 | 16:30:43.457 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 16:30:43.458 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
178 | 16:30:43.487 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 16:30:43.495 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 16:30:43.498 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 16:30:43.501 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 19)
182 | 16:30:43.545 |  | ←enobeB PCAP frame← TCP |  |  |
183 | 16:30:43.549 |  |  |  |  | →HTTP POST | HTTP-Proxy
184 | 16:30:43.559 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
185 | 16:30:43.560 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
186 | 16:30:43.562 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:631: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
187 | 16:30:43.609 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 16:30:43.655 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
189 | 16:30:43.657 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 16:30:43.658 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
191 | 16:30:43.687 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 16:30:43.695 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
193 | 16:30:43.698 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
194 | 16:30:43.701 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 20)
195 | 16:30:43.735 | →enobeB PCAP frame→ HTTPS: POST https://kms.mcstaasting.com/keymanagement/ide... |  |  |  |
196 | 16:30:43.737 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 16:30:43.744 |  |  |  |  | →HTTP POST | HTTP-Proxy
198 | 16:30:43.797 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
199 | 16:30:43.799 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
200 | 16:30:43.803 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:634: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
201 | 16:30:43.847 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 16:30:43.855 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
203 | 16:30:43.861 |  |  |  |  | →SIP REGISTER | P-CSCF
204 | 16:30:43.863 | →enobeB PCAP frame→ TCP |  |  |  |
205 | 16:30:43.868 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:838: IMS UDP_s port 192.168.16.111:5062 configured
206 | 16:30:43.889 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:789: IMS TCP_s port 192.168.16.111:5062 configured!
207 | 16:30:43.890 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:847: IMS UDP_c port 192.168.16.111:5061 configured
208 | 16:30:43.892 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
209 | 16:30:43.894 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
210 | 16:30:44.032 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 16:30:44.047 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
212 | 16:30:44.049 |  |  |  |  | ←SIP 200 OK | P-CSCF
213 | 16:30:44.329 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
214 | 16:30:44.359 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
215 | 16:30:44.361 |  |  |  |  | ←SIP 200 OK | P-CSCF
216 | 16:30:44.363 |  |  |  |  | MIKEY | Media-Server
217 | 16:30:44.656 |  |  |  |  | XML→ | Media-Server
218 | 16:30:44.662 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47889;transp... |  |  |
219 | 16:30:44.662 |  |  |  |  | ←XML | Media-Server
220 | 16:30:44.664 |  |  |  |  | ←SIP NOTIFY | P-CSCF
221 | 16:30:44.700 |  |  |  |  | →SIP 200 OK | P-CSCF
222 | 16:30:44.769 |  | ←enobeB PCAP frame← TCP |  |  |
223 | 16:30:44.807 | →enobeB PCAP frame→ TCP |  |  |  |
224 | 16:30:44.815 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
225 | 16:30:44.817 |  | ←enobeB PCAP frame← TCP |  |  |
226 | 16:30:44.823 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
227 | 16:30:44.847 | →enobeB PCAP frame→ TCP |  |  |  |
228 | 16:30:44.887 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
229 | 16:30:44.890 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
230 | 16:30:44.894 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
231 | 16:30:44.935 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 16:30:44.942 |  |  |  |  | →HTTP GET | HTTP-Proxy
233 | 16:30:44.949 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:815: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
234 | 16:30:44.953 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
235 | 16:30:44.955 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
236 | 16:30:44.967 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
237 | 16:30:45.007 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 16:30:45.009 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 16:30:45.012 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
240 | 16:30:45.047 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 16:30:45.087 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 16:30:45.089 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 16:30:45.127 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 16:30:45.135 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 16:30:45.137 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 16:30:45.143 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
247 | 16:30:45.167 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 16:30:45.207 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 16:30:45.210 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
250 | 16:30:45.214 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
251 | 16:30:45.255 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
252 | 16:30:45.262 |  |  |  |  | →HTTP GET | HTTP-Proxy
253 | 16:30:45.271 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:820: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
254 | 16:30:45.284 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
255 | 16:30:45.286 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
256 | 16:30:45.287 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
257 | 16:30:45.327 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 16:30:45.335 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 16:30:45.367 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 16:30:45.369 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 16:30:45.370 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 16:30:45.373 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
263 | 16:30:45.407 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 16:30:45.809 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
265 | 16:30:45.841 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
266 | 16:30:45.843 |  |  |  |  | ←SIP 200 OK | P-CSCF
267 | 16:30:45.846 |  |  |  |  | MIKEY | Media-Server
268 | 16:30:45.849 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 16:30:45.895 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 16:30:45.897 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 16:30:45.898 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 16:30:45.927 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 16:30:45.967 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
274 | 16:30:45.969 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
275 | 16:30:45.972 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
276 | 16:30:46.015 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
277 | 16:30:46.020 |  |  |  |  | →HTTP GET | HTTP-Proxy
278 | 16:30:46.022 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:825: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
279 | 16:30:46.024 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
280 | 16:30:46.025 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
281 | 16:30:46.047 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 16:30:46.087 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 16:30:46.089 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 16:30:46.092 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
285 | 16:30:46.127 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 16:30:46.155 |  |  |  |  | XML→ | Media-Server
287 | 16:30:46.159 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47889;transp... |  |  |
288 | 16:30:46.159 |  |  |  |  | ←XML | Media-Server
289 | 16:30:46.161 |  |  |  |  | ←SIP NOTIFY | P-CSCF
290 | 16:30:46.215 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
291 | 16:30:46.221 |  |  |  |  | →SIP 200 OK | P-CSCF
292 | 16:30:46.434 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 16:30:46.451 |  |  |  |  | →SIP PUBLISH | P-CSCF
294 | 16:30:46.477 |  |  |  |  | MIKEY | Media-Server
295 | 16:30:46.497 |  | ←enobeB PCAP frame← TCP |  |  |
296 | 16:30:46.498 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
297 | 16:30:46.567 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
298 | 16:30:46.569 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
299 | 16:30:46.572 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
300 | 16:30:46.615 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
301 | 16:30:46.620 |  |  |  |  | →HTTP GET | HTTP-Proxy
302 | 16:30:46.622 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:830: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
303 | 16:30:46.625 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
304 | 16:30:46.627 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
305 | 16:30:46.647 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 16:30:46.687 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 16:30:46.689 |  | ←enobeB PCAP frame← TCP |  |  |
308 | 16:30:46.692 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
309 | 16:30:46.727 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 16:30:46.776 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
311 | 16:30:46.776 |  |  |  |  | XML→ | Media-Server
312 | 16:30:46.779 |  |  |  |  | ←SIP 200 OK | P-CSCF
313 | 16:30:46.798 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
314 | 16:30:46.802 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
315 | 16:30:46.805 |  |  |  |  | ←SIP 200 OK | P-CSCF
316 | 16:30:46.806 |  |  |  |  | MIKEY | Media-Server
317 | 16:30:47.091 |  |  |  |  | XML→ | Media-Server
318 | 16:30:47.094 |  |  |  |  | Protected MCData Message | -
319 | 16:30:47.141 |  |  |  |  | ←XML | Media-Server
320 | 16:30:47.150 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47889;transp... |  |  |
321 | 16:30:47.150 |  |  |  |  | ←SIP NOTIFY | P-CSCF
322 | 16:30:47.181 |  |  |  |  | →SIP 200 OK | P-CSCF
323 | 16:30:47.184 |  |  |  |  | ←XML | Media-Server
324 | 16:30:47.193 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
325 | 16:30:47.195 |  |  |  |  | ←SIP MESSAGE | P-CSCF
326 | 16:30:47.543 |  |  |  |  | →SIP 200 OK | P-CSCF
327 | 16:30:49.548 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
328 | 16:30:49.588 |  | ←RRC DCCH RRC connection release |  |  |
329 | 16:30:49.589 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
330 | 16:30:49.602 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
331 | 16:30:49.603 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
332 | 16:30:49.603 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request to determine the current status of a functional alias and later notification of status changes of a functional alias
333 | 16:31:07.063 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
334 | 16:31:07.063 |  | →RRC CCCH RRC connection request |  |  |
335 | 16:31:07.063 |  | ←RRC CCCH RRC connection setup |  |  |
336 | 16:31:07.063 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
337 | 16:31:07.087 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
338 | 16:31:07.087 |  | →RRC DCCH RRC connection setup complete |  |  |
339 | 16:31:07.087 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
340 | 16:31:07.087 |  |  |  | →NAS EMM Service request |  |
341 | 16:31:07.087 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
342 | 16:31:07.087 |  |  |  | NAS K-enb 8ee1bbae27e2909bd1862fdf5c126c998... |  |
343 | 16:31:07.087 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
344 | 16:31:07.088 |  |  | RRC K-enb 8ee1bbae27e2909bd1862fdf5c126c998... |  |  |
345 | 16:31:07.088 |  |  | RRC EUTRA band combinations |  |  |
346 | 16:31:07.088 |  |  | RRC rrc-cip aa2b2adb354f8333a7e3bb72fd6fc87... |  |  |
347 | 16:31:07.088 |  |  | RRC rrc-int ed38e0945fbf262bcdb7a29459b4a4c... |  |  |
348 | 16:31:07.088 |  |  | RRC up-cip d6dc69c3f580d884fddf427b2d7323f8... |  |  |
349 | 16:31:07.088 |  |  | RRC up-int 100ebe69f890fe43d326a7cb581be475... |  |  |
350 | 16:31:07.088 |  | ←RRC DCCH Security mode command |  |  |
351 | 16:31:07.089 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
352 | 16:31:07.127 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
353 | 16:31:07.127 |  | →RRC DCCH Security mode complete |  |  |
354 | 16:31:07.127 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
355 | 16:31:07.127 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
356 | 16:31:07.167 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
357 | 16:31:07.167 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
358 | 16:31:07.190 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
359 | 16:31:07.193 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
360 | 16:31:07.195 |  |  |  |  | ←SIP 200 OK | P-CSCF
361 | 16:31:07.197 |  |  |  |  | XML→ | Media-Server
362 | 16:31:07.200 |  |  |  |  | ←XML | Media-Server
363 | 16:31:07.202 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47889;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
364 | 16:31:07.204 |  |  |  |  | ←SIP NOTIFY | P-CSCF
365 | 16:31:07.260 |  |  |  |  | →SIP 200 OK | P-CSCF
366 | 16:31:09.263 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
367 | 16:31:09.300 |  | ←RRC DCCH RRC connection release |  |  |
368 | 16:31:09.301 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
369 | 16:31:09.315 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
370 | 16:31:09.316 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request to change the status of a functional alias to 'activated'
371 | 16:31:09.316 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
372 | 16:31:13.253 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
373 | 16:31:13.253 |  | →RRC CCCH RRC connection request |  |  |
374 | 16:31:13.253 |  | ←RRC CCCH RRC connection setup |  |  |
375 | 16:31:13.253 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
376 | 16:31:13.287 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
377 | 16:31:13.287 |  | →RRC DCCH RRC connection setup complete |  |  |
378 | 16:31:13.287 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
379 | 16:31:13.287 |  |  |  | →NAS EMM Service request |  |
380 | 16:31:13.287 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
381 | 16:31:13.287 |  |  |  | NAS K-enb a204255593f8d2eba1afdffa908057558... |  |
382 | 16:31:13.287 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
383 | 16:31:13.288 |  |  | RRC K-enb a204255593f8d2eba1afdffa908057558... |  |  |
384 | 16:31:13.288 |  |  | RRC EUTRA band combinations |  |  |
385 | 16:31:13.288 |  |  | RRC rrc-cip e5bad5d5bd680e89ea57b8f87b00f7d... |  |  |
386 | 16:31:13.288 |  |  | RRC rrc-int 525144300421dbefa398c47c4ecd4f2... |  |  |
387 | 16:31:13.288 |  |  | RRC up-cip 2db72996c27ae1569427ce4f39a35c64... |  |  |
388 | 16:31:13.288 |  |  | RRC up-int a516213a54d8e65a37f32c1777701315... |  |  |
389 | 16:31:13.288 |  | ←RRC DCCH Security mode command |  |  |
390 | 16:31:13.289 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
391 | 16:31:13.327 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
392 | 16:31:13.327 |  | →RRC DCCH Security mode complete |  |  |
393 | 16:31:13.327 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
394 | 16:31:13.327 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
395 | 16:31:13.367 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
396 | 16:31:13.367 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
397 | 16:31:13.399 |  |  |  |  | →SIP PUBLISH | P-CSCF
398 | 16:31:13.408 |  |  |  |  | XML→ | Media-Server
399 | 16:31:13.410 |  |  |  |  | XML→ | Media-Server
400 | 16:31:13.412 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
401 | 16:31:13.415 |  |  |  |  | ←SIP 200 OK | P-CSCF
402 | 16:31:13.416 |  |  |  |  | ←XML | Media-Server
403 | 16:31:13.418 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47889;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
404 | 16:31:13.420 |  |  |  |  | ←SIP NOTIFY | P-CSCF
405 | 16:31:13.460 |  |  |  |  | →SIP 200 OK | P-CSCF
406 | 16:31:15.463 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
407 | 16:31:15.491 |  | ←RRC DCCH RRC connection release |  |  |
408 | 16:31:15.492 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
409 | 16:31:15.505 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
410 | 16:31:15.506 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1876: Test-Body Step 1
411 | 16:31:15.506 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request the establishment of a chat group call using the active functional alias with automatic commencement mode and implicit floor request
412 | 16:31:15.506 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
413 | 16:31:15.507 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1884: Test-Body Step 2
414 | 16:31:38.914 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
415 | 16:31:38.914 |  | →RRC CCCH RRC connection request |  |  |
416 | 16:31:38.914 |  | ←RRC CCCH RRC connection setup |  |  |
417 | 16:31:38.914 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
418 | 16:31:38.967 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
419 | 16:31:38.967 |  | →RRC DCCH RRC connection setup complete |  |  |
420 | 16:31:38.967 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
421 | 16:31:38.967 |  |  |  | →NAS EMM Service request |  |
422 | 16:31:38.967 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
423 | 16:31:38.967 |  |  |  | NAS K-enb 1dade6893d01ca5ceba5d339915251de2... |  |
424 | 16:31:38.967 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
425 | 16:31:38.968 |  |  | RRC K-enb 1dade6893d01ca5ceba5d339915251de2... |  |  |
426 | 16:31:38.968 |  |  | RRC EUTRA band combinations |  |  |
427 | 16:31:38.968 |  |  | RRC rrc-cip 380db3891c5d2b747a9fbfe945f6b96... |  |  |
428 | 16:31:38.968 |  |  | RRC rrc-int 7d906860e57b687b03620c6eeca90a7... |  |  |
429 | 16:31:38.968 |  |  | RRC up-cip 4ea2d7d0298e72d5190fd1259f2f8470... |  |  |
430 | 16:31:38.968 |  |  | RRC up-int 6acb56f718caa14c2b8583e575809aa2... |  |  |
431 | 16:31:38.968 |  | ←RRC DCCH Security mode command |  |  |
432 | 16:31:38.969 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
433 | 16:31:39.007 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
434 | 16:31:39.007 |  | →RRC DCCH Security mode complete |  |  |
435 | 16:31:39.007 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
436 | 16:31:39.007 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
437 | 16:31:39.047 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
438 | 16:31:39.047 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
439 | 16:31:39.078 |  |  |  |  | →SIP INVITE | P-CSCF
440 | 16:31:39.088 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:759: SRTP config: Master Key: D76D33DE1008DCC21E537D88AFC5091F, Master Salt: 50DD608BCA59F6E1EC82093A, MKI: 2EB056AB
441 | 16:31:39.089 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:185: RTP and FloorControl ports configured 192.168.16.111:60350:60351:60354
442 | 16:31:39.093 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
443 | 16:31:39.095 |  |  |  |  | XML→ | Media-Server
444 | 16:31:39.096 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
445 | 16:31:39.098 |  |  |  |  | ←SIP 100 Trying | P-CSCF
446 | 16:31:39.724 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
447 | 16:31:39.724 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
448 | 16:31:39.724 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
449 | 16:31:39.725 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
450 | 16:31:39.767 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
451 | 16:31:39.767 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
452 | 16:31:39.767 |  | →RRC DCCH UL information transfer |  |  |
453 | 16:31:39.767 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
454 | 16:31:39.767 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
455 | 16:31:39.776 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 16:31:39.805 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1888: Step 2 Verdict: Pass
457 | 16:31:39.813 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
458 | 16:31:39.815 |  |  |  |  | ←SIP 200 OK | P-CSCF
459 | 16:31:39.902 |  |  |  |  | →SIP ACK | P-CSCF
460 | 16:31:39.906 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1892: Test-Body Step 3
461 | 16:31:39.907 |  |  |  |  | UserCheck: Does the UE (MCPTT client) provide floor granted notification to the user?
462 | 16:31:40.167 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
463 | 16:31:40.247 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
464 | 16:31:40.255 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
465 | 16:31:40.263 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
466 | 16:31:40.287 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
467 | 16:31:46.055 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1893: Step 3 Verdict: Pass
468 | 16:31:46.055 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1895: Test-Body Step 4
469 | 16:31:46.056 |  |  |  |  | MMICmd: Make the UE (MCPTT client) release the call
470 | 16:31:46.057 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1898: Test-Body Step 5
471 | 16:31:46.158 |  |  |  |  | MMICmd: Release call (hang up the call)
472 | 16:31:56.821 |  |  |  |  | →SIP BYE | P-CSCF
473 | 16:31:56.822 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
474 | 16:31:56.825 |  |  |  |  | ←SIP 200 OK | P-CSCF
475 | 16:31:57.007 | →enobeB PCAP frame→ |  |  |  |
476 | 16:31:58.826 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
477 | 16:31:58.841 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
478 | 16:31:58.841 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
479 | 16:31:58.841 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
480 | 16:31:58.842 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
481 | 16:31:58.887 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
482 | 16:31:58.887 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
483 | 16:31:58.887 |  | →RRC DCCH UL information transfer |  |  |
484 | 16:31:58.887 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
485 | 16:31:58.887 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
486 | 16:31:58.911 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
487 | 16:31:58.913 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
488 | 16:31:58.950 |  | ←RRC DCCH RRC connection release |  |  |
489 | 16:31:58.951 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
490 | 16:31:58.965 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
491 | 16:31:58.966 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1900: Step 5 Verdict: Pass
492 | 16:31:58.969 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
493 | 16:31:58.969 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
494 | 16:31:59.719 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.