MSG #28 2023-06-16 16:30:20.735
NAS

     EMM: Authentication request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xe9f3a790
    Sequence number = 0x09
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x52 (Authentication request)
    NAS key set identifier:
      TSC = 0
      NAS key set identifier = 0
    Authentication parameter RAND:
      Data = a3 83 f7 a6 db a0 3b dc da 90 5f 8a dd f1 cf 81
    Authentication parameter AUTN:
      Length = 16
      Data = f9 d1 9e 23 32 7d 90 01 f6 dc dc 99 89 7d f8 1c