MSG #35 2023-06-16 16:30:20.807
NAS

     EMM: Authentication response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x33eb06d3
    Sequence number = 0x10
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x53 (Authentication response)
    Authentication response parameter:
      Length = 8
      Data = a3 dc 18 dc e3 3b 48 79