MSG #28 2023-06-16 15:32:17.655
NAS

     EMM: Authentication request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x8c4cc3b2
    Sequence number = 0x08
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x52 (Authentication request)
    NAS key set identifier:
      TSC = 0
      NAS key set identifier = 6
    Authentication parameter RAND:
      Data = c9 36 11 c5 51 75 ef 0c 08 cc d8 70 2e e9 6a e3
    Authentication parameter AUTN:
      Length = 16
      Data = d7 e7 5f 3b ed d8 90 01 3d e7 da 15 55 82 c6 6f