MSG #397 2023-06-16 15:32:58.701

SIP BYE message at 15:32:58.701

    BYE sip:mcptt-session-A@cf.mcstaasting.com SIP/2.0
    Via: SIP/2.0/UDP 192.168.3.2:47744;branch=z9hG4bK-503880837;rport
    From: <sip:PublicUserId-A@mcstaasting.com>;tag=1282482549
    To: <sip:mcptt-server-A@mcstaasting.com>;tag=abc-INVITE-Totag
    Call-ID: 81ff723e-e3fe-99ea-109b-1642df197647
    CSeq: 616960041 BYE
    Content-Length: 0
    Max-Forwards: 70
    Route: <sip:192.168.16.111:5062;lr>
    Route: <sip:orig@scscf.3gpp.org;lr>
    Route: <sip:scscf.other.com;lr>
    Route: <sip:pcscf.other.com;lr>
    Allow: INVITE, ACK, CANCEL, BYE, MESSAGE, OPTIONS, NOTIFY, PRACK, UPDATE, REFER
    Privacy: none
    P-Access-Network-Info: 3GPP-E-UTRAN-FDD;utran-cell-id-3gpp=0000000000000000
    User-Agent: MCS CLIENT SDK Nemergent 1.0 /v 8.1.2
    P-Preferred-Identity: <sip:PublicUserId-A@mcstaasting.com>
    Security-Client: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;prot=esp;mod=trans;spi-c=1286774454;spi-s=732422572;port-c=44953;port-s=47744;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-md5-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.7
    Require: sec-agree
    Proxy-Require: sec-agree