ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 15:32:09.616 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 15:32:09.617 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 15:32:09.618 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 15:32:09.619 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 15:32:09.620 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 15:32:09.620 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:829: IMS UDP port 192.168.16.111:5060 configured
7 | 15:32:09.622 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:779: IMS TCP port 192.168.16.111:5060 configured!
8 | 15:32:09.624 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:800: Http Proxy (CMS, KMS, GMS) at port 192.168.16.111:8100 configured!
9 | 15:32:09.625 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:811: IdM port 192.168.16.111:8080 configured!
10 | 15:32:09.627 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 15:32:10.828 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 15:32:10.830 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 15:32:12.560 |  | ←RRC BCCH SIB1 |  |  |
14 | 15:32:12.635 |  | ←RRC BCCH SIB |  |  |
15 | 15:32:12.640 |  | ←RRC BCCH SIB1 |  |  |
16 | 15:32:12.655 |  | ←RRC BCCH SIB |  |  |
17 | 15:32:12.675 |  | ←RRC BCCH SIB |  |  |
18 | 15:32:17.584 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 15:32:17.584 |  | →RRC CCCH RRC connection request |  |  |
20 | 15:32:17.584 |  | ←RRC CCCH RRC connection setup |  |  |
21 | 15:32:17.584 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 15:32:17.655 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 15:32:17.655 |  | →RRC DCCH RRC connection setup complete |  |  |
24 | 15:32:17.655 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 15:32:17.655 |  |  |  | →NAS EMM Attach request |  |
26 | 15:32:17.655 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 15:32:17.655 |  |  |  | NAS K-asme 6e1aef5a90276481b78d1d89bff634a1... |  |
28 | 15:32:17.655 |  |  |  | NAS ← EMM Authentication request |  |
29 | 15:32:17.656 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
30 | 15:32:17.656 |  | ←RRC DCCH DL information transfer |  |  |
31 | 15:32:17.657 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
32 | 15:32:17.727 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
33 | 15:32:17.727 |  | →RRC DCCH UL information transfer |  |  |
34 | 15:32:17.727 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
35 | 15:32:17.727 |  |  |  | →NAS EMM Authentication response |  |
36 | 15:32:17.727 |  |  |  | NAS UE auth OK |  |
37 | 15:32:17.727 |  |  |  | NAS 3GPP ctx tx_nas_count=0 rx_nas_count=16... |  |
38 | 15:32:17.727 |  |  |  | NAS K-nas-cip 7edf4daaa4460f46a0beeec6d4202... |  |
39 | 15:32:17.727 |  |  |  | NAS K-nas-int 2e9a193c2c6e14073b923cfa1bded... |  |
40 | 15:32:17.727 |  |  |  | NAS ← EMM Security mode command |  |
41 | 15:32:17.728 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
42 | 15:32:17.728 |  | ←RRC DCCH DL information transfer |  |  |
43 | 15:32:17.729 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 15:32:17.767 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 15:32:17.767 |  | →RRC DCCH UL information transfer |  |  |
46 | 15:32:17.767 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
47 | 15:32:17.767 |  |  |  | →NAS EMM Security mode complete |  |
48 | 15:32:17.767 |  |  |  | NAS ← ESM ESM information request |  |
49 | 15:32:17.768 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
50 | 15:32:17.768 |  | ←RRC DCCH DL information transfer |  |  |
51 | 15:32:17.769 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 15:32:17.807 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 15:32:17.807 |  | →RRC DCCH UL information transfer |  |  |
54 | 15:32:17.807 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
55 | 15:32:17.807 |  |  |  | →NAS ESM ESM information response |  |
56 | 15:32:17.807 |  |  |  | NAS ← EMM Attach accept |  |
57 | 15:32:17.807 |  |  |  | NAS K-enb bab1744ffacc6d529ffebcc300a7572c3... |  |
58 | 15:32:17.807 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
59 | 15:32:17.808 |  | ←RRC DCCH Security mode command |  |  |
60 | 15:32:17.808 |  |  | RRC K-enb bab1744ffacc6d529ffebcc300a7572c3... |  |  |
61 | 15:32:17.808 |  |  | RRC rrc-cip 84a1608bea877f0769bb078d7ba28e4... |  |  |
62 | 15:32:17.808 |  |  | RRC rrc-int 6a43489e95aba6f1907e51af8c463ee... |  |  |
63 | 15:32:17.808 |  |  | RRC up-cip 10d20eb247c8066376e661c077137c05... |  |  |
64 | 15:32:17.808 |  |  | RRC up-int 134873bf6bff301effaeea3c6f209659... |  |  |
65 | 15:32:17.809 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 15:32:17.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 15:32:17.847 |  | →RRC DCCH Security mode complete |  |  |
68 | 15:32:17.847 |  | ←RRC DCCH UE capability enquiry |  |  |
69 | 15:32:17.847 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 15:32:17.895 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 15:32:17.895 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
72 | 15:32:17.895 |  | →RRC DCCH UE capability information |  |  |
73 | 15:32:17.895 |  |  | RRC EUTRA band combinations |  |  |
74 | 15:32:17.895 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
75 | 15:32:17.895 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
76 | 15:32:17.927 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
77 | 15:32:17.927 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
78 | 15:32:17.967 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
79 | 15:32:17.967 |  | →RRC DCCH UL information transfer |  |  |
80 | 15:32:17.967 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
81 | 15:32:17.967 |  |  |  | →NAS EMM Attach complete |  |
82 | 15:32:17.967 |  |  |  | NAS ← EMM EMM information |  |
83 | 15:32:17.968 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
84 | 15:32:17.968 |  | ←RRC DCCH DL information transfer |  |  |
85 | 15:32:17.969 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
86 | 15:32:22.789 |  | ←RRC DCCH RRC connection release |  |  |
87 | 15:32:22.790 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
88 | 15:32:27.823 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
89 | 15:32:27.823 |  | →RRC CCCH RRC connection request |  |  |
90 | 15:32:27.823 |  | ←RRC CCCH RRC connection setup |  |  |
91 | 15:32:27.823 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
92 | 15:32:27.847 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
93 | 15:32:27.847 |  | →RRC DCCH RRC connection setup complete |  |  |
94 | 15:32:27.847 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
95 | 15:32:27.847 |  |  |  | →NAS EMM Service request |  |
96 | 15:32:27.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
97 | 15:32:27.847 |  |  |  | NAS K-enb 7ab322cb8360dc7b52b28f25fab472dcf... |  |
98 | 15:32:27.847 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
99 | 15:32:27.848 |  |  | RRC K-enb 7ab322cb8360dc7b52b28f25fab472dcf... |  |  |
100 | 15:32:27.848 |  |  | RRC EUTRA band combinations |  |  |
101 | 15:32:27.848 |  |  | RRC rrc-cip 9b8acc024f969bec50c9a3d6a87e20c... |  |  |
102 | 15:32:27.848 |  |  | RRC rrc-int 45eb97fc618e0e561e4abed91ccf139... |  |  |
103 | 15:32:27.848 |  |  | RRC up-cip b35c1f10a7df3afa4066f516ba60e4e3... |  |  |
104 | 15:32:27.848 |  |  | RRC up-int 37eee18e49b6bff475021909c4df11f2... |  |  |
105 | 15:32:27.848 |  | ←RRC DCCH Security mode command |  |  |
106 | 15:32:27.849 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
107 | 15:32:27.887 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
108 | 15:32:27.887 |  | →RRC DCCH Security mode complete |  |  |
109 | 15:32:27.887 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
110 | 15:32:27.887 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
111 | 15:32:27.927 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
112 | 15:32:27.927 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
113 | 15:32:27.930 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 15:32:27.967 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 15:32:27.975 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 15:32:27.977 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 15:32:27.991 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 15:32:28.047 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 15:32:28.055 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
120 | 15:32:28.059 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
121 | 15:32:28.062 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 16)
122 | 15:32:28.087 | →enobeB PCAP frame→ TCP |  |  |  |
123 | 15:32:28.095 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
124 | 15:32:28.102 |  |  |  |  | →HTTP GET | HTTP-Proxy
125 | 15:32:28.107 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:349: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
126 | 15:32:28.111 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 15:32:28.112 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
128 | 15:32:28.127 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 15:32:28.887 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 15:32:28.889 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 15:32:28.927 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 15:32:28.935 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 15:32:28.937 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 15:32:28.940 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 15:32:28.967 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 15:32:29.087 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 15:32:29.090 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 15:32:29.092 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
139 | 15:32:29.127 | →enobeB PCAP frame→ TCP |  |  |  |
140 | 15:32:29.145 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 15:32:29.148 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 15:32:29.148 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 15:32:29.150 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 15:32:29.155 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:602: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 15:32:29.155 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 15:32:34.146 |  | ←enobeB PCAP frame← TCP |  |  |
147 | 15:32:34.152 |  |  |  |  | →HTTP POST | IDMS-Endpoint
148 | 15:32:34.159 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
149 | 15:32:34.160 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 15:32:34.164 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:607: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 15:32:34.209 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 15:32:34.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:698: IdM port - Client closed the connection (id 18)
153 | 15:32:34.367 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 15:32:34.369 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 15:32:34.407 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 15:32:34.415 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
157 | 15:32:34.417 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 15:32:34.418 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
159 | 15:32:34.447 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 15:32:34.487 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 15:32:34.489 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 15:32:34.492 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:654: Client connected to IdM port (id 18)
163 | 15:32:34.535 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
164 | 15:32:34.540 |  |  |  |  | →HTTP POST | IDMS-Endpoint
165 | 15:32:34.542 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
166 | 15:32:34.544 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
167 | 15:32:34.548 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:612: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
168 | 15:32:34.607 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 15:32:34.687 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 15:32:34.689 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 15:32:34.727 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 15:32:34.735 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
173 | 15:32:34.737 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 15:32:34.742 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
175 | 15:32:34.767 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 15:32:34.775 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
177 | 15:32:34.778 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
178 | 15:32:34.780 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 19)
179 | 15:32:34.815 | →enobeB PCAP frame→ HTTPS: POST https://kms.mcstaasting.com/keymanagement/ide... |  |  |  |
180 | 15:32:34.817 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 15:32:34.822 |  |  |  |  | →HTTP POST | HTTP-Proxy
182 | 15:32:34.841 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
183 | 15:32:34.842 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
184 | 15:32:34.844 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:631: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
185 | 15:32:34.887 | →enobeB PCAP frame→ TCP |  |  |  |
186 | 15:32:34.889 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 15:32:34.927 | →enobeB PCAP frame→ TCP |  |  |  |
188 | 15:32:34.935 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
189 | 15:32:34.937 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 15:32:34.939 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
191 | 15:32:34.967 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 15:32:34.975 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
193 | 15:32:34.977 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
194 | 15:32:34.980 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 20)
195 | 15:32:35.015 | →enobeB PCAP frame→ HTTPS: POST https://kms.mcstaasting.com/keymanagement/ide... |  |  |  |
196 | 15:32:35.017 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 15:32:35.020 |  |  |  |  | →HTTP POST | HTTP-Proxy
198 | 15:32:35.052 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
199 | 15:32:35.054 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
200 | 15:32:35.058 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:634: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
201 | 15:32:35.087 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 15:32:35.127 | →enobeB PCAP frame→ TCP |  |  |  |
203 | 15:32:35.135 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
204 | 15:32:35.140 |  |  |  |  | →SIP REGISTER | P-CSCF
205 | 15:32:35.146 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:838: IMS UDP_s port 192.168.16.111:5062 configured
206 | 15:32:35.162 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:789: IMS TCP_s port 192.168.16.111:5062 configured!
207 | 15:32:35.164 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:847: IMS UDP_c port 192.168.16.111:5061 configured
208 | 15:32:35.165 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
209 | 15:32:35.167 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
210 | 15:32:35.313 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 15:32:35.330 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
212 | 15:32:35.332 |  |  |  |  | ←SIP 200 OK | P-CSCF
213 | 15:32:35.608 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
214 | 15:32:35.634 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
215 | 15:32:35.636 |  |  |  |  | ←SIP 200 OK | P-CSCF
216 | 15:32:35.639 |  |  |  |  | MIKEY | Media-Server
217 | 15:32:35.936 |  |  |  |  | XML→ | Media-Server
218 | 15:32:35.942 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47744;transp... |  |  |
219 | 15:32:35.942 |  |  |  |  | ←XML | Media-Server
220 | 15:32:35.944 |  |  |  |  | ←SIP NOTIFY | P-CSCF
221 | 15:32:35.981 |  |  |  |  | →SIP 200 OK | P-CSCF
222 | 15:32:36.049 |  | ←enobeB PCAP frame← TCP |  |  |
223 | 15:32:36.087 | →enobeB PCAP frame→ TCP |  |  |  |
224 | 15:32:36.095 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
225 | 15:32:36.097 |  | ←enobeB PCAP frame← TCP |  |  |
226 | 15:32:36.102 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
227 | 15:32:36.127 | →enobeB PCAP frame→ TCP |  |  |  |
228 | 15:32:36.167 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
229 | 15:32:36.170 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
230 | 15:32:36.181 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
231 | 15:32:36.215 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 15:32:36.221 |  |  |  |  | →HTTP GET | HTTP-Proxy
233 | 15:32:36.227 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:815: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
234 | 15:32:36.233 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
235 | 15:32:36.234 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
236 | 15:32:36.247 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
237 | 15:32:36.287 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 15:32:36.289 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 15:32:36.293 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
240 | 15:32:36.327 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 15:32:36.367 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 15:32:36.369 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 15:32:36.407 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 15:32:36.415 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 15:32:36.417 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 15:32:36.427 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
247 | 15:32:36.447 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 15:32:36.487 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 15:32:36.490 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
250 | 15:32:36.493 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
251 | 15:32:36.535 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
252 | 15:32:36.540 |  |  |  |  | →HTTP GET | HTTP-Proxy
253 | 15:32:36.541 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:820: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
254 | 15:32:36.547 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
255 | 15:32:36.548 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
256 | 15:32:36.548 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
257 | 15:32:36.567 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 15:32:36.575 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 15:32:36.617 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 15:32:36.647 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 15:32:36.649 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 15:32:36.652 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
263 | 15:32:36.687 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 15:32:37.093 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
265 | 15:32:37.115 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
266 | 15:32:37.117 |  |  |  |  | ←SIP 200 OK | P-CSCF
267 | 15:32:37.120 |  |  |  |  | MIKEY | Media-Server
268 | 15:32:37.129 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 15:32:37.175 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 15:32:37.177 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 15:32:37.179 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 15:32:37.207 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 15:32:37.247 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
274 | 15:32:37.249 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
275 | 15:32:37.252 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
276 | 15:32:37.295 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
277 | 15:32:37.300 |  |  |  |  | →HTTP GET | HTTP-Proxy
278 | 15:32:37.301 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:825: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
279 | 15:32:37.303 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
280 | 15:32:37.304 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
281 | 15:32:37.327 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 15:32:37.367 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 15:32:37.369 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 15:32:37.372 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
285 | 15:32:37.407 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 15:32:37.424 |  |  |  |  | XML→ | Media-Server
287 | 15:32:37.429 |  |  |  |  | ←XML | Media-Server
288 | 15:32:37.430 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47744;transp... |  |  |
289 | 15:32:37.432 |  |  |  |  | ←SIP NOTIFY | P-CSCF
290 | 15:32:37.455 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
291 | 15:32:37.460 |  |  |  |  | →SIP 200 OK | P-CSCF
292 | 15:32:37.714 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 15:32:37.730 |  |  |  |  | →SIP PUBLISH | P-CSCF
294 | 15:32:37.757 |  |  |  |  | MIKEY | Media-Server
295 | 15:32:37.775 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 15:32:37.777 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 15:32:37.778 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 15:32:37.807 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 15:32:37.847 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
300 | 15:32:37.849 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 15:32:37.852 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:645: Client connected to Http Proxy port (id 25)
302 | 15:32:37.895 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 15:32:37.900 |  |  |  |  | →HTTP GET | HTTP-Proxy
304 | 15:32:37.901 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:830: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
305 | 15:32:37.903 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
306 | 15:32:37.905 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
307 | 15:32:37.927 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 15:32:37.967 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 15:32:37.969 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 15:32:37.972 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:692: Http Proxy port - Client closed the connection (id 25)
311 | 15:32:38.007 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 15:32:38.055 |  |  |  |  | XML→ | Media-Server
313 | 15:32:38.056 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
314 | 15:32:38.059 |  |  |  |  | ←SIP 200 OK | P-CSCF
315 | 15:32:38.078 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
316 | 15:32:38.082 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
317 | 15:32:38.084 |  |  |  |  | ←SIP 200 OK | P-CSCF
318 | 15:32:38.085 |  |  |  |  | MIKEY | Media-Server
319 | 15:32:38.369 |  |  |  |  | XML→ | Media-Server
320 | 15:32:38.373 |  |  |  |  | Protected MCData Message | -
321 | 15:32:38.419 |  |  |  |  | ←XML | Media-Server
322 | 15:32:38.420 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47744;transp... |  |  |
323 | 15:32:38.422 |  |  |  |  | ←SIP NOTIFY | P-CSCF
324 | 15:32:38.460 |  |  |  |  | →SIP 200 OK | P-CSCF
325 | 15:32:38.463 |  |  |  |  | ←XML | Media-Server
326 | 15:32:38.467 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
327 | 15:32:38.469 |  |  |  |  | ←SIP MESSAGE | P-CSCF
328 | 15:32:38.815 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
329 | 15:32:38.822 |  |  |  |  | →SIP 200 OK | P-CSCF
330 | 15:32:40.829 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
331 | 15:32:40.857 |  | ←RRC DCCH RRC connection release |  |  |
332 | 15:32:40.858 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
333 | 15:32:40.872 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
334 | 15:32:40.873 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1145: Test-Body Step 1
335 | 15:32:40.875 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request the establishment of a remotely initiated ambient listening call to user B
336 | 15:32:40.877 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
337 | 15:32:40.877 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1148: Test-Body Step 2
338 | 15:32:45.053 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
339 | 15:32:45.053 |  | →RRC CCCH RRC connection request |  |  |
340 | 15:32:45.053 |  | ←RRC CCCH RRC connection setup |  |  |
341 | 15:32:45.053 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
342 | 15:32:45.087 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
343 | 15:32:45.087 |  | →RRC DCCH RRC connection setup complete |  |  |
344 | 15:32:45.087 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
345 | 15:32:45.087 |  |  |  | →NAS EMM Service request |  |
346 | 15:32:45.087 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
347 | 15:32:45.087 |  |  |  | NAS K-enb e3b18bc6cb896f22f12e7da4eabdf231c... |  |
348 | 15:32:45.087 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
349 | 15:32:45.088 |  |  | RRC K-enb e3b18bc6cb896f22f12e7da4eabdf231c... |  |  |
350 | 15:32:45.088 |  |  | RRC EUTRA band combinations |  |  |
351 | 15:32:45.088 |  |  | RRC rrc-cip 2a857679886a83f545ecd83dcc4e726... |  |  |
352 | 15:32:45.088 |  |  | RRC rrc-int 3c0c0c1cab98bd30505a09516ff73b9... |  |  |
353 | 15:32:45.088 |  |  | RRC up-cip cb8d531cf0c6ac392f82cb69760bcd7b... |  |  |
354 | 15:32:45.088 |  |  | RRC up-int d6256b8b93a7007b39e879a94eea9101... |  |  |
355 | 15:32:45.088 |  | ←RRC DCCH Security mode command |  |  |
356 | 15:32:45.089 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
357 | 15:32:45.127 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
358 | 15:32:45.127 |  | →RRC DCCH Security mode complete |  |  |
359 | 15:32:45.127 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
360 | 15:32:45.127 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
361 | 15:32:45.167 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
362 | 15:32:45.167 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
363 | 15:32:45.199 |  |  |  |  | →SIP INVITE | P-CSCF
364 | 15:32:45.208 |  |  |  |  | MIKEY | Media-Server
365 | 15:32:45.507 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:759: SRTP config: Master Key: 699064AEBA18C66E5A008E9139C1B646, Master Salt: D979D3181CAC960516F64D4A, MKI: 2D2D6CA1
366 | 15:32:45.507 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:185: RTP and FloorControl ports configured 192.168.16.111:60350:60351:60354
367 | 15:32:45.511 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
368 | 15:32:45.512 |  |  |  |  | XML→ | Media-Server
369 | 15:32:45.517 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
370 | 15:32:45.519 |  |  |  |  | ←SIP 100 Trying | P-CSCF
371 | 15:32:46.133 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
372 | 15:32:46.134 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
373 | 15:32:46.134 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
374 | 15:32:46.135 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
375 | 15:32:46.167 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
376 | 15:32:46.167 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
377 | 15:32:46.167 |  | →RRC DCCH UL information transfer |  |  |
378 | 15:32:46.167 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
379 | 15:32:46.167 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
380 | 15:32:46.176 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
381 | 15:32:46.220 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
382 | 15:32:46.222 |  |  |  |  | ←SIP 200 OK | P-CSCF
383 | 15:32:46.462 |  |  |  |  | →SIP ACK | P-CSCF
384 | 15:32:46.468 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1150: Step 2 Verdict: Pass
385 | 15:32:46.469 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1154: Test-Body Step 4
386 | 15:32:46.470 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1157: Test-Body Step 5
387 | 15:32:46.471 |  | ←enobeB PCAP frame← |  |  |
388 | 15:32:46.471 |  |  |  |  | UserCheck: Does the UE (MCPTT client) notify the user that the remotely initiated ambient listening call has been established?
389 | 15:32:46.473 |  |  |  |  | ←Floor Taken | Media-Server
390 | 15:32:50.383 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1158: Step 5 Verdict: Pass
391 | 15:32:50.383 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1160: Test-Body Step 6
392 | 15:32:50.384 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1163: Test-Body Step 6A
393 | 15:32:50.486 |  |  |  |  | MMICmd: Request PTT token
394 | 15:32:55.388 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1166: Test-Body Step 7 - 8
395 | 15:32:55.490 |  |  |  |  | MMICmd: Release call (hang up the call)
396 | 15:32:58.695 | →enobeB PCAP frame→ SIP over IPSEC: BYE sip:mcptt-session-A@cf.mcstaasting.com SIP/2.0... |  |  |  |
397 | 15:32:58.701 |  |  |  |  | →SIP BYE | P-CSCF
398 | 15:32:58.704 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
399 | 15:32:58.706 |  |  |  |  | ←SIP 200 OK | P-CSCF
400 | 15:32:58.887 | →enobeB PCAP frame→ |  |  |  |
401 | 15:33:00.715 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
402 | 15:33:00.733 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
403 | 15:33:00.734 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
404 | 15:33:00.734 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
405 | 15:33:00.735 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
406 | 15:33:00.767 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
407 | 15:33:00.767 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
408 | 15:33:00.767 |  | →RRC DCCH UL information transfer |  |  |
409 | 15:33:00.767 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
410 | 15:33:00.767 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
411 | 15:33:00.782 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
412 | 15:33:00.783 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
413 | 15:33:00.811 |  | ←RRC DCCH RRC connection release |  |  |
414 | 15:33:00.812 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
415 | 15:33:00.825 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
416 | 15:33:00.826 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1168: Step 8 Verdict: Pass
417 | 15:33:00.827 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1172: Test-Body Step 11
418 | 15:33:00.828 |  |  |  |  | MMICmd: Make the UE (MCPTT client) request the establishment of a remotely initiated ambient listening call to user B
419 | 15:33:00.830 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
420 | 15:33:00.830 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1175: Test-Body Step 12
421 | 15:33:05.473 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
422 | 15:33:05.473 |  | →RRC CCCH RRC connection request |  |  |
423 | 15:33:05.473 |  | ←RRC CCCH RRC connection setup |  |  |
424 | 15:33:05.473 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
425 | 15:33:05.527 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
426 | 15:33:05.527 |  | →RRC DCCH RRC connection setup complete |  |  |
427 | 15:33:05.527 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
428 | 15:33:05.527 |  |  |  | →NAS EMM Service request |  |
429 | 15:33:05.527 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
430 | 15:33:05.527 |  |  |  | NAS K-enb 3a05d0a9a797ebccc2ab79c7714c5d8c5... |  |
431 | 15:33:05.527 |  |  |  | NAS HINTS imsi=001010123456001 imeisv=01514... |  |
432 | 15:33:05.528 |  |  | RRC K-enb 3a05d0a9a797ebccc2ab79c7714c5d8c5... |  |  |
433 | 15:33:05.528 |  |  | RRC EUTRA band combinations |  |  |
434 | 15:33:05.528 |  |  | RRC rrc-cip e210c3eb0d4a6db6b10774b931f61ac... |  |  |
435 | 15:33:05.528 |  |  | RRC rrc-int 52d7707bca42c58c2d04e0eb139977f... |  |  |
436 | 15:33:05.528 |  |  | RRC up-cip 7ad52d2147e06856534e01964be73bd2... |  |  |
437 | 15:33:05.528 |  |  | RRC up-int eaea20625898305586ba68868a7108fe... |  |  |
438 | 15:33:05.528 |  | ←RRC DCCH Security mode command |  |  |
439 | 15:33:05.529 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
440 | 15:33:05.567 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
441 | 15:33:05.567 |  | →RRC DCCH Security mode complete |  |  |
442 | 15:33:05.567 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
443 | 15:33:05.567 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
444 | 15:33:05.607 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
445 | 15:33:05.607 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
446 | 15:33:05.639 |  |  |  |  | →SIP INVITE | P-CSCF
447 | 15:33:05.649 |  |  |  |  | MIKEY | Media-Server
448 | 15:33:05.942 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
449 | 15:33:05.943 |  |  |  |  | XML→ | Media-Server
450 | 15:33:05.946 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
451 | 15:33:05.949 |  |  |  |  | ←SIP 100 Trying | P-CSCF
452 | 15:33:06.573 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
453 | 15:33:06.574 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
454 | 15:33:06.574 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
455 | 15:33:06.575 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
456 | 15:33:06.607 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
457 | 15:33:06.607 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
458 | 15:33:06.607 |  | →RRC DCCH UL information transfer |  |  |
459 | 15:33:06.607 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
460 | 15:33:06.607 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
461 | 15:33:06.616 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
462 | 15:33:06.651 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
463 | 15:33:06.653 |  |  |  |  | ←SIP 200 OK | P-CSCF
464 | 15:33:06.900 |  |  |  |  | →SIP ACK | P-CSCF
465 | 15:33:06.901 |  | ←enobeB PCAP frame← |  |  |
466 | 15:33:06.902 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1177: Step 12 Verdict: Pass
467 | 15:33:06.902 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1181: Test-Body Step 14
468 | 15:33:06.903 |  |  |  |  | ←XML | Media-Server
469 | 15:33:06.903 |  |  |  |  | ←Floor Taken | Media-Server
470 | 15:33:06.910 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:47744;transport... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
471 | 15:33:06.911 |  |  |  |  | ←SIP BYE | P-CSCF
472 | 15:33:06.935 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
473 | 15:33:06.940 |  |  |  |  | →SIP 200 OK | P-CSCF
474 | 15:33:07.247 | →enobeB PCAP frame→ |  |  |  |
475 | 15:33:08.943 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
476 | 15:33:08.947 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
477 | 15:33:08.948 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
478 | 15:33:08.948 |  | ←RRC DCCH RRC connection reconfiguration |  |  |
479 | 15:33:08.949 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
480 | 15:33:08.967 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
481 | 15:33:08.967 |  | →RRC DCCH RRC connection reconfiguration com... |  |  |
482 | 15:33:08.967 |  | →RRC DCCH UL information transfer |  |  |
483 | 15:33:08.967 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
484 | 15:33:08.967 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
485 | 15:33:08.981 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
486 | 15:33:08.982 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
487 | 15:33:09.010 |  | ←RRC DCCH RRC connection release |  |  |
488 | 15:33:09.011 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
489 | 15:33:09.024 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
490 | 15:33:09.026 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1188: Step 16 Verdict: Pass
491 | 15:33:09.028 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
492 | 15:33:09.029 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
493 | 15:33:09.777 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.