#######################################################################

# Anritsu Generated PICS/PIXIT file

#

# Changes Applied: 3GPP_TS_34.123-3_AND_NR_n257_AND_NR_n257

#######################################################################

pc_1xCSfallback,                             BOOLEAN,       false   #-- @desc  Support of 1xCS fallback #-- @spec 36.523-2, A.4.2.1.1-1/3

pc_1xRTT,                                    BOOLEAN,       false   #-- @desc  UE supports CDMA2000 1xRTT band class #-- @spec 36.523-2, A.4.1-1/4

pc_4Layer_spatial_mux_tm3_tm4,               BOOLEAN,       false   #-- @desc  Support of 4 layer spatial multiplexing with transmission mode 3 and transmission mode 4 #-- @spec 36.523-2 A.4.4-1/159

pc_5GCN,                                     BOOLEAN,       false   #-- @desc  UE supports 5GS Core #-- @spec 38.508-2 Table A.4.1-5/1

pc_5GCN_N3AN,                                BOOLEAN,       false   #-- @desc  UE supports 5GS Core over non-3GPP Access Network #-- @spec 38.508-2 Table A.4.1-5/2

pc_5GC_NSSAA,                                BOOLEAN,       false   #-- @desc  Support of network slice-specific authentication and authorization #-- @spec 38.508-2 Table A.4.3.7-1/26

pc_5GC_NSSAA_EAP_AKA_Prime,                  BOOLEAN,       false   #-- @desc  Support of EAP-AKA as EAP method for network slice-specific authentication and authorization #-- @spec 38.508-2 Table A.4.3.7-1/27

pc_5GC_NSSRG,                                BOOLEAN,       false   #-- @desc  Support of Network Slice Simultaneous Registration Group #-- @spec 38.508-2 Table A.4.3.7-1/37

pc_5GC_RACS,                                 BOOLEAN,       false   #-- @desc  Support of RACS #-- @spec 38.508-2 Table A.4.3.7-1/17

pc_5GC_RACS_Manufacturer_URCID,              BOOLEAN,       false   #-- @desc  UE support of Manufacturer assigned radio capability ID #-- @spec 38.508-2 Table A.4.3.7-1/35

pc_5GS_IMS_eCall_Capable,                    BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services over 5GS #-- @spec 38.508-2 Table A.4.3.7-1/18

pc_5GS_IMS_eCall_Only,                       BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services over 5GS #-- @spec 34.229-2 Table A.12/64

pc_A5_4_CS,                                  BOOLEAN,       false   #-- @desc  Support of A54 #-- @spec 51.010-2, A.2/87

pc_APN_Default_Configuration,                ENUM-APN_DefaultConfiguration_Type,internet #-- @desc  The DNNAPN configuration specified in TS 38.508-1 [2] Table 4.8.4-1 which is to be used for the default DNNAPN. #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_Ethernet,                          CHARSTRING,    Ethernet #-- @desc  APNDNN ID of type Ethernet #-- @spec 

pc_APN_ID_IMS,                               CHARSTRING,    IMS     #-- @desc  APNDNN ID of type IMS #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_Internet,                          CHARSTRING,    internet #-- @desc  APNDNN ID of type Internet #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_MIOT,                              CHARSTRING,    MIOT    #-- @desc  APNDNN ID of type MIOT #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_ID_URLLC,                             CHARSTRING,    URLLC   #-- @desc  APNDNN ID of type URLLC #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_ID_V2X,                               CHARSTRING,    V2X     #-- @desc  APNDNN ID of type V2X #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_RateControl,                          BOOLEAN,       false   #-- @desc  The UE supports APN rate control #-- @spec 36.523-2 A.4.4-2/27

pc_A_BDS,                                    BOOLEAN,       false   #-- @desc Support for A-BDS #-- @spec 37.571-3 Table A.4.3-2/18

pc_A_GLONASS,                                BOOLEAN,       false   #-- @desc Support for A-GLONASS #-- @spec 37.571-3 Table A.4.3-2/7

pc_A_GPS_ADR,                                BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Gps #-- @spec 37.571-3 Table A.4.3-6/1

pc_A_GPS_ADR_ENH,                            BOOLEAN,       false   #-- @desc Support of ADR enhancements for Gps #-- @spec 37.571-3 Table A.4.3-6/13

pc_A_GPS_HA,                                 BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Gps #-- @spec 37.571-3 Table A.4.3-6/19

pc_A_GPS_L1C,                                BOOLEAN,       false   #-- @desc Support of A-GPS L1C signal #-- @spec 37.571-3 Table A.4.3-5/1

pc_A_GPS_L1C_A,                              BOOLEAN,       false   #-- @desc Support for A-GPS L1C/A #-- @spec 37.571-3 Table A.4.3-2/6

pc_A_GPS_L1C_A_MGPS,                         BOOLEAN,       false   #-- @desc Support for A-GPS L1C/A and Modernized GPS #-- @spec 37.571-3 Table A.4.3-2/8

pc_A_GPS_L2C,                                BOOLEAN,       false   #-- @desc Support of A-GPS L2C signal #-- @spec 37.571-3 Table A.4.3-5/2

pc_A_GPS_L5,                                 BOOLEAN,       false   #-- @desc Support of A-GPS L5 signal #-- @spec 37.571-3 Table A.4.3-5/3

pc_A_GPS_VelocityMeas,                       BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Gps #-- @spec 37.571-3 Table A.4.3-6/6

pc_A_Galileo,                                BOOLEAN,       false   #-- @desc Support for A-Galileo #-- @spec 37.571-3 Table A.4.3-2/9

pc_A_QZSS,                                   BOOLEAN,       false   #-- @desc Support of A-QZSS #-- @spec 37.571-3 Table A.4.3-2/14

pc_A_SBAS,                                   BOOLEAN,       false   #-- @desc Support of A-SBAS #-- @spec 37.571-3 Table A.4.3-2/13

pc_Additional_PDU_establishment,             BOOLEAN,       false   #-- @desc  ExpectedNoOfPDUSessionsAtRegistration + 1 #-- @spec 38.508-2 Table A.4.3.7-1/9

pc_Allowed_CSG_list,                         BOOLEAN,       false   #-- @desc  Support of Allowed CSG list #-- @spec 36.523-2 A.4.4-1/2

pc_Attach,                                   BOOLEAN,       false   #-- @desc  Support EPS attach (with or without pre-configuration) #-- @spec 36.523-2 A.4.4-2/1

pc_AttachWithIMSI,                           BOOLEAN,       false   #-- @desc  Support of Attach With IMSI #-- @spec 34.123-2 A.10/34

pc_AttachWithPDN,                            BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED with PDN #-- @spec 36.523-2 A.4.4.1-1/X3

pc_AttachWithoutPDN,                         BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED without PDN #-- @spec 36.523-2 A.4.4.1-1/X2

pc_Auto_Attach_after_TAU_Reject,             BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) after the TAU Reject #-- @spec 

pc_Auto_PDN_Connectivity,                    BOOLEAN,       false   #-- @desc  Support of automatic PDN Connectivity in EUTRAN #-- @spec 36.523-2 A.4.4-1/68

pc_AutomaticAttachSwitchON,                  BOOLEAN,       false   #-- @desc  Support of automatic PS attach procedure at switch on. #-- @spec 34.123-2 A.20/38

pc_Automatic_EPS_Re_Attach,                  BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) #-- @spec 36.523-2 A.4.4-1/64

pc_Automatic_Re_Attach,                      BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) during Network Initiated Detach with detach type set to re-attach required #-- @spec 36.523-2 A.4.4-1/27

pc_Autonomous_search_function_nr_CAG,        BOOLEAN,       false   #-- @desc  Support of autonomous search function to detect CAG cells on serving and non-serving frequencies #-- @spec 38.508-2 Table A.4.3.7-1/yz

pc_Available_PLMNs_AcT_Ind,                  BOOLEAN,       false   #-- @desc  Support of AccessTechnology indication in available PLMNs list #-- @spec 36.523-2 A.4.4-1/78

pc_B41_UE_PC2,                               BOOLEAN,       false   #-- @desc  Support of TDD Band 41 Power class 2 operation #-- @spec 36.523-2 A.4.4-1/139

pc_BDS,                                      BOOLEAN,       false   #-- @desc Support for BDS #-- @spec 37.571-3 Table A.4.3-1/13

pc_BDS_ADR,                                  BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for BDS #-- @spec 37.571-3 Table A.4.3-6/11

pc_BDS_ADR_ENH,                              BOOLEAN,       false   #-- @desc Support of ADR enhancements for BDS #-- @spec 37.571-3 Table A.4.3-6/18

pc_BDS_B1C,                                  BOOLEAN,       false   #-- @desc  Support for A-BDS B1C #-- @spec 37.571-3 Table A.4.3-5/17

pc_BDS_B1I,                                  BOOLEAN,       false   #-- @desc Support for A-BDS B1I #-- @spec 37.571-3 Table A.4.3-5/16

pc_BDS_B2a,                                  BOOLEAN,       false   #-- @desc  Support of B2a signal in BDS #-- @spec 37.571-3 Table A.4.3-5/18

pc_BDS_B3I,                                  BOOLEAN,       false   #-- @desc  Support of B3I signal in BDS #-- @spec 37.571-3 Table A.4.3-5/19

pc_BDS_DiffCorr,                             BOOLEAN,       false   #-- @desc Bbds-DifferentialCorrectionsSupport for B1I #-- @spec 37.571-3 Table A.4.3-7/59

pc_BDS_GridMod,                              BOOLEAN,       false   #-- @desc Bbds-GridModelSupport #-- @spec 37.571-3 Table A.4.3-7/60

pc_BDS_HA,                                   BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for BDS #-- @spec 37.571-3 Table A.4.3-6/24

pc_BDS_VelocityMeas,                         BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for BDS #-- @spec 37.571-3 Table A.4.3-6/12

pc_BSRVCC,                                   BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.ps2cs-srvcc-orig-pre-alerting media feature tag in INVITE request #-- @spec 34.229-2 A.12/36

pc_Background,                               BOOLEAN,       false   #-- @desc  UE Supports Background QoS class #-- @spec 34.123-2 A.6/4

pc_Band10_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 10 #-- @spec 34.123-2 A.15/22

pc_Band11_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 11 #-- @spec 34.123-2 Table A.15/23

pc_Band12_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 12 #-- @spec 34.123-2 Table A.15/24

pc_Band13_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 13 #-- @spec 34.123-2 Table A.15/25

pc_Band14_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 14 #-- @spec 34.123-2 Table A.15/26

pc_Band19_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 19 #-- @spec 34.123-2 Table A.15/27

pc_Band1_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 1 #-- @spec 34.123-2 A.15/2

pc_Band20_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 20 #-- @spec 34.123-2 Table A.15/30

pc_Band21_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 21 #-- @spec 34.123-2 Table A.15/28

pc_Band22_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 22 #-- @spec 34.123-2 Table A.15/29

pc_Band25_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 25 #-- @spec 34.123-2 Table A.15/31

pc_Band26_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 26 #-- @spec 34.123-2 Table A.15/32

pc_Band2_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 2 #-- @spec 34.123-2 A.15/3

pc_Band32_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 32 #-- @spec 34.123-2 A.15/33

pc_Band3_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 3 #-- @spec 34.123-2 A.15/14

pc_Band4_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 4 #-- @spec 34.123-2 A.15/15

pc_Band5_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 5 #-- @spec 34.123-2 A.15/16

pc_Band6_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 6 #-- @spec 34.123-2 A.15/17

pc_Band7_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 7 #-- @spec 34.123-2 A.15/18

pc_Band8_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 8 #-- @spec 34.123-2 A.15/19

pc_Band9_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 9 #-- @spec 34.123-2 A.15/20

pc_Bds_DiffCorr_B1C,                         BOOLEAN,       false   #-- @desc Bds-DifferentialCorrectionsSupport for B1C #-- @spec 37.571-3 Table A.4.3-7/103

pc_BidirecVoiceOverIMS,                      BOOLEAN,       false   #-- @desc  UE capable of initiating a bidirectional voice session over IMS #-- @spec 34.229-2 Table A.12/12

pc_Bluetooth,                                BOOLEAN,       false   #-- @desc Support for UE-Assisted Bluetooth #-- @spec 37.571-3 Table A.4.3-2/22

pc_CAG,                                      BOOLEAN,       false   #-- @desc  Support of Closed Access Group #-- @spec 38.508-2 Table A.4.3.7-1/23

pc_CE_Measurements,                          BOOLEAN,       false   #-- @desc  Support of intra-frequency RSRQ measurements and inter-frequency RSRP and RSRQ measurements in RRC_CONNECTED #-- @spec 38.508-2 Table A.4.4-1A/16

pc_CEmodeA,                                  BOOLEAN,       false   #-- @desc  Support of CE mode A #-- @spec 36.523-2 A.4.4-1/122

pc_CEmodeB,                                  BOOLEAN,       false   #-- @desc  Support of CE mode B #-- @spec 36.523-2 A.4.4-1/123

pc_CMAS_Message,                             BOOLEAN,       false   #-- @desc  Support of CMAS message #-- @spec 36.523-2 A.4.4-1/58

pc_CMAS_NR,                                  BOOLEAN,       TRUE    #-- @desc  Support of CMAS message on NR #-- @spec 38.508-2 Table A.4.3.7-1/7

pc_CRS_Interference_Handling,                BOOLEAN,       false   #-- @desc  Support of CRS interference handling #-- @spec 36.523-2 A.4.4-1A/7

pc_CS,                                       BOOLEAN,       TRUE    #-- @desc  UE supports CS domain services #-- @spec 34.123-2 A.3/1

pc_CSI_RS_DS_Meas,                           BOOLEAN,       false   #-- @desc  Support of CSI-RS based discovery signals measurement #-- @spec 36.523-2 A.4.4-1/118

pc_CS_Em_Call_in_1xRTT,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in 1xRTT #-- @spec 36.523-2 A.4.4-1/37

pc_CS_Em_Call_in_GERAN,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in GERAN #-- @spec 36.523-2 A.4.4-1/36

pc_CS_Em_Call_in_UTRA,                       BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in UTRA #-- @spec 36.523-2 A.4.4-1/35

pc_CS_Fallback,                              BOOLEAN,       false   #-- @desc  The UE supports CS fallback for voice calls. If true pc_CS and at least one of pc_FDD pc_TDD_HCR pc_TDD_LCR pc_TDD_VHCR or pc_UMTS_GSM is also true. #-- @spec 36.523-2, A.4.2.1.1-1/1

pc_CS_MO_LR_CSFallback,                      BOOLEAN,       false   #-- @desc Support for CS-MO-LR with CS Fallback for a position estimate #-- @spec 37.571-3 Table A.4.3-3/4

pc_CS_PS_data_centric,                       BOOLEAN,       false   #-- @desc  Support of CSPS mode 2 #-- @spec 36.523-2 A.4.4-2/5

pc_CS_PS_voice_centric,                      BOOLEAN,       false   #-- @desc  Support of configuring the UE to voice centric #-- @spec 36.523-2 A.4.4-2/4

pc_Category_M1_voice,                        BOOLEAN,       false   #-- @desc  Support for GSMA PRD NG.108 "IMS Profile for Voice and SMS for UE Category M1" #-- @spec 36.523-2 A.4.4-1/145

pc_Combined_Attach,                          BOOLEAN,       TRUE    #-- @desc  Support combined EPSIMSI attach (with or without pre-configuration) #-- @spec 36.523-2 A.4.4-2/2

pc_CommunicationHold_DuringEmergencyCall,    BOOLEAN,       false   #-- @desc  UE supports Communication Hold during emergency call #-- @spec 34.229-2, Table A.12/33

pc_Concatenated_SMS_IP_MO,                   BOOLEAN,       false   #-- @desc  Concatenated SM-over-IP sender #-- @spec 34.229-2 Table A.3A/64

pc_Concatenated_SMS_IP_MT,                   BOOLEAN,       false   #-- @desc  Concatenated SM-over-IP receiver #-- @spec 34.229-2 Table A.3A/65

pc_Control_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of Control Plane CIoT #-- @spec 36.523-2 A.4.4-1/143

pc_DC_SCG_DRB,                               BOOLEAN,       false   #-- @desc  Support of DC SCG DRB #-- @spec 36.523-2 A.4.2.1.1-1/10

pc_DC_Split_DRB,                             BOOLEAN,       false   #-- @desc  Support of DC Split DRB #-- @spec 36.523-2 A.4.2.1.1-1/9

pc_DL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of downlink 256 QAM #-- @spec 36.523-2 A.4.4-1/116

pc_DL_AoD_periodicalReporting_UEA,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode #-- @spec 37.571-3 Table A.4.3-6E/7

pc_DL_AoD_periodicalReporting_UEB,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode #-- @spec 37.571-3 Table A.4.3-6E/6

pc_DL_AoD_periodicalReporting_standalone,    BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode #-- @spec 37.571-3 Table A.4.3-6E/5

pc_DL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 2 carriers #-- @spec 36.523-2 A.4.3.3-1/1

pc_DL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 3 carriers #-- @spec 36.523-2 A.4.3.3-1/2

pc_DL_NR_CA_3CC,                             BOOLEAN,       false   #-- @desc  DL NR CA with 3 carriers #-- @spec 38.508-2 Table A.4.3.2A.1-1/2

pc_DL_PRS_RSRP_MeasFR1,                      BOOLEAN,       false   #-- @desc  Support of DL-PRS-RSRP-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6F/3

pc_DL_PRS_RSRP_MeasFR2,                      BOOLEAN,       false   #-- @desc  Support of DL-PRS-RSRP-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6F/4

pc_DL_TDOA_additionalPathsReport,            BOOLEAN,       false   #-- @desc  Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-6F/5

pc_DL_TDOA_periodicalReporting_UEA,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode #-- @spec 37.571-3 Table A.4.3-6F/8

pc_DL_TDOA_periodicalReporting_UEB,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode #-- @spec 37.571-3 Table A.4.3-6F/7

pc_DL_TDOA_periodicalReporting_standalone,   BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode #-- @spec 37.571-3 Table A.4.3-6F/6

pc_DL_interBand_CaBwClassComb_AA,            BOOLEAN,       TRUE    #-- @desc  DL Inter-band contiguous CA BW class A-A #-- @spec 36.523-2 A.4.3.3.3-1/1

pc_DL_intraBand_ContCaBWclassB,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class B #-- @spec 36.523-2 A.4.3.3.1-1/1

pc_DL_intraBand_ContCaBWclassC,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class C #-- @spec 36.523-2 A.4.3.3.1-1/2

pc_DL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       TRUE    #-- @desc  Support of DL intra-band non-contiguous CA BW Class Combination A-A #-- @spec 36.523-2 A.4.3.3.2-1/1

pc_DRX_Adaptation,                           BOOLEAN,       false   #-- @desc  Supports DRX adaptation #-- @spec 38.508-2 Table A.4.3.5-1/5

pc_DSMIPv6,                                  BOOLEAN,       false   #-- @desc  Support of Mobility management based on Dual-Stack Mobile IPv6 #-- @spec 36.523-2 A.4.4-1/6

pc_DaylightSavingTime,                       BOOLEAN,       false   #-- @desc  UE storesupdates the daylight saving time when receives information #-- @spec 36.523-2 A.4.4-1/93

pc_DualRM_Coding,                            BOOLEAN,       false   #-- @desc  Dual RM Coding #-- @spec 36.523/2 A.4.4-1/1ZZ

pc_Dynamic_GERAN_Rel_downgrade,              BOOLEAN,       false   #-- @desc  Dynamically downgrades the GERAN release when the support of EPS is disabled #-- @spec 36.523-2, A.4.4-2/18

pc_EAB,                                      BOOLEAN,       false   #-- @desc  Support of Extended Access Barring #-- @spec 36.523-2 A.4.4-1A/4

pc_EAB_override,                             BOOLEAN,       false   #-- @desc  Support of Extended Access Barring Override #-- @spec 36.523-2 A.4.4-1/91

pc_ECID,                                     BOOLEAN,       false   #-- @desc Support of UE assisted ECID #-- @spec 37.571-3 Table A.4.3-2/5

pc_ECID_Rsrp,                                BOOLEAN,       false   #-- @desc Support fo RSRP #-- @spec 37.571-3 Table A.4.3-4/1

pc_ECID_Rsrq,                                BOOLEAN,       false   #-- @desc Support of RSRQ #-- @spec 37.571-3 Table A.4.3-4/2

pc_ECID_UeRxTx,                              BOOLEAN,       false   #-- @desc Support of UE Rx-Tx Time Difference #-- @spec 37.571-3 Table A.4.3-4/3

pc_ECID_idleStateForMeasurements,            BOOLEAN,       false   #-- @desc Support of idleStateForMeasurements #-- @spec 37.571-3 Table A.4.3-2/7

pc_ECID_onNR,                                BOOLEAN,       false   #-- @desc  Support of UE assisted ECID (based on LTE signals) on NR #-- @spec 37.571-3 Table A.4.3-2/43

pc_ECID_periodicalReporting,                 BOOLEAN,       false   #-- @desc Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-4/5

pc_ECID_triggeredReporting,                  BOOLEAN,       false   #-- @desc Support of triggeredReporting #-- @spec 37.571-3 Table A.4.3-4/6

pc_ECID_ueRxTxSupTDD,                        BOOLEAN,       false   #-- @desc Support of ueRxTxSupTDD #-- @spec 37.571-3 Table A.4.3-4/4

pc_EDCH_UE_Category_FDD,                     INTEGER,       1       #-- @desc  FDD E-DCH physical layer categories #-- @spec 34.123-2 Table A.18a.2

pc_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  LCR TDD E-DCH physical layer categories #-- @spec 34.123-2 Table A.18b.2

pc_EDTM,                                     BOOLEAN,       false   #-- @desc  Support for EDTM #-- @spec 36.523-2 A.4.4-1/38

pc_EMM_Information,                          BOOLEAN,       false   #-- @desc  Support of EMM Information message #-- @spec 36.523-2 A.4.4-1/9

pc_EN_DC,                                    BOOLEAN,       TRUE    #-- @desc  EN-DC (Option 3) #-- @spec 38.508-2 Table A.4.1-1/5

pc_EN_DC_NR_UL_2CC,                          BOOLEAN,       false   #-- @desc  EN-DC with 2 NR UL carriers #-- @spec 38.508-2 Table A.4.3.2B.2.0-2A/2

pc_EPC_MO_LR_RequestAssistanceData,          BOOLEAN,       false   #-- @desc Support of EPC-MO-LR request for assistance data #-- @spec 37.571-3 Table A.4.3-3/1

pc_EPC_MO_LR_RequestPositionEstimate,        BOOLEAN,       false   #-- @desc Support of EPC-MO-LR request for a position estimate #-- @spec 37.571-3 Table A.4.3-3/2

pc_EPC_RACS,                                 BOOLEAN,       false   #-- @desc  Support of RACS #-- @spec 36.523-2 A.4.4-1/III

pc_EPS_IMS_EmergencyCall,                    BOOLEAN,       false   #-- @desc  Support of MS emergency call in EPS #-- @spec 36.523-2, A.4.2.1.1-1/4

pc_EPS_IMS_eCall_Capable,                    BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services over EPS #-- @spec 34.229-2 Table A.12/54

pc_EPS_IMS_eCall_Only,                       BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services over EPS #-- @spec 34.229-2 Table A.12/55

pc_EPS_Services_Disable,                     BOOLEAN,       false   #-- @desc  Support of disabling of EPS services #-- @spec 36.523-2 A.4.4-1/26

pc_EPS_fallback,                             BOOLEAN,       false   #-- @desc  Support of EPS fallback #-- @spec 38.508-2 Table A.4.3.7-1/12

pc_ESM_MO_Bearer_Allocation,                 BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource allocation procedure #-- @spec 36.523-2 A.4.4-1/19

pc_ESM_MO_Bearer_Modification,               BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource modification procedure #-- @spec 36.523-2 A.4.4-1/11

pc_ESM_Notification,                         BOOLEAN,       false   #-- @desc  Support of ESM Notification procedure #-- @spec 36.523-2 A.4.4.1-71

pc_ESM_UE_Modification_NW_TFT,               BOOLEAN,       false   #-- @desc  Support for UE requested modification of network allocated TFTs #-- @spec 36.523-2 A.4.4-1/54

pc_ETWS_NR,                                  BOOLEAN,       TRUE    #-- @desc  Support of ETWS message on NR #-- @spec 38.508-2 Table A.4.3.7-1/8

pc_ETWS_message,                             BOOLEAN,       false   #-- @desc  Support of ETWS message #-- @spec 36.523-2 A.4.4-1/20

pc_E_UTRAN_2_GERAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support for inter-RAT PS handover from E_UTRAN to GERAN #-- @spec 36.523-2 A.4.4-1/52

pc_E_UTRA_WLAN_offload,                      BOOLEAN,       false   #-- @desc  Support Offload tofrom WLAN and supports S2b #-- @spec 36.523-2 A.4.2.1.1-1/8

pc_EarlyMedia,                               BOOLEAN,       false   #-- @desc  UE supports early media #-- @spec 34.229-2 Table A.12/45

pc_EmergSpeech,                              BOOLEAN,       false   #-- @desc  Emergency Call #-- @spec 34.123-2 A.2/2

pc_EmergencyService_fallback,                BOOLEAN,       false   #-- @desc  Support of emergency services fallback #-- @spec 38.508-2 Table A.4.3.7-1/11

pc_Enable_Disable_SMSoverIMS,                BOOLEAN,       false   #-- @desc  UE supports enablingdisabling SMS over IMS #-- @spec 34.229-2 Table A.12/58

pc_Enhanced_1xCSfallback,                    BOOLEAN,       false   #-- @desc  Support of Enhanced 1xCS fallback #-- @spec 36.523-2, A.4.2.1.1-1/6

pc_FDD,                                      BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.101 #-- @spec 34.123-2 A.1/1

pc_FDD_TypeB_HalfDuplex,                     BOOLEAN,       false   #-- @desc  Support of Type B Half duplex FDD operation #-- @spec 36.523-2 A.4.4-1/103

pc_FDPCH,                                    BOOLEAN,       false   #-- @desc  Full support of F-DPCH #-- @spec 34.123-2 Table A.18a/19

pc_Fast_First_HPPLMN_Search,                 BOOLEAN,       false   #-- @desc  Support of Fast First Higher Piority PLMN search #-- @spec 36.523-2 A.4.4-1/138

pc_FeatrGrp_101_F,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling #-- @spec 36.523-2 A.4.5-3a/1

pc_FeatrGrp_101_T,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling #-- @spec 36.523-2 A.4.5-3b/1

pc_FeatrGrp_102_F,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports) #-- @spec 36.523-2 A.4.5-3a/2

pc_FeatrGrp_102_T,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports) #-- @spec 36.523-2 A.4.5-3b/2

pc_FeatrGrp_103_F,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/3

pc_FeatrGrp_103_T,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/3

pc_FeatrGrp_104_F,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/4

pc_FeatrGrp_104_T,                           BOOLEAN,       TRUE    #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/4

pc_FeatrGrp_105_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/5

pc_FeatrGrp_105_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/5

pc_FeatrGrp_106_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/6

pc_FeatrGrp_106_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/6

pc_FeatrGrp_107_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/7

pc_FeatrGrp_107_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/7

pc_FeatrGrp_108_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/8

pc_FeatrGrp_108_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/8

pc_FeatrGrp_109_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1 #-- @spec 36.523-2 A.4.5-3a/9

pc_FeatrGrp_109_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1 #-- @spec 36.523-2 A.4.5-3b/9

pc_FeatrGrp_10_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change) #-- @spec 36.523-2 A.4.5-1a/10

pc_FeatrGrp_10_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change) #-- @spec 36.523-2 A.4.5-1b/10

pc_FeatrGrp_110_F,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2 #-- @spec 36.523-2 A.4.5-3a/10

pc_FeatrGrp_110_T,                           BOOLEAN,       TRUE    #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2 #-- @spec 36.523-2 A.4.5-3b/10

pc_FeatrGrp_111_F,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6 #-- @spec 36.523-2 A.4.5-3a/11

pc_FeatrGrp_111_T,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6 #-- @spec 36.523-2 A.4.5-3b/11

pc_FeatrGrp_112_F,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure #-- @spec 36.523-2 A.4.5-3a/12

pc_FeatrGrp_112_T,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure #-- @spec 36.523-2 A.4.5-3b/12

pc_FeatrGrp_113_F,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells #-- @spec 36.523-2 A.4.5-3a/13

pc_FeatrGrp_113_T,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells #-- @spec 36.523-2 A.4.5-3b/13

pc_FeatrGrp_114_F,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report #-- @spec 36.523-2 A.4.5-3a/14

pc_FeatrGrp_114_T,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report #-- @spec 36.523-2 A.4.5-3b/14

pc_FeatrGrp_115_F,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction #-- @spec 36.523-2 A.4.5-3a/15

pc_FeatrGrp_115_T,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction #-- @spec 36.523-2 A.4.5-3b/15

pc_FeatrGrp_116_F,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL #-- @spec 36.523-2 A.4.5-3a/16

pc_FeatrGrp_116_T,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL #-- @spec 36.523-2 A.4.5-3b/16

pc_FeatrGrp_11_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover #-- @spec 36.523-2 A.4.5-1a/11

pc_FeatrGrp_11_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover #-- @spec 36.523-2 A.4.5-1b/11

pc_FeatrGrp_12_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover #-- @spec 36.523-2 A.4.5-1a/12

pc_FeatrGrp_12_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover #-- @spec 36.523-2 A.4.5-1b/12

pc_FeatrGrp_13_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD) #-- @spec 36.523-2 A.4.5-1a/13

pc_FeatrGrp_13_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD) #-- @spec 36.523-2 A.4.5-1b/13

pc_FeatrGrp_14_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2 #-- @spec 36.523-2 A.4.5-1a/14

pc_FeatrGrp_14_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2 #-- @spec 36.523-2 A.4.5-1b/14

pc_FeatrGrp_15_F,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold #-- @spec 36.523-2 A.4.5-1a/15

pc_FeatrGrp_15_T,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold #-- @spec 36.523-2 A.4.5-1b/15

pc_FeatrGrp_16_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements #-- @spec 36.523-2 A.4.5-1a/16

pc_FeatrGrp_16_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements #-- @spec 36.523-2 A.4.5-1b/16

pc_FeatrGrp_17_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1a/17

pc_FeatrGrp_17_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1b/17

pc_FeatrGrp_18_F,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1a/18

pc_FeatrGrp_18_T,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1b/18

pc_FeatrGrp_19_F,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events #-- @spec 36.523-2 A.4.5-1a/19

pc_FeatrGrp_19_T,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events #-- @spec 36.523-2 A.4.5-1b/19

pc_FeatrGrp_1_F,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI #-- @spec 36.523-2 A.4.5-1a/1

pc_FeatrGrp_1_T,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI #-- @spec 36.523-2 A.4.5-1b/1

pc_FeatrGrp_20_F,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB #-- @spec 36.523-2 A.4.5-1a/20

pc_FeatrGrp_20_T,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB #-- @spec 36.523-2 A.4.5-1b/20

pc_FeatrGrp_21_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1 #-- @spec 36.523-2 A.4.5-1a/21

pc_FeatrGrp_21_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1 #-- @spec 36.523-2 A.4.5-1b/21

pc_FeatrGrp_22_F,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/22

pc_FeatrGrp_22_T,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/22

pc_FeatrGrp_23_F,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/23

pc_FeatrGrp_23_T,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/23

pc_FeatrGrp_24_F,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/24

pc_FeatrGrp_24_T,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/24

pc_FeatrGrp_25_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/25

pc_FeatrGrp_25_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/25

pc_FeatrGrp_26_F,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/26

pc_FeatrGrp_26_T,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/26

pc_FeatrGrp_27_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover #-- @spec 36.523-2 A.4.5-1a/27

pc_FeatrGrp_27_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover #-- @spec 36.523-2 A.4.5-1b/27

pc_FeatrGrp_28_F,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling #-- @spec 36.523-2 A.4.5-1a/28

pc_FeatrGrp_28_T,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling #-- @spec 36.523-2 A.4.5-1b/28

pc_FeatrGrp_29_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling #-- @spec 36.523-2 A.4.5-1a/29

pc_FeatrGrp_29_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling #-- @spec 36.523-2 A.4.5-1b/29

pc_FeatrGrp_2_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI #-- @spec 36.523-2 A.4.5-1a/2

pc_FeatrGrp_2_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI #-- @spec 36.523-2 A.4.5-1b/2

pc_FeatrGrp_30_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD #-- @spec 36.523-2 A.4.5-1a/30

pc_FeatrGrp_30_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD #-- @spec 36.523-2 A.4.5-1b/30

pc_FeatrGrp_31_F,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList #-- @spec 36.523-2 A.4.5-1a/31

pc_FeatrGrp_31_T,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList #-- @spec 36.523-2 A.4.5-1b/31

pc_FeatrGrp_33_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to reportStrongestCellsForSON #-- @spec 36.523-2 A.4.5-1d/1

pc_FeatrGrp_33_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including: #-- @spec 36.523-2 A.4.5-1e/1

pc_FeatrGrp_34_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including: #-- @spec 36.523-2 A.4.5-1d/2

pc_FeatrGrp_34_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including: #-- @spec 36.523-2 A.4.5-1e/2

pc_FeatrGrp_35_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including: #-- @spec 36.523-2 A.4.5-1d/3

pc_FeatrGrp_35_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including: #-- @spec 36.523-2 A.4.5-1e/3

pc_FeatrGrp_36_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including: #-- @spec 36.523-2 A.4.5-1d/4

pc_FeatrGrp_36_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to portStrongestCellsForSON #-- @spec 36.523-2 A.4.5-1e/4

pc_FeatrGrp_37_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including: #-- @spec 36.523-2 A.4.5-1d/5

pc_FeatrGrp_37_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including: #-- @spec 36.523-2 A.4.5-1e/5

pc_FeatrGrp_38_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/6

pc_FeatrGrp_38_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/6

pc_FeatrGrp_39_F,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/7

pc_FeatrGrp_39_T,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/7

pc_FeatrGrp_3_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN #-- @spec 36.523-2 A.4.5-1a/3

pc_FeatrGrp_3_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN #-- @spec 36.523-2 A.4.5-1b/3

pc_FeatrGrp_40_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/8

pc_FeatrGrp_40_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/8

pc_FeatrGrp_41_F,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1 #-- @spec 36.523-2 A.4.5-1d/9

pc_FeatrGrp_41_T,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1 #-- @spec 36.523-2 A.4.5-1e/9

pc_FeatrGrp_42_F,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) #-- @spec 36.523-2 A.4.5-1d/10

pc_FeatrGrp_42_T,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) #-- @spec 36.523-2 A.4.5-1e/10

pc_FeatrGrp_4_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle #-- @spec 36.523-2 A.4.5-1a/4

pc_FeatrGrp_4_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle #-- @spec 36.523-2 A.4.5-1b/4

pc_FeatrGrp_5_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Long DRX cycle DRX command MAC control element #-- @spec 36.523-2 A.4.5-1a/5

pc_FeatrGrp_5_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Long DRX cycle DRX command MAC control element #-- @spec 36.523-2 A.4.5-1b/5

pc_FeatrGrp_6_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate #-- @spec 36.523-2 A.4.5-1a/6

pc_FeatrGrp_6_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate #-- @spec 36.523-2 A.4.5-1b/6

pc_FeatrGrp_7_F,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM #-- @spec 36.523-2 A.4.5-1a/7

pc_FeatrGrp_7_T,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM #-- @spec 36.523-2 A.4.5-1b/7

pc_FeatrGrp_8_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover #-- @spec 36.523-2 A.4.5-1a/8

pc_FeatrGrp_8_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover #-- @spec 36.523-2 A.4.5-1b/8

pc_FeatrGrp_9_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover #-- @spec 36.523-2 A.4.5-1a/9

pc_FeatrGrp_9_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover #-- @spec 36.523-2 A.4.5-1b/9

pc_FixedBroadband,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Broadband #-- @spec 34.229-2 Table A.18/3

pc_FlexibleStartPRB_PDSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PDSCH #-- @spec 36.523-2 A.4.4-1/222

pc_FlexibleStartPRB_PUSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PUSCH #-- @spec 36.523-2 A.4.4-1/223

pc_FlightPathPlan,                           BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement #-- @spec 36.523-2 A.4.4-1/kkj

pc_FullNameNetwork,                          BOOLEAN,       false   #-- @desc  Support of storage of the network full name #-- @spec 36.523-2 A.4.4-1/12

pc_GALILEO,                                  BOOLEAN,       false   #-- @desc Support for Galileo #-- @spec 37.571-3 Table A.4.3-1/9

pc_GALILEO_ADR,                              BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Galileo #-- @spec 37.571-3 Table A.4.3-6/16

pc_GALILEO_ADR_ENH,                          BOOLEAN,       false   #-- @desc Support of ADR enhancements for Galileo #-- @spec 37.571-3 Table A.4.3-6/5

pc_GALILEO_E1,                               BOOLEAN,       false   #-- @desc Support of E1 signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/11

pc_GALILEO_E5a,                              BOOLEAN,       false   #-- @desc Support of E5a signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/12

pc_GALILEO_E5aE5b,                           BOOLEAN,       false   #-- @desc Support of E5a+E5b signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/15

pc_GALILEO_E5b,                              BOOLEAN,       false   #-- @desc Support of E5b signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/13

pc_GALILEO_E6,                               BOOLEAN,       false   #-- @desc Support of E6 signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/14

pc_GALILEO_HA,                               BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Galileo #-- @spec 37.571-3 Table A.4.3-6/22

pc_GALILEO_VelocityMeas,                     BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Galileo #-- @spec 37.571-3 Table A.4.3-6/9

pc_GERAN,                                    BOOLEAN,       false   #-- @desc  UE Supports GSM andor GPRS #-- @spec 36.523-2 A.4.1-1/7

pc_GERAN_2_E_UTRAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support of GERAN to E-UTRAN PS Handover #-- @spec 36.523-2 A.4.4-1/29

pc_GERAN_2_E_UTRAN_meas,                     BOOLEAN,       false   #-- @desc  Supports Neighbour Cell measurements and Network controlled & autonomous cell reselection to E-UTRAN #-- @spec 36.523-2 A.4.4-1/21

pc_GERAN_2_E_UTRAN_measreporting_CCN,        BOOLEAN,       false   #-- @desc  Supports CCN towards E-UTRAN E-UTRAN Neighbour cell measurement reporting and Network controlled cell reselection to E-UTRAN #-- @spec 36.523-2 A.4.4-1/39

pc_GLONASS,                                  BOOLEAN,       false   #-- @desc Support for GLONASS #-- @spec 37.571-3 Table A.4.3-1/7

pc_GLONASS_ADR,                              BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Glonass #-- @spec 37.571-3 Table A.4.3-6/5

pc_GLONASS_ADR_ENH,                          BOOLEAN,       false   #-- @desc Support of ADR enhancements for Glonass #-- @spec 37.571-3 Table A.4.3-6/17

pc_GLONASS_G1,                               BOOLEAN,       false   #-- @desc Support of G1 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/8

pc_GLONASS_G2,                               BOOLEAN,       false   #-- @desc Support of G2 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/9

pc_GLONASS_G3,                               BOOLEAN,       false   #-- @desc Support of G3 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/10

pc_GLONASS_HA,                               BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Glonass #-- @spec 37.571-3 Table A.4.3-6/23

pc_GLONASS_VelocityMeas,                     BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Glonass #-- @spec 37.571-3 Table A.4.3-6/10

pc_GNSS_AA,                                  BOOLEAN,       false   #-- @desc Support of GNSS Acquisition Assistance #-- @spec 37.571-3 Table A.4.3-2/12

pc_GNSS_AcquAssistSup_BDS,                   BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/55

pc_GNSS_AcquAssistSup_Galileo,               BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for Galileo #-- @spec 37.571-3 Table A.4.3-7/33

pc_GNSS_AcquAssistSup_Glonass,               BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/34

pc_GNSS_AcquAssistSup_Gps,                   BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for GPS #-- @spec 37.571-3 Table A.4.3-7/30

pc_GNSS_AcquAssistSup_Qzss,                  BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/32

pc_GNSS_AcquAssistSup_Sbas,                  BOOLEAN,       false   #-- @desc Gnss-AcquisitionAssistanceSupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/31

pc_GNSS_AcquAssist_BDS_B1C,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/99

pc_GNSS_AcquAssist_BDS_B1I,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/98

pc_GNSS_AcquAssist_GPS_L1CA,                 BOOLEAN,       false   #-- @desc Support of GNSS-AcquisitionAssistance for GPS L1 C/A #-- @spec 37.571-3 Table A.4.3-7/61

pc_GNSS_AcquAssist_GPS_L5,                   BOOLEAN,       false   #-- @desc Support of GNSS-AcquisitionAssistance for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/62

pc_GNSS_AcquAssist_Galileo_E1,               BOOLEAN,       false   #-- @desc Support of GNSS-AcquisitionAssistance for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/63

pc_GNSS_AcquAssist_Galileo_E5A,              BOOLEAN,       false   #-- @desc Support of GNSS-AcquisitionAssistance for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/64

pc_GNSS_AlmanacSup_BDS,                      BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for BDS (Model-7) #-- @spec 37.571-3 Table A.4.3-7/56

pc_GNSS_AlmanacSup_Galileo,                  BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for Galileo (Model-1) #-- @spec 37.571-3 Table A.4.3-7/38

pc_GNSS_AlmanacSup_Glonass,                  BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for GLONASS (Model-5) #-- @spec 37.571-3 Table A.4.3-7/39

pc_GNSS_AlmanacSup_Gps,                      BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for GPS (Model-2) #-- @spec 37.571-3 Table A.4.3-7/35

pc_GNSS_AlmanacSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for QZSS (Model-2) #-- @spec 37.571-3 Table A.4.3-7/37

pc_GNSS_AlmanacSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-AlmanacSupport for SBAS (Model-6) #-- @spec 37.571-3 Table A.4.3-7/36

pc_GNSS_AuxInfoSup_BDS,                      BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/58

pc_GNSS_AuxInfoSup_Galileo,                  BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for Galileo #-- @spec 37.571-3 Table A.4.3-7/48

pc_GNSS_AuxInfoSup_Glonass,                  BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/49

pc_GNSS_AuxInfoSup_Gps,                      BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for GPS #-- @spec 37.571-3 Table A.4.3-7/45

pc_GNSS_AuxInfoSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/47

pc_GNSS_AuxInfoSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-AuxiliaryInformationSupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/46

pc_GNSS_DGNSS_Sup_BDS,                       BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/51

pc_GNSS_DGNSS_Sup_Bds_B1C,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/102

pc_GNSS_DGNSS_Sup_Galileo,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/13

pc_GNSS_DGNSS_Sup_Galileo_E5A,               BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/101

pc_GNSS_DGNSS_Sup_Glonass,                   BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/14

pc_GNSS_DGNSS_Sup_Gps,                       BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GPS L1 C/A #-- @spec 37.571-3 Table A.4.3-7/10

pc_GNSS_DGNSS_Sup_Gps_L5,                    BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/100

pc_GNSS_DGNSS_Sup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/12

pc_GNSS_DGNSS_Sup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-DifferentialCorrectionsSupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/11

pc_GNSS_DataBitsSup_BDS,                     BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/54

pc_GNSS_DataBitsSup_Galileo,                 BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for Galileo #-- @spec 37.571-3 Table A.4.3-7/28

pc_GNSS_DataBitsSup_Glonass,                 BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/29

pc_GNSS_DataBitsSup_Gps,                     BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for GPS #-- @spec 37.571-3 Table A.4.3-7/25

pc_GNSS_DataBitsSup_Qzss,                    BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/27

pc_GNSS_DataBitsSup_Sbas,                    BOOLEAN,       false   #-- @desc Gnss-DataBitAssistanceSupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/26

pc_GNSS_EOPSup,                              BOOLEAN,       false   #-- @desc Gnss-EarthOrientationParametersSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/4

pc_GNSS_EllipArc,                            BOOLEAN,       false   #-- @desc Ellipsoid Arc Support #-- @spec 37.571-3 Table A.4.3-8/7

pc_GNSS_EllipPoint,                          BOOLEAN,       false   #-- @desc Ellipsoid Point Support #-- @spec 37.571-3 Table A.4.3-8/1

pc_GNSS_EllipPointAlt,                       BOOLEAN,       false   #-- @desc Ellipsoid Point With Altitude Support #-- @spec 37.571-3 Table A.4.3-8/5

pc_GNSS_EllipPointAltUncertEllip,            BOOLEAN,       false   #-- @desc Ellipsoid Point With Altitude And Uncertainty Ellipsoid Support #-- @spec 37.571-3 Table A.4.3-8/6

pc_GNSS_EllipPointUncertCircle,              BOOLEAN,       false   #-- @desc Ellipsoid Point With Uncertainty Circle Support #-- @spec 37.571-3 Table A.4.3-8/2

pc_GNSS_EllipPointUncertEllip,               BOOLEAN,       false   #-- @desc Ellipsoid Point With Uncertainty Ellipse Support #-- @spec 37.571-3 Table A.4.3-8/3

pc_GNSS_FTA,                                 BOOLEAN,       false   #-- @desc Support of GNSS Fine Time Assistance #-- @spec 37.571-3 Table A.4.3-2/3

pc_GNSS_FTA_UEA,                             BOOLEAN,       false   #-- @desc Support of UE Fine Time Assistance measurements for UE-assisted Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/11

pc_GNSS_FTA_UEB,                             BOOLEAN,       false   #-- @desc Support of UE Fine Time Assistance measurements for UE-based Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/10

pc_GNSS_HA_EllipPointAltUncertEllip,         BOOLEAN,       false   #-- @desc High Accuracy Ellipsoid Point With Altitude And Uncertainty Ellipsoid-r15 #-- @spec 37.571-3 Table A.4.3-8/9

pc_GNSS_HA_EllipPointUncertCircle,           BOOLEAN,       false   #-- @desc High Accuracy Ellipsoid Point With Uncertainty Ellipse-r15 #-- @spec 37.571-3 Table A.4.3-8/8

pc_GNSS_HVVel,                               BOOLEAN,       false   #-- @desc Horizontal With Vertical Velocity Support #-- @spec 37.571-3 Table A.4.3-9/2

pc_GNSS_HVVelUncert,                         BOOLEAN,       false   #-- @desc Horizontal With Vertical Velocity And Uncertainty Support #-- @spec 37.571-3 Table A.4.3-9/4

pc_GNSS_HVel,                                BOOLEAN,       false   #-- @desc Horizontal Velocity Support #-- @spec 37.571-3 Table A.4.3-9/1

pc_GNSS_HVelUncert,                          BOOLEAN,       false   #-- @desc Horizontal Velocity With Uncertainty Support #-- @spec 37.571-3 Table A.4.3-9/3

pc_GNSS_IonoModSup,                          BOOLEAN,       false   #-- @desc Gnss-IonosphericModelSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/3

pc_GNSS_NavModSup_BDS,                       BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for BDS (Model-6) #-- @spec 37.571-3 Table A.4.3-7/52

pc_GNSS_NavModSup_Galileo,                   BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for Galileo (Model-1) #-- @spec 37.571-3 Table A.4.3-7/18

pc_GNSS_NavModSup_Glonass,                   BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for GLONASS (Model-4) #-- @spec 37.571-3 Table A.4.3-7/19

pc_GNSS_NavModSup_Gps,                       BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for GPS (Model-2) #-- @spec 37.571-3 Table A.4.3-7/15

pc_GNSS_NavModSup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for QZSS (Model-2) #-- @spec 37.571-3 Table A.4.3-7/17

pc_GNSS_NavModSup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-NavigationModelSupport for SBAS (Model-5) #-- @spec 37.571-3 Table A.4.3-7/16

pc_GNSS_Polygon,                             BOOLEAN,       false   #-- @desc Polygon Support #-- @spec 37.571-3 Table A.4.3-8/4

pc_GNSS_RTISup_BDS,                          BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for BDS #-- @spec 37.571-3 Table A.4.3-7/53

pc_GNSS_RTISup_Galileo,                      BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for Galileo #-- @spec 37.571-3 Table A.4.3-7/23

pc_GNSS_RTISup_Glonass,                      BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/24

pc_GNSS_RTISup_Gps,                          BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for GPS #-- @spec 37.571-3 Table A.4.3-7/20

pc_GNSS_RTISup_Qzss,                         BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/22

pc_GNSS_RTISup_Sbas,                         BOOLEAN,       false   #-- @desc Gnss-RealTimeIntegritySupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/21

pc_GNSS_RTK_AuxStationInfo,                  BOOLEAN,       false   #-- @desc Gnss-RTK-AuxiliaryStationDataSupport-r15 (Common assistance data) #-- @spec 37.571-3 Table A.4.3-7/66

pc_GNSS_RTK_BiasInfo_Glonass,                BOOLEAN,       false   #-- @desc Glo-RTK-BiasInformationSupport-r15 #-- @spec 37.571-3 Table A.4.3-7/74

pc_GNSS_RTK_FKP_Gradients_Bds,               BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/92

pc_GNSS_RTK_FKP_Gradients_Galileo,           BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/85

pc_GNSS_RTK_FKP_Gradients_Glonass,           BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/78

pc_GNSS_RTK_FKP_Gradients_Gps,               BOOLEAN,       false   #-- @desc Gnss-RTK-FKP-GradientsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/70

pc_GNSS_RTK_MAC_CorrectionDifferences_Bds,   BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/90

pc_GNSS_RTK_MAC_CorrectionDifferences_Galileo,BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/83

pc_GNSS_RTK_MAC_CorrectionDifferences_Glonass,BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/76

pc_GNSS_RTK_MAC_CorrectionDifferences_Gps,   BOOLEAN,       false   #-- @desc Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/68

pc_GNSS_RTK_OBS_Bds,                         BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/89

pc_GNSS_RTK_OBS_Bds_B1C,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/106

pc_GNSS_RTK_OBS_Galileo,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/82

pc_GNSS_RTK_OBS_Galileo_E5A,                 BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/105

pc_GNSS_RTK_OBS_Glonass,                     BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/75

pc_GNSS_RTK_OBS_Gps,                         BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GPS L1 C/A #-- @spec 37.571-3 Table A.4.3-7/67

pc_GNSS_RTK_OBS_Gps_L5,                      BOOLEAN,       false   #-- @desc Gnss-RTK-ObservationsSupport-r15 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/104

pc_GNSS_RTK_RefStationInfo,                  BOOLEAN,       false   #-- @desc Gnss-RTK-ReferenceStationInfoSupport-r15 (Common assistance data) #-- @spec 37.571-3 Table A.4.3-7/65

pc_GNSS_RTK_Residuals_Bds,                   BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/91

pc_GNSS_RTK_Residuals_Galileo,               BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/84

pc_GNSS_RTK_Residuals_Glonass,               BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/77

pc_GNSS_RTK_Residuals_Gps,                   BOOLEAN,       false   #-- @desc Gnss-RTK-ResidualsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/69

pc_GNSS_RTK_SSR_ClockCorrections_Bds,        BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/94

pc_GNSS_RTK_SSR_ClockCorrections_Galileo,    BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/87

pc_GNSS_RTK_SSR_ClockCorrections_Glonass,    BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/80

pc_GNSS_RTK_SSR_ClockCorrections_Gps,        BOOLEAN,       false   #-- @desc Gnss-SSR-ClockCorrectionsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/72

pc_GNSS_RTK_SSR_CodeBias_Bds,                BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/95

pc_GNSS_RTK_SSR_CodeBias_Bds_B1C,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/109

pc_GNSS_RTK_SSR_CodeBias_Galileo,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/88

pc_GNSS_RTK_SSR_CodeBias_Galileo_E5A,        BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/108

pc_GNSS_RTK_SSR_CodeBias_Glonass,            BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/81

pc_GNSS_RTK_SSR_CodeBias_Gps,                BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/73

pc_GNSS_RTK_SSR_CodeBias_Gps_L5,             BOOLEAN,       false   #-- @desc Gnss-SSR-CodeBiasSupport-r15 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/107

pc_GNSS_RTK_SSR_OrbitCorrections_Bds,        BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/93

pc_GNSS_RTK_SSR_OrbitCorrections_Galileo,    BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for Galileo #-- @spec 37.571-3 Table A.4.3-7/86

pc_GNSS_RTK_SSR_OrbitCorrections_Glonass,    BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/79

pc_GNSS_RTK_SSR_OrbitCorrections_Gps,        BOOLEAN,       false   #-- @desc Gnss-SSR-OrbitCorrectionsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/71

pc_GNSS_RefLocSup,                           BOOLEAN,       false   #-- @desc Gnss-ReferenceLocationSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/2

pc_GNSS_RefTimeSup,                          BOOLEAN,       false   #-- @desc Gnss-ReferenceTimeSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/1

pc_GNSS_SSR_GridCorrSupp_Bds,                BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/132

pc_GNSS_SSR_GridCorrSupp_Galileo,            BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/130

pc_GNSS_SSR_GridCorrSupp_Glonass,            BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/131

pc_GNSS_SSR_GridCorrSupp_Gps,                BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/128

pc_GNSS_SSR_GridCorrSupp_Qzss,               BOOLEAN,       false   #-- @desc Gnss-SSR-GriddedCorrectionSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/129

pc_GNSS_SSR_PhaseBias_Bds_B1C,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/122

pc_GNSS_SSR_PhaseBias_Bds_B1I,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/121

pc_GNSS_SSR_PhaseBias_Galileo_E1,            BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/118

pc_GNSS_SSR_PhaseBias_Galileo_E5A,           BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/119

pc_GNSS_SSR_PhaseBias_Glonass,               BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/120

pc_GNSS_SSR_PhaseBias_Gps_L1CA,              BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GPS L1 C/A #-- @spec 37.571-3 Table A.4.3-7/115

pc_GNSS_SSR_PhaseBias_Gps_L5,                BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/116

pc_GNSS_SSR_PhaseBias_Qzss,                  BOOLEAN,       false   #-- @desc Gnss-SSR-PhaseBiasSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/117

pc_GNSS_SSR_STEC_CorrSupp_Bds,               BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/127

pc_GNSS_SSR_STEC_CorrSupp_Galileo,           BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/125

pc_GNSS_SSR_STEC_CorrSupp_Glonass,           BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/126

pc_GNSS_SSR_STEC_CorrSupp_Gps,               BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/123

pc_GNSS_SSR_STEC_CorrSupp_Qzss,              BOOLEAN,       false   #-- @desc Gnss-SSR-STEC-CorrectionSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/124

pc_GNSS_SSR_URA_Bds,                         BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/114

pc_GNSS_SSR_URA_Galileo,                     BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/112

pc_GNSS_SSR_URA_Glonass,                     BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/113

pc_GNSS_SSR_URA_Gps,                         BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/110

pc_GNSS_SSR_URA_Qzss,                        BOOLEAN,       false   #-- @desc Gnss-SSR-URA-Support-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/111

pc_GNSS_TimeModSup_BDS,                      BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/50

pc_GNSS_TimeModSup_Galileo,                  BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for Galileo #-- @spec 37.571-3 Table A.4.3-7/8

pc_GNSS_TimeModSup_Glonass,                  BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for GLONASS #-- @spec 37.571-3 Table A.4.3-7/9

pc_GNSS_TimeModSup_Gps,                      BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for GPS #-- @spec 37.571-3 Table A.4.3-7/5

pc_GNSS_TimeModSup_Qzss,                     BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for QZSS #-- @spec 37.571-3 Table A.4.3-7/7

pc_GNSS_TimeModSup_Sbas,                     BOOLEAN,       false   #-- @desc Gnss-TimeModelsSupport for SBAS #-- @spec 37.571-3 Table A.4.3-7/6

pc_GNSS_UTCModSup_BDS,                       BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for BDS (Model-5) #-- @spec 37.571-3 Table A.4.3-7/57

pc_GNSS_UTCModSup_Galileo,                   BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for Galileo (Model-1) #-- @spec 37.571-3 Table A.4.3-7/43

pc_GNSS_UTCModSup_Glonass,                   BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for GLONASS (Model-3) #-- @spec 37.571-3 Table A.4.3-7/44

pc_GNSS_UTCModSup_Gps,                       BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for GPS (Model-1) #-- @spec 37.571-3 Table A.4.3-7/40

pc_GNSS_UTCModSup_Qzss,                      BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for QZSS (Model-1) #-- @spec 37.571-3 Table A.4.3-7/42

pc_GNSS_UTCModSup_Sbas,                      BOOLEAN,       false   #-- @desc Gnss-UTC-ModelSupport for SBAS (Model-4) #-- @spec 37.571-3 Table A.4.3-7/41

pc_GNSS_location_r16,                        BOOLEAN,       TRUE    #-- @desc  UE is equipped with a GNSS or A-GNSS receiver that may be used to provide detailed location information along with SON or MDT related measurements in RRC_CONNECTED RRC_IDLE and RRC_INACTIVE. #-- @spec 38.508-2 Table A.4.4-1/4

pc_GPRS,                                     BOOLEAN,       false   #-- @desc  Support of GPRS #-- @spec 51.010-2, A.2/41

pc_G_operation_mode_C,                       BOOLEAN,       false   #-- @desc  GERAN UE Operation Mode C #-- @spec 51.010-2, A.2/49

pc_HO_from_UTRA_to_eFDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (FDD) #-- @spec 36.523-2 A.4.4-1/8

pc_HO_from_UTRA_to_eTDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (TDD) #-- @spec 36.523-2 A.4.4-1/53

pc_HRPD,                                     BOOLEAN,       false   #-- @desc  UE supports CDMA2000 HRPD band class #-- @spec 36.523-2, A.4.1-1/3

pc_HSDPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - FDD #-- @spec 34.123-2 A.18a/14

pc_HSDPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - TDD #-- @spec 34.123-2 A.18b/10

pc_HSDSCH_UE_Category_FDD,                   INTEGER,       5       #-- @desc  FDD HS-DSCH physical layer categories #-- @spec 34.123-2 Table A.18a.1

pc_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  LCR TDD HS-DSCH physical layer categories #-- @spec 34.123-2 Table A.18b.1

pc_HSUPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - FDD #-- @spec 34.123-2 A.18a/18

pc_HSUPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - TDD #-- @spec 34.123-2 A.18b/14

pc_Highspeed_Enh_Prach,                      BOOLEAN,       false   #-- @desc  Support high speed enhancement for random access preambles generated from restricted set type B in high speed scenario as specifed in TS 36.211 #-- @spec 36.523-2 A.4.4-1/164

pc_HttpDigestAuthentication,                 BOOLEAN,       false   #-- @desc  HTTP Digest XCAP Authentication #-- @spec 34.229-2, Table A.6a/4

pc_HttpGBAAuthentication,                    BOOLEAN,       false   #-- @desc  GBA XCAP Authentication #-- @spec 34.229-2, Table A.6a/3

pc_IMS,                                      BOOLEAN,       false   #-- @desc  Support of IMS #-- @spec 36.523-2 A.4.4-1/25

pc_IMSI_Detach,                              BOOLEAN,       false   #-- @desc  Support of detach for non-EPS services #-- @spec 36.523-2 A.4.4-1/34

pc_IMS_5GS,                                  BOOLEAN,       false   #-- @desc  Support of IMS #-- @spec 38.508-2 Table A.4.4-1/2

pc_IMS_APN_default,                          BOOLEAN,       false   #-- @desc  Configured with IMS APN as default APN #-- @spec 36.523-2 A.4.4-2/11

pc_IMS_Audio_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE supports audio media feature tag #-- @spec 34.229-2 Table A.12/xx

pc_IMS_CS_PS_SRVCC,                          BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC #-- @spec 34.229-2 A.12/40

pc_IMS_CS_PS_SRVCCAlert,                     BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC in alerting state #-- @spec 34.229-2 A.12/41

pc_IMS_CS_PS_SRVCCMidCall,                   BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC and the MSC server assisted mid-call feature #-- @spec 34.229-2 A.12/42

pc_IMS_Deregistration,                       BOOLEAN,       false   #-- @desc  UE has the method that supports IMS deregistration #-- @spec 34.229-2 Table A.12/39

pc_IMS_Disable_Preconditions,                BOOLEAN,       false   #-- @desc  UE supports disabling preconditions #-- @spec 34.229-2 Table A.12/59

pc_IMS_E2ae,                                 BOOLEAN,       false   #-- @desc  UE supports end-to-access-edge media security using SDES #-- @spec 34.229-2 Table A.12/31

pc_IMS_EmergencyCall,                        BOOLEAN,       false   #-- @desc  UE supports IMS emergency services #-- @spec 34.229-2 Table A.12/26

pc_IMS_ExplicitConsultativeTransfer,         BOOLEAN,       false   #-- @desc  Explicit Communication Transfer - consultative transfer #-- @spec 34.229-2 Table A.16/11

pc_IMS_GIBA_Sec,                             BOOLEAN,       TRUE    #-- @desc  UE supports GIBA security only #-- @spec 34.229-2 Table A.6a/1

pc_IMS_GRUUsInSIP,                           BOOLEAN,       false   #-- @desc  UE supports obtaining and using GRUUs in the Session Initiation Protocol (SIP) #-- @spec 34.229-2 Table A.4/53

pc_IMS_Geolocation,                          BOOLEAN,       false   #-- @desc  UE is capable of obtaining location information #-- @spec 34.229-2 Table A.12/27

pc_IMS_SRVCCAlert,                           BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.srvcc-alerting media feature tag in INVITE request or 180 response #-- @spec 34.229-2 A.12/34

pc_IMS_Sec,                                  BOOLEAN,       TRUE    #-- @desc  UE supports full IMS security #-- @spec 34.229-2 Table A.6a/2

pc_IMS_Session_Timer,                        BOOLEAN,       false   #-- @desc  UE supports Session Timer #-- @spec 34.229-2 Table A.12/57

pc_IMS_Session_Timer_own_benefit,            BOOLEAN,       false   #-- @desc  UE uses Session Timer for its benefit alone #-- @spec 34.229-2 Table A.12/60

pc_IMS_Session_Timer_reINVITE,               BOOLEAN,       false   #-- @desc  UE supports usage of re-INVITE for session refresh #-- @spec 34.229-2 Table A.12/61

pc_IMS_TWS,                                  BOOLEAN,       false   #-- @desc  Three way session #-- @spec 34.229-2, Table A.16/14

pc_IMS_Video_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE indicates video media feature tag in REGISTER and INVITE request #-- @spec 34.229-2 Table A.12/32

pc_IMS_after_EmReg_rejection,                BOOLEAN,       false   #-- @desc  UE reattempts IMS emergency service without registration after rejection of emergency registration #-- @spec 34.229-2 Table A.12/52

pc_IMS_emergency_call,                       BOOLEAN,       false   #-- @desc  Support of MS emergency call #-- @spec 36.523-2, A.4.2.1.1-1/4

pc_IP_Ping,                                  BOOLEAN,       false   #-- @desc  Support of ICMP or ICMP IPv6 #-- @spec 38.508-2 Table A.4.4-1/1

pc_IPv4,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv4 (used IMS PICS as currently not defined in LTE) #-- @spec 34.229-2 A.7/1

pc_IPv4_Link_MTU_Parameter,                  BOOLEAN,       false   #-- @desc  UE supports IPv4 Link MTU parameter #-- @spec 36.523-2 A.4.4-2/26

pc_IPv6,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv6 (used IMS PICS as currently not defined in LTE) #-- @spec 34.229-2 A.7/2

pc_ISR,                                      BOOLEAN,       false   #-- @desc  Support of ISR #-- @spec 36.523-2 A.4.4-1/5

pc_ImmConnect,                               BOOLEAN,       false   #-- @desc  Immediate connection supported for all circuit switched basic services #-- @spec 34.123-2 A.20/6

pc_IndicateSigcomp,                          BOOLEAN,       false   #-- @desc  Indicate the willingness to receive the responses and requests compressed from initial REGISTER onwards by using the "comp=sigcomp" parameter #-- @spec 34.229-2 Table A.8/5

pc_InitiateP_CSCFDiscovery_viaDHCPv4,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv4 #-- @spec 34.229-2 Table A.13/1

pc_InitiateP_CSCFDiscovery_viaDHCPv6,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv6 #-- @spec 34.229-2 Table A.12/7

pc_InitiateP_CSCFDiscovery_viaPCO,           BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via PCO #-- @spec 34.229-2 Table A.12/5

pc_InitiateSession,                          BOOLEAN,       false   #-- @desc  Initiating a session #-- @spec 34.229-2 Table A.4/2B

pc_InitiatesDedicatedPDPContext,             BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate Dedicated PDP Context #-- @spec 34.229-2 Table A.12/4

pc_InterBand_CA_BetweenFR1_FR2,              BOOLEAN,       false   #-- @desc  Inter-Band CA between FR1 and FR2 #-- @spec 38.508-2 Table A.4.1-4A/7

pc_InterBand_CA_WithinFR1,                   BOOLEAN,       false   #-- @desc  Inter-Band CA within FR1 #-- @spec 38.508-2 Table A.4.1-4A/5

pc_InterBand_CA_WithinFR2,                   BOOLEAN,       false   #-- @desc  Inter-Band CA within FR2 #-- @spec 38.508-2 Table A.4.1-4A/6

pc_InterBand_ENDC_IncludingFR1_FR2,          BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including both FR1 and FR2 #-- @spec 38.508-2 Table A.4.1-4/5

pc_InterBand_ENDC_IncludingFR2,              BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including FR2 #-- @spec 38.508-2 Table A.4.1-4/4

pc_InterBand_ENDC_WithinFR1,                 BOOLEAN,       false   #-- @desc  Inter-Band EN-DC within FR1 #-- @spec 38.508-2 Table A.4.1-4/3

pc_InterBand_NRDC_BetweenFR1_FR2,            BOOLEAN,       false   #-- @desc  Inter-Band EN-DC bewtween FR1 and FR2 #-- @spec 38.508-2 Table A.4.1-4/6

pc_InterFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Inter Frequency Proximity Indication #-- @spec 36.523-2 A.4.4.1-b

pc_InterFreq_RSTD_WithGaps,                  BOOLEAN,       false   #-- @desc Support of inter-frequency RSTD measurements that require measurement gaps #-- @spec 37.571-3 Table A.4.3-2/16

pc_InterFreq_RSTD_withGaps,                  BOOLEAN,       false   #-- @desc Support of inter-frequency RSTD measurements that require measurement gaps #-- @spec 37.571-3 Table A.4.3-2/16

pc_InterRAT_DL_CompressedModeRequired,       BOOLEAN,       false   #-- @desc  UE supports DL DPCH compressed mode #-- @spec 34.123-2 A.18a/9a

pc_InterRAT_UL_CompressedModeRequired,       BOOLEAN,       false   #-- @desc  UE supports UL DPCH compressed mode #-- @spec 34.123-2 A.18a/8a

pc_Interactive,                              BOOLEAN,       false   #-- @desc  UE Supports Interactive QoS class #-- @spec 34.123-2 A.6/3

pc_IntraBand_Contiguous_CA_WithinFR1,        BOOLEAN,       false   #-- @desc  Intra-Band Contiguous CA within FR1 #-- @spec 38.508-2 Table A.4.1-4A/1

pc_IntraBand_Contiguous_CA_WithinFR2,        BOOLEAN,       false   #-- @desc  Intra-Band Contiguous CA within FR2 #-- @spec 38.508-2 Table A.4.1-4A/3

pc_IntraBand_Contiguous_ENDC,                BOOLEAN,       false   #-- @desc  Intra-Band Contiguous EN-DC #-- @spec 38.508-2 Table A.4.1-4/1

pc_IntraBand_NonContiguous_CA_WithinFR1,     BOOLEAN,       false   #-- @desc  Intra-Band Non-contiguous CA within FR1 #-- @spec 38.508-2 Table A.4.1-4A/2

pc_IntraBand_NonContiguous_CA_WithinFR2,     BOOLEAN,       false   #-- @desc  Intra-Band Non-contiguous CA within FR2 #-- @spec 38.508-2 Table A.4.1-4A/4

pc_IntraBand_NonContiguous_ENDC,             BOOLEAN,       false   #-- @desc  Intra-Band Non-Contiguous EN-DC #-- @spec 38.508-2 Table A.4.1-4/2

pc_IntraFreqA3_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of eventA3 for intra-frequency neighbouring cells in normal coverage and CE Mode A #-- @spec 36.523-2 A.4.4-1/141

pc_IntraFreqHO_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of intra-frequency handover to target cell in normal coverage and CE Mode A #-- @spec 36.523-2 A.4.4-1/142

pc_IntraFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Intra Frequency Proximity Indication #-- @spec 36.523-2 A.4.4.1-a

pc_KeepEpsBearerParametersAfterNormalDetach, BOOLEAN,       false   #-- @desc  If the UE supports this then the next ATTACH after DETACH shall be done using AT command AT+CGATT=1. #-- @spec 36.523-2 A.4.4.2-10

pc_LAP,                                      BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication. #-- @spec 34.123-2 A.10/31

pc_LAP_override,                             BOOLEAN,       false   #-- @desc  Support of Low Access Prioirty Override #-- @spec 34.123-2 A.10/37

pc_LPP,                                      BOOLEAN,       false   #-- @desc LTE Positioning Protocol (LPP) #-- @spec 37.571-3 Table A.4.2-1/1

pc_LPP_MsgSegmentation,                      BOOLEAN,       false   #-- @desc Support of LPP message segmentation #-- @spec 37.571-3 Table A.4.4-1/5

pc_LPP_SendingACK_ProvideCapabilities,       BOOLEAN,       false   #-- @desc Support of sending of acknowledgement request in LPP Provide Capabilities message #-- @spec 37.571-3 Table A.4.4-1/1

pc_LTE_UL_Segmentation,                      BOOLEAN,       false   #-- @desc  Support of RRC message Segmentation in the UL #-- @spec 36.523-2 A.4.4-1/216

pc_LocalTimeZone,                            BOOLEAN,       false   #-- @desc  Support of storage of the local time zone #-- @spec 36.523-2 A.4.4-1/14

pc_LoggedMeasurementsIdle,                   BOOLEAN,       false   #-- @desc  Support of logged measurements in RRC_IDLE #-- @spec 36.523-2 A.4.4-1/62

pc_MBS_AcquisitionAssist,                    BOOLEAN,       false   #-- @desc Support of mbs-AcquisitionAssistance #-- @spec 37.571-3 Table A.4.3-7A/2

pc_MBS_AlmanacAssist,                        BOOLEAN,       false   #-- @desc Support of mbs-AlmanacAssistance #-- @spec 37.571-3 Table A.4.3-7A/1

pc_MGPS,                                     BOOLEAN,       false   #-- @desc Support for Modernized GPS #-- @spec 37.571-3 Table A.4.3-1/8

pc_MO_PDU_Session_Modification,              BOOLEAN,       false   #-- @desc  Support of UE requested PDU session modification #-- @spec 38.508-2 Table A.4.3.7-1/13

pc_MTSI_ACR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Anonymous Communication Rejection #-- @spec 34.229-2 Table A.16/12

pc_MTSI_CommDivert,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Diversion #-- @spec 34.229-2 Table A.16/5

pc_MTSI_CommHold,                            BOOLEAN,       false   #-- @desc  Communication Hold #-- @spec 34.229-2 Table A.16/6

pc_MTSI_CommWaiting,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Waiting #-- @spec 34.229-2 Table A.16/13

pc_MTSI_Conference,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Conference #-- @spec 34.229-2 Table A.16/9

pc_MTSI_Incoming_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Incoming Communication Barring #-- @spec 34.229-2 Table A.16/7

pc_MTSI_MessageWait,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Message Waiting Indication #-- @spec 34.229-2 Table A.16/8

pc_MTSI_OIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Presentation #-- @spec 34.229-2 Table A.16/1

pc_MTSI_OIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction #-- @spec 34.229-2 Table A.16/2

pc_MTSI_OIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction - Configuration #-- @spec 34.229-2 Table A.16/2A

pc_MTSI_Outgoing_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Outgoing Communication Barring #-- @spec 34.229-2 Table A.16/15

pc_MTSI_Speech,                              BOOLEAN,       false   #-- @desc  MTSI media - Speech #-- @spec 34.229-2 Table A.15/1

pc_MTSI_Speech_AMRWB,                        BOOLEAN,       false   #-- @desc  MTSI media - Speech AMR wideband #-- @spec 34.229-2 Table A.15/2

pc_MTSI_Speech_EVS,                          BOOLEAN,       false   #-- @desc  MTSI media - Speech EVS #-- @spec 34.229-2 Table A.15/10

pc_MTSI_TIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Presentation #-- @spec 34.229-2 Table A.16/3

pc_MTSI_TIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction #-- @spec 34.229-2 Table A.16/4

pc_MTSI_TIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction - Configuration #-- @spec 34.229-2 Table A.16/4A

pc_MTSI_Video,                               BOOLEAN,       false   #-- @desc   MTSI media - Video #-- @spec 34.229-2 Table A.15/3

pc_MT_LR,                                    BOOLEAN,       false   #-- @desc Support of Mobile Terminated location request #-- @spec 37.571-3 tabel A.4.3-3/8

pc_MT_LR_loc_notif,                          BOOLEAN,       false   #-- @desc Support of EPC-MT-LR Location Notification #-- @spec 37.571-3 Table A.4.3-3/3

pc_Manual_CSG_Selection,                     BOOLEAN,       false   #-- @desc  Support of Manual CSG selection #-- @spec 36.523-2 A.4.4-1/49

pc_MinimumPeriodicSearchTimer,               BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer #-- @spec 34.123-2 A.10/32

pc_More_Than_128_CAbandComb,                 BOOLEAN,       false   #-- @desc  Support of more than 128 CA Band Combinations #-- @spec 36.523-2 A.4.4-1/102

pc_Multi_RTT,                                BOOLEAN,       false   #-- @desc  Support for UE-Assisted Multi-RTT #-- @spec 37.571-3 Table A.4.3-2/29

pc_Multi_RTT_additionalPathsReport,          BOOLEAN,       false   #-- @desc  Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-6C/7

pc_Multi_RTT_periodicalReporting,            BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-6C/8

pc_MultimediaTelephonyService,               BOOLEAN,       false   #-- @desc  Multimedia telephony service participant #-- @spec 34.229-2 Table A.3A/50

pc_Multiple_Cells_Meas_Ext,                  BOOLEAN,       false   #-- @desc  Support of measurement reporting triggered based on a number of cells #-- @spec 36.523-2 A.4.4-1/kkk

pc_Multiple_PDN,                             BOOLEAN,       false   #-- @desc  Support for multiple PDN connections #-- @spec 36.523-2 A.4.4-1/30

pc_NB_User_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of User Plane CIoT in NB-S1 mode #-- @spec 36.523-2 A.4.4-1/199

pc_NE_DC,                                    BOOLEAN,       false   #-- @desc  NE-DC (Option 4) #-- @spec 38.508-2 Table A.4.1-1/6

pc_NG102_Call_Combined_Registration_EUTRA,   BOOLEAN,       false   #-- @desc  Voice call after combined Registration E-UTRA #-- @spec 34.229-2 Table A.20/5

pc_NG102_Call_Combined_Registration_WLAN,    BOOLEAN,       false   #-- @desc  Voice call after combined Registration WLAN #-- @spec 34.229-2 Table A.20/7

pc_NG102_Combined_Registration_EUTRA,        BOOLEAN,       false   #-- @desc  Combined Registration E-UTRA #-- @spec 34.229-2 Table A.20/1

pc_NG102_Combined_Registration_WLAN,         BOOLEAN,       false   #-- @desc  Combined Registration WLAN #-- @spec 34.229-2 Table A.20/3

pc_NG102_Dual_Registration_EUTRA,            BOOLEAN,       false   #-- @desc  Dual Registration E-UTRA #-- @spec 34.229-2 Table A.20/2

pc_NG114_v1_0,                               BOOLEAN,       false   #-- @desc  Version 1.0 as of 07 August 2020 #-- @spec 34.229-2 Table A.21/1

pc_NG114_v1_0_EVS_A1,                        BOOLEAN,       false   #-- @desc  EVS Configuration A1 #-- @spec 34.229-2 Table A.22/mm

pc_NG114_v1_0_EVS_B0,                        BOOLEAN,       false   #-- @desc  EVS Configuration B0 #-- @spec 34.229-2 Table A.22/nn

pc_NG114_v1_0_audio,                         BOOLEAN,       false   #-- @desc  audio feature tag #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_default_config_evs_br,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBr #-- @spec 34.229-2 Table A.22/10

pc_NG114_v1_0_default_config_evs_bw,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBw #-- @spec 34.229-2 Table A.22/11

pc_NG114_v1_0_default_config_voice_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for voice exempt #-- @spec 34.229-2 Table A.22/8

pc_NG114_v1_0_final_SDP_offer,               BOOLEAN,       false   #-- @desc  final codec selection #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_first_SDP_answer,              BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to initial SDP offer #-- @spec 34.229-2 Table A.22/12

pc_NG114_v1_0_forking,                       BOOLEAN,       false   #-- @desc  Forking behavior #-- @spec 34.229-2 Table A.22/14

pc_NG114_v1_0_initial_SDP_offer,             BOOLEAN,       false   #-- @desc  Codecs and attributes in initial SDP offer #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_mmtel,                         BOOLEAN,       false   #-- @desc  mmtel ICSI value #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_second_SDP_answer,             BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to second SDP offer #-- @spec 34.229-2 Table A.22/13

pc_NG114_v1_0_video,                         BOOLEAN,       false   #-- @desc  video feature tag #-- @spec 34.229-2 Table A.22/

pc_NG114_v2_0,                               BOOLEAN,       false   #-- @desc  Version 2.0 as of 07 August 2021 #-- @spec 34.229-2 Table A.21/2

pc_NG114_v2_0_default_config_video_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for video exempt #-- @spec 34.229-2 Table A.22/9

pc_NGEN_DC,                                  BOOLEAN,       false   #-- @desc  NE-DC (Option 7) #-- @spec 38.508-2 Table A.4.1-1/7

pc_NG_RAN_EUTRA,                             BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA (Option 5) #-- @spec 38.508-2 Table A.4.1-3/4

pc_NG_RAN_NR,                                BOOLEAN,       false   #-- @desc  NG-RAN NR (Option 2) #-- @spec 38.508-2 Table A.4.1-3/1

pc_NGeFDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA FDD (Option 5) #-- @spec 38.508-2 Table A.4.1-1/3

pc_NGeTDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA TDD (Option 5) #-- @spec 38.508-2 Table A.4.1-1/4

pc_NMO_I_Behaviour,                          BOOLEAN,       false   #-- @desc  Support of the extended NMO I system information #-- @spec 34.123-2 A.10/33

pc_NR_5GC_EmergencyService_fallback,         BOOLEAN,       false   #-- @desc  Support of emergency services fallback in NR connected to 5GCN #-- @spec 38.508-2 Table A.4.3.7-1/11

pc_NR_5GC_EmergencyServices,                 BOOLEAN,       false   #-- @desc  Support of emergency services in NR connected to 5GCN #-- @spec 38.508-2 Table A.4.3.7-1/14

pc_NR_ECID,                                  BOOLEAN,       false   #-- @desc  Support for UE-Assisted NR E-CID #-- @spec 37.571-3 Table A.4.3-2/34

pc_NR_ECID_CSIRsrp,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRP #-- @spec 37.571-3 Table A.4.3-6A/3

pc_NR_ECID_CSIRsrq,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRQ #-- @spec 37.571-3 Table A.4.3-6A/4

pc_NR_ECID_SSRsrp,                           BOOLEAN,       false   #-- @desc  Support of SS RSRP #-- @spec 37.571-3 Table A.4.3-6A/1

pc_NR_ECID_SSRsrq,                           BOOLEAN,       false   #-- @desc  Support of SS RSRQ #-- @spec 37.571-3 Table A.4.3-6A/2

pc_NR_ECID_periodicalReporting,              BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-6A/5

pc_NR_ECID_triggeredReporting,               BOOLEAN,       false   #-- @desc  Support of triggeredReporting #-- @spec 37.571-3 Table A.4.3-6A/6

pc_NR_RRC_Release_With_Deprioritisation,     BOOLEAN,       false   #-- @desc  Support of  RRC connection release with deprioritisation #-- @spec 38.508-2 Table A.4.3.7-1/21

pc_NR_UL_SRS_Capability,                     BOOLEAN,       false   #-- @desc  Support for NR UL-SRS-Capability #-- @spec 37.571-3 Table A.4.3-2/35

pc_NR_UL_Segmentation,                       BOOLEAN,       false   #-- @desc  Support of RRC message Segmentation in the UL #-- @spec 38.508-2 Table A.4.3.7-1/18

pc_NR_dl_DedicatedMessageSegmentation,       BOOLEAN,       false   #-- @desc  Support of reception of segmented DL RRC messages #-- @spec Reference: 38.508-2 Table A.4.3.7-1/39

pc_NR_eDRX,                                  BOOLEAN,       false   #-- @desc  Support of Rel-17 extended DRX cycle up to 10485.76 seconds #-- @spec 38.508-2 Table A.4.3.7-1/43

pc_NR_ehc_r16,                               BOOLEAN,       false   #-- @desc  Support EHC (Ethernet header compression) #-- @spec 38.508-2 Table A.4.3.3-1/7

pc_NR_sl_TransmissionMode1_r16,              BOOLEAN,       false   #-- @desc  Support transmitting NR sidelink mode 1 scheduled by Uu #-- @spec 38.508-2 Table A.4.3.10-1/1

pc_NR_sl_TransmissionMode2_r16,              BOOLEAN,       false   #-- @desc  Support of NR sidelink transmission mode 2 #-- @spec 38.508-2 Table A.4.3.10-1/2

pc_NR_sl_csi_rs_portssidelink_p2,            BOOLEAN,       false   #-- @desc  Support of sidelink CSI report with 2 antenna ports #-- @spec 38.508-2 Table A.4.3.10-1/3

pc_NR_udc_continueUDC_r17,                   BOOLEAN,       false   #-- @desc  Support continuation of uplink data compression protocol operation #-- @spec 38.508-2 Table A.4.3.3-1/10

pc_NR_udc_r17,                               BOOLEAN,       false   #-- @desc  Support UDC (Uplink data compression) #-- @spec 38.508-2 Table A.4.3.3-1/8

pc_NR_udc_standardDictionary_r17,            BOOLEAN,       false   #-- @desc  Support standard Dictionary #-- @spec 38.508-2 Table A.4.3.3-1/9

pc_Navic_DGNSS_Sup,                          BOOLEAN,       false   #-- @desc Navic-DifferentialCorrectionsSupport-r16 for #-- @spec 37.571-3 Table A.4.3-7/133

pc_Navic_GridModelSupp,                      BOOLEAN,       false   #-- @desc Navic-GridModelSupport-r16 #-- @spec 37.571-3 Table A.4.3-7/134

pc_No_USIM_TestExecution,                    BOOLEAN,       false   #-- @desc  Support of test execution with no USIM #-- @spec 34.123-2 A.20/90

pc_NonIP_Link_MTU_Parameter,                 BOOLEAN,       false   #-- @desc  UE supports Non-IP Link MTU parameter #-- @spec 36.523-2 A.4.4-2/25

pc_OMA_LPPe,                                 BOOLEAN,       false   #-- @desc Support for OMA LPPe #-- @spec 37.571-3 Table A.4.2-1/2

pc_OTDOA,                                    BOOLEAN,       false   #-- @desc Support of UE assisted OTDOA #-- @spec 37.571-3 Table A.4.3-2/4

pc_OTDOA_additionalNeighbourCellInfoList,    BOOLEAN,       false   #-- @desc Support of additionalNeighbourCellInfoList #-- @spec 37.571-3 Table A.4.3-3A/2

pc_OTDOA_additionalPathsReport,              BOOLEAN,       false   #-- @desc Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-3A/7

pc_OTDOA_additional_prs_config,              BOOLEAN,       false   #-- @desc Support of additional-prs-config #-- @spec 37.571-3 Table A.4.3-3A/5

pc_OTDOA_densePrsConfig,                     BOOLEAN,       false   #-- @desc Support of densePrsConfig #-- @spec 37.571-3 Table A.4.3-3A/8

pc_OTDOA_idleStateForMeasurements,           BOOLEAN,       false   #-- @desc Support of idleStateForMeasurements #-- @spec 37.571-3 Table A.4.3-3A/15

pc_OTDOA_interFreqRSTDmeasurement,           BOOLEAN,       false   #-- @desc Support of interFreqRSTDmeasurement #-- @spec 37.571-3 Table A.4.3-3A/1

pc_OTDOA_interRAT_RSTDmeasurement,           BOOLEAN,       false   #-- @desc Support of interRAT-RSTDmeasurement #-- @spec 37.571-3 Table A.4.3-3A/18

pc_OTDOA_maxSupportedPrsBandwidth,           BOOLEAN,       false   #-- @desc Support of maxSupportedPrsBandwidth #-- @spec 37.571-3 Table A.4.3-3A/9

pc_OTDOA_maxSupportedPrsBandwidth_r14,       ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsBandwidth_r14,n6      #-- @desc  maxSupportedPrsBandwidth #-- @spec 37.571-3 Table A.4.3-3A/9

pc_OTDOA_maxSupportedPrsConfigs,             BOOLEAN,       false   #-- @desc Support of maxSupportedPrsConfigs #-- @spec 37.571-3 Table A.4.3-3A/12

pc_OTDOA_maxSupportedPrsConfigs_r14,         ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsConfigs_r14,c2      #-- @desc  maxSupportedPrsConfigs #-- @spec 37.571-3 Table A.4.3-3A/12

pc_OTDOA_motionMeasurements,                 BOOLEAN,       false   #-- @desc Support of motionMeasurements #-- @spec 37.571-3 Table A.4.3-3A/17

pc_OTDOA_multiPrbNprs,                       BOOLEAN,       false   #-- @desc Support of multiPrbNprs #-- @spec 37.571-3 Table A.4.3-3A/14

pc_OTDOA_numberOfRXantennas,                 BOOLEAN,       false   #-- @desc Support of numberOfRXantennas #-- @spec 37.571-3 Table A.4.3-3A/16

pc_OTDOA_numberOfRXantennas_r14,             ENUM-OTDOA_ProvideCapabilities.numberOfRXantennas_r14,rx1     #-- @desc  Support of numberOfRXantennas #-- @spec 37.571-3 Table A.4.3-3A/16

pc_OTDOA_onNR,                               BOOLEAN,       false   #-- @desc  Support of UE assisted OTDOA (based on LTE signals) on NR #-- @spec 37.571-3 Table A.4.3-2/42

pc_OTDOA_periodicalReporting,                BOOLEAN,       false   #-- @desc Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-3A/13

pc_OTDOA_prsFrequencyHopping,                BOOLEAN,       false   #-- @desc Support of prsFrequencyHopping #-- @spec 37.571-3 Table A.4.3-3A/11

pc_OTDOA_prsOccGroup,                        BOOLEAN,       false   #-- @desc Support of prsOccGroup #-- @spec 37.571-3 Table A.4.3-3A/10

pc_OTDOA_prs_based_tbs,                      BOOLEAN,       false   #-- @desc Support of prs-based-tbs #-- @spec 37.571-3 Table A.4.3-3A/6

pc_OTDOA_prs_id,                             BOOLEAN,       false   #-- @desc Support of prs-id #-- @spec 37.571-3 Table A.4.3-3A/3

pc_OTDOA_tp_separation_via_muting,           BOOLEAN,       false   #-- @desc Support of tp-separation-via-muting #-- @spec 37.571-3 Table A.4.3-3A/4

pc_P2X_UE,                                   BOOLEAN,       false   #-- @desc  Support of V2X communicatin as Pedestrian UE #-- @spec 36.523-2 A.4.4-1/XXX

pc_PDCP_Delay_r16,                           BOOLEAN,       false   #-- @desc  UE supports UL PDCP Packet Average Delay measurement and reporting in RRC_CONNECTED state #-- @spec 38.508-2 Table A.4.4-1/5

pc_PDCP_PktDelay,                            BOOLEAN,       false   #-- @desc  Support for PDCP Packet Delay per QCI #-- @spec 36.523-2 A.4.4-1/140

pc_PLMN_EF_LRPLMNSI_Automatic_Mode_Exception,BOOLEAN,       false   #-- @desc  Support of Automatic Mode EF_LRPLMSI PLMN Selection Expression #-- @spec 36.523-2 A.4.4-1/97

pc_PLMN_Manual_Mode_Exception,               BOOLEAN,       false   #-- @desc  Support of Manual Mode PLMN Selection Expression #-- @spec 36.523-2 A.4.4-1/98

pc_PPI_Support,                              BOOLEAN,       false   #-- @desc  Support of Power Preference Indication #-- @spec 36.523-2 A.4.4-1/86

pc_PRS_ProcessingSymbolsInEveryTms,          ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSymbolsInEveryTms_r16,n8      #-- @desc  PRS-ProcessingSymbolsInEveryTms for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/17

pc_PS,                                       BOOLEAN,       false   #-- @desc  Packet Switched #-- @spec 34.123-2 A.3/2

pc_PS_data_centric,                          BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS data centric #-- @spec 36.523-2 A.4.4-2/8

pc_PS_data_off,                              BOOLEAN,       false   #-- @desc  UE supports PS data off #-- @spec 34.229-2 Table A.12/62

pc_PS_voice_centric,                         BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS voice centric #-- @spec 36.523-2 A.4.4-2/7

pc_PUSCH_Ehn_MMTEL,                          BOOLEAN,       false   #-- @desc  Support of PUSCH enhancement for MMTEL voice and video enhancements mode #-- @spec 36.523-2 A.4.4-1/161

pc_PWS_UpperLayer,                           BOOLEAN,       false   #-- @desc  Presence of PWS upper layer for functions like duplicate definition #-- @spec 36.523-2 A.4.4-1/67

pc_P_CSCFDiscovery_viaDHCPv4,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv4 #-- @spec 34.229-2 Table A.13/2

pc_P_CSCFDiscovery_viaDHCPv6,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv6 #-- @spec 34.229-2 Table A.12/10

pc_P_CSCFDiscovery_viaPCO,                   BOOLEAN,       false   #-- @desc  UE supports P-CSCF Discovery via PCO #-- @spec 34.229-2 Table A.12/8

pc_ParamGpsAssisData,                        BOOLEAN,       false   #-- @desc Support of MO-LR request for assistance data #-- @spec 37.571-3 table A.4.3-3/5

pc_ParamPosEstimate,                         BOOLEAN,       false   #-- @desc Support of MO-LR request for a position estimate #-- @spec 37.571-3 table A.4.3-3/6

pc_Preconditions,                            BOOLEAN,       false   #-- @desc  Integration of resource management and SIP? (use of preconditions) #-- @spec 34.229-2 Table A.4/16

pc_ProvideDST_inUse,                         BOOLEAN,       false   #-- @desc  UE supports a mechanism to provide daylight saving time #-- @spec 36.523-2 A.4.4-2/xxx

pc_Provide_IMS_APN,                          BOOLEAN,       false   #-- @desc  Configured to provide IMS APN during initial attach #-- @spec 36.523-2 A.4.4-2/13

pc_Provide_IMS_as_second_APN,                BOOLEAN,       false   #-- @desc  Configured to provide IMS APN as the 2nd PDN connection #-- @spec 36.523-2 A.4.4-2/14

pc_Provide_Internet_as_second_APN,           BOOLEAN,       false   #-- @desc  Configured to provide Internet APN as the 2nd PDN connection #-- @spec 36.523-2 A.4.4-2/15

pc_QZSS_ADR,                                 BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Qzss #-- @spec 37.571-3 Table A.4.3-6/3

pc_QZSS_ADR_ENH,                             BOOLEAN,       false   #-- @desc Support of ADR enhancements for Qzss #-- @spec 37.571-3 Table A.4.3-6/15

pc_QZSS_HA,                                  BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Qzss #-- @spec 37.571-3 Table A.4.3-6/21

pc_QZSS_QZS_L1,                              BOOLEAN,       false   #-- @desc Support of QZS-L1 signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/4

pc_QZSS_QZS_L1C,                             BOOLEAN,       false   #-- @desc Support of QZS-L1C signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/5

pc_QZSS_QZS_L2C,                             BOOLEAN,       false   #-- @desc Support of QZS-L2C signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/6

pc_QZSS_QZS_L5,                              BOOLEAN,       false   #-- @desc Support of QZS-L5 signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/7

pc_QZSS_VelocityMeas,                        BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Qzss #-- @spec 37.571-3 Table A.4.3-6/8

pc_RLF_ReportForInterRAT_MRO,                BOOLEAN,       false   #-- @desc  Support of Radio Link Failure Report for InterRAT MRO #-- @spec 36.523-2 A.4.4-1/94

pc_ROHC_profile0x0001,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0001 #-- @spec 36.523-2 A.4.4-1/40

pc_ROHC_profile0x0002,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0002 #-- @spec 36.523-2 A.4.4-1/41

pc_ROHC_profile0x0003,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0003 #-- @spec 36.523-2 A.4.4-1/42

pc_ROHC_profile0x0004,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0004 #-- @spec 36.523-2 A.4.4-1/43

pc_ROHC_profile0x0006,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0006 #-- @spec 36.523-2 A.4.4-1/44

pc_ROHC_profile0x0101,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0101 #-- @spec 36.523-2 A.4.4-1/45

pc_ROHC_profile0x0102,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0102 #-- @spec 36.523-2 A.4.4-1/46

pc_ROHC_profile0x0103,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0103 #-- @spec 36.523-2 A.4.4-1/47

pc_ROHC_profile0x0104,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0104 #-- @spec 36.523-2 A.4.4-1/48

pc_RSRP_MeasFR1,                             BOOLEAN,       false   #-- @desc  Support of RSRP-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6C/3

pc_RSRP_MeasFR2,                             BOOLEAN,       false   #-- @desc  Support of RSRP-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6C/4

pc_RS_SINR_MeasEUTRA,                        BOOLEAN,       false   #-- @desc  Support of E-UTRA RS-SINR measurements #-- @spec 38.508-2 Table A.4.3.6-1/42

pc_Rach_Report,                              BOOLEAN,       false   #-- @desc  Support of delivery of rachReport upon request from the network #-- @spec 36.523-2 A.4.4-1/85

pc_Re_Attach_AfterDetachColl,                BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach #-- @spec 36.523-2 A.4.4-1/55

pc_RequestIPv4HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv4 address of the Home Agent during Attach procedure #-- @spec 36.523-2 A.4.4-1/23

pc_RequestIPv6HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv6 address of the Home Agent during Attach procedure #-- @spec 36.523-2 A.4.4-1/22

pc_SBAS_ADR,                                 BOOLEAN,       false   #-- @desc Support of ADR measurement reporting for Sbas #-- @spec 37.571-3 Table A.4.3-6/2

pc_SBAS_ADR_ENH,                             BOOLEAN,       false   #-- @desc Support of ADR enhancements for Sbas #-- @spec 37.571-3 Table A.4.3-6/14

pc_SBAS_HA,                                  BOOLEAN,       false   #-- @desc Support of High accuracy GNSS modes for Sbas #-- @spec 37.571-3 Table A.4.3-6/20

pc_SBAS_VelocityMeas,                        BOOLEAN,       false   #-- @desc Support of Velocity measurement reporting for Sbas #-- @spec 37.571-3 Table A.4.3-6/7

pc_SCPTM,                                    BOOLEAN,       false   #-- @desc  The UE supports SC-PTM #-- @spec 36.523-2 A.4.2.1.1-1/11

pc_SFTD_MeasNR_Cell_FDD,                     BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR neighbour cell in FDD #-- @spec 38.508-2 Table A.4.3.6-1/46

pc_SFTD_MeasNR_Cell_TDD,                     BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR neighbour cell in TDD #-- @spec 38.508-2 Table A.4.3.6-1/47

pc_SFTD_MeasNR_Neigh_FDD,                    BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR neighbour cell in FDD #-- @spec 38.508-2 Table A.4.3.6-1/48

pc_SFTD_MeasNR_Neigh_TDD,                    BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR neighbour cell in TDD #-- @spec 38.508-2 Table A.4.3.6-1/49

pc_SFTD_MeasPSCell_MRDC_FDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR PSCell #-- @spec 38.508-2 Table A.4.3.6-1/43

pc_SFTD_MeasPSCell_MRDC_TDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a E-UTRA PCell and an NR PSCell #-- @spec 38.508-2 Table A.4.3.6-1/44

pc_SFTD_MeasPSCell_NEDC,                     BOOLEAN,       false   #-- @desc  Support of SFTD measurements between the NR PCell and a configured E-UTRA PSCell #-- @spec 38.508-2 Table A.4.3.6-1/xx

pc_SFTD_MeasPSCell_NRDC_FDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR PSCell in FDD #-- @spec 38.508-2 Table A.4.3.6-1/50

pc_SFTD_MeasPSCell_NRDC_TDD,                 BOOLEAN,       false   #-- @desc  Support of SFTD measurements between a NR PCell and an NR PSCell in TDD #-- @spec 38.508-2 Table A.4.3.6-1/51

pc_SIP_Based_UserConfiguration,              BOOLEAN,       false   #-- @desc  SIP based user configuration #-- @spec 34.229-2 Table A.16/18

pc_SIP_Digest,                               BOOLEAN,       false   #-- @desc  SIP Digest without TLS #-- @spec 34.229-2 Table A.6a/5

pc_SI_Neighbour_UMTS_Autonomous_Gaps,        BOOLEAN,       false   #-- @desc  Upon configuration of si-RequestForHO by the network supports acquistion of relevant information from a neighbouring UMTS cell by reading the SI of the neighbouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/100

pc_SI_Neighbour_interFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intrer-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/104

pc_SI_Neighbour_intraFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intra-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/103

pc_SMS_IP_MO,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP sender #-- @spec 34.229-2 Table A.3A/61

pc_SMS_IP_MT,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP receiver #-- @spec 34.229-2 Table A.3A/62

pc_SMS_SGs,                                  BOOLEAN,       false   #-- @desc  The UE supports SMS over SGs and is configured for SMS over SGs.  If true at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. If it is set to true pc_combined_attach shall be set to true #-- @spec 36.523-2, A.4.2.1.1-1/2

pc_SMS_SGs_MO,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MO over SGs #-- @spec 36.523-2 A.4.4-1/4

pc_SMS_SGs_MT,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MT over SGs #-- @spec 36.523-2 A.4.4-1/3

pc_SMS_SGs_Multi_MO,                         BOOLEAN,       false   #-- @desc  Support of sending concatenated multiple short message over SGs #-- @spec 36.523-2 A.4.4.1-72

pc_SNPN,                                     BOOLEAN,       false   #-- @desc  Support of Stand-alone Non-Public Network #-- @spec 38.508-2 Table A.4.3.7-1/24

pc_SNPN_access_control_configuration,        BOOLEAN,       false   #-- @desc  Support of unified access control configuration in the list of subscriber data indicating for which access identities (see 3GPP TS 24.501 [64]) the ME is configured when the MS accesses an SNPN. #-- @spec 38.508-2 Table A.4.3.7-1/40

pc_SNPN_only,                                BOOLEAN,       false   #-- @desc  UE Supports only Stand-alone Non-Public Network #-- @spec 38.508-2 Table A.4.1-5/3

pc_SOR_ACKNotReqLocalRel,                    BOOLEAN,       false   #-- @desc  Support of UE local release when the security check is successful but SOR Transparent container indicates ACK has been NOT requested #-- @spec 38.508-2 Table A.4.3.7-1/20

pc_SRS_switching,                            BOOLEAN,       false   #-- @desc  Support of SRS switching between a band pair #-- @spec 36.523-2 A.4.4-1/166

pc_SRVCC_GERAN_UTRAN,                        BOOLEAN,       false   #-- @desc  Support for SRVCC from E-UTRAN to GERANUTRAN #-- @spec 36.523-2 A.4.4-1/32

pc_Semi_Persistence_Scheduling,              BOOLEAN,       TRUE    #-- @desc  Support of semi persistance scheduling #-- @spec 36.523-2 A.4.4-1/50

pc_Sens,                                     BOOLEAN,       false   #-- @desc Support for UE-Assisted Sensor #-- @spec 37.571-3 Table A.4.3-2/23

pc_ShortNameNetwork,                         BOOLEAN,       false   #-- @desc  Support of storage of the network short name #-- @spec 36.523-2 A.4.4-1/13

pc_Speech,                                   BOOLEAN,       false   #-- @desc  UE supports Speech #-- @spec 34.123-2 A.2/1

pc_Squal_based_CellReselection_between_E_UTRAN_and_GERAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from GERAN #-- @spec 36.523-2 A.4.4-1/79

pc_Squal_based_CellReselection_to_E_UTRAN_from_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from UTRAN #-- @spec 36.523-2 A.4.4-1/57

pc_Squal_based_CellReselection_to_UTRAN_from_E_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to UTRAN from E-UTRAN #-- @spec 36.523-2 A.4.4-1/56

pc_StandaloneGNSS_Location,                  BOOLEAN,       false   #-- @desc  Support of standalone GNSS receiver to provide detailed location information in RRC measurement report and logged measurements in RRC_IDLE #-- @spec 36.523-2 A.4.4-1/63

pc_Streaming,                                BOOLEAN,       false   #-- @desc  UE Supports Streaming QoS class #-- @spec 34.123-2 A.6/2

pc_SupportOpModeA,                           BOOLEAN,       false   #-- @desc  UE supports Operation Mode A #-- @spec 34.123-2 A.3/3

pc_SwitchOnOff,                              BOOLEAN,       TRUE    #-- @desc  switch onoff supported #-- @spec 34.123-2 A.20/35

pc_T3412Extended,                            BOOLEAN,       false   #-- @desc  Support of T3412 extended value IE #-- @spec 36.523-2 A.4.4-1/81

pc_TAU_connected_in_IMS,                     BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 36.523-2 A.4.4.1-73

pc_TAU_idle_in_IMS,                          BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 36.523-2 A.4.4.1-74

pc_TDD_HCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/2

pc_TDD_LCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/3

pc_TDD_SpecialSubframe,                      BOOLEAN,       false   #-- @desc  Support of TDD special subframe #-- @spec 36.523-2 A.4.4-1A/2

pc_TDD_VHCR,                                 BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/8

pc_TDD_band_UE_PC2,                          BOOLEAN,       false   #-- @desc  Support of TDD Bands 38 40 41 and 42 Power class 2 operation #-- @spec 36.523-2 A.4.4-1/139

pc_TTI_Bundling,                             BOOLEAN,       TRUE    #-- @desc  Support of TTI Bundling #-- @spec 36.523-2 A.4.4-1/51

pc_TestModeforCSGproximity,                  BOOLEAN,       false   #-- @desc  Support of UE radio bearer test mode for CSG proximity testing #-- @spec 34.123-2 A.13/5

pc_TransferEmergencyPDUN1toS1noN26,          BOOLEAN,       false   #-- @desc  Support of Emergency PDU session transfer from N1 mode to S1 mode when network does not support N26 interface #-- @spec 38.508-2 Table A.4.4-2/8

pc_TransferEmergencyPDUS1toN1noN26,          BOOLEAN,       false   #-- @desc  Support of Emergency PDN connection transfer from S1 mode to N1 mode when network does not support N26 interface #-- @spec 38.508-2 Table A.4.4-2/9

pc_UAI_rrm_RelaxationRRC_ConnectedRedCap,    BOOLEAN,       false   #-- @desc  Support of initiating #-- @spec 38.508-2 Table A.4.3.12-1/7

pc_UDC,                                      BOOLEAN,       false   #-- @desc  Support of the uplink data compression operation #-- @spec 36.523-2 A.4.4-1/179

pc_UDC_SIP,                                  BOOLEAN,       false   #-- @desc  Support of UL data compression with SIP static dictionary #-- @spec 36.523-2 A.4.4-1/180

pc_UEA_AGNSS,                                BOOLEAN,       false   #-- @desc Support of UE assisted Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/2

pc_UEA_A_GANSS,                              BOOLEAN,       false   #-- @desc Support of UE-Assisted A-GANSS #-- @spec 37.571-3 Table A.4.3-1/6

pc_UEA_DL_AoD,                               BOOLEAN,       false   #-- @desc  Support for UE-Assisted DL-AoD #-- @spec 37.571-3 Table A.4.3-2/30

pc_UEA_DL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Assisted DL-TDOA #-- @spec 37.571-3 Table A.4.3-2/32

pc_UEA_MBS,                                  BOOLEAN,       false   #-- @desc Support for UE-Assisted MBS #-- @spec 37.571-3 Table A.4.3-2/20

pc_UEB_AGNSS,                                BOOLEAN,       false   #-- @desc Support of UE based Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/1

pc_UEB_A_GANSS,                              BOOLEAN,       false   #-- @desc Support of UE-Based A-GANSS #-- @spec 37.571-3 Table A.4.3-1/5

pc_UEB_DL_AoD,                               BOOLEAN,       false   #-- @desc  Support for UE-Based DL-AoD #-- @spec 37.571-3 Table A.4.3-2/31

pc_UEB_DL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Based DL-TDOA #-- @spec 37.571-3 Table A.4.3-2/33

pc_UEB_MBS,                                  BOOLEAN,       false   #-- @desc Support for UE-Based MBS #-- @spec 37.571-3 Table A.4.3-2/26

pc_UEB_Sens,                                 BOOLEAN,       false   #-- @desc Support for UE-Based Sensor #-- @spec 37.571-3 Table A.4.3-2/28

pc_UEB_WLAN,                                 BOOLEAN,       false   #-- @desc Support for UE-Based WLAN #-- @spec 37.571-3 Table A.4.3-2/27

pc_UE_NoRegIMS_IMSVoPS_0,                    BOOLEAN,       false   #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to '0' #-- @spec 36.523-2 A.4.4-2/xx

pc_UE_NoReqIMS_IMSVoPS_0,                    BOOLEAN,       false   #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to 0 #-- @spec 36.523-2 A.4.4-2/xx

pc_UE_supports_user_initiated_PDN_disconnect,BOOLEAN,       false   #-- @desc  UE supports user initiated PDN disconnect #-- @spec 36.523-2 A.4.4-2/16

pc_UL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of uplink 256 QAM #-- @spec 36.523-2 A.4.4-1/183

pc_UL_64QAM,                                 BOOLEAN,       false   #-- @desc  Support of uplink 64 QAM #-- @spec 36.523-2 A.4.4-1/114

pc_UL_CA,                                    BOOLEAN,       false   #-- @desc  Support of UL CA #-- @spec 36.523-2, ???

pc_UL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 2 carriers #-- @spec 36.523-2 A.4.3.3-2/1

pc_UL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 3 carriers #-- @spec 36.523-2 A.4.3.3-2/2

pc_UL_CoMP,                                  BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation #-- @spec 36.523-2 A.4.4-1A/1

pc_UL_IntraBand_ContCaBWclassB,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class B #-- @spec 36.523-2 A.4.3.3.1-2/1

pc_UL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class C #-- @spec 36.523-2 A.4.3.3.1-2/2

pc_UL_MIMO,                                  BOOLEAN,       false   #-- @desc  Support of UL MIMO #-- @spec 36.523-2 A.4.4-170

pc_UL_NR_CA_2CC,                             BOOLEAN,       false   #-- @desc  UL NR CA with 2 carriers #-- @spec 38.508-2 Table A.4.3.2A.1-2/1

pc_UL_NR_CA_3CC,                             BOOLEAN,       false   #-- @desc  UL NR CA with 3 carriers #-- @spec 38.508-2 Table A.4.3.2A.1-2/2

pc_UL_SupportedInAllBandsInCAComb,           BOOLEAN,       false   #-- @desc  UL (Pcell) supported in each band of Inter-band CA combination under test #-- @spec 36.523-2 A.4.3.3.3-2/2

pc_UL_interBand_CaAA,                        BOOLEAN,       false   #-- @desc  Support of UL inter-band CA _ A-A #-- @spec 36.523-2 A.4.3.3.3-2A/1

pc_UL_interBand_CaBwClassComb_AA,            BOOLEAN,       TRUE    #-- @desc  UL Inter-band contiguous CA BW class A-A #-- @spec 36.523-2 A.4.3.3.3-2/1

pc_UL_intraBand_contCaTypeB,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type B #-- @spec 36.523-2 A.4.3.3.1-2A/1

pc_UL_intraBand_contCaTypeC,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type C #-- @spec 36.523-2 A.4.3.3.1-2A/2

pc_UL_intraBand_nonContCaAA,                 BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA _ A-A #-- @spec 36.523-2 A.4.3.3.2-2A/1

pc_UL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       TRUE    #-- @desc  Support of UL intra-band non-contiguous CA BW Class Combination A-A #-- @spec 36.523-2 A.4.3.3.2-2/1

pc_UL_intra_non_contiguous_CA_NR_FR1_Class_2A,BOOLEAN,       false   #-- @desc  UL NR FR1 Intra-band non-contiguous CA BW Class Combination (2A) #-- @spec 38.508-2 Table A.4.3.2A.3.1-2

pc_UL_intra_non_contiguous_CA_NR_FR2_Class_2A,BOOLEAN,       false   #-- @desc  UL NR FR2 Intra-band non-contiguous CA BW Class Combination (2A) #-- @spec 38.508-2 Table A.4.3.2A.3.2-3

pc_UMI_ProcNeeded_DuringCSFB,                BOOLEAN,       false   #-- @desc  Requiring UMI proceeding to paging response #-- @spec 36.523-2 A.4.4-2/6

pc_USIM_Removal,                             BOOLEAN,       false   #-- @desc  USIM removable without power down supported #-- @spec 36.523-2, A4.4-1/1

pc_USSI,                                     BOOLEAN,       false   #-- @desc  USSI #-- @spec 34.229-2 Table A.16/19

pc_UTRA,                                     BOOLEAN,       false   #-- @desc  UE supports UTRA #-- @spec 36.523-2 A.4.1-1/6

pc_UTRAN_ANR,                                BOOLEAN,       false   #-- @desc  Support of UTRAN ANR #-- @spec 36.523-2 A.4.4-1/65

pc_UTRAN_ProximityIndication,                BOOLEAN,       false   #-- @desc  Support of UTRAN Proximity Indication #-- @spec 36.523-2 A.4.4.1/77

pc_UTRA_CompressedModeRequired,              BOOLEAN,       false   #-- @desc  Support of Compressed Mode #-- @spec 36.523-2 A.4.4-1/28

pc_UTRA_FeatrGrp_1,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_PCH and URA_PCH to RRC_IDLE cell reselection #-- @spec 36.523-2 A.4.5-2/1

pc_UTRA_FeatrGrp_2,                          BOOLEAN,       false   #-- @desc  Support of EUTRAN measurements and reporting in connected mode #-- @spec 36.523-2 A.4.5-2/2

pc_UTRA_FeatrGrp_3,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for high priority layers #-- @spec 36.523-2 A.4.5-2/3

pc_UTRA_FeatrGrp_4,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for all layers #-- @spec 36.523-2 A.4.5-2/4

pc_UeAssistedAgps,                           BOOLEAN,       false   #-- @desc  Support of UE assisted Network Assisted GPS L1 CA #-- @spec 37.571-3 A.4.3-1/11

pc_UeBasedAgps,                              BOOLEAN,       false   #-- @desc  Support of UE based Network Assisted GPS L1 CA #-- @spec 37.571-3 A.4.3-1/10

pc_UniversalAndLocalTimeZone,                BOOLEAN,       false   #-- @desc  Support of storage of the universal time and local time zone #-- @spec 36.523-2 A.4.4-1/15

pc_UpdateUE_LocationInformation,             BOOLEAN,       TRUE    #-- @desc  Update UE Location Information #-- @spec 36.523-2 A.4.3-2/3

pc_Use_QCI_66,                               BOOLEAN,       false   #-- @desc  The UE supports a bearer with QCI 66 #-- @spec 36.523-2 A.4.4-2/33

pc_Use_SMS_over_IP,                          BOOLEAN,       false   #-- @desc  The UE is configured to use SMS over IP #-- @spec 36.523-2 A.4.4-2/xxx

pc_UserInitiatedPLMN_Reselection,            BOOLEAN,       false   #-- @desc  Support user initiated PLMN reselection in automatic mode #-- @spec 36.523-2 A.4.4-1/69

pc_UserInitiated_SNPN_Reselection,           BOOLEAN,       false   #-- @desc  Support of autonomous search function to detect CAG cells on serving and non-serving frequencies #-- @spec 38.508-2 Table A.4.3.7-1/xz

pc_User_Plane_CIoT_Optimisation,             BOOLEAN,       false   #-- @desc  Support of User Plane CIoT #-- @spec 36.523-2 A.4.4-1/132

pc_V2XCNPC5,                                 BOOLEAN,       false   #-- @desc  Support of V2X communication over NR-PC5 #-- @spec 38.508-2 Table A.4.3.7-1/34

pc_VideoCodecH264CBP,                        BOOLEAN,       false   #-- @desc  MTSI media - Video codec H.264 CBP Level 1.2 #-- @spec 34.229-2 Table A.15/9

pc_VideoCodecH264CBPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CBP Level 3.1 #-- @spec 34.229-2 Table A.15/13

pc_VideoCodecH264CHPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CHP Level 3.1 #-- @spec 34.229-2 Table A.15/12

pc_VideoCodecH265Lv31,                       BOOLEAN,       false   #-- @desc  Reference: 34.229-2 Table A.1511 #-- @spec 34.229-2 Table A.15/11

pc_VoLTE,                                    BOOLEAN,       TRUE    #-- @desc  Support of VoLTE in GSMA PRD IR.92: "IMS profile for Voice and SMS" #-- @spec 36.523-2 A.4.4-1/33

pc_WLAN,                                     BOOLEAN,       false   #-- @desc Support for UE-Assisted WLAN #-- @spec 37.571-3 Table A.4.3-2/21

pc_WLAN_APId,                                BOOLEAN,       false   #-- @desc Support of wlan-AP-Identifier #-- @spec 37.571-3 Table A.4.3-7B/1

pc_WLAN_APLocinfo,                           BOOLEAN,       false   #-- @desc Support of wlan-AP-Location #-- @spec 37.571-3 Table A.4.3-7B/2

pc_WLAN_IMS_EmergencyCall,                   BOOLEAN,       false   #-- @desc  UE supports IMS emergency call over WLAN #-- @spec 34.229-2 Table A.12/65

pc_WLAN_Meas_Imm_MDT,                        BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in Immediate MDT #-- @spec 36.523-2, A.4.4-1/187

pc_WLAN_Meas_logged_MDT,                     BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in logged MDT #-- @spec 36.523-2, A.4.4-1/185

pc_WLAN_XCAP_without_PDN,                    BOOLEAN,       false   #-- @desc  If PICS is true Wi-Fi access without PDN connection applies.  Otherwise EPC-integrated WLAN applies #-- @spec 34.229-2 a.12/49

pc_WLAN_voice,                               BOOLEAN,       false   #-- @desc  Support for IR.51 #-- @spec 36.523-2, A.4.4-1/117

pc_XCAP_UsernameIsConfiguredInUE,            BOOLEAN,       false   #-- @desc  UE indicated OMA-TS-XDM_MO-V1_1-20080627-A.doc section 5.2.8 "Node: <X>AAUTHNAME" is configured #-- @spec 34.229-2 Table A.12/37

pc_XCAP_XUIisDefaultPublicUserId,            BOOLEAN,       false   #-- @desc  UE uses the default public user id received in P-Associated-URI header in 200 OK for REGISTER as XCAP User Identity (XUI) #-- @spec 34.229-2 Table A.12/38

pc_XCAP_only_APN,                            BOOLEAN,       false   #-- @desc  Configured with an APN for XCAP only usage #-- @spec 36.523-2 A.4.4-2/12

pc_XCAP_over_Internet_APN,                   BOOLEAN,       false   #-- @desc  Configured to use Internet APN for XCAP signalling #-- @spec 36.523-2 A.4.4-2/17

pc_ZUC,                                      BOOLEAN,       false   #-- @desc  Support of ZUC algorithm #-- @spec 36.523-2 A.4.4-1/99

pc_am_WithLongSN,                            BOOLEAN,       false   #-- @desc  Support RLC AM with 18 bit length of RLC sequence number #-- @spec 38.508-2 Table A.4.3.4-1/1A

pc_am_WithShortSN,                           BOOLEAN,       TRUE    #-- @desc  Support RLC AM with 12 bit length of RLC sequence number #-- @spec 38.508-2 Table A.4.3.4-1/1

pc_as_ReflectiveQoS,                         BOOLEAN,       false   #-- @desc  Support of reflective QoS #-- @spec 38.508-2 Table A.4.3.7-1/4

pc_barometer_r16,                            BOOLEAN,       false   #-- @desc  UE supports uncompensated barometric pressure measurement reporting upon request from the network. #-- @spec 38.508-2 Table A.4.4-1/7

pc_bwp_DiffNumerology_FR1_FDD,               BOOLEAN,       false   #-- @desc  Support BWP adaptation up to 4 BWPs with the different numerologies via DCI and timer for FR1 FDD bands #-- @spec 38.508-2 Table A.4.3.2-1/44

pc_bwp_DiffNumerology_FR1_TDD,               BOOLEAN,       false   #-- @desc  Support BWP adaptation up to 4 BWPs with the different numerologies via DCI and timer for FR1 TDD bands #-- @spec 38.508-2 Table A.4.3.2-1/44a

pc_bwp_DiffNumerology_FR2,                   BOOLEAN,       false   #-- @desc  Support BWP adaptation up to 4 BWPs with the different numerologies via DCI and timer for FR2 bands #-- @spec 38.508-2 Table A.4.3.2-1/44b

pc_bwp_SameNumerology_upto2_FR1_FDD,         BOOLEAN,       false   #-- @desc  Support of BWP adaptation (up to 2 BWPs) with the same numerology for FR1 FDD bands #-- @spec 38.508-2 Table A.4.3.2-1/42

pc_bwp_SameNumerology_upto2_FR1_TDD,         BOOLEAN,       TRUE    #-- @desc  Support of BWP adaptation (up to 2 BWPs) with the same numerology #-- @spec 38.508-2 Table A.4.3.2-1/42

pc_bwp_SameNumerology_upto2_FR2,             BOOLEAN,       false   #-- @desc  Support of BWP adaptation (up to 2 BWPs) with the same numerology for FR2 bands #-- @spec 38.508-2 Table A.4.3.2-1/42b

pc_bwp_SameNumerology_upto4_FR1_FDD,         BOOLEAN,       false   #-- @desc  Support of BWP adaptation (up to 4 BWPs) with the same numerology for FR1 FDD bands #-- @spec 38.508-2 Table A.4.3.2-1/43

pc_bwp_SameNumerology_upto4_FR1_TDD,         BOOLEAN,       false   #-- @desc  Support of BWP adaptation (up to 4 BWPs) with the same numerology #-- @spec 38.508-2 Table A.4.3.2-1/43

pc_bwp_SameNumerology_upto4_FR2,             BOOLEAN,       false   #-- @desc  Support of BWP adaptation (up to 4 BWPs) with the same numerology for FR2 bands #-- @spec 38.508-2 Table A.4.3.2-1/43b

pc_bwp_SwitchingDelay_Type1,                 BOOLEAN,       false   #-- @desc  Supports DCI and timer based active BWP switching delay type1 #-- @spec 38.508-2 Table A.4.3.2-1/24

pc_bwp_SwitchingDelay_Type2,                 BOOLEAN,       TRUE    #-- @desc  Supports DCI and timer based active BWP switching delay type2 #-- @spec 38.508-2 Table A.4.3.2-1/24A

pc_bwp_WithoutRestriction,                   BOOLEAN,       false   #-- @desc  Support of BWP operation without bandwidth restriction #-- @spec 38.508-2 Table A.4.3.2-1/34

pc_ce_HARQ_AckBundling,                      BOOLEAN,       false   #-- @desc  Support of HARQ-ACK bundling #-- @spec 36.523-2 A.4.4-1/y

pc_ce_PUSCH_NB_MaxTBS,                       BOOLEAN,       false   #-- @desc  Support of ce-PUSCH-NB-MaxTBS-r14 #-- @spec 36.523-2 A.4.4-1/x

pc_cg_SDT_r17,                               BOOLEAN,       false   #-- @desc  Support of SDT in RRC_INACTIVE state via Configured Grant Type 1 #-- @spec 38.508-2 Table A.4.4-1/16

pc_condHandoverFailure_r16,                  BOOLEAN,       false   #-- @desc  Support conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover #-- @spec 38.508-2 Table A.4.3.8-1/12

pc_condHandoverTwoTriggerEvents_r16,         BOOLEAN,       false   #-- @desc  Support 2 trigger events for same execution condition of conditional handover #-- @spec 38.508-2 Table A.4.3.8-1/13

pc_condHandover_r16,                         BOOLEAN,       false   #-- @desc  Support conditional handover #-- @spec 38.508-2 Table A.4.3.8-1/11

pc_condPSCellChange_r16,                     BOOLEAN,       false   #-- @desc  Support conditional PSCell change #-- @spec 38.508-2 Table A.4.3.8-1/hh01

pc_configuredUL_GrantType1,                  BOOLEAN,       false   #-- @desc  Support Type 1 PUSCH transmissions with configured grant #-- @spec 38.508-2 Table A.4.3.2-1/10

pc_configuredUL_GrantType2,                  BOOLEAN,       false   #-- @desc  Support Type 2 PUSCH transmissions with configured grant #-- @spec 38.508-2 Table A.4.3.2-1/11

pc_csi_RSRP_AndRSRQ_MeasWithSSB,             BOOLEAN,       false   #-- @desc  Support CSI-RSRP and CSI-RSRQ measurement where CSI-RS resource is configured with an associated SSPBCH #-- @spec 38.508-2 Table A.4.3.6-1/4

pc_csi_RSRP_AndRSRQ_MeasWithoutSSB,          BOOLEAN,       false   #-- @desc  Support CSI-RSRP and CSI-RSRQ measurement where CSI-RS resource is configured without an associated SSPBCH #-- @spec 38.508-2 Table A.4.3.6-1/40

pc_csi_RS_CFRA_ForHO,                        BOOLEAN,       false   #-- @desc  Support handover using a contention free random access on PRACH resources that are associated with CSI-RS resources of the target cell #-- @spec 38.508-2 Table A.4.3.2-1/9

pc_dataInactMon,                             BOOLEAN,       false   #-- @desc  Support of data inactivity monitoring #-- @spec 36.523-2 A.4.2.1.1-1/14

pc_data_centric,                             BOOLEAN,       false   #-- @desc  Support of UEs usage setting as data centric #-- @spec 38.508-2 Table A.4.4-2/10

pc_dci_DL_PriorityIndicator_r16,             BOOLEAN,       false   #-- @desc  Supports the priority indicator field configured in DCI formats 1_1 and 1_2 in a BWP when configured to monitor both DCI formats 1_1 and 1_2 in the BWP. #-- @spec 38.508-2 Table A.4.3.2-1/80

pc_dci_Format1_2And0_2_r16,                  BOOLEAN,       false   #-- @desc  Support monitoring DCI format 1_2 for DL scheduling and monitoring DCI format 0_2 for UL scheduling #-- @spec 38.508-2 Table A.4.3.2-1/52

pc_dci_UL_PriorityIndicator_r16,             BOOLEAN,       false   #-- @desc  Supports the priority indicator field configured in DCI formats 0_1 and 0_2 in a BWP when configured to monitor both DCI formats 0_1 and 0_2 in the BWP #-- @spec 38.508-2 Table A.4.3.2-1/81

pc_directMCG_SCellActivationResume_r16,      BOOLEAN,       false   #-- @desc  Support direct NR MCG SCell activation as specified in TS 38.321 upon reception of an RRCResume message as specified in TS 38.331 #-- @spec 38.508-2 Table A.4.3.5-1/14

pc_directMCG_SCellActivation_r16,            BOOLEAN,       false   #-- @desc  Support direct NR MCG SCell activation as specified in TS 38.321 upon SCell addition upon reconfiguration with sync of the MCG as specified in TS 38.331. #-- @spec 38.508-2 Table A.4.3.5-1/13

pc_directSCG_SCellActivationResume_r16,      BOOLEAN,       false   #-- @desc  Support direct NR SCG SCell activation as specified in TS 38.321: #-- @spec 38.508-2 Table A.4.3.5-1/15

pc_directSCG_SCellActivation_r16,            BOOLEAN,       false   #-- @desc  Support direct NR SCG SCell activation, as specified in TS 38.321, upon SCell addition and upon reconfiguration with sync of the SCG, both performed via an RRCReconfiguration message received via SRB3 or contained in an RRC(Connection)Reconfiguration message received via SRB1, as specified in TS 38.331 and TS 36.331 #-- @spec 38.508-2 Table A.4.3.5-1/12

pc_dl_PRS_BufferType,                        ENUM-PRS_ProcessingCapabilityPerBand_r16.dl_PRS_BufferType_r16,type1   #-- @desc  dl-PRS-BufferType for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/15

pc_dl_RSTD_MeasurementPerPairOfTRP_FR1,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR1 #-- @spec 37.571-3 Table A.4.3-6F/1

pc_dl_RSTD_MeasurementPerPairOfTRP_FR2,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR2 #-- @spec 37.571-3 Table A.4.3-6F/2

pc_dl_SchedulingOffset_PDSCH_TypeA,          BOOLEAN,       TRUE    #-- @desc  Support of DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A. #-- @spec 38.508-2 Table A.4.3.2-1/xx

pc_downlinkSPS,                              BOOLEAN,       false   #-- @desc  Support PDSCH reception based on semi-persistent scheduling #-- @spec 38.508-2 Table A.4.3.2-1/1

pc_downlink_LAA,                             BOOLEAN,       false   #-- @desc  Supports downlink LAA operation #-- @spec 36.523-2 A.4.4-1/129

pc_durationOfPRS_ProcessingSymbols_r16,      ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSymbols_r16,nDot125 #-- @desc  durationOfPRS-ProcessingSymbols for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/16

pc_dynamicPowerSharingENDC,                  BOOLEAN,       false   #-- @desc  Support dynamic EN-DC power sharing for at least one EN-DC band combination_FR1 only #-- @spec 38.508-2 Table A.4.3.2-1/17

pc_dynamicSwitchRA_Type0_1_PDSCH,            BOOLEAN,       false   #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PDSCH #-- @spec 38.508-2 Table A.4.3.2-1/xx

pc_dynamicSwitchRA_Type0_1_PUSCH,            BOOLEAN,       TRUE    #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PUSCH #-- @spec 38.508-2 Table A.4.3.2-1/yy

pc_dynamicSwitch_SUL,                        BOOLEAN,       false   #-- @desc  Support supplemental uplink with dynamic switch (DCI based selection of PUSCH carrier) #-- @spec 38.508-2 Table A.4.3.2-1/13

pc_eAttachWithIMSI,                          BOOLEAN,       false   #-- @desc  Support of Attach With IMSI #-- @spec 36.523-2 A.4.4-1/80

pc_eBand103_Supp,                            BOOLEAN,       false   #-- @desc  Support of Band 103 #-- @spec 36.523-2 A.4.3.1-1/103

pc_eBand10_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 10 #-- @spec 36.523-2 A.4.3.1-1/10

pc_eBand11_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 11 #-- @spec 36.523-2 A.4.3.1-1/11

pc_eBand12_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 12 #-- @spec 36.523-2 A.4.3.1-1/12

pc_eBand13_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 13 #-- @spec 36.523-2 A.4.3.1-1/13

pc_eBand14_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 14 #-- @spec 36.523-2 A.4.3.1-1/14

pc_eBand17_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 17 #-- @spec 36.523-2 A.4.3.1-1/17

pc_eBand18_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 18 #-- @spec 36.523-2 A.4.3.1-1/18

pc_eBand19_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 19 #-- @spec 36.523-2 A.4.3.1-1/19

pc_eBand1_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 1 #-- @spec 36.523-2 A.4.3.1-1/1

pc_eBand20_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 20 #-- @spec 36.523-2 A.4.3.1-1/20

pc_eBand21_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 21 #-- @spec 36.523-2 A.4.3.1-1/21

pc_eBand22_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 22 #-- @spec 36.523-2 A.4.3.1-1/22

pc_eBand23_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 23 #-- @spec 36.523-2 A.4.3.1-1/23

pc_eBand24_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 24 #-- @spec 36.523-2 A.4.3.1-1/24

pc_eBand25_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 25 #-- @spec 36.523-2 A.4.3.1-1/25

pc_eBand26_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 26 #-- @spec 36.523-2 A.4.3.1-1/26

pc_eBand27_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 27 #-- @spec 36.523-2 A.4.3.1-1/27

pc_eBand28_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 28 #-- @spec 36.523-2 A.4.3.1-1/28

pc_eBand29_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 29 #-- @spec 36.523-2 A.4.3.1-1/29

pc_eBand2_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 2 #-- @spec 36.523-2 A.4.3.1-1/2

pc_eBand30_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 30 #-- @spec 36.523-2 A.4.3.1-1/30

pc_eBand31_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 31 #-- @spec 36.523-2 A.4.3.1-1/31

pc_eBand32_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 32 #-- @spec 36.523-2 A.4.3.1-1/32

pc_eBand33_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 33 #-- @spec 36.523-2 A.4.3.1-2/1

pc_eBand34_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 34 #-- @spec 36.523-2 A.4.3.1-2/2

pc_eBand35_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 35 #-- @spec 36.523-2 A.4.3.1-2/3

pc_eBand36_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 36 #-- @spec 36.523-2 A.4.3.1-2/4

pc_eBand37_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 37 #-- @spec 36.523-2 A.4.3.1-2/5

pc_eBand38_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 38 #-- @spec 36.523-2 A.4.3.1-2/6

pc_eBand39_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 39 #-- @spec 36.523-2 A.4.3.1-2/7

pc_eBand3_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 3 #-- @spec 36.523-2 A.4.3.1-1/3

pc_eBand40_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 40 #-- @spec 36.523-2 A.4.3.1-2/8

pc_eBand41_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 41 #-- @spec 36.523-2 A.4.3.1-2/9

pc_eBand42_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 42 #-- @spec 36.523-2 A.4.3.1-2/10

pc_eBand43_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 43 #-- @spec 36.523-2 A.4.3.1-2/11

pc_eBand44_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 44 #-- @spec 36.523-2 A.4.3.1-2/12

pc_eBand45_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 45 #-- @spec 36.523-2 A.4.3.1-2/13

pc_eBand46_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 46 #-- @spec 36.523-2 A.4.3.1-2/14

pc_eBand47_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 47 #-- @spec 36.523-2 A.4.3.1-2/15

pc_eBand48_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 48 #-- @spec 36.523-2 A.4.3.1-2/16

pc_eBand4_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 4 #-- @spec 36.523-2 A.4.3.1-1/4

pc_eBand53_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 53 #-- @spec 36.523-2 A.4.3.1-2/17

pc_eBand54_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 54 #-- @spec 36.523-2 A.4.3.1-2/18

pc_eBand5_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 5 #-- @spec 36.523-2 A.4.3.1-1/5

pc_eBand65_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 65 #-- @spec 36.523-2 A.4.3.1-1/33

pc_eBand66_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 66 #-- @spec 36.523-2 A.4.3.1-1/34

pc_eBand68_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 68 #-- @spec 36.523-2 A.4.3.1-1/36

pc_eBand69_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 69 #-- @spec 36.523-2 A.4.3.1-1/37

pc_eBand6_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 6 #-- @spec 36.523-2 A.4.3.1-1/6

pc_eBand70_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 70 #-- @spec 36.523-2 A.4.3.1-1/38

pc_eBand71_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 71 #-- @spec 36.523-2 A.4.3.1-1/39

pc_eBand72_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 72 #-- @spec 36.523-2 A.4.3.1-1/40

pc_eBand73_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 73 #-- @spec 36.523-2 A.4.3.1-1/41

pc_eBand74_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 74 #-- @spec 36.523-2 A.4.3.1-1/42

pc_eBand7_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 7 #-- @spec 36.523-2 A.4.3.1-1/7

pc_eBand85_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 85 #-- @spec 36.523-2 A.4.3.1-1/xx

pc_eBand87_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 87 #-- @spec 36.523-2 A.4.3.1-1/87

pc_eBand88_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 88 #-- @spec 36.523-2 A.4.3.1-1/88

pc_eBand8_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 8 #-- @spec 36.523-2 A.4.3.1-1/8

pc_eBand9_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 9 #-- @spec 36.523-2 A.4.3.1-1/9

pc_eCall_Test_Call,                          BOOLEAN,       false   #-- @desc  Capability to trigger a Test eCall #-- @spec 34.123-2 A.10/19

pc_eCall_automatic_Initiated,                BOOLEAN,       false   #-- @desc  Capability to initiate Automatic eCall #-- @spec 34.123-2 Table A.10/17

pc_eCall_manual_Initiated,                   BOOLEAN,       false   #-- @desc  Capability to initiate a Manual eCall #-- @spec 34.123-2 Table A.10/16

pc_eFDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA FDD #-- @spec 36.523-2 A.4.1-1/1

pc_eFDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA FDD bands #-- @spec 36.523-2 A.4.1-2/1

pc_eHARQ_Pattern_for_TTI_bundling,           BOOLEAN,       false   #-- @desc  Support of enhanced HARQ pattern for TTI bundling operation for FDD #-- @spec 36.523-2 A.4.4-1/107

pc_eIMTA_TDD,                                BOOLEAN,       false   #-- @desc  Support of TDD ULDL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD Pcell #-- @spec 36.523-2 A.4.4-1/124

pc_eMBMS,                                    BOOLEAN,       false   #-- @desc  Support of eMBMS #-- @spec 36.523-2 A.4.2.1.1-1/5

pc_eMBMS_SC,                                 BOOLEAN,       false   #-- @desc  Support of eMBMS service continuity #-- @spec 36.523-2 A.4.2.1.1-1/7

pc_eMinimumPeriodicSearchTimer,              BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer #-- @spec 36.523-2 A.4.4-1/84

pc_ePDCCH,                                   BOOLEAN,       false   #-- @desc  Support of ePDCCH #-- @spec 36.523-2 A.4.4-1/87

pc_ePSM,                                     BOOLEAN,       false   #-- @desc  Support of Power Saving Mode (in EUTRA) #-- @spec 36.523-2 A.4.4-1/115

pc_eRedirectionUTRA,                         BOOLEAN,       false   #-- @desc  Support of use of the UTRA system information provided by RRCConnectionRelease upon redirection #-- @spec 36.523-2 A.4.4-1/31

pc_eTDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA TDD #-- @spec 36.523-2 A.4.1-1/2

pc_eTDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA TDD bands #-- @spec 36.523-2 A.4.1-2/2

pc_eWLAN,                                    BOOLEAN,       false   #-- @desc  WLAN #-- @spec 36.523-2 A.4.1-1/5

pc_earlyMeasLog_r17,                         BOOLEAN,       false   #-- @desc  Support of the storage of Early Measurement Logging in logged measurements. #-- @spec 38.508-2 Table A.4.4-1/YYX

pc_edrx,                                     BOOLEAN,       false   #-- @desc  Support of extended DRX #-- @spec 36.523-2 A.4.4-1/121

pc_eutra_CGI_Reporting,                      BOOLEAN,       TRUE    #-- @desc  Support acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the EN-DC is not configured. #-- @spec 38.508-2 Table A.4.3.6-1/7

pc_eutra_CGI_Reporting_NEDC,                 BOOLEAN,       false   #-- @desc  Support acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NE-DC is configured. #-- @spec 38.508-2 Table A.4.3.6-1/57

pc_eutra_EPC_HO_ToNR_FDD_FR1_r15,            BOOLEAN,       false   #-- @desc  Support inter-RAT Handover to NR FR1 FDD from EUTRA connected to EPC #-- @spec 38.508-2 Table A.4.3.8-1/7

pc_eutra_EPC_HO_ToNR_TDD_FR1_r15,            BOOLEAN,       false   #-- @desc  Support inter-RAT Handover to NR FR1 TDD from EUTRA connected to EPC #-- @spec 38.508-2 Table A.4.3.8-1/6

pc_eutra_EPC_HO_ToNR_TDD_FR2_r15,            BOOLEAN,       false   #-- @desc  Support inter-RAT Handover to NR FR2 TDD from EUTRA connected to EPC #-- @spec 38.508-2 Table A.4.3.8-1/8

pc_eventA_MeasAndReport,                     BOOLEAN,       false   #-- @desc  Support NR measurements and events A triggered reporting #-- @spec 38.508-2 Table A.4.3.6-1/1

pc_eventB_MeasAndReport,                     BOOLEAN,       TRUE    #-- @desc  Support inter-RAT EUTRA measurements and events B triggered reporting #-- @spec 38.508-2 Table A.4.3.6-1/5

pc_extendedBand_n77_2_r17,                   BOOLEAN,       false   #-- @desc  Supports the restriction to 3450 - 3650 MHz and 3650 - 3980 ranges of band n77 #-- @spec 38.508-2 Table A.4.3.2-1/96

pc_extendedBand_n77_r16,                     BOOLEAN,       false   #-- @desc  Supports the restriction to 3450 - 3550 MHz and 3700 - 3980 MHz ranges of band n77 #-- @spec 38.508-2 Table A.4.3.2-1/95

pc_extendedLongDRX,                          BOOLEAN,       false   #-- @desc  Support of extended Long DRX cycle #-- @spec 36.523-2 A.4.4-1/128

pc_fixed_broadband_XCAP,                     BOOLEAN,       false   #-- @desc  The UE uses XCAP in fixed broadband access #-- @spec 34.229-2 Table A.12/50

pc_freqBandPriorityAdjustment,               BOOLEAN,       false   #-- @desc  Support of prioritization of the frequency bands in multiBandInfoList over the band in freqBandIndicator as defined by freqBandIndicatorPriority-r12 #-- @spec 36.523-2 A.4.4-1/125

pc_gnss_heightMeas,                          BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement #-- @spec 36.523-2 A.4.4-1/yyy

pc_gp10_en_dc,                               BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 10 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/16

pc_gp10_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 10 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/26

pc_gp11_en_dc,                               BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 1 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/17

pc_gp11_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 11 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/27

pc_gp12_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 12 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/28

pc_gp15_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 15 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/29

pc_gp16_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 16 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/30

pc_gp17_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 17 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/31

pc_gp18_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 18 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/32

pc_gp19_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 19 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/33

pc_gp20_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 20 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/34

pc_gp21_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 21 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/35

pc_gp22_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 22 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/36

pc_gp23_nr,                                  BOOLEAN,       false   #-- @desc  Support measurement gap pattern 23 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/37

pc_gp2_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 2 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/18

pc_gp3_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 3 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/19

pc_gp4_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 4 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/10

pc_gp4_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 4 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/20

pc_gp5_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 5 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/11

pc_gp5_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 5 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/21

pc_gp6_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 6 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/12

pc_gp6_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 6 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/22

pc_gp7_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 7 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/13

pc_gp7_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 7 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/23

pc_gp8_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 8 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/14

pc_gp8_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 8 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/24

pc_gp9_en_dc,                                BOOLEAN,       false   #-- @desc  Support NR supports gap pattern 9 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 Table A.4.3.6-1/15

pc_gp9_nr,                                   BOOLEAN,       false   #-- @desc  Support measurement gap pattern 9 configured by NR RRC #-- @spec 38.508-2 Table A.4.3.6-1/25

pc_halfDuplexFDD_TypeA_RedCap_r17,           BOOLEAN,       false   #-- @desc  Support of Half-duplex FDD operation (instead of full-duplex FDD operation) type A for RedCap UE. #-- @spec 38.508-2 Table A.4.3.12-1/5

pc_handoverInterF,                           BOOLEAN,       TRUE    #-- @desc  Support inter-frequency Handover from the corresponding duplex mode or from the corresponding frequency range #-- @spec 38.508-2 Table A.4.3.8-1/2

pc_handoverUTRA_FDD_r16,                     BOOLEAN,       false   #-- @desc  Support inter-RAT Handover from NR to UTRA-FDD CELL_DCH CS #-- @spec 38.508-2 Table A.4.3.8-1/14

pc_heightMeas,                               BOOLEAN,       false   #-- @desc  Support of height-based measurement reporting #-- @spec 36.523-2 A.4.4-1/xxx

pc_idleInactiveNR_MeasReport,                BOOLEAN,       false   #-- @desc  Support configuration of NR SSB measurements in RRC_IDLERRC_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 #-- @spec 38.508-2 Table A.4.3.6-1/54

pc_immMeasWLAN_r16,                          BOOLEAN,       false   #-- @desc  UE supports WLAN measurements in RRC_CONNECTED state #-- @spec 38.508-2 Table A.4.4-1/11

pc_inactiveState,                            BOOLEAN,       TRUE    #-- @desc  Support of RRC_INACTIVE as specified in TS 38.331 #-- @spec 38.508-2 Table A.4.3.7-1/19

pc_independentGapConfig,                     BOOLEAN,       false   #-- @desc  Support two independent measurement gap configurations for FR1 and FR2 #-- @spec 38.508-2 Table A.4.3.6-1/2

pc_interFreqDAPS_r16,                        BOOLEAN,       false   #-- @desc  Support inter-frequency DAPS handover #-- @spec 38.508-2 Table A.4.3.8-1/15

pc_interRAT_NR_ToENDC,                       BOOLEAN,       false   #-- @desc  Support inter-RAT Handover from NR to EN-DC #-- @spec 38.508-2 Table A.4.3.8-1/10

pc_interleavingVRB_ToPRB_PDSCH,              BOOLEAN,       false   #-- @desc  Support receiving PDSCH with interleved VRB-to-PRB mapping #-- @spec 38.508-2 Table A.4.3.2-1/16

pc_intraAndInterF_MeasAndReport,             BOOLEAN,       false   #-- @desc  Support NR intra-freq and inter-freq measurements and at least periodical reporting #-- @spec 38.508-2 Table A.4.3.6-1/3

pc_intraFreqDAPS_r16,                        BOOLEAN,       false   #-- @desc  Support intra-frequency DAPS handover #-- @spec 38.508-2 Table A.4.3.8-1/15

pc_intraFreq_CE_NeedForGaps,                 BOOLEAN,       false   #-- @desc  Require intra-frequency measurement gaps for operating in CE Mode A or CE Mode B #-- @spec 36.523-2 A.4.4-1/158

pc_lch_PriorityBasedPrioritization_r16,      BOOLEAN,       false   #-- @desc  Support LCH-based prioritization #-- @spec 38.508-2 Table A.4.3.5-1/6

pc_lch_ToGrantPriorityRestriction_r16,       BOOLEAN,       false   #-- @desc  Supports restricting data transmission from a given LCH to a configured (sub-) set of dynamic grant priority levels #-- @spec 38.508-2 Table A.4.3.2-1/82

pc_lcp_Restriction,                          BOOLEAN,       false   #-- @desc  Support the selection of logical channels for each UL grant based on RRC configured restriction #-- @spec 38.508-2 Table A.4.3.5-1/xx

pc_loggedMeasWLAN_r16,                       BOOLEAN,       false   #-- @desc  Support of WLAN measurements in RRC_IDLE and RRC_INACTIVE state #-- @spec 38.508-2 Table A.4.4-1/13

pc_loggedMeasurements_r16,                   BOOLEAN,       false   #-- @desc  UE supports logged measurements in RRC_IDLE and RRC_INACTIVE. A UE that supports logged measurements shall support both periodical logging and event-triggered logging. The memory size of MDT logged   measurements is 64KB. #-- @spec 38.508-2 Table A.4.4-1/6

pc_logicalChannelSR_DelayTimer,              BOOLEAN,       TRUE    #-- @desc  Supports the logicalChannelSR-DelayTimer #-- @spec 38.508-2 Table A.4.3.5-1/4

pc_longDRX_Cycle,                            BOOLEAN,       TRUE    #-- @desc  Support long DRX cycle #-- @spec 38.508-2 Table A.4.3.5-1/1

pc_longSN,                                   BOOLEAN,       false   #-- @desc  Support of 18 bit length of PDCP sequence number #-- @spec 38.508-2 Table A.4.3.3-1/1A

pc_maxDL_PRS_RSRP_MeasurementFR1,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR1 #-- @spec 37.571-3 Table A.4.3-6E/1

pc_maxDL_PRS_RSRP_MeasurementFR2,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR2 #-- @spec 37.571-3 Table A.4.3-6E/2

pc_maxNrOfDL_PRS_ResourceSetPerTrpPerFrequencyLayer,INTEGER,       1       #-- @desc  maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer #-- @spec 37.571-3 Table A.4.3-6B/1

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr1,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr1_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr1 #-- @spec 37.571-3 Table A.4.3-6B/8

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr2,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr2_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr2 #-- @spec 37.571-3 Table A.4.3-6B/22

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_Only_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-Only #-- @spec 37.571-3 Table A.4.3-6B/6

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr2_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr2_Only_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr2-Only #-- @spec 37.571-3 Table A.4.3-6B/7

pc_maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer,ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/5

pc_maxNrOfDL_PRS_ResourcesPerResourceSet,    ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerResourceSet_r16,n1      #-- @desc  maxNrOfDL-PRS-ResourcesPerResourceSet for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/4

pc_maxNrOfPosLayer,                          INTEGER,       1       #-- @desc  maxNrOfPosLayer #-- @spec 37.571-3 Table A.4.3-6B/3

pc_maxNrOfRx_TX_MeasFR1,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6C/1

pc_maxNrOfRx_TX_MeasFR2,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6C/2

pc_maxNrOfTRP_AcrossFreqs,                   ENUM-NR_DL_PRS_ResourcesCapability_r16.maxNrOfTRP_AcrossFreqs_r16,n4      #-- @desc  maxNrOfTRP-AcrossFreqs #-- @spec 37.571-3 Table A.4.3-6B/2

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS120,ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs120_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 120kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/21

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS15, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs15_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 15kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/18

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS30, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs30_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 30kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/19

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS60, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs60_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 60kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/20

pc_maxNumberAP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberAP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberAP-SRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/16

pc_maxNumberMIMO_LayersPDSCH_eightLayers,    BOOLEAN,       false   #-- @desc  The maximum number of spatial multiplexing layer(s) supported by the UE for DL reception is 8 Layers. For single CC standalone NR it is mandatory with capability signalling to support at least 4 MIMO layers in the bands where 4Rx is specified as mandatory for the given UE and at least 2 MIMO layers in FR2. If absent the UE doesn't support MIMO on this carrier. #-- @spec 38.508-2 Table A.4.3.2-1/23

pc_maxNumberMIMO_LayersPDSCH_fourLayers,     BOOLEAN,       false   #-- @desc  The maximum number of spatial multiplexing layer(s) supported by the UE for DL reception is 4 Layers. #-- @spec 38.508-2 Table A.4.3.2-1/23A

pc_maxNumberMIMO_LayersPDSCH_twoLayers,      BOOLEAN,       TRUE    #-- @desc  The maximum number of spatial multiplexing layer(s) supported by the UE for DL reception is 2 Layers. #-- @spec 38.508-2 Table A.4.3.2-1/23B

pc_maxNumberPUSCH_TypeA_Repetition_r17,      BOOLEAN,       false   #-- @desc  Support the increased maximum number of PUSCH Type A repetitions up to 32 #-- @spec 38.508-2 Table A.4.3.2-1/115

pc_maxNumberPathLossEstimatePerServing,      ENUM-OLPC_SRS_Pos_r16.maxNumberPathLossEstimatePerServing_r16,n1      #-- @desc  maxNumberPathLossEstimatePerServing for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/6

pc_maxNumberPeriodicSRS_PosResourcesPerBWP,  ENUM-SRS_PosResourcesPerBand_r16.maxNumberPeriodicSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberPeriodicSRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/15

pc_maxNumberSP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSP-SRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/17

pc_maxNumberSRS_PosPathLossEstimateAllServingCells,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosPathLossEstimateAllServingCells_r16,n1      #-- @desc  maxNumberSRS-PosPathLossEstimateAllServingCells #-- @spec 37.571-3 Table A.4.3-6D/1

pc_maxNumberSRS_PosResourceSetsPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourceSetsPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourceSetsPerBWP #-- @spec 37.571-3 Table A.4.3-6D/13

pc_maxNumberSRS_PosResourcesPerBWP,          ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/14

pc_maxNumberSRS_PosSpatialRelationsAllServingCell,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosSpatialRelationsAllServingCells_r16,n0      #-- @desc  maxNumberSRS-PosSpatialRelationsAllServingCells #-- @spec 37.571-3 Table A.4.3-6D/2

pc_maxNumberSearchSpaces,                    BOOLEAN,       false   #-- @desc  UE supports maxNumberSearchSpaces #-- @spec 38.306, 4.2.7

pc_maxSupportedFreqLayers,                   INTEGER,       1       #-- @desc  maxSupportedFreqLayers-r16 #-- @spec 37.571-3 Table A.4.3-6B/11

pc_mpsPriorityIndication_r16,                BOOLEAN,       false   #-- @desc  Support of mpsPriorityIndication on RRC release with redirect #-- @spec 38.508-2 Table A.4.4-1/26

pc_multipleConfiguredGrants_r16,             BOOLEAN,       false   #-- @desc  Support PUSCH transmissions on multiple configured uplink grants #-- @spec 38.508-2 Table A.4.3.5-1/10

pc_multipleTimingAdvance,                    BOOLEAN,       false   #-- @desc  Support of multiple timing advances #-- @spec 36.523-2 A.4.4-1A/3

pc_multipleUplinkSPS,                        BOOLEAN,       false   #-- @desc  Support of multiple uplink SPS and reporting SPS assistance information #-- @spec 36.523-2 A.4.4-1/177

pc_multiple_CEF_Report_r17,                  BOOLEAN,       false   #-- @desc  Support of storage and delivery of multiple CEF reports #-- @spec 38.508-2 Table A.4.4-1/xx

pc_noOf_PDNsNewConnection,                   INTEGER,       0       #-- @desc  Number of UE requested PDN connection establishments after ATTACH in a new signaling connection #-- @spec 38.508-2 Table A.4.4-2/6

pc_noOf_PDNsSameConnection,                  INTEGER,       0       #-- @desc  Number of UE requested PDN connection establishments after ATTACH during the same signaling connection #-- @spec 38.508-2 Table A.4.4-2/5

pc_noOf_PDUs,                                INTEGER,       1       #-- @desc  Number of UE requested PDU session establishments after REGISTRATION #-- @spec 38.508-2 Table A.4.4-n/3

pc_noOf_PDUsNewConnection,                   INTEGER,       1       #-- @desc  Number of UE-requested PDU session establishments after REGISTRATION in a new signaling connection #-- @spec 38.508-2 Table A.4.4-2/4

pc_noOf_PDUsSameConnection,                  INTEGER,       0       #-- @desc  Number of UE requested PDU session establishments after REGISTRATION during the same signaling connection #-- @spec 38.508-2 Table A.4.4-2/3

pc_nrBand100_Supp,                           BOOLEAN,       false   #-- @desc  NR FDD FR1 Band n100 #-- @spec 38.508-2 Table A.4.3.1-1/19

pc_nrBand101_Supp,                           BOOLEAN,       false   #-- @desc  NR TDD FR1 Band n101 #-- @spec 38.508-2 Table A.4.3.1-2/13

pc_nrBand12_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 12 #-- @spec 38.508-2 Table A.4.3.1-1/6d

pc_nrBand14_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 14 #-- @spec 38.508-2 Table A.4.3.1-1/6e

pc_nrBand18_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 18 #-- @spec 38.508-2 Table A.4.3.1-1/6f

pc_nrBand1_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 1 #-- @spec 38.508-2 Table A.4.3.1-1/1

pc_nrBand20_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 20 #-- @spec 38.508-2 Table A.4.3.1-1/7

pc_nrBand24_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 24 #-- @spec 38.508-2 Table A.4.3.1-1/7d

pc_nrBand257_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 257 #-- @spec 38.508-2 Table A.4.3.1-1/6

pc_nrBand258_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 258 #-- @spec 38.508-2 Table A.4.3.1-3/2

pc_nrBand259_Supp,                           BOOLEAN,       false   #-- @desc  NR Band 259 #-- @spec 38.508-2 Table A.4.3.1-3/2a

pc_nrBand25_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 25 #-- @spec 38.508-2 Table A.4.3.1-1/7e

pc_nrBand260_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 260 #-- @spec 38.508-2 Table A.4.3.1-1/6

pc_nrBand261_Supp,                           BOOLEAN,       TRUE    #-- @desc  NR Band 261 #-- @spec 38.508-2 Table A.4.3.1-1/6

pc_nrBand26_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 26 #-- @spec 38.508-2 Table A.4.3.1-1/7f

pc_nrBand28_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 28 #-- @spec 38.508-2 Table A.4.3.1-1/8

pc_nrBand29_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 29 #-- @spec 38.508-2 Table A.4.3.1-6/3

pc_nrBand2_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 2 #-- @spec 38.508-2 Table A.4.3.1-1/2

pc_nrBand30_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 30 #-- @spec 38.508-2 Table A.4.3.1-1/8b

pc_nrBand34_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 34 #-- @spec 38.508-2 Table A.4.3.1-2/0

pc_nrBand38_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 38 #-- @spec 38.508-2 Table A.4.3.1-2/1

pc_nrBand39_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 39 #-- @spec 38.508-2 Table A.4.3.1-2/1a

pc_nrBand3_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 3 #-- @spec 38.508-2 Table A.4.3.1-1/3

pc_nrBand40_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 40 #-- @spec 38.508-2 Table A.4.3.1-2/1b

pc_nrBand41_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 41 #-- @spec 38.508-2 Table A.4.3.1-2/2

pc_nrBand41_maxUplinkDutyCycle_PC1dot5_MPE_FR1_r16,ENUM-MaxUplinkDutyCycle_PC1dot5_MPE_FR1_r16,n10     #-- @desc  NR_n41 maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 #-- @spec 

pc_nrBand46_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 46 #-- @spec 38.508-2 Table A.4.3.1-2/2e

pc_nrBand48_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 48 #-- @spec 38.508-2 Table A.4.3.1-2/2g

pc_nrBand50_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 50 #-- @spec 38.508-2 Table A.4.3.1-2/2i

pc_nrBand51_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 51 #-- @spec 38.508-2 Table A.4.3.1-2/2k

pc_nrBand53_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 53 #-- @spec 38.508-2 Table A.4.3.1-2/2l

pc_nrBand5_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 5 #-- @spec 38.508-2 Table A.4.3.1-1/4

pc_nrBand65_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 65 #-- @spec 38.508-2 Table A.4.3.1-1/8a

pc_nrBand66_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 66 #-- @spec 38.508-2 Table A.4.3.1-1/9

pc_nrBand70_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 70 #-- @spec 38.508-2 Table A.4.3.1-1/10

pc_nrBand71_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 70 #-- @spec 38.508-2 Table A.4.3.1-1/10

pc_nrBand74_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 74 #-- @spec 38.508-2 Table A.4.3.1-1/14

pc_nrBand75_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 75 #-- @spec 38.508-2 Table A.4.3.1-6/1

pc_nrBand76_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 76 #-- @spec 38.508-2 Table A.4.3.1-6/2

pc_nrBand77_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 77 #-- @spec 38.508-2 Table A.4.3.1-2/3

pc_nrBand78_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 78 #-- @spec 38.508-2 Table A.4.3.1-2/4

pc_nrBand79_Supp,                            BOOLEAN,       TRUE    #-- @desc  NR Band 79 #-- @spec 38.508-2 Table A.4.3.1-2/5

pc_nrBand79_maxUplinkDutyCycle_PC1dot5_MPE_FR1_r16,ENUM-MaxUplinkDutyCycle_PC1dot5_MPE_FR1_r16,n10     #-- @desc  NR_n79 maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 #-- @spec 

pc_nrBand7_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 7 #-- @spec 38.508-2 Table A.4.3.1-1/5

pc_nrBand80_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 80 #-- @spec 38.508-2 Table A.4.3.1-5/1

pc_nrBand81_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 81 #-- @spec 38.508-2 Table A.4.3.1-5/2

pc_nrBand82_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 82 #-- @spec 38.508-2 Table A.4.3.1-5/3

pc_nrBand83_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 83 #-- @spec 38.508-2 Table A.4.3.1-5/4

pc_nrBand84_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 84 #-- @spec 38.508-2 Table A.4.3.1-5/5

pc_nrBand86_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 86 #-- @spec 38.508-2 Table A.4.3.1-5/6

pc_nrBand8_Supp,                             BOOLEAN,       TRUE    #-- @desc  NR Band 8 #-- @spec 38.508-2 Table A.4.3.1-1/6

pc_nrBand91_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 91 #-- @spec 38.508-2 Table A.4.3.1-1/15

pc_nrBand92_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 92 #-- @spec 38.508-2 Table A.4.3.1-1/16

pc_nrBand93_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 93 #-- @spec 38.508-2 Table A.4.3.1-1/17

pc_nrBand94_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 94 #-- @spec 38.508-2 Table A.4.3.1-1/18

pc_nrBand95_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 95 #-- @spec 38.508-2 Table A.4.3.1-5/7

pc_nrBand96_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 96 #-- @spec 38.508-2 Table A.4.3.1-2/12

pc_nrBand97_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 97 #-- @spec 38.508-2 Table A.4.3.1-5/8

pc_nrBand99_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 99 #-- @spec 38.508-2 Table A.4.3.1-5/9

pc_nrFDD,                                    BOOLEAN,       TRUE    #-- @desc  NR FDD (Option 2) #-- @spec 38.508-2 Table A.4.1-1/1

pc_nrFDD_MultiBand,                          BOOLEAN,       TRUE    #-- @desc  Support of multiple NR FDD bands #-- @spec 38.508-2 Table A.4.1-2/1

pc_nrFR1,                                    BOOLEAN,       TRUE    #-- @desc  Support of frequency range FR1 #-- @spec 38.508-2 Table A.4.1-2/7

pc_nrFR2,                                    BOOLEAN,       TRUE    #-- @desc  Support of frequency range FR2 #-- @spec 38.508-2 Table A.4.1-2/8

pc_nrSDL,                                    BOOLEAN,       false   #-- @desc  Support of NR SDL #-- @spec 38.508-2 Table A.4.1-2/4

pc_nrSDL_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR SDL bands #-- @spec 38.508-2 Table A.4.1-2/6

pc_nrSL,                                     BOOLEAN,       false   #-- @desc  NR sidelink #-- @spec 38.508-2 Table A.4.1-1/3

pc_nrSUL,                                    BOOLEAN,       false   #-- @desc  Support of NR SUL #-- @spec 38.508-2 Table A.4.1-2/3

pc_nrSUL_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR SUL bands #-- @spec 38.508-2 Table A.4.1-2/5

pc_nrTDD,                                    BOOLEAN,       TRUE    #-- @desc  NR TDD (Option 2) #-- @spec 38.508-2 Table A.4.1-1/2

pc_nrTDD_MultiBand,                          BOOLEAN,       TRUE    #-- @desc  Support of multiple NR TDD bands #-- @spec 38.508-2 Table A.4.1-2/2

pc_nr_CGI_Reporting,                         BOOLEAN,       TRUE    #-- @desc  Support acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when EN-DC is not configured #-- @spec 38.508-2 Table A.4.3.6-1/8

pc_nr_CGI_Reporting_ENDC,                    BOOLEAN,       false   #-- @desc  Support acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the EN-DC is configured. #-- @spec 38.508-2 Table A.4.3.6-1/9

pc_nr_CGI_Reporting_NEDC,                    BOOLEAN,       false   #-- @desc  Support acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NE-DC is configured. #-- @spec 38.508-2 Table A.4.3.6-1/59

pc_nr_CGI_Reporting_NPN_r16,                 BOOLEAN,       TRUE    #-- @desc  Support of acquisition of CGI related information from a neighbouring intra-frequency or inter-frequency NPN CAG cell #-- @spec 38.508-2 Table A.4.3.6-1/zz

pc_olpc_SRS_PosBasedOnPRS_Neigh,             BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/5

pc_olpc_SRS_PosBasedOnPRS_Serving,           BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/3

pc_olpc_SRS_PosBasedOnSSB_Neigh,             BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnSSB-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/4

pc_onDemandSI_Report_r17,                    BOOLEAN,       false   #-- @desc  Support of delivery of on-Demand SI information upon request from the network #-- @spec 38.508-2 Table A.4.4-1/24

pc_orientation_r16,                          BOOLEAN,       false   #-- @desc  UE supports orientation information reporting upon request from the network. #-- @spec 38.508-2 Table A.4.4-1/8

pc_outOfOrderDelivery,                       BOOLEAN,       false   #-- @desc  Supports Out of order delivery of data to upper layers by PDCP #-- @spec 38.508-2 Table A.4.3.3-1/2

pc_pdcp_DuplicationMCG_OrSCG_DRB,            BOOLEAN,       false   #-- @desc  Support CA-based PDCP duplication over MCG or SCG DRB #-- @spec 38.508-2 Table A.4.3.3-1/3

pc_pdcp_DuplicationMoreThanTwoRLC_r16,       BOOLEAN,       false   #-- @desc  Support PDCP duplication with more than two RLC entities #-- @spec 38.508-2 Table A.4.3.3-1/5

pc_pdcp_DuplicationSplitDRB,                 BOOLEAN,       false   #-- @desc  Support PDCP duplication with more than two RLC entities #-- @spec 38.508-2 Table A.4.3.3-1/4

pc_pdcp_DuplicationSplitSRB,                 BOOLEAN,       false   #-- @desc  Support PDCP duplication over split SRB12 #-- @spec 38.508-2 Table A.4.3.3-1/5

pc_pdsch_256QAM_FR1,                         BOOLEAN,       TRUE    #-- @desc  Support 256QAM for PDSCH for FR1 #-- @spec 38.508-2 Table A.4.3.2-1/2

pc_pdsch_256QAM_FR2,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PDSCH for FR2 #-- @spec 38.508-2 Table A.4.3.2-1/3

pc_pdsch_MappingTypeA,                       BOOLEAN,       false   #-- @desc  support receiving PDSCH using PDSCH mapping type A with less than seven symbols #-- @spec 38.508-2 Table A.4.3.2-1/5

pc_pdsch_MappingTypeB,                       BOOLEAN,       false   #-- @desc  support receiving PDSCH using PDSCH mapping type B with less than seven symbols #-- @spec 38.508-2 Table A.4.3.2-1/6

pc_pdsch_RepetitionMultiSlots,               BOOLEAN,       false   #-- @desc  Support PDSCH Reception when configured with higher layer parameter aggregationFactorDL>1 #-- @spec 38.508-2 Table A.4.3.2-1/12

pc_pei_SubgroupingSupportBandList_r17,       BOOLEAN,       false   #-- @desc  Supports receiving paging early indication and UE subgrouping indication with UEID #-- @spec 38.508-2 Table A.4.3.7-1/42

pc_periodicEUTRA_MeasAndReport,              BOOLEAN,       false   #-- @desc  Supports periodic EUTRA measurement and reporting. #-- @spec 38.508-2 Table A.4.3.6-1/X1

pc_prs_FromServNeighCellAsQCL,               BOOLEAN,       false   #-- @desc  Support of prs-FromServNeighCellAsQCL for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/10

pc_pucch_Repetition_F0_1_2_3_4_DynamicIndication_r17,BOOLEAN,       false   #-- @desc  Support repetitions for PUCCH format 0 1 2 3 and 4 over multiple PUCCH subslots based on dynamic repetition indication #-- @spec 38.508-2 Table A.4.3.2-1/114

pc_puschTypeA_RepetitionsAvailSlot_r17,      BOOLEAN,       false   #-- @desc  Support PUSCH repetitions based on available slots #-- @spec 38.508-2 Table A.4.3.2-1/116

pc_pusch_256QAM_FR1,                         BOOLEAN,       TRUE    #-- @desc  Support 256QAM for PUSCH for FR1 #-- @spec 38.508-2 Table A.4.3.2-1/4

pc_pusch_256QAM_FR2,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PUSCH for at least one NR FR2 band #-- @spec 38.508-2 Table A.4.3.2-1/4a

pc_pusch_RepetitionCRC_r17,                  BOOLEAN,       false   #-- @desc  Support of repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0_0 with CRC scrambled by TC-RNTI. #-- @spec 38.508-2 Table A.4.3.2-1/85

pc_pusch_RepetitionMultiSlots,               BOOLEAN,       false   #-- @desc  Supports transmitting PUSCH scheduled by DCI format 0_0 or 0_1 when configured with higher layer parameter aggregationFactorUL > 1 #-- @spec 38.508-2 Table A.4.3.2-1/21

pc_pusch_RepetitionTypeB_r16,                BOOLEAN,       false   #-- @desc  Support PUSCH repetition type B #-- @spec 38.508-2 Table A.4.3.2-1/45

pc_qci1Indication_inRLF,                     BOOLEAN,       false   #-- @desc  Support of QCI1 indication in Radio Link Failure Report #-- @spec 36.523-2 A.4.4-1/131

pc_qoe_MTSI_MeasReport,                      BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for MTSI Service #-- @spec 36.523-2 A.4.4-1/182

pc_qoe_MeasReport,                           BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for Streaming Service #-- @spec 36.523-2 A.4.4-1/181

pc_ra_SDT_r17,                               BOOLEAN,       false   #-- @desc  Support of SDT in RRC_INACTIVE state via Random Access Procedure #-- @spec 38.508-2 Table A.4.4-1/14

pc_ra_Type0_PUSCH,                           BOOLEAN,       TRUE    #-- @desc  Support resource allocation Type 0 for PUSCH #-- @spec 38.508-2 Table A.4.3.2-1/7

pc_rachReport_r16,                           BOOLEAN,       TRUE    #-- @desc  Support of rachReport #-- @spec 38.508-2 Table A.4.4-1/3

pc_recommendedBitRate,                       BOOLEAN,       false   #-- @desc  Supports the bit rate recommendation message from the gNB to the UE as specified in TS 38.321 #-- @spec 38.508-2 Table A.4.3.5-1/AA

pc_recommendedBitRateQuery,                  BOOLEAN,       false   #-- @desc  Supports the bit rate recommendation query message from the UE to the gNB as specified in TS 38.321 #-- @spec 38.508-2 Table A.4.3.5-1/BB

pc_reducedCP_Latency,                        BOOLEAN,       false   #-- @desc  Support reduced control plane latency as defined in TS 38.331 #-- @spec 38.508-2 Table A.4.3.7-1/28

pc_releasePreference_r16,                    BOOLEAN,       TRUE    #-- @desc  Support of release preference assistance information #-- @spec 38.508-2 Table A.4.3.7-1/29

pc_reqFreqBands,                             BOOLEAN,       false   #-- @desc  Support of reception of requested Frequency Bands #-- @spec 36.523-2 A.4.4-1/101

pc_resumeWithSCG_Config_r16,                 BOOLEAN,       false   #-- @desc  Support of (re-)configuration of an SCG during the resume procedure. #-- @spec 38.508-2 Table A.4.3.7-1/44

pc_rrm_RelaxationRRC_ConnectedRedCap_r17,    BOOLEAN,       false   #-- @desc  Support of relaxed RRM measurements in RRC_CONNECTED for RedCap UE. #-- @spec 38.508-2 Table A.4.3.12-1/6

pc_rssiAndChannelOccupancyReporting,         BOOLEAN,       false   #-- @desc  Supports measurement and reporting for RSSI and channel occupancy #-- @spec 36.523-2 A.4.4-1/130

pc_scellDormancyOutsideActiveTime_r16,       BOOLEAN,       false   #-- @desc  Support of receiving SCell dormancy indication on SPCell using DCI format 2_6 outside the active time #-- @spec 38.508-2 Table A.4.3.2-1/35

pc_scptm_NonServingCell,                     BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on a cell that may be additionally configured as an Scell #-- @spec 36.523-2 A.4.4-1/127

pc_scptm_SCell,                              BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on configured SCell #-- @spec 36.523-2 A.4.4-1/126

pc_shortDRX_Cycle,                           BOOLEAN,       TRUE    #-- @desc  Support short DRX cycle #-- @spec 38.508-2 Table A.4.3.5-1/2

pc_shortSN,                                  BOOLEAN,       TRUE    #-- @desc  Support 12 bit length of PDCP sequence number #-- @spec 38.508-2 Table A.4.3.3-1/1

pc_shortSPS_intervalFDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in FDD mode #-- @spec 36.523-2 A.4.4-1/170

pc_shortSPS_intervalTDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in TDD mode #-- @spec 36.523-2 A.4.4-1/171

pc_simulLTE_NR_PRS,                          BOOLEAN,       false   #-- @desc  Support of simulLTE-NR-PRS #-- @spec 37.571-3 Table A.4.3-6B/12

pc_simul_NR_DL_AoD_DL_TDOA,                  BOOLEAN,       false   #-- @desc  Support of simul-NR-DL-AoD-DL-TDOA for at least one NR band #-- @spec 37.571-3 Table A.4.3-6E/3

pc_simul_NR_DL_AoD_Multi_RTT,                BOOLEAN,       false   #-- @desc  Support of simul-NR-DL-AoD-Multi-RTT for at least one NR band #-- @spec 37.571-3 Table A.4.3-6E/4

pc_skipUplinkDynamic,                        BOOLEAN,       false   #-- @desc  Support of skipping UL transmissions if no data is available #-- @spec 36.523-2 A.4.4-1/173

pc_skipUplinkSPS,                            BOOLEAN,       false   #-- @desc  Support of skipping SPS UL transmissions if no data is available #-- @spec 36.523-2 A.4.4-1/172

pc_skipUplinkTxDynamic,                      BOOLEAN,       false   #-- @desc  Support skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission #-- @spec 38.508-2 Table A.4.3.5-1/3

pc_sliceInfoforCellReselection_r17,          BOOLEAN,       false   #-- @desc  Support of slice reselection information in SIB and on RRC release for slice based cell reselection in RRC _IDLE and RRC INACTIVE #-- @spec 38.508-2 Table A.4.3.7-1/38

pc_sms_over_NAS,                             BOOLEAN,       false   #-- @desc  Support of SMS over NAS #-- @spec 38.508-2 Table A.4.3.7-1/6

pc_spatialBundlingHARQ_ACK,                  BOOLEAN,       false   #-- @desc  Supports spatial bundling of HARQ-ACK bits carried on PUCCH or PUSCH per PUCCH group.  With spatial bundling 2 HARQ-ACK bits for a DL MIMO data is bundled into a single bit by logical AND operation #-- @spec 38.508-2 Table A.4.3.2-1/19

pc_spatialRelation_SRS_PosBasedOnCSI_RS_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnCSI-RS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/8

pc_spatialRelation_SRS_PosBasedOnPRS_Neigh,  BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/12

pc_spatialRelation_SRS_PosBasedOnPRS_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/9

pc_spatialRelation_SRS_PosBasedOnSRS,        BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSRS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/10

pc_spatialRelation_SRS_PosBasedOnSSB_Neigh,  BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/11

pc_spatialRelation_SRS_PosBasedOnSSB_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/7

pc_speed_r16,                                BOOLEAN,       false   #-- @desc  UE supports speed information reporting upon request from the network. #-- @spec 38.508-2 Table A.4.4-1/9

pc_splitDRB_withUL_Both_MCG_SCG,             BOOLEAN,       TRUE    #-- @desc  Support UL transmission via both MCG path and SCG path for the split DRB #-- @spec 38.508-2 Table A.4.3.7-1/2

pc_splitSRB_WithOneUL_Path,                  BOOLEAN,       false   #-- @desc  Support UL transmission via either MCG path or SCG path for the split SRB #-- @spec 38.508-2 Table A.4.3.7-1/1

pc_srb3,                                     BOOLEAN,       false   #-- @desc  Support direct SRB between the SN and the UE #-- @spec 38.508-2 Table A.4.3.7-1/3

pc_srb_SDT_r17,                              BOOLEAN,       false   #-- @desc  Support of SRB SDT in RRC_INACTIVE state #-- @spec 38.508-2 Table A.4.4-1/15

pc_srs_AssocPRS_MultiLayersFR1,              BOOLEAN,       false   #-- @desc  Support of srs-AssocPRS-MultiLayersFR1 #-- @spec 37.571-3 Table A.4.3-6C/5

pc_srs_AssocPRS_MultiLayersFR2,              BOOLEAN,       false   #-- @desc  Support of srs-AssocPRS-MultiLayersFR2 #-- @spec 37.571-3 Table A.4.3-6C/6

pc_ss_CCH_Interference_Handling,             BOOLEAN,       false   #-- @desc  Support of Synchronisation signal and common channel interference handling #-- @spec 36.523-2 A.4.4-1A/8

pc_ss_SINR_Meas,                             BOOLEAN,       TRUE    #-- @desc  Support SS-SINR measurements #-- @spec 38.508-2 Table A.4.3.6-1/6

pc_ss_rsrp_SINR,                             BOOLEAN,       TRUE    #-- @desc UE supports rsrp SINR #-- @spec 38.523-3

pc_ssb_FromNeighCellAsQCL,                   BOOLEAN,       false   #-- @desc  Support of ssb-FromNeighCellAsQCL for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/9

pc_supportOf16DRB_RedCap_r17,                BOOLEAN,       false   #-- @desc  Support of 16 DRBs for RedCap UEs. #-- @spec 38.508-2 Table A.4.3.12-1/1

pc_supportOfRedCap_r17,                      BOOLEAN,       false   #-- @desc  Support of RedCap. #-- @spec 38.508-2 Table A.4.3.12-1/2

pc_supportedBandwidthPRS_FR1,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr1,mhz5    #-- @desc  supportedBandwidthPRS in FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/13

pc_supportedBandwidthPRS_FR2,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr2,mhz50   #-- @desc  supportedBandwidthPRS in FR2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/14

pc_tb_ProcessingMultiSlotPUSCH_r17,          BOOLEAN,       false   #-- @desc  Supports TB processing over multi-slot PUSCH without repetition #-- @spec 38.508-2 Table A.4.3.2-1/117

pc_tb_ProcessingRepMultiSlotPUSCH_r17,       BOOLEAN,       false   #-- @desc  Supports repetition of TB processing over multi-slot PUSCH #-- @spec 38.508-2 Table A.4.3.2-1/118

pc_tdd_FDD_CA_FDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the second bit setting to 1 #-- @spec 36.523-2 A.4.4-1/109

pc_tdd_FDD_CA_TDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the first bit setting to 1 #-- @spec 36.523-2 A.4.4-1/108

pc_twoPUCCH_group,                           BOOLEAN,       false   #-- @desc  Supports two PUCCH group in CA with a same numerology across CCs for data and control channel #-- @spec 38.508-2 Table A.4.3.2-1/83

pc_twoStepRACH_r16,                          BOOLEAN,       false   #-- @desc  Support of 2-Step RACH #-- @spec 38.508-2 Table A.4.3.2-1/46

pc_twoStepScheduling_uplink_LAA,             BOOLEAN,       false   #-- @desc  Supports two step uplink scheduling using PUSCH trigger A and PUSCH trigger B #-- @spec 36.523-2 A.4.4-1/176

pc_ue_CategoryDL_0,                          BOOLEAN,       false   #-- @desc  UE Category DL 0 #-- @spec 36.523-2 A.4.3.2-2/1

pc_ue_CategoryDL_10,                         BOOLEAN,       false   #-- @desc  UE Category DL 10 #-- @spec 36.523-2 A.4.3.2-2/5

pc_ue_CategoryDL_11,                         BOOLEAN,       TRUE    #-- @desc  UE Category DL 11 #-- @spec 36.523-2 A.4.3.2-2/6

pc_ue_CategoryDL_12,                         BOOLEAN,       false   #-- @desc  UE Category DL 12 #-- @spec 36.523-2 A.4.3.2-2/7

pc_ue_CategoryDL_13,                         BOOLEAN,       false   #-- @desc  UE Category DL 13 #-- @spec 36.523-2 A.4.3.2-2/8

pc_ue_CategoryDL_14,                         BOOLEAN,       false   #-- @desc  UE Category DL 14 #-- @spec 36.523-2 A.4.3.2-2/9

pc_ue_CategoryDL_15,                         BOOLEAN,       TRUE    #-- @desc  UE Category DL 15 #-- @spec 36.523-2 A.4.3.2-2/10

pc_ue_CategoryDL_16,                         BOOLEAN,       false   #-- @desc  UE Category DL 16 #-- @spec 36.523-2 A.4.3.2-2/11

pc_ue_CategoryDL_17,                         BOOLEAN,       false   #-- @desc  UE Category DL 17 #-- @spec 36.523-2 A.4.3.2-2/12

pc_ue_CategoryDL_18,                         BOOLEAN,       false   #-- @desc  UE Category DL 18 #-- @spec 36.523-2 A.4.3.2-2/13

pc_ue_CategoryDL_19,                         BOOLEAN,       false   #-- @desc  UE Category DL 19 #-- @spec 36.523-2 A.4.3.2-2/14

pc_ue_CategoryDL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category UL 1bis and Category 1 UE #-- @spec 36.523-2 A.4.3.2-2A/2

pc_ue_CategoryDL_20,                         BOOLEAN,       false   #-- @desc  UE Category DL 20 #-- @spec 36.523-2 A.4.3.2-2/15

pc_ue_CategoryDL_21,                         BOOLEAN,       false   #-- @desc  UE Category DL 21 #-- @spec 36.523-2 A.4.3.2-2/16

pc_ue_CategoryDL_22,                         BOOLEAN,       false   #-- @desc  UE Category DL 22 #-- @spec 36.523-2 A.4.3.2-2/17

pc_ue_CategoryDL_23,                         BOOLEAN,       false   #-- @desc  UE Category DL 23 #-- @spec 36.523-2 A.4.3.2-2/18

pc_ue_CategoryDL_24,                         BOOLEAN,       false   #-- @desc  UE Category DL 24 #-- @spec 36.523-2 A.4.3.2-2/19

pc_ue_CategoryDL_25,                         BOOLEAN,       false   #-- @desc  UE Category DL 25 #-- @spec 36.523-2 A.4.3.2-2/20

pc_ue_CategoryDL_26,                         BOOLEAN,       false   #-- @desc  UE Category DL 26 #-- @spec 36.523-2 A.4.3.2-2/21

pc_ue_CategoryDL_4,                          BOOLEAN,       false   #-- @desc  UE Category DL 4 #-- @spec 36.523-2 A.4.3.2-2/1A

pc_ue_CategoryDL_6,                          BOOLEAN,       false   #-- @desc  UE Category DL 6 #-- @spec 36.523-2 A.4.3.2-2/2

pc_ue_CategoryDL_7,                          BOOLEAN,       false   #-- @desc  UE Category DL 7 #-- @spec 36.523-2 A.4.3.2-2/3

pc_ue_CategoryDL_9,                          BOOLEAN,       false   #-- @desc  UE Category DL 9 #-- @spec 36.523-2 A.4.3.2-2/4

pc_ue_CategoryDL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M0 #-- @spec 36.523-2 A.4.3.2-2A/1

pc_ue_CategoryDL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M2 #-- @spec 36.523-2 A.4.3.2-2A/3

pc_ue_CategoryUL_0,                          BOOLEAN,       false   #-- @desc  UE Category UL 0 #-- @spec 36.523-2 A.4.3.2-3/1

pc_ue_CategoryUL_13,                         BOOLEAN,       false   #-- @desc  UE Category UL 13 #-- @spec 36.523-2 A.4.3.2-3/6

pc_ue_CategoryUL_14,                         BOOLEAN,       false   #-- @desc  UE Category UL 14 #-- @spec 36.523-2 A.4.3.2-3/7

pc_ue_CategoryUL_15,                         BOOLEAN,       false   #-- @desc  UE Category UL 15 #-- @spec 36.523-2 A.4.3.2-3/8

pc_ue_CategoryUL_16,                         BOOLEAN,       false   #-- @desc  UE Category UL 16 #-- @spec 36.523-2 A.4.3.2-3/9

pc_ue_CategoryUL_17,                         BOOLEAN,       false   #-- @desc  UE Category UL 17 #-- @spec 36.523-2 A.4.3.2-3/10

pc_ue_CategoryUL_18,                         BOOLEAN,       false   #-- @desc  UE Category UL 18 #-- @spec 36.523-2 A.4.3.2-3/11

pc_ue_CategoryUL_19,                         BOOLEAN,       false   #-- @desc  UE Category UL 19 #-- @spec 36.523-2 A.4.3.2-3/12

pc_ue_CategoryUL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category DL 1bis #-- @spec 36.523-2 A.4.3.2-3A/2

pc_ue_CategoryUL_20,                         BOOLEAN,       false   #-- @desc  UE Category UL 20 #-- @spec 36.523-2 A.4.3.2-3/13

pc_ue_CategoryUL_21,                         BOOLEAN,       false   #-- @desc  UE Category UL 21 #-- @spec 36.523-2 A.4.3.2-3/14

pc_ue_CategoryUL_22,                         BOOLEAN,       false   #-- @desc  UE Category UL 22 #-- @spec 36.523-2 A.4.3.2-3/15

pc_ue_CategoryUL_23,                         BOOLEAN,       false   #-- @desc  UE Category UL 23 #-- @spec 36.523-2 A.4.3.2-3/16

pc_ue_CategoryUL_24,                         BOOLEAN,       false   #-- @desc  UE Category UL 24 #-- @spec 36.523-2 A.4.3.2-3/17

pc_ue_CategoryUL_25,                         BOOLEAN,       false   #-- @desc  UE Category UL 25 #-- @spec 36.523-2 A.4.3.2-3/18

pc_ue_CategoryUL_26,                         BOOLEAN,       false   #-- @desc  UE Category UL 26 #-- @spec 36.523-2 A.4.3.2-3/19

pc_ue_CategoryUL_3,                          BOOLEAN,       false   #-- @desc  UE Category UL 3 #-- @spec 36.523-2 A.4.3.2-3/2

pc_ue_CategoryUL_5,                          BOOLEAN,       TRUE    #-- @desc  UE Category UL 5 #-- @spec 36.523-2 A.4.3.2-3/3

pc_ue_CategoryUL_7,                          BOOLEAN,       false   #-- @desc  UE Category UL 7 #-- @spec 36.523-2 A.4.3.2-3/4

pc_ue_CategoryUL_8,                          BOOLEAN,       false   #-- @desc  UE Category UL 8 #-- @spec 36.523-2 A.4.3.2-3/5

pc_ue_CategoryUL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M1 #-- @spec 36.523-2 A.4.3.2-3A/1

pc_ue_CategoryUL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M2 #-- @spec 36.523-2 A.4.3.2-3A/3

pc_ue_Category_1,                            BOOLEAN,       false   #-- @desc  UE Category 1 #-- @spec 36.523-2 A.4.3.2-1/1

pc_ue_Category_10,                           BOOLEAN,       false   #-- @desc  UE Category 10 #-- @spec 36.523-2 A.4.3.2-1/10

pc_ue_Category_11,                           BOOLEAN,       TRUE    #-- @desc  UE Category 11 #-- @spec 36.523-2 A.4.3.2-1/11

pc_ue_Category_12,                           BOOLEAN,       false   #-- @desc  UE Category 12 #-- @spec 36.523-2 A.4.3.2-1/12

pc_ue_Category_2,                            BOOLEAN,       false   #-- @desc  UE Category 2 #-- @spec 36.523-2 A.4.3.2-1/2

pc_ue_Category_3,                            BOOLEAN,       false   #-- @desc  UE Category 3 #-- @spec 36.523-2 A.4.3.2-1/3

pc_ue_Category_4,                            BOOLEAN,       TRUE    #-- @desc  UE Category 4 #-- @spec 36.523-2 A.4.3.2-1/4

pc_ue_Category_5,                            BOOLEAN,       false   #-- @desc  UE Category 5 #-- @spec 36.523-2 A.4.3.2-1/5

pc_ue_Category_6,                            BOOLEAN,       TRUE    #-- @desc  UE Category 6 #-- @spec 36.523-2 A.4.3.2-1/6

pc_ue_Category_7,                            BOOLEAN,       false   #-- @desc  UE Category 7 #-- @spec 36.523-2 A.4.3.2-1/7

pc_ue_Category_8,                            BOOLEAN,       false   #-- @desc  UE Category 8 #-- @spec 36.523-2 A.4.3.2-1/8

pc_ue_Category_9,                            BOOLEAN,       TRUE    #-- @desc  UE Category 9 #-- @spec 36.523-2 A.4.3.2-1/9

pc_um_WithLongSN,                            BOOLEAN,       TRUE    #-- @desc  Support RLC UM with 12 bit length of RLC sequence number #-- @spec 38.508-2 Table A.4.3.4-1/2

pc_um_WithShortSN,                           BOOLEAN,       TRUE    #-- @desc  Support RLC UM with 6 bit length of RLC sequence number #-- @spec 38.508-2 Table A.4.3.4-1/3

pc_uplink_LAA,                               BOOLEAN,       false   #-- @desc  Supports uplink LAA operation #-- @spec 36.523-2 A.4.4-1/174

pc_v2xPartialSensing,                        BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using UE autonomous resource selection mode with partial sensing #-- @spec 36.523-2 A.4.4-1/154

pc_voiceFallbackIndication,                  BOOLEAN,       TRUE    #-- @desc  Support of voiceFallbackIndication #-- @spec 38.508-2 Table A.4.3.7-1/15

pc_voiceOverNR,                              BOOLEAN,       TRUE    #-- @desc  Support IMS voice over NR #-- @spec 38.508-2 Table A.4.3.7-1/XX

pc_voice_PS_1_CS_2,                          BOOLEAN,       false   #-- @desc  Configured voice domain preference #-- @spec 36.523-2 A.4.4-2/9

pc_wakeUpSignal,                             BOOLEAN,       false   #-- @desc  Support of Wake Up Signal #-- @spec 36.523-2 A.4.4-1/210

px_AccessPointName,                          OCTETSTRING,   03696D73 #-- @desc  Access Point Name #-- @spec 

px_AquireGNSS_MaxTime,                       INTEGER,       60      #-- @desc  The maximume time (in seconds) taken for the UE to acquire GNSS and derive UTC time (and normally position) and then start to transit or receive as appropriate #-- @spec 

px_AttachTypeTested,                         ENUM-EUTRA_ATTACH_TESTED_Type,COMBINED_ATTACH #-- @desc  Attach Type to be tested if UE supports both pc_Attach and pc_Combined_Attach #-- @spec 

px_AuthAMF,                                  BITSTRING,     1001000100010001 #-- @desc  Authentication Management Field (16 bits). The value shall be different from '1111 1111 1111 111'B (AMFresynch). #-- @spec 34.123-3, Table B.1

px_AuthK,                                    BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  Authentication Key #-- @spec 34.123-3, Table B.1

px_BcapDataCompression,                      BITSTRING,     0       #-- @desc  Data compression supported (used in the Bearer Capability).Default value: Default IMSI #-- @spec 34.123-3, Table B.2

px_BcapFNUR,                                 BITSTRING,     00001   #-- @desc  Fixed Network User rate supported: 00001B: FNUR 9.6 kbits 00010B: FNUR 14.4 kbits 00011B: FNUR 19.2 kbits 00100B: FNUR 28.8 kbits 00101B: FNUR 38.4 kbits 00110B: FNUR 48.0 kbits 00111B: FNUR 56.0 kbits 01000B: FNUR 64.0 kbits 01001B: FNUR 33.6 kbits 01010B: FNUR 32.0 kbits. #-- @spec 34.123-3, Table B.2

px_CipherAlg,                                BITSTRING,     010     #-- Anritsu TTCN CR required px_CipherAlg type @desc  NAS Ciphering Algorithm Default value: (GEA2) #-- @spec 

px_CipherKey,                                BITSTRING,     0101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher Key #-- @spec 51.010-5, Table B.1

px_CipherKey128,                             BITSTRING,     01011110010010101011001101011000100100010011011101011101001010100101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher key (128 bits) to be used e.g. for A54 and GEA4 #-- @spec 34.123-3, Table B.1.11

px_DelayBeforeIntraCellHO,                   INTEGER,       300     #-- @desc  Temporary PIXIT used to define the delay before an intra cell handover #-- @spec 

px_DigestPasswordForXCAP,                    CHARSTRING,    XCAP-Password #-- @desc  XCAP password #-- @spec 34.229-3

px_ENDC_BandCombination,                     ENUM-ENDC_BandCombination_Type,DC_13A_n257A #-- @desc  Band combination for EN-DC test cases #-- @spec 

px_ENDC_CA_BandCombination,                  ENUM-ENDC_CA_BandCombination_Type,DC_1A_n28A_n78A #-- @desc  EN-DC CA Band Combination #-- @spec 

px_ENDC_SecondaryBandCombination,            ENUM-ENDC_BandCombination_Type,DC_13A_n257A #-- @desc  Secondary band combination for EN-DC test cases #-- @spec 

px_EUTRA_CA_BandCombination,                 ENUM-CA_BandCombination_Type,CA_1C   #-- @desc  CA band combination applied in CA test cases #-- @spec 

px_EUTRA_DC_BandCombination,                 ENUM-DC_BandCombination_Type,DC_1A_3A #-- @desc  DC band combination applied in DC test cases #-- @spec 

px_EllipsoidPointWithAltitude,               OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_EmergencyCallNumber,                      CHARSTRING,    112     #-- @desc  Emergency Number used by UE to initiate an emergency call #-- @spec 34.123-3, Table B.1.2

px_FDD_OperationBand,                        INTEGER,       1       #-- @desc  The operation band under test as defined in 34.108 clause 5.1.1. Value 1 means Band 1 2 means Band 2 etc.This pixit shall be set in synchronisation with the values that are being set to 6 other Pixits viz: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid #-- @spec 34.123-3, Table B.1

px_FRESH,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  no default value can be proposed #-- @spec 34.123-3, Table B.1

px_GERAN_BandUnderTest,                      ENUM-GERAN_BandUnderTestType,GSM_P900 #-- @desc  Indicates which band is under test.  The type is different to the parameter defined in 34.123-3 #-- @spec 

px_GPRS_CipheringAlgorithm,                  ENUM-GPRS_CipheringAlgorithm_Type,gea2    #-- @desc  NAS Ciphering Algorithm Default value: (GEA2) #-- @spec 34.123-3, Table B.1

px_GSM_CipherAlg,                            BITSTRING,     000     #-- @desc  GSM Cipher algorithm. #-- @spec 51.010-5, Table B.1

px_GSM_CipheringOnOff,                       BITSTRING,     1       #-- @desc  GSM Ciphering to be started or not #-- @spec 51.010-5, Table B.1

px_GeoInfo,                                  OCTETSTRING,   9032B9D66360B600323C3C006544 #-- @desc Geographical information to be sent as Location Estimate in FACILITY message from the System Simulator. #-- @spec 37.571-4 Table B.1.13

px_GnssScenario2012,                         BOOLEAN,       false   #-- @desc  Usage of GNSS scenarios with date in 2012 from 3GPP TS 37.571-5 #-- @spec 37.571-4 Table 8.2-1

px_HorizontalVelocity,                       OCTETSTRING,   123456  #-- @desc  Horizontal Velocity to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_IMEISV_Def,                               HEXSTRING,     0044001520200000 #-- @desc  Default IMEISV value.  No default can be proposed as this is a manufacturer defined value #-- @spec 34.123-3, Table B.1

px_IMEI_Def,                                 HEXSTRING,     004400152020000 #-- @desc  Default IMEI value transmitted by UE.  Digit 15 shall be set as a Spare Digit i.e. shall be set to '0' (see TS 23.003) #-- @spec 34.123-3, Table B.1

px_IMSI_Def,                                 HEXSTRING,     001010000000333 #-- @desc  Default IMSI #-- @spec 34.123-3, Table B.1

px_IMSI_Diff,                                HEXSTRING,     001010654321063 #-- @desc  Different IMSI from the IMSI stored in the USIM #-- @spec 34.123-3, Table B.1

px_IMS_AssociatedTelUri,                     CHARSTRING,    tel:+331234567 #-- @desc  Set as record 3 in EFIMPU as defined in TS 34.229-1[5] #-- @spec 34.229-3

px_IMS_CalleeContactUri,                     CHARSTRING,    sip:User-B-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog #-- @spec 34.229-3

px_IMS_CalleeContactUri2,                    CHARSTRING,    sip:User-C-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog #-- @spec 34.229-3

px_IMS_CalleeUri,                            CHARSTRING,    sip:User-B@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE #-- @spec 34.229-3

px_IMS_CalleeUri2,                           CHARSTRING,    sip:User-C@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE #-- @spec 34.229-3

px_IMS_CiphAlgo_Def,                         ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ciphering Algorithm #-- @spec 34.229-3

px_IMS_HomeDomainName,                       CHARSTRING,    3gpp.org #-- @desc  Home Domain Name. #-- @spec 34.229-3

px_IMS_HomeDomainName_Refreshed,             CHARSTRING,    refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_IPSecAlgorithm,                       ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Integrity Algorithm #-- @spec 34.229-3

px_IMS_MessageAccountIdentity,               CHARSTRING,    testaccountidentity #-- @desc  message accout identity configured at the UE as used for subscription to message-summary event package #-- @spec 

px_IMS_Private_UserId,                       CHARSTRING,    privateuser@3gpp.org #-- @desc  Private User Identity.When usingan ISIM this is set to the same value as EFIMPI.When ISIM is not used just USIM the private user identity is derived from px_IMSI. #-- @spec 34.229-3

px_IMS_Private_UserId_Refreshed,             CHARSTRING,    privateuser@refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_PublicUserIdentity1,                  CHARSTRING,    sip:PublicId1@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the first record in EFIMPU. #-- @spec 34.229-3

px_IMS_PublicUserIdentity1_Refreshed,        CHARSTRING,    sip:PublicId1@refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_PublicUserIdentity2,                  CHARSTRING,    sip:PublicId2@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the second record in EFIMPU. #-- @spec 34.229-3

px_IMS_PublicUserIdentity3,                  CHARSTRING,    sip:PublicId3@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the third record in EFIMPU. #-- @spec 34.229-3

px_IMS_SPI_ValidValueList_PDN1,              CHARSTRING,    256,258,264,266 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN1; each value shall be greater than or equal to 256 #-- @spec 34.229-3

px_IMS_SPI_ValidValueList_PDN2,              CHARSTRING,    260,262,268,270 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN2; each value shall be greater than or equal to 256 #-- @spec 34.229-3

px_IP_MTU_Size,                              INTEGER,       1300    #-- @desc  MTU size. This value is specific to the SS. #-- @spec 

px_IPv4_Address,                             CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address #-- @spec 

px_IPv4_Address1_NW,                         CHARSTRING,    192.168.0.3 #-- @desc  IPv4 Gateway Address in PDN1 #-- @spec 

px_IPv4_Address1_RemoteUE,                   CHARSTRING,    192.168.0.6 #-- @desc  IPv4 Address of remote UE connected to PDN1 #-- @spec 

px_IPv4_Address1_UE,                         CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address connected to PDN1 #-- @spec 

px_IPv4_Address2,                            CHARSTRING,    192.168.1.2 #-- @desc  2nd IPv4 Address @sic R5s110011 sic@ #-- @spec 

px_IPv4_Address2_NW,                         CHARSTRING,    192.168.1.4 #-- @desc  IPv4 Gateway Address in PDN2 #-- @spec 

px_IPv4_Address2_RemoteUE,                   CHARSTRING,    192.168.1.6 #-- @desc  IPv4 Address of remote UE connected to PDN2 #-- @spec 

px_IPv4_Address2_UE,                         CHARSTRING,    192.168.1.2 #-- @desc  IPv4 Address connected to PDN2 #-- @spec 

px_IPv4_Address2a_UE,                        CHARSTRING,    192.168.1.3 #-- @desc  IPv4 Address connected to PDN2a #-- @spec 

px_IPv4_Address3_NW,                         CHARSTRING,    192.168.1.8 #-- @desc  IPv4 Gateway Address in PDN3 #-- @spec 

px_IPv4_Address3_RemoteUE,                   CHARSTRING,    192.168.1.9 #-- @desc  IPv4 Address of remote UE connected to PDN3 #-- @spec 

px_IPv4_Address3_UE,                         CHARSTRING,    192.168.1.7 #-- @desc  IPv4 Address connected to PDN3 #-- @spec 

px_IPv4_Address4_NW,                         CHARSTRING,    192.168.2.1 #-- @desc  IPv4 Gateway Address in PDN4 #-- @spec 

px_IPv4_Address4_UE,                         CHARSTRING,    192.168.2.2 #-- @desc  IPv4 Address connected to PDN4 #-- @spec 

px_IPv4_Address5_NW,                         CHARSTRING,    192.168.2.3 #-- @desc  IPv4 Gateway Address in PDN5 #-- @spec 

px_IPv4_Address5_UE,                         CHARSTRING,    192.168.2.4 #-- @desc  IPv4 Address connected to PDN5 #-- @spec 

px_IPv4_Address6_NW,                         CHARSTRING,    192.168.2.5 #-- @desc  IPv4 Gateway Address in PDN6 #-- @spec 

px_IPv4_Address6_UE,                         CHARSTRING,    192.168.2.6 #-- @desc  IPv4 Address connected to PDN6 #-- @spec 

px_IPv4_Address_HomeAgent,                   CHARSTRING,    192.168.0.5 #-- @desc  IPv4 Home Address Agent #-- @spec 

px_IPv4_Address_Other,                       CHARSTRING,    192.168.0.8 #-- @desc  Other IPv4 Address #-- @spec 

px_IPv6_Address,                             CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address #-- @spec 

px_IPv6_Address1_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 Gateway Address in PDN1 #-- @spec 

px_IPv6_Address1_RemoteUE,                   CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN1 #-- @spec 

px_IPv6_Address1_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address in PDN1 #-- @spec 

px_IPv6_Address2,                            CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  2nd IPv6 Address  @sic R5s110011 sic@ #-- @spec 

px_IPv6_Address2_NW,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:4444 #-- @desc  IPv6 Gateway Address in PDN2 #-- @spec 

px_IPv6_Address2_RemoteUE,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN2 #-- @spec 

px_IPv6_Address2_UE,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  IPv6 Address in PDN2 #-- @spec 

px_IPv6_Address2a_UE,                        CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Address in PDN2a #-- @spec 

px_IPv6_Address3_NW,                         CHARSTRING,    C0C0:C0C0:C0C0:C004:C0C0:C0C0:C0C0:C0C0 #-- @desc  IPv6 Gateway Address in PDN3 #-- @spec 

px_IPv6_Address3_RemoteUE,                   CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:9999 #-- @desc  IPv6 Address of remote UE in PDN3 #-- @spec 

px_IPv6_Address3_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:7777 #-- @desc  IPv6 Address in PDN3 #-- @spec 

px_IPv6_Address4_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:1111 #-- @desc  IPv6 Gateway Address in PDN4 #-- @spec 

px_IPv6_Address4_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:2222 #-- @desc  IPv6 Address in PDN4 #-- @spec 

px_IPv6_Address5_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:3333 #-- @desc  IPv6 Gateway Address in PDN5 #-- @spec 

px_IPv6_Address5_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:4444 #-- @desc  IPv6 Address in PDN5 #-- @spec 

px_IPv6_Address6_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:5555 #-- @desc  IPv6 Gateway Address in PDN6 #-- @spec 

px_IPv6_Address6_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:5555:6666 #-- @desc  IPv6 Address in PDN6 #-- @spec 

px_IPv6_Address_BSF,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 BSF address #-- @spec 

px_IPv6_Address_HomeAgent,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Home Address Agent #-- @spec 

px_IPv6_Address_Other,                       CHARSTRING,    1111:2222:3333:4444:5555:5555:6666:8888 #-- @desc  Other IPv6 Address #-- @spec 

px_LcsClientAddressDigits,                   CHARSTRING,    123456  #-- @desc LCS Client external address Digits #-- @spec 37.571-4 Table B.1.13

px_LcsClientAddressNPI,                      BITSTRING,     0001    #-- @desc LCS Client external address NPI #-- @spec 37.571-4 Table B.1.13

px_LcsClientAddressTOA,                      BITSTRING,     1001    #-- @desc LCS Client external address TOA #-- @spec 37.571-4 Table B.1.13

px_LcsClientName,                            CHARSTRING,    OPERATOR #-- @desc LCS Client name #-- @spec 37.571-4 Table B.1.13

px_MFBI_BandChannelBandwidth,                ENUM-Dl_Bandwidth_Type,n25     #-- @desc  MFBI E-UTRAN Channel Bandwidth #-- @spec 

px_MFBI_FrequencyBand,                       INTEGER,       26      #-- @desc  a supported E-UTRA MFBI frequency band #-- @spec 

px_MFBI_UTRAN_FrequencyBand,                 INTEGER,       26      #-- @desc  A supported UTRAN MFBI frequency band. #-- @spec 34.123-3, Table B.1.20

px_MS_ClsmkESIND,                            BITSTRING,     0       #-- @desc  Default Early Sending Indication #-- @spec 34.123-3, Table B.1

px_MS_ClsmkRevLvl,                           BITSTRING,     10      #-- @desc  Default Revision Level #-- @spec 34.123-3, Table B.1

px_MobileDataOn,                             BOOLEAN,       true    #-- @desc  Specifies whether mobile data associated with Internet PDN is enabled on the DUT #-- @spec 

px_NAS_5GC_AuthenticationType,               ENUM-NAS_5GC_AKA_Type,AKA_5G  #-- @desc  NAS 5GC Authentication type #-- @spec 

px_NAS_5GC_CipheringAlgorithm,               BITSTRING,     0010    #-- @desc  NAS 5GC Ciphering Algorithm #-- @spec 

px_NAS_5GC_IntegrityAlgorithm,               BITSTRING,     0010    #-- @desc  NAS 5GC Integrity Algorithm #-- @spec 

px_NAS_5GC_XRES_Length,                      INTEGER,       16      #-- @desc  NAS 5GC XRES length in octets used in Authentication #-- @spec 

px_NAS_CipheringAlgorithm,                   BITSTRING,     001     #-- @desc  NAS Ciphering Algorithm (eea1) #-- @spec 

px_NAS_IntegrityProtAlgorithm,               BITSTRING,     001     #-- @desc  NAS Integrity Algorithm (eia1) #-- @spec 

px_NEDC_BandCombination,                     ENUM-NEDC_BandCombination_Type,DC_n28A_3A #-- @desc  NE-DC Band Combination #-- @spec 

px_NEDC_SecondaryBandCombination,            ENUM-NEDC_BandCombination_Type,DC_n28A_39A #-- @desc  Secondary NE-DC Band Combination #-- @spec 

px_NR_CA_3CC_BandCombination,                ENUM-NR_CA_3CC_BandCombination_Type,CA_n257H #-- @desc  NR CA Band Combination with 3CC #-- @spec 

px_NR_CA_BandCombination,                    ENUM-NR_CA_BandCombination_Type,CA_n79A_n257A #-- @desc  NR CA Band Combination #-- @spec 

px_NR_CipheringAlgorithm,                    ENUM-CipheringAlgorithm,nea1    #-- @desc  Ciphering Algorithm #-- @spec 

px_NR_DC_BandCombination,                    ENUM-NR_DC_BandCombination_Type,DC_n79A_n257A #-- @desc  NR CA Band Combination #-- @spec 

px_NR_DC_CA_BandCombination,                 ENUM-NR_DC_CA_BandCombination_Type,DC_n79A_n257G #-- @desc  NR DC CA Band Combination #-- @spec 

px_NR_IntegrityProtAlgorithm,                ENUM-IntegrityProtAlgorithm,nia1    #-- @desc  Integrity Algorithm #-- @spec 

px_NR_OverlappingNotSupportedBand_MFBI,      INTEGER,       77      #-- @desc  A not supported NR band that is overlapping with a supported band (px_NR_PrimaryBand). Applied to MFBI test case scenario. #-- @spec 

px_NR_PrimaryBand,                           INTEGER,       257     #-- @desc  NR primary band #-- @spec 

px_NR_PrimaryBandDeltaNRf1,                  INTEGER,       -9      #-- @desc  delta frequency in dB for NR primary band test frequency NRf1 #-- @spec 

px_NR_PrimaryBandDeltaNRf2,                  INTEGER,       -9      #-- @desc  delta frequency in dB for NR primary band test frequency NRf2 #-- @spec 

px_NR_PrimaryBandDeltaNRf3,                  INTEGER,       0       #-- @desc  delta frequency in dB for NR primary band test frequency NRf3 #-- @spec 

px_NR_PrimaryBandDeltaNRf4,                  INTEGER,       0       #-- @desc  delta frequency in dB for NR primary band test frequency NRf4 #-- @spec 

px_NR_PrimaryBandDeltas_DeltaNRf1,           INTEGER,       -9      #-- @desc  ?(f) in dB for NR primary band test frequencies NRf1, NRf2, NRf3 and NRf4 #-- @spec 

px_NR_RATComb_Tested,                        ENUM-NR_RATComb_Tested_Type,NR_UTRA #-- @desc  This parameter represents the network RAT capability  preference and indicates which if #-- @spec 

px_NR_SecondaryBand,                         INTEGER,       257     #-- @desc  NR secondary band #-- @spec 

px_NR_SecondaryBandDeltaNRf1,                INTEGER,       -9      #-- @desc  delta frequency in dB for NR secondary band test frequency NRf1 #-- @spec 

px_NR_SecondaryBandDeltaNRf2,                INTEGER,       -9      #-- @desc  delta frequency in dB for NR secondary band test frequency NRf2 #-- @spec 

px_NR_SecondaryBandDeltaNRf3,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf3 #-- @spec 

px_NR_SecondaryBandDeltaNRf4,                INTEGER,       0       #-- @desc  delta frequency in dB for NR secondary band test frequency NRf4 #-- @spec 

px_NR_SidelinkBand,                          INTEGER,       47      #-- @desc  NR sidelink band #-- @spec 

px_NR_V2X_ConcurrentOperationBandCombination,ENUM-NR_V2X_ConcurrentOperationBandCombination_Type,V2X_n71_n47 #-- @desc  V2X operating bands for con-current operation #-- @spec 

px_NoTDD_LCR_onLTE,                          BOOLEAN,       false   #-- @desc  Only applicable to UE supporting (at least) LTE and LCR TDD.  If set to true the UE is configured not to report support of LCR TDD (IE utraTDD128 in UECapabilityInformation) when being camped on an LTE cell with no detectable LCR TDD cell in the environment. #-- @spec 

px_OverlappingNotSupportedFrequencyBand_MFBI,INTEGER,       27      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band #-- @spec 

px_OverlappingSupportedFrequencyBand_MFBI,   INTEGER,       26      #-- @desc  a supported E-UTRA frequency band overlapping withpx_OverlappingNotSupportedFrequencyBand_MFBI applied to MFBI enhancement test case scenario. #-- @spec 

px_PTMSI_Def,                                OCTETSTRING,   C2345678 #-- @desc  Default PTMSI #-- @spec 34.123-3, Table B.1

px_PTMSI_SigDef,                             OCTETSTRING,   AB1234  #-- @desc  Default PTMSI signature (3 octets 3GPP 24.008   10.5.5.8). #-- @spec 34.123-3, Table B.1

px_PWS_CB_DataCodingScheme,                  BITSTRING,     1010    #-- @desc  CMAS or ETWS data coding scheme of the alphabetcodingand the applied language (see TS 23.401) #-- @spec 

px_PWS_CB_DataPage1,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 1 warning data message #-- @spec 

px_PWS_CB_DataPage2,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 2 warning data message #-- @spec 

px_PWS_CB_DataPage3,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 3 warning data message #-- @spec 

px_PWS_CB_DataPage4,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 4 warning data message #-- @spec 

px_PowerLevel,                               BITSTRING,     00000   #-- @desc  power level value for L1 header #-- @spec 51.010-5, Table B.1

px_RATComb_Tested,                           ENUM-RATComb_Tested_Type,EUTRA_UTRA #-- @desc  This parameter represents the network RAT capabilitypreference and indicates which if any is supported RAT combination is to be tested #-- @spec 

px_RRC_CipheringAlgorithm,                   CHARSTRING,    eea1    #-- @desc  Ciphering Algorithm #-- @spec 

px_RRC_CipheringAlgorithm_r12,               ENUM-CipheringAlgorithm_r12,eea1    #-- @desc  Ciphering Algorithm #-- @spec 

px_RRC_IntegrityProtAlgorithm,               ENUM-IntegrityProtAlgorithm_Type,eia1    #-- @desc  Integrity Algorithm #-- @spec 

px_RRC_PS_ServTested,                        ENUM-RRC_ServTested,ps_Interactive #-- @desc  PS Service to be tested #-- @spec 34.123-3, Table B.1

px_RXLEV_ACCESS_MIN,                         BITSTRING,     000000  #-- @desc   minimum received signal level at MS #-- @spec 51.010-5, Table B.1

px_Release_check_in_eMBMS_TCs,               BOOLEAN,       true    #-- Anritsu TTCN WA for release check in MBMS #-- @spec 

px_ReportUTRA_RAT,                           ENUM-ReportUTRA_RAT_Type,both    #-- @desc  Specifies which UTRA RATs a UE reports on #-- @spec 

px_ResetStoredInfo,                          BOOLEAN,       false   #-- @desc Support of RESETUEPOSITIONINGSTOREDINFORMATION command as defined in 3GPP TS 34.109 cl. 6.10 #-- @spec 34.109 cl. 6.10

px_SMSTransport_CP_CIoT,                     BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise the SMS service as transport mechanism for user data for Control Plane CIoT Optimisation #-- @spec 

px_SMS_ChkMsgReceived,                       BOOLEAN,       true    #-- @desc  Whether the operator can check an MT Short Message received #-- @spec 

px_SMS_IndexOffset,                          INTEGER,       100     #-- @desc  Memory location index at UE for SMS storage used in +CMSS command #-- @spec 34.123-3, Table B.1.2

px_SMS_MsgFrmt,                              CHARSTRING,    1       #-- @desc  SMS message format <mode> (see TS 27.005 cl.3.2.). NOTE: Default value is for text mode. Change value to 0 to execute tests with PDU mode #-- @spec 

px_SMS_PrefMem1,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 1 <mem1> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_PrefMem2,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 2 <mem2> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_PrefMem3,                             CHARSTRING,    MT      #-- @desc  SMS Preferred Memory 3 <mem3> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_SMSC_InternationalNumber,             CHARSTRING,    112233445566778 #-- @desc  international number of the SMSC: #-- @spec 34.229-3

px_SMS_Service,                              CHARSTRING,    0       #-- @desc  SMS Service <service> of TS 27.005 [31] clause 3.2.1 #-- @spec 34.123-3, Table B.1.2

px_SPI_pc,                                   INTEGER,       5000    #-- Anritsu TTCN WA for SPI #-- @spec 

px_SPI_ps,                                   INTEGER,       1000    #-- Anritsu TTCN WA for SPI #-- @spec 

px_SRNC_Id,                                  BITSTRING,     000000000001 #-- @desc  SRNC Id #-- @spec 34.123-3, Table B.1

px_SRNTI,                                    BITSTRING,     00000000000000000001 #-- @desc  S RNTI #-- @spec 34.123-3, Table B.1

px_SinglePLMN_Tested,                        ENUM-SinglePLMN_TestedType,MultiPLMN #-- @desc  This parameter represents the network capabilitypreference to support multi PLMNs on the same test Band and indicates the preference of multi PLMNs or single PLMN test environment. This PIXIT shall be set to SinglePLMN when only one frequency is defined for the test band #-- @spec 

px_SplitOnCCCH,                              BITSTRING,     0       #-- @desc  Split pg cycle on CCCH supported indication #-- @spec 51.010-5, Table B.1

px_StartStop,                                BOOLEAN,       TRUE    #-- Anritsu TTCN WA for Automation EnableDisable #-- @spec 

px_StartString,                              CHARSTRING,    StartTest: #-- Anritsu TTCN WA for Automation Starting test cases string e.g.: StartTest:TC_7_1_2_1 #-- @spec 

px_StopString,                               CHARSTRING,    EndTest: #-- Anritsu TTCN WA for Automation Stopping test cases string e.g.: StopTest:Passed #-- @spec 

px_TDD_OperationBandCharstring,              CHARSTRING,    a       #-- @desc  Applicable for TDD. The operation band under test as defined in 34.108 clause 5.1.2 #-- @spec 

px_TMSI_Def,                                 OCTETSTRING,   12345678 #-- @desc  Default TMSI #-- @spec 34.123-3, Table B.1

px_TSC,                                      BITSTRING,     011     #-- @desc  Training sequence code for traffic channels. #-- @spec 51.010-5, Table B.1

px_TestLoopModeB_Delay,                      OCTETSTRING,   5A      #-- @desc  This parameter represents the IP PDU delay to be used for UE test loop mode B intest cases where long delay may be needed e.g. because of user interaction. #-- @spec 

px_TimingAdvance,                            BITSTRING,     0000000 #-- @desc  Timing advance value for L1 header #-- @spec 51.010-5, Table B.1

px_UARFCN_D_High,                            INTEGER,       10837   #-- @desc  High Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_D_Low,                             INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_D_Mid,                             INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_High_TDD,                          INTEGER,       9596    #-- @desc  High Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Low_TDD,                           INTEGER,       9504    #-- @desc  Low Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Mid_TDD,                           INTEGER,       9550    #-- @desc  Mid Range downlink UARFCN value for LCR TDD #-- @spec 

px_UE_CS_PS_UsageSetting_Tested,             ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CSPS mode is under test @sic R5s120274 sic@ #-- @spec 

px_UE_PS_UsageSetting_Tested,                ENUM-PS_MODE,  VOICE_CENTRIC #-- @desc  specifies which PS mode is under test @sic R5s120274 sic@ #-- @spec 

px_UEwithISIM,                               BOOLEAN,       true    #-- @desc  true - UE has ISIM; false - UE has USIM only #-- @spec 34.229-3

px_UTRAN_CipheringAlgorithm,                 ENUM-CipheringAlgorithm_r7,uea2    #-- @desc  UTRAN Ciphering algorithm #-- @spec 

px_UTRAN_ModeUnderTest,                      ENUM-UTRAN_FDD_TDD_Type,UTRAN_FDD #-- @desc  specifies which radio access technology is being tested in UTRAN #-- @spec 

px_UTRAN_OverlappingNotSupportedFrequencyBandMFBI,INTEGER,       27      #-- @desc  A not supported UTRAN frequency band that is overlapping with a supported MFBI band (px_MFBI_UTRAN_FrequencyBand). This pixit shall be set also in accordance with the values of the 3 Pixits: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid. #-- @spec 

px_UeLcsNotification,                        INTEGER,       20      #-- @desc Value for UE LCS Notification timeout timer (in seconds) #-- @spec 37.571-4 Table B.1.13

px_WLANBand,                                 ENUM-WLAN_Band_Type,Band2_4Ghz #-- @desc  WLAN ISM Band #-- @spec 

px_WLAN_BeaconRSSI,                          INTEGER,       78      #-- @desc  Beacon RSSI value for IMS over WLAN test cases #-- @spec 

px_WLAN_NetworkAddrIPv4,                     CHARSTRING,    192.168.3.1 #-- @desc  IPv4 WLAN Network Address #-- @spec 

px_WLAN_NetworkAddrIPv6,                     CHARSTRING,    1111:2222:3333:4444:5555:6666:3333:2222 #-- @desc  IPv6 WLAN Network Address #-- @spec 

px_WLAN_PDN1_ToOffload,                      BOOLEAN,       true    #-- @desc  If set to true the first PDN connection is offloaded to WLAN. If set to false the second PDN connection is offloaded to WLAN. #-- @spec 

px_WLAN_RulesToBeTested,                     CHARSTRING,    ANDSF_Rules #-- @desc  Rules to be tested in WLAN test cases #-- @spec 

px_WLAN_UE_AddrIPv4,                         CHARSTRING,    1.1.1.30 #-- @desc  IPv4 WLAN UE Address #-- @spec 

px_WLAN_UE_AddrIPv6,                         CHARSTRING,    1111:1111:1111:1111:1111:1111:1111:2222 #-- @desc  IPv6 WLAN UE Address #-- @spec 

px_XCAP_RootUri,                             CHARSTRING,    /XCAP.3gpp.org #-- @desc  XCAP Root URI #-- @spec 

px_XCAP_TargetUri,                           CHARSTRING,    sip:user@domain.com #-- @desc  Target (SIP or TEL URI) where to forward to #-- @spec 

px_XCAP_Username,                            CHARSTRING,    0       #-- @desc  username to be used for HTTP authentication in case of pc_XCAP_UsernameIsConfiguredInUE==true #-- @spec 

px_eAuthRAND,                                BITSTRING,     10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111 #-- @desc  Random Challenge #-- @spec 

px_eJapanMCC_Band6,                          HEXSTRING,     442     #-- @desc  Japan MCC code to be used for Band 6. The same value will be used for E-UTRAN and Inter-RAT cells. Type is different to that defined in 34.123-3. #-- @spec 

px_eMaxNumberROHC_ContextSessions,           ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions @sic R5s130329 sic@ #-- @spec 

px_ePDG_Ipsec_CipheringAlgorithm,            ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ipsec Ciphering Algorithm used in ePDG #-- @spec 

px_ePDG_Ipsec_IntegrityAlgorithm,            ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Ipsec Integrity Algorithm used in ePDG #-- @spec 

px_ePDG_OperatorProvisionedFQDN,             CHARSTRING,    en.test.org #-- @desc  domain name of the ePDG to be considered to assign the IP addresses of the ePDG in responses to DNS queries #-- @spec 

px_ePrimaryBandChannelBandwidth,             ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_ePrimaryFrequencyBand #-- @spec 

px_ePrimaryFrequencyBand,                    INTEGER,       2       #-- @desc  E-UTRAN primary frequency band #-- @spec 

px_eSecondaryBandChannelBandwidth,           ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_eSecondaryFrequencyBand #-- @spec 

px_eSecondaryFrequencyBand,                  INTEGER,       2       #-- @desc  E-UTRAN secondary frequency band #-- @spec 

px_eTDDsubframeConfig,                       ENUM-TDD_SubframeAssignment_Type,sa1     #-- @desc  TDD uplink-downlink subframe configuration #-- @spec 

px_nPrimaryFrequencyBand,                    INTEGER,       257     #-- @desc  NR primary frequency band #-- @spec 

px_nonSMSTransport_CP_CIoT,                  BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise non-SMS services as transport mechanism for user data for Control Plane CIoT Optimisation #-- @spec 

