    Log Viewer Console 397.3.0.0
    Copyright © 2024, Keysight Technologies

    LogFile                      : TC_8_1_3_1_2_20240227_131925_n257_PASS_v77.0.alf
    This file produced           : 20/03/2024 09:45:58 +00:00
    This file produced UTC       : 20/03/2024 09:45:58
    Test activity start time     : 27/02/2024 13:19:32 -08:00
    Test activity start time UTC : 27/02/2024 21:19:31

    Export options:
    Filter              : 5G_NR_Filter_SA

| Details

    recordType = 22
    fileName = NR5GC_Testsuite_v77_0
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 86
    text = ----------------------------------------------------------------------------------------------------

    recordType = 22
    fileName = NR5GC_Testsuite_v77_0
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 87
    text = Test case started             : TC_8_1_3_1_2_NR5GC

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 83
    text = Mapping port "MTC_NR5GC:Ut" to port "SYSTEM_NR5GC:Ut"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 193
    text = Mapping port "NR5GC:SYS" to port "SYSTEM_NR5GC:NR_SYS"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 194
    text = Mapping port "NR5GC:SYSIND" to port "SYSTEM_NR5GC:NR_SYSIND"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 195
    text = Mapping port "NR5GC:DRB" to port "SYSTEM_NR5GC:NR_DRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 41
    text = Connecting port "NR5GC:NASCTRL" to port "NASEMU_NRNG:CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 41
    text = Connecting port "NR5GC:SRB" to port "NASEMU_NRNG:TC_SRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 48
    text = Mapping port "NASEMU_NRNG:SYS_SRB" to port "SYSTEM_NR5GC:NR_SRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 353
    text = Mapping port "IP:IP_CTRL" to port "SYSTEM_NR5GC:IP_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 354
    text = Mapping port "IP:IPSEC_CTRL" to port "SYSTEM_NR5GC:IPSEC_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 355
    text = Mapping port "IPMUX:IP_SOCK" to port "SYSTEM_NR5GC:IP_SOCK"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 355
    text = Connecting port "IP:IP_SOCK_DATA" to port "IPMUX:IP_SOCK_DATA"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 355
    text = Connecting port "IP:IP_SOCK_CTRL" to port "IPMUX:IP_SOCK_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 355
    text = Connecting port "IP:IP_SOCK_CTRL_QUEUE" to port "IPMUX:IP_SOCK_CTRL_QUEUE"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 61
    text = Connecting port "NR5GC:IP" to port "IP:NR_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS1:IMS_CTRL" to port "IP:IMS_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS1:IMS_Server" to port "IP:IMS_Server"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS1:IMS_Client" to port "IP:IMS_Client"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS1:MMI" to port "MTC_NR5GC:PTC_Ut"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS1:IPCAN" to port "NR5GC:IMS"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 82
    text = Connecting port "MTC_NR5GC:PTC_Ut" to port "NR5GC:UT"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2200
    text = Parameter: IMS_Component.vc_IMS_Global.Ctrl.TestBody = False

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'POWER_OFF'
    			ParameterList = Omit
    	CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF
    	Result = True
    	ResultString = ''

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC_Testsuite_v77_0.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 7195
    outStr = Timer: t_GuardTimer, Duration: 300s, Started: 13:20:00

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfoInit.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 280
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		DeltaValues
    			DeltaPrimary
    				DeltaBand = 257
    				Ssb_NRf1
    					R15 = 2054683
    				Ssb_NRf2
    					R15 = 2070811
    				Ssb_NRf3
    					R15 = 2086939
    				Ssb_NRf4
    					R15 = 2102779
    			DeltaSecondary
    				DeltaBand = 79
    				Ssb_NRf1
    					R15 = 694176
    				Ssb_NRf2
    					R15 = 704928
    				Ssb_NRf3
    					R15 = 717216
    				Ssb_NRf4
    					R15 = 727968

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		DeltaValues
    			DeltaPrimaryBand
    				DeltaNRf1 = -3
    				DeltaNRf2 = -3
    				DeltaNRf3 = -3
    				DeltaNRf4 = -3
    			DeltaSecondaryBand
    				DeltaNRf1 = 0
    				DeltaNRf2 = 0
    				DeltaNRf3 = 0
    				DeltaNRf4 = 0

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: PDSCH_Config___6
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___6
    		PDSCH_Config___6 = resourceAllocationType0 (0)

    summary = Message Mismatch: PDSCH_Config___14
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___14
    		PDSCH_Config___14 = qam256 (0)

    summary = Message Mismatch: PUSCH_Config___7
    MATCH_MISMATCH
    	Message Mismatch: PUSCH_Config___7
    		PUSCH_Config___7 = resourceAllocationType0 (0)

    BCCH-BCH-Message
    	message = mib =
    		systemFrameNumber = 000000
    		subCarrierSpacingCommon = scs30or120
    		ssb-SubcarrierOffset = 10
    		dmrs-TypeA-Position = pos2
    		pdcch-ConfigSIB1
    			controlResourceSetZero = 1
    			searchSpaceZero = 0
    		cellBarred = notBarred
    		intraFreqReselection = allowed
    		spare = 0

    BCCH-DL-SCH-Message
    	message = c1 = systemInformationBlockType1 =
    		cellSelectionInfo
    			q-RxLevMin = -57
    		cellAccessRelatedInfo
    			plmn-IdentityInfoList = SEQUENCE OF PLMN-IdentityInfo
    				PLMN-IdentityInfo(1)
    					plmn-IdentityList = SEQUENCE OF PLMN-Identity
    						PLMN-Identity(1)
    							mcc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 0
    								MCC-MNC-Digit(3) = 1
    							mnc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 1
    					trackingAreaCode = 000000000000000000000001
    					ranac = 1
    					cellIdentity = 000000000000000000000000010000000000
    					cellReservedForOperatorUse = notReserved
    		connEstFailureControl
    			connEstFailCount = n1
    			connEstFailOffsetValidity = s30
    			connEstFailOffset = 1
    		si-SchedulingInfo
    			schedulingInfoList = SEQUENCE OF SchedulingInfo
    				SchedulingInfo(1)
    					si-BroadcastStatus = broadcasting
    					si-Periodicity = rf32
    					sib-MappingInfo = SEQUENCE OF SIB-TypeInfo
    						SIB-TypeInfo(1)
    							type = sibType2
    							valueTag = 0
    			si-WindowLength = s160
    			systemInformationAreaID = 000000000000000000000001
    		servingCellConfigCommon
    			downlinkConfigCommon
    				frequencyInfoDL
    					frequencyBandList = SEQUENCE OF NR-MultiBandInfo
    						NR-MultiBandInfo(1)
    							freqBandIndicatorNR = 257
    							nr-NS-PmaxList = SEQUENCE OF NR-NS-PmaxValue
    								NR-NS-PmaxValue(1)
    									additionalSpectrumEmission = 0
    					offsetToPointA = 18
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz120
    							carrierBandwidth = 66
    				initialDownlinkBWP
    					genericParameters
    						locationAndBandwidth = 17875
    						subcarrierSpacing = kHz120
    					pdcch-ConfigCommon = setup =
    						controlResourceSetZero = 1
    						commonSearchSpaceList = SEQUENCE OF SearchSpace
    							SearchSpace(1)
    								searchSpaceId = 1
    								controlResourceSetId = 0
    								monitoringSlotPeriodicityAndOffset = sl1 = NULL
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n3
    									aggregationLevel4 = n2
    									aggregationLevel8 = n1
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    							SearchSpace(2)
    								searchSpaceId = 3
    								controlResourceSetId = 0
    								monitoringSlotPeriodicityAndOffset = sl10 = 5
    								duration = 2
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n3
    									aggregationLevel4 = n2
    									aggregationLevel8 = n1
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    						searchSpaceSIB1 = 0
    						searchSpaceOtherSystemInformation = 3
    						pagingSearchSpace = 0
    						ra-SearchSpace = 1
    					pdsch-ConfigCommon = setup =
    						pdsch-TimeDomainAllocationList = SEQUENCE OF PDSCH-TimeDomainResourceAllocation
    							PDSCH-TimeDomainResourceAllocation(1)
    								mappingType = typeA
    								startSymbolAndLength = 53
    				bcch-Config
    					modificationPeriodCoeff = n4
    				pcch-Config
    					defaultPagingCycle = rf128
    					nAndPagingFrameOffset = halfT = 0
    					ns = one
    			uplinkConfigCommon
    				frequencyInfoUL
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz120
    							carrierBandwidth = 66
    					p-Max = 23
    				initialUplinkBWP
    					genericParameters
    						locationAndBandwidth = 17875
    						subcarrierSpacing = kHz120
    					rach-ConfigCommon = setup =
    						rach-ConfigGeneric
    							prach-ConfigurationIndex = 149
    							msg1-FDM = one
    							msg1-FrequencyStart = 0
    							zeroCorrelationZoneConfig = 15
    							preambleReceivedTargetPower = -118
    							preambleTransMax = n7
    							powerRampingStep = dB4
    							ra-ResponseWindow = sl20
    						ssb-perRACH-OccasionAndCB-PreamblesPerSSB = one = n4
    						ra-ContentionResolutionTimer = sf64
    						rsrp-ThresholdSSB = 0
    						prach-RootSequenceIndex = l139 = 0
    						msg1-SubcarrierSpacing = kHz120
    						restrictedSetConfig = unrestrictedSet
    					pusch-ConfigCommon = setup =
    						pusch-TimeDomainAllocationList = SEQUENCE OF PUSCH-TimeDomainResourceAllocation
    							PUSCH-TimeDomainResourceAllocation(1)
    								k2 = 4
    								mappingType = typeA
    								startSymbolAndLength = 27
    							PUSCH-TimeDomainResourceAllocation(2)
    								k2 = 3
    								mappingType = typeA
    								startSymbolAndLength = 27
    						msg3-DeltaPreamble = 1
    						p0-NominalWithGrant = -90
    					pucch-ConfigCommon = setup =
    						pucch-ResourceCommon = 0
    						pucch-GroupHopping = enable
    						p0-nominal = -90
    				timeAlignmentTimerCommon = infinity
    			ssb-PositionsInBurst
    				inOneGroup = 01000000
    				groupPresence = 10000000
    			ssb-PeriodicityServingCell = ms20
    			tdd-UL-DL-ConfigurationCommon
    				referenceSubcarrierSpacing = kHz120
    				pattern1
    					dl-UL-TransmissionPeriodicity = ms0p625
    					nrofDownlinkSlots = 3
    					nrofDownlinkSymbols = 10
    					nrofUplinkSlots = 1
    					nrofUplinkSymbols = 2
    			ss-PBCH-BlockPower = 0
    		ims-EmergencySupport = true
    		ue-TimersAndConstants
    			t300 = ms1000
    			t301 = ms1000
    			t310 = ms1000
    			n310 = n1
    			t311 = ms30000
    			n311 = n1
    			t319 = ms1000

    BCCH-DL-SCH-Message
    	message = c1 = systemInformation =
    		criticalExtensions = systemInformation =
    			sib-TypeAndInfo = SEQUENCE OF CHOICE
    				CHOICE(1) = sib2 =
    					cellReselectionInfoCommon
    						nrofSS-BlocksToAverage = 2
    						absThreshSS-BlocksConsolidation
    							thresholdRSRP = 0
    						rangeToBestCell = dB0
    						q-Hyst = dB0
    					cellReselectionServingFreqInfo
    						threshServingLowP = 0
    						cellReselectionPriority = 4
    					intraFreqCellReselectionInfo
    						q-RxLevMin = -55
    						s-IntraSearchP = 31
    						t-ReselectionNR = 0
    						smtc
    							periodicityAndOffset = sf20 = 0
    							duration = sf3
    						ssb-ToMeasure = longBitmap = 1100000000000000000000000000000000000000000000000000000000000000
    						deriveSSB-IndexFromCell = TRUE

    DL-CCCH-Message
    	message = c1 = rrcSetup =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetup =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 1
    			masterCellGroup = CONTAINING =
    				cellGroupId = 0
    				rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    					RLC-BearerConfig(1)
    						logicalChannelIdentity = 1
    						servedRadioBearer = srb-Identity = 1
    						mac-LogicalChannelConfig
    							ul-SpecificParameters
    								priority = 1
    								prioritisedBitRate = infinity
    								bucketSizeDuration = ms50
    								logicalChannelGroup = 0
    								schedulingRequestID = 0
    								logicalChannelSR-Mask = FALSE
    								logicalChannelSR-DelayTimerApplied = FALSE
    				mac-CellGroupConfig
    					schedulingRequestConfig
    						schedulingRequestToAddModList = SEQUENCE OF SchedulingRequestToAddMod
    							SchedulingRequestToAddMod(1)
    								schedulingRequestId = 0
    								sr-TransMax = n16
    					bsr-Config
    						periodicBSR-Timer = sf1
    						retxBSR-Timer = sf80
    					tag-Config
    						tag-ToAddModList = SEQUENCE OF TAG
    							TAG(1)
    								tag-Id = 0
    								timeAlignmentTimer = infinity
    					phr-Config = setup =
    						phr-PeriodicTimer = sf10
    						phr-ProhibitTimer = sf0
    						phr-Tx-PowerFactorChange = dB1
    						multiplePHR = FALSE
    						dummy = FALSE
    						phr-Type2OtherCell = FALSE
    						phr-ModeOtherCG = real
    					skipUplinkTxDynamic = FALSE
    				physicalCellGroupConfig
    					p-NR-FR1 = 23
    					pdsch-HARQ-ACK-Codebook = dynamic
    				spCellConfig
    					rlf-TimersAndConstants = setup =
    						t310 = ms1000
    						n310 = n1
    						n311 = n1
    						t311 = ms1000
    					spCellConfigDedicated
    						initialDownlinkBWP
    							pdcch-Config = setup =
    								controlResourceSetToAddModList = SEQUENCE OF ControlResourceSet
    									ControlResourceSet(1)
    										controlResourceSetId = 1
    										frequencyDomainResources = 111100000000000000000000000000000000000000000
    										duration = 2
    										cce-REG-MappingType = nonInterleaved = NULL
    										precoderGranularity = sameAsREG-bundle
    								searchSpacesToAddModList = SEQUENCE OF SearchSpace
    									SearchSpace(1)
    										searchSpaceId = 2
    										controlResourceSetId = 1
    										monitoringSlotPeriodicityAndOffset = sl1 = NULL
    										monitoringSymbolsWithinSlot = 10000000000000
    										nrofCandidates
    											aggregationLevel1 = n0
    											aggregationLevel2 = n3
    											aggregationLevel4 = n2
    											aggregationLevel8 = n1
    											aggregationLevel16 = n0
    										searchSpaceType = ue-Specific =
    											dci-Formats = formats0-1-And-1-1
    							pdsch-Config = setup =
    								dataScramblingIdentityPDSCH = 0
    								dmrs-DownlinkForPDSCH-MappingTypeA = setup =
    									dmrs-AdditionalPosition = pos0
    									phaseTrackingRS = setup =
    										epre-Ratio = 0
    								tci-StatesToAddModList = SEQUENCE OF TCI-State
    									TCI-State(1)
    										tci-StateId = 0
    										qcl-Type1
    											referenceSignal = ssb = 1
    											qcl-Type = typeD
    								resourceAllocation = resourceAllocationType1
    								rbg-Size = config1
    								prb-BundlingType = staticBundling =
    									bundleSize = wideband
    							radioLinkMonitoringConfig = setup =
    								failureDetectionResourcesToAddModList = SEQUENCE OF RadioLinkMonitoringRS
    									RadioLinkMonitoringRS(1)
    										radioLinkMonitoringRS-Id = 0
    										purpose = rlf
    										detectionResource = ssb-Index = 1
    						firstActiveDownlinkBWP-Id = 0
    						defaultDownlinkBWP-Id = 0
    						uplinkConfig
    							initialUplinkBWP
    								pucch-Config = setup =
    									resourceSetToAddModList = SEQUENCE OF PUCCH-ResourceSet
    										PUCCH-ResourceSet(1)
    											pucch-ResourceSetId = 0
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 0
    												PUCCH-ResourceId(2) = 1
    												PUCCH-ResourceId(3) = 2
    												PUCCH-ResourceId(4) = 3
    												PUCCH-ResourceId(5) = 4
    												PUCCH-ResourceId(6) = 5
    												PUCCH-ResourceId(7) = 6
    												PUCCH-ResourceId(8) = 7
    										PUCCH-ResourceSet(2)
    											pucch-ResourceSetId = 1
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 8
    												PUCCH-ResourceId(2) = 9
    												PUCCH-ResourceId(3) = 10
    												PUCCH-ResourceId(4) = 11
    												PUCCH-ResourceId(5) = 12
    												PUCCH-ResourceId(6) = 13
    												PUCCH-ResourceId(7) = 14
    												PUCCH-ResourceId(8) = 15
    									resourceToAddModList = SEQUENCE OF PUCCH-Resource
    										PUCCH-Resource(1)
    											pucch-ResourceId = 0
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(2)
    											pucch-ResourceId = 1
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(3)
    											pucch-ResourceId = 2
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(4)
    											pucch-ResourceId = 3
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(5)
    											pucch-ResourceId = 4
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(6)
    											pucch-ResourceId = 5
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(7)
    											pucch-ResourceId = 6
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(8)
    											pucch-ResourceId = 7
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format1 =
    												initialCyclicShift = 0
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    												timeDomainOCC = 0
    										PUCCH-Resource(9)
    											pucch-ResourceId = 8
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(10)
    											pucch-ResourceId = 9
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(11)
    											pucch-ResourceId = 10
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(12)
    											pucch-ResourceId = 11
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(13)
    											pucch-ResourceId = 12
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(14)
    											pucch-ResourceId = 13
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(15)
    											pucch-ResourceId = 14
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(16)
    											pucch-ResourceId = 15
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format3 =
    												nrofPRBs = 1
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    									format1 = setup =
    										interslotFrequencyHopping = enabled
    									format2 = setup =
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									format3 = setup =
    										interslotFrequencyHopping = enabled
    										additionalDMRS = true
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									schedulingRequestResourceToAddModList = SEQUENCE OF SchedulingRequestResourceConfig
    										SchedulingRequestResourceConfig(1)
    											schedulingRequestResourceId = 1
    											schedulingRequestID = 0
    											periodicityAndOffset = sl80 = 9
    											resource = 6
    									dl-DataToUL-ACK = SEQUENCE OF INTEGER
    										INTEGER(1) = 2
    										INTEGER(2) = 3
    										INTEGER(3) = 4
    										INTEGER(4) = 5
    										INTEGER(5) = 6
    										INTEGER(6) = 7
    										INTEGER(7) = 8
    										INTEGER(8) = 9
    									pucch-PowerControl
    										deltaF-PUCCH-f0 = 0
    										deltaF-PUCCH-f1 = 0
    										deltaF-PUCCH-f2 = 0
    										deltaF-PUCCH-f3 = 0
    										deltaF-PUCCH-f4 = 0
    										pathlossReferenceRSs = SEQUENCE OF PUCCH-PathlossReferenceRS
    											PUCCH-PathlossReferenceRS(1)
    												pucch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 1
    								pusch-Config = setup =
    									txConfig = codebook
    									dmrs-UplinkForPUSCH-MappingTypeA = setup =
    										dmrs-AdditionalPosition = pos0
    										transformPrecodingDisabled
    									pusch-PowerControl
    										msg3-Alpha = alpha08
    										p0-NominalWithoutGrant = -90
    										p0-AlphaSets = SEQUENCE OF P0-PUSCH-AlphaSet
    											P0-PUSCH-AlphaSet(1)
    												p0-PUSCH-AlphaSetId = 0
    												p0 = 0
    												alpha = alpha08
    										pathlossReferenceRSToAddModList = SEQUENCE OF PUSCH-PathlossReferenceRS
    											PUSCH-PathlossReferenceRS(1)
    												pusch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 1
    										sri-PUSCH-MappingToAddModList = SEQUENCE OF SRI-PUSCH-PowerControl
    											SRI-PUSCH-PowerControl(1)
    												sri-PUSCH-PowerControlId = 0
    												sri-PUSCH-PathlossReferenceRS-Id = 0
    												sri-P0-PUSCH-AlphaSetId = 0
    												sri-PUSCH-ClosedLoopIndex = i0
    									resourceAllocation = resourceAllocationType1
    									codebookSubset = nonCoherent
    									maxRank = 1
    									uci-OnPUSCH = setup =
    										betaOffsets = semiStatic =
    											betaOffsetACK-Index1 = 9
    											betaOffsetACK-Index2 = 9
    											betaOffsetACK-Index3 = 9
    											betaOffsetCSI-Part1-Index1 = 6
    											betaOffsetCSI-Part1-Index2 = 6
    											betaOffsetCSI-Part2-Index1 = 6
    											betaOffsetCSI-Part2-Index2 = 6
    										scaling = f1
    								srs-Config = setup =
    									srs-ResourceSetToAddModList = SEQUENCE OF SRS-ResourceSet
    										SRS-ResourceSet(1)
    											srs-ResourceSetId = 0
    											srs-ResourceIdList = SEQUENCE OF SRS-ResourceId
    												SRS-ResourceId(1) = 0
    											resourceType = aperiodic =
    												aperiodicSRS-ResourceTrigger = 1
    												slotOffset = 4
    											usage = codebook
    											alpha = alpha0
    											p0 = 0
    											pathlossReferenceRS = ssb-Index = 1
    									srs-ResourceToAddModList = SEQUENCE OF SRS-Resource
    										SRS-Resource(1)
    											srs-ResourceId = 0
    											nrofSRS-Ports = port1
    											transmissionComb = n2 =
    												combOffset-n2 = 0
    												cyclicShift-n2 = 0
    											resourceMapping
    												startPosition = 0
    												nrofSymbols = n1
    												repetitionFactor = n1
    											freqDomainPosition = 0
    											freqDomainShift = 0
    											freqHopping
    												c-SRS = 17
    												b-SRS = 0
    												b-hop = 0
    											groupOrSequenceHopping = groupHopping
    											resourceType = aperiodic =
    											sequenceId = 0
    											spatialRelationInfo
    												referenceSignal = ssb-Index = 1
    							firstActiveUplinkBWP-Id = 0
    							pusch-ServingCellConfig = setup =
    						pdcch-ServingCellConfig = setup =
    						pdsch-ServingCellConfig = setup =
    						tag-Id = 0

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig
    					CA_Capability = None (3)
    				CellConfigCommon
    					C_RNTI = 4097
    					CellTimingInfo
    						TcOffset = 0
    						Tcell = 0
    						SfnOffset = 0
    						HsfnOffset = 0
    					InitialCellPower
    						MaxReferencePower = -82
    						Attenuation
    							Off = True
    				PhysicalLayer
    					Common
    						PhysicalCellId = 42
    						DuplexMode
    							TDD
    								Config
    									Common
    										R15
    											referenceSubcarrierSpacing = kHz120 (3)
    											pattern1
    												dl_UL_TransmissionPeriodicity = ms0p625 (1)
    												nrofDownlinkSlots = 3
    												nrofDownlinkSymbols = 10
    												nrofUplinkSlots = 1
    												nrofUplinkSymbols = 2
    												dl_UL_TransmissionPeriodicity_v1530 = Omit
    											pattern2 = Omit
    									Dedicated = Omit
    					Downlink
    						FrequencyInfoDL
    							R15
    								absoluteFrequencySSB = 2054683
    								frequencyBandList
    									FreqBandIndicatorNR = 257
    								absoluteFrequencyPointA = 2054207
    								scs_SpecificCarrierList
    									SCS_SpecificCarrier
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz120 (3)
    										carrierBandwidth = 66
    										txDirectCurrentLocation = Omit
    						SSPbchBlock
    							SubCarrierSpacing = kHz120 (3)
    							SubcarrierOffset = 10
    							Periodicity = ms20 (2)
    							HalfFrameOffset = 0
    							BurstConfig
    								BlockPattern = caseD (3)
    								PositionsInBurst
    									longBitmap = 0100000000000000000000000000000000000000000000000000000000000000'B
    								BeamArray = Omit
    							RelativeTxPower
    								PbchToDmrs = 0
    								PssToSss = 0
    								SssToSsbBeam = 0
    								DmrsToSss = 0
    						PdschCellLevelConfig
    							DMRS_TypeA_Position = pos2 (0)
    							RateMatchPattern
    								PatternList = Omit
    								PatternListLteCrs = Omit
    							ServingCellConfig
    								R15
    									codeBlockGroupTransmission = Omit
    									xOverhead = Omit
    									nrofHARQ_ProcessesForPDSCH = Omit
    									pucch_Cell = Omit
    									maxMIMO_Layers = Omit
    									processingType2Enabled = Omit
    									pdsch_CodeBlockGroupTransmissionList_r16 = Omit
    									downlinkHARQ_FeedbackDisabled_r17 = Omit
    									nrofHARQ_ProcessesForPDSCH_v1700 = Omit
    						BWPs
    							ActiveBWP = 0
    							BwpArray
    								NR_DownlinkBWP_Type
    									Id = 0
    									BWP
    										R15
    											locationAndBandwidth = 17875
    											subcarrierSpacing = kHz120 (3)
    											cyclicPrefix = Omit
    									Pdcch
    										SearchSpaceArray
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType0 (0)
    														CandidatePriority = 0
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType2 (3)
    														CandidatePriority = 3
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 0
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl160 = 1
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n0 (0)
    															aggregationLevel4 = n4 (4)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n1 (1)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType1 (2)
    														CandidatePriority = 2
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType3 (5)
    														CandidatePriority = 4
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 1
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = ussDL (6)
    														CandidatePriority = 5
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = ussUL (7)
    														CandidatePriority = 9
    												AggregationLevel = AggregationLevel2 (1)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 2
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															ue_Specific
    																dci_Formats = formats0_1_And_1_1 (1)
    																dci_Formats_MT_r16 = Omit
    																dci_FormatsSL_r16 = Omit
    																dci_FormatsExt_r16 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType0A (1)
    														CandidatePriority = 1
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 3
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl10 = 5
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    										CoresetArray
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 0
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														interleaved
    															reg_BundleSize = n6 (2)
    															interleaverSize = n2 (0)
    															shiftIndex = 42
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    													rb_Offset_r16 = Omit
    													tci_PresentDCI_1_2_r16 = Omit
    													coresetPoolIndex_r16 = Omit
    													controlResourceSetId_v1610 = Omit
    													followUnifiedTCI_State_r17 = Omit
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 1
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														nonInterleaved = Null
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    													rb_Offset_r16 = Omit
    													tci_PresentDCI_1_2_r16 = Omit
    													coresetPoolIndex_r16 = Omit
    													controlResourceSetId_v1610 = Omit
    													followUnifiedTCI_State_r17 = Omit
    										RelativeTxPower
    											PdcchToCell = 0
    											PdcchToDmrs = 0
    										Coreset0_OffsetRBs = 4
    									Pdsch
    										ConfigCommon
    											R15
    												pdsch_TimeDomainAllocationList
    													PDSCH_TimeDomainResourceAllocation
    														k0 = Omit
    														mappingType = typeA (0)
    														startSymbolAndLength = 53
    										ConfigDedicated
    											R15
    												dataScramblingIdentityPDSCH = 0
    												dmrs_DownlinkForPDSCH_MappingTypeA
    													setup
    														dmrs_Type = Omit
    														dmrs_AdditionalPosition = pos0 (0)
    														maxLength = Omit
    														scramblingID0 = Omit
    														scramblingID1 = Omit
    														phaseTrackingRS
    															setup
    																frequencyDensity = Omit
    																timeDensity = Omit
    																epre_Ratio = 0
    																resourceElementOffset = Omit
    																maxNrofPorts_r16 = Omit
    														dmrs_Downlink_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB = Omit
    												tci_StatesToAddModList
    													TCI_State
    														tci_StateId = 0
    														qcl_Type1
    															cell = Omit
    															bwp_Id = Omit
    															referenceSignal
    																ssb = 1
    															qcl_Type = typeD (3)
    														qcl_Type2 = Omit
    														additionalPCI_r17 = Omit
    														pathlossReferenceRS_Id_r17 = Omit
    														ul_powerControl_r17 = Omit
    												tci_StatesToReleaseList = Omit
    												vrb_ToPRB_Interleaver = Omit
    												resourceAllocation = resourceAllocationType1 (1)
    												pdsch_TimeDomainAllocationList = Omit
    												pdsch_AggregationFactor = Omit
    												rateMatchPatternToAddModList = Omit
    												rateMatchPatternToReleaseList = Omit
    												rateMatchPatternGroup1 = Omit
    												rateMatchPatternGroup2 = Omit
    												rbg_Size = config1 (0)
    												mcs_Table = Omit
    												maxNrofCodeWordsScheduledByDCI = Omit
    												prb_BundlingType
    													staticBundling
    														bundleSize = wideband (1)
    												zp_CSI_RS_ResourceToAddModList = Omit
    												zp_CSI_RS_ResourceToReleaseList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												p_ZP_CSI_RS_ResourceSet = Omit
    												maxMIMO_Layers_r16 = Omit
    												minimumSchedulingOffsetK0_r16 = Omit
    												antennaPortsFieldPresenceDCI_1_2_r16 = Omit
    												aperiodicZP_CSI_RS_ResourceSetsToAddModListDCI_1_2_r16 = Omit
    												aperiodicZP_CSI_RS_ResourceSetsToReleaseListDCI_1_2_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeA_DCI_1_2_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB_DCI_1_2_r16 = Omit
    												dmrs_SequenceInitializationDCI_1_2_r16 = Omit
    												harq_ProcessNumberSizeDCI_1_2_r16 = Omit
    												mcs_TableDCI_1_2_r16 = Omit
    												numberOfBitsForRV_DCI_1_2_r16 = Omit
    												pdsch_TimeDomainAllocationListDCI_1_2_r16 = Omit
    												prb_BundlingTypeDCI_1_2_r16 = Omit
    												priorityIndicatorDCI_1_2_r16 = Omit
    												rateMatchPatternGroup1DCI_1_2_r16 = Omit
    												rateMatchPatternGroup2DCI_1_2_r16 = Omit
    												resourceAllocationType1GranularityDCI_1_2_r16 = Omit
    												vrb_ToPRB_InterleaverDCI_1_2_r16 = Omit
    												referenceOfSLIVDCI_1_2_r16 = Omit
    												resourceAllocationDCI_1_2_r16 = Omit
    												priorityIndicatorDCI_1_1_r16 = Omit
    												dataScramblingIdentityPDSCH2_r16 = Omit
    												pdsch_TimeDomainAllocationList_r16 = Omit
    												repetitionSchemeConfig_r16 = Omit
    												repetitionSchemeConfig_v1630 = Omit
    												pdsch_HARQ_ACK_OneShotFeedbackDCI_1_2_r17 = Omit
    												pdsch_HARQ_ACK_EnhType3DCI_1_2_r17 = Omit
    												pdsch_HARQ_ACK_EnhType3DCI_Field_1_2_r17 = Omit
    												pdsch_HARQ_ACK_RetxDCI_1_2_r17 = Omit
    												pucch_sSCellDynDCI_1_2_r17 = Omit
    												dl_OrJointTCI_StateList_r17 = Omit
    												beamAppTime_r17 = Omit
    												dummy = Omit
    												dmrs_FD_OCC_DisabledForRank1_PDSCH_r17 = Omit
    												minimumSchedulingOffsetK0_r17 = Omit
    												harq_ProcessNumberSizeDCI_1_2_v1700 = Omit
    												harq_ProcessNumberSizeDCI_1_1_r17 = Omit
    												mcs_Table_r17 = Omit
    												mcs_TableDCI_1_2_r17 = Omit
    												xOverheadMulticast_r17 = Omit
    												priorityIndicatorDCI_4_2_r17 = Omit
    												sizeDCI_4_2_r17 = Omit
    												pdsch_TimeDomainAllocationListForMultiPDSCH_r17 = Omit
    										RelativeTxPower
    											PdschToCell = -3
    											PdschToDmrs = -3
    											PdschToPtrs = -3
    									Sps = Omit
    									SL_Pdcch = Omit
    									NCD_SSPbchBlock = Omit
    							InitialBWP_RedCap = Omit
    						CsiConfig
    							None = True
    					Uplink
    						Uplink
    							Config
    								FrequencyInfoUL
    									R15
    										frequencyBandList = Omit
    										absoluteFrequencyPointA = Omit
    										scs_SpecificCarrierList
    											SCS_SpecificCarrier
    												offsetToCarrier = 0
    												subcarrierSpacing = kHz120 (3)
    												carrierBandwidth = 66
    												txDirectCurrentLocation = Omit
    										additionalSpectrumEmission = 0
    										p_Max = 23
    										frequencyShift7p5khz = Omit
    								BWPs
    									ActiveBWP
    										SameIdAsDL = True
    									BwpArray
    										NR_UplinkBWP_Type
    											Id = 0
    											Common
    												R15
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 149
    																msg1_FDM = one (0)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    																prach_ConfigurationPeriodScaling_IAB_r16 = Omit
    																prach_ConfigurationFrameOffset_IAB_r16 = Omit
    																prach_ConfigurationSOffset_IAB_r16 = Omit
    																ra_ResponseWindow_v1610 = Omit
    																prach_ConfigurationIndex_v1610 = Omit
    																ra_ResponseWindow_v1700 = Omit
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n4 (0)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 0
    															msg1_SubcarrierSpacing = kHz120 (3)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    															ra_PrioritizationForAccessIdentity_r16 = Omit
    															prach_RootSequenceIndex_r16 = Omit
    															ra_PrioritizationForSlicing_r17 = Omit
    															featureCombinationPreamblesList_r17 = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 3
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    															nrofPRBs = Omit
    															intra_SlotFH_r17 = Omit
    															pucch_ResourceCommonRedCap_r17 = Omit
    															additionalPRBOffset_r17 = Omit
    													rach_ConfigCommonIAB_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													msgA_ConfigCommon_r16 = Omit
    													enableRA_PrioritizationForSlicing_r17 = Omit
    													additionalRACH_ConfigList_r17 = Omit
    													rsrp_ThresholdMsg3_r17 = Omit
    													numberOfMsg3_RepetitionsList_r17 = Omit
    													mcs_Msg3_Repetitions_r17 = Omit
    											Dedicated
    												R15
    													pucch_Config
    														setup
    															resourceSetToAddModList
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 0
    																	resourceList
    																		IntegerType = 0
    																		IntegerType = 1
    																		IntegerType = 2
    																		IntegerType = 3
    																		IntegerType = 4
    																		IntegerType = 5
    																		IntegerType = 6
    																		IntegerType = 7
    																	maxPayloadSize = Omit
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 1
    																	resourceList
    																		IntegerType = 8
    																		IntegerType = 9
    																		IntegerType = 10
    																		IntegerType = 11
    																		IntegerType = 12
    																		IntegerType = 13
    																		IntegerType = 14
    																		IntegerType = 15
    																	maxPayloadSize = Omit
    															resourceSetToReleaseList = Omit
    															resourceToAddModList
    																PUCCH_Resource
    																	pucch_ResourceId = 0
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 1
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 2
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 3
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 4
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 5
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 6
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 7
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format1
    																			initialCyclicShift = 0
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    																			timeDomainOCC = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 8
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 9
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 10
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 11
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 12
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 13
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 14
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 15
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format3
    																			nrofPRBs = 1
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    															resourceToReleaseList = Omit
    															format1
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = Omit
    																	maxCodeRate = Omit
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = Omit
    															format2
    																setup
    																	interslotFrequencyHopping = Omit
    																	additionalDMRS = Omit
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format3
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format4 = Omit
    															schedulingRequestResourceToAddModList
    																SchedulingRequestResourceConfig
    																	schedulingRequestResourceId = 1
    																	schedulingRequestID = 0
    																	periodicityAndOffset
    																		sl80 = 9
    																	resource = 6
    															schedulingRequestResourceToReleaseList = Omit
    															multi_CSI_PUCCH_ResourceList = Omit
    															dl_DataToUL_ACK
    																PUCCH_Config___11___oftype = 2
    																PUCCH_Config___11___oftype = 3
    																PUCCH_Config___11___oftype = 4
    																PUCCH_Config___11___oftype = 5
    																PUCCH_Config___11___oftype = 6
    																PUCCH_Config___11___oftype = 7
    																PUCCH_Config___11___oftype = 8
    																PUCCH_Config___11___oftype = 9
    															spatialRelationInfoToAddModList = Omit
    															spatialRelationInfoToReleaseList = Omit
    															pucch_PowerControl
    																deltaF_PUCCH_f0 = 0
    																deltaF_PUCCH_f1 = 0
    																deltaF_PUCCH_f2 = 0
    																deltaF_PUCCH_f3 = 0
    																deltaF_PUCCH_f4 = 0
    																p0_Set = Omit
    																pathlossReferenceRSs
    																	PUCCH_PathlossReferenceRS
    																		pucch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																twoPUCCH_PC_AdjustmentStates = Omit
    																pathlossReferenceRSs_v1610 = Omit
    															resourceToAddModListExt_v1610 = Omit
    															dl_DataToUL_ACK_r16 = Omit
    															ul_AccessConfigListDCI_1_1_r16 = Omit
    															subslotLengthForPUCCH_r16 = Omit
    															dl_DataToUL_ACK_DCI_1_2_r16 = Omit
    															numberOfBitsForPUCCH_ResourceIndicatorDCI_1_2_r16 = Omit
    															dmrs_UplinkTransformPrecodingPUCCH_r16 = Omit
    															spatialRelationInfoToAddModListSizeExt_v1610 = Omit
    															spatialRelationInfoToReleaseListSizeExt_v1610 = Omit
    															spatialRelationInfoToAddModListExt_v1610 = Omit
    															spatialRelationInfoToReleaseListExt_v1610 = Omit
    															resourceGroupToAddModList_r16 = Omit
    															resourceGroupToReleaseList_r16 = Omit
    															sps_PUCCH_AN_List_r16 = Omit
    															schedulingRequestResourceToAddModListExt_v1610 = Omit
    															format0_r17 = Omit
    															format2Ext_r17 = Omit
    															format3Ext_r17 = Omit
    															format4Ext_r17 = Omit
    															ul_AccessConfigListDCI_1_2_r17 = Omit
    															mappingPattern_r17 = Omit
    															powerControlSetInfoToAddModList_r17 = Omit
    															powerControlSetInfoToReleaseList_r17 = Omit
    															secondTPCFieldDCI_1_1_r17 = Omit
    															secondTPCFieldDCI_1_2_r17 = Omit
    															dl_DataToUL_ACK_r17 = Omit
    															dl_DataToUL_ACK_DCI_1_2_r17 = Omit
    															ul_AccessConfigListDCI_1_1_r17 = Omit
    															schedulingRequestResourceToAddModListExt_v1700 = Omit
    															dmrs_BundlingPUCCH_Config_r17 = Omit
    															dl_DataToUL_ACK_v1700 = Omit
    															dl_DataToUL_ACK_MulticastDCI_Format4_1_r17 = Omit
    															sps_PUCCH_AN_ListMulticast_r17 = Omit
    													pusch_Config
    														setup
    															dataScramblingIdentityPUSCH = Omit
    															txConfig = codebook (0)
    															dmrs_UplinkForPUSCH_MappingTypeA
    																setup
    																	dmrs_Type = Omit
    																	dmrs_AdditionalPosition = pos0 (0)
    																	phaseTrackingRS = Omit
    																	maxLength = Omit
    																	transformPrecodingDisabled
    																		scramblingID0 = Omit
    																		scramblingID1 = Omit
    																		dmrs_Uplink_r16 = Omit
    																	transformPrecodingEnabled = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB = Omit
    															pusch_PowerControl
    																tpc_Accumulation = Omit
    																msg3_Alpha = alpha08 (5)
    																p0_NominalWithoutGrant = -90
    																p0_AlphaSets
    																	P0_PUSCH_AlphaSet
    																		p0_PUSCH_AlphaSetId = 0
    																		p0 = 0
    																		alpha = alpha08 (5)
    																pathlossReferenceRSToAddModList
    																	PUSCH_PathlossReferenceRS
    																		pusch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																pathlossReferenceRSToReleaseList = Omit
    																twoPUSCH_PC_AdjustmentStates = Omit
    																deltaMCS = Omit
    																sri_PUSCH_MappingToAddModList
    																	SRI_PUSCH_PowerControl
    																		sri_PUSCH_PowerControlId = 0
    																		sri_PUSCH_PathlossReferenceRS_Id = 0
    																		sri_P0_PUSCH_AlphaSetId = 0
    																		sri_PUSCH_ClosedLoopIndex = i0 (0)
    																sri_PUSCH_MappingToReleaseList = Omit
    															frequencyHopping = Omit
    															frequencyHoppingOffsetLists = Omit
    															resourceAllocation = resourceAllocationType1 (1)
    															pusch_TimeDomainAllocationList = Omit
    															pusch_AggregationFactor = Omit
    															mcs_Table = Omit
    															mcs_TableTransformPrecoder = Omit
    															transformPrecoder = Omit
    															codebookSubset = nonCoherent (2)
    															maxRank = 1
    															rbg_Size = Omit
    															uci_OnPUSCH
    																setup
    																	betaOffsets
    																		semiStatic
    																			betaOffsetACK_Index1 = 9
    																			betaOffsetACK_Index2 = 9
    																			betaOffsetACK_Index3 = 9
    																			betaOffsetCSI_Part1_Index1 = 6
    																			betaOffsetCSI_Part1_Index2 = 6
    																			betaOffsetCSI_Part2_Index1 = 6
    																			betaOffsetCSI_Part2_Index2 = 6
    																	scaling = f1 (3)
    															tp_pi2BPSK = Omit
    															minimumSchedulingOffsetK2_r16 = Omit
    															ul_AccessConfigListDCI_0_1_r16 = Omit
    															harq_ProcessNumberSizeDCI_0_2_r16 = Omit
    															dmrs_SequenceInitializationDCI_0_2_r16 = Omit
    															numberOfBitsForRV_DCI_0_2_r16 = Omit
    															antennaPortsFieldPresenceDCI_0_2_r16 = Omit
    															dmrs_UplinkForPUSCH_MappingTypeA_DCI_0_2_r16 = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB_DCI_0_2_r16 = Omit
    															frequencyHoppingDCI_0_2_r16 = Omit
    															frequencyHoppingOffsetListsDCI_0_2_r16 = Omit
    															codebookSubsetDCI_0_2_r16 = Omit
    															invalidSymbolPatternIndicatorDCI_0_2_r16 = Omit
    															maxRankDCI_0_2_r16 = Omit
    															mcs_TableDCI_0_2_r16 = Omit
    															mcs_TableTransformPrecoderDCI_0_2_r16 = Omit
    															priorityIndicatorDCI_0_2_r16 = Omit
    															pusch_RepTypeIndicatorDCI_0_2_r16 = Omit
    															resourceAllocationDCI_0_2_r16 = Omit
    															resourceAllocationType1GranularityDCI_0_2_r16 = Omit
    															uci_OnPUSCH_ListDCI_0_2_r16 = Omit
    															pusch_TimeDomainAllocationListDCI_0_2_r16 = Omit
    															pusch_TimeDomainAllocationListDCI_0_1_r16 = Omit
    															invalidSymbolPatternIndicatorDCI_0_1_r16 = Omit
    															priorityIndicatorDCI_0_1_r16 = Omit
    															pusch_RepTypeIndicatorDCI_0_1_r16 = Omit
    															frequencyHoppingDCI_0_1_r16 = Omit
    															uci_OnPUSCH_ListDCI_0_1_r16 = Omit
    															invalidSymbolPattern_r16 = Omit
    															pusch_PowerControl_v1610 = Omit
    															ul_FullPowerTransmission_r16 = Omit
    															pusch_TimeDomainAllocationListForMultiPUSCH_r16 = Omit
    															numberOfInvalidSymbolsForDL_UL_Switching_r16 = Omit
    															ul_AccessConfigListDCI_0_2_r17 = Omit
    															betaOffsetsCrossPri0_r17 = Omit
    															betaOffsetsCrossPri1_r17 = Omit
    															betaOffsetsCrossPri0DCI_0_2_r17 = Omit
    															betaOffsetsCrossPri1DCI_0_2_r17 = Omit
    															mappingPattern_r17 = Omit
    															secondTPCFieldDCI_0_1_r17 = Omit
    															secondTPCFieldDCI_0_2_r17 = Omit
    															sequenceOffsetForRV_r17 = Omit
    															ul_AccessConfigListDCI_0_1_r17 = Omit
    															minimumSchedulingOffsetK2_r17 = Omit
    															availableSlotCounting_r17 = Omit
    															dmrs_BundlingPUSCH_Config_r17 = Omit
    															harq_ProcessNumberSizeDCI_0_2_v1700 = Omit
    															harq_ProcessNumberSizeDCI_0_1_r17 = Omit
    															mpe_ResourcePoolToAddModList_r17 = Omit
    															mpe_ResourcePoolToReleaseList_r17 = Omit
    													configuredGrantConfig = Omit
    													srs_Config
    														setup
    															srs_ResourceSetToReleaseList = Omit
    															srs_ResourceSetToAddModList
    																SRS_ResourceSet
    																	srs_ResourceSetId = 0
    																	srs_ResourceIdList
    																		IntegerType = 0
    																	resourceType
    																		aperiodic
    																			aperiodicSRS_ResourceTrigger = 1
    																			csi_RS = Omit
    																			slotOffset = 4
    																			aperiodicSRS_ResourceTriggerList = Omit
    																	usage = codebook (1)
    																	alpha = alpha0 (0)
    																	p0 = 0
    																	pathlossReferenceRS
    																		ssb_Index = 1
    																	srs_PowerControlAdjustmentStates = Omit
    																	pathlossReferenceRSList_r16 = Omit
    																	usagePDC_r17 = Omit
    																	availableSlotOffsetList_r17 = Omit
    																	followUnifiedTCI_StateSRS_r17 = Omit
    															srs_ResourceToReleaseList = Omit
    															srs_ResourceToAddModList
    																SRS_Resource
    																	srs_ResourceId = 0
    																	nrofSRS_Ports = port1 (0)
    																	ptrs_PortIndex = Omit
    																	transmissionComb
    																		n2
    																			combOffset_n2 = 0
    																			cyclicShift_n2 = 0
    																	resourceMapping
    																		startPosition = 0
    																		nrofSymbols = n1 (0)
    																		repetitionFactor = n1 (0)
    																	freqDomainPosition = 0
    																	freqDomainShift = 0
    																	freqHopping
    																		c_SRS = 17
    																		b_SRS = 0
    																		b_hop = 0
    																	groupOrSequenceHopping = groupHopping (1)
    																	resourceType
    																		aperiodic
    																	sequenceId = 0
    																	spatialRelationInfo
    																		servingCellId = Omit
    																		referenceSignal
    																			ssb_Index = 1
    																	resourceMapping_r16 = Omit
    																	spatialRelationInfo_PDC_r17 = Omit
    																	resourceMapping_r17 = Omit
    																	partialFreqSounding_r17 = Omit
    																	transmissionComb_n8_r17 = Omit
    																	srs_TCI_State_r17 = Omit
    																	repetitionFactor_v1730 = Omit
    																	srs_DLorJointTCI_State_v1730 = Omit
    															tpc_Accumulation = Omit
    															srs_RequestDCI_1_2_r16 = Omit
    															srs_RequestDCI_0_2_r16 = Omit
    															srs_ResourceSetToAddModListDCI_0_2_r16 = Omit
    															srs_ResourceSetToReleaseListDCI_0_2_r16 = Omit
    															srs_PosResourceSetToReleaseList_r16 = Omit
    															srs_PosResourceSetToAddModList_r16 = Omit
    															srs_PosResourceToReleaseList_r16 = Omit
    															srs_PosResourceToAddModList_r16 = Omit
    													beamFailureRecoveryConfig = Omit
    													sl_PUCCH_Config_r16 = Omit
    													cp_ExtensionC2_r16 = Omit
    													cp_ExtensionC3_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													pucch_ConfigurationList_r16 = Omit
    													lbt_FailureRecoveryConfig_r16 = Omit
    													configuredGrantConfigToAddModList_r16 = Omit
    													configuredGrantConfigToReleaseList_r16 = Omit
    													configuredGrantConfigType2DeactivationStateList_r16 = Omit
    													ul_TCI_StateList_r17 = Omit
    													ul_powerControl_r17 = Omit
    													pucch_ConfigurationListMulticast1_r17 = Omit
    													pucch_ConfigurationListMulticast2_r17 = Omit
    													pucch_ConfigMulticast1_r17 = Omit
    													pucch_ConfigMulticast2_r17 = Omit
    													pathlossReferenceRSToAddModList_r17 = Omit
    													pathlossReferenceRSToReleaseList_r17 = Omit
    									InitialBWP_RedCap = Omit
    								RACH_ConfigDedicated = Omit
    								SI_RequestConfig = Omit
    						SupplementaryUplink = Omit
    						TimingAdvance
    							InitialValue = 0
    						PUSCH_ServingCellConfig
    							R15
    								codeBlockGroupTransmission = Omit
    								rateMatching = Omit
    								xOverhead = Omit
    								maxMIMO_Layers = Omit
    								processingType2Enabled = Omit
    								maxMIMO_LayersDCI_0_2_r16 = Omit
    								nrofHARQ_ProcessesForPUSCH_r17 = Omit
    								uplinkHARQ_mode_r17 = Omit
    						PUSCH_ServingCellConfigSUL = Omit
    				BcchConfig
    					Pbch = True
    					Pdsch
    						Sib1Schedul
    							SearchSpaceAndDci
    								AssignedBWPs
    									ActiveBWP = Omit
    									InitialBWP = True
    									DedicatedBWPs
    									InitialBWP_RedCap = Omit
    								SearchSpaceType = cssType0 (0)
    								DciInfo
    									ResoureAssignment
    										ResourceAllocationType = resourceAllocationType1 (1)
    										FreqDomain
    											Automatic
    												FirstRbIndex = 0
    												MaxRbCnt = 7
    										TimeDomain
    											Index = 0000'B
    										TransportBlockScheduling
    											Automatic
    												TransportBlock1 = qpsk (0)
    												TransportBlock2 = Omit
    												RedundancyVersionList
    													NR_RedundancyVersion_Type = 0
    										HarqProcessConfig
    											Broadcast = True
    									VrbPrbMapping
    										Index = 0'B
    									Format
    										Format_1_0_SI_RNTI
    											SystemInfoIndicator = 0'B
    							Periodicity = 20
    							SlotOffsetList
    								IntegerType = 2
    						SiSchedul
    							WindowLength = s160 (5)
    							SiList
    								NR_OtherSiSchedul_Type
    									Periodicity = rf32 (2)
    									Window
    										NR_SingleSiSchedul_Type
    											SearchSpaceAndDci
    												AssignedBWPs
    													ActiveBWP = Omit
    													InitialBWP = True
    													DedicatedBWPs
    													InitialBWP_RedCap = Omit
    												SearchSpaceType = cssType0A (1)
    												DciInfo
    													ResoureAssignment
    														ResourceAllocationType = resourceAllocationType1 (1)
    														FreqDomain
    															Automatic
    																FirstRbIndex = 0
    																MaxRbCnt = 7
    														TimeDomain
    															Index = 0000'B
    														TransportBlockScheduling
    															Automatic
    																TransportBlock1 = qpsk (0)
    																TransportBlock2 = Omit
    																RedundancyVersionList
    																	NR_RedundancyVersion_Type = 0
    														HarqProcessConfig
    															Broadcast = True
    													VrbPrbMapping
    														Index = 0'B
    													Format
    														Format_1_0_SI_RNTI
    															SystemInfoIndicator = 1'B
    											SlotOffset = 6
    							SegmentedSiList = Omit
    							PosSiSchedulInfo = Omit
    					BcchInfo
    						MIB
    							message_
    								mib
    									systemFrameNumber = 000000'B
    									subCarrierSpacingCommon = scs30or120 (1)
    									ssb_SubcarrierOffset = 10
    									dmrs_TypeA_Position = pos2 (0)
    									pdcch_ConfigSIB1
    										controlResourceSetZero = 1
    										searchSpaceZero = 0
    									cellBarred = notBarred (1)
    									intraFreqReselection = allowed (0)
    									spare = 0'B
    						SIB1
    							message_
    								c1
    									systemInformationBlockType1
    										cellSelectionInfo
    											q_RxLevMin = -57
    											q_RxLevMinOffset = Omit
    											q_RxLevMinSUL = Omit
    											q_QualMin = Omit
    											q_QualMinOffset = Omit
    										cellAccessRelatedInfo
    											plmn_IdentityInfoList
    												PLMN_IdentityInfo
    													plmn_IdentityList
    														PLMN_Identity
    															mcc
    																IntegerType = 0
    																IntegerType = 0
    																IntegerType = 1
    															mnc
    																IntegerType = 0
    																IntegerType = 1
    													trackingAreaCode = 000000000000000000000001'B
    													ranac = 1
    													cellIdentity = 000000000000000000000000010000000000'B
    													cellReservedForOperatorUse = notReserved (1)
    													iab_Support_r16 = Omit
    													trackingAreaList_r17 = Omit
    													gNB_ID_Length_r17 = Omit
    											cellReservedForOtherUse = Omit
    											cellReservedForFutureUse_r16 = Omit
    											npn_IdentityInfoList_r16 = Omit
    											snpn_AccessInfoList_r17 = Omit
    										connEstFailureControl
    											connEstFailCount = n1 (0)
    											connEstFailOffsetValidity = s30 (0)
    											connEstFailOffset = 1
    										si_SchedulingInfo
    											schedulingInfoList
    												SchedulingInfo
    													si_BroadcastStatus = broadcasting (0)
    													si_Periodicity = rf32 (2)
    													sib_MappingInfo
    														SIB_TypeInfo
    															type_ = sibType2 (0)
    															valueTag = 0
    															areaScope = Omit
    											si_WindowLength = s160 (5)
    											si_RequestConfig = Omit
    											si_RequestConfigSUL = Omit
    											systemInformationAreaID = 000000000000000000000001'B
    										servingCellConfigCommon
    											downlinkConfigCommon
    												frequencyInfoDL
    													frequencyBandList
    														NR_MultiBandInfo
    															freqBandIndicatorNR = 257
    															nr_NS_PmaxList
    																NR_NS_PmaxValue
    																	additionalPmax = Omit
    																	additionalSpectrumEmission = 0
    													offsetToPointA = 18
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz120 (3)
    															carrierBandwidth = 66
    															txDirectCurrentLocation = Omit
    												initialDownlinkBWP
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													pdcch_ConfigCommon
    														setup
    															controlResourceSetZero = 1
    															commonControlResourceSet = Omit
    															searchSpaceZero = Omit
    															commonSearchSpaceList
    																SearchSpace
    																	searchSpaceId = 1
    																	controlResourceSetId = 0
    																	monitoringSlotPeriodicityAndOffset
    																		sl1 = Null
    																	duration = Omit
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n3 (3)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n1 (1)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    																SearchSpace
    																	searchSpaceId = 3
    																	controlResourceSetId = 0
    																	monitoringSlotPeriodicityAndOffset
    																		sl10 = 5
    																	duration = 2
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n3 (3)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n1 (1)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    															searchSpaceSIB1 = 0
    															searchSpaceOtherSystemInformation = 3
    															pagingSearchSpace = 0
    															ra_SearchSpace = 1
    															firstPDCCH_MonitoringOccasionOfPO = Omit
    															commonSearchSpaceListExt_r16 = Omit
    															sdt_SearchSpace_r17 = Omit
    															searchSpaceMCCH_r17 = Omit
    															searchSpaceMTCH_r17 = Omit
    															commonSearchSpaceListExt2_r17 = Omit
    															firstPDCCH_MonitoringOccasionOfPO_v1710 = Omit
    															pei_ConfigBWP_r17 = Omit
    															followUnifiedTCI_State_v1720 = Omit
    													pdsch_ConfigCommon
    														setup
    															pdsch_TimeDomainAllocationList
    																PDSCH_TimeDomainResourceAllocation
    																	k0 = Omit
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 53
    												bcch_Config
    													modificationPeriodCoeff = n4 (1)
    												pcch_Config
    													defaultPagingCycle = rf128 (2)
    													nAndPagingFrameOffset
    														halfT = 0
    													ns = one (2)
    													firstPDCCH_MonitoringOccasionOfPO = Omit
    													nrofPDCCH_MonitoringOccasionPerSSB_InPO_r16 = Omit
    													ranPagingInIdlePO_r17 = Omit
    													firstPDCCH_MonitoringOccasionOfPO_v1710 = Omit
    												pei_Config_r17 = Omit
    												initialDownlinkBWP_RedCap_r17 = Omit
    											uplinkConfigCommon
    												frequencyInfoUL
    													frequencyBandList = Omit
    													absoluteFrequencyPointA = Omit
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz120 (3)
    															carrierBandwidth = 66
    															txDirectCurrentLocation = Omit
    													p_Max = 23
    													frequencyShift7p5khz = Omit
    												initialUplinkBWP
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 149
    																msg1_FDM = one (0)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    																prach_ConfigurationPeriodScaling_IAB_r16 = Omit
    																prach_ConfigurationFrameOffset_IAB_r16 = Omit
    																prach_ConfigurationSOffset_IAB_r16 = Omit
    																ra_ResponseWindow_v1610 = Omit
    																prach_ConfigurationIndex_v1610 = Omit
    																ra_ResponseWindow_v1700 = Omit
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n4 (0)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 0
    															msg1_SubcarrierSpacing = kHz120 (3)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    															ra_PrioritizationForAccessIdentity_r16 = Omit
    															prach_RootSequenceIndex_r16 = Omit
    															ra_PrioritizationForSlicing_r17 = Omit
    															featureCombinationPreamblesList_r17 = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 3
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    															nrofPRBs = Omit
    															intra_SlotFH_r17 = Omit
    															pucch_ResourceCommonRedCap_r17 = Omit
    															additionalPRBOffset_r17 = Omit
    													rach_ConfigCommonIAB_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													msgA_ConfigCommon_r16 = Omit
    													enableRA_PrioritizationForSlicing_r17 = Omit
    													additionalRACH_ConfigList_r17 = Omit
    													rsrp_ThresholdMsg3_r17 = Omit
    													numberOfMsg3_RepetitionsList_r17 = Omit
    													mcs_Msg3_Repetitions_r17 = Omit
    												timeAlignmentTimerCommon = infinity_ (7)
    											supplementaryUplink = Omit
    											n_TimingAdvanceOffset = Omit
    											ssb_PositionsInBurst
    												inOneGroup = 01000000'B
    												groupPresence = 10000000'B
    											ssb_PeriodicityServingCell = ms20 (2)
    											tdd_UL_DL_ConfigurationCommon
    												referenceSubcarrierSpacing = kHz120 (3)
    												pattern1
    													dl_UL_TransmissionPeriodicity = ms0p625 (1)
    													nrofDownlinkSlots = 3
    													nrofDownlinkSymbols = 10
    													nrofUplinkSlots = 1
    													nrofUplinkSymbols = 2
    													dl_UL_TransmissionPeriodicity_v1530 = Omit
    												pattern2 = Omit
    											ss_PBCH_BlockPower = 0
    											channelAccessMode_r16 = Omit
    											discoveryBurstWindowLength_r16 = Omit
    											highSpeedConfig_r16 = Omit
    											channelAccessMode2_r17 = Omit
    											discoveryBurstWindowLength_v1700 = Omit
    											highSpeedConfigFR2_r17 = Omit
    											uplinkConfigCommon_v1700 = Omit
    											enhancedMeasurementLEO_r17 = Omit
    											ra_ChannelAccess_r17 = Omit
    										ims_EmergencySupport = true_ (0)
    										eCallOverIMS_Support = Omit
    										ue_TimersAndConstants
    											t300 = ms1000 (5)
    											t301 = ms1000 (5)
    											t310 = ms1000 (5)
    											n310 = n1 (0)
    											t311 = ms30000 (6)
    											n311 = n1 (0)
    											t319 = ms1000 (5)
    										uac_BarringInfo = Omit
    										useFullResumeID = Omit
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											idleModeMeasurementsEUTRA_r16 = Omit
    											idleModeMeasurementsNR_r16 = Omit
    											posSI_SchedulingInfo_r16 = Omit
    											nonCriticalExtension
    												uac_BarringInfo_v1630 = Omit
    												nonCriticalExtension
    													hsdn_Cell_r17 = Omit
    													uac_BarringInfo_v1700 = Omit
    													sdt_ConfigCommon_r17 = Omit
    													redCap_ConfigCommon_r17 = Omit
    													featurePriorities_r17 = Omit
    													si_SchedulingInfo_v1700 = Omit
    													hyperSFN_r17 = Omit
    													eDRX_AllowedIdle_r17 = Omit
    													eDRX_AllowedInactive_r17 = Omit
    													intraFreqReselectionRedCap_r17 = Omit
    													cellBarredNTN_r17 = Omit
    													nonCriticalExtension = Omit
    						SIs
    							BCCH_DL_SCH_Message
    								message_
    									c1
    										systemInformation
    											criticalExtensions
    												systemInformation
    													sib_TypeAndInfo
    														SystemInformation_IEs___0___oftype
    															sib2
    																cellReselectionInfoCommon
    																	nrofSS_BlocksToAverage = 2
    																	absThreshSS_BlocksConsolidation
    																		thresholdRSRP = 0
    																		thresholdRSRQ = Omit
    																		thresholdSINR = Omit
    																	rangeToBestCell = dB0 (15)
    																	q_Hyst = dB0 (0)
    																	speedStateReselectionPars = Omit
    																cellReselectionServingFreqInfo
    																	s_NonIntraSearchP = Omit
    																	s_NonIntraSearchQ = Omit
    																	threshServingLowP = 0
    																	threshServingLowQ = Omit
    																	cellReselectionPriority = 4
    																	cellReselectionSubPriority = Omit
    																intraFreqCellReselectionInfo
    																	q_RxLevMin = -55
    																	q_RxLevMinSUL = Omit
    																	q_QualMin = Omit
    																	s_IntraSearchP = 31
    																	s_IntraSearchQ = Omit
    																	t_ReselectionNR = 0
    																	frequencyBandList = Omit
    																	frequencyBandListSUL = Omit
    																	p_Max = Omit
    																	smtc
    																		periodicityAndOffset
    																			sf20 = 0
    																		duration = sf3 (2)
    																	ss_RSSI_Measurement = Omit
    																	ssb_ToMeasure
    																		longBitmap = 1100000000000000000000000000000000000000000000000000000000000000'B
    																	deriveSSB_IndexFromCell = True
    																	t_ReselectionNR_SF = Omit
    																	smtc2_LP_r16 = Omit
    																	ssb_PositionQCL_Common_r16 = Omit
    																	ssb_PositionQCL_Common_r17 = Omit
    																	smtc4list_r17 = Omit
    																relaxedMeasurement_r16 = Omit
    																cellEquivalentSize_r17 = Omit
    																relaxedMeasurement_r17 = Omit
    													lateNonCriticalExtension = Omit
    													nonCriticalExtension = Omit
    						SegmentedSIs = Omit
    						PosSIs = Omit
    						NCD_MIBs = Omit
    				PcchConfig
    					SearchSpaceAndDci
    						AssignedBWPs
    							ActiveBWP = Omit
    							InitialBWP = True
    							DedicatedBWPs
    							InitialBWP_RedCap = Omit
    						SearchSpaceType = cssType2 (3)
    						DciInfo
    							ResoureAssignment
    								ResourceAllocationType = resourceAllocationType1 (1)
    								FreqDomain
    									Automatic
    										FirstRbIndex = 7
    										MaxRbCnt = 17
    								TimeDomain
    									Index = 0000'B
    								TransportBlockScheduling
    									Automatic
    										TransportBlock1 = qpsk (0)
    										TransportBlock2 = Omit
    										RedundancyVersionList
    								HarqProcessConfig
    									None = True
    							VrbPrbMapping
    								Index = 0'B
    							Format
    								Format_1_0_P_RNTI
    									ShortMessageIndicator = 01'B
    									ShortMessages = 00000000'B
    									TbScaling = 00'B
    									TrsAvailabilityIndication
    										None = True
    				RachProcedureConfig
    					RachProcedureList
    						NR_RachProcedure_Type
    							MsgB = Omit
    							RandomAccessResponse
    								SearchSpaceAndDci
    									AssignedBWPs
    										ActiveBWP = Omit
    										InitialBWP = True
    										DedicatedBWPs
    										InitialBWP_RedCap = Omit
    									SearchSpaceType = cssType1 (2)
    									DciInfo
    										ResoureAssignment
    											ResourceAllocationType = resourceAllocationType1 (1)
    											FreqDomain
    												Automatic
    													FirstRbIndex = 7
    													MaxRbCnt = 17
    											TimeDomain
    												Index = 0000'B
    											TransportBlockScheduling
    												Automatic
    													TransportBlock1 = qpsk (0)
    													TransportBlock2 = Omit
    													RedundancyVersionList
    											HarqProcessConfig
    												None = True
    										VrbPrbMapping
    											Index = 0'B
    										Format
    											Format_1_0_RA_RNTI
    												TbScaling = 00'B
    												LSBsOfSFN
    													None = True
    								MacPdu
    									SubPduList
    										NR_RAR_SubPdu_Type
    											RapIdAndPayload
    												RapId
    													Automatic = True
    												Payload
    													TimingAdvance = 0
    													UplinkGrant
    														HoppingFlag = 0'B
    														Msg3FrequencyResourceAllocation = 00000100001000'B
    														Msg3TimeResourceAllocation = 0001'B
    														MCS = 0010'B
    														TPC_Command = 011'B
    														CQI_Req = 0'B
    													TempC_RNTI
    														SameAsC_RNTI = True
    									CrcError = False
    							ContentionResolution
    								Msg4_Based
    									SearchSpaceAndDci
    										AssignedBWPs
    											ActiveBWP = Omit
    											InitialBWP = True
    											DedicatedBWPs
    											InitialBWP_RedCap = Omit
    										SearchSpaceType = cssType1 (2)
    										DciInfo
    											ResoureAssignment
    												ResourceAllocationType = resourceAllocationType1 (1)
    												FreqDomain
    													Automatic
    														FirstRbIndex = 7
    														MaxRbCnt = 17
    												TimeDomain
    													Index = 0000'B
    												TransportBlockScheduling
    													Automatic
    														TransportBlock1 = qam64 (2)
    														TransportBlock2 = Omit
    														RedundancyVersionList
    															NR_RedundancyVersion_Type = 0
    															NR_RedundancyVersion_Type = 2
    															NR_RedundancyVersion_Type = 3
    															NR_RedundancyVersion_Type = 1
    															NR_RedundancyVersion_Type = 0
    												HarqProcessConfig
    													AnyProcess = True
    											VrbPrbMapping
    												Index = 0'B
    											Format
    												Format_1_0
    													DAI
    														Index
    															Automatic = True
    													TpcCommandPucch
    														Value = 01'B
    													PucchResourceIndicator
    														Value = 110'B
    													PdschHarqTimingIndicator
    														Value = 111'B
    													ChannelAccessCPext
    														None = True
    									ContentionResolutionId
    										XorMask = 000000000000000000000000000000000000000000000000'B
    									RrcPdu
    										RrcCcchMsg = '204004069AE0048020C3CC00F80200D07800020D62EA000808012D80DA8000F8000000000183708420000D116D000000122440000083A74001020266AAE92838002081840A1839388122858C1A3878FC000082021810010404B04002080A60C0041016C200082031850010406B0C002080E61C00412140310001E258624003C4B2C5000789698B000F12DB18001E25C634003C4BAC7000789798F001058506092BCA18162437234567897D421084000CD01A4901E2AE00C10A00400018FFD29498C637281E000020D1940402000000000882000008848000'O
    									CrcError = False
    				DcchDtchConfig
    					DL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    								InitialBWP_RedCap = Omit
    							SearchSpaceType = ussDL (6)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										Automatic
    											FirstRbIndex = 12
    											MaxRbCnt = 17
    									TimeDomain
    										Index = 'B
    									TransportBlockScheduling
    										Automatic
    											TransportBlock1 = qam64 (2)
    											TransportBlock2 = Omit
    											RedundancyVersionList
    												NR_RedundancyVersion_Type = 0
    												NR_RedundancyVersion_Type = 2
    												NR_RedundancyVersion_Type = 3
    												NR_RedundancyVersion_Type = 1
    												NR_RedundancyVersion_Type = 0
    									HarqProcessConfig
    										AnyProcess = True
    								VrbPrbMapping
    									None = True
    								Format
    									Format_1_1
    										CarrierIndicator
    											None = True
    										BWPIndicator
    											Index = 'B
    										PrbBundlingSizeIndicator
    											None = True
    										RateMatchingIndicator
    											Bitmap = 'B
    										ZP_CSI_RS_Trigger
    											Index = 'B
    										DAI
    											TwoBits
    												Automatic = True
    										TpcCommandPucch
    											Value = 01'B
    										SecondTpcCommand
    											None = True
    										PucchResourceIndicator
    											Value = 110'B
    										PdschHarqTimingIndicator
    											Value = 110'B
    										OneShotHarqAckRequest
    											None = True
    										EnhancedType3CodebookIndicator
    											None = True
    										PdschGroupIndex
    											None = True
    										NewFeedbackIndicator
    											None = True
    										NumberRequestedPdschGroup
    											None = True
    										HarqAckRetransmissionIndicator
    											None = True
    										AntennaPorts
    											Index = 0000'B
    										TCI
    											None = True
    										SrsRequest
    											SingleUL = 00'B
    										SrsOffsetIndicator
    											None = True
    										CBGTI
    											Bitmap = 'B
    										CBGFI
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    										PriorityIndicator
    											None = True
    										ChannelAccessCPext
    											None = True
    										MinimumApplicableSchedulingOffset
    											None = True
    										SCellDormancyIndication
    											None = True
    										PdcchMonitoringAdaptationIndication
    											None = True
    										PucchCellIndicator
    											None = True
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    								InitialBWP_RedCap = Omit
    							SearchSpaceType = ussUL (7)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain
    										Index = 0'B
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig
    										AnyProcess = True
    								PuschHoppingCtrl
    									None = True
    								TpcCommandPusch
    									Value = 01'B
    								UL_SUL_Indicator
    									None = True
    								Format
    									Format_0_1
    										CarrierIndicator
    											None = True
    										DfiFlag
    											None = True
    										BWPIndicator
    											Index = 'B
    										FirstDAI
    											DynamicCodebook
    												Automatic = True
    										SecondDAI
    											None = True
    										ThirdDAI
    											None = True
    										SecondTpcCommandPusch
    											None = True
    										SrsResourceSetIndicator
    											None = True
    										SrsResourceIndicator
    											CodeBook = 'B
    										SecondSrsResourceIndicator
    											None = True
    										PrecodingInfo
    											CodeBook = 'B
    										SecondPrecodingInfo
    											None = True
    										AntennaPorts
    											Index = 000'B
    										SrsRequest
    											SingleUL = 00'B
    										SrsOffsetIndicator
    											None = True
    										CsiRequest
    											Index = 'B
    										CBGTI
    											Index = 'B
    										PtrsDmrsAssociation
    											None = True
    										SecondPtrsDmrsAssociation
    											None = True
    										BetaOffsetIndicator
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    										UlschIndicator
    											Value = 1'B
    										ChannelAccessCPextCAPC
    											None = True
    										OpenLoopPowerControl
    											None = True
    										PriorityIndicator
    											None = True
    										InvalidSymbolPatternIndicator
    											None = True
    										MinimumApplicableSchedulingOffset
    											None = True
    										SCellDormancyIndication
    											None = True
    										SidelinkAssignmentIndex
    											None = True
    										PdcchMonitoringAdaptationIndication
    											None = True
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl
    						None = True
    					MeasGapCtrl
    						None = True
    				ServingCellConfig
    					SpCell
    						ServingCellIndex = 0
    						CellGroupConfig
    							CellGroupId = 0
    							SCellList
    							MAC_CellGroupConfig
    								R15
    									drx_Config = Omit
    									schedulingRequestConfig
    										schedulingRequestToAddModList
    											SchedulingRequestToAddMod
    												schedulingRequestId = 0
    												sr_ProhibitTimer = Omit
    												sr_TransMax = n16 (2)
    										schedulingRequestToReleaseList = Omit
    									bsr_Config
    										periodicBSR_Timer = sf1 (0)
    										retxBSR_Timer = sf80 (3)
    										logicalChannelSR_DelayTimer = Omit
    									tag_Config
    										tag_ToReleaseList = Omit
    										tag_ToAddModList
    											TAG
    												tag_Id = 0
    												timeAlignmentTimer = infinity_ (7)
    									phr_Config
    										setup
    											phr_PeriodicTimer = sf10 (0)
    											phr_ProhibitTimer = sf0 (0)
    											phr_Tx_PowerFactorChange = dB1 (0)
    											multiplePHR = False
    											dummy = False
    											phr_Type2OtherCell = False
    											phr_ModeOtherCG = real (0)
    											mpe_Reporting_FR2_r16 = Omit
    											mpe_Reporting_FR2_r17 = Omit
    											twoPHRMode_r17 = Omit
    									skipUplinkTxDynamic = False
    									csi_Mask = Omit
    									dataInactivityTimer = Omit
    									usePreBSR_r16 = Omit
    									schedulingRequestID_LBT_SCell_r16 = Omit
    									lch_BasedPrioritization_r16 = Omit
    									schedulingRequestID_BFR_SCell_r16 = Omit
    									drx_ConfigSecondaryGroup_r16 = Omit
    									enhancedSkipUplinkTxDynamic_r16 = Omit
    									enhancedSkipUplinkTxConfigured_r16 = Omit
    									intraCG_Prioritization_r17 = Omit
    									drx_ConfigSL_r17 = Omit
    									drx_ConfigExt_v1700 = Omit
    									schedulingRequestID_BFR_r17 = Omit
    									schedulingRequestID_BFR2_r17 = Omit
    									schedulingRequestConfig_v1700 = Omit
    									tar_Config_r17 = Omit
    									g_RNTI_ConfigToAddModList_r17 = Omit
    									g_RNTI_ConfigToReleaseList_r17 = Omit
    									g_CS_RNTI_ConfigToAddModList_r17 = Omit
    									g_CS_RNTI_ConfigToReleaseList_r17 = Omit
    									allowCSI_SRS_Tx_MulticastDRX_Active_r17 = Omit
    									schedulingRequestID_PosMG_Request_r17 = Omit
    									drx_LastTransmissionUL_r17 = Omit
    									posMG_Request_r17 = Omit
    							PhysicalCellGroupConfig
    								R15
    									harq_ACK_SpatialBundlingPUCCH = Omit
    									harq_ACK_SpatialBundlingPUSCH = Omit
    									p_NR_FR1 = 23
    									pdsch_HARQ_ACK_Codebook = dynamic (1)
    									tpc_SRS_RNTI = Omit
    									tpc_PUCCH_RNTI = Omit
    									tpc_PUSCH_RNTI = Omit
    									sp_CSI_RNTI = Omit
    									cs_RNTI = Omit
    									mcs_C_RNTI = Omit
    									p_UE_FR1 = Omit
    									xScale = Omit
    									pdcch_BlindDetection = Omit
    									dcp_Config_r16 = Omit
    									harq_ACK_SpatialBundlingPUCCH_secondaryPUCCHgroup_r16 = Omit
    									harq_ACK_SpatialBundlingPUSCH_secondaryPUCCHgroup_r16 = Omit
    									pdsch_HARQ_ACK_Codebook_secondaryPUCCHgroup_r16 = Omit
    									p_NR_FR2_r16 = Omit
    									p_UE_FR2_r16 = Omit
    									nrdc_PCmode_FR1_r16 = Omit
    									nrdc_PCmode_FR2_r16 = Omit
    									pdsch_HARQ_ACK_Codebook_r16 = Omit
    									nfi_TotalDAI_Included_r16 = Omit
    									ul_TotalDAI_Included_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedback_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedbackNDI_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedbackCBG_r16 = Omit
    									downlinkAssignmentIndexDCI_0_2_r16 = Omit
    									downlinkAssignmentIndexDCI_1_2_r16 = Omit
    									pdsch_HARQ_ACK_CodebookList_r16 = Omit
    									ackNackFeedbackMode_r16 = Omit
    									pdcch_BlindDetectionCA_CombIndicator_r16 = Omit
    									pdcch_BlindDetection2_r16 = Omit
    									pdcch_BlindDetection3_r16 = Omit
    									bdFactorR_r16 = Omit
    									pdsch_HARQ_ACK_EnhType3ToAddModList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3ToReleaseList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3SecondaryToAddModList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3SecondaryToReleaseList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3DCI_FieldSecondaryPUCCHgroup_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3DCI_Field_r17 = Omit
    									pdsch_HARQ_ACK_Retx_r17 = Omit
    									pdsch_HARQ_ACK_RetxSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCell_r17 = Omit
    									pucch_sSCellSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCellDyn_r17 = Omit
    									pucch_sSCellDynSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCellPattern_r17 = Omit
    									pucch_sSCellPatternSecondaryPUCCHgroup_r17 = Omit
    									uci_MuxWithDiffPrio_r17 = Omit
    									uci_MuxWithDiffPrioSecondaryPUCCHgroup_r17 = Omit
    									simultaneousPUCCH_PUSCH_r17 = Omit
    									simultaneousPUCCH_PUSCH_SecondaryPUCCHgroup_r17 = Omit
    									prioLowDG_HighCG_r17 = Omit
    									prioHighDG_LowCG_r17 = Omit
    									twoQCLTypeDforPDCCHRepetition_r17 = Omit
    									multicastConfig_r17 = Omit
    									pdcch_BlindDetectionCA_CombIndicator_r17 = Omit
    									simultaneousSR_PUSCH_diffPUCCH_Groups_r17 = Omit
    									intraBandNC_PRACH_simulTx_r17 = Omit
    									pdcch_BlindDetection4_r17 = Omit
    				SidelinkScheduled = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 0
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										TM = True
    									TestMode
    										None = True
    								LogicalChannelId = Omit
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3

    summary = Message Mismatch: PDSCH_Config___6
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___6
    		PDSCH_Config___6 = resourceAllocationType0 (0)

    summary = Message Mismatch: PDSCH_Config___14
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___14
    		PDSCH_Config___14 = qam256 (0)

    summary = Message Mismatch: PUSCH_Config___7
    MATCH_MISMATCH
    	Message Mismatch: PUSCH_Config___7
    		PUSCH_Config___7 = resourceAllocationType0 (0)

    BCCH-BCH-Message
    	message = mib =
    		systemFrameNumber = 000000
    		subCarrierSpacingCommon = scs30or120
    		ssb-SubcarrierOffset = 10
    		dmrs-TypeA-Position = pos2
    		pdcch-ConfigSIB1
    			controlResourceSetZero = 1
    			searchSpaceZero = 0
    		cellBarred = notBarred
    		intraFreqReselection = allowed
    		spare = 0

    BCCH-DL-SCH-Message
    	message = c1 = systemInformationBlockType1 =
    		cellSelectionInfo
    			q-RxLevMin = -57
    		cellAccessRelatedInfo
    			plmn-IdentityInfoList = SEQUENCE OF PLMN-IdentityInfo
    				PLMN-IdentityInfo(1)
    					plmn-IdentityList = SEQUENCE OF PLMN-Identity
    						PLMN-Identity(1)
    							mcc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 0
    								MCC-MNC-Digit(3) = 1
    							mnc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 1
    					trackingAreaCode = 000000000000000000000001
    					ranac = 1
    					cellIdentity = 000000000000000000000000010000000010
    					cellReservedForOperatorUse = notReserved
    		connEstFailureControl
    			connEstFailCount = n1
    			connEstFailOffsetValidity = s30
    			connEstFailOffset = 1
    		si-SchedulingInfo
    			schedulingInfoList = SEQUENCE OF SchedulingInfo
    				SchedulingInfo(1)
    					si-BroadcastStatus = broadcasting
    					si-Periodicity = rf32
    					sib-MappingInfo = SEQUENCE OF SIB-TypeInfo
    						SIB-TypeInfo(1)
    							type = sibType2
    							valueTag = 0
    			si-WindowLength = s160
    			systemInformationAreaID = 000000000000000000000001
    		servingCellConfigCommon
    			downlinkConfigCommon
    				frequencyInfoDL
    					frequencyBandList = SEQUENCE OF NR-MultiBandInfo
    						NR-MultiBandInfo(1)
    							freqBandIndicatorNR = 257
    							nr-NS-PmaxList = SEQUENCE OF NR-NS-PmaxValue
    								NR-NS-PmaxValue(1)
    									additionalSpectrumEmission = 0
    					offsetToPointA = 18
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz120
    							carrierBandwidth = 66
    				initialDownlinkBWP
    					genericParameters
    						locationAndBandwidth = 17875
    						subcarrierSpacing = kHz120
    					pdcch-ConfigCommon = setup =
    						controlResourceSetZero = 1
    						commonSearchSpaceList = SEQUENCE OF SearchSpace
    							SearchSpace(1)
    								searchSpaceId = 1
    								controlResourceSetId = 0
    								monitoringSlotPeriodicityAndOffset = sl1 = NULL
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n3
    									aggregationLevel4 = n2
    									aggregationLevel8 = n1
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    							SearchSpace(2)
    								searchSpaceId = 3
    								controlResourceSetId = 0
    								monitoringSlotPeriodicityAndOffset = sl10 = 5
    								duration = 2
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n3
    									aggregationLevel4 = n2
    									aggregationLevel8 = n1
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    						searchSpaceSIB1 = 0
    						searchSpaceOtherSystemInformation = 3
    						pagingSearchSpace = 0
    						ra-SearchSpace = 1
    					pdsch-ConfigCommon = setup =
    						pdsch-TimeDomainAllocationList = SEQUENCE OF PDSCH-TimeDomainResourceAllocation
    							PDSCH-TimeDomainResourceAllocation(1)
    								mappingType = typeA
    								startSymbolAndLength = 53
    				bcch-Config
    					modificationPeriodCoeff = n4
    				pcch-Config
    					defaultPagingCycle = rf128
    					nAndPagingFrameOffset = halfT = 0
    					ns = one
    			uplinkConfigCommon
    				frequencyInfoUL
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz120
    							carrierBandwidth = 66
    					p-Max = 23
    				initialUplinkBWP
    					genericParameters
    						locationAndBandwidth = 17875
    						subcarrierSpacing = kHz120
    					rach-ConfigCommon = setup =
    						rach-ConfigGeneric
    							prach-ConfigurationIndex = 149
    							msg1-FDM = one
    							msg1-FrequencyStart = 0
    							zeroCorrelationZoneConfig = 15
    							preambleReceivedTargetPower = -118
    							preambleTransMax = n7
    							powerRampingStep = dB4
    							ra-ResponseWindow = sl20
    						ssb-perRACH-OccasionAndCB-PreamblesPerSSB = one = n4
    						ra-ContentionResolutionTimer = sf64
    						rsrp-ThresholdSSB = 0
    						prach-RootSequenceIndex = l139 = 32
    						msg1-SubcarrierSpacing = kHz120
    						restrictedSetConfig = unrestrictedSet
    					pusch-ConfigCommon = setup =
    						pusch-TimeDomainAllocationList = SEQUENCE OF PUSCH-TimeDomainResourceAllocation
    							PUSCH-TimeDomainResourceAllocation(1)
    								k2 = 4
    								mappingType = typeA
    								startSymbolAndLength = 27
    							PUSCH-TimeDomainResourceAllocation(2)
    								k2 = 3
    								mappingType = typeA
    								startSymbolAndLength = 27
    						msg3-DeltaPreamble = 1
    						p0-NominalWithGrant = -90
    					pucch-ConfigCommon = setup =
    						pucch-ResourceCommon = 0
    						pucch-GroupHopping = enable
    						p0-nominal = -90
    				timeAlignmentTimerCommon = infinity
    			ssb-PositionsInBurst
    				inOneGroup = 10000000
    				groupPresence = 10000000
    			ssb-PeriodicityServingCell = ms20
    			tdd-UL-DL-ConfigurationCommon
    				referenceSubcarrierSpacing = kHz120
    				pattern1
    					dl-UL-TransmissionPeriodicity = ms0p625
    					nrofDownlinkSlots = 3
    					nrofDownlinkSymbols = 10
    					nrofUplinkSlots = 1
    					nrofUplinkSymbols = 2
    			ss-PBCH-BlockPower = 0
    		ims-EmergencySupport = true
    		ue-TimersAndConstants
    			t300 = ms1000
    			t301 = ms1000
    			t310 = ms1000
    			n310 = n1
    			t311 = ms30000
    			n311 = n1
    			t319 = ms1000

    BCCH-DL-SCH-Message
    	message = c1 = systemInformation =
    		criticalExtensions = systemInformation =
    			sib-TypeAndInfo = SEQUENCE OF CHOICE
    				CHOICE(1) = sib2 =
    					cellReselectionInfoCommon
    						nrofSS-BlocksToAverage = 2
    						absThreshSS-BlocksConsolidation
    							thresholdRSRP = 0
    						rangeToBestCell = dB0
    						q-Hyst = dB0
    					cellReselectionServingFreqInfo
    						threshServingLowP = 0
    						cellReselectionPriority = 4
    					intraFreqCellReselectionInfo
    						q-RxLevMin = -55
    						s-IntraSearchP = 31
    						t-ReselectionNR = 0
    						smtc
    							periodicityAndOffset = sf20 = 0
    							duration = sf3
    						ssb-ToMeasure = longBitmap = 1100000000000000000000000000000000000000000000000000000000000000
    						deriveSSB-IndexFromCell = TRUE

    DL-CCCH-Message
    	message = c1 = rrcSetup =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetup =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 1
    			masterCellGroup = CONTAINING =
    				cellGroupId = 0
    				rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    					RLC-BearerConfig(1)
    						logicalChannelIdentity = 1
    						servedRadioBearer = srb-Identity = 1
    						mac-LogicalChannelConfig
    							ul-SpecificParameters
    								priority = 1
    								prioritisedBitRate = infinity
    								bucketSizeDuration = ms50
    								logicalChannelGroup = 0
    								schedulingRequestID = 0
    								logicalChannelSR-Mask = FALSE
    								logicalChannelSR-DelayTimerApplied = FALSE
    				mac-CellGroupConfig
    					schedulingRequestConfig
    						schedulingRequestToAddModList = SEQUENCE OF SchedulingRequestToAddMod
    							SchedulingRequestToAddMod(1)
    								schedulingRequestId = 0
    								sr-TransMax = n16
    					bsr-Config
    						periodicBSR-Timer = sf1
    						retxBSR-Timer = sf80
    					tag-Config
    						tag-ToAddModList = SEQUENCE OF TAG
    							TAG(1)
    								tag-Id = 0
    								timeAlignmentTimer = infinity
    					phr-Config = setup =
    						phr-PeriodicTimer = sf10
    						phr-ProhibitTimer = sf0
    						phr-Tx-PowerFactorChange = dB1
    						multiplePHR = FALSE
    						dummy = FALSE
    						phr-Type2OtherCell = FALSE
    						phr-ModeOtherCG = real
    					skipUplinkTxDynamic = FALSE
    				physicalCellGroupConfig
    					p-NR-FR1 = 23
    					pdsch-HARQ-ACK-Codebook = dynamic
    				spCellConfig
    					rlf-TimersAndConstants = setup =
    						t310 = ms1000
    						n310 = n1
    						n311 = n1
    						t311 = ms1000
    					spCellConfigDedicated
    						initialDownlinkBWP
    							pdcch-Config = setup =
    								controlResourceSetToAddModList = SEQUENCE OF ControlResourceSet
    									ControlResourceSet(1)
    										controlResourceSetId = 1
    										frequencyDomainResources = 111100000000000000000000000000000000000000000
    										duration = 2
    										cce-REG-MappingType = nonInterleaved = NULL
    										precoderGranularity = sameAsREG-bundle
    								searchSpacesToAddModList = SEQUENCE OF SearchSpace
    									SearchSpace(1)
    										searchSpaceId = 2
    										controlResourceSetId = 1
    										monitoringSlotPeriodicityAndOffset = sl1 = NULL
    										monitoringSymbolsWithinSlot = 10000000000000
    										nrofCandidates
    											aggregationLevel1 = n0
    											aggregationLevel2 = n3
    											aggregationLevel4 = n2
    											aggregationLevel8 = n1
    											aggregationLevel16 = n0
    										searchSpaceType = ue-Specific =
    											dci-Formats = formats0-1-And-1-1
    							pdsch-Config = setup =
    								dataScramblingIdentityPDSCH = 0
    								dmrs-DownlinkForPDSCH-MappingTypeA = setup =
    									dmrs-AdditionalPosition = pos0
    									phaseTrackingRS = setup =
    										epre-Ratio = 0
    								tci-StatesToAddModList = SEQUENCE OF TCI-State
    									TCI-State(1)
    										tci-StateId = 0
    										qcl-Type1
    											referenceSignal = ssb = 0
    											qcl-Type = typeD
    								resourceAllocation = resourceAllocationType1
    								rbg-Size = config1
    								prb-BundlingType = staticBundling =
    									bundleSize = wideband
    							radioLinkMonitoringConfig = setup =
    								failureDetectionResourcesToAddModList = SEQUENCE OF RadioLinkMonitoringRS
    									RadioLinkMonitoringRS(1)
    										radioLinkMonitoringRS-Id = 0
    										purpose = rlf
    										detectionResource = ssb-Index = 0
    						firstActiveDownlinkBWP-Id = 0
    						defaultDownlinkBWP-Id = 0
    						uplinkConfig
    							initialUplinkBWP
    								pucch-Config = setup =
    									resourceSetToAddModList = SEQUENCE OF PUCCH-ResourceSet
    										PUCCH-ResourceSet(1)
    											pucch-ResourceSetId = 0
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 0
    												PUCCH-ResourceId(2) = 1
    												PUCCH-ResourceId(3) = 2
    												PUCCH-ResourceId(4) = 3
    												PUCCH-ResourceId(5) = 4
    												PUCCH-ResourceId(6) = 5
    												PUCCH-ResourceId(7) = 6
    												PUCCH-ResourceId(8) = 7
    										PUCCH-ResourceSet(2)
    											pucch-ResourceSetId = 1
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 8
    												PUCCH-ResourceId(2) = 9
    												PUCCH-ResourceId(3) = 10
    												PUCCH-ResourceId(4) = 11
    												PUCCH-ResourceId(5) = 12
    												PUCCH-ResourceId(6) = 13
    												PUCCH-ResourceId(7) = 14
    												PUCCH-ResourceId(8) = 15
    									resourceToAddModList = SEQUENCE OF PUCCH-Resource
    										PUCCH-Resource(1)
    											pucch-ResourceId = 0
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(2)
    											pucch-ResourceId = 1
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(3)
    											pucch-ResourceId = 2
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(4)
    											pucch-ResourceId = 3
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(5)
    											pucch-ResourceId = 4
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(6)
    											pucch-ResourceId = 5
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(7)
    											pucch-ResourceId = 6
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(8)
    											pucch-ResourceId = 7
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format1 =
    												initialCyclicShift = 0
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    												timeDomainOCC = 0
    										PUCCH-Resource(9)
    											pucch-ResourceId = 8
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(10)
    											pucch-ResourceId = 9
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(11)
    											pucch-ResourceId = 10
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(12)
    											pucch-ResourceId = 11
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(13)
    											pucch-ResourceId = 12
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(14)
    											pucch-ResourceId = 13
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(15)
    											pucch-ResourceId = 14
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 60
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(16)
    											pucch-ResourceId = 15
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 65
    											format = format3 =
    												nrofPRBs = 1
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    									format1 = setup =
    										interslotFrequencyHopping = enabled
    									format2 = setup =
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									format3 = setup =
    										interslotFrequencyHopping = enabled
    										additionalDMRS = true
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									schedulingRequestResourceToAddModList = SEQUENCE OF SchedulingRequestResourceConfig
    										SchedulingRequestResourceConfig(1)
    											schedulingRequestResourceId = 1
    											schedulingRequestID = 0
    											periodicityAndOffset = sl80 = 9
    											resource = 6
    									dl-DataToUL-ACK = SEQUENCE OF INTEGER
    										INTEGER(1) = 2
    										INTEGER(2) = 3
    										INTEGER(3) = 4
    										INTEGER(4) = 5
    										INTEGER(5) = 6
    										INTEGER(6) = 7
    										INTEGER(7) = 8
    										INTEGER(8) = 9
    									pucch-PowerControl
    										deltaF-PUCCH-f0 = 0
    										deltaF-PUCCH-f1 = 0
    										deltaF-PUCCH-f2 = 0
    										deltaF-PUCCH-f3 = 0
    										deltaF-PUCCH-f4 = 0
    										pathlossReferenceRSs = SEQUENCE OF PUCCH-PathlossReferenceRS
    											PUCCH-PathlossReferenceRS(1)
    												pucch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 0
    								pusch-Config = setup =
    									txConfig = codebook
    									dmrs-UplinkForPUSCH-MappingTypeA = setup =
    										dmrs-AdditionalPosition = pos0
    										transformPrecodingDisabled
    									pusch-PowerControl
    										msg3-Alpha = alpha08
    										p0-NominalWithoutGrant = -90
    										p0-AlphaSets = SEQUENCE OF P0-PUSCH-AlphaSet
    											P0-PUSCH-AlphaSet(1)
    												p0-PUSCH-AlphaSetId = 0
    												p0 = 0
    												alpha = alpha08
    										pathlossReferenceRSToAddModList = SEQUENCE OF PUSCH-PathlossReferenceRS
    											PUSCH-PathlossReferenceRS(1)
    												pusch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 0
    										sri-PUSCH-MappingToAddModList = SEQUENCE OF SRI-PUSCH-PowerControl
    											SRI-PUSCH-PowerControl(1)
    												sri-PUSCH-PowerControlId = 0
    												sri-PUSCH-PathlossReferenceRS-Id = 0
    												sri-P0-PUSCH-AlphaSetId = 0
    												sri-PUSCH-ClosedLoopIndex = i0
    									resourceAllocation = resourceAllocationType1
    									codebookSubset = nonCoherent
    									maxRank = 1
    									uci-OnPUSCH = setup =
    										betaOffsets = semiStatic =
    											betaOffsetACK-Index1 = 9
    											betaOffsetACK-Index2 = 9
    											betaOffsetACK-Index3 = 9
    											betaOffsetCSI-Part1-Index1 = 6
    											betaOffsetCSI-Part1-Index2 = 6
    											betaOffsetCSI-Part2-Index1 = 6
    											betaOffsetCSI-Part2-Index2 = 6
    										scaling = f1
    								srs-Config = setup =
    									srs-ResourceSetToAddModList = SEQUENCE OF SRS-ResourceSet
    										SRS-ResourceSet(1)
    											srs-ResourceSetId = 0
    											srs-ResourceIdList = SEQUENCE OF SRS-ResourceId
    												SRS-ResourceId(1) = 0
    											resourceType = aperiodic =
    												aperiodicSRS-ResourceTrigger = 1
    												slotOffset = 4
    											usage = codebook
    											alpha = alpha0
    											p0 = 0
    											pathlossReferenceRS = ssb-Index = 0
    									srs-ResourceToAddModList = SEQUENCE OF SRS-Resource
    										SRS-Resource(1)
    											srs-ResourceId = 0
    											nrofSRS-Ports = port1
    											transmissionComb = n2 =
    												combOffset-n2 = 0
    												cyclicShift-n2 = 0
    											resourceMapping
    												startPosition = 0
    												nrofSymbols = n1
    												repetitionFactor = n1
    											freqDomainPosition = 0
    											freqDomainShift = 0
    											freqHopping
    												c-SRS = 17
    												b-SRS = 0
    												b-hop = 0
    											groupOrSequenceHopping = groupHopping
    											resourceType = aperiodic =
    											sequenceId = 0
    											spatialRelationInfo
    												referenceSignal = ssb-Index = 0
    							firstActiveUplinkBWP-Id = 0
    							pusch-ServingCellConfig = setup =
    						pdcch-ServingCellConfig = setup =
    						pdsch-ServingCellConfig = setup =
    						tag-Id = 0

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell2 (2)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig
    					CA_Capability = None (3)
    				CellConfigCommon
    					C_RNTI = 4097
    					CellTimingInfo
    						TcOffset = 0
    						Tcell = 0
    						SfnOffset = 0
    						HsfnOffset = 0
    					InitialCellPower
    						MaxReferencePower = -82
    						Attenuation
    							Off = True
    				PhysicalLayer
    					Common
    						PhysicalCellId = 50
    						DuplexMode
    							TDD
    								Config
    									Common
    										R15
    											referenceSubcarrierSpacing = kHz120 (3)
    											pattern1
    												dl_UL_TransmissionPeriodicity = ms0p625 (1)
    												nrofDownlinkSlots = 3
    												nrofDownlinkSymbols = 10
    												nrofUplinkSlots = 1
    												nrofUplinkSymbols = 2
    												dl_UL_TransmissionPeriodicity_v1530 = Omit
    											pattern2 = Omit
    									Dedicated = Omit
    					Downlink
    						FrequencyInfoDL
    							R15
    								absoluteFrequencySSB = 2054683
    								frequencyBandList
    									FreqBandIndicatorNR = 257
    								absoluteFrequencyPointA = 2054207
    								scs_SpecificCarrierList
    									SCS_SpecificCarrier
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz120 (3)
    										carrierBandwidth = 66
    										txDirectCurrentLocation = Omit
    						SSPbchBlock
    							SubCarrierSpacing = kHz120 (3)
    							SubcarrierOffset = 10
    							Periodicity = ms20 (2)
    							HalfFrameOffset = 0
    							BurstConfig
    								BlockPattern = caseD (3)
    								PositionsInBurst
    									longBitmap = 1000000000000000000000000000000000000000000000000000000000000000'B
    								BeamArray = Omit
    							RelativeTxPower
    								PbchToDmrs = 0
    								PssToSss = 0
    								SssToSsbBeam = 0
    								DmrsToSss = 0
    						PdschCellLevelConfig
    							DMRS_TypeA_Position = pos2 (0)
    							RateMatchPattern
    								PatternList = Omit
    								PatternListLteCrs = Omit
    							ServingCellConfig
    								R15
    									codeBlockGroupTransmission = Omit
    									xOverhead = Omit
    									nrofHARQ_ProcessesForPDSCH = Omit
    									pucch_Cell = Omit
    									maxMIMO_Layers = Omit
    									processingType2Enabled = Omit
    									pdsch_CodeBlockGroupTransmissionList_r16 = Omit
    									downlinkHARQ_FeedbackDisabled_r17 = Omit
    									nrofHARQ_ProcessesForPDSCH_v1700 = Omit
    						BWPs
    							ActiveBWP = 0
    							BwpArray
    								NR_DownlinkBWP_Type
    									Id = 0
    									BWP
    										R15
    											locationAndBandwidth = 17875
    											subcarrierSpacing = kHz120 (3)
    											cyclicPrefix = Omit
    									Pdcch
    										SearchSpaceArray
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType0 (0)
    														CandidatePriority = 0
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType2 (3)
    														CandidatePriority = 3
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 0
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl160 = 1
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n0 (0)
    															aggregationLevel4 = n4 (4)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n1 (1)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType1 (2)
    														CandidatePriority = 2
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType3 (5)
    														CandidatePriority = 4
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 1
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = ussDL (6)
    														CandidatePriority = 5
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = ussUL (7)
    														CandidatePriority = 9
    												AggregationLevel = AggregationLevel2 (1)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 2
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															ue_Specific
    																dci_Formats = formats0_1_And_1_1 (1)
    																dci_Formats_MT_r16 = Omit
    																dci_FormatsSL_r16 = Omit
    																dci_FormatsExt_r16 = Omit
    													R16 = Omit
    													R17 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														Type = cssType0A (1)
    														CandidatePriority = 1
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 3
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl10 = 5
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n3 (3)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    													R16 = Omit
    													R17 = Omit
    										CoresetArray
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 0
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														interleaved
    															reg_BundleSize = n6 (2)
    															interleaverSize = n2 (0)
    															shiftIndex = 50
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    													rb_Offset_r16 = Omit
    													tci_PresentDCI_1_2_r16 = Omit
    													coresetPoolIndex_r16 = Omit
    													controlResourceSetId_v1610 = Omit
    													followUnifiedTCI_State_r17 = Omit
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 1
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														nonInterleaved = Null
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    													rb_Offset_r16 = Omit
    													tci_PresentDCI_1_2_r16 = Omit
    													coresetPoolIndex_r16 = Omit
    													controlResourceSetId_v1610 = Omit
    													followUnifiedTCI_State_r17 = Omit
    										RelativeTxPower
    											PdcchToCell = 0
    											PdcchToDmrs = 0
    										Coreset0_OffsetRBs = 4
    									Pdsch
    										ConfigCommon
    											R15
    												pdsch_TimeDomainAllocationList
    													PDSCH_TimeDomainResourceAllocation
    														k0 = Omit
    														mappingType = typeA (0)
    														startSymbolAndLength = 53
    										ConfigDedicated
    											R15
    												dataScramblingIdentityPDSCH = 0
    												dmrs_DownlinkForPDSCH_MappingTypeA
    													setup
    														dmrs_Type = Omit
    														dmrs_AdditionalPosition = pos0 (0)
    														maxLength = Omit
    														scramblingID0 = Omit
    														scramblingID1 = Omit
    														phaseTrackingRS
    															setup
    																frequencyDensity = Omit
    																timeDensity = Omit
    																epre_Ratio = 0
    																resourceElementOffset = Omit
    																maxNrofPorts_r16 = Omit
    														dmrs_Downlink_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB = Omit
    												tci_StatesToAddModList
    													TCI_State
    														tci_StateId = 0
    														qcl_Type1
    															cell = Omit
    															bwp_Id = Omit
    															referenceSignal
    																ssb = 0
    															qcl_Type = typeD (3)
    														qcl_Type2 = Omit
    														additionalPCI_r17 = Omit
    														pathlossReferenceRS_Id_r17 = Omit
    														ul_powerControl_r17 = Omit
    												tci_StatesToReleaseList = Omit
    												vrb_ToPRB_Interleaver = Omit
    												resourceAllocation = resourceAllocationType1 (1)
    												pdsch_TimeDomainAllocationList = Omit
    												pdsch_AggregationFactor = Omit
    												rateMatchPatternToAddModList = Omit
    												rateMatchPatternToReleaseList = Omit
    												rateMatchPatternGroup1 = Omit
    												rateMatchPatternGroup2 = Omit
    												rbg_Size = config1 (0)
    												mcs_Table = Omit
    												maxNrofCodeWordsScheduledByDCI = Omit
    												prb_BundlingType
    													staticBundling
    														bundleSize = wideband (1)
    												zp_CSI_RS_ResourceToAddModList = Omit
    												zp_CSI_RS_ResourceToReleaseList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												p_ZP_CSI_RS_ResourceSet = Omit
    												maxMIMO_Layers_r16 = Omit
    												minimumSchedulingOffsetK0_r16 = Omit
    												antennaPortsFieldPresenceDCI_1_2_r16 = Omit
    												aperiodicZP_CSI_RS_ResourceSetsToAddModListDCI_1_2_r16 = Omit
    												aperiodicZP_CSI_RS_ResourceSetsToReleaseListDCI_1_2_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeA_DCI_1_2_r16 = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB_DCI_1_2_r16 = Omit
    												dmrs_SequenceInitializationDCI_1_2_r16 = Omit
    												harq_ProcessNumberSizeDCI_1_2_r16 = Omit
    												mcs_TableDCI_1_2_r16 = Omit
    												numberOfBitsForRV_DCI_1_2_r16 = Omit
    												pdsch_TimeDomainAllocationListDCI_1_2_r16 = Omit
    												prb_BundlingTypeDCI_1_2_r16 = Omit
    												priorityIndicatorDCI_1_2_r16 = Omit
    												rateMatchPatternGroup1DCI_1_2_r16 = Omit
    												rateMatchPatternGroup2DCI_1_2_r16 = Omit
    												resourceAllocationType1GranularityDCI_1_2_r16 = Omit
    												vrb_ToPRB_InterleaverDCI_1_2_r16 = Omit
    												referenceOfSLIVDCI_1_2_r16 = Omit
    												resourceAllocationDCI_1_2_r16 = Omit
    												priorityIndicatorDCI_1_1_r16 = Omit
    												dataScramblingIdentityPDSCH2_r16 = Omit
    												pdsch_TimeDomainAllocationList_r16 = Omit
    												repetitionSchemeConfig_r16 = Omit
    												repetitionSchemeConfig_v1630 = Omit
    												pdsch_HARQ_ACK_OneShotFeedbackDCI_1_2_r17 = Omit
    												pdsch_HARQ_ACK_EnhType3DCI_1_2_r17 = Omit
    												pdsch_HARQ_ACK_EnhType3DCI_Field_1_2_r17 = Omit
    												pdsch_HARQ_ACK_RetxDCI_1_2_r17 = Omit
    												pucch_sSCellDynDCI_1_2_r17 = Omit
    												dl_OrJointTCI_StateList_r17 = Omit
    												beamAppTime_r17 = Omit
    												dummy = Omit
    												dmrs_FD_OCC_DisabledForRank1_PDSCH_r17 = Omit
    												minimumSchedulingOffsetK0_r17 = Omit
    												harq_ProcessNumberSizeDCI_1_2_v1700 = Omit
    												harq_ProcessNumberSizeDCI_1_1_r17 = Omit
    												mcs_Table_r17 = Omit
    												mcs_TableDCI_1_2_r17 = Omit
    												xOverheadMulticast_r17 = Omit
    												priorityIndicatorDCI_4_2_r17 = Omit
    												sizeDCI_4_2_r17 = Omit
    												pdsch_TimeDomainAllocationListForMultiPDSCH_r17 = Omit
    										RelativeTxPower
    											PdschToCell = -3
    											PdschToDmrs = -3
    											PdschToPtrs = -3
    									Sps = Omit
    									SL_Pdcch = Omit
    									NCD_SSPbchBlock = Omit
    							InitialBWP_RedCap = Omit
    						CsiConfig
    							None = True
    					Uplink
    						Uplink
    							Config
    								FrequencyInfoUL
    									R15
    										frequencyBandList = Omit
    										absoluteFrequencyPointA = Omit
    										scs_SpecificCarrierList
    											SCS_SpecificCarrier
    												offsetToCarrier = 0
    												subcarrierSpacing = kHz120 (3)
    												carrierBandwidth = 66
    												txDirectCurrentLocation = Omit
    										additionalSpectrumEmission = 0
    										p_Max = 23
    										frequencyShift7p5khz = Omit
    								BWPs
    									ActiveBWP
    										SameIdAsDL = True
    									BwpArray
    										NR_UplinkBWP_Type
    											Id = 0
    											Common
    												R15
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 149
    																msg1_FDM = one (0)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    																prach_ConfigurationPeriodScaling_IAB_r16 = Omit
    																prach_ConfigurationFrameOffset_IAB_r16 = Omit
    																prach_ConfigurationSOffset_IAB_r16 = Omit
    																ra_ResponseWindow_v1610 = Omit
    																prach_ConfigurationIndex_v1610 = Omit
    																ra_ResponseWindow_v1700 = Omit
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n4 (0)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 32
    															msg1_SubcarrierSpacing = kHz120 (3)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    															ra_PrioritizationForAccessIdentity_r16 = Omit
    															prach_RootSequenceIndex_r16 = Omit
    															ra_PrioritizationForSlicing_r17 = Omit
    															featureCombinationPreamblesList_r17 = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 3
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    															nrofPRBs = Omit
    															intra_SlotFH_r17 = Omit
    															pucch_ResourceCommonRedCap_r17 = Omit
    															additionalPRBOffset_r17 = Omit
    													rach_ConfigCommonIAB_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													msgA_ConfigCommon_r16 = Omit
    													enableRA_PrioritizationForSlicing_r17 = Omit
    													additionalRACH_ConfigList_r17 = Omit
    													rsrp_ThresholdMsg3_r17 = Omit
    													numberOfMsg3_RepetitionsList_r17 = Omit
    													mcs_Msg3_Repetitions_r17 = Omit
    											Dedicated
    												R15
    													pucch_Config
    														setup
    															resourceSetToAddModList
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 0
    																	resourceList
    																		IntegerType = 0
    																		IntegerType = 1
    																		IntegerType = 2
    																		IntegerType = 3
    																		IntegerType = 4
    																		IntegerType = 5
    																		IntegerType = 6
    																		IntegerType = 7
    																	maxPayloadSize = Omit
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 1
    																	resourceList
    																		IntegerType = 8
    																		IntegerType = 9
    																		IntegerType = 10
    																		IntegerType = 11
    																		IntegerType = 12
    																		IntegerType = 13
    																		IntegerType = 14
    																		IntegerType = 15
    																	maxPayloadSize = Omit
    															resourceSetToReleaseList = Omit
    															resourceToAddModList
    																PUCCH_Resource
    																	pucch_ResourceId = 0
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 1
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 2
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 3
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 4
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 5
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 6
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 7
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format1
    																			initialCyclicShift = 0
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    																			timeDomainOCC = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 8
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 9
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 10
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 11
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 12
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 13
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 14
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 60
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 15
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 65
    																	format
    																		format3
    																			nrofPRBs = 1
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    															resourceToReleaseList = Omit
    															format1
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = Omit
    																	maxCodeRate = Omit
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = Omit
    															format2
    																setup
    																	interslotFrequencyHopping = Omit
    																	additionalDMRS = Omit
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format3
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format4 = Omit
    															schedulingRequestResourceToAddModList
    																SchedulingRequestResourceConfig
    																	schedulingRequestResourceId = 1
    																	schedulingRequestID = 0
    																	periodicityAndOffset
    																		sl80 = 9
    																	resource = 6
    															schedulingRequestResourceToReleaseList = Omit
    															multi_CSI_PUCCH_ResourceList = Omit
    															dl_DataToUL_ACK
    																PUCCH_Config___11___oftype = 2
    																PUCCH_Config___11___oftype = 3
    																PUCCH_Config___11___oftype = 4
    																PUCCH_Config___11___oftype = 5
    																PUCCH_Config___11___oftype = 6
    																PUCCH_Config___11___oftype = 7
    																PUCCH_Config___11___oftype = 8
    																PUCCH_Config___11___oftype = 9
    															spatialRelationInfoToAddModList = Omit
    															spatialRelationInfoToReleaseList = Omit
    															pucch_PowerControl
    																deltaF_PUCCH_f0 = 0
    																deltaF_PUCCH_f1 = 0
    																deltaF_PUCCH_f2 = 0
    																deltaF_PUCCH_f3 = 0
    																deltaF_PUCCH_f4 = 0
    																p0_Set = Omit
    																pathlossReferenceRSs
    																	PUCCH_PathlossReferenceRS
    																		pucch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 0
    																twoPUCCH_PC_AdjustmentStates = Omit
    																pathlossReferenceRSs_v1610 = Omit
    															resourceToAddModListExt_v1610 = Omit
    															dl_DataToUL_ACK_r16 = Omit
    															ul_AccessConfigListDCI_1_1_r16 = Omit
    															subslotLengthForPUCCH_r16 = Omit
    															dl_DataToUL_ACK_DCI_1_2_r16 = Omit
    															numberOfBitsForPUCCH_ResourceIndicatorDCI_1_2_r16 = Omit
    															dmrs_UplinkTransformPrecodingPUCCH_r16 = Omit
    															spatialRelationInfoToAddModListSizeExt_v1610 = Omit
    															spatialRelationInfoToReleaseListSizeExt_v1610 = Omit
    															spatialRelationInfoToAddModListExt_v1610 = Omit
    															spatialRelationInfoToReleaseListExt_v1610 = Omit
    															resourceGroupToAddModList_r16 = Omit
    															resourceGroupToReleaseList_r16 = Omit
    															sps_PUCCH_AN_List_r16 = Omit
    															schedulingRequestResourceToAddModListExt_v1610 = Omit
    															format0_r17 = Omit
    															format2Ext_r17 = Omit
    															format3Ext_r17 = Omit
    															format4Ext_r17 = Omit
    															ul_AccessConfigListDCI_1_2_r17 = Omit
    															mappingPattern_r17 = Omit
    															powerControlSetInfoToAddModList_r17 = Omit
    															powerControlSetInfoToReleaseList_r17 = Omit
    															secondTPCFieldDCI_1_1_r17 = Omit
    															secondTPCFieldDCI_1_2_r17 = Omit
    															dl_DataToUL_ACK_r17 = Omit
    															dl_DataToUL_ACK_DCI_1_2_r17 = Omit
    															ul_AccessConfigListDCI_1_1_r17 = Omit
    															schedulingRequestResourceToAddModListExt_v1700 = Omit
    															dmrs_BundlingPUCCH_Config_r17 = Omit
    															dl_DataToUL_ACK_v1700 = Omit
    															dl_DataToUL_ACK_MulticastDCI_Format4_1_r17 = Omit
    															sps_PUCCH_AN_ListMulticast_r17 = Omit
    													pusch_Config
    														setup
    															dataScramblingIdentityPUSCH = Omit
    															txConfig = codebook (0)
    															dmrs_UplinkForPUSCH_MappingTypeA
    																setup
    																	dmrs_Type = Omit
    																	dmrs_AdditionalPosition = pos0 (0)
    																	phaseTrackingRS = Omit
    																	maxLength = Omit
    																	transformPrecodingDisabled
    																		scramblingID0 = Omit
    																		scramblingID1 = Omit
    																		dmrs_Uplink_r16 = Omit
    																	transformPrecodingEnabled = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB = Omit
    															pusch_PowerControl
    																tpc_Accumulation = Omit
    																msg3_Alpha = alpha08 (5)
    																p0_NominalWithoutGrant = -90
    																p0_AlphaSets
    																	P0_PUSCH_AlphaSet
    																		p0_PUSCH_AlphaSetId = 0
    																		p0 = 0
    																		alpha = alpha08 (5)
    																pathlossReferenceRSToAddModList
    																	PUSCH_PathlossReferenceRS
    																		pusch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 0
    																pathlossReferenceRSToReleaseList = Omit
    																twoPUSCH_PC_AdjustmentStates = Omit
    																deltaMCS = Omit
    																sri_PUSCH_MappingToAddModList
    																	SRI_PUSCH_PowerControl
    																		sri_PUSCH_PowerControlId = 0
    																		sri_PUSCH_PathlossReferenceRS_Id = 0
    																		sri_P0_PUSCH_AlphaSetId = 0
    																		sri_PUSCH_ClosedLoopIndex = i0 (0)
    																sri_PUSCH_MappingToReleaseList = Omit
    															frequencyHopping = Omit
    															frequencyHoppingOffsetLists = Omit
    															resourceAllocation = resourceAllocationType1 (1)
    															pusch_TimeDomainAllocationList = Omit
    															pusch_AggregationFactor = Omit
    															mcs_Table = Omit
    															mcs_TableTransformPrecoder = Omit
    															transformPrecoder = Omit
    															codebookSubset = nonCoherent (2)
    															maxRank = 1
    															rbg_Size = Omit
    															uci_OnPUSCH
    																setup
    																	betaOffsets
    																		semiStatic
    																			betaOffsetACK_Index1 = 9
    																			betaOffsetACK_Index2 = 9
    																			betaOffsetACK_Index3 = 9
    																			betaOffsetCSI_Part1_Index1 = 6
    																			betaOffsetCSI_Part1_Index2 = 6
    																			betaOffsetCSI_Part2_Index1 = 6
    																			betaOffsetCSI_Part2_Index2 = 6
    																	scaling = f1 (3)
    															tp_pi2BPSK = Omit
    															minimumSchedulingOffsetK2_r16 = Omit
    															ul_AccessConfigListDCI_0_1_r16 = Omit
    															harq_ProcessNumberSizeDCI_0_2_r16 = Omit
    															dmrs_SequenceInitializationDCI_0_2_r16 = Omit
    															numberOfBitsForRV_DCI_0_2_r16 = Omit
    															antennaPortsFieldPresenceDCI_0_2_r16 = Omit
    															dmrs_UplinkForPUSCH_MappingTypeA_DCI_0_2_r16 = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB_DCI_0_2_r16 = Omit
    															frequencyHoppingDCI_0_2_r16 = Omit
    															frequencyHoppingOffsetListsDCI_0_2_r16 = Omit
    															codebookSubsetDCI_0_2_r16 = Omit
    															invalidSymbolPatternIndicatorDCI_0_2_r16 = Omit
    															maxRankDCI_0_2_r16 = Omit
    															mcs_TableDCI_0_2_r16 = Omit
    															mcs_TableTransformPrecoderDCI_0_2_r16 = Omit
    															priorityIndicatorDCI_0_2_r16 = Omit
    															pusch_RepTypeIndicatorDCI_0_2_r16 = Omit
    															resourceAllocationDCI_0_2_r16 = Omit
    															resourceAllocationType1GranularityDCI_0_2_r16 = Omit
    															uci_OnPUSCH_ListDCI_0_2_r16 = Omit
    															pusch_TimeDomainAllocationListDCI_0_2_r16 = Omit
    															pusch_TimeDomainAllocationListDCI_0_1_r16 = Omit
    															invalidSymbolPatternIndicatorDCI_0_1_r16 = Omit
    															priorityIndicatorDCI_0_1_r16 = Omit
    															pusch_RepTypeIndicatorDCI_0_1_r16 = Omit
    															frequencyHoppingDCI_0_1_r16 = Omit
    															uci_OnPUSCH_ListDCI_0_1_r16 = Omit
    															invalidSymbolPattern_r16 = Omit
    															pusch_PowerControl_v1610 = Omit
    															ul_FullPowerTransmission_r16 = Omit
    															pusch_TimeDomainAllocationListForMultiPUSCH_r16 = Omit
    															numberOfInvalidSymbolsForDL_UL_Switching_r16 = Omit
    															ul_AccessConfigListDCI_0_2_r17 = Omit
    															betaOffsetsCrossPri0_r17 = Omit
    															betaOffsetsCrossPri1_r17 = Omit
    															betaOffsetsCrossPri0DCI_0_2_r17 = Omit
    															betaOffsetsCrossPri1DCI_0_2_r17 = Omit
    															mappingPattern_r17 = Omit
    															secondTPCFieldDCI_0_1_r17 = Omit
    															secondTPCFieldDCI_0_2_r17 = Omit
    															sequenceOffsetForRV_r17 = Omit
    															ul_AccessConfigListDCI_0_1_r17 = Omit
    															minimumSchedulingOffsetK2_r17 = Omit
    															availableSlotCounting_r17 = Omit
    															dmrs_BundlingPUSCH_Config_r17 = Omit
    															harq_ProcessNumberSizeDCI_0_2_v1700 = Omit
    															harq_ProcessNumberSizeDCI_0_1_r17 = Omit
    															mpe_ResourcePoolToAddModList_r17 = Omit
    															mpe_ResourcePoolToReleaseList_r17 = Omit
    													configuredGrantConfig = Omit
    													srs_Config
    														setup
    															srs_ResourceSetToReleaseList = Omit
    															srs_ResourceSetToAddModList
    																SRS_ResourceSet
    																	srs_ResourceSetId = 0
    																	srs_ResourceIdList
    																		IntegerType = 0
    																	resourceType
    																		aperiodic
    																			aperiodicSRS_ResourceTrigger = 1
    																			csi_RS = Omit
    																			slotOffset = 4
    																			aperiodicSRS_ResourceTriggerList = Omit
    																	usage = codebook (1)
    																	alpha = alpha0 (0)
    																	p0 = 0
    																	pathlossReferenceRS
    																		ssb_Index = 0
    																	srs_PowerControlAdjustmentStates = Omit
    																	pathlossReferenceRSList_r16 = Omit
    																	usagePDC_r17 = Omit
    																	availableSlotOffsetList_r17 = Omit
    																	followUnifiedTCI_StateSRS_r17 = Omit
    															srs_ResourceToReleaseList = Omit
    															srs_ResourceToAddModList
    																SRS_Resource
    																	srs_ResourceId = 0
    																	nrofSRS_Ports = port1 (0)
    																	ptrs_PortIndex = Omit
    																	transmissionComb
    																		n2
    																			combOffset_n2 = 0
    																			cyclicShift_n2 = 0
    																	resourceMapping
    																		startPosition = 0
    																		nrofSymbols = n1 (0)
    																		repetitionFactor = n1 (0)
    																	freqDomainPosition = 0
    																	freqDomainShift = 0
    																	freqHopping
    																		c_SRS = 17
    																		b_SRS = 0
    																		b_hop = 0
    																	groupOrSequenceHopping = groupHopping (1)
    																	resourceType
    																		aperiodic
    																	sequenceId = 0
    																	spatialRelationInfo
    																		servingCellId = Omit
    																		referenceSignal
    																			ssb_Index = 0
    																	resourceMapping_r16 = Omit
    																	spatialRelationInfo_PDC_r17 = Omit
    																	resourceMapping_r17 = Omit
    																	partialFreqSounding_r17 = Omit
    																	transmissionComb_n8_r17 = Omit
    																	srs_TCI_State_r17 = Omit
    																	repetitionFactor_v1730 = Omit
    																	srs_DLorJointTCI_State_v1730 = Omit
    															tpc_Accumulation = Omit
    															srs_RequestDCI_1_2_r16 = Omit
    															srs_RequestDCI_0_2_r16 = Omit
    															srs_ResourceSetToAddModListDCI_0_2_r16 = Omit
    															srs_ResourceSetToReleaseListDCI_0_2_r16 = Omit
    															srs_PosResourceSetToReleaseList_r16 = Omit
    															srs_PosResourceSetToAddModList_r16 = Omit
    															srs_PosResourceToReleaseList_r16 = Omit
    															srs_PosResourceToAddModList_r16 = Omit
    													beamFailureRecoveryConfig = Omit
    													sl_PUCCH_Config_r16 = Omit
    													cp_ExtensionC2_r16 = Omit
    													cp_ExtensionC3_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													pucch_ConfigurationList_r16 = Omit
    													lbt_FailureRecoveryConfig_r16 = Omit
    													configuredGrantConfigToAddModList_r16 = Omit
    													configuredGrantConfigToReleaseList_r16 = Omit
    													configuredGrantConfigType2DeactivationStateList_r16 = Omit
    													ul_TCI_StateList_r17 = Omit
    													ul_powerControl_r17 = Omit
    													pucch_ConfigurationListMulticast1_r17 = Omit
    													pucch_ConfigurationListMulticast2_r17 = Omit
    													pucch_ConfigMulticast1_r17 = Omit
    													pucch_ConfigMulticast2_r17 = Omit
    													pathlossReferenceRSToAddModList_r17 = Omit
    													pathlossReferenceRSToReleaseList_r17 = Omit
    									InitialBWP_RedCap = Omit
    								RACH_ConfigDedicated = Omit
    								SI_RequestConfig = Omit
    						SupplementaryUplink = Omit
    						TimingAdvance
    							InitialValue = 0
    						PUSCH_ServingCellConfig
    							R15
    								codeBlockGroupTransmission = Omit
    								rateMatching = Omit
    								xOverhead = Omit
    								maxMIMO_Layers = Omit
    								processingType2Enabled = Omit
    								maxMIMO_LayersDCI_0_2_r16 = Omit
    								nrofHARQ_ProcessesForPUSCH_r17 = Omit
    								uplinkHARQ_mode_r17 = Omit
    						PUSCH_ServingCellConfigSUL = Omit
    				BcchConfig
    					Pbch = True
    					Pdsch
    						Sib1Schedul
    							SearchSpaceAndDci
    								AssignedBWPs
    									ActiveBWP = Omit
    									InitialBWP = True
    									DedicatedBWPs
    									InitialBWP_RedCap = Omit
    								SearchSpaceType = cssType0 (0)
    								DciInfo
    									ResoureAssignment
    										ResourceAllocationType = resourceAllocationType1 (1)
    										FreqDomain
    											Automatic
    												FirstRbIndex = 17
    												MaxRbCnt = 7
    										TimeDomain
    											Index = 0000'B
    										TransportBlockScheduling
    											Automatic
    												TransportBlock1 = qpsk (0)
    												TransportBlock2 = Omit
    												RedundancyVersionList
    													NR_RedundancyVersion_Type = 0
    										HarqProcessConfig
    											Broadcast = True
    									VrbPrbMapping
    										Index = 0'B
    									Format
    										Format_1_0_SI_RNTI
    											SystemInfoIndicator = 0'B
    							Periodicity = 20
    							SlotOffsetList
    								IntegerType = 1
    						SiSchedul
    							WindowLength = s160 (5)
    							SiList
    								NR_OtherSiSchedul_Type
    									Periodicity = rf32 (2)
    									Window
    										NR_SingleSiSchedul_Type
    											SearchSpaceAndDci
    												AssignedBWPs
    													ActiveBWP = Omit
    													InitialBWP = True
    													DedicatedBWPs
    													InitialBWP_RedCap = Omit
    												SearchSpaceType = cssType0A (1)
    												DciInfo
    													ResoureAssignment
    														ResourceAllocationType = resourceAllocationType1 (1)
    														FreqDomain
    															Automatic
    																FirstRbIndex = 17
    																MaxRbCnt = 7
    														TimeDomain
    															Index = 0000'B
    														TransportBlockScheduling
    															Automatic
    																TransportBlock1 = qpsk (0)
    																TransportBlock2 = Omit
    																RedundancyVersionList
    																	NR_RedundancyVersion_Type = 0
    														HarqProcessConfig
    															Broadcast = True
    													VrbPrbMapping
    														Index = 0'B
    													Format
    														Format_1_0_SI_RNTI
    															SystemInfoIndicator = 1'B
    											SlotOffset = 5
    							SegmentedSiList = Omit
    							PosSiSchedulInfo = Omit
    					BcchInfo
    						MIB
    							message_
    								mib
    									systemFrameNumber = 000000'B
    									subCarrierSpacingCommon = scs30or120 (1)
    									ssb_SubcarrierOffset = 10
    									dmrs_TypeA_Position = pos2 (0)
    									pdcch_ConfigSIB1
    										controlResourceSetZero = 1
    										searchSpaceZero = 0
    									cellBarred = notBarred (1)
    									intraFreqReselection = allowed (0)
    									spare = 0'B
    						SIB1
    							message_
    								c1
    									systemInformationBlockType1
    										cellSelectionInfo
    											q_RxLevMin = -57
    											q_RxLevMinOffset = Omit
    											q_RxLevMinSUL = Omit
    											q_QualMin = Omit
    											q_QualMinOffset = Omit
    										cellAccessRelatedInfo
    											plmn_IdentityInfoList
    												PLMN_IdentityInfo
    													plmn_IdentityList
    														PLMN_Identity
    															mcc
    																IntegerType = 0
    																IntegerType = 0
    																IntegerType = 1
    															mnc
    																IntegerType = 0
    																IntegerType = 1
    													trackingAreaCode = 000000000000000000000001'B
    													ranac = 1
    													cellIdentity = 000000000000000000000000010000000010'B
    													cellReservedForOperatorUse = notReserved (1)
    													iab_Support_r16 = Omit
    													trackingAreaList_r17 = Omit
    													gNB_ID_Length_r17 = Omit
    											cellReservedForOtherUse = Omit
    											cellReservedForFutureUse_r16 = Omit
    											npn_IdentityInfoList_r16 = Omit
    											snpn_AccessInfoList_r17 = Omit
    										connEstFailureControl
    											connEstFailCount = n1 (0)
    											connEstFailOffsetValidity = s30 (0)
    											connEstFailOffset = 1
    										si_SchedulingInfo
    											schedulingInfoList
    												SchedulingInfo
    													si_BroadcastStatus = broadcasting (0)
    													si_Periodicity = rf32 (2)
    													sib_MappingInfo
    														SIB_TypeInfo
    															type_ = sibType2 (0)
    															valueTag = 0
    															areaScope = Omit
    											si_WindowLength = s160 (5)
    											si_RequestConfig = Omit
    											si_RequestConfigSUL = Omit
    											systemInformationAreaID = 000000000000000000000001'B
    										servingCellConfigCommon
    											downlinkConfigCommon
    												frequencyInfoDL
    													frequencyBandList
    														NR_MultiBandInfo
    															freqBandIndicatorNR = 257
    															nr_NS_PmaxList
    																NR_NS_PmaxValue
    																	additionalPmax = Omit
    																	additionalSpectrumEmission = 0
    													offsetToPointA = 18
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz120 (3)
    															carrierBandwidth = 66
    															txDirectCurrentLocation = Omit
    												initialDownlinkBWP
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													pdcch_ConfigCommon
    														setup
    															controlResourceSetZero = 1
    															commonControlResourceSet = Omit
    															searchSpaceZero = Omit
    															commonSearchSpaceList
    																SearchSpace
    																	searchSpaceId = 1
    																	controlResourceSetId = 0
    																	monitoringSlotPeriodicityAndOffset
    																		sl1 = Null
    																	duration = Omit
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n3 (3)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n1 (1)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    																SearchSpace
    																	searchSpaceId = 3
    																	controlResourceSetId = 0
    																	monitoringSlotPeriodicityAndOffset
    																		sl10 = 5
    																	duration = 2
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n3 (3)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n1 (1)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    															searchSpaceSIB1 = 0
    															searchSpaceOtherSystemInformation = 3
    															pagingSearchSpace = 0
    															ra_SearchSpace = 1
    															firstPDCCH_MonitoringOccasionOfPO = Omit
    															commonSearchSpaceListExt_r16 = Omit
    															sdt_SearchSpace_r17 = Omit
    															searchSpaceMCCH_r17 = Omit
    															searchSpaceMTCH_r17 = Omit
    															commonSearchSpaceListExt2_r17 = Omit
    															firstPDCCH_MonitoringOccasionOfPO_v1710 = Omit
    															pei_ConfigBWP_r17 = Omit
    															followUnifiedTCI_State_v1720 = Omit
    													pdsch_ConfigCommon
    														setup
    															pdsch_TimeDomainAllocationList
    																PDSCH_TimeDomainResourceAllocation
    																	k0 = Omit
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 53
    												bcch_Config
    													modificationPeriodCoeff = n4 (1)
    												pcch_Config
    													defaultPagingCycle = rf128 (2)
    													nAndPagingFrameOffset
    														halfT = 0
    													ns = one (2)
    													firstPDCCH_MonitoringOccasionOfPO = Omit
    													nrofPDCCH_MonitoringOccasionPerSSB_InPO_r16 = Omit
    													ranPagingInIdlePO_r17 = Omit
    													firstPDCCH_MonitoringOccasionOfPO_v1710 = Omit
    												pei_Config_r17 = Omit
    												initialDownlinkBWP_RedCap_r17 = Omit
    											uplinkConfigCommon
    												frequencyInfoUL
    													frequencyBandList = Omit
    													absoluteFrequencyPointA = Omit
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz120 (3)
    															carrierBandwidth = 66
    															txDirectCurrentLocation = Omit
    													p_Max = 23
    													frequencyShift7p5khz = Omit
    												initialUplinkBWP
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 149
    																msg1_FDM = one (0)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    																prach_ConfigurationPeriodScaling_IAB_r16 = Omit
    																prach_ConfigurationFrameOffset_IAB_r16 = Omit
    																prach_ConfigurationSOffset_IAB_r16 = Omit
    																ra_ResponseWindow_v1610 = Omit
    																prach_ConfigurationIndex_v1610 = Omit
    																ra_ResponseWindow_v1700 = Omit
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n4 (0)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 32
    															msg1_SubcarrierSpacing = kHz120 (3)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    															ra_PrioritizationForAccessIdentity_r16 = Omit
    															prach_RootSequenceIndex_r16 = Omit
    															ra_PrioritizationForSlicing_r17 = Omit
    															featureCombinationPreamblesList_r17 = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 3
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    															nrofPRBs = Omit
    															intra_SlotFH_r17 = Omit
    															pucch_ResourceCommonRedCap_r17 = Omit
    															additionalPRBOffset_r17 = Omit
    													rach_ConfigCommonIAB_r16 = Omit
    													useInterlacePUCCH_PUSCH_r16 = Omit
    													msgA_ConfigCommon_r16 = Omit
    													enableRA_PrioritizationForSlicing_r17 = Omit
    													additionalRACH_ConfigList_r17 = Omit
    													rsrp_ThresholdMsg3_r17 = Omit
    													numberOfMsg3_RepetitionsList_r17 = Omit
    													mcs_Msg3_Repetitions_r17 = Omit
    												timeAlignmentTimerCommon = infinity_ (7)
    											supplementaryUplink = Omit
    											n_TimingAdvanceOffset = Omit
    											ssb_PositionsInBurst
    												inOneGroup = 10000000'B
    												groupPresence = 10000000'B
    											ssb_PeriodicityServingCell = ms20 (2)
    											tdd_UL_DL_ConfigurationCommon
    												referenceSubcarrierSpacing = kHz120 (3)
    												pattern1
    													dl_UL_TransmissionPeriodicity = ms0p625 (1)
    													nrofDownlinkSlots = 3
    													nrofDownlinkSymbols = 10
    													nrofUplinkSlots = 1
    													nrofUplinkSymbols = 2
    													dl_UL_TransmissionPeriodicity_v1530 = Omit
    												pattern2 = Omit
    											ss_PBCH_BlockPower = 0
    											channelAccessMode_r16 = Omit
    											discoveryBurstWindowLength_r16 = Omit
    											highSpeedConfig_r16 = Omit
    											channelAccessMode2_r17 = Omit
    											discoveryBurstWindowLength_v1700 = Omit
    											highSpeedConfigFR2_r17 = Omit
    											uplinkConfigCommon_v1700 = Omit
    											enhancedMeasurementLEO_r17 = Omit
    											ra_ChannelAccess_r17 = Omit
    										ims_EmergencySupport = true_ (0)
    										eCallOverIMS_Support = Omit
    										ue_TimersAndConstants
    											t300 = ms1000 (5)
    											t301 = ms1000 (5)
    											t310 = ms1000 (5)
    											n310 = n1 (0)
    											t311 = ms30000 (6)
    											n311 = n1 (0)
    											t319 = ms1000 (5)
    										uac_BarringInfo = Omit
    										useFullResumeID = Omit
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											idleModeMeasurementsEUTRA_r16 = Omit
    											idleModeMeasurementsNR_r16 = Omit
    											posSI_SchedulingInfo_r16 = Omit
    											nonCriticalExtension
    												uac_BarringInfo_v1630 = Omit
    												nonCriticalExtension
    													hsdn_Cell_r17 = Omit
    													uac_BarringInfo_v1700 = Omit
    													sdt_ConfigCommon_r17 = Omit
    													redCap_ConfigCommon_r17 = Omit
    													featurePriorities_r17 = Omit
    													si_SchedulingInfo_v1700 = Omit
    													hyperSFN_r17 = Omit
    													eDRX_AllowedIdle_r17 = Omit
    													eDRX_AllowedInactive_r17 = Omit
    													intraFreqReselectionRedCap_r17 = Omit
    													cellBarredNTN_r17 = Omit
    													nonCriticalExtension = Omit
    						SIs
    							BCCH_DL_SCH_Message
    								message_
    									c1
    										systemInformation
    											criticalExtensions
    												systemInformation
    													sib_TypeAndInfo
    														SystemInformation_IEs___0___oftype
    															sib2
    																cellReselectionInfoCommon
    																	nrofSS_BlocksToAverage = 2
    																	absThreshSS_BlocksConsolidation
    																		thresholdRSRP = 0
    																		thresholdRSRQ = Omit
    																		thresholdSINR = Omit
    																	rangeToBestCell = dB0 (15)
    																	q_Hyst = dB0 (0)
    																	speedStateReselectionPars = Omit
    																cellReselectionServingFreqInfo
    																	s_NonIntraSearchP = Omit
    																	s_NonIntraSearchQ = Omit
    																	threshServingLowP = 0
    																	threshServingLowQ = Omit
    																	cellReselectionPriority = 4
    																	cellReselectionSubPriority = Omit
    																intraFreqCellReselectionInfo
    																	q_RxLevMin = -55
    																	q_RxLevMinSUL = Omit
    																	q_QualMin = Omit
    																	s_IntraSearchP = 31
    																	s_IntraSearchQ = Omit
    																	t_ReselectionNR = 0
    																	frequencyBandList = Omit
    																	frequencyBandListSUL = Omit
    																	p_Max = Omit
    																	smtc
    																		periodicityAndOffset
    																			sf20 = 0
    																		duration = sf3 (2)
    																	ss_RSSI_Measurement = Omit
    																	ssb_ToMeasure
    																		longBitmap = 1100000000000000000000000000000000000000000000000000000000000000'B
    																	deriveSSB_IndexFromCell = True
    																	t_ReselectionNR_SF = Omit
    																	smtc2_LP_r16 = Omit
    																	ssb_PositionQCL_Common_r16 = Omit
    																	ssb_PositionQCL_Common_r17 = Omit
    																	smtc4list_r17 = Omit
    																relaxedMeasurement_r16 = Omit
    																cellEquivalentSize_r17 = Omit
    																relaxedMeasurement_r17 = Omit
    													lateNonCriticalExtension = Omit
    													nonCriticalExtension = Omit
    						SegmentedSIs = Omit
    						PosSIs = Omit
    						NCD_MIBs = Omit
    				PcchConfig
    					SearchSpaceAndDci
    						AssignedBWPs
    							ActiveBWP = Omit
    							InitialBWP = True
    							DedicatedBWPs
    							InitialBWP_RedCap = Omit
    						SearchSpaceType = cssType2 (3)
    						DciInfo
    							ResoureAssignment
    								ResourceAllocationType = resourceAllocationType1 (1)
    								FreqDomain
    									Automatic
    										FirstRbIndex = 0
    										MaxRbCnt = 17
    								TimeDomain
    									Index = 0000'B
    								TransportBlockScheduling
    									Automatic
    										TransportBlock1 = qpsk (0)
    										TransportBlock2 = Omit
    										RedundancyVersionList
    								HarqProcessConfig
    									None = True
    							VrbPrbMapping
    								Index = 0'B
    							Format
    								Format_1_0_P_RNTI
    									ShortMessageIndicator = 01'B
    									ShortMessages = 00000000'B
    									TbScaling = 00'B
    									TrsAvailabilityIndication
    										None = True
    				RachProcedureConfig
    					RachProcedureList
    						NR_RachProcedure_Type
    							MsgB = Omit
    							RandomAccessResponse
    								SearchSpaceAndDci
    									AssignedBWPs
    										ActiveBWP = Omit
    										InitialBWP = True
    										DedicatedBWPs
    										InitialBWP_RedCap = Omit
    									SearchSpaceType = cssType1 (2)
    									DciInfo
    										ResoureAssignment
    											ResourceAllocationType = resourceAllocationType1 (1)
    											FreqDomain
    												Automatic
    													FirstRbIndex = 0
    													MaxRbCnt = 17
    											TimeDomain
    												Index = 0000'B
    											TransportBlockScheduling
    												Automatic
    													TransportBlock1 = qpsk (0)
    													TransportBlock2 = Omit
    													RedundancyVersionList
    											HarqProcessConfig
    												None = True
    										VrbPrbMapping
    											Index = 0'B
    										Format
    											Format_1_0_RA_RNTI
    												TbScaling = 00'B
    												LSBsOfSFN
    													None = True
    								MacPdu
    									SubPduList
    										NR_RAR_SubPdu_Type
    											RapIdAndPayload
    												RapId
    													Automatic = True
    												Payload
    													TimingAdvance = 0
    													UplinkGrant
    														HoppingFlag = 0'B
    														Msg3FrequencyResourceAllocation = 00000100001000'B
    														Msg3TimeResourceAllocation = 0001'B
    														MCS = 0010'B
    														TPC_Command = 011'B
    														CQI_Req = 0'B
    													TempC_RNTI
    														SameAsC_RNTI = True
    									CrcError = False
    							ContentionResolution
    								Msg4_Based
    									SearchSpaceAndDci
    										AssignedBWPs
    											ActiveBWP = Omit
    											InitialBWP = True
    											DedicatedBWPs
    											InitialBWP_RedCap = Omit
    										SearchSpaceType = cssType1 (2)
    										DciInfo
    											ResoureAssignment
    												ResourceAllocationType = resourceAllocationType1 (1)
    												FreqDomain
    													Automatic
    														FirstRbIndex = 0
    														MaxRbCnt = 17
    												TimeDomain
    													Index = 0000'B
    												TransportBlockScheduling
    													Automatic
    														TransportBlock1 = qam64 (2)
    														TransportBlock2 = Omit
    														RedundancyVersionList
    															NR_RedundancyVersion_Type = 0
    															NR_RedundancyVersion_Type = 2
    															NR_RedundancyVersion_Type = 3
    															NR_RedundancyVersion_Type = 1
    															NR_RedundancyVersion_Type = 0
    												HarqProcessConfig
    													AnyProcess = True
    											VrbPrbMapping
    												Index = 0'B
    											Format
    												Format_1_0
    													DAI
    														Index
    															Automatic = True
    													TpcCommandPucch
    														Value = 01'B
    													PucchResourceIndicator
    														Value = 110'B
    													PdschHarqTimingIndicator
    														Value = 111'B
    													ChannelAccessCPext
    														None = True
    									ContentionResolutionId
    										XorMask = 000000000000000000000000000000000000000000000000'B
    									RrcPdu
    										RrcCcchMsg = '204004069AE0048020C3CC00F80200D07800020D62EA000808012D80DA8000F8000000000183708420000D116D000000122440000081A74001000266AAE92838002081840A1839388122858C1A3878FC000082021810010404B04002080A60C0041016C200082031850010406B0C002080E61C00412140310001E258624003C4B2C5000789698B000F12DB18001E25C634003C4BAC7000789798F001058506092BCA18162437234567897D4210840004D01A4901E2AE00C10A00000018FFD29498C637281E000020D1940002000000000882000000848000'O
    									CrcError = False
    				DcchDtchConfig
    					DL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    								InitialBWP_RedCap = Omit
    							SearchSpaceType = ussDL (6)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										Automatic
    											FirstRbIndex = 0
    											MaxRbCnt = 17
    									TimeDomain
    										Index = 'B
    									TransportBlockScheduling
    										Automatic
    											TransportBlock1 = qam64 (2)
    											TransportBlock2 = Omit
    											RedundancyVersionList
    												NR_RedundancyVersion_Type = 0
    												NR_RedundancyVersion_Type = 2
    												NR_RedundancyVersion_Type = 3
    												NR_RedundancyVersion_Type = 1
    												NR_RedundancyVersion_Type = 0
    									HarqProcessConfig
    										AnyProcess = True
    								VrbPrbMapping
    									None = True
    								Format
    									Format_1_1
    										CarrierIndicator
    											None = True
    										BWPIndicator
    											Index = 'B
    										PrbBundlingSizeIndicator
    											None = True
    										RateMatchingIndicator
    											Bitmap = 'B
    										ZP_CSI_RS_Trigger
    											Index = 'B
    										DAI
    											TwoBits
    												Automatic = True
    										TpcCommandPucch
    											Value = 01'B
    										SecondTpcCommand
    											None = True
    										PucchResourceIndicator
    											Value = 110'B
    										PdschHarqTimingIndicator
    											Value = 110'B
    										OneShotHarqAckRequest
    											None = True
    										EnhancedType3CodebookIndicator
    											None = True
    										PdschGroupIndex
    											None = True
    										NewFeedbackIndicator
    											None = True
    										NumberRequestedPdschGroup
    											None = True
    										HarqAckRetransmissionIndicator
    											None = True
    										AntennaPorts
    											Index = 0000'B
    										TCI
    											None = True
    										SrsRequest
    											SingleUL = 00'B
    										SrsOffsetIndicator
    											None = True
    										CBGTI
    											Bitmap = 'B
    										CBGFI
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    										PriorityIndicator
    											None = True
    										ChannelAccessCPext
    											None = True
    										MinimumApplicableSchedulingOffset
    											None = True
    										SCellDormancyIndication
    											None = True
    										PdcchMonitoringAdaptationIndication
    											None = True
    										PucchCellIndicator
    											None = True
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    								InitialBWP_RedCap = Omit
    							SearchSpaceType = ussUL (7)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain
    										Index = 0'B
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig
    										AnyProcess = True
    								PuschHoppingCtrl
    									None = True
    								TpcCommandPusch
    									Value = 01'B
    								UL_SUL_Indicator
    									None = True
    								Format
    									Format_0_1
    										CarrierIndicator
    											None = True
    										DfiFlag
    											None = True
    										BWPIndicator
    											Index = 'B
    										FirstDAI
    											DynamicCodebook
    												Automatic = True
    										SecondDAI
    											None = True
    										ThirdDAI
    											None = True
    										SecondTpcCommandPusch
    											None = True
    										SrsResourceSetIndicator
    											None = True
    										SrsResourceIndicator
    											CodeBook = 'B
    										SecondSrsResourceIndicator
    											None = True
    										PrecodingInfo
    											CodeBook = 'B
    										SecondPrecodingInfo
    											None = True
    										AntennaPorts
    											Index = 000'B
    										SrsRequest
    											SingleUL = 00'B
    										SrsOffsetIndicator
    											None = True
    										CsiRequest
    											Index = 'B
    										CBGTI
    											Index = 'B
    										PtrsDmrsAssociation
    											None = True
    										SecondPtrsDmrsAssociation
    											None = True
    										BetaOffsetIndicator
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    										UlschIndicator
    											Value = 1'B
    										ChannelAccessCPextCAPC
    											None = True
    										OpenLoopPowerControl
    											None = True
    										PriorityIndicator
    											None = True
    										InvalidSymbolPatternIndicator
    											None = True
    										MinimumApplicableSchedulingOffset
    											None = True
    										SCellDormancyIndication
    											None = True
    										SidelinkAssignmentIndex
    											None = True
    										PdcchMonitoringAdaptationIndication
    											None = True
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl
    						None = True
    					MeasGapCtrl
    						None = True
    				ServingCellConfig
    					SpCell
    						ServingCellIndex = 0
    						CellGroupConfig
    							CellGroupId = 0
    							SCellList
    							MAC_CellGroupConfig
    								R15
    									drx_Config = Omit
    									schedulingRequestConfig
    										schedulingRequestToAddModList
    											SchedulingRequestToAddMod
    												schedulingRequestId = 0
    												sr_ProhibitTimer = Omit
    												sr_TransMax = n16 (2)
    										schedulingRequestToReleaseList = Omit
    									bsr_Config
    										periodicBSR_Timer = sf1 (0)
    										retxBSR_Timer = sf80 (3)
    										logicalChannelSR_DelayTimer = Omit
    									tag_Config
    										tag_ToReleaseList = Omit
    										tag_ToAddModList
    											TAG
    												tag_Id = 0
    												timeAlignmentTimer = infinity_ (7)
    									phr_Config
    										setup
    											phr_PeriodicTimer = sf10 (0)
    											phr_ProhibitTimer = sf0 (0)
    											phr_Tx_PowerFactorChange = dB1 (0)
    											multiplePHR = False
    											dummy = False
    											phr_Type2OtherCell = False
    											phr_ModeOtherCG = real (0)
    											mpe_Reporting_FR2_r16 = Omit
    											mpe_Reporting_FR2_r17 = Omit
    											twoPHRMode_r17 = Omit
    									skipUplinkTxDynamic = False
    									csi_Mask = Omit
    									dataInactivityTimer = Omit
    									usePreBSR_r16 = Omit
    									schedulingRequestID_LBT_SCell_r16 = Omit
    									lch_BasedPrioritization_r16 = Omit
    									schedulingRequestID_BFR_SCell_r16 = Omit
    									drx_ConfigSecondaryGroup_r16 = Omit
    									enhancedSkipUplinkTxDynamic_r16 = Omit
    									enhancedSkipUplinkTxConfigured_r16 = Omit
    									intraCG_Prioritization_r17 = Omit
    									drx_ConfigSL_r17 = Omit
    									drx_ConfigExt_v1700 = Omit
    									schedulingRequestID_BFR_r17 = Omit
    									schedulingRequestID_BFR2_r17 = Omit
    									schedulingRequestConfig_v1700 = Omit
    									tar_Config_r17 = Omit
    									g_RNTI_ConfigToAddModList_r17 = Omit
    									g_RNTI_ConfigToReleaseList_r17 = Omit
    									g_CS_RNTI_ConfigToAddModList_r17 = Omit
    									g_CS_RNTI_ConfigToReleaseList_r17 = Omit
    									allowCSI_SRS_Tx_MulticastDRX_Active_r17 = Omit
    									schedulingRequestID_PosMG_Request_r17 = Omit
    									drx_LastTransmissionUL_r17 = Omit
    									posMG_Request_r17 = Omit
    							PhysicalCellGroupConfig
    								R15
    									harq_ACK_SpatialBundlingPUCCH = Omit
    									harq_ACK_SpatialBundlingPUSCH = Omit
    									p_NR_FR1 = 23
    									pdsch_HARQ_ACK_Codebook = dynamic (1)
    									tpc_SRS_RNTI = Omit
    									tpc_PUCCH_RNTI = Omit
    									tpc_PUSCH_RNTI = Omit
    									sp_CSI_RNTI = Omit
    									cs_RNTI = Omit
    									mcs_C_RNTI = Omit
    									p_UE_FR1 = Omit
    									xScale = Omit
    									pdcch_BlindDetection = Omit
    									dcp_Config_r16 = Omit
    									harq_ACK_SpatialBundlingPUCCH_secondaryPUCCHgroup_r16 = Omit
    									harq_ACK_SpatialBundlingPUSCH_secondaryPUCCHgroup_r16 = Omit
    									pdsch_HARQ_ACK_Codebook_secondaryPUCCHgroup_r16 = Omit
    									p_NR_FR2_r16 = Omit
    									p_UE_FR2_r16 = Omit
    									nrdc_PCmode_FR1_r16 = Omit
    									nrdc_PCmode_FR2_r16 = Omit
    									pdsch_HARQ_ACK_Codebook_r16 = Omit
    									nfi_TotalDAI_Included_r16 = Omit
    									ul_TotalDAI_Included_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedback_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedbackNDI_r16 = Omit
    									pdsch_HARQ_ACK_OneShotFeedbackCBG_r16 = Omit
    									downlinkAssignmentIndexDCI_0_2_r16 = Omit
    									downlinkAssignmentIndexDCI_1_2_r16 = Omit
    									pdsch_HARQ_ACK_CodebookList_r16 = Omit
    									ackNackFeedbackMode_r16 = Omit
    									pdcch_BlindDetectionCA_CombIndicator_r16 = Omit
    									pdcch_BlindDetection2_r16 = Omit
    									pdcch_BlindDetection3_r16 = Omit
    									bdFactorR_r16 = Omit
    									pdsch_HARQ_ACK_EnhType3ToAddModList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3ToReleaseList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3SecondaryToAddModList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3SecondaryToReleaseList_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3DCI_FieldSecondaryPUCCHgroup_r17 = Omit
    									pdsch_HARQ_ACK_EnhType3DCI_Field_r17 = Omit
    									pdsch_HARQ_ACK_Retx_r17 = Omit
    									pdsch_HARQ_ACK_RetxSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCell_r17 = Omit
    									pucch_sSCellSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCellDyn_r17 = Omit
    									pucch_sSCellDynSecondaryPUCCHgroup_r17 = Omit
    									pucch_sSCellPattern_r17 = Omit
    									pucch_sSCellPatternSecondaryPUCCHgroup_r17 = Omit
    									uci_MuxWithDiffPrio_r17 = Omit
    									uci_MuxWithDiffPrioSecondaryPUCCHgroup_r17 = Omit
    									simultaneousPUCCH_PUSCH_r17 = Omit
    									simultaneousPUCCH_PUSCH_SecondaryPUCCHgroup_r17 = Omit
    									prioLowDG_HighCG_r17 = Omit
    									prioHighDG_LowCG_r17 = Omit
    									twoQCLTypeDforPDCCHRepetition_r17 = Omit
    									multicastConfig_r17 = Omit
    									pdcch_BlindDetectionCA_CombIndicator_r17 = Omit
    									simultaneousSR_PUSCH_diffPUCCH_Groups_r17 = Omit
    									intraBandNC_PRACH_simulTx_r17 = Omit
    									pdcch_BlindDetection4_r17 = Omit
    				SidelinkScheduled = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell2 (2)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell2 (2)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 0
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										TM = True
    									TestMode
    										None = True
    								LogicalChannelId = Omit
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell2 (2)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 0
    				TimingInfo = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    IMS_IPCAN_Coordination_MSG
    	IPCAN_IMS_Control
    		Reset = WithCNF (0)

    IMS_IPCAN_Coordination_MSG
    	TriggerEvent
    		Reason = ''

    IP_ConfigReq_Type
    	RestoreRoutingTable = True

    IP_Indication_Type
    	Cnf = True

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    UT_COMMON_CMD
    	Cmd = SWITCH_ON (137)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_ON'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = randomValue = 101001011011011100010011011010010000011
    			establishmentCause = mo-Signalling
    			spare = 0

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 473
    				Subframe
    					Number = 8
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								randomValue = 101001011011011100010011011010010000011'B
    							establishmentCause = mo_Signalling (3)
    							spare = 0'B

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 473
    				Subframe
    					Number = 8
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									randomValue = 101001011011011100010011011010010000011'B
    								establishmentCause = mo_Signalling (3)
    								spare = 0'B
    		Nas = Omit

    REGISTRATION REQUEST
    	Extended protocol discriminator [8 bits] = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	fivegs_mm_mt [8 bits] = 0x41 [ 65 ]
    	ngKSI
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x7 [ 7 ]
    	5GS registration type
    		for_f [1 bit] = 0x1 [ 1 ]
    		s_val [3 bits] = 0x1 [ 1 ]
    	5GS mobile identity
    		iel [16 bits] = 0xB [ 11 ]
    		Identity digit [4 bits] = 0xF [ 15 ]
    		Spare bit [1 bit] = 0x0 [ 0 ]
    		fivegs_typ_id [3 bits] = 0x2 [ 2 ]
    		MCC digit 2 [4 bits] = 0x0 [ 0 ]
    		MCC digit 1 [4 bits] = 0x0 [ 0 ]
    		MNC digit 3 [4 bits] = 0xF [ 15 ]
    		MCC digit 3 [4 bits] = 0x1 [ 1 ]
    		MNC digit 2 [4 bits] = 0x1 [ 1 ]
    		MNC digit 1 [4 bits] = 0x0 [ 0 ]
    		AMF Region ID = 0xFE [ 254 ]
    		AMF Set ID = 0x00 [ 0 ]
    		AMF Set ID (continued) [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	UE security capability
    		iei [8 bits] = 0x2E [ 46 ]
    		iel [8 bits] = 0x2 [ 2 ]
    		ea0_128 [1 bit] = 0x1 [ 1 ]
    		ea1_128 [1 bit] = 0x1 [ 1 ]
    		ea2_128 [1 bit] = 0x1 [ 1 ]
    		ea3 [1 bit] = 0x1 [ 1 ]
    		ea4 [1 bit] = 0x0 [ 0 ]
    		ea5 [1 bit] = 0x0 [ 0 ]
    		ea6 [1 bit] = 0x0 [ 0 ]
    		ea7 [1 bit] = 0x0 [ 0 ]
    		ia0 [1 bit] = 0x0 [ 0 ]
    		ia1_128 [1 bit] = 0x1 [ 1 ]
    		ia2_128 [1 bit] = 0x1 [ 1 ]
    		ia3 [1 bit] = 0x1 [ 1 ]
    		ia4 [1 bit] = 0x0 [ 0 ]
    		ia5 [1 bit] = 0x0 [ 0 ]
    		ia6 [1 bit] = 0x0 [ 0 ]
    		ia7 [1 bit] = 0x0 [ 0 ]

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			registeredAMF
    				amf-Identifier = 111111100000000001000001
    			guami-Type = native
    			dedicatedNAS-Message = 7E004179000BF200F110FE0041C23456782E02F070
    			nonCriticalExtension
    				nonCriticalExtension
    					ul-RRC-Segmentation-r16 = true

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 475
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF
    									plmn_Identity = Omit
    									amf_Identifier = 111111100000000001000001'B
    								guami_Type = native (0)
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E004179000BF200F110FE0041C23456782E02F070'O
    								ng_5G_S_TMSI_Value = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									iab_NodeIndication_r16 = Omit
    									idleMeasAvailable_r16 = Omit
    									ue_MeasurementsAvailable_r16 = Omit
    									mobilityHistoryAvail_r16 = Omit
    									mobilityState_r16 = Omit
    									nonCriticalExtension
    										ul_RRC_Segmentation_r16 = true_ (0)
    										nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 475
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF
    										plmn_Identity = Omit
    										amf_Identifier = 111111100000000001000001'B
    									guami_Type = native (0)
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E004179000BF200F110FE0041C23456782E02F070'O
    									ng_5G_S_TMSI_Value = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										iab_NodeIndication_r16 = Omit
    										idleMeasAvailable_r16 = Omit
    										ue_MeasurementsAvailable_r16 = Omit
    										mobilityHistoryAvail_r16 = Omit
    										mobilityState_r16 = Omit
    										nonCriticalExtension
    											ul_RRC_Segmentation_r16 = true_ (0)
    											nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0000'B
    					NasCount = '00FFFFFF'O
    				Pdu
    					Msg
    						registration_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000001'B
    							ngNasKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 111'B
    							registrationType
    								fOR = 1'B
    								registrationType = 001'B
    							ngMobileId
    								iei = Omit
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    							nonCurrentNativeKSI = Omit
    							gmmCapability = Omit
    							ueSecurityCapability
    								iei = '2E'O
    								iel = '02'O
    								ngeaCap = 'F0'O
    								ngiaCap = '70'O
    								eeaCap = Omit
    								eiaCap = Omit
    								spare = Omit
    							requestedNSSAI = Omit
    							lastVisitedRegisteredTai = Omit
    							s1_UE_Capability = Omit
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							micoInd = Omit
    							ueStatus = Omit
    							additionalGUTI = Omit
    							allowedPDUSessionStatus = Omit
    							ueUsageSetting = Omit
    							reqDRXParams = Omit
    							epsMessage = Omit
    							ladnInd = Omit
    							payloadContainerType = Omit
    							payload = Omit
    							networkSlicingInd = Omit
    							updateType = Omit
    							msClassmark2 = Omit
    							supportedCodecs = Omit
    							nasMsg = Omit
    							epsBearerContextStatus = Omit
    							requestedExtdDRXParams = Omit
    							t3324Value = Omit
    							ueRadioCapabilityId = Omit
    							requestedMappedNSSAI = Omit
    							additionalInfoReq = Omit
    							requestedWUSAssistanceInfo = Omit
    							n5GCInd = Omit
    							requestedNB_N1DRXParams = Omit
    							ueRequestType = Omit
    							pagingRestrict = Omit
    							serviceLvlAA = Omit
    							nId = Omit
    							msPLMNwDisasterCondition = Omit
    							requestedPEIPS_AssistInfo = Omit
    							t3512Value = Omit
    					PiggybackedPduList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0000'B
    					ForceMacError = False
    				Pdu
    					Msg
    						authentication_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01010110'B
    							spareHalfOctet2 = '0'H
    							ngNasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							abba
    								iei = Omit
    								iel = '02'O
    								abbaValue = '0000'O
    							rand
    								iei = '21'O
    								randValue = 10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111'B
    							autn
    								iei = '20'O
    								iel = '10'O
    								aUTN = 01101110001100100011101100110110110001000110110010000000000000001010001111011111000011100110111000110010001110111011011011000100'B
    							eapMessage = Omit
    					PiggybackedPduList = Omit

    Authentication Request
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	auth_mt [8 bits] = 0x56 [ 86 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	NAS key set identifierASME
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	abba
    		iel [8 bits] = 0x2 [ 2 ]
    		abb = 0x0000 [ 0 ]
    	Authentication parameter rand
    		iei [8 bits] = 0x21 [ 33 ]
    		Authentication parameter random = 0xA3DE0C6D363E30C364A4078F1BF8D577
    	Authentication parameter AUTN
    		iei [8 bits] = 0x20 [ 32 ]
    		iel [8 bits] = 0x10 [ 16 ]
    		Value = 0x6E323B36C46C8000A3DF0E6E323BB6C4

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E00560002000021A3DE0C6D363E30C364A4078F1BF8D57720106E323B36C46C8000A3DF0E6E323BB6C4

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E00560002000021A3DE0C6D363E30C364A4078F1BF8D57720106E323B36C46C8000A3DF0E6E323BB6C4'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Authentication Response
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x57 [ 87 ]
    	auth_res_param
    		iei [8 bits] = 0x2D [ 45 ]
    		iel [8 bits] = 0x10 [ 16 ]
    		Authentication response parameter information = 0xD7C360C5A57C8F4F03BD1E406604EEC2

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E00572D10D7C360C5A57C8F4F03BD1E406604EEC2

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 506
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E00572D10D7C360C5A57C8F4F03BD1E406604EEC2'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 506
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0000'B
    					NasCount = '00FFFFFF'O
    				Pdu
    					Msg
    						authentication_Response
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01010111'B
    							authResponseParam
    								iei = '2D'O
    								iel = '10'O
    								res = 11010111110000110110000011000101101001010111110010001111010011110000001110111101000111100100000001100110000001001110111011000010'B
    							eapMessage = Omit
    					PiggybackedPduList = Omit

    NG_NAS_CTRL_REQ
    	Common
    		ControlInfo
    			CnfFlag = True
    	Request
    		Security
    			StartRestart
    				Integrity
    					Algorithm = 0010'B
    					K_NAS = 01010110100101101010000011001111010100100111110100111111100011011100100111011111001111001100110000011001100001010011000001000111'B
    				Ciphering
    					Algorithm = 0010'B
    					K_NAS = 10101001100001010001101000010011110110111101001011110110111110100001001001000110011101101110111001000010100100001100100001011011'B
    				NasCountReset = True

    NG_NAS_CTRL_CNF
    	Common
    	Confirm
    		Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0011'B
    					ForceMacError = False
    				Pdu
    					Msg
    						security_Mode_Command
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01011101'B
    							nasSecurityAlgorithms
    								iei = Omit
    								cipheringType = 0010'B
    								integrityType = 0010'B
    							spareHalfOctet2 = '0'H
    							ngNasKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							ueSecurityCapability
    								iei = Omit
    								iel = '02'O
    								ngeaCap = 'F0'O
    								ngiaCap = '70'O
    								eeaCap = Omit
    								eiaCap = Omit
    								spare = Omit
    							imeisvRequest = Omit
    							epsSecurityAlgorithms = Omit
    							add5GSecurityInfo
    								iei = '36'O
    								iel = '01'O
    								spareBits = 000000'B
    								rinmr = 1'B
    								hdp = 0'B
    							eapMessage = Omit
    							abba = Omit
    							replayedUESecurityCap = Omit
    					PiggybackedPduList = Omit

    Security Mode Command
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x5D [ 93 ]
    	sel_nas_secu_alg
    		Type of ciphering algorithm [4 bits] = 0x2 [ 2 ]
    		Type of integrity protection algorithm [4 bits] = 0x2 [ 2 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	ngksi
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	replay_ue_secu_cap
    		iel [8 bits] = 0x2 [ 2 ]
    		ea0_128 [1 bit] = 0x1 [ 1 ]
    		ea1_128 [1 bit] = 0x1 [ 1 ]
    		ea2_128 [1 bit] = 0x1 [ 1 ]
    		ea3 [1 bit] = 0x1 [ 1 ]
    		ea4 [1 bit] = 0x0 [ 0 ]
    		ea5 [1 bit] = 0x0 [ 0 ]
    		ea6 [1 bit] = 0x0 [ 0 ]
    		ea7 [1 bit] = 0x0 [ 0 ]
    		ia0 [1 bit] = 0x0 [ 0 ]
    		ia1_128 [1 bit] = 0x1 [ 1 ]
    		ia2_128 [1 bit] = 0x1 [ 1 ]
    		ia3 [1 bit] = 0x1 [ 1 ]
    		ia4 [1 bit] = 0x0 [ 0 ]
    		ia5 [1 bit] = 0x0 [ 0 ]
    		ia6 [1 bit] = 0x0 [ 0 ]
    		ia7 [1 bit] = 0x0 [ 0 ]
    	add_fiveg_secu_info
    		iei [8 bits] = 0x36 [ 54 ]
    		length_addfiveg [8 bits] = 0x1 [ 1 ]
    		Spare bits [6 bits] = 0x0 [ 0 ]
    		rinm_r [1 bit] = 0x1 [ 1 ]
    		hdp [1 bit] = 0x0 [ 0 ]

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E032FC5D9E3007E005D220002F070360102

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E032FC5D9E3007E005D220002F070360102'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E047C3D109D0043C47FE3C9DF0A2152B98B7652A18B854EC82325DE0B4EED5945355C7764166453041DBE91D70D95EEFA792F98D384C43B0E9987F1637570BA6A

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 525
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E047C3D109D0043C47FE3C9DF0A2152B98B7652A18B854EC82325DE0B4EED5945355C7764166453041DBE91D70D95EEFA792F98D384C43B0E9987F1637570BA6A'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Security Mode Complete
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x5E [ 94 ]
    	NAS message container
    		iei [8 bits] = 0x71 [ 113 ]
    		iel [16 bits] = 0x34 [ 52 ]
    		NAS message contents = 0x7E004179000BF200F110FE0041C2345678100200402E02F0702F0801010102010301045200F11000000118010174000090530101

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 525
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0100'B
    					NasCount = '00000000'O
    				Pdu
    					Msg
    						security_Mode_Complete
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01011110'B
    							imeisv = Omit
    							nasMsg
    								iei = '71'O
    								iel = '0034'O
    								replayedNASMsgContainerValue = '7E004179000BF200F110FE0041C2345678100200402E02F0702F0801010102010301045200F11000000118010174000090530101'O
    							nonIMEISV_PEI = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								registration_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01000001'B
    									ngNasKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 111'B
    									registrationType
    										fOR = 1'B
    										registrationType = 001'B
    									ngMobileId
    										iei = Omit
    										iel = '000B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 010'B
    										otherDigits = '00F110FE0041C2345678'O
    									nonCurrentNativeKSI = Omit
    									gmmCapability
    										iei = '10'O
    										iel = '02'O
    										sgc = 0'B
    										ngIPHC_CP_CIoT = 0'B
    										n3Data = 0'B
    										ng_CP_CIoT = 0'B
    										restrictEC = 0'B
    										lpp = 0'B
    										hoAttach = 0'B
    										s1Cap = 0'B
    										racs = 0'B
    										nssaa = 1'B
    										ngLCS = 0'B
    										v2xNPC5 = 0'B
    										v2xEPC5 = 0'B
    										v2x = 0'B
    										ng_UP_CIoT = 0'B
    										ngSRVCC = 0'B
    										ngProSeL2relay = Omit
    										ngProSe_dc = Omit
    										ngProSe_dd = Omit
    										erNSSAI = Omit
    										ngEHC_CP_CIoT = Omit
    										multipleUP = Omit
    										wusa = Omit
    										cag = Omit
    										pr = Omit
    										rpr = Omit
    										piv = Omit
    										ncr = Omit
    										nrPSSI = Omit
    										ngProSeL3rmt = Omit
    										ngProSeL2rmt = Omit
    										ngProSeL3relay = Omit
    										mpsiu = Omit
    										uas = Omit
    										nsag = Omit
    										exCAG = Omit
    										ssnpnsi = Omit
    										eventNotification = Omit
    										mint = Omit
    										nssrg = Omit
    										spareBits = Omit
    										rcman = Omit
    										rcmap = Omit
    										spare = Omit
    									ueSecurityCapability
    										iei = '2E'O
    										iel = '02'O
    										ngeaCap = 'F0'O
    										ngiaCap = '70'O
    										eeaCap = Omit
    										eiaCap = Omit
    										spare = Omit
    									requestedNSSAI
    										iei = '2F'O
    										lvPart
    											iel = '08'O
    											s_nssai
    												S_NSSAI_LV
    													iel = '01'O
    													vPart
    														sst = '01'O
    														sd = Omit
    														mappedSST = Omit
    														mappedSD = Omit
    												S_NSSAI_LV
    													iel = '01'O
    													vPart
    														sst = '02'O
    														sd = Omit
    														mappedSST = Omit
    														mappedSD = Omit
    												S_NSSAI_LV
    													iel = '01'O
    													vPart
    														sst = '03'O
    														sd = Omit
    														mappedSST = Omit
    														mappedSD = Omit
    												S_NSSAI_LV
    													iel = '01'O
    													vPart
    														sst = '04'O
    														sd = Omit
    														mappedSST = Omit
    														mappedSD = Omit
    									lastVisitedRegisteredTai
    										iei = '52'O
    										plmnId = '00F110'O
    										tac = '000001'O
    									s1_UE_Capability = Omit
    									ulDataStatus = Omit
    									pduSessionStatus = Omit
    									micoInd = Omit
    									ueStatus = Omit
    									additionalGUTI = Omit
    									allowedPDUSessionStatus = Omit
    									ueUsageSetting
    										iei = '18'O
    										iel = '01'O
    										spare = 0000000'B
    										ueUsageSetting = 1'B
    									reqDRXParams = Omit
    									epsMessage = Omit
    									ladnInd
    										iei = '74'O
    										iel = '0000'O
    										listOfLADN_DNNValues = Omit
    									payloadContainerType = Omit
    									payload = Omit
    									networkSlicingInd
    										iei = '9'H
    										spare = 00'B
    										dcni = 0'B
    										nssci = 0'B
    									updateType
    										iei = '53'O
    										iel = '01'O
    										spare = 00'B
    										eps_PNB_CIoT = 00'B
    										ng_PNB_CIoT = 00'B
    										ngRAN_RCU = 0'B
    										smsRequested = 1'B
    									msClassmark2 = Omit
    									supportedCodecs = Omit
    									nasMsg = Omit
    									epsBearerContextStatus = Omit
    									requestedExtdDRXParams = Omit
    									t3324Value = Omit
    									ueRadioCapabilityId = Omit
    									requestedMappedNSSAI = Omit
    									additionalInfoReq = Omit
    									requestedWUSAssistanceInfo = Omit
    									n5GCInd = Omit
    									requestedNB_N1DRXParams = Omit
    									ueRequestType = Omit
    									pagingRestrict = Omit
    									serviceLvlAA = Omit
    									nId = Omit
    									msPLMNwDisasterCondition = Omit
    									requestedPEIPS_AssistInfo = Omit
    									t3512Value = Omit
    							PiggybackedPduList = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 1'B
    		BitStringType
    ConstraintMismatch::Expected:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 0'B
    		BitStringType

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 01110001101100010111101001001011010111011111101100010110011010011111011101101101111111110000000110000110011010000101010001010100'B
    					KUPint = 10100011001111010111100111110111010001001100111000011111110010111001011011011111101000011001001011111101001110111001011000010001'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01011101101111111000001111010101010010111110001011011001110001111111101110000000010111011111100010111100001010011011111110000111'B
    					KUPenc = 01000010111001011010101101111100101001011001110010110101110100110011010101001111101000000100010010101110111100101000101001001100'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 4
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 3
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea1
    					integrityProtAlgorithm = nia1

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea1 (1)
    										integrityProtAlgorithm = nia1 (1)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 553
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 553
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityEnquiry
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								ueCapabilityEnquiry
    									ue_CapabilityRAT_RequestList
    										UE_CapabilityRAT_Request
    											rat_Type = nr (0)
    											capabilityRequestFilter = '80041000'O
    									lateNonCriticalExtension = Omit
    									ue_CapabilityEnquiryExt = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = ueCapabilityEnquiry =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = ueCapabilityEnquiry =
    			ue-CapabilityRAT-RequestList = SEQUENCE OF UE-CapabilityRAT-Request
    				UE-CapabilityRAT-Request(1)
    					rat-Type = nr
    					capabilityRequestFilter = 80041000

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityEnquiry
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							ueCapabilityEnquiry
    								ue_CapabilityRAT_RequestList
    									UE_CapabilityRAT_Request
    										rat_Type = nr (0)
    										capabilityRequestFilter = '80041000'O
    								lateNonCriticalExtension = Omit
    								ue_CapabilityEnquiryExt = Omit

    UL-DCCH-Message
    	message = c1 = ueCapabilityInformation =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = ueCapabilityInformation =
    			ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    				UE-CapabilityRAT-Container(1)
    					rat-Type = nr
    					ue-CapabilityRAT-Container =
    	UE-CapabilityRAT-Container(1)
    		UE-NR-Capability
    			accessStratumRelease = rel17
    			pdcp-Parameters
    				supportedROHC-Profiles
    					profile0x0000 = TRUE
    					profile0x0001 = TRUE
    					profile0x0002 = TRUE
    					profile0x0003 = FALSE
    					profile0x0004 = FALSE
    					profile0x0006 = FALSE
    					profile0x0101 = FALSE
    					profile0x0102 = FALSE
    					profile0x0103 = FALSE
    					profile0x0104 = FALSE
    				maxNumberROHC-ContextSessions = cs24
    				continueROHC-Context = supported
    				shortSN = supported
    			rlc-Parameters
    				am-WithShortSN = supported
    				um-WithShortSN = supported
    				um-WithLongSN = supported
    			mac-Parameters
    				mac-ParametersCommon
    					dummy = supported
    				mac-ParametersXDD-Diff
    					logicalChannelSR-DelayTimer = supported
    					longDRX-Cycle = supported
    					shortDRX-Cycle = supported
    			phy-Parameters
    				phy-ParametersCommon
    					dynamicHARQ-ACK-Codebook = supported
    					semiStaticHARQ-ACK-Codebook = supported
    					dynamicBetaOffsetInd-HARQ-ACK-CSI = supported
    					ra-Type0-PUSCH = supported
    					dynamicSwitchRA-Type0-1-PUSCH = supported
    					pdsch-MappingTypeA = supported
    					rateMatchingResrcSetSemi-Static = supported
    					rateMatchingResrcSetDynamic = supported
    					bwp-SwitchingDelay = type2
    					rateMatchingCtrlResrcSetDynamic = supported
    					maxLayersMIMO-Indication = supported
    					codebookVariantsList-r16 = SEQUENCE OF SupportedCSI-RS-Resource
    						SupportedCSI-RS-Resource(1)
    							maxNumberTxPortsPerResource = p2
    							maxNumberResourcesPerBand = 2
    							totalNumberTxPortsPerBand = 4
    						SupportedCSI-RS-Resource(2)
    							maxNumberTxPortsPerResource = p8
    							maxNumberResourcesPerBand = 4
    							totalNumberTxPortsPerBand = 32
    						SupportedCSI-RS-Resource(3)
    							maxNumberTxPortsPerResource = p16
    							maxNumberResourcesPerBand = 2
    							totalNumberTxPortsPerBand = 32
    						SupportedCSI-RS-Resource(4)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 1
    							totalNumberTxPortsPerBand = 32
    						SupportedCSI-RS-Resource(5)
    							maxNumberTxPortsPerResource = p2
    							maxNumberResourcesPerBand = 20
    							totalNumberTxPortsPerBand = 40
    						SupportedCSI-RS-Resource(6)
    							maxNumberTxPortsPerResource = p8
    							maxNumberResourcesPerBand = 8
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(7)
    							maxNumberTxPortsPerResource = p8
    							maxNumberResourcesPerBand = 12
    							totalNumberTxPortsPerBand = 96
    						SupportedCSI-RS-Resource(8)
    							maxNumberTxPortsPerResource = p16
    							maxNumberResourcesPerBand = 6
    							totalNumberTxPortsPerBand = 96
    						SupportedCSI-RS-Resource(9)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 3
    							totalNumberTxPortsPerBand = 96
    						SupportedCSI-RS-Resource(10)
    							maxNumberTxPortsPerResource = p16
    							maxNumberResourcesPerBand = 4
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(11)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 2
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(12)
    							maxNumberTxPortsPerResource = p2
    							maxNumberResourcesPerBand = 16
    							totalNumberTxPortsPerBand = 32
    						SupportedCSI-RS-Resource(13)
    							maxNumberTxPortsPerResource = p4
    							maxNumberResourcesPerBand = 8
    							totalNumberTxPortsPerBand = 32
    						SupportedCSI-RS-Resource(14)
    							maxNumberTxPortsPerResource = p8
    							maxNumberResourcesPerBand = 16
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(15)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 16
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(16)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 2
    							totalNumberTxPortsPerBand = 40
    						SupportedCSI-RS-Resource(17)
    							maxNumberTxPortsPerResource = p8
    							maxNumberResourcesPerBand = 16
    							totalNumberTxPortsPerBand = 128
    						SupportedCSI-RS-Resource(18)
    							maxNumberTxPortsPerResource = p16
    							maxNumberResourcesPerBand = 8
    							totalNumberTxPortsPerBand = 128
    						SupportedCSI-RS-Resource(19)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 4
    							totalNumberTxPortsPerBand = 128
    						SupportedCSI-RS-Resource(20)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 3
    							totalNumberTxPortsPerBand = 72
    						SupportedCSI-RS-Resource(21)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 14
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(22)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 17
    							totalNumberTxPortsPerBand = 64
    						SupportedCSI-RS-Resource(23)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 3
    							totalNumberTxPortsPerBand = 80
    						SupportedCSI-RS-Resource(24)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 4
    							totalNumberTxPortsPerBand = 80
    						SupportedCSI-RS-Resource(25)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 4
    							totalNumberTxPortsPerBand = 96
    						SupportedCSI-RS-Resource(26)
    							maxNumberTxPortsPerResource = p32
    							maxNumberResourcesPerBand = 12
    							totalNumberTxPortsPerBand = 64
    				phy-ParametersXDD-Diff
    					dl-SchedulingOffset-PDSCH-TypeA = supported
    				phy-ParametersFRX-Diff
    					twoFL-DMRS = 11
    					supportedDMRS-TypeUL = type1And2
    					pucch-F2-WithFH = supported
    					pucch-F3-WithFH = supported
    					pdcch-BlindDetectionCA = 6
    					absoluteTPC-Command = supported
    					pusch-HalfPi-BPSK = supported
    					pucch-F3-4-HalfPi-BPSK = supported
    					mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot
    						sameSymbol = supported
    					dl-SchedulingOffset-PDSCH-TypeA = supported
    					oneFL-DMRS-TwoAdditionalDMRS-UL = supported
    					twoFL-DMRS-TwoAdditionalDMRS-UL = supported
    					pdcch-BlindDetectionNRDC
    						pdcch-BlindDetectionMCG-UE = 2
    						pdcch-BlindDetectionSCG-UE = 5
    				phy-ParametersFR1
    					pdsch-256QAM-FR1 = supported
    					pdsch-RE-MappingFR1-PerSymbol = n10
    					pdsch-RE-MappingFR1-PerSlot = n32
    				phy-ParametersFR2
    					pdsch-RE-MappingFR2-PerSymbol = n6
    					pCell-FR2 = supported
    					pdsch-RE-MappingFR2-PerSlot = n64
    			rf-Parameters
    				supportedBandListNR = SEQUENCE OF BandNR
    					BandNR(1)
    						bandNR = 1
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							dummy4
    								burstLength = 1
    								maxSimultaneousResourceSetsPerCC = 5
    								maxConfiguredResourceSetsPerCC = 1
    								maxConfiguredResourceSetsAllCC = 32
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(2)
    						bandNR = 3
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(3)
    						bandNR = 5
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(4)
    						bandNR = 8
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(5)
    						bandNR = 28
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111010000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111010000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(6)
    						bandNR = 78
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-DL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    						channelBWs-UL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    					BandNR(7)
    						bandNR = 7
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(8)
    						bandNR = 26
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111110000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(9)
    						bandNR = 38
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011000
    							scs-60kHz = 0000000000
    						txDiversity-r16 = supported
    					BandNR(10)
    						bandNR = 77
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-DL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    						channelBWs-UL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    					BandNR(11)
    						bandNR = 20
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(12)
    						bandNR = 41
    						modifiedMPR-Behaviour = 11000000
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-DL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    						channelBWs-UL-v1590 = fr1 =
    							scs-30kHz = 1000000000000000
    					BandNR(13)
    						bandNR = 79
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0000001111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0000001111
    							scs-60kHz = 0000000000
    					BandNR(14)
    						bandNR = 40
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc2
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-DL-v1590 = fr1 =
    							scs-30kHz = 0001000000000000
    						channelBWs-UL-v1590 = fr1 =
    							scs-30kHz = 0001000000000000
    					BandNR(15)
    						bandNR = 75
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111010000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(16)
    						bandNR = 2
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(17)
    						bandNR = 12
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1110000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1110000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(18)
    						bandNR = 14
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1100000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1100000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(19)
    						bandNR = 30
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0100000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0100000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(20)
    						bandNR = 66
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						asymmetricBandwidthCombinationSet = 1
    					BandNR(21)
    						bandNR = 71
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						asymmetricBandwidthCombinationSet = 11
    					BandNR(22)
    						bandNR = 48
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-30kHz = sym14
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(2)
    												maxNumberTxPortsPerResource = p16
    												maxNumberResourcesPerBand = 6
    												totalNumberTxPortsPerBand = 96
    											SupportedCSI-RS-Resource(3)
    												maxNumberTxPortsPerResource = p32
    												maxNumberResourcesPerBand = 3
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 32
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						bwp-SameNumerology = upto2
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						channelBWs-DL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011111
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 0000000000
    							scs-30kHz = 0001011000
    							scs-60kHz = 0000000000
    					BandNR(23)
    						bandNR = 25
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111111000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(24)
    						bandNR = 92
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n16
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 2
    							maxNumberCSI-RS-SSB-CBD = 8
    							beamReportTiming
    								scs-15kHz = sym8
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n16
    								maxNumberCSI-RS-Resource = n64
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p8
    												maxNumberResourcesPerBand = 12
    												totalNumberTxPortsPerBand = 96
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 4
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 8
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 64
    								maxConfigNumberCSI-IM-PerCC = n8
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 4
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 64
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 2
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 4
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 8
    								maxConfiguredResourceSetsAllCC = 32
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 6
    										INTEGER(2) = 7
    										INTEGER(3) = 8
    						multipleTCI = supported
    						pusch-256QAM = supported
    						ue-PowerClass = pc3
    						rateMatchingLTE-CRS = supported
    						channelBWs-DL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    						channelBWs-UL = fr1 =
    							scs-15kHz = 1111000000
    							scs-30kHz = 0000000000
    							scs-60kHz = 0000000000
    					BandNR(25)
    						bandNR = 257
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n64
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							beamCorrespondenceWithoutUL-BeamSweeping = supported
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberRxBeam = 2
    							maxNumberRxTxBeamSwitchDL
    								scs-120kHz = n14
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 16
    							maxNumberCSI-RS-SSB-CBD = 64
    							beamReportTiming
    								scs-120kHz = sym28
    							dummy6 = true
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n8
    								maxNumberCSI-RS-Resource = n32
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							beamSwitchTiming
    								scs-120kHz = sym28
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p2
    												maxNumberResourcesPerBand = 16
    												totalNumberTxPortsPerBand = 32
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 1
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 2
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 16
    								maxConfigNumberCSI-IM-PerCC = n2
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 1
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 3
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 64
    								maxConfiguredResourceSetsAllCC = 256
    							spatialRelations
    								maxNumberConfiguredSpatialRelations = n16
    								maxNumberActiveSpatialRelations = n1
    								maxNumberDL-RS-QCL-TypeD = n2
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    						multipleTCI = supported
    						ue-PowerClass = pc1
    						channelBWs-DL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 010
    						channelBWs-UL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 010
    						pucch-SpatialRelInfoMAC-CE = supported
    					BandNR(26)
    						bandNR = 258
    						modifiedMPR-Behaviour = 11000000
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n64
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							beamCorrespondenceWithoutUL-BeamSweeping = supported
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberRxBeam = 2
    							maxNumberRxTxBeamSwitchDL
    								scs-120kHz = n14
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 16
    							maxNumberCSI-RS-SSB-CBD = 64
    							beamReportTiming
    								scs-120kHz = sym28
    							dummy6 = true
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n8
    								maxNumberCSI-RS-Resource = n32
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							beamSwitchTiming
    								scs-120kHz = sym28
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p2
    												maxNumberResourcesPerBand = 16
    												totalNumberTxPortsPerBand = 32
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 1
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 2
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 16
    								maxConfigNumberCSI-IM-PerCC = n2
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 1
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 3
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 64
    								maxConfiguredResourceSetsAllCC = 256
    							spatialRelations
    								maxNumberConfiguredSpatialRelations = n16
    								maxNumberActiveSpatialRelations = n1
    								maxNumberDL-RS-QCL-TypeD = n2
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    						multipleTCI = supported
    						ue-PowerClass = pc1
    						channelBWs-DL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 010
    						channelBWs-UL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 010
    						pucch-SpatialRelInfoMAC-CE = supported
    					BandNR(27)
    						bandNR = 260
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n64
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							beamCorrespondenceWithoutUL-BeamSweeping = supported
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberRxBeam = 2
    							maxNumberRxTxBeamSwitchDL
    								scs-120kHz = n14
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 16
    							maxNumberCSI-RS-SSB-CBD = 64
    							beamReportTiming
    								scs-120kHz = sym28
    							dummy6 = true
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n8
    								maxNumberCSI-RS-Resource = n32
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							beamSwitchTiming
    								scs-120kHz = sym28
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p2
    												maxNumberResourcesPerBand = 16
    												totalNumberTxPortsPerBand = 32
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 1
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 2
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 16
    								maxConfigNumberCSI-IM-PerCC = n2
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 1
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 3
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 64
    								maxConfiguredResourceSetsAllCC = 256
    							spatialRelations
    								maxNumberConfiguredSpatialRelations = n16
    								maxNumberActiveSpatialRelations = n1
    								maxNumberDL-RS-QCL-TypeD = n2
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    						multipleTCI = supported
    						ue-PowerClass = pc1
    						channelBWs-DL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 110
    						channelBWs-UL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 110
    						pucch-SpatialRelInfoMAC-CE = supported
    					BandNR(28)
    						bandNR = 261
    						mimo-ParametersPerBand
    							tci-StatePDSCH
    								maxNumberConfiguredTCIstatesPerCC = n64
    								maxNumberActiveTCI-PerBWP = n1
    							pusch-TransCoherence = nonCoherent
    							beamCorrespondenceWithoutUL-BeamSweeping = supported
    							periodicBeamReport = supported
    							aperiodicBeamReport = supported
    							maxNumberRxBeam = 2
    							maxNumberRxTxBeamSwitchDL
    								scs-120kHz = n14
    							maxNumberNonGroupBeamReporting = n4
    							maxNumberSSB-BFD = 16
    							maxNumberCSI-RS-SSB-CBD = 64
    							beamReportTiming
    								scs-120kHz = sym28
    							dummy6 = true
    							beamManagementSSB-CSI-RS
    								maxNumberSSB-CSI-RS-ResourceOneTx = n8
    								maxNumberCSI-RS-Resource = n32
    								maxNumberCSI-RS-ResourceTwoTx = n0
    								supportedCSI-RS-Density = oneAndThree
    								maxNumberAperiodicCSI-RS-Resource = n32
    							beamSwitchTiming
    								scs-120kHz = sym28
    							codebookParameters
    								type1
    									singlePanel
    										supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    											SupportedCSI-RS-Resource(1)
    												maxNumberTxPortsPerResource = p2
    												maxNumberResourcesPerBand = 16
    												totalNumberTxPortsPerBand = 32
    										modes = mode1
    										maxNumberCSI-RS-PerResourceSet = 1
    							csi-RS-IM-ReceptionForFeedback
    								maxConfigNumberNZP-CSI-RS-PerCC = 2
    								maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 16
    								maxConfigNumberCSI-IM-PerCC = n2
    								maxNumberSimultaneousNZP-CSI-RS-PerCC = 1
    								totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    							csi-ReportFramework
    								maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    								maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 2
    								maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    								maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    								maxNumberAperiodicCSI-triggeringStatePerCC = n63
    								maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    								simultaneousCSI-ReportsPerCC = 3
    							csi-RS-ForTracking
    								maxBurstLength = 2
    								maxSimultaneousResourceSetsPerCC = 1
    								maxConfiguredResourceSetsPerCC = 64
    								maxConfiguredResourceSetsAllCC = 256
    							spatialRelations
    								maxNumberConfiguredSpatialRelations = n16
    								maxNumberActiveSpatialRelations = n1
    								maxNumberDL-RS-QCL-TypeD = n2
    							codebookParametersPerBand-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    						multipleTCI = supported
    						ue-PowerClass = pc1
    						channelBWs-DL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 110
    						channelBWs-UL = fr2 =
    							scs-60kHz = 000
    							scs-120kHz = 110
    						pucch-SpatialRelInfoMAC-CE = supported
    				supportedBandCombinationList = SEQUENCE OF BandCombination
    					BandCombination(1)
    						bandList = SEQUENCE OF BandParameters
    							BandParameters(1) = nr =
    								bandNR = 257
    								ca-BandwidthClassDL-NR = m
    								ca-BandwidthClassUL-NR = i
    						featureSetCombination = 1
    						ca-ParametersNR
    							simultaneousRxTxInterBandCA = supported
    						supportedBandwidthCombinationSet = 10001
    					BandCombination(2)
    						bandList = SEQUENCE OF BandParameters
    							BandParameters(1) = nr =
    								bandNR = 257
    								ca-BandwidthClassDL-NR = f
    								ca-BandwidthClassUL-NR = d
    						featureSetCombination = 2
    						ca-ParametersNR
    							simultaneousRxTxInterBandCA = supported
    						supportedBandwidthCombinationSet = 10001
    					BandCombination(3)
    						bandList = SEQUENCE OF BandParameters
    							BandParameters(1) = nr =
    								bandNR = 257
    								ca-BandwidthClassDL-NR = a
    								ca-BandwidthClassUL-NR = a
    							BandParameters(2) = nr =
    								bandNR = 257
    								ca-BandwidthClassDL-NR = a
    						featureSetCombination = 0
    						ca-ParametersNR
    							simultaneousRxTxInterBandCA = supported
    						supportedBandwidthCombinationSet = 10001
    				appliedFreqBandListFilter = SEQUENCE OF FreqBandInformation
    					FreqBandInformation(1) = bandInformationNR =
    						bandNR = 257
    				supportedBandCombinationList-v1540 = SEQUENCE OF BandCombination-v1540
    					BandCombination-v1540(1)
    						bandList-v1540 = SEQUENCE OF BandParameters-v1540
    							BandParameters-v1540(1)
    						ca-ParametersNR-v1540
    							csi-RS-IM-ReceptionForFeedbackPerBandComb
    								maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 8
    								totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 32
    							simultaneousCSI-ReportsAllCC = 10
    					BandCombination-v1540(2)
    						bandList-v1540 = SEQUENCE OF BandParameters-v1540
    							BandParameters-v1540(1)
    						ca-ParametersNR-v1540
    							csi-RS-IM-ReceptionForFeedbackPerBandComb
    								maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 8
    								totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 32
    							simultaneousCSI-ReportsAllCC = 10
    					BandCombination-v1540(3)
    						bandList-v1540 = SEQUENCE OF BandParameters-v1540
    							BandParameters-v1540(1)
    							BandParameters-v1540(2)
    						ca-ParametersNR-v1540
    							csi-RS-IM-ReceptionForFeedbackPerBandComb
    								maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 8
    								totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 32
    							simultaneousCSI-ReportsAllCC = 10
    				supportedBandCombinationList-v1610 = SEQUENCE OF BandCombination-v1610
    					BandCombination-v1610(1)
    						ca-ParametersNR-v1610
    							codebookParametersPerBC-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    					BandCombination-v1610(2)
    						ca-ParametersNR-v1610
    							codebookParametersPerBC-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    					BandCombination-v1610(3)
    						ca-ParametersNR-v1610
    							codebookParametersPerBC-r16
    								supportedCSI-RS-ResourceListAlt-r16
    									type1-SinglePanel-r16 = SEQUENCE OF INTEGER
    										INTEGER(1) = 12
    			measAndMobParameters
    				measAndMobParametersCommon
    					ssb-RLM = supported
    					eventB-MeasAndReport = supported
    					handoverFDD-TDD = supported
    					nr-CGI-Reporting = supported
    					reportAddNeighMeasForPeriodic-r16 = supported
    				measAndMobParametersXDD-Diff
    					handoverInterF = supported
    				measAndMobParametersFRX-Diff
    					ss-SINR-Meas = supported
    					handoverInterF = supported
    					simultaneousRxDataSSB-DiffNumerology = supported
    			fr1-Add-UE-NR-Capabilities
    				phy-ParametersFRX-Diff
    					supportedDMRS-TypeDL = type1And2
    					onePortsPTRS = 01
    					pucch-F4-WithFH = supported
    					tpc-SRS-RNTI = supported
    					almostContiguousCP-OFDM-UL = supported
    			fr2-Add-UE-NR-Capabilities
    				phy-ParametersFRX-Diff
    					supportedDMRS-TypeDL = type1
    					onePortsPTRS = 11
    					mux-SR-HARQ-ACK-PUCCH = supported
    			featureSets
    				featureSetsDownlink = SEQUENCE OF FeatureSetDownlink
    					FeatureSetDownlink(1)
    						featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    							FeatureSetDownlinkPerCC-Id(1) = 1
    						intraBandFreqSeparationDL = mhz800
    						scellWithoutSSB = supported
    						type1-3-CSS = supported
    						ue-SpecificUL-DL-Assignment = supported
    						timeDurationForQCL
    							scs-120kHz = s28
    					FeatureSetDownlink(2)
    						featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    							FeatureSetDownlinkPerCC-Id(1) = 1
    							FeatureSetDownlinkPerCC-Id(2) = 1
    							FeatureSetDownlinkPerCC-Id(3) = 1
    							FeatureSetDownlinkPerCC-Id(4) = 1
    							FeatureSetDownlinkPerCC-Id(5) = 1
    							FeatureSetDownlinkPerCC-Id(6) = 1
    							FeatureSetDownlinkPerCC-Id(7) = 1
    							FeatureSetDownlinkPerCC-Id(8) = 1
    						intraBandFreqSeparationDL = mhz800
    						scellWithoutSSB = supported
    						type1-3-CSS = supported
    						ue-SpecificUL-DL-Assignment = supported
    						timeDurationForQCL
    							scs-120kHz = s28
    					FeatureSetDownlink(3)
    						featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    							FeatureSetDownlinkPerCC-Id(1) = 1
    							FeatureSetDownlinkPerCC-Id(2) = 1
    							FeatureSetDownlinkPerCC-Id(3) = 1
    							FeatureSetDownlinkPerCC-Id(4) = 1
    						intraBandFreqSeparationDL = mhz800
    						scellWithoutSSB = supported
    						type1-3-CSS = supported
    						ue-SpecificUL-DL-Assignment = supported
    						timeDurationForQCL
    							scs-120kHz = s28
    				featureSetsDownlinkPerCC = SEQUENCE OF FeatureSetDownlinkPerCC
    					FeatureSetDownlinkPerCC(1)
    						supportedSubcarrierSpacingDL = kHz120
    						supportedBandwidthDL = fr2 = mhz100
    						maxNumberMIMO-LayersPDSCH = twoLayers
    						supportedModulationOrderDL = qam64
    				featureSetsUplink = SEQUENCE OF FeatureSetUplink
    					FeatureSetUplink(1)
    						featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    							FeatureSetUplinkPerCC-Id(1) = 1
    						supportedSRS-Resources
    							maxNumberAperiodicSRS-PerBWP = n1
    							maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    							maxNumberPeriodicSRS-PerBWP = n1
    							maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    							maxNumberSemiPersistentSRS-PerBWP = n1
    							maxNumberSemiPersistentSRS-PerBWP-PerSlot = 1
    							maxNumberSRS-Ports-PerResource = n2
    					FeatureSetUplink(2)
    						featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    							FeatureSetUplinkPerCC-Id(1) = 1
    							FeatureSetUplinkPerCC-Id(2) = 1
    							FeatureSetUplinkPerCC-Id(3) = 1
    							FeatureSetUplinkPerCC-Id(4) = 1
    						supportedSRS-Resources
    							maxNumberAperiodicSRS-PerBWP = n1
    							maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    							maxNumberPeriodicSRS-PerBWP = n1
    							maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    							maxNumberSemiPersistentSRS-PerBWP = n1
    							maxNumberSemiPersistentSRS-PerBWP-PerSlot = 1
    							maxNumberSRS-Ports-PerResource = n2
    					FeatureSetUplink(3)
    						featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    							FeatureSetUplinkPerCC-Id(1) = 1
    							FeatureSetUplinkPerCC-Id(2) = 1
    						supportedSRS-Resources
    							maxNumberAperiodicSRS-PerBWP = n1
    							maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    							maxNumberPeriodicSRS-PerBWP = n1
    							maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    							maxNumberSemiPersistentSRS-PerBWP = n1
    							maxNumberSemiPersistentSRS-PerBWP-PerSlot = 1
    							maxNumberSRS-Ports-PerResource = n2
    				featureSetsUplinkPerCC = SEQUENCE OF FeatureSetUplinkPerCC
    					FeatureSetUplinkPerCC(1)
    						supportedSubcarrierSpacingUL = kHz120
    						supportedBandwidthUL = fr2 = mhz100
    						mimo-CB-PUSCH
    							maxNumberMIMO-LayersCB-PUSCH = twoLayers
    							maxNumberSRS-ResourcePerSet = 1
    						supportedModulationOrderUL = qam64
    				featureSetsUplink-v1540 = SEQUENCE OF FeatureSetUplink-v1540
    					FeatureSetUplink-v1540(1)
    						pa-PhaseDiscontinuityImpacts = supported
    					FeatureSetUplink-v1540(2)
    						pa-PhaseDiscontinuityImpacts = supported
    					FeatureSetUplink-v1540(3)
    						pa-PhaseDiscontinuityImpacts = supported
    				featureSetsUplink-v1710 = SEQUENCE OF FeatureSetUplink-v1710
    					FeatureSetUplink-v1710(1)
    						ue-PowerClassPerBandPerBC-r17 = pc3
    					FeatureSetUplink-v1710(2)
    						ue-PowerClassPerBandPerBC-r17 = pc3
    					FeatureSetUplink-v1710(3)
    						ue-PowerClassPerBandPerBC-r17 = pc3
    			featureSetCombinations = SEQUENCE OF FeatureSetCombination
    				FeatureSetCombination(1) = SEQUENCE OF FeatureSetsPerBand
    					FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    						FeatureSet(1) = nr =
    							downlinkSetNR = 1
    							uplinkSetNR = 1
    					FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    						FeatureSet(1) = nr =
    							downlinkSetNR = 1
    							uplinkSetNR = 0
    				FeatureSetCombination(2) = SEQUENCE OF FeatureSetsPerBand
    					FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    						FeatureSet(1) = nr =
    							downlinkSetNR = 2
    							uplinkSetNR = 2
    				FeatureSetCombination(3) = SEQUENCE OF FeatureSetsPerBand
    					FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    						FeatureSet(1) = nr =
    							downlinkSetNR = 3
    							uplinkSetNR = 3
    			nonCriticalExtension
    				inactiveState = supported
    				nonCriticalExtension
    					overheatingInd = supported
    					fr1-Add-UE-NR-Capabilities-v1540
    						ims-ParametersFRX-Diff
    							voiceOverNR = supported
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									powSav-Parameters-r16
    										powSav-ParametersCommon-r16
    											maxCC-Preference-r16 = supported
    											releasePreference-r16 = supported
    									fr1-Add-UE-NR-Capabilities-v1610
    										powSav-ParametersFRX-Diff-r16
    											maxMIMO-LayerPreference-r16 = supported
    									highSpeedParameters-r16
    										measurementEnhancement-r16 = supported
    										demodulationEnhancement-r16 = supported
    									ue-BasedPerfMeas-Parameters-r16
    										loggedMeasurements-r16 = supported
    										gnss-Location-r16 = supported
    									son-Parameters-r16
    										rach-Report-r16 = supported
    									nonCriticalExtension
    										nonCriticalExtension
    											nonCriticalExtension
    												ul-RRC-Segmentation-r16 = supported

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 556
    				Subframe
    					Number = 4
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityInformation
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							ueCapabilityInformation
    								ue_CapabilityRAT_ContainerList
    									UE_CapabilityRAT_Container
    										rat_Type = nr (0)
    										ue_CapabilityRAT_Container = ' 'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 556
    				Subframe
    					Number = 4
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityInformation
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								ueCapabilityInformation
    									ue_CapabilityRAT_ContainerList
    										UE_CapabilityRAT_Container
    											rat_Type = nr (0)
    											ue_CapabilityRAT_Container = ' 'O
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 1

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 3

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 5

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 8

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 28

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 78

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 7

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 26

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 38

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 77

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 20

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 41

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 79

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 40

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 75

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 2

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 12

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 14

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 30

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 66

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 71

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 48

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 25

    summary = Message Mismatch: FreqBandIndicatorNR
    MATCH_MISMATCH
    	Message Mismatch: FreqBandIndicatorNR
    		bandNR = 92

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						registration_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000010'B
    							registrationResult
    								iel = '01'O
    								spare = 0'B
    								disasterRoamingResult = 0'B
    								emergencyRegistered = 0'B
    								nssaaPerformed = 0'B
    								smsAllowed = 0'B
    								resultValue = 001'B
    							guti
    								iei = '77'O
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    							equivalentPlmns = Omit
    							taiList
    								iei = '54'O
    								lvPart
    									iel = '07'O
    									listOfPartialTais
    										NG_ListOfPartialTaiList
    											allowedType = 0'B
    											typeOfList = 00'B
    											numberOfElements = 00000'B
    											partialTaiList
    												type0List
    													NG_Type0Element
    														plmnId = '00F110'O
    														tacList
    															OctetStringType = '000001'O
    							allowedNSSAI
    								iei = '15'O
    								lvPart
    									iel = '08'O
    									s_nssai
    										S_NSSAI_LV
    											iel = '01'O
    											vPart
    												sst = '01'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    										S_NSSAI_LV
    											iel = '01'O
    											vPart
    												sst = '02'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    										S_NSSAI_LV
    											iel = '01'O
    											vPart
    												sst = '03'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    										S_NSSAI_LV
    											iel = '01'O
    											vPart
    												sst = '04'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    							rejectedNSSAI = Omit
    							configuredNSSAI = Omit
    							ngs_NetworkFeatureSupport
    								iei = '21'O
    								iel = '03'O
    								mpsi = 0'B
    								iwk_N26 = 0'B
    								emf = 00'B
    								emc = 11'B
    								imsVoPS_n3GPP = 0'B
    								imsVoPS_3GPP = 1'B
    								ng_UP_CIoT = 0'B
    								ngIPHC_CP_CIoT = 0'B
    								n3Data = 0'B
    								ng_CP_CIoT = 0'B
    								restrictEC = 00'B
    								mcsi = 0'B
    								emcn3 = 0'B
    								spareBit = 0'B
    								pr = 0'B
    								rpr = 0'B
    								piv = 0'B
    								ncr = 0'B
    								ngEHC_CP_CIoT = 0'B
    								atsInd = 0'B
    								ngLCS = 0'B
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							ladnInfo = Omit
    							micoInd = Omit
    							networkSlicingInd = Omit
    							saiList = Omit
    							t3512Value
    								iei = '5E'O
    								iel = '01'O
    								unit = 111'B
    								gprsTimerValue = 00000'B
    							non3GPPDeregisterValue = Omit
    							t3502Value = Omit
    							emergencyNumberList = Omit
    							xtdEmergencyNumberList = Omit
    							sorTransparentContainer = Omit
    							eapMessage = Omit
    							inclusionModeNSSAI = Omit
    							operatorAccessCatDefs = Omit
    							negotiatedDRXParams = Omit
    							non3GPP_NW_ProvidedPolicies = Omit
    							epsBearerContextStatus = Omit
    							negotiatedExtdDRXParams = Omit
    							t3447Value = Omit
    							t3448Value = Omit
    							t3324Value = Omit
    							ueRadioCapabilityId = Omit
    							ueRadioCapIdDeletionInd = Omit
    							pendingNSSAI = Omit
    							cipheringKeyData = Omit
    							cagInfoList = Omit
    							truncatedS_TMSIConfig = Omit
    							negotiatedWUSAssistanceInfo = Omit
    							negotiatedNB_N1DRXParams = Omit
    							extdRejectedNSSAI = Omit
    							serviceLvlAA = Omit
    							negotiatedPEIPS_AssistInfo = Omit
    							ngAddRequestResult = Omit
    							nssrgInfo = Omit
    							disasterRoamingWaitRange = Omit
    							disasterReturnWaitRange = Omit
    							disasterPLMNList = Omit
    							forbidTAIList_Roaming = Omit
    							forbidTAIList_RegProvService = Omit
    							extdCAGInfoList = Omit
    							nsagInfo = Omit
    					PiggybackedPduList = Omit

    REGISTRATION ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	reg_acc_mt [8 bits] = 0x42 [ 66 ]
    	5GS registration result
    		iel [8 bits] = 0x1 [ 1 ]
    		Spare bits [2 bits] = 0x0 [ 0 ]
    		emergency_registered [1 bit] = 0x0 [ 0 ]
    		nssaa_performed [1 bit] = 0x0 [ 0 ]
    		sms_allowed [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x1 [ 1 ]
    	5GS mobile identity
    		iei [8 bits] = 0x77 [ 119 ]
    		iel [16 bits] = 0xB [ 11 ]
    		Identity digit [4 bits] = 0xF [ 15 ]
    		Spare bit [1 bit] = 0x0 [ 0 ]
    		fivegs_typ_id [3 bits] = 0x2 [ 2 ]
    		MCC digit 2 [4 bits] = 0x0 [ 0 ]
    		MCC digit 1 [4 bits] = 0x0 [ 0 ]
    		MNC digit 3 [4 bits] = 0xF [ 15 ]
    		MCC digit 3 [4 bits] = 0x1 [ 1 ]
    		MNC digit 2 [4 bits] = 0x1 [ 1 ]
    		MNC digit 1 [4 bits] = 0x0 [ 0 ]
    		AMF Region ID = 0xFE [ 254 ]
    		AMF Set ID = 0x00 [ 0 ]
    		AMF Set ID (continued) [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	Tracking area identity list
    		iei [8 bits] = 0x54 [ 84 ]
    		iel [8 bits] = 0x7 [ 7 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		Type of list [2 bits] = 0x0 [ 0 ]
    		number of elements [5 bits] = 0x0 [ 0 ]
    		Mobile country code, 2 digits = 0x00 [ 0 ]
    		Mobile network code digit 3 = 0xF [ 15 ]
    		Mobile country code digit 3 = 0x1 [ 1 ]
    		Mobile network code, 2 BCD digits = 0x10 [ 16 ]
    		Tracking area code 1 = 0x00 [ 0 ]
    		Tracking area code 1 continued = 0x0001 [ 1 ]
    	Allowed NSSAI
    		iei [8 bits] = 0x15 [ 21 ]
    		iel [8 bits] = 0x8 [ 8 ]
    		len_s_nssai_1 [8 bits] = 0x1 [ 1 ]
    		sst_1 = 0x01 [ 1 ]
    		len_s_nssai_2 [8 bits] = 0x1 [ 1 ]
    		sst_2 = 0x02 [ 2 ]
    		len_s_nssai_3 [8 bits] = 0x1 [ 1 ]
    		sst_3 = 0x03 [ 3 ]
    		len_s_nssai_4 [8 bits] = 0x1 [ 1 ]
    		sst_4 = 0x04 [ 4 ]
    	nwfeaturesupport
    		iei [8 bits] = 0x21 [ 33 ]
    		iel [8 bits] = 0x3 [ 3 ]
    		MPSI [1 bit] = 0x0 [ 0 ]
    		iwk_n26 [1 bit] = 0x0 [ 0 ]
    		emf [2 bits] = 0x0 [ 0 ]
    		emc [2 bits] = 0x3 [ 3 ]
    		ims_vops_n3gpp [1 bit] = 0x0 [ 0 ]
    		ims_vops_3gpp [1 bit] = 0x1 [ 1 ]
    		fiveg_up_ciot [1 bit] = 0x0 [ 0 ]
    		fiveg_iphc_cp_ciot [1 bit] = 0x0 [ 0 ]
    		n3data [1 bit] = 0x0 [ 0 ]
    		fiveg_cp_ciot [1 bit] = 0x0 [ 0 ]
    		restrictec [2 bits] = 0x0 [ 0 ]
    		mcsi [1 bit] = 0x0 [ 0 ]
    		emcn3 [1 bit] = 0x0 [ 0 ]
    		Spare bits [5 bits] = 0x0 [ 0 ]
    		fiveg_ehc_cp_ciot [1 bit] = 0x0 [ 0 ]
    		ats_ind [1 bit] = 0x0 [ 0 ]
    		fiveg_lcs [1 bit] = 0x0 [ 0 ]
    	t3512_val
    		iei [8 bits] = 0x5E [ 94 ]
    		iel [8 bits] = 0x1 [ 1 ]
    		unit_lt [3 bits] = 0x7 [ 7 ]
    		Value [5 bits] = 0x0 [ 0 ]

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E0207E71DC70114593B0E158FBEAA4EEA51FC93D8D6375AEE1F4CD8CAFF368FB69045D52ADDFB5A52C1CFBE3889B47B78FC92A41C

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E0207E71DC70114593B0E158FBEAA4EEA51FC93D8D6375AEE1F4CD8CAFF368FB69045D52ADDFB5A52C1CFBE3889B47B78FC92A41C'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E020FDB604C019CDF4C

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 563
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E020FDB604C019CDF4C'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    REGISTRATION COMPLETE
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	reg_comp_msg_id = 0x43 [ 67 ]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 563
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000001'O
    				Pdu
    					Msg
    						registration_Complete
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000011'B
    							sorTransparentContainer = Omit
    					PiggybackedPduList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 567
    				Subframe
    					Number = 0
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					SymbolOffset = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 305
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 13:20:10

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 597
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 597
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000110'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000101'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 597
    			Subframe
    				Number = 2
    			HSFN
    				Number = 2
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 597
    			Subframe
    				Number = 2
    			HSFN
    				Number = 2
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 597
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 597
    			Subframe
    				Number = 7
    			HSFN
    				Number = 2
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 597
    				Subframe
    					Number = 7
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 602
    			Subframe
    				Number = 7
    			HSFN
    				Number = 2
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 602
    				Subframe
    					Number = 7
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 603
    			Subframe
    				Number = 2
    			HSFN
    				Number = 2
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 603
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 313
    outStr = Timer: t_Timer, Expired: 13:20:12

    UT_COMMON_CMD
    	Cmd = REQUEST_PDPCONTEXT (116)
    	CnfReq = CNF_REQUIRED (1)
    	ParameterList
    		Ut_Parameter_Type
    			Name = 'RequestPDP'
    			Value = '1,"IPV4V6","internet",,,,,,,,,,,,,,0,"",0,'

    UT_SYSTEM_REQ
    	Cmd
    		AT = 'AT+CGDCONT=1,"IPV4V6","internet",,,,,,,,,,,,,,0,"",0,'
    	CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF
    	Result = True
    	ResultString = 'OK'

    UT_COMMON_CNF
    	Result = True
    	ResultString = 'OK'

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    UT_COMMON_CMD
    	Cmd = ACTIVATE_BEARER (1)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList
    		Ut_Parameter_Type
    			Name = 'Cid'
    			Value = '1'

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 421
    outStr = Timer: t_Wait, Duration: 10s, Started: 13:20:12

    UT_SYSTEM_REQ
    	Cmd
    		AT = 'AT+CGACT=1,1'
    	CnfRequired = NO_CNF_REQUIRED (0)

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = ng-5G-S-TMSI-Part1 = 100000111000010001101000101011001111000
    			establishmentCause = mo-Data
    			spare = 0

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 849
    				Subframe
    					Number = 4
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 2
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    							establishmentCause = mo_Data (4)
    							spare = 0'B

    timerEvent = 7
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 424
    outStr = Timer: t_Wait, Stopped: 13:20:13

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 849
    				Subframe
    					Number = 4
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 2
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    								establishmentCause = mo_Data (4)
    								spare = 0'B
    		Nas = Omit

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x0 [ 0 ]
    	sr_ngksi
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		AMF Set ID = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	nas_msg_cont
    		iei [8 bits] = 0x71 [ 113 ]
    		iel [16 bits] = 0x11 [ 17 ]
    		NAS message container = 0xC83C155F8238BD015948948A18A6C838AD

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			dedicatedNAS-Message = 7E01DA31C25E027E004C000007F40041C2345678710011C83C155F8238BD015948948A18A6C838AD
    			ng-5G-S-TMSI-Value = ng-5G-S-TMSI-Part2 = 000000000
    			nonCriticalExtension
    				nonCriticalExtension
    					ul-RRC-Segmentation-r16 = true

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 854
    				Subframe
    					Number = 0
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF = Omit
    								guami_Type = Omit
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E01DA31C25E027E004C000007F40041C2345678710011C83C155F8238BD015948948A18A6C838AD'O
    								ng_5G_S_TMSI_Value
    									ng_5G_S_TMSI_Part2 = 000000000'B
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									iab_NodeIndication_r16 = Omit
    									idleMeasAvailable_r16 = Omit
    									ue_MeasurementsAvailable_r16 = Omit
    									mobilityHistoryAvail_r16 = Omit
    									mobilityState_r16 = Omit
    									nonCriticalExtension
    										ul_RRC_Segmentation_r16 = true_ (0)
    										nonCriticalExtension = Omit

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x0 [ 0 ]
    	sr_ngksi
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		AMF Set ID = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	pdu_sess_st
    		iei [8 bits] = 0x50 [ 80 ]
    		iel [8 bits] = 0x2 [ 2 ]
    		PSI(0) - spare coded as zero [1 bit] = 0x0 [ 0 ]
    		psi2 [1 bit] = 0x0 [ 0 ]
    		psi3 [1 bit] = 0x0 [ 0 ]
    		psi4 [1 bit] = 0x0 [ 0 ]
    		psi5 [1 bit] = 0x0 [ 0 ]
    		psi6 [1 bit] = 0x0 [ 0 ]
    		psi7 [1 bit] = 0x1 [ 1 ]
    		psi8 [1 bit] = 0x0 [ 0 ]
    		psi9 [1 bit] = 0x0 [ 0 ]
    		psi10 [1 bit] = 0x0 [ 0 ]
    		psi11 [1 bit] = 0x0 [ 0 ]
    		psi12 [1 bit] = 0x0 [ 0 ]
    		psi13 [1 bit] = 0x0 [ 0 ]
    		psi14 [1 bit] = 0x0 [ 0 ]
    		psi15 [1 bit] = 0x0 [ 0 ]
    		psi16 [1 bit] = 0x0 [ 0 ]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 854
    				Subframe
    					Number = 0
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF = Omit
    									guami_Type = Omit
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E01DA31C25E027E004C000007F40041C2345678710011C83C155F8238BD015948948A18A6C838AD'O
    									ng_5G_S_TMSI_Value
    										ng_5G_S_TMSI_Part2 = 000000000'B
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										iab_NodeIndication_r16 = Omit
    										idleMeasAvailable_r16 = Omit
    										ue_MeasurementsAvailable_r16 = Omit
    										mobilityHistoryAvail_r16 = Omit
    										mobilityState_r16 = Omit
    										nonCriticalExtension
    											ul_RRC_Segmentation_r16 = true_ (0)
    											nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000002'O
    				Pdu
    					Msg
    						service_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001100'B
    							serviceType = 0000'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							s_TMSI
    								iei = Omit
    								iel = '0007'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 100'B
    								otherDigits = '0041C2345678'O
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							allowedPDUSessionStatus = Omit
    							nasMsg
    								iei = '71'O
    								iel = '0011'O
    								replayedNASMsgContainerValue = 'C83C155F8238BD015948948A18A6C838AD'O
    							ueRequestType = Omit
    							pagingRestrict = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								service_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01001100'B
    									serviceType = 0000'B
    									ngKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									s_TMSI
    										iei = Omit
    										iel = '0007'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 100'B
    										otherDigits = '0041C2345678'O
    									ulDataStatus = Omit
    									pduSessionStatus
    										iei = '50'O
    										iel = '02'O
    										psi0_7 = 00000010'B
    										psi8_15 = 00000000'B
    										spare = Omit
    									allowedPDUSessionStatus = Omit
    									nasMsg = Omit
    									ueRequestType = Omit
    									pagingRestrict = Omit
    							PiggybackedPduList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 00101101010110111011101100000010010111001000001000000101000000001101011111010011000110101011011100101100100110111110011101101010'B
    					KUPint = 11100111100000010001010101100001011011001001110100000010101010100000101100010100111100100011011000101100101000101000000001011110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 00100101111010000100101001010010001011111111110111010011000011110000100100011110111010001110011000110111010101100000000110101111'B
    					KUPenc = 01111001100001101100110100001100101011010000000010111001101010011001100010000101010011100110111101100011110001011010101100011110'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea1
    					integrityProtAlgorithm = nia1

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea1 (1)
    										integrityProtAlgorithm = nia1 (1)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 869
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 869
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						service_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001110'B
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							eapMessage = Omit
    							t3448 = Omit
    							ngAddRequestResult = Omit
    							forbidTAIList_Roaming = Omit
    							forbidTAIList_RegProvService = Omit
    					PiggybackedPduList = Omit

    SERVICE ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4E [ 78 ]

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 1585
    outStr = Timer: t_Wait, Duration: 8s, Started: 13:20:13

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E0235C34693026D81A5

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E0235C34693026D81A5'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0237F932B50354BD28D00F1FA6B68860667D888FF45424F9718B6E6875B9009253F51CC22D08B09D0C904717B76A84BFC5D0A4CBC7D895C0CACC6CBE1D816C7C73BE37DB06965C81A1BE29B03A859CDDE0F03363C7F10B4B

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 871
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0237F932B50354BD28D00F1FA6B68860667D888FF45424F9718B6E6875B9009253F51CC22D08B09D0C904717B76A84BFC5D0A4CBC7D895C0CACC6CBE1D816C7C73BE37DB06965C81A1BE29B03A859CDDE0F03363C7F10B4B'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    PDU SESSION ESTABLISHMENT REQUEST
    	Extended protocol discriminator = 0x2E [ 46 ]
    	PDU session ID [8 bits] = 0x1 [ 1 ]
    	PTI [8 bits] = 0x1 [ 1 ]
    	pdu_sesn_est_req_msg_id [8 bits] = 0xC1 [ 193 ]
    	int_pro_max_dr
    		max_up = 0xFF [ 255 ]
    		max_dl = 0xFF [ 255 ]
    	pdu_sesn_typ
    		iei [4 bits] = 0x9 [ 9 ]
    		Value [4 bits] = 0x3 [ 3 ]
    	ssc_mode
    		iei [4 bits] = 0xA [ 10 ]
    		Value [4 bits] = 0x1 [ 1 ]
    	fivegsm_capability
    		iei [8 bits] = 0x28 [ 40 ]
    		iel [8 bits] = 0x1 [ 1 ]
    		Spare bits [6 bits] = 0x0 [ 0 ]
    		mh6_pdu [1 bit] = 0x0 [ 0 ]
    		rqos [1 bit] = 0x0 [ 0 ]
    	extd_prt_config_opt
    		iei [8 bits] = 0x7B [ 123 ]
    		iel [16 bits] = 0x30 [ 48 ]
    		ext [1 bit] = 0x1 [ 1 ]
    		Spare bits [4 bits] = 0x0 [ 0 ]
    		config_protocol [3 bits] = 0x0 [ 0 ]
    		identifier1 = 0x8021 [ 32801 ]
    		length_identifier1 = 0x10 [ 16 ]
    		identifier1_contents = 0x01000010810600000000830600000000
    		identifier2 = 0x000D [ 13 ]
    		length_identifier2 = 0x00 [ 0 ]
    		identifier3 = 0x0003 [ 3 ]
    		length_identifier3 = 0x00 [ 0 ]
    		identifier4 = 0x000A [ 10 ]
    		length_identifier4 = 0x00 [ 0 ]
    		identifier5 = 0x0005 [ 5 ]
    		length_identifier5 = 0x00 [ 0 ]
    		identifier6 = 0x0010 [ 16 ]
    		length_identifier6 = 0x00 [ 0 ]
    		identifier6_contents = 0x [ 0 ]
    		identifier7 = 0x0011 [ 17 ]
    		length_identifier7 = 0x00 [ 0 ]
    		identifier7_contents = 0x [ 0 ]
    		identifier8 = 0x0017 [ 23 ]
    		length_identifier8 = 0x01 [ 1 ]
    		identifier8_contents = 0x01 [ 1 ]
    		iei [8 bits] = 0x0 [ 0 ]
    		iel [8 bits] = 0x23 [ 35 ]
    		sessionpairid = 0x00 [ 0 ]

    UL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x67 [ 103 ]
    	Payload container type
    		payload_typ_val [4 bits] = 0x1 [ 1 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Payload container
    		iel [16 bits] = 0x3E [ 62 ]
    		Contents = 0x2E0101C1FFFF93A12801007B00308080211001000010810600000000830600000000000D00000300000A0000050000100000110000170101002300002400
    	PDU session ID
    		iei [8 bits] = 0x12 [ 18 ]
    		Value = 0x01 [ 1 ]
    	Request type
    		iei [4 bits] = 0x8 [ 8 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x1 [ 1 ]
    	DNN
    		iei [8 bits] = 0x25 [ 37 ]
    		iel [8 bits] = 0x9 [ 9 ]
    		DNN value = 0x08696E7465726E6574 [ <0x08>internet ]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 871
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000003'O
    				Pdu
    					Msg
    						ul_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01100111'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '003E'O
    								payload = '2E0101C1FFFF93A12801007B00308080211001000010810600000000830600000000000D00000300000A0000050000100000110000170101002300002400'O
    							pduSessionId
    								iei = '12'O
    								sessionId = '01'O
    							oldPDUSessionId = Omit
    							requestType
    								iei = '8'H
    								spare = 0'B
    								requestValue = 001'B
    							s_NSSAI = Omit
    							dnn
    								iei = '25'O
    								iel = '09'O
    								dnnValue = '08696E7465726E6574'O
    							additionalInfo = Omit
    							maPDUSessionInfo = Omit
    							releaseAssistanceInd = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								pdu_Session_Establishment_Request
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '01'O
    									procedureTransactionIdentifier = '01'O
    									messageType = 11000001'B
    									integrityProtMaxDataRate
    										iei = Omit
    										maxDataRateUL = 'FF'O
    										maxDataRateDL = 'FF'O
    									pduSessionType
    										iei = '9'H
    										spare = 0'B
    										typeValue = 011'B
    									sscMode
    										iei = 'A'H
    										spare = 0'B
    										sscModeValue = 001'B
    									smCapability
    										iei = '28'O
    										iel = '01'O
    										tpmic = 0'B
    										atsssST = 0000'B
    										ept_S1 = 0'B
    										mh6_PDU = 0'B
    										rQoS = 0'B
    										spareBits = Omit
    										apmqf = Omit
    										spare = Omit
    									maxNumPacketFilters = Omit
    									alwaysOnPDUSessionReq = Omit
    									smPDU_RequestContainer = Omit
    									extdProtocolConfigurationOptions
    										iei = '7B'O
    										iel = '0030'O
    										ext = 1'B
    										spare = 0000'B
    										configProtocol = 000'B
    										pco
    											ProtocolContainer
    												protocolID = '8021'O
    												protocolLength = '10'O
    												protocolLongLength = Omit
    												content = '01000010810600000000830600000000'O
    											ProtocolContainer
    												protocolID = '000D'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0003'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '000A'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0005'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0010'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0011'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0017'O
    												protocolLength = '01'O
    												protocolLongLength = Omit
    												content = '01'O
    											ProtocolContainer
    												protocolID = '0023'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    											ProtocolContainer
    												protocolID = '0024'O
    												protocolLength = '00'O
    												protocolLongLength = Omit
    												content = Omit
    									ipHeaderCompressionConfig = Omit
    									ds_TT_EthernetPortMACAddr = Omit
    									ueDS_TT_ResidenceTime = Omit
    									portManagementInfoContainer = Omit
    									ethernetHeaderCompressConfig = Omit
    									suggestedInterfaceId = Omit
    									serviceLvlAA = Omit
    									requestedMBS = Omit
    									pduSessionPairId = Omit
    									rsn = Omit
    							PiggybackedPduList = Omit

    timerEvent = 7
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 1599
    outStr = Timer: t_Wait, Stopped: 13:20:13

    summary = Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    MATCH_MISMATCH
    	Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    		PDUType = Internet_DNN (4)

    ConstraintMismatch::Received:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 011'B
    		typeValue
    ConstraintMismatch::Expected:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 101'B
    		typeValue

    ConstraintMismatch::Received:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 001'B
    		requestValue
    ConstraintMismatch::Expected:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 011'B
    		requestValue

    ConstraintMismatch::Received:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 001'B
    		requestValue
    ConstraintMismatch::Expected:
    summary = Message Mismatch: B3_Type
    MATCH_MISMATCH
    	Message Mismatch: B3_Type = 100'B
    		requestValue

    summary = Message Mismatch: PDU_PDN_DNN_Type
    MATCH_MISMATCH
    	Message Mismatch: PDU_PDN_DNN_Type
    		PDU_PDN_DNN_Type = IMS_DNN (3)

    IP_ConfigReq_Type
    	StartPDN
    		PdnId = PDN_3 (2)
    		DrbInfo
    			Nr5GC
    				CellId = nr_Cell1 (1)
    				QosFlow
    					PDU_SessionId = 1
    					QFI = 1

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId = Omit
    		Ind = Omit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		ICMPv6_ServerAddress = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId = Omit
    		Ind = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 67
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId = Omit
    		Ind = Omit

    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    			Port = 53
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 67
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    			Port = 53
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    			Port = 67
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId = Omit
    		Ind = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    IP_SOCKET_IND
    	CTRL
    		ConnectionId = Omit
    		Ind = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId = Omit
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_Indication_Type
    	Cnf = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							Config
    								SdapConfig
    									Pdu_SessionId = 1
    									Sdap_HeaderDL = Absent (1)
    									Sdap_HeaderUL = Present (0)
    									MappedQoS_Flows
    										IntegerType = 1
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = False
    												OutOfOrderDelivery = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms30 (5)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms30 (6)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 5
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 00101101010110111011101100000010010111001000001000000101000000001101011111010011000110101011011100101100100110111110011101101010'B
    					KUPint = 11100111100000010001010101100001011011001001110100000010101010100000101100010100111100100011011000101100101000101000000001011110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 00100101111010000100101001010010001011111111110111010011000011110000100100011110111010001110011000110111010101100000000110101111'B
    					KUPenc = 01111001100001101100110100001100101011010000000010111001101010011001100010000101010011100110111101100011110001011010101100011110'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 3
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 2
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												reestablishPDCP = Omit
    												discardOnPDCP = Omit
    												pdcp_Config = Omit
    												srb_Identity_v1700 = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												cnAssociation
    													sdap_Config
    														pdu_Session = 1
    														sdap_HeaderDL = absent (1)
    														sdap_HeaderUL = present_ (0)
    														defaultDRB = True
    														mappedQoS_FlowsToAdd
    															IntegerType = 1
    														mappedQoS_FlowsToRelease = Omit
    												drb_Identity = 2
    												reestablishPDCP = Omit
    												recoverPDCP = Omit
    												pdcp_Config
    													drb
    														discardTimer = infinity_ (15)
    														pdcp_SN_SizeUL = len18bits (1)
    														pdcp_SN_SizeDL = len18bits (1)
    														headerCompression
    															notUsed = Null
    														integrityProtection = Omit
    														statusReportRequired = true_ (0)
    														outOfOrderDelivery = Omit
    													moreThanOneRLC = Omit
    													t_Reordering = Omit
    													cipheringDisabled = Omit
    													discardTimerExt_r16 = Omit
    													moreThanTwoRLC_DRB_r16 = Omit
    													ethernetHeaderCompression_r16 = Omit
    													survivalTimeStateSupport_r17 = Omit
    													uplinkDataCompression_r17 = Omit
    													discardTimerExt2_r17 = Omit
    													initialRX_DELIV_r17 = Omit
    												daps_Config_r16 = Omit
    										drb_ToReleaseList = Omit
    										securityConfig
    											securityAlgorithmConfig
    												cipheringAlgorithm = nea1 (1)
    												integrityProtAlgorithm = nia1 (1)
    											keyToUse = master (0)
    										mrb_ToAddModList_r17 = Omit
    										mrb_ToReleaseList_r17 = Omit
    										srb4_ToAddMod_r17 = Omit
    										srb4_ToRelease_r17 = Omit
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '4002B242316475CC320C3CC81212832F3000'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						dl_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01101000'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '0000'O
    								payload = ''O
    							pduSessionId
    								iei = '12'O
    								sessionId = '01'O
    							additionalInfo = Omit
    							gmmCause = Omit
    							backOffTimerValue = Omit
    							lowerBoundTimerValue = Omit
    					PiggybackedPduList
    						NG_NAS_DL_Pdu_Type
    							Msg
    								pdu_Session_Establishment_Accept
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '01'O
    									procedureTransactionIdentifier = '01'O
    									messageType = 11000010'B
    									sscMode
    										iei = Omit
    										spare = 0'B
    										sscModeValue = 001'B
    									pduSessionType
    										iei = Omit
    										spare = 0'B
    										typeValue = 011'B
    									authorizedQoSRules
    										iei = Omit
    										iel = '0009'O
    										listofQoSRules
    											QoS_Rule
    												identifier = '01'O
    												iel = '0006'O
    												ruleOperationCode = 001'B
    												dqrBit = 1'B
    												numOfPacketFilters = 0001'B
    												packetFilterList
    													new
    														NG_PacketFilter_Type2
    															spare = 00'B
    															direction = 11'B
    															packetFilterId = 0001'B
    															len = '01'O
    															contents = '01'O
    												precedence = 'FF'O
    												spare = 0'B
    												segregation = 0'B
    												flowIdentifier = 000001'B
    									sessionAMBR
    										iei = Omit
    										iel = '06'O
    										unitDL = '05'O
    										downlink = '0004'O
    										unitUL = '05'O
    										uplink = '0004'O
    									gsmCause = Omit
    									pduAddress
    										iei = '29'O
    										iel = '0D'O
    										spare = 0000'B
    										si16LLA = 0'B
    										typeValue = 011'B
    										adressInfo = '0000000014285731C0A8001C'O
    										ipv6Address = Omit
    									rqTimerValue = Omit
    									s_NSSAI
    										iei = '22'O
    										lvPart
    											iel = '01'O
    											vPart
    												sst = '01'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    									alwaysOnPDUSessionInd = Omit
    									mappedEPSContexts = Omit
    									eapMessage = Omit
    									authorizedQoSFlowDescr
    										iei = '79'O
    										iel = '0006'O
    										listofFlows
    											QoS_Flow
    												spare2 = 00'B
    												qfi = 000001'B
    												operationCode = 001'B
    												spare6 = 000000'B
    												eBit = 1'B
    												numOfParameters = 000001'B
    												parameterList
    													QoSParameters
    														id = '01'O
    														lenOfContent = '01'O
    														qosParam = '09'O
    									extdProtocolConfigurationOptions = Omit
    									dnn
    										iei = '25'O
    										iel = '09'O
    										dnnValue = '08696E7465726E6574'O
    									ngs_NetworkFeatureSupport = Omit
    									servingPLMNRateControl = Omit
    									atsssContainer = Omit
    									controlPlaneOnlyIndication = Omit
    									ipHeaderCompressionConfig = Omit
    									ethernetHeaderCompressConfig = Omit
    									serviceLvlAA = Omit
    									receivedMBS = Omit
    							PiggybackedPduList = Omit

    PDU SESSION ESTABLISHMENT ACCEPT
    	Extended protocol discriminator = 0x2E [ 46 ]
    	PDU session ID [8 bits] = 0x1 [ 1 ]
    	PTI [8 bits] = 0x1 [ 1 ]
    	PDU SESSION ESTABLISHMENT ACCEPT message identity [8 bits] = 0xC2 [ 194 ]
    	Selected SSC mode
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		SSC mode value [3 bits] = 0x1 [ 1 ]
    	Selected PDU session type
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		PDU session type value [3 bits] = 0x3 [ 3 ]
    	Authorized Qos rules
    		iel [16 bits] = 0x9 [ 9 ]
    			identifier = 0x01 [ 1 ]
    			length_of_qos_rule [16 bits] = 0x6 [ 6 ]
    			rule_op_code [3 bits] = 0x1 [ 1 ]
    			dqr_bit [1 bit] = 0x1 [ 1 ]
    			numof_pack_flt [4 bits] = 0x1 [ 1 ]
    			spare2bits1 [2 bits] = 0x0 [ 0 ]
    			pkt_flt_dir1 [2 bits] = 0x3 [ 3 ]
    			pkt_flt_id1 [4 bits] = 0x1 [ 1 ]
    			len_pkt_flt_con1 [8 bits] = 0x1 [ 1 ]
    			pkt_flt_con1 = 0x01 [ 1 ]
    			qrs_rule_pre = 0xFF [ 255 ]
    			Spare bits [1 bit] = 0x0 [ 0 ]
    			segregation [1 bit] = 0x0 [ 0 ]
    			qrs_flow_iden [6 bits] = 0x1 [ 1 ]
    	Session AMBR
    		length [8 bits] = 0x6 [ 6 ]
    		Unit for Session-AMBR for downlink = 0x05 [ 5 ]
    		Session-AMBR for downlink = 0x0004 [ 4 ]
    		Unit for Session-AMBR for uplink = 0x05 [ 5 ]
    		Session-AMBR for uplink = 0x0004 [ 4 ]
    	PDU address
    		iei [8 bits] = 0x29 [ 41 ]
    		iel [8 bits] = 0xD [ 13 ]
    		Spare bits [4 bits] = 0x0 [ 0 ]
    		SMF's IPv6 link local address field presence [1 bit] = 0x0 [ 0 ]
    		PDU session type value [3 bits] = 0x3 [ 3 ]
    		ipv4 = 0x0000000014285731C0A8001C
    	s_nssai
    		iei [8 bits] = 0x22 [ 34 ]
    		iel [8 bits] = 0x1 [ 1 ]
    		sst = 0x01 [ 1 ]
    	auth_qos_flow
    		iei [8 bits] = 0x79 [ 121 ]
    		flowiel [16 bits] = 0x6 [ 6 ]
    			Spare bits [2 bits] = 0x0 [ 0 ]
    			QFI [6 bits] = 0x1 [ 1 ]
    			opn_cod [3 bits] = 0x1 [ 1 ]
    			spar [5 bits] = 0x0 [ 0 ]
    			spare_1 [1 bit] = 0x0 [ 0 ]
    			e [1 bit] = 0x1 [ 1 ]
    			numof_par [6 bits] = 0x1 [ 1 ]
    			parameter1_identifier [8 bits] = 0x1 [ 1 ]
    			parameter1_length [8 bits] = 0x1 [ 1 ]
    			contents1 = 0x09 [ 9 ]
    	DNN
    		iei [8 bits] = 0x25 [ 37 ]
    		iel [8 bits] = 0x9 [ 9 ]
    		DNN value = 0x08696E7465726E6574 [ <0x08>internet ]

    DL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	fivegs_mm_mt [8 bits] = 0x68 [ 104 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Payload container type
    		payload_typ_val [4 bits] = 0x1 [ 1 ]
    	Payload container
    		iel [16 bits] = 0x3D [ 61 ]
    		Contents = 0x2E0101C213000901000631310101FF0106050004050004290D030000000014285731C0A8001C220101790006012041010109250908696E7465726E6574
    	PDU session ID
    		iei [8 bits] = 0x12 [ 18 ]
    		Value = 0x01 [ 1 ]

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						cnAssociation = sdap-Config =
    							pdu-Session = 1
    							sdap-HeaderDL = absent
    							sdap-HeaderUL = present
    							defaultDRB = TRUE
    							mappedQoS-FlowsToAdd = SEQUENCE OF QFI
    								QFI(1) = 1
    						drb-Identity = 2
    						pdcp-Config
    							drb
    								discardTimer = infinity
    								pdcp-SN-SizeUL = len18bits
    								pdcp-SN-SizeDL = len18bits
    								headerCompression = notUsed = NULL
    								statusReportRequired = true
    				securityConfig
    					securityAlgorithmConfig
    						cipheringAlgorithm = nea1
    						integrityProtAlgorithm = nia1
    					keyToUse = master
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    						RLC-BearerConfig(1)
    							logicalChannelIdentity = 5
    							servedRadioBearer = drb-Identity = 2
    							rlc-Config = am =
    								ul-AM-RLC
    									sn-FieldLength = size18
    									t-PollRetransmit = ms30
    									pollPDU = p32768
    									pollByte = kB750
    									maxRetxThreshold = t8
    								dl-AM-RLC
    									sn-FieldLength = size18
    									t-Reassembly = ms30
    									t-StatusProhibit = ms30
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 1
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 1
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    						RLC-BearerConfig(2)
    							logicalChannelIdentity = 2
    							servedRadioBearer = srb-Identity = 2
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 3
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 0
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E025B90C6830355C0F0E97D10B8309989A3449BED6D6969F38F6AD3EF397DD11575EDA027731650EAE8AD31B90C4631A0BE0BBA0B8CEE8DAADA9FF525D153A4B7616BEA8AA1E1F1D6BE295E

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList
    										SRB_ToAddMod
    											srb_Identity = 2
    											reestablishPDCP = Omit
    											discardOnPDCP = Omit
    											pdcp_Config = Omit
    											srb_Identity_v1700 = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList
    										DRB_ToAddMod
    											cnAssociation
    												sdap_Config
    													pdu_Session = 1
    													sdap_HeaderDL = absent (1)
    													sdap_HeaderUL = present_ (0)
    													defaultDRB = True
    													mappedQoS_FlowsToAdd
    														IntegerType = 1
    													mappedQoS_FlowsToRelease = Omit
    											drb_Identity = 2
    											reestablishPDCP = Omit
    											recoverPDCP = Omit
    											pdcp_Config
    												drb
    													discardTimer = infinity_ (15)
    													pdcp_SN_SizeUL = len18bits (1)
    													pdcp_SN_SizeDL = len18bits (1)
    													headerCompression
    														notUsed = Null
    													integrityProtection = Omit
    													statusReportRequired = true_ (0)
    													outOfOrderDelivery = Omit
    												moreThanOneRLC = Omit
    												t_Reordering = Omit
    												cipheringDisabled = Omit
    												discardTimerExt_r16 = Omit
    												moreThanTwoRLC_DRB_r16 = Omit
    												ethernetHeaderCompression_r16 = Omit
    												survivalTimeStateSupport_r17 = Omit
    												uplinkDataCompression_r17 = Omit
    												discardTimerExt2_r17 = Omit
    												initialRX_DELIV_r17 = Omit
    											daps_Config_r16 = Omit
    									drb_ToReleaseList = Omit
    									securityConfig
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    										keyToUse = master (0)
    									mrb_ToAddModList_r17 = Omit
    									mrb_ToReleaseList_r17 = Omit
    									srb4_ToAddMod_r17 = Omit
    									srb4_ToRelease_r17 = Omit
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '4002B242316475CC320C3CC81212832F3000'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E025B90C6830355C0F0E97D10B8309989A3449BED6D6969F38F6AD3EF397DD11575EDA027731650EAE8AD31B90C4631A0BE0BBA0B8CEE8DAADA9FF525D153A4B7616BEA8AA1E1F1D6BE295E'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 904
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 904
    				Subframe
    					Number = 2
    				HSFN
    					Number = 2
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    summary = Message Mismatch: PDU_PDN_DNN_Type
    MATCH_MISMATCH
    	Message Mismatch: PDU_PDN_DNN_Type
    		PDU_PDN_DNN_Type = IMS_DNN (3)

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 487
    outStr = Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 13:20:14

    IP PDU
    	IP Header
    		IP Version = IPv6
    		Traffic Class = 0
    		Flow Label =  = 0x00000
    		Payload Length = 8 (in octets)
    		Protocol = 58(ICMP for IPv6)
    		Hop Limit = 255
    		Source Address = 0xfe80:0x0:0x0:0x0:0x0:0x0:0x1428:0x5731
    		Destination Address = 0xff02:0x0:0x0:0x0:0x0:0x0:0x0:0x2
    		ICMPv6
    			Type = 133(Router Solicitation)
    			Code = 0
    			CheckSum = 0x11de
    			Router Solicitation
    				Reserved = 0
    				Options
    					Type = 0 - Unknown Options Type
    					Length = 0 (in 8 octets)
    	Length = Encoded Hex data not long enough for decodded message type
    		Hex Data Length = 48
    		Decode Data Length = 50

    Details = RX at [FN,SFN] = [913 2], First 8 bytes of RX DataUnit = 0x60 0x00 0x00 0x00 0x00 0x08 0x3a 0xff

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    						ScopeId = Omit
    				Port = Omit
    		Ind
    			ICMP
    				RecvFrom
    					Buffer = '850011DE00000000'O
    					DrbInfo
    						Nr5GC
    							CellId = nr_Cell1 (1)
    							QosFlow
    								PDU_SessionId = 1
    								QFI = 1

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    							ScopeId = Omit
    					Port = Omit
    			Ind
    				ICMP
    					RecvFrom
    						Buffer = '850011DE00000000'O
    						DrbInfo
    							Nr5GC
    								CellId = nr_Cell1 (1)
    								QosFlow
    									PDU_SessionId = 1
    									QFI = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 67
    				Remote
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    							ScopeId = Omit
    					Port = AnyValue
    			Ind
    				UDP
    					RecvFrom
    						Buffer
    						DrbInfo
    							Nr5GC
    								CellId
    								QosFlow
    									PDU_SessionId
    									QFI

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    						ScopeId = Omit
    				Port = Omit
    		Ind
    			ICMP
    				RecvFrom
    					Buffer = '850011DE00000000'O
    					DrbInfo
    						Nr5GC
    							CellId = nr_Cell1 (1)
    							QosFlow
    								PDU_SessionId = 1
    								QFI = 1

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    						ScopeId = Omit
    				Port = Omit
    		Req
    			ICMP
    				SendTo
    					Buffer = '86005DF14000FFFF000000000000000003044040FFFFFFFFFFFFFFFF0000000030000000000000020000000000000000'O

    IP PDU
    	IP Header
    		IP Version = IPv6
    		Traffic Class = 0
    		Flow Label =  = 0x00000
    		Payload Length = 48 (in octets)
    		Protocol = 58(ICMP for IPv6)
    		Hop Limit = 255
    		Source Address = 0xfe80:0x0:0x0:0x0:0x0:0x0:0x0:0x2
    		Destination Address = 0xfe80:0x0:0x0:0x0:0x0:0x0:0x1428:0x5731
    		ICMPv6
    			Type = 134(Router Advertisement)
    			Code = 0
    			CheckSum = 0x5df1
    			Router Advertisement
    				Cur Hop Limit = 64
    				M = 0
    				O = 0
    				Reserved = 0
    				Router Lifetime = 65535
    				Reachable Time = 0
    				Retrans Timer = 0
    				Options
    					Type = 3(Prefix Information)
    					Length = 4 (in 8 octets)
    					Prefix Information
    						Prefix Length = 64
    						L = 1
    						A = 187
    						Reserved1 = 4
    						Valid Lifetime = 4294967295
    						Preferred Lifetime = 4294967295
    						Reserved2 = 0
    						Prefix = 0x3000:0x0:0x0:0x2:0x0:0x0:0x0:0x0

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:1428:5731'
    						ScopeId = Omit
    				Port = Omit
    		Req
    			ICMP
    				SendTo
    					Buffer = '86005DF14000FFFF000000000000000003044040FFFFFFFFFFFFFFFF0000000030000000000000020000000000000000'O

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 489
    outStr = Timer: t_WaitForUPlaneSignalling, Expired: 13:20:15

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 1
    				Subframe
    					Number = 1
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					SymbolOffset = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 305
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 13:20:15

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 31
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 31
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000001'B

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 31
    			Subframe
    				Number = 2
    			HSFN
    				Number = 3
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 31
    			Subframe
    				Number = 2
    			HSFN
    				Number = 3
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 31
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 31
    			Subframe
    				Number = 7
    			HSFN
    				Number = 3
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 31
    				Subframe
    					Number = 7
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 36
    			Subframe
    				Number = 7
    			HSFN
    				Number = 3
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 36
    				Subframe
    					Number = 7
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 37
    			Subframe
    				Number = 2
    			HSFN
    				Number = 3
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 37
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 313
    outStr = Timer: t_Timer, Expired: 13:20:16

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common\CommonDefs.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 616
    outStr = Timer: t_Delay, Duration: 1s, Started: 13:20:16

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common\CommonDefs.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 617
    outStr = Timer: t_Delay, Expired: 13:20:17

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 225
    				Subframe
    					Number = 0
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					SymbolOffset = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    PCCH-Message
    	message = c1 = paging =
    		pagingRecordList = SEQUENCE OF PagingRecord
    			PagingRecord(1)
    				ue-Identity = ng-5G-S-TMSI = 000000000100000111000010001101000101011001111000

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 240
    				Subframe
    					Number = 0
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 2
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Paging
    			Paging
    				message_
    					c1
    						paging
    							pagingRecordList
    								PagingRecord
    									ue_Identity
    										ng_5G_S_TMSI = 000000000100000111000010001101000101011001111000'B
    									accessType = Omit
    							lateNonCriticalExtension = Omit
    							nonCriticalExtension = Omit
    			SlotOffsetList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = ng-5G-S-TMSI-Part1 = 100000111000010001101000101011001111000
    			establishmentCause = mt-Access
    			spare = 0

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 246
    				Subframe
    					Number = 1
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 6
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    							establishmentCause = mt_Access (2)
    							spare = 0'B

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 246
    				Subframe
    					Number = 1
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 6
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    								establishmentCause = mt_Access (2)
    								spare = 0'B
    		Nas = Omit

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x2 [ 2 ]
    	sr_ngksi
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		AMF Set ID = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	nas_msg_cont
    		iei [8 bits] = 0x71 [ 113 ]
    		iel [16 bits] = 0x11 [ 17 ]
    		NAS message container = 0xA67FF2C3DBADB3B0C99C2B09E1E4D4D05D

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			dedicatedNAS-Message = 7E01C90A95A3047E004C200007F40041C2345678710011A67FF2C3DBADB3B0C99C2B09E1E4D4D05D
    			ng-5G-S-TMSI-Value = ng-5G-S-TMSI-Part2 = 000000000
    			nonCriticalExtension
    				nonCriticalExtension
    					ul-RRC-Segmentation-r16 = true

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 248
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF = Omit
    								guami_Type = Omit
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E01C90A95A3047E004C200007F40041C2345678710011A67FF2C3DBADB3B0C99C2B09E1E4D4D05D'O
    								ng_5G_S_TMSI_Value
    									ng_5G_S_TMSI_Part2 = 000000000'B
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									iab_NodeIndication_r16 = Omit
    									idleMeasAvailable_r16 = Omit
    									ue_MeasurementsAvailable_r16 = Omit
    									mobilityHistoryAvail_r16 = Omit
    									mobilityState_r16 = Omit
    									nonCriticalExtension
    										ul_RRC_Segmentation_r16 = true_ (0)
    										nonCriticalExtension = Omit

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x2 [ 2 ]
    	sr_ngksi
    		nas_tsc [1 bit] = 0x0 [ 0 ]
    		NAS key set identifier [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		AMF Set ID = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]
    	pdu_sess_st
    		iei [8 bits] = 0x50 [ 80 ]
    		iel [8 bits] = 0x2 [ 2 ]
    		PSI(0) - spare coded as zero [1 bit] = 0x0 [ 0 ]
    		psi2 [1 bit] = 0x0 [ 0 ]
    		psi3 [1 bit] = 0x0 [ 0 ]
    		psi4 [1 bit] = 0x0 [ 0 ]
    		psi5 [1 bit] = 0x0 [ 0 ]
    		psi6 [1 bit] = 0x0 [ 0 ]
    		psi7 [1 bit] = 0x1 [ 1 ]
    		psi8 [1 bit] = 0x0 [ 0 ]
    		psi9 [1 bit] = 0x0 [ 0 ]
    		psi10 [1 bit] = 0x0 [ 0 ]
    		psi11 [1 bit] = 0x0 [ 0 ]
    		psi12 [1 bit] = 0x0 [ 0 ]
    		psi13 [1 bit] = 0x0 [ 0 ]
    		psi14 [1 bit] = 0x0 [ 0 ]
    		psi15 [1 bit] = 0x0 [ 0 ]
    		psi16 [1 bit] = 0x0 [ 0 ]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 248
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF = Omit
    									guami_Type = Omit
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E01C90A95A3047E004C200007F40041C2345678710011A67FF2C3DBADB3B0C99C2B09E1E4D4D05D'O
    									ng_5G_S_TMSI_Value
    										ng_5G_S_TMSI_Part2 = 000000000'B
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										iab_NodeIndication_r16 = Omit
    										idleMeasAvailable_r16 = Omit
    										ue_MeasurementsAvailable_r16 = Omit
    										mobilityHistoryAvail_r16 = Omit
    										mobilityState_r16 = Omit
    										nonCriticalExtension
    											ul_RRC_Segmentation_r16 = true_ (0)
    											nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000004'O
    				Pdu
    					Msg
    						service_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001100'B
    							serviceType = 0010'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							s_TMSI
    								iei = Omit
    								iel = '0007'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 100'B
    								otherDigits = '0041C2345678'O
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							allowedPDUSessionStatus = Omit
    							nasMsg
    								iei = '71'O
    								iel = '0011'O
    								replayedNASMsgContainerValue = 'A67FF2C3DBADB3B0C99C2B09E1E4D4D05D'O
    							ueRequestType = Omit
    							pagingRestrict = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								service_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01001100'B
    									serviceType = 0010'B
    									ngKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									s_TMSI
    										iei = Omit
    										iel = '0007'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 100'B
    										otherDigits = '0041C2345678'O
    									ulDataStatus = Omit
    									pduSessionStatus
    										iei = '50'O
    										iel = '02'O
    										psi0_7 = 00000010'B
    										psi8_15 = 00000000'B
    										spare = Omit
    									allowedPDUSessionStatus = Omit
    									nasMsg = Omit
    									ueRequestType = Omit
    									pagingRestrict = Omit
    							PiggybackedPduList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_1_3_1_2_NR5GC'

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 00101001100010110011010001010110001111010010001011110010001110001110000100011000110111100001110001100101110010011000110010011010'B
    					KUPint = 11101010000101100010000110111100010100011100111001000100001110100101010011110010010001110000101101100000000010001011101110001000'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01100000011100001110000011111001100101001101110111110011110011011000001001101010010011110101010110110111110011110001001101100101'B
    					KUPenc = 10110100110101011001010100010011000010111101110001001101100100110001100011110001100001111010110000001001011000110101001000100010'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea1
    					integrityProtAlgorithm = nia1

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea1 (1)
    										integrityProtAlgorithm = nia1 (1)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 287
    				Subframe
    					Number = 4
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 287
    				Subframe
    					Number = 4
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			SS_Config
    				Id
    					Drb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							Config
    								SdapConfig
    									Pdu_SessionId = 1
    									Sdap_HeaderDL = Absent (1)
    									Sdap_HeaderUL = Present (0)
    									MappedQoS_Flows
    										IntegerType = 1
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = False
    												OutOfOrderDelivery = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms30 (5)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms30 (6)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 5
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 00101001100010110011010001010110001111010010001011110010001110001110000100011000110111100001110001100101110010011000110010011010'B
    					KUPint = 11101010000101100010000110111100010100011100111001000100001110100101010011110010010001110000101101100000000010001011101110001000'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01100000011100001110000011111001100101001101110111110011110011011000001001101010010011110101010110110111110011110001001101100101'B
    					KUPenc = 10110100110101011001010100010011000010111101110001001101100100110001100011110001100001111010110000001001011000110101001000100010'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 2
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												reestablishPDCP = Omit
    												discardOnPDCP = Omit
    												pdcp_Config = Omit
    												srb_Identity_v1700 = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												cnAssociation
    													sdap_Config
    														pdu_Session = 1
    														sdap_HeaderDL = absent (1)
    														sdap_HeaderUL = present_ (0)
    														defaultDRB = True
    														mappedQoS_FlowsToAdd
    															IntegerType = 1
    														mappedQoS_FlowsToRelease = Omit
    												drb_Identity = 2
    												reestablishPDCP = Omit
    												recoverPDCP = Omit
    												pdcp_Config
    													drb
    														discardTimer = infinity_ (15)
    														pdcp_SN_SizeUL = len18bits (1)
    														pdcp_SN_SizeDL = len18bits (1)
    														headerCompression
    															notUsed = Null
    														integrityProtection = Omit
    														statusReportRequired = true_ (0)
    														outOfOrderDelivery = Omit
    													moreThanOneRLC = Omit
    													t_Reordering = Omit
    													cipheringDisabled = Omit
    													discardTimerExt_r16 = Omit
    													moreThanTwoRLC_DRB_r16 = Omit
    													ethernetHeaderCompression_r16 = Omit
    													survivalTimeStateSupport_r17 = Omit
    													uplinkDataCompression_r17 = Omit
    													discardTimerExt2_r17 = Omit
    													initialRX_DELIV_r17 = Omit
    												daps_Config_r16 = Omit
    										drb_ToReleaseList = Omit
    										securityConfig
    											securityAlgorithmConfig
    												cipheringAlgorithm = nea1 (1)
    												integrityProtAlgorithm = nia1 (1)
    											keyToUse = master (0)
    										mrb_ToAddModList_r17 = Omit
    										mrb_ToReleaseList_r17 = Omit
    										srb4_ToAddMod_r17 = Omit
    										srb4_ToRelease_r17 = Omit
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '400290941979802C908C591D730C830F3200'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						service_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001110'B
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							eapMessage = Omit
    							t3448 = Omit
    							ngAddRequestResult = Omit
    							forbidTAIList_Roaming = Omit
    							forbidTAIList_RegProvService = Omit
    					PiggybackedPduList = Omit

    SERVICE ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4E [ 78 ]

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						cnAssociation = sdap-Config =
    							pdu-Session = 1
    							sdap-HeaderDL = absent
    							sdap-HeaderUL = present
    							defaultDRB = TRUE
    							mappedQoS-FlowsToAdd = SEQUENCE OF QFI
    								QFI(1) = 1
    						drb-Identity = 2
    						pdcp-Config
    							drb
    								discardTimer = infinity
    								pdcp-SN-SizeUL = len18bits
    								pdcp-SN-SizeDL = len18bits
    								headerCompression = notUsed = NULL
    								statusReportRequired = true
    				securityConfig
    					securityAlgorithmConfig
    						cipheringAlgorithm = nea1
    						integrityProtAlgorithm = nia1
    					keyToUse = master
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    						RLC-BearerConfig(1)
    							logicalChannelIdentity = 2
    							servedRadioBearer = srb-Identity = 2
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 3
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 0
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    						RLC-BearerConfig(2)
    							logicalChannelIdentity = 5
    							servedRadioBearer = drb-Identity = 2
    							rlc-Config = am =
    								ul-AM-RLC
    									sn-FieldLength = size18
    									t-PollRetransmit = ms30
    									pollPDU = p32768
    									pollByte = kB750
    									maxRetxThreshold = t8
    								dl-AM-RLC
    									sn-FieldLength = size18
    									t-Reassembly = ms30
    									t-StatusProhibit = ms30
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 1
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 1
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E02C8F41E7E047F557C

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList
    										SRB_ToAddMod
    											srb_Identity = 2
    											reestablishPDCP = Omit
    											discardOnPDCP = Omit
    											pdcp_Config = Omit
    											srb_Identity_v1700 = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList
    										DRB_ToAddMod
    											cnAssociation
    												sdap_Config
    													pdu_Session = 1
    													sdap_HeaderDL = absent (1)
    													sdap_HeaderUL = present_ (0)
    													defaultDRB = True
    													mappedQoS_FlowsToAdd
    														IntegerType = 1
    													mappedQoS_FlowsToRelease = Omit
    											drb_Identity = 2
    											reestablishPDCP = Omit
    											recoverPDCP = Omit
    											pdcp_Config
    												drb
    													discardTimer = infinity_ (15)
    													pdcp_SN_SizeUL = len18bits (1)
    													pdcp_SN_SizeDL = len18bits (1)
    													headerCompression
    														notUsed = Null
    													integrityProtection = Omit
    													statusReportRequired = true_ (0)
    													outOfOrderDelivery = Omit
    												moreThanOneRLC = Omit
    												t_Reordering = Omit
    												cipheringDisabled = Omit
    												discardTimerExt_r16 = Omit
    												moreThanTwoRLC_DRB_r16 = Omit
    												ethernetHeaderCompression_r16 = Omit
    												survivalTimeStateSupport_r17 = Omit
    												uplinkDataCompression_r17 = Omit
    												discardTimerExt2_r17 = Omit
    												initialRX_DELIV_r17 = Omit
    											daps_Config_r16 = Omit
    									drb_ToReleaseList = Omit
    									securityConfig
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    										keyToUse = master (0)
    									mrb_ToAddModList_r17 = Omit
    									mrb_ToReleaseList_r17 = Omit
    									srb4_ToAddMod_r17 = Omit
    									srb4_ToRelease_r17 = Omit
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '400290941979802C908C591D730C830F3200'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E02C8F41E7E047F557C'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 311
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 311
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 316
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = True

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 317
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.VerdictCtrl = normal
    File: NR_Component_Base.ttcn [Line: 317]

    recordType = 24
    summary = Preamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 419
    text = Parameter: RRC_Measurement_NR5GC.v_MeasGapUE = Omit
    File: RRC_Measurement_NR5GC.ttcn [Line: 419]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 424
    text = Parameter: RRC_Measurement_NR5GC.v_Delay = 10
    File: RRC_Measurement_NR5GC.ttcn [Line: 424]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 450
    text = Parameter: RRC_Measurement_NR5GC.v_CellPower_Serving_FR1 = -85
    File: RRC_Measurement_NR5GC.ttcn [Line: 450]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 451
    text = Parameter: RRC_Measurement_NR5GC.v_CellPower_Leaving_FR1 = -91
    File: RRC_Measurement_NR5GC.ttcn [Line: 451]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 452
    text = Parameter: RRC_Measurement_NR5GC.v_CellPower_EntryCondition_FR1 = -79
    File: RRC_Measurement_NR5GC.ttcn [Line: 452]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 927
    text = Parameter: NR_ConfigurationSteps.v_NR_TestEnvironment = OTA
    File: NR_ConfigurationSteps.ttcn [Line: 927]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 929
    text = Parameter: NR_ConfigurationSteps.v_CnfFlag = True
    File: NR_ConfigurationSteps.ttcn [Line: 929]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 0
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 940
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].CellId = nr_Cell1
    File: NR_ConfigurationSteps.ttcn [Line: 940]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 886
    text = Parameter: NR_ConfigurationSteps.v_CurrentRefPowerLevel = -82
    File: NR_ConfigurationSteps.ttcn [Line: 886]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 893
    text = Parameter: NR_ConfigurationSteps.v_AttenuationValue = 9
    File: NR_ConfigurationSteps.ttcn [Line: 893]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 898
    text = Parameter: NR_ConfigurationSteps.v_Attenuation.Value = 9
    File: NR_ConfigurationSteps.ttcn [Line: 898]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 53
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 53]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 948
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].TimingInfo = Omit
    File: NR_ConfigurationSteps.ttcn [Line: 948]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 1
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 940
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].CellId = nr_Cell2
    File: NR_ConfigurationSteps.ttcn [Line: 940]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 886
    text = Parameter: NR_ConfigurationSteps.v_CurrentRefPowerLevel = -82
    File: NR_ConfigurationSteps.ttcn [Line: 886]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 893
    text = Parameter: NR_ConfigurationSteps.v_AttenuationValue = 18
    File: NR_ConfigurationSteps.ttcn [Line: 893]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 898
    text = Parameter: NR_ConfigurationSteps.v_Attenuation.Value = 18
    File: NR_ConfigurationSteps.ttcn [Line: 898]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 53
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 53]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 948
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].TimingInfo = Omit
    File: NR_ConfigurationSteps.ttcn [Line: 948]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 2
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common4G5G\Common4G5G_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 373
    text = Parameter: Common4G5G_Templates.v_CnfFlag = True
    File: Common4G5G_Templates.ttcn [Line: 373]

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 9
    				TimingInfo = Omit
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell2 (2)
    				Attenuation
    					Value = 18
    				TimingInfo = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    recordType = 24
    summary = Steps 1-2

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2952
    text = Parameter: NR_CellInfo.v_FreqBandIndicatorNR = 257
    File: NR_CellInfo.ttcn [Line: 2952]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 3133
    text = Parameter: NR_CellInfo.v_FreqBandIndicatorNR = 257
    File: NR_CellInfo.ttcn [Line: 3133]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 89
    text = Parameter: NR_FrequencyInit_SA.v_IsFR1 = False
    File: NR_FrequencyInit_SA.ttcn [Line: 89]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 470
    text = Parameter: RRC_Measurement_NR5GC.v_RsrpThres = 2
    File: RRC_Measurement_NR5GC.ttcn [Line: 470]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 156
    text = Parameter: NR_Measurement_Functions.v_MeasObjectToAddModList = Omit
    File: NR_Measurement_Functions.ttcn [Line: 156]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 160
    text = Parameter: NR_Measurement_Functions.v_MeasObjCounter = 0
    File: NR_Measurement_Functions.ttcn [Line: 160]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2952
    text = Parameter: NR_CellInfo.v_FreqBandIndicatorNR = 257
    File: NR_CellInfo.ttcn [Line: 2952]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 65
    text = Parameter: NR_Measurement_Functions.v_FreqBandIndicator = 257
    File: NR_Measurement_Functions.ttcn [Line: 65]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 66
    text = Parameter: NR_Measurement_Functions.v_SSB_Freq = 2054683
    File: NR_Measurement_Functions.ttcn [Line: 66]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 67
    text = Parameter: NR_Measurement_Functions.v_SubCarrierSpacing = kHz120
    File: NR_Measurement_Functions.ttcn [Line: 67]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 26
    text = Parameter: NR_FrequencyInit_SA.v_IsFDD = False
    File: NR_FrequencyInit_SA.ttcn [Line: 26]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_SysInfo_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 914
    text = Parameter: NR_SysInfo_Templates.v_TDD = True
    File: NR_SysInfo_Templates.ttcn [Line: 914]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 26
    text = Parameter: NR_FrequencyInit_SA.v_IsFDD = False
    File: NR_FrequencyInit_SA.ttcn [Line: 26]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_SysInfo_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 915
    text = Parameter: NR_SysInfo_Templates.v_FDD = False
    File: NR_SysInfo_Templates.ttcn [Line: 915]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 89
    text = Parameter: NR_FrequencyInit_SA.v_IsFR1 = False
    File: NR_FrequencyInit_SA.ttcn [Line: 89]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_SysInfo_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 916
    text = Parameter: NR_SysInfo_Templates.v_FR1 = False
    File: NR_SysInfo_Templates.ttcn [Line: 916]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 153
    text = Parameter: NR_FrequencyInit_SA.v_IsBelow1_88GHz = False
    File: NR_FrequencyInit_SA.ttcn [Line: 153]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR_CommonFrequency\NR_FrequencyInit_SA.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 26
    text = Parameter: NR_FrequencyInit_SA.v_IsFDD = False
    File: NR_FrequencyInit_SA.ttcn [Line: 26]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfoInit.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 1933
    text = Parameter: NR_CellInfoInit.v_DeriveSSB_IndexFromCell = True
    File: NR_CellInfoInit.ttcn [Line: 1933]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 174
    text = Parameter: NR_Measurement_Functions.v_MeasObjCounter = 1
    File: NR_Measurement_Functions.ttcn [Line: 174]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 559
    text = Parameter: NR_Measurement_Functions.v_SCellConfig = Omit
    File: NR_Measurement_Functions.ttcn [Line: 559]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 560
    text = Parameter: NR_Measurement_Functions.v_CellGroupId = 0
    File: NR_Measurement_Functions.ttcn [Line: 560]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common4G5G\Common4G5G_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 371
    text = Parameter: Common4G5G_Templates.v_CnfFlag = False
    File: Common4G5G_Templates.ttcn [Line: 371]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig = Omit
    									secondaryCellGroup = Omit
    									measConfig
    										measObjectToRemoveList = Omit
    										measObjectToAddModList
    											MeasObjectToAddMod
    												measObjectId = 1
    												measObject
    													measObjectNR
    														ssbFrequency = 2054683
    														ssbSubcarrierSpacing = kHz120 (3)
    														smtc1
    															periodicityAndOffset
    																sf20 = 0
    															duration = sf3 (2)
    														smtc2 = Omit
    														refFreqCSI_RS = Omit
    														referenceSignalConfig
    															ssb_ConfigMobility
    																ssb_ToMeasure
    																	setup
    																		longBitmap = 1100000000000000000000000000000000000000000000000000000000000000'B
    																deriveSSB_IndexFromCell = True
    																ss_RSSI_Measurement = Omit
    																ssb_PositionQCL_Common_r16 = Omit
    																ssb_PositionQCL_CellsToAddModList_r16 = Omit
    																ssb_PositionQCL_CellsToRemoveList_r16 = Omit
    																deriveSSB_IndexFromCellInter_r17 = Omit
    																ssb_PositionQCL_Common_r17 = Omit
    																ssb_PositionQCL_Cells_r17 = Omit
    																cca_CellsToAddModList_r17 = Omit
    																cca_CellsToRemoveList_r17 = Omit
    															csi_rs_ResourceConfigMobility = Omit
    														absThreshSS_BlocksConsolidation
    															thresholdRSRP = Omit
    															thresholdRSRQ = Omit
    															thresholdSINR = Omit
    														absThreshCSI_RS_Consolidation = Omit
    														nrofSS_BlocksToAverage = Omit
    														nrofCSI_RS_ResourcesToAverage = Omit
    														quantityConfigIndex = 1
    														offsetMO
    															rsrpOffsetSSB = dB0 (15)
    															rsrqOffsetSSB = dB0 (15)
    															sinrOffsetSSB = dB0 (15)
    															rsrpOffsetCSI_RS = dB0 (15)
    															rsrqOffsetCSI_RS = dB0 (15)
    															sinrOffsetCSI_RS = dB0 (15)
    														cellsToRemoveList = Omit
    														cellsToAddModList = Omit
    														excludedCellsToRemoveList = Omit
    														excludedCellsToAddModList = Omit
    														allowedCellsToRemoveList = Omit
    														allowedCellsToAddModList = Omit
    														freqBandIndicatorNR = 257
    														measCycleSCell = Omit
    														smtc3list_r16 = Omit
    														rmtc_Config_r16 = Omit
    														t312_r16 = Omit
    														associatedMeasGapSSB_r17 = Omit
    														associatedMeasGapCSIRS_r17 = Omit
    														smtc4list_r17 = Omit
    														measCyclePSCell_r17 = Omit
    														cellsToAddModListExt_v1710 = Omit
    														associatedMeasGapSSB2_v1720 = Omit
    														associatedMeasGapCSIRS2_v1720 = Omit
    										reportConfigToRemoveList = Omit
    										reportConfigToAddModList
    											ReportConfigToAddMod
    												reportConfigId = 1
    												reportConfig
    													reportConfigNR
    														reportType
    															eventTriggered
    																eventId
    																	eventA3
    																		a3_Offset
    																			rsrp = 2
    																		reportOnLeave = False
    																		hysteresis = 4
    																		timeToTrigger = ms320 (8)
    																		useAllowedCellList = False
    																rsType = ssb (0)
    																reportInterval = ms480 (2)
    																reportAmount = infinity_ (7)
    																reportQuantityCell
    																	rsrp = True
    																	rsrq = False
    																	sinr = False
    																maxReportCells = 8
    																reportQuantityRS_Indexes = Omit
    																maxNrofRS_IndexesToReport = Omit
    																includeBeamMeasurements = False
    																reportAddNeighMeas = Omit
    																measRSSI_ReportConfig_r16 = Omit
    																useT312_r16 = Omit
    																includeCommonLocationInfo_r16 = Omit
    																includeBT_Meas_r16 = Omit
    																includeWLAN_Meas_r16 = Omit
    																includeSensor_Meas_r16 = Omit
    																coarseLocationRequest_r17 = Omit
    																reportQuantityRelay_r17 = Omit
    										measIdToRemoveList = Omit
    										measIdToAddModList
    											MeasIdToAddMod
    												measId = 1
    												measObjectId = 1
    												reportConfigId = 1
    										s_MeasureConfig = Omit
    										quantityConfig
    											quantityConfigNR_List
    												QuantityConfigNR
    													quantityConfigCell
    														ssb_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    														csi_RS_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    													quantityConfigRS_Index
    														ssb_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    														csi_RS_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    												QuantityConfigNR
    													quantityConfigCell
    														ssb_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    														csi_RS_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    													quantityConfigRS_Index
    														ssb_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    														csi_RS_FilterConfig
    															filterCoefficientRSRP = fc4 (4)
    															filterCoefficientRSRQ = fc4 (4)
    															filterCoefficientRS_SINR = fc4 (4)
    											quantityConfigEUTRA = Omit
    											quantityConfigUTRA_FDD_r16 = Omit
    											quantityConfigCLI_r16 = Omit
    										measGapConfig = Omit
    										measGapSharingConfig = Omit
    										interFrequencyConfig_NoGap_r16 = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '041100000200'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension
    											otherConfig_v1540 = Omit
    											nonCriticalExtension
    												mrdc_SecondaryCellGroupConfig = Omit
    												radioBearerConfig2 = Omit
    												sk_Counter = Omit
    												nonCriticalExtension
    													otherConfig_v1610 = Omit
    													bap_Config_r16 = Omit
    													iab_IP_AddressConfigurationList_r16 = Omit
    													conditionalReconfiguration_r16 = Omit
    													daps_SourceRelease_r16 = Omit
    													t316_r16 = Omit
    													needForGapsConfigNR_r16 = Omit
    													onDemandSIB_Request_r16 = Omit
    													dedicatedPosSysInfoDelivery_r16 = Omit
    													sl_ConfigDedicatedNR_r16 = Omit
    													sl_ConfigDedicatedEUTRA_Info_r16 = Omit
    													targetCellSMTC_SCG_r16 = Omit
    													nonCriticalExtension = Omit
    		Nas = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 126
    text = Parameter: NasEmu5G_Main_NRNG.v_RrcPduIsPresent = True
    File: NasEmu5G_Main_NRNG.ttcn [Line: 126]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 127
    text = Parameter: NasEmu5G_Main_NRNG.v_NasPduIsPresent = False
    File: NasEmu5G_Main_NRNG.ttcn [Line: 127]

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			measConfig
    				measObjectToAddModList = SEQUENCE OF MeasObjectToAddMod
    					MeasObjectToAddMod(1)
    						measObjectId = 1
    						measObject = measObjectNR =
    							ssbFrequency = 2054683
    							ssbSubcarrierSpacing = kHz120
    							smtc1
    								periodicityAndOffset = sf20 = 0
    								duration = sf3
    							referenceSignalConfig
    								ssb-ConfigMobility
    									ssb-ToMeasure = setup = longBitmap = 1100000000000000000000000000000000000000000000000000000000000000
    									deriveSSB-IndexFromCell = TRUE
    							absThreshSS-BlocksConsolidation
    							quantityConfigIndex = 1
    							offsetMO
    								rsrpOffsetSSB  = dB0
    								rsrqOffsetSSB  = dB0
    								sinrOffsetSSB  = dB0
    								rsrpOffsetCSI-RS  = dB0
    								rsrqOffsetCSI-RS  = dB0
    								sinrOffsetCSI-RS  = dB0
    							freqBandIndicatorNR = 257
    				reportConfigToAddModList = SEQUENCE OF ReportConfigToAddMod
    					ReportConfigToAddMod(1)
    						reportConfigId = 1
    						reportConfig = reportConfigNR =
    							reportType = eventTriggered =
    								eventId = eventA3 =
    									a3-Offset = rsrp = 2
    									reportOnLeave = FALSE
    									hysteresis = 4
    									timeToTrigger = ms320
    									useAllowedCellList = FALSE
    								rsType = ssb
    								reportInterval = ms480
    								reportAmount = infinity
    								reportQuantityCell
    									rsrp = TRUE
    									rsrq = FALSE
    									sinr = FALSE
    								maxReportCells = 8
    								includeBeamMeasurements = FALSE
    				measIdToAddModList = SEQUENCE OF MeasIdToAddMod
    					MeasIdToAddMod(1)
    						measId = 1
    						measObjectId = 1
    						reportConfigId = 1
    				quantityConfig
    					quantityConfigNR-List = SEQUENCE OF QuantityConfigNR
    						QuantityConfigNR(1)
    							quantityConfigCell
    								ssb-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    								csi-RS-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    							quantityConfigRS-Index
    								ssb-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    								csi-RS-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    						QuantityConfigNR(2)
    							quantityConfigCell
    								ssb-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    								csi-RS-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    							quantityConfigRS-Index
    								ssb-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    								csi-RS-FilterConfig
    									filterCoefficientRSRP  = fc4
    									filterCoefficientRSRQ  = fc4
    									filterCoefficientRS-SINR  = fc4
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					spCellConfig
    						servCellIndex = 0
    						spCellConfigDedicated
    							tag-Id = 0
    							servingCellMO = 1
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig = Omit
    								secondaryCellGroup = Omit
    								measConfig
    									measObjectToRemoveList = Omit
    									measObjectToAddModList
    										MeasObjectToAddMod
    											measObjectId = 1
    											measObject
    												measObjectNR
    													ssbFrequency = 2054683
    													ssbSubcarrierSpacing = kHz120 (3)
    													smtc1
    														periodicityAndOffset
    															sf20 = 0
    														duration = sf3 (2)
    													smtc2 = Omit
    													refFreqCSI_RS = Omit
    													referenceSignalConfig
    														ssb_ConfigMobility
    															ssb_ToMeasure
    																setup
    																	longBitmap = 1100000000000000000000000000000000000000000000000000000000000000'B
    															deriveSSB_IndexFromCell = True
    															ss_RSSI_Measurement = Omit
    															ssb_PositionQCL_Common_r16 = Omit
    															ssb_PositionQCL_CellsToAddModList_r16 = Omit
    															ssb_PositionQCL_CellsToRemoveList_r16 = Omit
    															deriveSSB_IndexFromCellInter_r17 = Omit
    															ssb_PositionQCL_Common_r17 = Omit
    															ssb_PositionQCL_Cells_r17 = Omit
    															cca_CellsToAddModList_r17 = Omit
    															cca_CellsToRemoveList_r17 = Omit
    														csi_rs_ResourceConfigMobility = Omit
    													absThreshSS_BlocksConsolidation
    														thresholdRSRP = Omit
    														thresholdRSRQ = Omit
    														thresholdSINR = Omit
    													absThreshCSI_RS_Consolidation = Omit
    													nrofSS_BlocksToAverage = Omit
    													nrofCSI_RS_ResourcesToAverage = Omit
    													quantityConfigIndex = 1
    													offsetMO
    														rsrpOffsetSSB = dB0 (15)
    														rsrqOffsetSSB = dB0 (15)
    														sinrOffsetSSB = dB0 (15)
    														rsrpOffsetCSI_RS = dB0 (15)
    														rsrqOffsetCSI_RS = dB0 (15)
    														sinrOffsetCSI_RS = dB0 (15)
    													cellsToRemoveList = Omit
    													cellsToAddModList = Omit
    													excludedCellsToRemoveList = Omit
    													excludedCellsToAddModList = Omit
    													allowedCellsToRemoveList = Omit
    													allowedCellsToAddModList = Omit
    													freqBandIndicatorNR = 257
    													measCycleSCell = Omit
    													smtc3list_r16 = Omit
    													rmtc_Config_r16 = Omit
    													t312_r16 = Omit
    													associatedMeasGapSSB_r17 = Omit
    													associatedMeasGapCSIRS_r17 = Omit
    													smtc4list_r17 = Omit
    													measCyclePSCell_r17 = Omit
    													cellsToAddModListExt_v1710 = Omit
    													associatedMeasGapSSB2_v1720 = Omit
    													associatedMeasGapCSIRS2_v1720 = Omit
    									reportConfigToRemoveList = Omit
    									reportConfigToAddModList
    										ReportConfigToAddMod
    											reportConfigId = 1
    											reportConfig
    												reportConfigNR
    													reportType
    														eventTriggered
    															eventId
    																eventA3
    																	a3_Offset
    																		rsrp = 2
    																	reportOnLeave = False
    																	hysteresis = 4
    																	timeToTrigger = ms320 (8)
    																	useAllowedCellList = False
    															rsType = ssb (0)
    															reportInterval = ms480 (2)
    															reportAmount = infinity_ (7)
    															reportQuantityCell
    																rsrp = True
    																rsrq = False
    																sinr = False
    															maxReportCells = 8
    															reportQuantityRS_Indexes = Omit
    															maxNrofRS_IndexesToReport = Omit
    															includeBeamMeasurements = False
    															reportAddNeighMeas = Omit
    															measRSSI_ReportConfig_r16 = Omit
    															useT312_r16 = Omit
    															includeCommonLocationInfo_r16 = Omit
    															includeBT_Meas_r16 = Omit
    															includeWLAN_Meas_r16 = Omit
    															includeSensor_Meas_r16 = Omit
    															coarseLocationRequest_r17 = Omit
    															reportQuantityRelay_r17 = Omit
    									measIdToRemoveList = Omit
    									measIdToAddModList
    										MeasIdToAddMod
    											measId = 1
    											measObjectId = 1
    											reportConfigId = 1
    									s_MeasureConfig = Omit
    									quantityConfig
    										quantityConfigNR_List
    											QuantityConfigNR
    												quantityConfigCell
    													ssb_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    													csi_RS_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    												quantityConfigRS_Index
    													ssb_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    													csi_RS_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    											QuantityConfigNR
    												quantityConfigCell
    													ssb_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    													csi_RS_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    												quantityConfigRS_Index
    													ssb_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    													csi_RS_FilterConfig
    														filterCoefficientRSRP = fc4 (4)
    														filterCoefficientRSRQ = fc4 (4)
    														filterCoefficientRS_SINR = fc4 (4)
    										quantityConfigEUTRA = Omit
    										quantityConfigUTRA_FDD_r16 = Omit
    										quantityConfigCLI_r16 = Omit
    									measGapConfig = Omit
    									measGapSharingConfig = Omit
    									interFrequencyConfig_NoGap_r16 = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '041100000200'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList = Omit
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension
    										otherConfig_v1540 = Omit
    										nonCriticalExtension
    											mrdc_SecondaryCellGroupConfig = Omit
    											radioBearerConfig2 = Omit
    											sk_Counter = Omit
    											nonCriticalExtension
    												otherConfig_v1610 = Omit
    												bap_Config_r16 = Omit
    												iab_IP_AddressConfigurationList_r16 = Omit
    												conditionalReconfiguration_r16 = Omit
    												daps_SourceRelease_r16 = Omit
    												t316_r16 = Omit
    												needForGapsConfigNR_r16 = Omit
    												onDemandSIB_Request_r16 = Omit
    												dedicatedPosSysInfoDelivery_r16 = Omit
    												sl_ConfigDedicatedNR_r16 = Omit
    												sl_ConfigDedicatedEUTRA_Info_r16 = Omit
    												targetCellSMTC_SCG_r16 = Omit
    												nonCriticalExtension = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 416
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 229
    text = Parameter: NasEmu5G_Main_NRNG.v_RrcPduPresent = True
    File: NasEmu5G_Main_NRNG.ttcn [Line: 229]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 230
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 230]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 231
    text = Parameter: NasEmu5G_Main_NRNG.v_IntegrityError = False
    File: NasEmu5G_Main_NRNG.ttcn [Line: 231]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 416
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    recordType = 24
    summary = Step  3

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 927
    text = Parameter: NR_ConfigurationSteps.v_NR_TestEnvironment = OTA
    File: NR_ConfigurationSteps.ttcn [Line: 927]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 929
    text = Parameter: NR_ConfigurationSteps.v_CnfFlag = True
    File: NR_ConfigurationSteps.ttcn [Line: 929]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 0
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 940
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].CellId = nr_Cell2
    File: NR_ConfigurationSteps.ttcn [Line: 940]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 886
    text = Parameter: NR_ConfigurationSteps.v_CurrentRefPowerLevel = -82
    File: NR_ConfigurationSteps.ttcn [Line: 886]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 893
    text = Parameter: NR_ConfigurationSteps.v_AttenuationValue = 0
    File: NR_ConfigurationSteps.ttcn [Line: 893]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 898
    text = Parameter: NR_ConfigurationSteps.v_Attenuation.Value = 0
    File: NR_ConfigurationSteps.ttcn [Line: 898]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 53
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 53]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 948
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].TimingInfo = Omit
    File: NR_ConfigurationSteps.ttcn [Line: 948]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 1
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common4G5G\Common4G5G_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 373
    text = Parameter: Common4G5G_Templates.v_CnfFlag = True
    File: Common4G5G_Templates.ttcn [Line: 373]

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell2 (2)
    				Attenuation
    					Value = 0
    				TimingInfo = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    recordType = 24
    summary = Step  4

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 504
    text = Parameter: RRC_Measurement_NR5GC.v_PhysCellIdServing = 42
    File: RRC_Measurement_NR5GC.ttcn [Line: 504]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\NR5GC\8_1_3\RRC_Measurement_NR5GC.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 505
    text = Parameter: RRC_Measurement_NR5GC.v_PhysCellIdNeighbour = 50
    File: RRC_Measurement_NR5GC.ttcn [Line: 505]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_RRC_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 132
    text = Parameter: NR_RRC_Templates.v_ServCellIndex = 0
    File: NR_RRC_Templates.ttcn [Line: 132]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 329
    text = Parameter: NR_Measurement_Functions.v_Counter = 0
    File: NR_Measurement_Functions.ttcn [Line: 329]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 330
    text = Parameter: NR_Measurement_Functions.v_PreviousSfn = -1
    File: NR_Measurement_Functions.ttcn [Line: 330]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 332
    text = Parameter: NR_Measurement_Functions.v_MinTolerance = 0
    File: NR_Measurement_Functions.ttcn [Line: 332]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 333
    text = Parameter: NR_Measurement_Functions.v_MaxTolerance = 0
    File: NR_Measurement_Functions.ttcn [Line: 333]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 337
    text = Parameter: NR_Measurement_Functions.v_VerdictMessage = 'Received a measurement report for the measId 1'
    File: NR_Measurement_Functions.ttcn [Line: 337]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_RRC_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 132
    text = Parameter: NR_RRC_Templates.v_ServCellIndex = 0
    File: NR_RRC_Templates.ttcn [Line: 132]

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 0
    						measResultServingCell
    							physCellId = 42
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 101
    										rsrq = 66
    				measResultNeighCells = measResultListNR = SEQUENCE OF MeasResultNR
    					MeasResultNR(1)
    						physCellId = 50
    						measResult
    							cellResults
    								resultsSSB-Cell
    									rsrp = 107

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 544
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					measurementReport
    						criticalExtensions
    							measurementReport
    								measResults
    									measId = 1
    									measResultServingMOList
    										MeasResultServMO
    											servCellId = 0
    											measResultServingCell
    												physCellId = 42
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 101
    															rsrq = 66
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    											measResultBestNeighCell = Omit
    									measResultNeighCells
    										measResultListNR
    											MeasResultNR
    												physCellId = 50
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 107
    															rsrq = Omit
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 229
    text = Parameter: NasEmu5G_Main_NRNG.v_RrcPduPresent = True
    File: NasEmu5G_Main_NRNG.ttcn [Line: 229]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 230
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 230]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 231
    text = Parameter: NasEmu5G_Main_NRNG.v_IntegrityError = False
    File: NasEmu5G_Main_NRNG.ttcn [Line: 231]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 544
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						measurementReport
    							criticalExtensions
    								measurementReport
    									measResults
    										measId = 1
    										measResultServingMOList
    											MeasResultServMO
    												servCellId = 0
    												measResultServingCell
    													physCellId = 42
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 101
    																rsrq = 66
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    												measResultBestNeighCell = Omit
    										measResultNeighCells
    											measResultListNR
    												MeasResultNR
    													physCellId = 50
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 107
    																rsrq = Omit
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    recordType = 24
    summary = Received a measurement report for the measId 1

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Received a measurement report for the measId 1

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 380
    text = Parameter: NR_Measurement_Functions.v_Counter = 1
    File: NR_Measurement_Functions.ttcn [Line: 380]

    recordType = 24
    summary = Steps 5-5A

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 927
    text = Parameter: NR_ConfigurationSteps.v_NR_TestEnvironment = OTA
    File: NR_ConfigurationSteps.ttcn [Line: 927]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 929
    text = Parameter: NR_ConfigurationSteps.v_CnfFlag = True
    File: NR_ConfigurationSteps.ttcn [Line: 929]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 0
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 940
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].CellId = nr_Cell1
    File: NR_ConfigurationSteps.ttcn [Line: 940]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 886
    text = Parameter: NR_ConfigurationSteps.v_CurrentRefPowerLevel = -82
    File: NR_ConfigurationSteps.ttcn [Line: 886]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 893
    text = Parameter: NR_ConfigurationSteps.v_AttenuationValue = 9
    File: NR_ConfigurationSteps.ttcn [Line: 893]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 898
    text = Parameter: NR_ConfigurationSteps.v_Attenuation.Value = 9
    File: NR_ConfigurationSteps.ttcn [Line: 898]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2801
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 53
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 53]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 948
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].TimingInfo = Omit
    File: NR_ConfigurationSteps.ttcn [Line: 948]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 1
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 940
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].CellId = nr_Cell2
    File: NR_ConfigurationSteps.ttcn [Line: 940]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 886
    text = Parameter: NR_ConfigurationSteps.v_CurrentRefPowerLevel = -82
    File: NR_ConfigurationSteps.ttcn [Line: 886]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 893
    text = Parameter: NR_ConfigurationSteps.v_AttenuationValue = 18
    File: NR_ConfigurationSteps.ttcn [Line: 893]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 898
    text = Parameter: NR_ConfigurationSteps.v_Attenuation.Value = 18
    File: NR_ConfigurationSteps.ttcn [Line: 898]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2783
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2783]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2798
    text = Parameter: NR_CellInfo.v_Index = 0
    File: NR_CellInfo.ttcn [Line: 2798]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 2802
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 2802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_CellInfo.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 53
    text = Parameter: NR_CellInfo.v_Index = 1
    File: NR_CellInfo.ttcn [Line: 53]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 948
    text = Parameter: NR_ConfigurationSteps.v_CellAttenuationList[i].TimingInfo = Omit
    File: NR_ConfigurationSteps.ttcn [Line: 948]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_ConfigurationSteps.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 938
    text = Parameter: NR_ConfigurationSteps.i = 2
    File: NR_ConfigurationSteps.ttcn [Line: 938]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common4G5G\Common4G5G_Templates.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 373
    text = Parameter: Common4G5G_Templates.v_CnfFlag = True
    File: Common4G5G_Templates.ttcn [Line: 373]

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 0
    						measResultServingCell
    							physCellId = 42
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 101
    										rsrq = 66
    				measResultNeighCells = measResultListNR = SEQUENCE OF MeasResultNR
    					MeasResultNR(1)
    						physCellId = 50
    						measResult
    							cellResults
    								resultsSSB-Cell
    									rsrp = 109

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 592
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					measurementReport
    						criticalExtensions
    							measurementReport
    								measResults
    									measId = 1
    									measResultServingMOList
    										MeasResultServMO
    											servCellId = 0
    											measResultServingCell
    												physCellId = 42
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 101
    															rsrq = 66
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    											measResultBestNeighCell = Omit
    									measResultNeighCells
    										measResultListNR
    											MeasResultNR
    												physCellId = 50
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 109
    															rsrq = Omit
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 229
    text = Parameter: NasEmu5G_Main_NRNG.v_RrcPduPresent = True
    File: NasEmu5G_Main_NRNG.ttcn [Line: 229]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 230
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 230]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 231
    text = Parameter: NasEmu5G_Main_NRNG.v_IntegrityError = False
    File: NasEmu5G_Main_NRNG.ttcn [Line: 231]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 9
    				TimingInfo = Omit
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell2 (2)
    				Attenuation
    					Value = 18
    				TimingInfo = Omit

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common\CommonDefs.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 616
    outStr = Timer: t_Delay, Duration: 10s, Started: 13:20:21

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 592
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						measurementReport
    							criticalExtensions
    								measurementReport
    									measResults
    										measId = 1
    										measResultServingMOList
    											MeasResultServMO
    												servCellId = 0
    												measResultServingCell
    													physCellId = 42
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 101
    																rsrq = 66
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    												measResultBestNeighCell = Omit
    										measResultNeighCells
    											measResultListNR
    												MeasResultNR
    													physCellId = 50
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 109
    																rsrq = Omit
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 0
    						measResultServingCell
    							physCellId = 42
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 101
    										rsrq = 66
    				measResultNeighCells = measResultListNR = SEQUENCE OF MeasResultNR
    					MeasResultNR(1)
    						physCellId = 50
    						measResult
    							cellResults
    								resultsSSB-Cell
    									rsrp = 100

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 640
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					measurementReport
    						criticalExtensions
    							measurementReport
    								measResults
    									measId = 1
    									measResultServingMOList
    										MeasResultServMO
    											servCellId = 0
    											measResultServingCell
    												physCellId = 42
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 101
    															rsrq = 66
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    											measResultBestNeighCell = Omit
    									measResultNeighCells
    										measResultListNR
    											MeasResultNR
    												physCellId = 50
    												measResult
    													cellResults
    														resultsSSB_Cell
    															rsrp = 100
    															rsrq = Omit
    															sinr = Omit
    														resultsCSI_RS_Cell = Omit
    													rsIndexResults = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 229
    text = Parameter: NasEmu5G_Main_NRNG.v_RrcPduPresent = True
    File: NasEmu5G_Main_NRNG.ttcn [Line: 229]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 230
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 230]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 231
    text = Parameter: NasEmu5G_Main_NRNG.v_IntegrityError = False
    File: NasEmu5G_Main_NRNG.ttcn [Line: 231]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 640
    				Subframe
    					Number = 2
    				HSFN
    					Number = 3
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						measurementReport
    							criticalExtensions
    								measurementReport
    									measResults
    										measId = 1
    										measResultServingMOList
    											MeasResultServMO
    												servCellId = 0
    												measResultServingCell
    													physCellId = 42
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 101
    																rsrq = 66
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    												measResultBestNeighCell = Omit
    										measResultNeighCells
    											measResultListNR
    												MeasResultNR
    													physCellId = 50
    													measResult
    														cellResults
    															resultsSSB_Cell
    																rsrp = 100
    																rsrq = Omit
    																sinr = Omit
    															resultsCSI_RS_Cell = Omit
    														rsIndexResults = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NasEmulation\NasEmu5G_Main_NRNG.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 118
    text = Parameter: NasEmu5G_Main_NRNG.v_NoOfNasPdus = 0
    File: NasEmu5G_Main_NRNG.ttcn [Line: 118]

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\Common\CommonDefs.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 617
    outStr = Timer: t_Delay, Expired: 13:20:31

    recordType = 24
    summary = Step 6

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 254
    outStr = Timer: t_Wait, Duration: 10s, Started: 13:20:31

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Measurement_Functions.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 257
    outStr = Timer: t_Wait, Expired: 13:20:41

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 316
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    IP_ConfigReq_Type
    	ChangeCell
    		Nr = nr_Cell1 (1)

    IP_Indication_Type
    	Cnf = True

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    UT_COMMON_CMD
    	Cmd = SWITCH_OFF (136)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_OFF'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E021840ACB605976266168D7A59F4B1CF522184771E9D40

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 41
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E021840ACB605976266168D7A59F4B1CF522184771E9D40'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    DEREGISTRATION REQUEST ORIGINATED
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	dereg_req_mt [8 bits] = 0x45 [ 69 ]
    	de_reg_tp
    		switch_off [1 bit] = 0x0 [ 0 ]
    		re_reg_req [1 bit] = 0x0 [ 0 ]
    		Access_typ [2 bits] = 0x0 [ 0 ]
    	ngksi
    		Type of security context flag [1 bit] = 0x1 [ 1 ]
    		nas_key_set_identi [3 bits] = 0x1 [ 1 ]
    	fivegs_mob_id
    		iel [16 bits] = 0xB [ 11 ]
    		Identity digit [4 bits] = 0xF [ 15 ]
    		Spare bit [1 bit] = 0x0 [ 0 ]
    		fivegs_typ_id [3 bits] = 0x2 [ 2 ]
    		MCC digit 2 [4 bits] = 0x0 [ 0 ]
    		MCC digit 1 [4 bits] = 0x0 [ 0 ]
    		MNC digit 3 [4 bits] = 0xF [ 15 ]
    		MCC digit 3 [4 bits] = 0x1 [ 1 ]
    		MNC digit 2 [4 bits] = 0x1 [ 1 ]
    		MNC digit 1 [4 bits] = 0x0 [ 0 ]
    		AMF Region ID = 0xFE [ 254 ]
    		AMF Set ID = 0x00 [ 0 ]
    		AMF Set ID (continued) [2 bits] = 0x1 [ 1 ]
    		AMF Pointer [6 bits] = 0x1 [ 1 ]
    		5G-TMSI = 0xC2345678 [ 3258209912 ]

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 41
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000005'O
    				Pdu
    					Msg
    						deregistration_RequestMO
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000101'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							deregistrationType
    								switchOff = 1'B
    								reRegistration = 0'B
    								accessType = 01'B
    							ngMobileId
    								iei = Omit
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    					PiggybackedPduList = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 81
    				Subframe
    					Number = 0
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					SymbolOffset = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 305
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 13:20:47

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 111
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 111
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000111'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 111
    			Subframe
    				Number = 2
    			HSFN
    				Number = 6
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 111
    			Subframe
    				Number = 2
    			HSFN
    				Number = 6
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 111
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit
    				SidelinkScheduled = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 111
    			Subframe
    				Number = 7
    			HSFN
    				Number = 6
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 111
    				Subframe
    					Number = 7
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 116
    			Subframe
    				Number = 7
    			HSFN
    				Number = 6
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 116
    				Subframe
    					Number = 7
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					Release = True

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 117
    			Subframe
    				Number = 2
    			HSFN
    				Number = 6
    			Slot
    				SlotOffset
    					Numerology3 = 0
    			Symbol
    				FirstSymbol = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology3
    			Symbol
    				FirstSymbol

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 117
    				Subframe
    					Number = 2
    				HSFN
    					Number = 6
    				Slot
    					SlotOffset
    						Numerology3 = 0
    				Symbol
    					FirstSymbol = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    										DuplicateDiscarding = Omit
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_8_1_3_1_2_NR5GC
    lineNo = 313
    outStr = Timer: t_Timer, Expired: 13:20:48

    IP_ConfigReq_Type
    	StopPDN
    		All = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    			Port = 53
    		Remote = Omit

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.11'
    					ScopeId
    			Port = 67
    		Remote = Omit

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.11'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.11'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				Close = True

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				Close = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				Close = True

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 1
    			DataMode = Omit

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				Close = True

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				Close = True

    DRBMUX_CONFIG_REQ
    	RoutingInfo

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    IP_Indication_Type
    	Cnf = True

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		MacBearerRouting = Omit
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			Release = True

    recordType = 24
    summary = Postamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    verdict = PASS
    summary = Test case ended: TC_8_1_3_1_2_NR5GC, Verdict: PASS

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Unmapping port "MTC_NR5GC:Ut" from port "SYSTEM_NR5GC:Ut"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "MTC_NR5GC:PTC_Ut" from port "IMS1:MMI"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "MTC_NR5GC:PTC_Ut" from port "NR5GC:UT"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "NR5GC:NASCTRL" from port "NASEMU_NRNG:CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "NR5GC:SRB" from port "NASEMU_NRNG:TC_SRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "NR5GC:IP" from port "IP:NR_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "NR5GC:IMS" from port "IMS1:IPCAN"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IMS_CTRL" from port "IMS1:IMS_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IMS_Client" from port "IMS1:IMS_Client"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IP_SOCK_CTRL_QUEUE" from port "IPMUX:IP_SOCK_CTRL_QUEUE"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IP_SOCK_DATA" from port "IPMUX:IP_SOCK_DATA"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IP_SOCK_CTRL" from port "IPMUX:IP_SOCK_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v77.0\NR5GC_Testsuite\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 159
    text = Disconnecting port "IP:IMS_Server" from port "IMS1:IMS_Server"

    recordType = 24
    fileName
    descriptionId = TC_8_1_3_1_2_NR5GC
    lineNo = 0
    text = Test Procedure: Final Verdict

    recordType = 24
    summary = Final Verdict

    verdict = PASS
    summary = TEST CASE ENDED: TC_8_1_3_1_2_NR5GC