3GPP TS 37.571-4 V17.5.0 (2024-03)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

User Equipment (UE) conformance specification for

UE positioning;

Part 4: Test suites

(Release 17)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

PIXIT, positioning, TTCN, UE

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 5

Introduction 5

1 Scope 6

2 References 6

3 Definitions, symbols and abbreviations 8

3.1 Definitions 8

3.2 Symbols 8

3.3 Abbreviations 8

4 A-GPS system architecture and test model 8

4.1 ATS and module structure 8

4.2 Upper tester 8

4.3 SV PCO 8

4.4 A-GPS Primitives 8

4.5 Specific test suite operation for A-GPS testing 8

5 A-GNSS and LTE positioning system architecture and test models 9

5.1 Test system architecture 9

5.1.1 General system architecture 9

5.1.2 Component architecture 9

5.1.2.1 Interfaces 10

5.2 Test model 10

5.2.1 LTE GNSS test model 11

5.2.2 UTRA A-GNSS test model 12

5.3 ASP specifications 13

5.4 LTE OTDOA test model 13

5.5 LTE ECID test model 14

6 LTE indoor positioning system architecture and test models 14

6.1 Test system architecture 14

6.1.1 General system architecture 14

6.1.2 Component architecture 14

6.1.2.1 Interfaces 15

6.2 Test model 15

6.2.1 LTE indoor positioning test model 15

6A LTE test models requiring GNSS support 16

6B NG-RAN NR positioning system architecture and test models 16

6B.1 Test system architecture 16

6B.1.1 General system architecture 16

6B.1.2 Component architecture 16

6B.2 Test models 17

6B.2.1 NR GNSS positioning test model 17

6B.2.2 NR indoor positioning test model 18

6B.2.3 NR OTDOA (LTE) positioning test model 18

6B.2.4 NR Multi-RTT, DL-AoD and DL-TDOA positioning test model 20

6B.2.5 NR E-CID test model 20

6C NR/5GC test models requiring GNSS support 21

7 Upper Tester Interface 21

7.1 MMI for A-GPS 21

7.2 MMI for A-GNSS, LTE and NR positioning 21

8 IXIT Proforma 22

8.1 A-GPS test suite parameters declarations 22

8.2 A-GNSS, LTE and NR positioning test suite parameters declarations 22

9 Other SS Requirements with TTCN-3 impact 22

9.1 Codec Requirements 22

Annex A (normative): Test Suites 23

A.1 UTRA A-GPS test suite 23

A.1.1 Baseline of specifications 23

A.1.2 AGPS ATS 23

A.1.3 The TTCN Machine Processable form (TTCN.MP) 24

A.2 UTRA A-GNSS, LTE and NR/5GC positioning test suite 24

A.2.1 Baseline of specifications 24

A.2.2 E-UTRA LTE positioning Test Cases 24

A.2.3 UTRA A-GNSS Test Cases 25

A.2.4 NR/5GC Test Cases 25

Annex B (informative): ASN.1 modules 27

B.1 A-GPS ASN.1 module 27

B.2 A-GNSS ASN.1 modules 27

B.3 LPP ASN.1 27

Annex C (informative) TTCN-3 Definitions 28

C.1 EUTRA\_POS\_ASP\_TypeDefs 28

C.1.1 System\_Configuration\_PosExt 28

C.1.2 Cell\_Configuration\_PosExt 28

C.1.2.1 Cell\_Configuration\_Common\_PosExt 28

C.1.2.2 Downlink\_Physical\_Layer\_Configuration\_PosExt 29

C.1.3 System\_Interface\_PosExt 29

C.2 References to TTCN-3 30

Annex D (informative) Positioning System Simulator ASP Definitions in TTCN-3 31

D.1 PosSystem\_ASP\_TypeDefs 31

D.1.1 PosSystem\_Load\_Scenario 31

D.1.2 PosSystem\_Retrieve\_Data 32

D.1.2.1 SatSystem\_Retrieve\_UTRAN\_Data 32

D.1.2.2 PosSystem\_Retrieve\_LPP\_Data 33

D.1.2.3 PosSystem\_Retrieve\_Data\_Common 34

D.1.3 PosSystem\_PowerControl 34

D.1.4 PosSystem\_GnssUtcTime 35

D.1.5 System\_Interface 35

D.2 CommonDefs 36

D.3 References to TTCN-3 37

Annex E (informative) TTCN-3 Definitions 37

E.1 NR5GC\_POS\_ASP\_TypeDefs 37

E.1.1 NR\_System\_Configuration\_PosExt 37

E.1.2 NR\_Cell\_Configuration\_PosExt 38

E.1.2.1 NR\_Cell\_Configuration\_Common\_PosExt 38

E.1.2.2 Downlink\_Physical\_Layer\_Configuration\_PosExt 38

E.1.3 NR\_System\_Interface\_PosExt 40

E.2 References to TTCN-3 40

Annex F (informative): Change history 41

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present document is part 4 of a multi-part conformance test specification. The specification contains a TTCN design frame work and the detailed test specifications in TTCN for the UE:

- A-GPS at the UTRA Uu interface in TTCN-2;

- A-GNSS at the UTRA Uu interface in TTCN-3;

- LTE positioning at the LTE-Uu interface in TTCN-3.

- NR positioning at the NR-Uu interface in TTCN-3.

The present document is part 4 of a multi-parts TS:

**-** 3GPP TS 37.571-1: User Equipment (UE) conformance specification for UE positioning; Part 1: Terminal conformance.

- 3GPP TS 37.571-2: User Equipment (UE) conformance specification for UE positioning; Part 2: Protocol conformance.

- 3GPP TS 37.571-3: User Equipment (UE) conformance specification for UE positioning; Part 3: Implementation Conformance Statement (ICS).

- **3GPP TS 37.571-4: User Equipment (UE) conformance specification for UE positioning; Part 4: Test suites.**

- 3GPP TS 37.571-5: User Equipment (UE) conformance specification for UE positioning; Part 5: Test scenarios and assistance data.

# 1 Scope

The present document specifies the protocol and signalling conformance testing in TTCN for the UE:

- A-GPS at the UTRA Uu interface;

- LTE positioning at the LTE-Uu interface;

- A-GNSS at the UTRA Uu interface.

- NR positioning at the NR-Uu interface.

The following TTCN test specification and design considerations can be found in the present document:

- Test system architecture;

- Test models and ASP definitions;

- Test methods and usage of communication ports definitions;

- Test configurations;

- Design principles and assumptions;

- TTCN styles and conventions;

- Partial PIXIT proforma;

- Test suites in TTCN-2 and TTCN-3;

- The Test Suites designed and implemented in the present document are based on the test specifications in prose in 3GPP TS 37.571‑2 [3];

- The applicability of the individual test cases is specified in the test ICS proforma specification in 3GPP TS 37.571‑3 [4].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document in the same Release as the present document unless the context in which the reference is made suggests a different Release is relevant (information on the applicable release in a particular context can be found in e.g. test case title, description or applicability, message description or content).

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 37.571-1: " User Equipment (UE) conformance specification for UE positioning; Part 1: Conformance test specification".

[3] 3GPP TS 37.571-2: " User Equipment (UE) conformance specification for UE positioning; Part 2: Protocol conformance".

[4] 3GPP TS 37.571-3: " User Equipment (UE) conformance specification for UE positioning; Part 3: Implementation Conformance Statement (ICS)".

[5] 3GPP TS 37.571-5: " User Equipment (UE) conformance specification for UE positioning; Part 5: Test scenarios and assistance data".

[6] 3GPP TS 36.523-3: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Packet Core (EPC); User Equipment (UE) conformance specification; Part 3: Test suites".

[7] 3GPP TS 36.508: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Packet Core (EPC); Common test environments for User Equipment (UE) conformance testing".

[8] 3GPP TS 34.123-3: "User Equipment (UE) conformance specification; Part 3: Abstract test suite (ATS)".

[9] 3GPP TS 34.108: "Common test environments for User Equipment (UE); Conformance testing".

[10] 3GPP TS 37.355: " LTE Positioning Protocol (LPP)".

[11] 3GPP TS 24.301: "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3".

[12] 3GPP TS 25.331: "Radio Resource Control (RRC); Protocol specification".

[13] 3GPP TS 24.080: "Mobile radio interface layer 3 supplementary services specification; Formats and coding".

[14] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[15] ITU-T Recommendation X.880: "Information technology - Remote Operations: Concepts, model and notation".

[16] ITU-T Recommendation Q.773: "Transaction capabilities formats and encoding".

[17] ETSI ES 201 873-1: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN-3 Core Language".

[18] 3GPP TS 34.109: "Terminal logical test interface; Special conformance testing functions".

[19] 3GPP TS 23.038: "Alphabets and language-specific information".

[20] ETSI TR 101 666 (V1.0.0): "Information technology; Open Systems Interconnection Conformance testing methodology and framework; The Tree and Tabular Combined Notation (TTCN) (Ed. 2++)".

[21] 3GPP TS 24.008: "Mobile radio interface Layer 3 specification; Core network protocols; Stage 3".

[22] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[23] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical channels and modulation".

[24] 3GPP TS 38.523-3: "5GS; User Equipment (UE) conformance specification; Part 3: Protocol Test Suites".

[25] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[26] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[27] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[28] 3GPP TS 38.508-1: "5GS; User Equipment (UE) conformance specification; Part 1: Common test environment".

[29] 3GPP TS 38.211: "NR; Physical channels and modulation".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905  [1] apply.

## 3.2 Symbols

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] apply.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply:

ASP Abstract Service Primitive

# 4 A-GPS system architecture and test model

A-GPS signalling conformance tests are specified in TTCN-2. The system architecture and the test model are based on 3GPP TS 34.123-3 [8].

## 4.1 ATS and module structure

Refer to 3GPP TS 34.123-3 [8], clause 5.

## 4.2 Upper tester

Refer to 3GPP TS 34.123-3 [8], clause 7.3.5.1.

## 4.3 SV PCO

Refer to 3GPP TS 34.123-3 [8], clause 7.3.5.2.

## 4.4 A-GPS Primitives

Refer to 3GPP TS 34.123-3[8], clause 7.3.5.3.

## 4.5 Specific test suite operation for A-GPS testing

Refer to 3GPP TS 34.123-3 [8], clause 8.7.7.

# 5 A-GNSS and LTE positioning system architecture and test models

## 5.1 Test system architecture

### 5.1.1 General system architecture

Refer to 3GPP TS 36.523-3 [6], clause 4.1.1.

### 5.1.2 Component architecture

Each access technology (RAT) is hosted by a separate TTCN-3 parallel component (PTC):

- E-UTRA PTC;

- UTRA PTC.

The PTCs are controlled by the TTCN-3 positioning master test component (POS MTC) which:

- Is an extension of the MTC as defined in 3GPP TS 36.523-3 [6], clause 4.1.2.

- Controls the SS Positioning Simulator.

Figure 5.1.2-1 shows this component architecture for an E-UTRA and UTRA scenario.



Figure 5.1.2-1: Component architecture for an E-UTRA and UTRA scenario

The PTCs are allocated according to the following principles:

- For LTE positioning tests cases, the E-UTRA PTC is created.

- For LTE positioning CS fallback test cases, E-UTRA and UTRA PTCs are created.

- For UTRA A-GNSS test cases, the UTRA PTC is created.

#### 5.1.2.1 Interfaces

A number of interfaces are taken into consideration.

**POS MTC - PTC**:

Common synchronisation of PTCs.

Positioning simulator command/data coordination messages.

Upper tester primitives.

**POS MTC - System Interface**:

Upper tester primitives.

**POS MTC- Positioning Simulator**:

Positioning simulator command and data primitives.

**PTC - PTC**:

Primitives containing information for IRAT handover.

**PTC - System Interface**:

Primitives containing peer-to-peer message.

Configuration primitives.

## 5.2 Test model

In order to perform the LTE positioning and A-GNSS tests, the Positioning Simulator shall have two basic functional unites:

- Satellite simulator generating and broadcasting satellite signals.

- Assistance data source storing the data associated with the pre-defined GPS and GNSS test scenarios (see 3GPP TS 37.571-5 [5]).

This specification supports the following GNSS: GPS, Galileo, GLONASS and BDS.

### 5.2.1 LTE GNSS test model



Figure 5.2.1-1: E-UTRA Test model for LTE positioning GNSS testing

The LTE positioning test model consists of an SS E-UTRAN protocol stack and a positioning simulator. The SS E-UTRA emulation part is the same as the model defined in 3GPP TS 36.523-3 [6].

The UE is configured in normal mode. On UE side Ciphering/Integrity (PDCP and NAS) is enabled. The tests are performed on C-Plane.

The ASPs at POS Port are used to:

- Load a pre-defined test scenario into the positioning simulator.

- Start or stop generating and broadcasting satellite signals from the positioning simulator.

- Retrieve the GNSS assistance data from assistance data source.

Under the ASP commands, the upper tester loads or re-loads pre-defined GNSS test scenario to the positioning simulator. The generated satellite signals shall simulate the GNSS environment as specified in 3GPP TS 37.571-2 [3], clause 5.

The SS also sends the GNSS assistance data to the UE through LPP signalling (see 3GPP TS 37.355 [10]) to facilitate the UE acquiring and tracking satellites. Such assistance data shall be consistent to within ±2 seconds with the satellite signals generated (see 3GPP TS 37.571-2 [3], clause 5.2.1).

The assistance data source shall provide the assistance data consistent to +1/-0 second with the GNSS test scenario currently running in the satellite simulator (i.e. the data shall be up to 1 second in advance of the scenario); this allows for a further 2 seconds of latency in the SS. In case multiple satellite systems are configured in a test, the assistance data are requested or retrieved in a single ASP command for all satellite systems.

The UE positioning services are encoded in a TCAP [16] ROSE component [15] of the facility information element [14] in the Supplement Service [13] conveyed in the NAS messages. The facility information element is encoded in BER in TTCN referred to 3GPP TS 24.080 [13], clause 3.6.1 and 3GPP TS 29.002 [14], clause 17.1.1.

### 5.2.2 UTRA A-GNSS test model



Figure 5.2.2-1: UTRA Test model for A-GNSS testing

The A-GNSS test model consists of an SS UTRAN protocol stack and a positioning simulator. The SS UTRA emulation part is the same as the model defined in 3GPP TS 36.523-3 [6], clause 4.4.1.

The UE is configured in normal mode. Ciphering and Integrity (RRC) are enabled. The tests are performed on C-Plane.

The ASPs at POS Port are used to:

- Load a pre-defined test scenario into the positioning simulator.

- Start or stop generating and broadcasting satellite signals from the positioning simulator.

- Retrieve the GPS and GNSS assistance data from assistance data source.

Under the ASP commands, the upper tester loads or re-loads pre-defined GPS or GNSS test scenario to the positioning simulator. The generated satellite signals shall simulate the A-GPS and A-GNSS environment as specified in 3GPP TS 37.571-2 [3], clause 4.2.

The SS also sends the GPS or GNSS assistance data to the UE through RRC signalling to facilitate the UE acquiring and tracking satellites. Such assistance data shall be consistent to within ±2 seconds with the satellite signals generated (see 3GPP TS 37.571-2 [3], clause 4.2).

The assistance data source shall provide the assistance data consistent to +1/-0 second with the GPS or GNSS test scenario currently running in the satellite simulator (i.e. the data shall be up to 1 second in advance of the scenario); this allows for a further 2 seconds of latency in the SS. In case multiple satellite systems are configured in a test, the assistance data are requested or retrieved in a single ASP command for all satellite systems.

The UE positioning services are encoded in a TCAP [16] ROSE component [15] of the facility information element [14] in the Supplement Service [13] conveyed in the NAS messages. The facility information element is encoded in BER in TTCN referred to 3GPP TS 24.080 [13], clause 3.6.1 and 3GPP TS 29.002 [14], clause 17.1.1.

## 5.3 ASP specifications

The E-UTRAN and UTRAN ASP definitions are specified according to 3GPP TS 36.523-3 [6], clause 6.

The positioning simulator ASP definitions are documented in annex C.

## 5.4 LTE OTDOA test model



Figure 5.4-1: E-UTRA OTDOA test model

The LTE OTDOA test model consists of an SS E-UTRAN protocol stack. The SS E‑UTRA emulation part is the same as the model defined in 3GPP TS 36.523-3 [6] with an additional port to configure the antenna port 6 and the Positioning Reference Signal (PRS) in the LTE cells. The extension of LTE ASPs is defined in annex C.

The simulated OTDOA environment is specified in 3GPP TS 37.571-2 [3], clause 5.2.2), cells are synchronous and configured with the timing offset set to 0. The PRS is transmitted according to 3GPP TS 36.211 [23], clause 6.10.4.

The UE is configured in normal mode. On UE side Ciphering/Integrity (PDCP and NAS) is enabled. The tests are performed on C-Plane.

The PRS signals are transmitted by the SS E-UTRAN, the assistance data are written in TTCN.

## 5.5 LTE ECID test model

The test model is referred to the LTE positioning test model defined in clause 5.2.1; except that no satellite signals are required.

# 6 LTE indoor positioning system architecture and test models

## 6.1 Test system architecture

### 6.1.1 General system architecture

Refer to 3GPP TS 36.523-3 [6], clause 4.1.1.

### 6.1.2 Component architecture

The same architecture as in 5.1.2 applies, excluding the UTRA PTC.



Figure 6.1.2-1: Component architecture for an E-UTRA scenario

#### 6.1.2.1 Interfaces

Refer to 5.1.2.1.

## 6.2 Test model

### 6.2.1 LTE indoor positioning test model



Figure 6.2.1-1: E-UTRA Test model for LTE indoor positioning testing

The LTE Indoor Positioning test model consists of an SS E-UTRAN protocol stack and an Indoor Positioning simulator. Depending on the Indoor Positioning Technology to be tested, the Indoor Positioning simulator will generate:

- MBS beacon signals, for MBS test cases;

- WLAN signals, for WLAN test cases;

- Bluetooth signals, for Bluetooth test cases.

- The Indoor Positioning simulator will be switched off for Sensor test cases.

The SS E-UTRA emulation part is the same as the model defined in 3GPP TS 36.523-3 [6].

The UE is configured in normal mode. On UE side Ciphering/Integrity (PDCP and NAS) is enabled. The tests are performed on C-Plane.

The ASPs at POS Port are used to:

- Load a pre-defined test scenario into the Indoor Positioning simulator.

- Start or stop generating and broadcasting signals from the Indoor Positioning simulator.

- Retrieve the appropriate (MBS, WLAN, Sensor) assistance data from the assistance data source.

Under the ASP commands, the upper tester loads or re-loads pre-defined test scenario to the Indoor Positioning simulator. The generated signals shall simulate the corresponding Indoor Positioning environment as specified in 3GPP TS 37.571-2 [3], clause 5.

The SS also sends the appropriate assistance data to the UE through LPP signalling (see 3GPP TS 37.355 [10]) to facilitate the UE acquisition of MBS Beacons or WLAN APs. For UE-based tests, the SS also sends the appropriate assistance data to enable the UE to calculate its position for MBS or WLAN tests, or calculate altitude based on barometric pressure sensor measurements.

The UE positioning services are encoded in a TCAP [16] ROSE component [15] of the facility information element [14] in the Supplement Service [13] conveyed in the NAS messages. The facility information element is encoded in BER in TTCN referred to 3GPP TS 24.080 [13], clause 3.6.1 and 3GPP TS 29.002 [14], clause 17.1.1.

# 6A LTE test models requiring GNSS support

Several LTE test models specified in TS 36.523-3 [6] require the presence of a GNSS emulation. Those are:

- V2X services: refer to TS 36.523-3 [6] clause 4.2.11

- Aerial UE: refer to TS 36.523-3 [6] clause 4.2.12

The positioning simulator shall be capable of generating and broadcasting the following GNSS: GPS, Galileo, GLONASS and BDS.

The ASPs at POS Port for the both test models are used to:

- Load a pre-defined test scenario into the positioning simulator.

- Start or stop generating and broadcasting satellite signals from the positioning simulator.

The ASPs at POS Port for V2X services are additionally used to:

- Trigger the positioning simulator to move in the test scenario to the next geographical area or zone.

- Trigger the positioning simulator to switch on/off the transmitter without stopping the UTC time sequence.

The ASPs at POS Port for aerial UE communication are additionally used to:

- Set an initial altitude above the sea level. Geographical latitude and longitude are defined in the test scenario and remain constant during the test execution.

- Trigger the positioning simulator to simulate a vertical movement in the test scenario towards a specified altitude level.

# 6B NG-RAN NR positioning system architecture and test models

## 6B.1 Test system architecture

### 6B.1.1 General system architecture

Refer to 3GPP TS 36.523-3 [6], clause 4.1.1.

### 6B.1.2 Component architecture

The NR PTC is controlled by the TTCN-3 positioning master test component (POS MTC) which:

- Is an extension of the MTC as defined in 3GPP TS 38.523-3 [24], clause 4.2.

- Controls the SS Positioning Simulator.



Figure 6B.1.2-1: Component architecture for a NR scenario

As specified in TS 37.571-2 [2], subclause 8.2.8:

- The connection between the Position Simulator and the UE (Satellite signal) shall be conducted.

- The connection between the System Simulator and the UE (Radio Interface) shall be conducted for NR FR1 and radiated (OTA) for NR FR2.

## 6B.2 Test models

### 6B.2.1 NR GNSS positioning test model

The NR positioning test model consists of an SS NR protocol stack and a positioning simulator. The SS NR/5GC emulation part is the same as the model defined in 3GPP TS 38.523-3 [24]. The positioning simulator is the same as for LTE positioning test model defined in clause 5.2.1.



Figure 6B.2.1-1: Test model for NR GNSS positioning testing

### 6B.2.2 NR indoor positioning test model

The NR indoor positioning test model is the same as the NR positioning test model in clause 6B.2.1 but replacing the Positioning simulator with an Indoor Positioning simulator. The same principles as in clause 6.2.1 apply but replacing LTE with NR.

### 6B.2.3 NR OTDOA (LTE) positioning test model

OTDOA measurements are not supported on NR cells in Rel-15. The OTDOA measurements are provided by LTE cells instead. The UE will be attached to an NR cell and the LPP session will be established over NR/5GC NAS. The UE will report OTDOA RSTD measurements from LTE neighbour cells.

The NR OTDOA (LTE) positioning model consists of an SS NR/5GC protocol stack and a SS E-UTRAN protocol stack. The SS NR/5GC emulation part is the same as the model defined in 3GPP TS 38.523-3 [34]. The SS E-UTRAN emulation part is the same as the model defined in clause 5.4 (i.e. including an additional port to configure the antenna port 6 and the Positioning Reference Signal (PRS) in the LTE cells). The E-UTRA PTC will not be connected to NASEMU or IMS/IP PTCs.



Figure 6B.2.3-1: Test model for NR OTDOA (LTE) positioning testing

### 6B.2.4 NR Multi-RTT, DL-AoD and DL-TDOA positioning test model




Figure 6B.2.4-1: NR Multi-RTT, DL-AoD and DL-TDOA test model

The NR Multi-RTT, DL-AoD and DL-TDOA test model is the same as the NR/5GC Layer 3 test model (TS 38.523-3 [24], clause 5.2.1.1) with an additional port to configure the DL Positioning Reference Signal (DL-PRS) in the NR cells. The extension of NR ASPs is defined in annex X [TBD].

The simulated NR Multi-RTT, DL-AoD and DL-TDOA environments are specified in TS 37.571-2 [3], clauses 8.2.9, 8.2.10 and 8.2.11, respectively. The DL-PRS is transmitted according to TS 38.211 [29], clause 7.4.1.7.

The UE is configured in normal mode. On UE side Ciphering/Integrity (PDCP and NAS) is enabled. The tests are performed on C-Plane.

The DL-PRS is transmitted by the physical layer of the NR cell(s) in the SS. The assistance data to provide the UE with the configuration of the DL-PRS is sent from the SS to the UE via LPP signalling.

For Multi-RTT, the SS will be also configured through the NR\_SYS port to receive UL-SRS from the UE.

### 6B.2.5 NR E-CID test model

The test model is the same as the NR/5GC Layer 3 test model (TS 38.523-3 [24], clause 5.2.1.1).

# 6C NR/5GC test models requiring GNSS support

The NR sidelink test model specified in TS 38.523-3 [24] clause 5.2.1.6 requires the presence of a GNSS emulation.

The positioning simulator shall be capable of generating and broadcasting the following GNSS: GPS, Galileo, GLONASS and BDS.

The ASPs at POS Port for NR sidelink are used to:

- Load a pre-defined test scenario into the positioning simulator.

- Start or stop generating and broadcasting satellite signals from the positioning simulator.

- Trigger the positioning simulator to move in the test scenario to the next geographical area or zone.

- Trigger the positioning simulator to switch on/off the transmitter without stopping the UTC time sequence.

- Retrieve the current UTC time of the GNSS scenario.

# 7 Upper Tester Interface

## 7.1 MMI for A-GPS

Refer to 3GPP TS 34.123-3 [8], clause B.1.12.

## 7.2 MMI for A-GNSS, LTE and NR positioning

Refer to 3GPP TS 36.523-3 [6], clause 5.

The following MMI commands are defined for A-GNSS, LTE and NR positioning.

Table 7.2-1: MMI commands

|  |  |  |
| --- | --- | --- |
| Command | Parameters | |
|  | Name | Value |
| "CHECK\_LCS\_CLIENT" | none | |
| “LOCATION\_INFO” | none | |

Table 7.2-2: MMI commands imported from 3GPP TS 36.523-3 [6], clause 5

|  |
| --- |
| Command |
| "SWITCH\_ON" |
| "SWITCH\_OFF" |
| "POWER\_ON" |
| "POWER\_OFF" |
| "CHECK\_DTCH\_THROUGHCONNECTED" |
| "CLEAR\_STORED\_ASSISTANCE\_DATA" |

The following AT commands are applied in TTCN.

Table 7.2-3: AT Commands

|  |  |
| --- | --- |
| Command | Reference |
| AT+CMOLR | TS 27.007 [32] |
| AT+CMTLR | TS 27.007 [32] |
| AT+CMTLRA | TS 27.007 [32] |

# 8 IXIT Proforma

## 8.1 A-GPS test suite parameters declarations

Refer to 3GPP TS 34.123-3 [8], clause B.1.13.

## 8.2 A-GNSS, LTE and NR positioning test suite parameters declarations

Same PIXIT parameters are referred to clause 8.1.

Table 8.2-1: Void

# 9 Other SS Requirements with TTCN-3 impact

## 9.1 Codec Requirements

Refer to 3GPP TS 36.523-3 [6] clause 8.1 and TS 38.523-3 [24] clause 8.1.

Annex A (normative):  
Test Suites

This annex contains the approved TTCN Test Suites.

# A.1 UTRA A-GPS test suite

This annex includes the reference to those approved A-GPS ATS which are contained in 3GPP TS 34.123-3 [8], clause A.11.

The ATSs have been produced using the Tree and Tabular Combined Notation (TTCN2) according to TR 101 666 [20].

## A.1.1 Baseline of specifications

Table A.1.1-1 shows the baseline of the relevant core specifications and the test specifications which the delivered ATSs are referred to.

Table A.1.1-1: Versions of the test and Core specifications

|  |  |
| --- | --- |
| Core specifications | 3GPP TS 25.331 [12] |
| Test specifications | 3GPP TS 37.571-2 [3] |
| 3GPP TS 37.571-3 [4] |
| 3GPP TS 37.571-5 [6] |
| 3GPP TS 34.123-3 [8] |
| 3GPP TS 34.108 [9] |
| 3GPP TS 34.109 [18] |

## A.1.2 AGPS ATS

The approved AGPS test cases are listed. An "X" in columns FDD or LCR TDD indicates the test case approved for the relevant ATS.

Table A.1.2-1: AGPS TTCN test cases

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test case reference | | Description | FDD | TDD |
| TS 37.571-2 [3] | TS 34.123-3 [8] |
| 6.1.1.1 | 17.2.2.1 | LCS Network Induced location request/UE-Based GPS/Emergency Call/with USIM | X |  |
| 6.1.1.2 | 17.2.2.2 | LCS Network Induced location request/UE-Based GPS/Emergency Call/without USIM | X |  |
| 6.1.1.3 | 17.2.2.3 | LCS Network induced location request/UE-Assisted GPS/Emergency call/With USIM | X |  |
| 6.1.1.4 | 17.2.2.4 | LCS Network induced location request/UE-Assisted GPS/Emergency call/Without USIM | X |  |
| 6.1.2.1 | 17.2.3.2 | LCS Mobile originated location request/UE-Based GPS/Position estimate request/Success | X |  |
| 6.1.2.7 | 17.2.3.9 | LCS Mobile originated location request/UE-Assisted GPS/Position Estimate/Success | X |  |
| 6.1.3.1 | 17.2.4.1 | LCS Mobile terminated location request/UE-Based GPS | X |  |
| 6.1.3.2 | 17.2.4.2 | LCS Mobile-terminated location request/UE-Based GPS/Request for additional assistance data/Success | X |  |
| 6.1.3.3 | 17.2.4.3 | LCS Mobile-terminated location request/UE-Based GPS/Failure - Not Enough Satellites | X |  |
| 6.1.3.4 | 17.2.4.4 | LCS Mobile terminated location request/UE-Assisted GPS/Success | X |  |
| 6.1.3.5 | 17.2.4.5 | LCS Mobile terminated location request/UE-Assisted GPS/Request for additional assistance data/Success | X |  |
| 6.1.3.7 | 17.2.4.7 | LCS Mobile terminated location request/UE-Based GPS/Privacy Verification/Location Not Allowed if No Response | X |  |

## A.1.3 The TTCN Machine Processable form (TTCN.MP)

The TTCN.MP representation corresponding to the corresponding FDD ATS is referred to 3GPP TS 34.123-3 [8], clause A.11.

# A.2 UTRA A-GNSS, LTE and NR/5GC positioning test suite

The test suites have been produced using the Testing and Test Control Notation version 3 (TTCN-3) according to ES 201 873-1 [17].

## A.2.1 Baseline of specifications

Table A.2.1-1 shows the baseline of the relevant core specifications and the test specifications which the delivered TTCN test suites are referred to.

Table A.2.1-1: References of the test and Core specifications

|  |  |
| --- | --- |
| **Core specifications** | 3GPP TS 37.355 [10] |
| **baseline** | 3GPP TS 24.301 [11] |
|  | 3GPP TS 25.331 [12] |
|  | 3GPP TS 24.501 [25] |
|  | 3GPP TS 36.331 [26] |
|  | 3GPP TS 38.331 [27] |
| **Test specifications** | 3GPP TS 37.571-2 [3] |
|  | 3GPP TS 37.571-3 [4] |
|  | 3GPP TS 37.571-5 [5] |
|  | 3GPP TS 36.508 [7] |
|  | 3GPP TS 38.508-1 [28] |

The Test Suite in TTCN3 is contained in multiple ASCII files which accompany the present document.

## A.2.2 E-UTRA LTE positioning Test Cases

Table A.2.2-1 lists all approved test cases.

Table A.2.2-1: E-UTRA LTE positioning TTCN test cases

|  |  |
| --- | --- |
| Test case | Description |
| 7.1.1 | UE Network Capability |
| 7.2.1.1 | Location Notification |
| 7.2.1.2 | Privacy Verification – Location Allowed if no Response |
| 7.2.1.3 | Privacy Verification – Location not Allowed if No Response |
| 7.2.2.2.5s | Basic Self Location: UE-assisted sub-test 5 |
| 7.2.2.2.6.FDDs | Basic Self Location: UE-assisted sub-test 6 (FDD) |
| 7.2.2.2.6.TDDs | Basic Self Location: UE-assisted sub-test 6 (TDD) |
| 7.3.1.1 | Position Capability Transfer |
| 7.3.2.1 | LPP Duplicated Message |
| 7.3.2.2 | LPP Acknowledgment |
| 7.3.2.3 | LPP Retransmission |
| 7.3.3.1 | LPP Requested Method not Supported – UE-Assisted sub-test 1 |
| 7.3.4.2.5s | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted sub-test 5 |
| 7.3.4.2.6s | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted sub-test 6 |
| 7.3.4.2.7s | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted sub-test 7 |
| 7.3.4.4.5s | E-SMLC Initiated Position Measurement without assistance data: UE-Assisted sub-test 5 |
| 7.3.4.4.7s | E-SMLC Initiated Position Measurement without assistance data: UE-Assisted sub-test 7 |
| 7.3.5.1.5s | E-SMLC initiated Abort sub-test 5 |

## A.2.3 UTRA A-GNSS Test Cases

Table A.2.3-1 lists all approved test cases.

Table A.2.3-1: UTRA A-GNSS TTCN test cases

|  |  |
| --- | --- |
| Test case | Description |
| 6.2.1.1.4s | NI-LR Emergency Call: UE-Based A-GNSS sub-test 4 |
| 6.2.2.1.4s | MO-LR Position Estimate: UE-Based A-GNSS sub-test 4 |
| 6.2.2.3.4s | MO-LR Position Estimate: UE-Based A-GNSS – Failure Not Enough Satellites sub-test 4 |
| 6.2.3.2.4s | MT-LR Position Estimate: UE-Based A-GNSS – Failure Not Enough Satellites sub-test 4 |
| 6.2.3.3 | Location Notification |
| 6.2.3.4 | Privacy Verification - Location Allowed if No Response |
| 6.2.3.5 | Privacy Verification - Location Not Allowed if No Response |

## A.2.4 NR/5GC Test Cases

Table A.2.4-1 lists all approved test cases.

Table A.2.4-1: NR/5GC TTCN test cases

|  |  |
| --- | --- |
| Test case | Description |
| 9.3.1.1.NR5GC | Position Capability Transfer |
| 9.3.1.2.5s.NR5GC | LPP Abort: Subtest 5 |
| 9.3.1.2.15s.NR5GC | LPP Abort: Subtest 15 |
| 9.3.1.2.19s.NR5GC | LPP Abort: Subtest 19 |
| 9.3.1.2.20s.NR5GC | LPP Abort: Subtest 20 |
| 9.3.1.2.21s.NR5GC | LPP Abort: Subtest 21 |
| 9.3.2.1.NR5GC | LPP Duplicated Message |
| 9.3.2.2.NR5GC | LPP Acknowledgement |
| 9.3.2.3.NR5GC | LPP Retransmission |
| 9.3.4.1.15s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Based: Subtest 15 |
| 9.3.4.2.15s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted: Subtest 15 |
| 9.3.4.2.19s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted: Subtest 19 |
| 9.3.4.2.20s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted: Subtest 20 |
| 9.3.4.2.21s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted: Subtest 21 |
| 9.3.4.2.22s.NR5GC | E-SMLC Initiated Assistance Data Delivery followed by Location Information Transfer: UE-Assisted: Subtest 22 |
| 9.3.4.3.15s.NR5GC | E-SMLC Initiated Position Measurement without Assistance Data: UE-Based: Subtest 15 |
| 9.3.4.4.15s.NR5GC | E-SMLC Initiated Position Measurement without Assistance Data: UE-Assisted: Subtest 15 |
| 9.3.4.4.19s.NR5GC | E-SMLC Initiated Position Measurement without Assistance Data: UE-Assisted: Subtest 19 |
| 9.3.4.4.20s.NR5GC | E-SMLC Initiated Position Measurement without Assistance Data: UE-Assisted: Subtest 20 |
| 9.3.4.4.21s.NR5GC | E-SMLC Initiated Position Measurement without Assistance Data: UE-Assisted: Subtest 21 |

Annex B (informative):  
ASN.1 modules

# B.1 A-GPS ASN.1 module

Refer to 3GPP TS 34.123-3 [8], annex H.1.

# B.2 A-GNSS ASN.1 modules

Refer to 3GPP TS 34.123-3 [8], annex H.2.

# B.3 LPP ASN.1

The LPP asn.1 modules are extracted from 3GPP TS 37.355 [10] without any change.

Annex C (informative)  
TTCN-3 Definitions

# C.1 EUTRA\_POS\_ASP\_TypeDefs

Type definitions for configuration of Positioning Reference Signal in the system simulator;  
Common design principles: refer to 3GPP TS 36.523-3 [6] annex D.

## C.1.1 System\_Configuration\_PosExt

Formal ASP Definitions for EUTRA PRS system configuration

SystemRequest\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **SystemRequest\_PosExt\_Type** | |
| **Comment** | NOTE: Same structure as SystemRequest\_Type in 3GPP TS 36.523-3 [6] annex D | |
| Cell | [CellConfigRequest\_PosExt\_Type](#CellConfigRequest_PosExt_Type) | configure PRS in an LTE cell;  the cell shall be configured as usual beforehand and SS shall raise an error when the cell does not exist yet;  there is no explicit release of the PRS but the whole cell needs to be released |

SystemConfirm\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **SystemConfirm\_PosExt\_Type** | |
| **Comment** | confirmations for system configuration;  in general to be sent after the configuration has been done | |
| Cell | Null\_Type | (no further parameters from SS) |

## C.1.2 Cell\_Configuration\_PosExt

Specific Info for PRS Cell Configuration Primitive

### C.1.2.1 Cell\_Configuration\_Common\_PosExt

CellConfigRequest\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **CellConfigRequest\_PosExt\_Type** | |
| **Comment** | NOTE: Same structure as SystemRequest\_Type in 3GPP TS 36.523-3 [6] annex D | |
| AddOrReconfigure | [CellConfigInfo\_PosExt\_Type](#CellConfigInfo_PosExt_Type) | for PRS configuration of given cell:  CellId : identifier of the cell to be configured  RoutingInfo : None  TimingInfo : Now (for initial configuration and for reconfiguration in general)  ControlInfo : CnfFlag:=true; FollowOnFlag:=false (in general) |

CellConfigInfo\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **CellConfigInfo\_PosExt\_Type** | | |
| **Comment** | NOTE: Same structure as SystemRequest\_Type in 3GPP TS 36.523-3 [6] annex D  common information for initial cell configuration or reconfiguration;  in case of reconfiguration OMIT means 'keep configuration as it is' | | |
| Basic | [BasicCellConfig\_PosExt\_Type](#BasicCellConfig_PosExt_Type) | opt | Extended PRS information for a cell |

BasicCellConfig\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **BasicCellConfig\_PosExt\_Type** | | |
| **Comment** | NOTE: Same structure as SystemRequest\_Type in 3GPP TS 36.523-3 [6] annex D  Physical layer: | | |
| PhysicalLayerConfigDL | [PhysicalLayerConfigDL\_PosExt\_Type](#PhysicalLayerConfigDL_PosExt_Type) | opt | Default settings regarding physical control PRS signal |

### C.1.2.2 Downlink\_Physical\_Layer\_Configuration\_PosExt

Downlink physical layer configuration:  
- DL antenna configuration for port 6.  
- PRS configuration.

AntennaPort6\_Config\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **AntennaPort6\_Config\_Type** | | |
| **Comment** | to configure antenna port 6 for positioning;  all fields are declared as optional to allow single reconfigurations; in this case omit means "keep as it is" | | |
| Port | AntennaPort\_Type | opt |  |
| PRS | PRS\_Info | opt |  |
| RelativeTxPower | ToRS\_EPRE\_Ratio\_Type | opt | power ratio for Dl-PRS resource elements relative to the RS |

PhysicalLayerConfigDL\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **PhysicalLayerConfigDL\_PosExt\_Type** | | |
| **Comment** | all fields are declared as optional to allow single reconfigurations; in this case omit means "keep as it is" | | |
| AntennaPort6 | [AntennaPort6\_Config\_Type](#AntennaPort6_Config_Type) | opt |  |

## C.1.3 System\_Interface\_PosExt

SYSTEM\_CTRL\_POSEXT\_REQ

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **SYSTEM\_CTRL\_POSEXT\_REQ** | | |
| **Comment** |  | | |
| Common | ReqAspCommonPart\_Type |  | For configuration of antenna port 6 TimingInfo is now |
| Request | [SystemRequest\_PosExt\_Type](#SystemRequest_PosExt_Type) |  | configure a PRS in a cell |

SYSTEM\_CTRL\_POSEXT\_CNF

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **SYSTEM\_CTRL\_POSEXT\_CNF** | | |
| **Comment** |  | | |
| Common | CnfAspCommonPart\_Type |  | TimingInfo is ignored by TTCN  => SS may set TimingInfo to "None" |
| Confirm | [SystemConfirm\_PosExt\_Type](#SystemConfirm_PosExt_Type) |  |  |

EUTRA\_SYSTEM\_POSEXT\_PORT

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Port Type** | | |
| **Name** | **EUTRA\_SYSTEM\_POSEXT\_PORT** | |
| **Comment** | EUTRA PTC: Ext Port for system configuration of antenna port 6 | |
| out | [SYSTEM\_CTRL\_POSEXT\_REQ](#SYSTEM_CTRL_POSEXT_REQ) |  |
| in | [SYSTEM\_CTRL\_POSEXT\_CNF](#SYSTEM_CTRL_POSEXT_CNF) |  |

# C.2 References to TTCN-3

|  |  |  |
| --- | --- | --- |
| **References to TTCN-3** | | |
| **EUTRA\_POS\_ASP\_TypeDefs** | EUTRA/EUTRA\_POS\_ASP\_TypeDefs.ttcn | Rev 36622 |

Annex D (informative)  
Positioning System Simulator ASP Definitions in TTCN-3

# D.1 PosSystem\_ASP\_TypeDefs

PosSystem\_ASP\_TypeDefs: Constant Definitions

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Basic Types** | | | |
| **tsc\_MaxPosSystems** | integer | 12 |  |

PositioningSystemType

|  |  |
| --- | --- |
| **TTCN-3 Enumerated Type** | |
| **Name** | **PositioningSystemType** |
| **Comment** |  |
| gps |  |
| modernizedGPS |  |
| glonass |  |
| galileo |  |
| qzss |  |
| otdoa |  |
| ecid |  |
| bds |  |
| mbs |  |
| wlan |  |
| bluetooth |  |
| sensor |  |

PositioningSystemList\_Type

|  |  |
| --- | --- |
| **TTCN-3 Record of Type** | |
| **Name** | **PositioningSystemList\_Type** |
| **Comment** |  |
| record length (1..[tsc\_MaxPosSystems](#tsc_MaxPosSystems)) of [PositioningSystemType](#PositioningSystemType) | |

Altitude\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **Altitude\_Type** | | |
| **Comment** |  | | |
| Height | integer |  | Height above a sea level in meters |

## D.1.1 PosSystem\_Load\_Scenario

Load scenarios follow 3GPP TS 37.571-5 [5]

PosSystem\_Load\_Scenario: Basic Type Definitions

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Basic Types** | | |
| **ScenarioNumber\_Type** | integer |  |

PositioningScenario\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **PositioningScenario\_Type** | |
| **Comment** |  | |
| LTE\_Positioning | [ScenarioNumber\_Type](#ScenarioNumber_Type) | Reference to 3GPP TS 37.571-5 [5] |
| AGNSS | [ScenarioNumber\_Type](#ScenarioNumber_Type) | Reference to 3GPP TS 37.571-5 [5] |
| V2X | [ScenarioNumber\_Type](#ScenarioNumber_Type) | V2X Reference to 3GPP TS 36.508 [7] clause 4.11 |
| NR\_Positioning | [ScenarioNumber\_Type](#ScenarioNumber_Type) | Reference to 3GPP TS 37.571-5 [5] |
| Aerial | [ScenarioNumber\_Type](#ScenarioNumber_Type) | Reference to 3GPP TS 36.508 [7] clause 4.12 |
| NR\_Sidelink | [ScenarioNumber\_Type](#ScenarioNumber_Type) | Reference to 3GPP TS 38.508-1 [30] clause 4.11 |

## D.1.2 PosSystem\_Retrieve\_Data

### D.1.2.1 SatSystem\_Retrieve\_UTRAN\_Data

UTRAN\_GPS\_AssistanceDataRequest\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **UTRAN\_GPS\_AssistanceDataRequest\_Type** | | |
| **Comment** |  | | |
| AssistanceDataReqGPS | bitstring |  | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GPS-AdditionalAssistanceDataRequest |

UTRAN\_GANSS\_AssistanceDataRequest\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **UTRAN\_GANSS\_AssistanceDataRequest\_Type** | | |
| **Comment** |  | | |
| AssistanceDataReqGANSS | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GANSS-AdditionalAssistanceDataRequest |
| AssistanceDataReqGANSSv860ext | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GANSS-AdditionalAssistanceDataRequest-v860ext |
| AssistanceDataReqGANSSvc50ext | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GANSS-AdditionalAssistanceDataRequest-vc50ext |

UTRAN\_AssistanceDataRequest\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **UTRAN\_AssistanceDataRequest\_Type** | |
| **Comment** |  | |
| GPS | [UTRAN\_GPS\_AssistanceDataRequest\_Type](#UTRAN_GPS_AssistanceDataRequest_Type) |  |
| GANSS | [UTRAN\_GANSS\_AssistanceDataRequest\_Type](#UTRAN_GANSS_AssistanceDataRequest_Type) |  |

UTRAN\_AssistanceDataRequestList\_Type

|  |  |
| --- | --- |
| **TTCN-3 Record of Type** | |
| **Name** | **UTRAN\_AssistanceDataRequestList\_Type** |
| **Comment** |  |
| record length(1..[tsc\_MaxPosSystems](#tsc_MaxPosSystems)) of [UTRAN\_AssistanceDataRequest\_Type](#UTRAN_AssistanceDataRequest_Type) | |

UTRAN\_GPS\_AssistanceData\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **UTRAN\_GPS\_AssistanceData\_Type** | | |
| **Comment** | The returned Almanac information is split into two fields:  Almanac for satellites 1 to 16 in AssistanceDataGPSr7 together with other information;  Almanac for satellites 17 to 31: in 'almanacSat17To31' | | |
| AssistanceDataGPSr7 | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GPS-AssistanceData-r7 |
| AssistanceDataGPSr12 | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GPS-AssistanceData-r12 |
| AlmanacSatInfoList17To31 | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type AlmanacSatInfoList |

UTRAN\_GANSS\_AssistanceData\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **UTRAN\_GANSS\_AssistanceData\_Type** | | |
| **Comment** |  | | |
| AssistanceDataGANSS\_r8 | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GANSS-AssistanceData-r8 |
| AssistanceDataGANSS\_r12 | bitstring | opt | bitstring containing 3GPP TS 25.331 [12] type UE-Positioning-GANSS-AssistanceData-r12 |

UTRAN\_AssistanceData\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **UTRAN\_AssistanceData\_Type** | |
| **Comment** |  | |
| GPS | [UTRAN\_GPS\_AssistanceData\_Type](#UTRAN_GPS_AssistanceData_Type) |  |
| GANSS | [UTRAN\_GANSS\_AssistanceData\_Type](#UTRAN_GANSS_AssistanceData_Type) |  |

UTRAN\_AssistanceDataList\_Type

|  |  |
| --- | --- |
| **TTCN-3 Record of Type** | |
| **Name** | **UTRAN\_AssistanceDataList\_Type** |
| **Comment** |  |
| record length(1..[tsc\_MaxPosSystems](#tsc_MaxPosSystems)) of [UTRAN\_AssistanceData\_Type](#UTRAN_AssistanceData_Type) | |

### D.1.2.2 PosSystem\_Retrieve\_LPP\_Data

When data is to be requested for more than one positioning system, they will be included into one single template. This template will include a list with one element for each positioning system.  
See template "cs\_RequestAssistData\_UEB\_GpsAndGlonass" as an example.

LPP\_AssistanceDataRequest\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **LPP\_AssistanceDataRequest\_Type** | |
| **Comment** |  | |
| LPP\_AssistanceData | bitstring | bitstring containing 3GPP TS 37.355 [10] type RequestAssistanceData-r9-IEs |

LPP\_AssistanceDataProvide\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **LPP\_AssistanceDataProvide\_Type** | |
| **Comment** |  | |
| LPP\_AssistanceData | bitstring | bitstring containing 3GPP TS 37.355 [10] type ProvideAssistanceData-r9-IEs |

LPP\_AssistanceDataRequestList\_Type

|  |  |
| --- | --- |
| **TTCN-3 Record of Type** | |
| **Name** | **LPP\_AssistanceDataRequestList\_Type** |
| **Comment** |  |
| record length(1..[tsc\_MaxPosSystems](#tsc_MaxPosSystems)) of [LPP\_AssistanceDataRequest\_Type](#LPP_AssistanceDataRequest_Type) | |

LPP\_AssistanceDataList\_Type

|  |  |
| --- | --- |
| **TTCN-3 Record of Type** | |
| **Name** | **LPP\_AssistanceDataList\_Type** |
| **Comment** |  |
| record length(1..[tsc\_MaxPosSystems](#tsc_MaxPosSystems)) of [LPP\_AssistanceDataProvide\_Type](#LPP_AssistanceDataProvide_Type) | |

### D.1.2.3 PosSystem\_Retrieve\_Data\_Common

AssistanceDataRetrieveRequest\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **AssistanceDataRetrieveRequest\_Type** | |
| **Comment** |  | |
| LPP | [LPP\_AssistanceDataRequestList\_Type](#LPP_AssistanceDataRequestList_Type) | LTE/NR positioning |
| UTRA\_GNSS | [UTRAN\_AssistanceDataRequestList\_Type](#UTRAN_AssistanceDataRequestList_Type) | Retrieve A-GNSS data list in the order of positioning system provided in PositioningSystemList |

AssistanceDataRetrieveResponse\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **AssistanceDataRetrieveResponse\_Type** | |
| **Comment** |  | |
| LPP | [LPP\_AssistanceDataList\_Type](#LPP_AssistanceDataList_Type) | LTE/NR positioning |
| UTRA\_AGNSS | [UTRAN\_AssistanceDataList\_Type](#UTRAN_AssistanceDataList_Type) | Retrieve A-GNSS data list in the order of positioning system provided in PositioningSystemList |

## D.1.3 PosSystem\_PowerControl

PowerControl\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **PowerControl\_Type** | |
| **Comment** | V2X. The GNSS simulator is switched on/off without stopping the UTC time sequence | |
| PowerOn | [Null\_Type](#Null_Type) | By default the power is on in the GNSS simulator |
| PowerOff | [Null\_Type](#Null_Type) |  |

## D.1.4 PosSystem\_GnssUtcTime

GnssUtcTime\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **GnssUtcTime\_Type** | | |
| **Comment** |  | | |
| Struct\_tm | [Struct\_tm\_Type](#Struct_tm_Type) |  | Local GNSS time |
| TimezoneInfo | integer |  | Difference (in seconds) between the UTC time (GMT) and the local time |

## D.1.5 System\_Interface

Common ASP definitions

PosSystemCrtlRequest\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **PosSystemCrtlRequest\_Type** | |
| **Comment** |  | |
| Start | [Null\_Type](#Null_Type) |  |
| Stop | [Null\_Type](#Null_Type) |  |
| LoadScenario | [PositioningScenario\_Type](#PositioningScenario_Type) |  |
| RetrieveData | [AssistanceDataRetrieveRequest\_Type](#AssistanceDataRetrieveRequest_Type) |  |
| TriggerMove | [Null\_Type](#Null_Type) | V2X. Start moving to the next area/zone in the scenario |
| TriggerPowerOnOff | [PowerControl\_Type](#PowerControl_Type) | V2X. Switch on/off the transmitter without stopping UTC time sequence |
| SetAltitude | [Altitude\_Type](#Altitude_Type) | Aerial Set the height above the sea level to the provided value |
| TriggerAerialMove | [Altitude\_Type](#Altitude_Type) | Aerial Start moving towards target height |
| RetrieveGnssUtcTime | [Null\_Type](#Null_Type) | Get current UTC time of the GNSS scenario. This can only be used once a GNSS scenario has been loaded and started |

PosSystemCrtlConfirm\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **PosSystemCrtlConfirm\_Type** | |
| **Comment** | In general, to be sent after the configuration has been done | |
| Start | [Null\_Type](#Null_Type) |  |
| Stop | [Null\_Type](#Null_Type) |  |
| LoadScenario | [Null\_Type](#Null_Type) |  |
| RetrieveData | [AssistanceDataRetrieveResponse\_Type](#AssistanceDataRetrieveResponse_Type) |  |
| TriggerMove | [Null\_Type](#Null_Type) | V2X |
| TriggerPowerOnOff | [Null\_Type](#Null_Type) | V2X |
| SetAltitude | [Null\_Type](#Null_Type) | Aerial |
| TriggerAerialMove | [Null\_Type](#Null_Type) | Aerial |
| RetrieveGnssUtcTime | [GnssUtcTime\_Type](#GnssUtcTime_Type) |  |

POS\_SYSTEM\_CTRL\_REQ

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **POS\_SYSTEM\_CTRL\_REQ** | | |
| **Comment** |  | | |
| PositioningSystemList | [PositioningSystemList\_Type](#PositioningSystemList_Type) |  | The list of positioning systems to be configured; there is only one system of one type in the list e.g. gps, galileo etc. |
| CnfFlag | boolean |  | true => SS shall send CNF |
| Request | [PosSystemCrtlRequest\_Type](#PosSystemCrtlRequest_Type) |  |  |

POS\_SYSTEM\_CTRL\_CNF

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **POS\_SYSTEM\_CTRL\_CNF** | | |
| **Comment** |  | | |
| PositioningSystemList | [PositioningSystemList\_Type](#PositioningSystemList_Type) |  |  |
| Confirm | [PosSystemCrtlConfirm\_Type](#PosSystemCrtlConfirm_Type) |  |  |

POS\_MTC\_SYSTEM\_PORT

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Port Type** | | |
| **Name** | **POS\_MTC\_SYSTEM\_PORT** | |
| **Comment** | Positioning: port at the MTC to be mapped to the system | |
| out | [POS\_SYSTEM\_CTRL\_REQ](#POS_SYSTEM_CTRL_REQ) |  |
| in | [POS\_SYSTEM\_CTRL\_CNF](#POS_SYSTEM_CTRL_CNF) |  |

POS\_MTC\_PTC\_PORT

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Port Type** | | |
| **Name** | **POS\_MTC\_PTC\_PORT** | |
| **Comment** | Positioning: port at the MTC to hand over information from the positioning system to the PTC(s) | |
| out | [POS\_SYSTEM\_CTRL\_CNF](#POS_SYSTEM_CTRL_CNF) |  |
| in | [POS\_SYSTEM\_CTRL\_REQ](#POS_SYSTEM_CTRL_REQ) |  |

POS\_PTC\_MTC\_PORT

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Port Type** | | |
| **Name** | **POS\_PTC\_MTC\_PORT** | |
| **Comment** | Positioning: port at the PTC(s) to send commands to the positioning system via the MTC | |
| out | [POS\_SYSTEM\_CTRL\_REQ](#POS_SYSTEM_CTRL_REQ) |  |
| in | [POS\_SYSTEM\_CTRL\_CNF](#POS_SYSTEM_CTRL_CNF) |  |

# D.2 CommonDefs

CommonDefs: Basic Type Definitions

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Basic Types** | | |
| **Null\_Type** | boolean (true) | dummy type for 'typeless' fields in unions |

Struct\_tm\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **Struct\_tm\_Type** | | |
| **Comment** | TTCN-3 equivalent for the "struct tm" as defined on C standard library (time.h or ctime.h for C or C++) | | |
| tm\_sec | integer |  | seconds after the minute 0..61 (tm\_sec is generally 0-59. Extra range to accommodate for leap seconds in certain systems) |
| tm\_min | integer |  | minutes after the hour 0..59 |
| tm\_hour | integer |  | hours since midnight 0..23 |
| tm\_mday | integer |  | day of the month 1..31 |
| tm\_mon | integer |  | months since January 0..11 |
| tm\_year | integer |  | years since 1900 |
| tm\_wday | integer |  | days since Sunday 0..6 |
| tm\_yday | integer |  | days since January 1 0..365 |
| tm\_isdst | integer |  | Daylight Saving Time flag |

# D.3 References to TTCN-3

|  |  |  |
| --- | --- | --- |
| **References to TTCN-3** | | |
| **PosSystem\_ASP\_TypeDefs** | POS/PosSystem\_ASP\_TypeDefs.ttcn | Rev 32599 |
| **CommonDefs** | Common/CommonDefs.ttcn | Rev 32608 |

Annex E (informative)  
TTCN-3 Definitions

# E.1 NR5GC\_POS\_ASP\_TypeDefs

Type definitions for configuration of DL Positioning Reference Signal in the system simulator;  
Common design principles: refer to 3GPP TS 38.523-3 [24] annex D.

## E.1.1 NR\_System\_Configuration\_PosExt

Formal ASP Definitions for NR5GC DL-PRS system configuration

NR\_SystemRequest\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **NR\_SystemRequest\_PosExt\_Type** | |
| **Comment** | NOTE: Same structure as NR\_SystemRequest\_Type in 3GPP TS 38.523-3 [24] annex D | |
| Cell | [NR\_CellConfigRequest\_PosExt\_Type](#NR_CellConfigRequest_PosExt_Type) | configure DL-PRS in an NR cell;  the cell shall be configured as usual beforehand and SS shall raise an error when the cell does not exist yet;  there is no explicit release of the PRS but the whole cell needs to be released |

NR\_SystemConfirm\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **NR\_SystemConfirm\_PosExt\_Type** | |
| **Comment** | confirmations for system configuration;  in general to be sent after the configuration has been done | |
| Cell | Null\_Type | (no further parameters from SS) |

## E.1.2 NR\_Cell\_Configuration\_PosExt

Specific Info for DL-PRS Cell Configuration Primitive

### E.1.2.1 NR\_Cell\_Configuration\_Common\_PosExt

NR\_CellConfigRequest\_PosExt\_Type

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Union Type** | | |
| **Name** | **NR\_CellConfigRequest\_PosExt\_Type** | |
| **Comment** | NOTE: Same structure as NR\_SystemRequest\_Type in 3GPP TS 38.523-3 [24] annex D | |
| AddOrReconfigure | [NR\_CellConfigInfo\_PosExt\_Type](#NR_CellConfigInfo_PosExt_Type) | for PRS configuration of given cell:  CellId : identifier of the cell to be configured  RoutingInfo : None  RlcBearerRouting : 'None'  MacBearerRouting : 'omit'  TimingInfo : Now (for initial configuration and for reconfiguration in general)  ControlInfo : CnfFlag:=true; FollowOnFlag:=false (in general) |

NR\_CellConfigInfo\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **NR\_CellConfigInfo\_PosExt\_Type** | | |
| **Comment** | NOTE: Same structure as NR\_SystemRequest\_Type in 3GPP TS 38.523-3 [24] annex D  common information for initial cell configuration or reconfiguration;  in case of reconfiguration OMIT means 'keep configuration as it is' | | |
| PhysicalLayer | [NR\_CellConfigPhysicalLayer\_PosExt\_Type](#NR_CellConfigPhysicalLayer_PosExt_Type) | opt | Extended DL-PRS information for a cell |

NR\_CellConfigPhysicalLayer\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **NR\_CellConfigPhysicalLayer\_PosExt\_Type** | | |
| **Comment** | NOTE: Same structure as NR\_SystemRequest\_Type in 3GPP TS 38.523-3 [24] annex D  Physical layer: | | |
| Downlink | [NR\_CellConfigPhysicalLayerDownlink\_PosExt\_Type](#NR_CellCon__PhysicalLayerDownlink_PosExt) | opt | Default settings regarding physical control DL-PRS signal |

### E.1.2.2 Downlink\_Physical\_Layer\_Configuration\_PosExt

Downlink physical layer configuration:  
- DL-PRS Frequency Layer configuration.  
- DL-PRS TRP configuration.

Downlink\_Physical\_Layer\_Configuration\_PosExt: Basic Type Definitions

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Basic Types** | | |
| **DlPrs\_CombSizeN\_Type** | NR\_DL\_PRS\_PositioningFrequencyLayer\_r16.dl\_PRS\_CombSizeN\_r16 |  |

DlPrs\_FreqLayerConfig\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **DlPrs\_FreqLayerConfig\_Type** | | |
| **Comment** |  | | |
| DlPrs\_ResourceBW | integer | opt |  |
| DlPrs\_CombSizeN | [DlPrs\_CombSizeN\_Type](#DlPrs_CombSizeN_Type) | opt |  |

DlPrs\_TRPConfig\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **DlPrs\_TRPConfig\_Type** | | |
| **Comment** |  | | |
| NrDlPrsSfn0Offset | NR\_DL\_PRS\_SFN0\_Offset\_r16 | opt |  |
| NrDlPrsExpectedRstd | integer | opt |  |
| NrDlPrsExpectedRstdUncertainty | integer | opt |  |
| NrDlPrsInfo | NR\_DL\_PRS\_Info\_r16 | opt |  |

DlPrs\_EPREs\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **DlPrs\_EPREs\_Type** | | |
| **Comment** | EPRE for DL-PRS relative to SSS | | |
| DlPrsToSSS | NR\_EPRE\_Ratio\_Type | opt | Positioning reference signal;  38.211 clause 7.4.1.7 |

DL\_PRSConfig\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **DL\_PRSConfig\_Type** | | |
| **Comment** | to configure DL-PRS for positioning;  all fields are declared as optional to allow single reconfigurations; in this case omit means "keep as it is" | | |
| DlPrs\_FreqLayerConfig | [DlPrs\_FreqLayerConfig\_Type](#DlPrs_FreqLayerConfig_Type) | opt |  |
| DlPrs\_TRPConfig | [DlPrs\_TRPConfig\_Type](#DlPrs_TRPConfig_Type) | opt |  |
| RelativeTxPower | [DlPrs\_EPREs\_Type](#DlPrs_EPREs_Type) | opt | transmit power for DL-PRS signal |

NR\_CellConfigPhysicalLayerDownlink\_PosExt\_Type

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **NR\_CellConfigPhysicalLayerDownlink\_PosExt\_Type** | | |
| **Comment** | all fields are declared as optional to allow single reconfigurations; in this case omit means "keep as it is" | | |
| DL\_PRSConfig | [DL\_PRSConfig\_Type](#DL_PRSConfig_Type) | opt |  |

## E.1.3 NR\_System\_Interface\_PosExt

NR\_SYSTEM\_CTRL\_POSEXT\_REQ

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **NR\_SYSTEM\_CTRL\_POSEXT\_REQ** | | |
| **Comment** |  | | |
| Common | NR\_ReqAspCommonPart\_Type |  | For configuration of DL-PRS TimingInfo is now |
| Request | [NR\_SystemRequest\_PosExt\_Type](#NR_SystemRequest_PosExt_Type) |  | configure a DL-PRS in a cell |

NR\_SYSTEM\_CTRL\_POSEXT\_CNF

|  |  |  |  |
| --- | --- | --- | --- |
| **TTCN-3 Record Type** | | | |
| **Name** | **NR\_SYSTEM\_CTRL\_POSEXT\_CNF** | | |
| **Comment** |  | | |
| Common | NR\_CnfAspCommonPart\_Type |  | TimingInfo is ignored by TTCN  => SS may set TimingInfo to "None" |
| Confirm | [NR\_SystemConfirm\_PosExt\_Type](#NR_SystemConfirm_PosExt_Type) |  |  |

NR\_SYSTEM\_POSEXT\_PORT

|  |  |  |
| --- | --- | --- |
| **TTCN-3 Port Type** | | |
| **Name** | **NR\_SYSTEM\_POSEXT\_PORT** | |
| **Comment** | NR PTC: Ext Port for system configuration of DL-PRS | |
| out | [NR\_SYSTEM\_CTRL\_POSEXT\_REQ](#NR_SYSTEM_CTRL_POSEXT_REQ) |  |
| in | [NR\_SYSTEM\_CTRL\_POSEXT\_CNF](#NR_SYSTEM_CTRL_POSEXT_CNF) |  |

# E.2 References to TTCN-3

|  |  |  |
| --- | --- | --- |
| **References to TTCN-3** | | |
| **NR5GC\_POS\_ASP\_TypeDefs** | NR5GC/NR5GC\_POS\_ASP\_TypeDefs.ttcn | Rev 36621 |

Annex F (informative):  
Change history

| **Change history** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 2011-06 | RAN5#51 | R5-112203 | - | - | Initial proposal for A-GNSS |  | 0.0.1 |
| 2011-09 | RAN5#52 | R5-113037 | - | - | Introduced positioning test model | 0.0.1 | 0.1.0 |
| 2011-11 | RAN5#53 | R5-115106 | - | - | Imported A-GPS test model from 3GPP TS 34.123-3 | 0.1.0 | 1.0.0 |
| 2011-12 | RAN#54 | RP-111627 | - | - | Presentation of V1.0.0 | 0.1.0 | 1.0.0 |
| 2012-05 | RAN5#55 | R5-121083 | - | - | Presentation of V1.1.0 | 1.0.0 | 1.1.0 |
| 2012-06 | RAN#56 | RP-120614 | - | - | Presentation of V2.0.0 | 1.0.0 | 2.0.0 |
| 2012-06 | RAN#56 | - | - | - | Editorial corrections and formattings. | 2.0.0 | 9.0.0 |
| 2012-06 | RAN#56 | - | - | - | Raised to v10.0.0 with no change. | 9.0.0 | 10.0.0 |
| 2012-09 | RAN#57 | R5-123690 | 0001 | - | 37571-4: Routine maintenance and updates | 10.0.0 | 10.1.0 |
| 2013-06 | RAN#60 | R5-131136 | 0003 | - | 37571-4: Routine maintenance and updates | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130125 | 0004 | - | Addition of EUTRA UE Positioning test case 7.1.1 | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130145 | 0005 | - | Addition of EUTRA UE Positioning test case 7.3.1.1 | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130147 | 0006 | - | Addition of EUTRA UE Positioning test case 7.3.2.1 | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130149 | 0007 | - | Addition of EUTRA UE Positioning test case 7.3.2.2 | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130151 | 0008 | - | Addition of EUTRA UE Positioning test case 7.3.2.3 | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130153 | 0009 | - | Addition of EUTRA UE Positioning test case 7.3.5.1\_6s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130155 | 0010 | - | Addition of EUTRA UE Positioning test case 7.3.5.1\_5s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130157 | 0011 | - | Addition of EUTRA UE Positioning test case 7.3.4.2\_5s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130159 | 0012 | - | Addition of EUTRA UE Positioning test case 7.3.4.2\_6s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130288 | 0013 | - | Addition of EUTRA UE Positioning test case 7.3.4.4\_5s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | R5s130290 | 0014 | - | Addition of EUTRA UE Positioning test case 7.3.5.1\_1s | 10.1.0 | 10.2.0 |
| 2013-06 | RAN#60 | RP-130616 | 0015 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.1.0 | 10.2.0 |
| 2013-09 | RAN#61 | R5s130421 | 0016 | - | Correction to EUTRA UE Positioning test cases 7.3.4.2.5s and 7.3.4.4.5s | 10.2.0 | 10.3.0 |
| 2013-09 | RAN#61 | R5s130457 | 0017 | - | Correction to EUTRA UE Positioning test case 7.3.5.1.1s | 10.2.0 | 10.3.0 |
| 2013-09 | RAN#61 | R5s130468 | 0018 | - | Correction to EUTRA UE Positioning test cases 7.3.1.1 | 10.2.0 | 10.3.0 |
| 2013-09 | RAN#61 | RP-131167 | 0019 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.2.0 | 10.3.0 |
| 2013-12 | RAN#62 | R5s130618 | 0020 | - | Addition of EUTRA UE Positioning test case 7.3.4.1\_1s | 10.3.0 | 10.4.0 |
| 2013-12 | RAN#62 | R5s130627 | 0021 | - | Addition of EUTRA UE Positioning test case 7.3.4.3\_1s | 10.3.0 | 10.4.0 |
| 2013-12 | RAN#62 | RP-131871 | 0022 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.3.0 | 10.4.0 |
| 2014-03 | RAN#63 | R5-140326 | 0023 | - | A-GNSS ASN.1 reference | 10.4.0 | 10.5.0 |
| 2014-03 | RAN#63 | R5s130913 | 0024 | - | Correction to function fl\_TC\_7\_3\_5\_1\_GNSS\_TestBody | 10.4.0 | 10.5.0 |
| 2014-03 | RAN#63 | R5s130914 | 0025 | - | Correction to svID values in AcquisitionAssist and AuxiliaryInformation | 10.4.0 | 10.5.0 |
| 2014-03 | RAN#63 | R5s131009 | 0026 | - | Addition of EUTRA UE Positioning test case 7.3.5.1\_2s | 10.4.0 | 10.5.0 |
| 2014-03 | RAN#63 | R5s131011 | 0027 | - | Addition of EUTRA UE Positioning test case 7.3.5.1\_4s | 10.4.0 | 10.5.0 |
| 2014-03 | RAN#63 | RP-140316 | 0028 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.4.0 | 10.5.0 |
| 2014-06 | RAN#64 | R5s140086 | 0029 | - | Addition of EUTRA UE Positioning test case 7.2.1.1 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140088 | 0030 | - | Addition of EUTRA UE Positioning test case 7.2.1.2 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140090 | 0031 | - | Addition of EUTRA UE Positioning test case 7.2.1.3 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140242 | 0032 | - | Correction to LTE UE Positioning test case 7.3.5.1 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140253 | 0033 | - | Addition of EUTRA UE Positioning test case 7.3.4.4.1s | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140255 | 0034 | - | Addition of EUTRA UE Positioning test case 7.3.4.2.1s | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140257 | 0035 | - | Correction to LTE UE Positioning test case 7.3.4.3.1s | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140316 | 0036 | - | Addition of UTRAN UE Positioning test case 6.2.3.3 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140318 | 0037 | - | Addition of UTRAN UE Positioning test case 6.2.3.4 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140320 | 0038 | - | Addition of UTRAN UE Positioning test case 6.2.3.5 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140433 | 0039 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.3.4s | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140435 | 0040 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.4.4s | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | RP-140825 | 0041 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140086 | 0029 | - | Addition of EUTRA UE Positioning test case 7.2.1.1 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140088 | 0030 | - | Addition of EUTRA UE Positioning test case 7.2.1.2 | 10.5.0 | 10.6.0 |
| 2014-06 | RAN#64 | R5s140090 | 0031 | - | Addition of EUTRA UE Positioning test case 7.2.1.3 | 10.5.0 | 10.6.0 |
| 2014-09 | RAN#65 | R5-144256 | 0042 | - | Routine maintenance and updates | 10.6.0 | 10.7.0 |
| 2014-12 | RAN#66 | R5s140739 | 0043 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.2.4s | 10.7.0 | 10.8.0 |
| 2014-12 | RAN#66 | R5s140777 | 0044 | - | Usage of <MULTIPLE\_CNF> in UpperTesterFunctions | 10.7.0 | 10.8.0 |
| 2014-12 | RAN#66 | RP-142067 | 0045 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.7.0 | 10.8.0 |
| 2015-03 | RAN#67 | R5s141359 | 0047 | - | Correction of errors in implementation of positioning CRs | 10.8.0 | 10.9.0 |
| 2015-03 | RAN#67 | R5s150027 | 0048 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.1.4s | 10.8.0 | 10.9.0 |
| 2015-03 | RAN#67 | RP-150336 | 0049 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 10.8.0 | 10.9.0 |
| 2015-03 | RAN#67 | - | - | - | upgraded to Rel-11 with no change | 10.9.0 | 11.0.0 |
| 2015-03 | RAN#67 | R5-150735 | 0046 | - | Addition of BeiDou Test Model | 11.0.0 | 12.0.0 |
| 2015-06 | RAN#68 | RP-150897 | 0050 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150013 | 0051 | - | Addition of UTRAN UE Positioning test case 6.2.3.2.4s | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150222 | 0052 | - | Correction to POS ATS in TTCN-3 delivery 15wk10 | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150331 | 0053 | - | Rel-12 baseline upgrade for POS Test Suite | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150343 | 0054 | - | Corrections to UTRAN UE Positioning functions | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150344 | 0055 | - | Correction to LTE UE Positioning test cases 7.3.5.1.5s and 7.5.1 | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150345 | 0056 | - | Correction to GLONASS LPP test cases | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150353 | 0057 | - | Improvement of function f\_POS\_CheckGnssSupportList | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150404 | 0058 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.3.1 | 12.0.0 | 12.1.0 |
| 2015-06 | RAN#68 | R5s150439 | 0059 | - | Correction to selection of Assistance Data for sub-test 4 | 12.0.0 | 12.1.0 |
| 2015-09 | RAN#69 | RP-151421 | 0060 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | R5s150011 | 0061 | - | Addition of UTRAN UE Positioning test case 6.2.1.1.4s | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | R5s150589 | 0062 | - | Correction to EUTRA Positioning functions | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | R5s150590 | 0063 | - | Correction to Upper Tester modules | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | R5s150706 | 0064 | - | Addition of UTRAN UE Positioning test case 6.2.2.1.4s | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | R5s150708 | 0065 | - | Addition of UTRAN UE Positioning test case 6.2.2.3.4s | 12.1.0 | 12.2.0 |
| 2015-09 | RAN#69 | - | - | - | update of the "non-specific references" in section 2 according to the approved R5-153582 and an action point on ETSI MCC | 12.1.0 | 12.2.0 |
| 2015-12 | RAN#70 | R5s150710 | 0068 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.2.7s | 12.2.0 | 12.3.0 |
| 2015-12 | RAN#70 | R5s150712 | 0069 | - | Addition of GCF WI-166 EUTRA UE Positioning test case 7.3.4.4.7s | 12.2.0 | 12.3.0 |
| 2015-12 | RAN#70 | R5s150805 | 0070 | - | Correction to POS capability check procedure | 12.2.0 | 12.3.0 |
| 2015-12 | RAN#70 | R5s150911 | 0071 | - | Code improvements in Positioning test cases | 12.2.0 | 12.3.0 |
| 2015-12 | RAN#70 | RP-151697 | 0072 | - | CR to 37.571-4: Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 12.2.0 | 12.3.0 |
| 2016-03 | RAN#71 | R5s151010 | 0073 | - | Correction to POS type definition in ATS\_15wk38 | 12.3.0 | 12.4.0 |
| 2016-06 | RAN#72 | [R5s160479](http://www.3gpp.org/ftp/tsg_ran/WG5_Test_ex-T1/TTCN/TTCN_CRs/2016/Docs/R5s160479.zip) | 0074 | 1 | Correction to LTE Positioning test cases | 12.4.0 | 12.5.0 |
| 2016-06 | RAN#72 | [R5s160480](http://www.3gpp.org/ftp/tsg_ran/WG5_Test_ex-T1/TTCN/TTCN_CRs/2016/Docs/R5s160480.zip) | 0075 | 1 | Correction to UTRA Positioning test cases | 12.4.0 | 12.5.0 |
| 2016-09 | RAN#73 | R5s160713 | 0076 | - | Rel-13 baseline upgrade for POS Test Suite | 12.5.0 | 13.0.0 |
| 2016-12 | RAN#74 | - | - | - | updated to deliver latest TTCN | 13.0.0 | 13.1.0 |
| 2017-03 | RAN#75 | R5-171531 | 0082 | - | Indoor Positioning: Introduction of Test Model | 13.1.0 | 13.2.0 |
| 2017-03 | RAN#75 | [R5s170127](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170127.zip) | 0078 | 1 | Correction to GCF WI-166 EUTRA UE Positioning test case 7.3.4.4.7s | 13.1.0 | 13.2.0 |
| 2017-03 | RAN#75 | [R5s170128](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170128.zip) | 0079 | 1 | Correction to function f\_POS\_CheckCapabilities() for OTDOA | 13.1.0 | 13.2.0 |
| 2017-03 | RAN#75 | [R5s170186](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170186.zip)/RP-170104 | 0084 |  | Update ASP changes due to inclusion of iPOS in 37.571-4 (prose), Annex D | 13.1.0 | 13.2.0 |
| 2017-06 | RAN#76 | [R5s170311](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170311.zip) | 0085 | - | Addition of LTE UE Positioning test case 7.3.4.1.10s | 13.2.0 | 13.3.0 |
| 2017-06 | RAN#76 | [R5s170313](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170313.zip) | 0086 | - | Addition of LTE UE Positioning test case 7.3.4.3.10s | 13.2.0 | 13.3.0 |
| 2017-06 | RAN#76 | [R5s170363](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170363.zip) | 0087 | - | Aligning name of PICS used in TTCN to the TS 37.571-3 definition | 13.2.0 | 13.3.0 |
| 2017-06 | RAN#76 | [R5s170383](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170383.zip) | 0083 | 1 | Corrections to UE Positioning test cases | 13.2.0 | 13.3.0 |
| 2017-06 | RAN#76 | [R5s170416](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170416.zip) | 0088 | - | Update of TC list in 37.571-4 (prose), Annex A, due to merging of GNSS subtest | 13.2.0 | 13.3.0 |
| 2017-09 | RAN#77 | [R5s170630](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170630.zip) | 0089 | 1 | Correction to function ‘f\_POS\_CheckGnssSupportList’ | 13.3.0 | 13.4.0 |
| 2017-09 | RAN#77 | [R5s170599](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170599.zip) | 0090 |  | Rel-14 baseline upgrade for POS Test Suite | 13.4.0 | 14.0.0 |
| 2017-09 | RAN#77 | R5-173663 | 0091 | - | Indoor Positioning Enhancements: Introduction of Test Model | 13.4.0 | 14.0.0 |
| 2017-12 | RAN#78 | R5-176982 | 0093 | 1 | GNSS Test Model updates for V2X | 14.0.0 | 14.1.0 |
| 2017-12 | RAN#78 | [R5s170860](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2017/Docs/R5s170860.zip) | 0092 | 1 | Correction to UE Positioning test case 7.3.1.1 | 14.0.0 | 14.1.0 |
| 2018-03 | RAN#79 | R5-180677 | 0099 | - | Routine maintenance for TS 37.571-4 | 14.1.0 | 14.2.0 |
| 2018-03 | RAN#79 | [R5s180081](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180081.zip) | 0094 | 1 | Correction to EUTRA release information for UE Positioning TCs | 14.1.0 | 14.2.0 |
| 2018-03 | RAN#79 | [R5s180113](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180113.zip) | 0095 | 1 | Addition of LTE UE Positioning test case 7.3.4.2.15s (BDS) | 14.1.0 | 14.2.0 |
| 2018-03 | RAN#79 | [R5s180114](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180114.zip) | 0096 | 1 | Addition of LTE UE Positioning test case 7.3.4.4.15s (BDS) | 14.1.0 | 14.2.0 |
| 2018-03 | RAN#79 | [R5s180115](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180115.zip) | 0097 | 1 | Addition of LTE UE Positioning test case 7.3.5.1.15s (BDS) | 14.1.0 | 14.2.0 |
| 2018-06 | RAN#80 | R5-182292 | 0102 | - | V2X: Test Model updates | 14.2.0 | 14.3.0 |
| 2018-06 | RAN#80 | [R5s180327](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180327.zip) | 0101 | 1 | Correction / improvement to UE Positioning TCs 7.2.2.1 + 7.2.2.2 | 14.2.0 | 14.3.0 |
| 2018-12 | RAN#82 | [R5s180569](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180569.zip) | 0105 | - | Correction to number of almanac elements for Galileo | 14.3.0 | 14.4.0 |
| 2018-12 | RAN#82 | [R5s180554](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2018/Docs/R5s180554.zip) | 0103 | - | Rel-15 Sep'18 baseline upgrade for POS Test Suite | 14.4.0 | 15.0.0 |
| 2019-03 | RAN#83 | R5s190056 | 0106 | - | Correction to checking LPP ePDU capabilities | 15.0.0 | 15.1.0 |
| 2019-09 | RAN#85 | R5-197174 | 0111 | 1 | UE Positioning over NR: Initial Test Model | 15.1.0 | 15.2.0 |
| 2019-09 | RAN#85 | [R5s190462](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2019/Docs/R5s190462.zip) | 0109 | - | Correction to f\_POS\_CheckCapabilities\_Agnss | 15.1.0 | 15.2.0 |
| 2019-09 | RAN#85 | [R5s190463](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2019/Docs/R5s190463.zip) | 0110 | - | Correction to f\_POS\_CheckGnssSupportList | 15.1.0 | 15.2.0 |
| 2019-09 | RAN#85 | [R5s190759](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2019/Docs/R5s190759.zip) | 0112 | - | Rel-15 Jun'19 partial baseline upgrade for POS TTCN-3 Test Suite | 15.1.0 | 15.2.0 |
| 2019-12 | RAN#86 | R5-198140 | 0113 | - | Aerial Vehicles: Test Model addition | 15.2.0 | 15.3.0 |
| 2019-12 | RAN#86 | R5-198142 | 0114 | - | UE Positioning over NR: Test Model updates | 15.2.0 | 15.3.0 |
| 2019-12 | RAN#86 | R5-198156 | 0115 | - | Routine maintenance for TS 37.571-4 | 15.2.0 | 15.3.0 |
| 2019-12 | RAN#86 | [R5s191048](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2019/Docs/R5s191048.zip) | 0116 | - | Correction to the initialisation function for LTE Positioning test cases | 15.2.0 | 15.3.0 |
| 2020-03 | RAN#87 | R5-200261 | 0118 | - | Routine maintenance for TS 37.571-4 | 15.3.0 | 15.4.0 |
| 2020-03 | RAN#87 | R5-200262 | 0119 | - | Editorial changes to TS 37.571-X titles to remove references to individual RATs | 15.3.0 | 15.4.0 |
| 2020-06 | RAN#88 | [R5s200581](http://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s200581.zip) | 0120 | - | Correction to f\_POS\_CheckGnssSupportList | 15.4.0 | 15.5.0 |
| 2020-12 | RAN#90 | [R5s201391](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201391.zip) | 0122 | - | Addition of 5G UE Positioning test case 9.3.1.1 | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201393](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201393.zip) | 0123 | - | Addition of 5G UE Positioning test case 9.3.1.2.15s | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201395](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201395.zip) | 0124 | - | Addition of 5G UE Positioning test case 9.3.2.1 | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201397](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201397.zip) | 0125 | - | Addition of 5G UE Positioning test case 9.3.2.2 | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201399](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201399.zip) | 0126 | - | Addition of 5G UE Positioning test case 9.3.2.3 | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201401](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201401.zip) | 0127 | - | Addition of 5G UE Positioning test case 9.3.4.1.15s | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201403](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201403.zip) | 0128 | - | Addition of 5G UE Positioning test case 9.3.4.2.15s | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201405](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201405.zip) | 0129 | - | Addition of 5G UE Positioning test case 9.3.4.3.15s | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201407](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201407.zip) | 0130 | - | Addition of 5G UE Positioning test case 9.3.4.4.15s | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201460](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201460.zip) | 0131 | - | Correction to several NR5GC UE Positioning Test related functions | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201529](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201529.zip) | 0132 | - | Correction to function f\_POS\_NR\_SendLppAck() | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201649](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201649.zip) | 0134 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 15.5.0 | 15.6.0 |
| 2020-12 | RAN#90 | [R5s201388](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2020/Docs/R5s201388.zip) | 0121 | - | Rel-16 Sep'20 baseline upgrade for POS Test Suite | 15.6.0 | 16.0.0 |
| 2021-03 | RAN#91 | [R5s210208](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210208.zip) | 0133 | 1 | Correction to function f\_POS\_NR\_CheckAgnssMultiFreq | 16.0.0 | 16.1.0 |
| 2021-03 | RAN#91 | [R5s210262](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210262.zip) | 0135 | 1 | Correction to a NR5GC UE Positioning related function | 16.0.0 | 16.1.0 |
| 2021-06 | RAN#92 | R5-212285 | 0138 | - | Routine maintenance for TS 37.571-4 | 16.1.0 | 16.2.0 |
| 2021-06 | RAN#92 | [R5s210416](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210416.zip) | 0136 | - | Correction for common POS function f\_POS\_SelectTemplateReq\_IonosphModel() | 16.1.0 | 16.2.0 |
| 2021-09 | RAN#93 | R5-214729 | 0143 | - | Routine maintenance for TS 37.571-4 | 16.2.0 | 16.3.0 |
| 2021-09 | RAN#93 | [R5s210887](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210887.zip) | 0144 | - | Correction to NR5GC Positioning Functions | 16.2.0 | 16.3.0 |
| 2021-09 | RAN#93 | [R5s210922](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210922.zip) | 0141 | 1 | Correction for multi frequency GNSS support checking | 16.2.0 | 16.3.0 |
| 2021-09 | RAN#93 | [R5s210926](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s210926.zip) | 0142 | 1 | Addition of NR5GC Positioning test case 9.3.1.2.5s | 16.2.0 | 16.3.0 |
| 2021-09 | RAN#93 | [R5s211177](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s211177.zip) | 0145 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 16.2.0 | 16.3.0 |
| 2021-12 | RAN#94 | R5-216658 | 0149 | - | NR Positioning: Test Model addition | 16.3.0 | 16.4.0 |
| 2021-12 | RAN#94 | R5-217256 | 0151 | - | Include new pixit for the 2012 GNSS scenarios | 16.3.0 | 16.4.0 |
| 2021-12 | RAN#94 | [R5s211307](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s211307.zip) | 0147 | - | Correction to POS\_Parameters | 16.3.0 | 16.4.0 |
| 2021-12 | RAN#94 | [R5s211515](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s211515.zip) | 0148 | - | Correction to f\_POS\_OTDOA\_CheckEutraBand | 16.3.0 | 16.4.0 |
| 2021-12 | RAN#94 | [R5s211696](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2021/Docs/R5s211696.zip) | 0153 | - | Add new ASP definitions for NR test model extension in Rel-16 | 16.3.0 | 16.4.0 |
| 2022-03 | RAN#95 | R5-220457 | 0156 | - | 5G V2X: GNSS Test Model updates for NR sidelink | 16.4.0 | 16.5.0 |
| 2022-03 | RAN#95 | [R5s220170](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220170.zip) | 0152 | 1 | Correction to NR5GC\_Positioning\_Functions for capability check | 16.4.0 | 16.5.0 |
| 2022-03 | RAN#95 | [R5s220432](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220432.zip) | 0154 | 1 | Correction to f\_POS\_NR\_CheckCapabilities\_NR\_Ecid | 16.4.0 | 16.5.0 |
| 2022-03 | RAN#95 | [R5s220433](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220433.zip) | 0155 | 1 | Correction to SVIDs for 2012 GNSS scenario | 16.4.0 | 16.5.0 |
| 2022-03 | RAN#95 | [R5s220439](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220439.zip) | 0158 | - | Update of TTCN type definitions, Annex D | 16.4.0 | 16.5.0 |
| 2022-06 | RAN#96 | [R5s220671](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220671.zip) | 0159 | - | Correction to f\_UT\_AT\_CheckNotifyLocationRequest | 16.5.0 | 16.6.0 |
| 2022-06 | RAN#96 | [R5s220672](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220672.zip) | 0160 | - | Correction to f\_POS\_NR\_Set\_DlPrsPeriodicityAndOffset\_11ms | 16.5.0 | 16.6.0 |
| 2022-09 | RAN#97 | [R5s220765](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220765.zip) | 0163 | - | Correction to function f\_TC\_7\_3\_4\_2\_7s\_EUTRA | 16.6.0 | 16.7.0 |
| 2022-09 | RAN#97 | [R5s220799](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220799.zip) | 0164 | - | Correction to f\_TC\_7\_3\_4\_4\_7s\_EUTRA | 16.6.0 | 16.7.0 |
| 2022-09 | RAN#97 | [R5s220900](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s220900.zip) | 0162 | 1 | Addition of LTE POS testcase 7.2.2.2.5s | 16.6.0 | 16.7.0 |
| 2022-09 | RAN#97 | [R5s221026](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221026.zip) | 0165 | - | Rel-16 Mar'22 partial baseline upgrade for POS Test Suite | 16.6.0 | 16.7.0 |
| 2022-09 | RAN#97 | [R5s221073](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221073.zip) | 0173 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 16.6.0 | 16.7.0 |
| 2022-12 | RAN#98 | [R5s221296](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221296.zip) | 0166 | 1 | Correction to f\_POS\_NR\_CheckCapabilities\_Prs\_ProcessingCapabilityBandList | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221350](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221350.zip) | 0168 | 1 | Addition of POS testcase 9.3.1.2.19s | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221351](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221351.zip) | 0169 | 1 | Addition of POS testcase 9.3.4.2.19s | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221352](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221352.zip) | 0170 | 1 | Addition of POS testcase 9.3.4.2.20s | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221353](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221353.zip) | 0171 | 1 | Addition of POS testcase 9.3.4.2.21s | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221354](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221354.zip) | 0172 | 1 | Addition of POS testcase 9.3.4.2.22s | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221363](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221363.zip) | 0175 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 16.7.0 | 16.8.0 |
| 2022-12 | RAN#98 | [R5s221180](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2022/Docs/R5s221180.zip) | 0174 | - | Rel-17 Sep'22 baseline upgrade for POS Test Suite | 16.8.0 | 17.0.0 |
| 2023-03 | RAN#99 | [R5s230101](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230101.zip) | 0178 | - | Addition of NR POS testcase 9.3.4.4.21s | 17.0.0 | 17.1.0 |
| 2023-03 | RAN#99 | [R5s230205](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230205.zip) | 0176 | 1 | Addition of NR POS testcase 9.3.4.4.19s | 17.0.0 | 17.1.0 |
| 2023-03 | RAN#99 | [R5s230206](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230206.zip) | 0177 | 1 | Addition of NR POS testcase 9.3.4.4.20s | 17.0.0 | 17.1.0 |
| 2023-03 | RAN#99 | [R5s230260](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230260.zip) | 0179 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 17.0.0 | 17.1.0 |
| 2023-06 | RAN#100 | [R5s230438](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230438.zip) | 0180 | - | Addition of LTE POS testcase 7.2.2.2.6.FDDs | 17.1.0 | 17.2.0 |
| 2023-06 | RAN#100 | [R5s230440](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230440.zip) | 0181 | - | Addition of LTE POS testcase 7.2.2.2.6.TDDs | 17.1.0 | 17.2.0 |
| 2023-06 | RAN#100 | [R5s230473](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230473.zip) | 0182 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 17.1.0 | 17.2.0 |
| 2023-09 | RAN#101 | [R5s230498](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230498.zip) | 0183 | - | Correction for NR5GC positioning test cases | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230499](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230499.zip) | 0184 | - | Correction for EUTRA positioning test case 7.3.4.4\_7s | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230502](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230502.zip) | 0185 | - | Addition of CNF templates in PosSystem\_Control | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230513](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230513.zip) | 0186 | - | Correction to f\_NR\_ConfigUlSrsMultiRTT | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230595](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230595.zip) | 0187 | - | Correction for GNSS 15s test cases | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230608](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230608.zip) | 0188 | - | Correction to svID values in AcquisitionAssist and AuxiliaryInformation for GNSS Scenarios 2020 | 17.2.0 | 17.3.0 |
| 2023-09 | RAN#101 | [R5s230674](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230674.zip) | 0191 | - | Update of TTCN type definitions, Annexes C and E | 17.2.0 | 17.3.0 |
| 2023-12 | RAN#102 | [R5s230711](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230711.zip) | 0192 | - | Correction for positioning test cases | 17.3.0 | 17.4.0 |
| 2023-12 | RAN#102 | [R5s230755](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230755.zip) | 0193 | - | Correction for function f\_POS\_NR\_CheckCapabilities\_Prs\_ProcessingCapabilityBandList() | 17.3.0 | 17.4.0 |
| 2023-12 | RAN#102 | [R5s230842](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230842.zip) | 0189 | 1 | Rel-17 June'23 partial baseline upgrade for POS Test Suite | 17.3.0 | 17.4.0 |
| 2023-12 | RAN#102 | [R5s230846](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2023/Docs/R5s230846.zip) | 0190 | 1 | Corrections on control module for POS Test Suite | 17.3.0 | 17.4.0 |
| 2024-03 | RAN#103 | R5-240553 | 0198 | - | Removal of PIXIT for deprecated signalling GNSS scenarios | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240144](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240144.zip) | 0195 | - | Correction to f\_POS\_NR\_Set\_DlPrsAssistanceDataPerTRP | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240146](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240146.zip) | 0196 | - | Addition of NR5GC POS test case 9.3.1.2.21s | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240160](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240160.zip) | 0197 | - | Correction to f\_POS\_NR\_CheckCapabilities | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240169](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240169.zip) | 0200 | - | Addition of NR POS Test case 9.3.1.2.20s | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240199](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240199.zip) | 0194 | 1 | Correction to function f\_POS\_NR\_CheckCapabilities\_NR\_Ecid | 17.4.0 | 17.5.0 |
| 2024-03 | RAN#103 | [R5s240240](https://www.3gpp.org/ftp/TSG_RAN/WG5_Test_ex-T1/TTCN/TTCN_CRs/2024/Docs/R5s240240.zip) | 0201 | - | Add new verified and e-mail agreed TTCN test cases in the TC lists in 37.571-4 (prose), Annex A | 17.4.0 | 17.5.0 |