**3GPP TSG-SA3 Meeting #108-e *draft\_S3-222020-r1***

**Online, , 22nd Aug 2022 - 26th Aug 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | 1 | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  with existing procedures |
|  |  |
| ***Source to WG:*** | Ericsson, Huawei, Xiaomi |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2022-08-15 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The identifier AF-Service-Identifier is used in TS 23.502, 4.15.3.2.10, for the interaction between an untrusted AF and NEF for the NSACF notification procedure. However the ENSI parameter used in the security handling of the same procedure in TS 33.501, 16.6.3 for the same purposes as the AF-Service-Identifier. Therefore the ENSI parameter is redundant and proposed to be removed in order to algn TS 23.502, 4.5.3.2.10 and TS 33.501 16.6.3. |
|  |  |
| ***Summary of change:*** | The ENSI parameter is replaced with the AF-Service-Identifer in the EventFilter parameter for AF deployed outside the 3GPP operator domain.  |
|  |  |
| ***Consequences if not approved:*** | Unclear specification. |
|  |  |
| ***Clauses affected:*** | 16.6.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* BEGIN CHANGES \*\*\*

### 16.6.3 Subscription/unsubscription procedure of NSACF notification service



Figure 16.6.3-1: Subscription/unsubscription of NSACF notification procedure

0. Authentication of AF: AF is authenticated by NRF or authenticated by NEF based on description in clause 13 or clause 12. A token is generated for AF after authentication and authorization.

Editor’s Note: It is FFS how AF outside the 3GPP operator domain is authorized.

1. To subscribe or unsubscribe for the number of UEs or the number of PDU Sessions per network slice notification with the NSACF, the AF sends Nnef\_EventExposure\_Subscribe/Unsubscribe Request (Event ID, Event Filter, Event Reporting information) message to the NEF as described in TS 23.502 [8]. The Event Filter parameter shall be AF-Service-Identifier for an AF deployed outside the 3GPP operator domain. Other parameters are specified in TS 23.502 [8]. The AF-Service-Identifier defined in TS 23.502 [8]. AF-Service-Identifier is a kind of ENSI.

2. The NEF confirms with Nnef\_ SliceStatusEventExposure \_Subscribe/Unsubscribe Response message to the AF.

The Event Filter parameter is the mapped AF-Service-Identifier for the AF deployed outside the 3GPP operator domain.

3. The NEF checks whether the AF is authorised for the requested subscription based on the AF token. It needs to check whether the token claims match the AF’s identity and the Event Filter parameter. If authorised, the NEF may query the NRF to find the NSACF responsible for the requested S-NSSAI (NEF needs to map to S-NSSAI based on AF-Service-Identifier for the AF deployed outside the 3GPP operator domain).

4. The NEF forwards the request to the NSACF with Nnsacf\_SliceEventExposure\_Subscribe/Unsubscribe Request (Event ID, Event Filter, Event Reporting information). The Event Filter parameter shall be the mapped S-NSSAI for the AF deployed outside the 3GPP operator domain.

5. The NSACF confirms with Nnsacf\_SliceEventExposure\_Subscribe/Usubscribe Response message to the NEF as in TS 23.502 [8].

6-7a. The NSACF triggers a notification towards the AF and sends the Nnsacf\_SliceEvent Exposure\_Notify (Event ID, Event Filter, Event Reporting information) message to the NEF as described in TS 23.502 [8].

7b-9. The NEF forwards the message to the AF for single NSACF or aggregates reporting information for multiple NSACFs in the Nnef\_EventExposure\_Notify (Event ID, Event Filter, Event Reporting information) message as described in TS 23.502 [8]. The Event Filter parameter shall be the mapped AF-Service-Identifier from the S-NSSAI for the AF deployed outside the 3GPP operator domain.

\*\*\* END CHANGES \*\*\*