**3GPP TSG-SA3 Meeting #85-LI-e *s3i220224***

**Online, , 25th Apr 2022 - 29th Apr 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **33.128** | **CR** | **0344** | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Addition of Handover LI Stage 3 |
|  |  |
| ***Source to WG:*** | SA3-LI (OTD) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI18 |  | ***Date:*** | 2022-04-24 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | This contribution adds the capability to perform LI on RAN and inter-system handovers which is currently not supported in TS 33.128. Related to Stage 2 in s3i220223. |
|  |  |
| ***Summary of change:*** | Creates new clause 6.2.2.2.X and associated sub-clauses for reporting Handovers. Modifies and adds to ASN.1 for repoting relevant parameters.  |
|  |  |
| ***Consequences if not approved:*** | TS 33.128 will be incomplete and unable to report handovers.  |
|  |  |
| ***Clauses affected:*** | 6.2.2.2.X (new), Annex A |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR … CR …  |
|  |  |
| ***Other comments:*** | Related to Stage 2 in s3i220223.ASN.1 is in Forge and can be found here: <https://forge.3gpp.org/rep/sa3/li/-/merge_requests/33/diffs?commit_id=6fd5f1590c103e26ae19f04a7343a377b455156d>  |
|  |  |
| ***This CR’s revision history:*** | s3i220224 |

START OF FIRST CHANGE

6.2.2.2.X Handovers

6.2.2.2.X.1 General

The present clause provides the LI requirements for NG interface-based handovers which occur for a target UE. Such handovers may be intra 5GS (inter-gNB), 5GS to EPS (inter-system), EPS to 5GS (inter-system), or 5GS to UTRA (inter-system).

The following xIRI records are used to report handover related events between the AMF and RAN nodes for the target UE:

 - AMFRANHandoverCommand

 - AMFRANHandoverRequest

 - AMFRANHandoverNotify

The above xIRIs shall include the information transferred between the AMF and RAN nodes, as a part of handover preparation, resource allocation, and handover notification.

6.2.2.2.X.2 Handover command

The IRI-POI in the AMF shall generate an xIRI containing an AMFRANHandoverCommand record when the IRI-POI present in the AMF detects that the AMF has sent a HANDOVER COMMAND message to the source RAN node (old RAN node) in response to a HANDOVER REQUIRED message for the target UE.

Table 6.2.2.2.X.2-1: Payload for AMFRANHandoverCommand record

|  |  |  |
| --- | --- | --- |
| **Field name** | **Description** | **M/C/O** |
| userIdentifiers | List of identifiers, including the target identifier, associated with the target UE registration stored in the AMF context. See TS 29.518 [22]clause 6.1.2.2.5. | M |
| aMFMessageType | Identifies the type of message being sent. This value shall be “initiating” for this xIRI. See TS 38.413 [23] clause 9.3.1.1 | M |
| aMFUENGAPID | Identity that the AMF uses to uniquely identify the target UE over the NG Interface. See TS 38.413 [23] clause 9.3.1.1. This is correlated to the SUPI known in the UE AMF context. | M |
| rANUENGAPID | Identity that the AMF receives from the NG-RAN node uniquely identifying the target UE with the NG-RAN Node. See TS 38.413 [23] clause 9.3.3.2. | M |
| handoverType | Identifies the type of handover indicated by the source RAN node to the AMF. See TS 38.413 [23] clause 9.3.1.22. | M |
| nASSecurityParameters | Includes security related parameters for inter-system handovers. Shall be included for inter-system handovers. See TS 38.413 [23] clause 9.3.3.26. | C |
| targetToSourceContainer | Provides radio related information about the gaining NG-RAN node. See TS 38.413 [23] clause 9.3.1.21. | M |

6.2.2.2.X.3 Handover request

The IRI-POI in the AMF shall generate an xIRI containing an AMFRANHandoverRequest record when the IRI-POI in the AMF detects that the AMF received a HANDOVER REQUEST ACKNOWLEDGE message from the gaining RAN node (new RAN node) for the target UE.

NOTE: The gaining RAN node sends the HANDOVER REQUEST ACKNOWLEDGE in response to a HANDOVER REQUEST from the AMF.

**Table 6.2.2.2.X.3-1: Payload for AMFRANHandoverRequest record**

|  |  |  |
| --- | --- | --- |
| **Field name** | **Description** | **M/C/O** |
| userIdentifiers | List of user identifiers associated with the target UE registration stored in the AMF context. See TS 29.518 [22] clause 6.1.2.2.5. | M |
| aMFmessageType | Identifies the type of message being sent. See TS 38.413 [23] clause 9.3.1.1. | M |
| aMFUENGAPID | Identity that the AMF uses to uniquely identify the target UE over the NG Interface, See TS 38.413 [23] clause 9.3.1.1. This is correlated to the SUPI known in the UE AMF context. | M |
| rANUENGAPID | Identity that the AMF receives from the NG-RAN node uniquely identifying the target UE within the NG-RAN Node. See TS 38.413 [23] clause 9.3.3.2. | M |
| handoverType | Identifies the type of handover indicated by the AMF to gaining RAN Node as seen in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.22. | M |
| handoverCause | Indicates the cause of handover as seen in the HANDOVER REQUEST message from AMF to gaining RAN node. See TS 38.413 [23] clause 9.3.1.2. | M |
| uEAMBR | Indicates UE aggregate maximum uplink and downlink bitrates as sent in the HANDOVER REQUEST message from AMF to gaining RAN node. See TS 38.413 [23] clause 9.3.1.58. | M |
| uESecurityCapabilities | Indicates the UE support of specific encryption and integrity protection algorithms as sent in HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.86. | C |
| securityContext | Provides the gaining RAN node with the next-hop chaining counter and information to generate security keys for User Plane traffic and RRC messages as seen in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.88. | M |
| pDUSessionResourceInformation | Indicates the PDU Session to be transferred and Handover Command Transfer information as seen in the HANDOVER REQUEST and confirmed in the HANDOVER REQUEST ACKNOWLEDGE message. See TS 38.413 [23] clauses 9.3.1.50 and 9.3.4.10. | M |
| allowedNSSAI | Indicates UE allowed NSSAI as seen in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.31. | M |
| aMFTraceActivation | Indicates whether MDT Trace is requested in HANDOVER REQUEST and provides parameters for Trace Activation. See TS 38.413 [23] clauses 8.4.2.2 and 9.3.1.14. | C |
| rANSourceToTargetContainer | Provides radio related information via the AMF in the HANDOVER REQUEST from source to gaining NG-RAN node. See TS 38.413 [23] clause 9.3.1.21. | M |
| mobilityRestrictionList | Provides roaming or access restrictions related to mobility from AMF to gaining RAN Node. Include if sent in HANDOVER REQUEST. See TS 38.413 [23] clause 9.3.1.85. | C |
| locationReportingRequestType | Indicates the type of location reporting requested in the HANDOVER REQUEST. Include if in HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.65. | C |
| gUAMI | Identifies the globally unique AMF Identity of the serving AMF. See TS 38.413 [23] clause 9.3.3.3. | M |
| voiceEPSFallback | Indicates to the gaining RAN node that the UE and AMF support voice EPS Fallback. Include if in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.116. | C |
| sRVCCOperation | Indicates to gaining RAN node if SRVCC operation is possible. Include if in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.128. | C |
| iABAuthorizedIndicator | Indicates to the gaining RAN node if UE is allowed to operate as IAB node. Include if in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.129. | C |
| nRV2XAuthorizedIndicator | Indicates to the gaining RAN node if the UE is authorized to use NR sidelink for vehicle or pedestrian V2X Services. Include if in the HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.146. | C |
| lTEV2XAuthorizedIndicator | Indicates to the gaining RAN node if the UE is authorized to use LTE sidelink for vehicle or pedestrian V2X Services. Include if in the HANDOVER REQUEST. See clause TS 38.413 [23] 9.3.1.147. | C |
| nRSidelinkAMBR | Indicates to the gaining RAN node the AMBR for the UE using NR V2X services. Include if UE is NR V2X Authorized. See TS 38.413 [23] clause 9.3.1.148. | C |
| lTEUESidelinkAMBR | Indicates to the gaining RAN node the AMBR for the UE using LTE V2X services. Include if UE is NR V2X Authorized. See TS 38.413 [23] clause 9.3.1.149. | C |
| pC5QoSParameters | Provides information to the gaining RAN node regarding the PC5 QoS parameters for the UE’s sidelink communications for NR PC5. Include if in HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.150. | C |
| mDTPLMNList | Indicates to the gaining RAN node what PLMNs should be considered as valid for MDT Trace request. Include if in HANDOVER REQUEST message. See TS 38.413 [23] clause 9.3.1.168. | C |
| uERadioCapability | Identifier that provides the UE radio capabilities to the gaining RAN node. Include if in HANDOVER REQUEST message. See TS 23.003 [19] clause and TS 38.413 [23] clause 9.3.1.142. | C |
| handoverRequestACKTransferInfo | Contains tunnel and QoS information passed from gaining RAN node via the AMF, destined for UPF in the HANDOVER REQUEST ACKNOWLEDGE message. See TS 38.413 [23] clause 9.3.4.11. | M |
| targetToSourceContainer | Provides radio related information from gaining to losing NG-RAN node that the AMF receives from the gaining RAN Node in the HANDOVER REQUEST ACKNOWLEDGE message. See TS 38.413 [23] clause 9.3.1.21. | M |
| criticality | Indicates IE criticality, IE Identifier, and type of error. Include if sent in the HANDOVER REQUEST ACKNOWLEDGE message from gaining RAN node to AMF. See TS 38.413 [23] clause 9.3.1.3.  | C |
| nPNAccessInformation | Globally identifies the secondary NG-RAN node CAG Cells. Include if sent in the HANDOVER REQUEST ACKNOWLEDGE message from gaining RAN node to AMF. See TS 38.413 [23] clause 9.3.3.46. | C |
| rEDCAPIndicaton | Indicates to the AMF if the gaining RAN node supports UE reduced capability request. Include if in the HANDOVER REQUEST ACKNOWLEDGE message. See TS 38.413 [23] clause 9.3.1.228. | C |

6.2.2.2.X.4 Handover notify

The IRI-POI in the AMF shall generate an AMFRANHandover Notify record when the IRI-POI in the AMF detects that the AMF has received HANDOVER NOTIFY from the gaining RAN node indicating handover is complete and target UE has been identified in the gaining node.

Table 6.2.2.2.X.4-1: Payload for AMFRANHandoverNotify record

|  |  |  |
| --- | --- | --- |
| **Field name** | **Description** | **M/C/O** |
| userIdentifiers | List of user identifiers associated with the target UE registration stored in the AMF context. See TS 29.518 [22]clause 6.1.2.2.5. | M |
| aMFMessageType | Identifies the type of message being sent. See TS 38.413 [23] clause 9.3.1.1 | M |
| aMFUENGAPID | Identity that the AMF uses to uniquely identify the target UE over the NG Interface. See TS 38.413 [23] clause 9.3.1.1. This is correlated to the SUPI known in the UE AMF context. | M |
| rANUENGAPID | Identity that the AMF receives from the NG-RAN node uniquely identifying the target UE with the NG-RAN Node. See TS 38.413 [23] clause 9.3.3.2. | M |
| location | User location information that the AMF receives from gaining RAN node in HANDOVER NOTIFY message. see TS 38.413 clauses 9.2.3.7 and 9.3.1.16. | M |

END OF FIRST CHANGE

START OF SECOND CHANGE

Annex A (normative):
ASN.1 Schema for the Internal and External Interfaces

TS33128Payloads

{itu-t(0) identified-organization(4) etsi(0) securityDomain(2) lawfulIntercept(2) threeGPP(4) ts33128(19) r17(17) version3(3)}

DEFINITIONS IMPLICIT TAGS EXTENSIBILITY IMPLIED ::=

BEGIN

-- =============

-- Relative OIDs

-- =============

tS33128PayloadsOID RELATIVE-OID ::= {threeGPP(4) ts33128(19) r17(17) version3(3)}

xIRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xIRI(1)}

xCCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xCC(2)}

iRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID iRI(3)}

cCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID cC(4)}

lINotificationPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID lINotification(5)}

-- ===============

-- X2 xIRI payload

-- ===============

XIRIPayload ::= SEQUENCE

{

 xIRIPayloadOID [1] RELATIVE-OID,

 event [2] XIRIEvent

}

XIRIEvent ::= CHOICE

{

 -- Access and mobility related events, see clause 6.2.2

 registration [1] AMFRegistration,

 deregistration [2] AMFDeregistration,

 locationUpdate [3] AMFLocationUpdate,

 startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

 unsuccessfulAMProcedure [5] AMFUnsuccessfulProcedure,

 -- PDU session-related events, see clause 6.2.3

 pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

 pDUSessionModification [7] SMFPDUSessionModification,

 pDUSessionRelease [8] SMFPDUSessionRelease,

 startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

 unsuccessfulSMProcedure [10] SMFUnsuccessfulProcedure,

 -- Subscriber-management related events, see clause 7.2.2

 servingSystemMessage [11] UDMServingSystemMessage,

 -- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

 sMSMessage [12] SMSMessage,

 -- LALS-related events, see clause 7.3.3

 lALSReport [13] LALSReport,

 -- PDHR/PDSR-related events, see clause 6.2.3.4.1

 pDHeaderReport [14] PDHeaderReport,

 pDSummaryReport [15] PDSummaryReport,

 -- tag 16 is reserved because there is no equivalent mDFCellSiteReport in XIRIEvent

 -- MMS-related events, see clause 7.4.2

 mMSSend [17] MMSSend,

 mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

 mMSNotification [19] MMSNotification,

 mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

 mMSNotificationResponse [21] MMSNotificationResponse,

 mMSRetrieval [22] MMSRetrieval,

 mMSDeliveryAck [23] MMSDeliveryAck,

 mMSForward [24] MMSForward,

 mMSDeleteFromRelay [25] MMSDeleteFromRelay,

 mMSDeliveryReport [26] MMSDeliveryReport,

 mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

 mMSReadReport [28] MMSReadReport,

 mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

 mMSCancel [30] MMSCancel,

 mMSMBoxStore [31] MMSMBoxStore,

 mMSMBoxUpload [32] MMSMBoxUpload,

 mMSMBoxDelete [33] MMSMBoxDelete,

 mMSMBoxViewRequest [34] MMSMBoxViewRequest,

 mMSMBoxViewResponse [35] MMSMBoxViewResponse,

 -- PTC-related events, see clause 7.5.2

 pTCRegistration [36] PTCRegistration,

 pTCSessionInitiation [37] PTCSessionInitiation,

 pTCSessionAbandon [38] PTCSessionAbandon,

 pTCSessionStart [39] PTCSessionStart,

 pTCSessionEnd [40] PTCSessionEnd,

 pTCStartOfInterception [41] PTCStartOfInterception,

 pTCPreEstablishedSession [42] PTCPreEstablishedSession,

 pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

 pTCPartyJoin [44] PTCPartyJoin,

 pTCPartyDrop [45] PTCPartyDrop,

 pTCPartyHold [46] PTCPartyHold,

 pTCMediaModification [47] PTCMediaModification,

 pTCGroupAdvertisement [48] PTCGroupAdvertisement,

 pTCFloorControl [49] PTCFloorControl,

 pTCTargetPresence [50] PTCTargetPresence,

 pTCParticipantPresence [51] PTCParticipantPresence,

 pTCListManagement [52] PTCListManagement,

 pTCAccessPolicy [53] PTCAccessPolicy,

 -- More Subscriber-management related events, see clause 7.2.2

 subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

 cancelLocationMessage [55] UDMCancelLocationMessage,

 -- SMS-related events continued from choice 12

 sMSReport [56] SMSReport,

 -- MA PDU session-related events, see clause 6.2.3.2.7

 sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

 sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

 sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

 startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

 unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

 -- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

 aMFIdentifierAssociation [62] AMFIdentifierAssociation,

 mMEIdentifierAssociation [63] MMEIdentifierAssociation,

 -- PDU to MA PDU session-related events, see clause 6.2.3.2.8

 sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

 -- NEF services related events, see clause 7.7.2

 nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

 nEFPDUSessionModification [66] NEFPDUSessionModification,

 nEFPDUSessionRelease [67] NEFPDUSessionRelease,

 nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

 nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

 nEFdeviceTrigger [70] NEFDeviceTrigger,

 nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

 nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

 nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

 nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

 nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

 -- SCEF services related events, see clause 7.8.2

 sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

 sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

 sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

 sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

 sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

 sCEFdeviceTrigger [81] SCEFDeviceTrigger,

 sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

 sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

 sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

 sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

 sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

 -- EPS Events, see clause 6.3

 -- MME Events, see clause 6.3.2.2

 mMEAttach [87] MMEAttach,

 mMEDetach [88] MMEDetach,

 mMELocationUpdate [89] MMELocationUpdate,

 mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

 mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

 -- AKMA key management events, see clause 7.9.1

 aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

 aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

 aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

 aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

 aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

 aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

 aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

 aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

 -- HR LI Events, see clause 7.10.3.3

 n9HRPDUSessionInfo [100] N9HRPDUSessionInfo,

 s8HRBearerInfo [101] S8HRBearerInfo,

 -- Separated Location Reporting, see clause 7.3.4

 separatedLocationReporting [102] SeparatedLocationReporting,

 -- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.2

 sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

 sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

 -- IMS events, see clause 7.11.4.2

 iMSMessage [105] IMSMessage,

 startOfInterceptionForActiveIMSSession [106] StartOfInterceptionForActiveIMSSession,

 iMSCCUnavailable [107] IMSCCUnavailable,

 -- UDM events, see clause 7.2.2

 uDMLocationInformationResult [108] UDMLocationInformationResult,

 uDMUEInformationResponse [109] UDMUEInformationResponse,

 uDMUEAuthenticationResponse [110] UDMUEAuthenticationResponse,

 -- AMF events, see 6.2.2.2.8

 positioningInfoTransfer [111] AMFPositioningInfoTransfer,

 -- MME Events, see clause 6.3.2.2.8

 mMEPositioningInfoTransfer [112] MMEPositioningInfoTransfer,

 -- AMF events, see 6.2.2.2.X

 aMFRANHandoverCommand [1000] AMFRANHandoverCommand,

 aMFRANHandoverRequest [1001] AMFRANHandoverRequest,

 aMFRANHandoverNotify [1002] AMFRANHandoverNofiy

}

-- ==============

-- X3 xCC payload

-- ==============

-- No additional xCC payload definitions required in the present document.

-- ===============

-- HI2 IRI payload

-- ===============

IRIPayload ::= SEQUENCE

{

 iRIPayloadOID [1] RELATIVE-OID,

 event [2] IRIEvent,

 targetIdentifiers [3] SEQUENCE OF IRITargetIdentifier OPTIONAL

}

IRIEvent ::= CHOICE

{

 -- Registration-related events, see clause 6.2.2

 registration [1] AMFRegistration,

 deregistration [2] AMFDeregistration,

 locationUpdate [3] AMFLocationUpdate,

 startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

 unsuccessfulRegistrationProcedure [5] AMFUnsuccessfulProcedure,

 -- PDU session-related events, see clause 6.2.3

 pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

 pDUSessionModification [7] SMFPDUSessionModification,

 pDUSessionRelease [8] SMFPDUSessionRelease,

 startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

 unsuccessfulSessionProcedure [10] SMFUnsuccessfulProcedure,

 -- Subscriber-management related events, see clause 7.2.2

 servingSystemMessage [11] UDMServingSystemMessage,

 -- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

 sMSMessage [12] SMSMessage,

 -- LALS-related events, see clause 7.3.3

 lALSReport [13] LALSReport,

 -- PDHR/PDSR-related events, see clause 6.2.3.4.1

 pDHeaderReport [14] PDHeaderReport,

 pDSummaryReport [15] PDSummaryReport,

 -- MDF-related events, see clause 7.3.2

 mDFCellSiteReport [16] MDFCellSiteReport,

 -- MMS-related events, see clause 7.4.2

 mMSSend [17] MMSSend,

 mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

 mMSNotification [19] MMSNotification,

 mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

 mMSNotificationResponse [21] MMSNotificationResponse,

 mMSRetrieval [22] MMSRetrieval,

 mMSDeliveryAck [23] MMSDeliveryAck,

 mMSForward [24] MMSForward,

 mMSDeleteFromRelay [25] MMSDeleteFromRelay,

 mMSDeliveryReport [26] MMSDeliveryReport,

 mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

 mMSReadReport [28] MMSReadReport,

 mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

 mMSCancel [30] MMSCancel,

 mMSMBoxStore [31] MMSMBoxStore,

 mMSMBoxUpload [32] MMSMBoxUpload,

 mMSMBoxDelete [33] MMSMBoxDelete,

 mMSMBoxViewRequest [34] MMSMBoxViewRequest,

 mMSMBoxViewResponse [35] MMSMBoxViewResponse,

 -- PTC-related events, see clause 7.5.2

 pTCRegistration [36] PTCRegistration,

 pTCSessionInitiation [37] PTCSessionInitiation,

 pTCSessionAbandon [38] PTCSessionAbandon,

 pTCSessionStart [39] PTCSessionStart,

 pTCSessionEnd [40] PTCSessionEnd,

 pTCStartOfInterception [41] PTCStartOfInterception,

 pTCPreEstablishedSession [42] PTCPreEstablishedSession,

 pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

 pTCPartyJoin [44] PTCPartyJoin,

 pTCPartyDrop [45] PTCPartyDrop,

 pTCPartyHold [46] PTCPartyHold,

 pTCMediaModification [47] PTCMediaModification,

 pTCGroupAdvertisement [48] PTCGroupAdvertisement,

 pTCFloorControl [49] PTCFloorControl,

 pTCTargetPresence [50] PTCTargetPresence,

 pTCParticipantPresence [51] PTCParticipantPresence,

 pTCListManagement [52] PTCListManagement,

 pTCAccessPolicy [53] PTCAccessPolicy,

 -- More Subscriber-management related events, see clause 7.2.2

 subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

 cancelLocationMessage [55] UDMCancelLocationMessage,

 -- SMS-related events, continued from choice 12

 sMSReport [56] SMSReport,

 -- MA PDU session-related events, see clause 6.2.3.2.7

 sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

 sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

 sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

 startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

 unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

 -- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

 aMFIdentifierAssociation [62] AMFIdentifierAssociation,

 mMEIdentifierAssociation [63] MMEIdentifierAssociation,

 -- PDU to MA PDU session-related events, see clause 6.2.3.2.8

 sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

 -- NEF services related events, see clause 7.7.2,

 nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

 nEFPDUSessionModification [66] NEFPDUSessionModification,

 nEFPDUSessionRelease [67] NEFPDUSessionRelease,

 nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

 nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

 nEFdeviceTrigger [70] NEFDeviceTrigger,

 nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

 nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

 nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

 nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

 nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

 -- SCEF services related events, see clause 7.8.2

 sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

 sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

 sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

 sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

 sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

 sCEFdeviceTrigger [81] SCEFDeviceTrigger,

 sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

 sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

 sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

 sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

 sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

 -- EPS Events, see clause 6.3

 -- MME Events, see clause 6.3.2.2

 mMEAttach [87] MMEAttach,

 mMEDetach [88] MMEDetach,

 mMELocationUpdate [89] MMELocationUpdate,

 mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

 mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

 -- AKMA key management events, see clause 7.9.1

 aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

 aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

 aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

 aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

 aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

 aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

 aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

 aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

 -- tag 100 is reserved because there is no equivalent n9HRPDUSessionInfo in IRIEvent.

 -- tag 101 is reserved because there is no equivalent S8HRBearerInfo in IRIEvent.

 -- Separated Location Reporting, see clause 7.3.4

 separatedLocationReporting [102] SeparatedLocationReporting,

 -- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.3

 sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

 sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

 -- IMS events, see clause 7.11.4.2

 iMSMessage [105] IMSMessage,

 startOfInterceptionForActiveIMSSession [106] StartOfInterceptionForActiveIMSSession,

 iMSCCUnavailable [107] IMSCCUnavailable,

 -- UDM events, see clause 7.2.2

 uDMLocationInformationResultRecord [108] UDMLocationInformationResult,

 uDMUEInformationResponse [109] UDMUEInformationResponse,

 uDMUEAuthenticationResponse [110] UDMUEAuthenticationResponse,

 -- AMF events, see 6.2.2.2.8

 positioningInfoTransfer [111] AMFPositioningInfoTransfer,

 -- MME Events, see clause 6.3.2.2.8

 mMEPositioningInfoTransfer [112] MMEPositioningInfoTransfer,

 -- AMF events, see 6.2.2.2.X

 aMFRANHandoverCommand [1000] AMFRANHandoverCommand,

 aMFRANHandoverRequest [1001] AMFRANHandoverRequest,

 aMFRANHandoverNotify [1002] AMFRANHandoverNofiy

}

IRITargetIdentifier ::= SEQUENCE

{

 identifier [1] TargetIdentifier,

 provenance [2] TargetIdentifierProvenance OPTIONAL

}

-- ==============

-- HI3 CC payload

-- ==============

CCPayload ::= SEQUENCE

{

 cCPayloadOID [1] RELATIVE-OID,

 pDU [2] CCPDU

}

CCPDU ::= CHOICE

{

 uPFCCPDU [1] UPFCCPDU,

 extendedUPFCCPDU [2] ExtendedUPFCCPDU,

 mMSCCPDU [3] MMSCCPDU,

 nIDDCCPDU [4] NIDDCCPDU,

 pTCCCPDU [5] PTCCCPDU

}

-- ===========================

-- HI4 LI notification payload

-- ===========================

LINotificationPayload ::= SEQUENCE

{

 lINotificationPayloadOID [1] RELATIVE-OID,

 notification [2] LINotificationMessage

}

LINotificationMessage ::= CHOICE

{

 lINotification [1] LINotification

}

-- =================

-- HR LI definitions

-- =================

N9HRPDUSessionInfo ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 pDUSessionID [3] PDUSessionID,

 location [4] Location OPTIONAL,

 sNSSAI [5] SNSSAI OPTIONAL,

 dNN [6] DNN OPTIONAL,

 messageCause [7] N9HRMessageCause

}

S8HRBearerInfo ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 bearerID [3] EPSBearerID,

 linkedBearerID [4] EPSBearerID OPTIONAL,

 location [5] Location OPTIONAL,

 aPN [6] APN OPTIONAL,

 sGWIPAddress [7] IPAddress OPTIONAL,

 messageCause [8] S8HRMessageCause

}

-- ================

-- HR LI parameters

-- ================

N9HRMessageCause ::= ENUMERATED

{

 pDUSessionEstablished(1),

 pDUSessionModified(2),

 pDUSessionReleased(3),

 updatedLocationAvailable(4),

 sMFChanged(5),

 other(6),

 hRLIEnabled(7)

}

S8HRMessageCause ::= ENUMERATED

{

 bearerActivated(1),

 bearerModified(2),

 bearerDeleted(3),

 pDNDisconnected(4),

 updatedLocationAvailable(5),

 sGWChanged(6),

 other(7),

 hRLIEnabled(8)

}

-- ==================

-- 5G NEF definitions

-- ==================

-- See clause 7.7.2.1.2 for details of this structure

NEFPDUSessionEstablishment ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 pDUSessionID [3] PDUSessionID,

 sNSSAI [4] SNSSAI,

 nEFID [5] NEFID,

 dNN [6] DNN,

 rDSSupport [7] RDSSupport,

 sMFID [8] SMFID,

 aFID [9] AFID

}

-- See clause 7.7.2.1.3 for details of this structure

NEFPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 sNSSAI [3] SNSSAI,

 initiator [4] Initiator,

 rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

 rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

 applicationID [7] ApplicationID OPTIONAL,

 aFID [8] AFID OPTIONAL,

 rDSAction [9] RDSAction OPTIONAL,

 serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.7.2.1.4 for details of this structure

NEFPDUSessionRelease ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 pDUSessionID [3] PDUSessionID,

 timeOfFirstPacket [4] Timestamp OPTIONAL,

 timeOfLastPacket [5] Timestamp OPTIONAL,

 uplinkVolume [6] INTEGER OPTIONAL,

 downlinkVolume [7] INTEGER OPTIONAL,

 releaseCause [8] NEFReleaseCause

}

-- See clause 7.7.2.1.5 for details of this structure

NEFUnsuccessfulProcedure ::= SEQUENCE

{

 failureCause [1] NEFFailureCause,

 sUPI [2] SUPI,

 gPSI [3] GPSI OPTIONAL,

 pDUSessionID [4] PDUSessionID,

 dNN [5] DNN OPTIONAL,

 sNSSAI [6] SNSSAI OPTIONAL,

 rDSDestinationPortNumber [7] RDSPortNumber,

 applicationID [8] ApplicationID,

 aFID [9] AFID

}

-- See clause 7.7.2.1.6 for details of this structure

NEFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 pDUSessionID [3] PDUSessionID,

 dNN [4] DNN,

 sNSSAI [5] SNSSAI,

 nEFID [6] NEFID,

 rDSSupport [7] RDSSupport,

 sMFID [8] SMFID,

 aFID [9] AFID

}

-- See clause 7.7.3.1.1 for details of this structure

NEFDeviceTrigger ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 triggerId [3] TriggerID,

 aFID [4] AFID,

 triggerPayload [5] TriggerPayload OPTIONAL,

 validityPeriod [6] INTEGER OPTIONAL,

 priorityDT [7] PriorityDT OPTIONAL,

 sourcePortId [8] PortNumber OPTIONAL,

 destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.2 for details of this structure

NEFDeviceTriggerReplace ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 triggerId [3] TriggerID,

 aFID [4] AFID,

 triggerPayload [5] TriggerPayload OPTIONAL,

 validityPeriod [6] INTEGER OPTIONAL,

 priorityDT [7] PriorityDT OPTIONAL,

 sourcePortId [8] PortNumber OPTIONAL,

 destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.3 for details of this structure

NEFDeviceTriggerCancellation ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 triggerId [3] TriggerID

}

-- See clause 7.7.3.1.4 for details of this structure

NEFDeviceTriggerReportNotify ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 triggerId [3] TriggerID,

 deviceTriggerDeliveryResult [4] DeviceTriggerDeliveryResult

}

-- See clause 7.7.4.1.1 for details of this structure

NEFMSISDNLessMOSMS ::= SEQUENCE

{

 sUPI [1] SUPI,

 gPSI [2] GPSI,

 terminatingSMSParty [3] AFID,

 sMS [4] SMSTPDUData OPTIONAL,

 sourcePort [5] PortNumber OPTIONAL,

 destinationPort [6] PortNumber OPTIONAL

}

-- See clause 7.7.5.1.1 for details of this structure

NEFExpectedUEBehaviourUpdate ::= SEQUENCE

{

 gPSI [1] GPSI,

 expectedUEMovingTrajectory [2] SEQUENCE OF UMTLocationArea5G OPTIONAL,

 stationaryIndication [3] StationaryIndication OPTIONAL,

 communicationDurationTime [4] INTEGER OPTIONAL,

 periodicTime [5] INTEGER OPTIONAL,

 scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

 scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

 batteryIndication [8] BatteryIndication OPTIONAL,

 trafficProfile [9] TrafficProfile OPTIONAL,

 expectedTimeAndDayOfWeekInTrajectory [10] SEQUENCE OF UMTLocationArea5G OPTIONAL,

 aFID [11] AFID,

 validityTime [12] Timestamp OPTIONAL

}

-- ==========================

-- Common SCEF/NEF parameters

-- ==========================

RDSSupport ::= BOOLEAN

RDSPortNumber ::= INTEGER (0..15)

RDSAction ::= ENUMERATED

{

 reservePort(1),

 releasePort(2)

}

SerializationFormat ::= ENUMERATED

{

 xml(1),

 json(2),

 cbor(3)

}

ApplicationID ::= OCTET STRING

NIDDCCPDU ::= OCTET STRING

TriggerID ::= UTF8String

PriorityDT ::= ENUMERATED

{

 noPriority(1),

 priority(2)

}

TriggerPayload ::= OCTET STRING

DeviceTriggerDeliveryResult ::= ENUMERATED

{

 success(1),

 unknown(2),

 failure(3),

 triggered(4),

 expired(5),

 unconfirmed(6),

 replaced(7),

 terminate(8)

}

StationaryIndication ::= ENUMERATED

{

 stationary(1),

 mobile(2)

}

BatteryIndication ::= ENUMERATED

{

 batteryRecharge(1),

 batteryReplace(2),

 batteryNoRecharge(3),

 batteryNoReplace(4),

 noBattery(5)

}

ScheduledCommunicationTime ::= SEQUENCE

{

 days [1] SEQUENCE OF Daytime

}

UMTLocationArea5G ::= SEQUENCE

{

 timeOfDay [1] Daytime,

 durationSec [2] INTEGER,

 location [3] NRLocation

}

Daytime ::= SEQUENCE

{

 daysOfWeek [1] Day OPTIONAL,

 timeOfDayStart [2] Timestamp OPTIONAL,

 timeOfDayEnd [3] Timestamp OPTIONAL

}

Day ::= ENUMERATED

{

 monday(1),

 tuesday(2),

 wednesday(3),

 thursday(4),

 friday(5),

 saturday(6),

 sunday(7)

}

TrafficProfile ::= ENUMERATED

{

 singleTransUL(1),

 singleTransDL(2),

 dualTransULFirst(3),

 dualTransDLFirst(4),

 multiTrans(5)

}

ScheduledCommunicationType ::= ENUMERATED

{

 downlinkOnly(1),

 uplinkOnly(2),

 bidirectional(3)

}

-- =================

-- 5G NEF parameters

-- =================

NEFFailureCause ::= ENUMERATED

{

 userUnknown(1),

 niddConfigurationNotAvailable(2),

 contextNotFound(3),

 portNotFree(4),

 portNotAssociatedWithSpecifiedApplication(5)

}

NEFReleaseCause ::= ENUMERATED

{

 sMFRelease(1),

 dNRelease(2),

 uDMRelease(3),

 cHFRelease(4),

 localConfigurationPolicy(5),

 unknownCause(6)

}

AFID ::= UTF8String

NEFID ::= UTF8String

-- ==================

-- SCEF definitions

-- ==================

-- See clause 7.8.2.1.2 for details of this structure

SCEFPDNConnectionEstablishment ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 iMEI [4] IMEI OPTIONAL,

 ePSBearerID [5] EPSBearerID,

 sCEFID [6] SCEFID,

 aPN [7] APN,

 rDSSupport [8] RDSSupport,

 sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.3 for details of this structure

SCEFPDNConnectionUpdate ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 initiator [4] Initiator,

 rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

 rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

 applicationID [7] ApplicationID OPTIONAL,

 sCSASID [8] SCSASID OPTIONAL,

 rDSAction [9] RDSAction OPTIONAL,

 serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.8.2.1.4 for details of this structure

SCEFPDNConnectionRelease ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 ePSBearerID [4] EPSBearerID,

 timeOfFirstPacket [5] Timestamp OPTIONAL,

 timeOfLastPacket [6] Timestamp OPTIONAL,

 uplinkVolume [7] INTEGER OPTIONAL,

 downlinkVolume [8] INTEGER OPTIONAL,

 releaseCause [9] SCEFReleaseCause

}

-- See clause 7.8.2.1.5 for details of this structure

SCEFUnsuccessfulProcedure ::= SEQUENCE

{

 failureCause [1] SCEFFailureCause,

 iMSI [2] IMSI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 externalIdentifier [4] NAI OPTIONAL,

 ePSBearerID [5] EPSBearerID,

 aPN [6] APN,

 rDSDestinationPortNumber [7] RDSPortNumber OPTIONAL,

 applicationID [8] ApplicationID OPTIONAL,

 sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.6 for details of this structure

SCEFStartOfInterceptionWithEstablishedPDNConnection ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 iMEI [4] IMEI OPTIONAL,

 ePSBearerID [5] EPSBearerID,

 sCEFID [6] SCEFID,

 aPN [7] APN,

 rDSSupport [8] RDSSupport,

 sCSASID [9] SCSASID

}

-- See clause 7.8.3.1.1 for details of this structure

SCEFDeviceTrigger ::= SEQUENCE

{

 iMSI [1] IMSI,

 mSISDN [2] MSISDN,

 externalIdentifier [3] NAI,

 triggerId [4] TriggerID,

 sCSASID [5] SCSASID OPTIONAL,

 triggerPayload [6] TriggerPayload OPTIONAL,

 validityPeriod [7] INTEGER OPTIONAL,

 priorityDT [8] PriorityDT OPTIONAL,

 sourcePortId [9] PortNumber OPTIONAL,

 destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.2 for details of this structure

SCEFDeviceTriggerReplace ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 triggerId [4] TriggerID,

 sCSASID [5] SCSASID OPTIONAL,

 triggerPayload [6] TriggerPayload OPTIONAL,

 validityPeriod [7] INTEGER OPTIONAL,

 priorityDT [8] PriorityDT OPTIONAL,

 sourcePortId [9] PortNumber OPTIONAL,

 destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.3 for details of this structure

SCEFDeviceTriggerCancellation ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 triggerId [4] TriggerID

}

-- See clause 7.8.3.1.4 for details of this structure

SCEFDeviceTriggerReportNotify ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifier [3] NAI OPTIONAL,

 triggerId [4] TriggerID,

 deviceTriggerDeliveryResult [5] DeviceTriggerDeliveryResult

}

-- See clause 7.8.4.1.1 for details of this structure

SCEFMSISDNLessMOSMS ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 externalIdentifie [3] NAI OPTIONAL,

 terminatingSMSParty [4] SCSASID,

 sMS [5] SMSTPDUData OPTIONAL,

 sourcePort [6] PortNumber OPTIONAL,

 destinationPort [7] PortNumber OPTIONAL

}

-- See clause 7.8.5.1.1 for details of this structure

SCEFCommunicationPatternUpdate ::= SEQUENCE

{

 mSISDN [1] MSISDN OPTIONAL,

 externalIdentifier [2] NAI OPTIONAL,

 periodicCommunicationIndicator [3] PeriodicCommunicationIndicator OPTIONAL,

 communicationDurationTime [4] INTEGER OPTIONAL,

 periodicTime [5] INTEGER OPTIONAL,

 scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

 scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

 stationaryIndication [8] StationaryIndication OPTIONAL,

 batteryIndication [9] BatteryIndication OPTIONAL,

 trafficProfile [10] TrafficProfile OPTIONAL,

 expectedUEMovingTrajectory [11] SEQUENCE OF UMTLocationArea5G OPTIONAL,

 sCSASID [13] SCSASID,

 validityTime [14] Timestamp OPTIONAL

}

-- =================

-- SCEF parameters

-- =================

SCEFFailureCause ::= ENUMERATED

{

 userUnknown(1),

 niddConfigurationNotAvailable(2),

 invalidEPSBearer(3),

 operationNotAllowed(4),

 portNotFree(5),

 portNotAssociatedWithSpecifiedApplication(6)

}

SCEFReleaseCause ::= ENUMERATED

{

 mMERelease(1),

 dNRelease(2),

 hSSRelease(3),

 localConfigurationPolicy(4),

 unknownCause(5)

}

SCSASID ::= UTF8String

SCEFID ::= UTF8String

PeriodicCommunicationIndicator ::= ENUMERATED

{

 periodic(1),

 nonPeriodic(2)

}

EPSBearerID ::= INTEGER (0..255)

APN ::= UTF8String

-- =======================

-- AKMA AAnF definitions

-- =======================

AAnFAnchorKeyRegister ::= SEQUENCE

{

 aKID [1] NAI,

 sUPI [2] SUPI,

 kAKMA [3] KAKMA OPTIONAL

}

AAnFKAKMAApplicationKeyGet ::= SEQUENCE

{

 type [1] KeyGetType,

 aKID [2] NAI,

 keyInfo [3] AFKeyInfo

}

AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial ::= SEQUENCE

{

 aKID [1] NAI,

 kAKMA [2] KAKMA OPTIONAL,

 aFKeyList [3] SEQUENCE OF AFKeyInfo OPTIONAL

}

AAnFAKMAContextRemovalRecord ::= SEQUENCE

{

 aKID [1] NAI,

 nFID [2] NFID

}

-- ======================

-- AKMA common parameters

-- ======================

FQDN ::= UTF8String

NFID ::= UTF8String

UAProtocolID ::= OCTET STRING (SIZE(5))

AKMAAFID ::= SEQUENCE

{

 aFFQDN [1] FQDN,

 uaProtocolID [2] UAProtocolID

}

UAStarParams ::= CHOICE

{

 tls12 [1] TLS12UAStarParams,

 generic [2] GenericUAStarParams

}

GenericUAStarParams ::= SEQUENCE

{

 genericClientParams [1] OCTET STRING,

 genericServerParams [2] OCTET STRING

}

-- ===========================================

-- Specific UaStarParmas for TLS 1.2 (RFC5246)

-- ===========================================

TLSCipherType ::= ENUMERATED

{

 stream(1),

 block(2),

 aead(3)

}

TLSCompressionAlgorithm ::= ENUMERATED

{

 null(1),

 deflate(2)

}

TLSPRFAlgorithm ::= ENUMERATED

{

 rfc5246(1)

}

TLSCipherSuite ::= SEQUENCE (SIZE(2)) OF INTEGER (0..255)

TLS12UAStarParams ::= SEQUENCE

{

 preMasterSecret [1] OCTET STRING (SIZE(6)) OPTIONAL,

 masterSecret [2] OCTET STRING (SIZE(6)),

 pRFAlgorithm [3] TLSPRFAlgorithm,

 cipherSuite [4] TLSCipherSuite,

 cipherType [5] TLSCipherType,

 encKeyLength [6] INTEGER (0..255),

 blockLength [7] INTEGER (0..255),

 fixedIVLength [8] INTEGER (0..255),

 recordIVLength [9] INTEGER (0..255),

 macLength [10] INTEGER (0..255),

 macKeyLength [11] INTEGER (0..255),

 compressionAlgorithm [12] TLSCompressionAlgorithm,

 clientRandom [13] OCTET STRING (SIZE(4)),

 serverRandom [14] OCTET STRING (SIZE(4)),

 clientSequenceNumber [15] INTEGER,

 serverSequenceNumber [16] INTEGER,

 sessionID [17] OCTET STRING (SIZE(0..32)),

 tLSExtensions [18] OCTET STRING (SIZE(0..65535))

}

KAF ::= OCTET STRING

KAKMA ::= OCTET STRING

-- ====================

-- AKMA AAnF parameters

-- ====================

KeyGetType ::= ENUMERATED

{

 internal(1),

 external(2)

}

AFKeyInfo ::= SEQUENCE

{

 aFID [1] AKMAAFID,

 kAF [2] KAF,

 kAFExpTime [3] KAFExpiryTime

}

-- =======================

-- AKMA AF definitions

-- =======================

AFAKMAApplicationKeyRefresh ::= SEQUENCE

{

 aFID [1] AFID,

 aKID [2] NAI,

 kAF [3] KAF,

 uaStarParams [4] UAStarParams OPTIONAL

}

AFStartOfInterceptWithEstablishedAKMAApplicationKey ::= SEQUENCE

{

 aFID [1] FQDN,

 aKID [2] NAI,

 kAFParamList [3] SEQUENCE OF AFSecurityParams

}

AFAuxiliarySecurityParameterEstablishment ::= SEQUENCE

{

 aFSecurityParams [1] AFSecurityParams

}

AFSecurityParams ::= SEQUENCE

{

 aFID [1] AFID,

 aKID [2] NAI,

 kAF [3] KAF,

 uaStarParams [4] UAStarParams

}

AFApplicationKeyRemoval ::= SEQUENCE

{

 aFID [1] AFID,

 aKID [2] NAI,

 removalCause [3] AFKeyRemovalCause

}

-- ===================

-- AKMA AF parameters

-- ===================

KAFParams ::= SEQUENCE

{

 aKID [1] NAI,

 kAF [2] KAF,

 kAFExpTime [3] KAFExpiryTime,

 uaStarParams [4] UAStarParams

}

KAFExpiryTime ::= GeneralizedTime

AFKeyRemovalCause ::= ENUMERATED

{

 unknown(1),

 keyExpiry(2),

 applicationSpecific(3)

}

-- ==================

-- 5G AMF definitions

-- ==================

-- See clause 6.2.2.2.2 for details of this structure

AMFRegistration ::= SEQUENCE

{

 registrationType [1] AMFRegistrationType,

 registrationResult [2] AMFRegistrationResult,

 slice [3] Slice OPTIONAL,

 sUPI [4] SUPI,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI,

 location [9] Location OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 fiveGSTAIList [11] TAIList OPTIONAL,

 sMSOverNasIndicator [12] SMSOverNASIndicator OPTIONAL,

 oldGUTI [13] EPS5GGUTI OPTIONAL,

 eMM5GRegStatus [14] EMM5GMMStatus OPTIONAL,

 nonIMEISVPEI [15] NonIMEISVPEI OPTIONAL,

 mACRestIndicator [16] MACRestrictionIndicator OPTIONAL

}

-- See clause 6.2.2.2.3 for details of this structure

AMFDeregistration ::= SEQUENCE

{

 deregistrationDirection [1] AMFDirection,

 accessType [2] AccessType,

 sUPI [3] SUPI OPTIONAL,

 sUCI [4] SUCI OPTIONAL,

 pEI [5] PEI OPTIONAL,

 gPSI [6] GPSI OPTIONAL,

 gUTI [7] FiveGGUTI OPTIONAL,

 cause [8] FiveGMMCause OPTIONAL,

 location [9] Location OPTIONAL,

 switchOffIndicator [10] SwitchOffIndicator OPTIONAL,

 reRegRequiredIndicator [11] ReRegRequiredIndicator OPTIONAL

}

-- See clause 6.2.2.2.4 for details of this structure

AMFLocationUpdate ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI OPTIONAL,

 location [6] Location,

 sMSOverNASIndicator [7] SMSOverNASIndicator OPTIONAL,

 oldGUTI [8] EPS5GGUTI OPTIONAL

}

-- See clause 6.2.2.2.5 for details of this structure

AMFStartOfInterceptionWithRegisteredUE ::= SEQUENCE

{

 registrationResult [1] AMFRegistrationResult,

 registrationType [2] AMFRegistrationType OPTIONAL,

 slice [3] Slice OPTIONAL,

 sUPI [4] SUPI,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI,

 location [9] Location OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 timeOfRegistration [11] Timestamp OPTIONAL,

 fiveGSTAIList [12] TAIList OPTIONAL,

 sMSOverNASIndicator [13] SMSOverNASIndicator OPTIONAL,

 oldGUTI [14] EPS5GGUTI OPTIONAL,

 eMM5GRegStatus [15] EMM5GMMStatus OPTIONAL

}

-- See clause 6.2.2.2.6 for details of this structure

AMFUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] AMFFailedProcedureType,

 failureCause [2] AMFFailureCause,

 requestedSlice [3] NSSAI OPTIONAL,

 sUPI [4] SUPI OPTIONAL,

 sUCI [5] SUCI OPTIONAL,

 pEI [6] PEI OPTIONAL,

 gPSI [7] GPSI OPTIONAL,

 gUTI [8] FiveGGUTI OPTIONAL,

 location [9] Location OPTIONAL

}

-- See clause 6.2.2.2.8 on for details of this structure

AMFPositioningInfoTransfer ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI OPTIONAL,

 nRPPaMessage [6] OCTET STRING OPTIONAL,

 lPPMessage [7] OCTET STRING OPTIONAL,

 lcsCorrelationId [8] UTF8String (SIZE(1..255))

}

-- See clause 6.2.2.2.X.2 for details of this structure

AMFRANHandoverCommand ::= SEQUENCE

{

 userIdentifiers [1] UserIdentifiers,

 aMFMessageType [2] AMFMessageType,

 aMFUENGAPID [3] AMFUENGAPID,

 rANUENGAPID [4] RANUENGAPID,

 handoverType [5] HandoverType,

 nASSecurityParameters [6] OCTET STRING OPTIONAL,

 targetToSourceContainer [7] RANTargetToSourceContainer,

}

-- See clause 6.2.2.2.X.3 for details of this structure

AMFRANHandoverRequest ::= SEQUENCE

{

 userIdentifiers [1] UserIdentifiers,

 aMFmessageType [2] AMFMessageType,

 aMFUENGAPID [3] AMFUENGAPID,

 rANUENGAPID [4] RANUENGAPID,

 handoverType [5] HandoverType,

 handoverCause [6] HandoverCause,

 uEAMBR [7] BitRate,

 uESecurityCapabilities [8] UESecurityCapabilities OPTIONAL,

 securityContext [9] SecurityContext,

 pDUSessionResouceInformation [10] PDUSessionResourceInformation,

 allowedNSSAI [11] AllowedNSSAI,

 aMFTraceActivation [12] AMFTraceActivation OPTIONAL,

 rANsourceToTargetContainer [13] RANSourceToTargetContainer,

 mobilityRestrictionList [14] MobilityRestrictionList OPTIONAL,

 locationReportingRequestType [15] LocationReportingRequestType,

 gUAMI [16] GUAMI,

 voiceEPSFallback [17] VoiceEPSFallback OPTIONAL,

 sRVCCOperation [18] SRVCCOperation OPTIONAL,

 iABAuthorizedIndicator [19] IABAuthorizedIndicator OPTIONAL,

 nRV2XAuthorizedIndicator [20] NRV2XAuthorizedIndicator OPTIONAL,

 lTEV2XAuthorizedIndicator [21] LTEV2XAuthorizedIndicator OPTIONAL,

 nRSidelinkAMBR [22] BitRate OPTIONAL,

 lTEUESidelinkAMBR [23] BitRate OPTIONAL,

 pC5QoSParameters [24] PC5QoSParameters OPTIONAL,

 mDTPLMNList [25] PLMNList OPTIONAL,

 uERadioCapability [26] UERadioCapability OPTIONAL,

 aMFHandoverRequestACKTransferInfo [27] AMFHandoverRequestACKTransferInfo OPTIONAL,

 targetToSourceContainer [28] RANTargetToSourceContainer,

 criticality [29] AMFProcedureCriticality OPTIONAL,

 nPNAccessInformation [30] NPNAccessInformation OPTIONAL,

 rEDCAPIndication [31] REDCAPIndication OPTIONAL

}

-- See clause 6.2.2.2.X.4 for details of this structure

AMFRANHandoverNotify ::= SEQUENCE

{

 userIdentifiers [1] UserIdentifiers,

 aMFMessageType [2] AMFMessageType,

 aMFUENGAPID [4] AMFUENGAPID,

 rANUENGAPID [5] RANUENGAPID,

 location [6] Location

}

-- =================

-- 5G AMF parameters

-- =================

AMFID ::= SEQUENCE

{

 aMFRegionID [1] AMFRegionID,

 aMFSetID [2] AMFSetID,

 aMFPointer [3] AMFPointer

}

AMFDirection ::= ENUMERATED

{

 networkInitiated(1),

 uEInitiated(2)

}

AMFFailedProcedureType ::= ENUMERATED

{

 registration(1),

 sMS(2),

 pDUSessionEstablishment(3)

}

AMFFailureCause ::= CHOICE

{

 fiveGMMCause [1] FiveGMMCause,

 fiveGSMCause [2] FiveGSMCause

}

-- see Clause 9.3.4.11 of TS 38.413[23] for details

AMFHandoverRequestACKTransferInfo ::= OCTET STRING

AMFHandoverRequestAcknowledge ::= SEQUENCE

{

 messageType [1] AMFMessageType,

 aMFUENGAPID [2] AMFUENGAPID,

 rANUENGAPID [3] RANUENGAPID,

 pDUSessionID [4] PDUSessionID,

 handoverRequestACKTransferInfo [5] AMFHandoverReqACKTransInfo,

 targetToSourceContainer [6] RANTargetToSourceContainer,

 criticality [7] AMFProcedureCriticality OPTIONAL,

 nPNAccessInformation [8] NPNAccessInformation OPTIONAL,

 rEDCAPIndication [9] REDCAPIndication OPTIONAL

}

AMFHandoverRequestAcknowledge ::= OCTET STRING

AMFIECriticality ::= ENUMERATED

{

 reject(1),

 ignore(2),

 notify(3)

}

AMFIEIdentifier ::= INTEGER (0..65535)

AMFMessageType ::= SEQUENCE

{

 aMFprocedureCode [1] AMFProcedureCode,

 typeOfMessage [2] TypeOfMessage

}

AMFPointer ::= INTEGER (0..63)

AMFProcedureCode ::= INTEGER (0..255)

AMFProcedureCriticality ::= SEQUENCE

{

 aMFIECriticality [1] AMFIECriticality,

 aMFIEIdentifier [2] AMFIEIdentifier,

 typeOfError [3] TypeOfError

}

AMFRegistrationResult ::= ENUMERATED

{

 threeGPPAccess(1),

 nonThreeGPPAccess(2),

 threeGPPAndNonThreeGPPAccess(3)

}

AMFRegionID ::= INTEGER (0..255)

AMFRegistrationType ::= ENUMERATED

{

 initial(1),

 mobility(2),

 periodic(3),

 emergency(4)

}

AMFSetID ::= INTEGER (0..1023)

AMFTraceActivation ::= SEQUENCE

{

 nGRANTraceID [1] NGRANTraceID,

 interfacesToTrace [2] InterfacesToTrace,

 aMFtraceDepth [3] AMFTraceDepth,

 traceCollectionEntityIPAddress [4] IPAddress

}

AMFTraceDepth ::= ENUMERATED

{

 minimum(1),

 medium(2),

 maximum(3),

 minimumWithoutVendorSpecificExtension(4),

 mediumWithoutVendorSpecificExtension(5),

 maximumWithoutVendorSpecificExtension(6)

}

AMFUENGAPID ::= INTEGER (0..1099511627775)

InterfacesToTrace ::= BIT STRING (SIZE(8))

-- see Clause 5.6 of TS 32.422 for details of this structure

NGRANTraceID ::= OCTET STRING (SIZE(8))

-- ==================

-- 5G SMF definitions

-- ==================

-- See clause 6.2.3.2.2 for details of this structure

SMFPDUSessionEstablishment ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 gTPTunnelID [6] FTEID,

 pDUSessionType [7] PDUSessionType,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 location [11] Location OPTIONAL,

 dNN [12] DNN,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 uEEPSPDNConnection [19] UEEPSPDNConnection OPTIONAL,

 ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.3 for details of this structure

SMFPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 sNSSAI [5] SNSSAI OPTIONAL,

 non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

 location [7] Location OPTIONAL,

 requestType [8] FiveGSMRequestType,

 accessType [9] AccessType OPTIONAL,

 rATType [10] RATType OPTIONAL,

 pDUSessionID [11] PDUSessionID OPTIONAL,

 ePS5GSComboInfo [12] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.4 for details of this structure

SMFPDUSessionRelease ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 pDUSessionID [4] PDUSessionID,

 timeOfFirstPacket [5] Timestamp OPTIONAL,

 timeOfLastPacket [6] Timestamp OPTIONAL,

 uplinkVolume [7] INTEGER OPTIONAL,

 downlinkVolume [8] INTEGER OPTIONAL,

 location [9] Location OPTIONAL,

 cause [10] SMFErrorCodes OPTIONAL,

 ePS5GSComboInfo [11] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.5 for details of this structure

SMFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 gTPTunnelID [6] FTEID,

 pDUSessionType [7] PDUSessionType,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress,

 non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

 location [11] Location OPTIONAL,

 dNN [12] DNN,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 timeOfSessionEstablishment [19] Timestamp OPTIONAL,

 ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.6 for details of this structure

SMFUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] SMFFailedProcedureType,

 failureCause [2] FiveGSMCause,

 initiator [3] Initiator,

 requestedSlice [4] NSSAI OPTIONAL,

 sUPI [5] SUPI OPTIONAL,

 sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [7] PEI OPTIONAL,

 gPSI [8] GPSI OPTIONAL,

 pDUSessionID [9] PDUSessionID OPTIONAL,

 uEEndpoint [10] SEQUENCE OF UEEndpointAddress OPTIONAL,

 non3GPPAccessEndpoint [11] UEEndpointAddress OPTIONAL,

 dNN [12] DNN OPTIONAL,

 aMFID [13] AMFID OPTIONAL,

 hSMFURI [14] HSMFURI OPTIONAL,

 requestType [15] FiveGSMRequestType OPTIONAL,

 accessType [16] AccessType OPTIONAL,

 rATType [17] RATType OPTIONAL,

 sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

 location [19] Location OPTIONAL

}

-- See clause 6.2.3.2.8 for details of this structure

SMFPDUtoMAPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 sNSSAI [5] SNSSAI OPTIONAL,

 non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

 location [7] Location OPTIONAL,

 requestType [8] FiveGSMRequestType,

 accessType [9] AccessType OPTIONAL,

 rATType [10] RATType OPTIONAL,

 pDUSessionID [11] PDUSessionID,

 requestIndication [12] RequestIndication,

 aTSSSContainer [13] ATSSSContainer

}

-- See clause 6.2.3.2.7.1 for details of this structure

SMFMAPDUSessionEstablishment ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 pDUSessionType [6] PDUSessionType,

 accessInfo [7] SEQUENCE OF AccessInfo,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [10] Location OPTIONAL,

 dNN [11] DNN,

 aMFID [12] AMFID OPTIONAL,

 hSMFURI [13] HSMFURI OPTIONAL,

 requestType [14] FiveGSMRequestType,

 sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

 servingNetwork [16] SMFServingNetwork,

 oldPDUSessionID [17] PDUSessionID OPTIONAL,

 mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [20] SMFMAAcceptedIndication,

 aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.2 for details of this structure

SMFMAPDUSessionModification ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 accessInfo [6] SEQUENCE OF AccessInfo OPTIONAL,

 sNSSAI [7] SNSSAI OPTIONAL,

 location [8] Location OPTIONAL,

 requestType [9] FiveGSMRequestType OPTIONAL,

 servingNetwork [10] SMFServingNetwork,

 oldPDUSessionID [11] PDUSessionID OPTIONAL,

 mAUpgradeIndication [12] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [13] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [14] SMFMAAcceptedIndication,

 aTSSSContainer [15] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.3 for details of this structure

SMFMAPDUSessionRelease ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 pDUSessionID [4] PDUSessionID,

 timeOfFirstPacket [5] Timestamp OPTIONAL,

 timeOfLastPacket [6] Timestamp OPTIONAL,

 uplinkVolume [7] INTEGER OPTIONAL,

 downlinkVolume [8] INTEGER OPTIONAL,

 location [9] Location OPTIONAL,

 cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.7.4 for details of this structure

SMFStartOfInterceptionWithEstablishedMAPDUSession ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 pDUSessionID [5] PDUSessionID,

 pDUSessionType [6] PDUSessionType,

 accessInfo [7] SEQUENCE OF AccessInfo,

 sNSSAI [8] SNSSAI OPTIONAL,

 uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [10] Location OPTIONAL,

 dNN [11] DNN,

 aMFID [12] AMFID OPTIONAL,

 hSMFURI [13] HSMFURI OPTIONAL,

 requestType [14] FiveGSMRequestType OPTIONAL,

 sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

 servingNetwork [16] SMFServingNetwork,

 oldPDUSessionID [17] PDUSessionID OPTIONAL,

 mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

 ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

 mAAcceptedIndication [20] SMFMAAcceptedIndication,

 aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.5 for details of this structure

SMFMAUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] SMFFailedProcedureType,

 failureCause [2] FiveGSMCause,

 requestedSlice [3] NSSAI OPTIONAL,

 initiator [4] Initiator,

 sUPI [5] SUPI OPTIONAL,

 sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

 pEI [7] PEI OPTIONAL,

 gPSI [8] GPSI OPTIONAL,

 pDUSessionID [9] PDUSessionID OPTIONAL,

 accessInfo [10] SEQUENCE OF AccessInfo,

 uEEndpoint [11] SEQUENCE OF UEEndpointAddress OPTIONAL,

 location [12] Location OPTIONAL,

 dNN [13] DNN OPTIONAL,

 aMFID [14] AMFID OPTIONAL,

 hSMFURI [15] HSMFURI OPTIONAL,

 requestType [16] FiveGSMRequestType OPTIONAL,

 sMPDUDNRequest [17] SMPDUDNRequest OPTIONAL

}

-- =================

-- 5G SMF parameters

-- =================

SMFID ::= UTF8String

SMFFailedProcedureType ::= ENUMERATED

{

 pDUSessionEstablishment(1),

 pDUSessionModification(2),

 pDUSessionRelease(3)

}

SMFServingNetwork ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 nID [2] NID OPTIONAL

}

AccessInfo ::= SEQUENCE

{

 accessType [1] AccessType,

 rATType [2] RATType OPTIONAL,

 gTPTunnelID [3] FTEID,

 non3GPPAccessEndpoint [4] UEEndpointAddress OPTIONAL,

 establishmentStatus [5] EstablishmentStatus,

 aNTypeToReactivate [6] AccessType OPTIONAL

}

-- see Clause 6.1.2 of TS 24.193[44] for the details of the ATSSS container contents.

ATSSSContainer ::= OCTET STRING

EstablishmentStatus ::= ENUMERATED

{

 established(0),

 released(1)

}

SMFMAUpgradeIndication ::= BOOLEAN

-- Given in YAML encoding as defined in clause 6.1.6.2.31 of TS 29.502[16]

SMFEPSPDNCnxInfo ::= UTF8String

SMFMAAcceptedIndication ::= BOOLEAN

-- see Clause 6.1.6.3.8 of TS 29.502[16] for the details of this structure.

SMFErrorCodes ::= UTF8String

-- see Clause 6.1.6.3.2 of TS 29.502[16] for details of this structure.

UEEPSPDNConnection ::= OCTET STRING

-- see Clause 6.1.6.3.6 of TS 29.502[16] for the details of this structure.

RequestIndication ::= ENUMERATED

{

 uEREQPDUSESMOD(0),

 uEREQPDUSESREL(1),

 pDUSESMOB(2),

 nWREQPDUSESAUTH(3),

 nWREQPDUSESMOD(4),

 nWREQPDUSESREL(5),

 eBIASSIGNMENTREQ(6),

 rELDUETO5GANREQUEST(7)

}

-- ======================

-- PGW-C + SMF Parameters

-- ======================

EPS5GSComboInfo ::= SEQUENCE

{

 ePSInterworkingIndication [1] EPSInterworkingIndication,

 ePSSubscriberIDs [2] EPSSubscriberIDs,

 ePSPDNCnxInfo [3] EPSPDNCnxInfo OPTIONAL,

 ePSBearerInfo [4] EPSBearerInfo OPTIONAL

}

EPSInterworkingIndication ::= ENUMERATED

{

 none(1),

 withN26(2),

 withoutN26(3),

 iwkNon3GPP(4)

}

EPSSubscriberIDs ::= SEQUENCE

{

 iMSI [1] IMSI OPTIONAL,

 mSISDN [2] MSISDN OPTIONAL,

 iMEI [3] IMEI OPTIONAL

}

EPSPDNCnxInfo ::= SEQUENCE

{

 pGWS8ControlPlaneFTEID [1] FTEID,

 linkedBearerID [2] EPSBearerID OPTIONAL

}

EPSBearerInfo ::= SEQUENCE OF EPSBearers

EPSBearers ::= SEQUENCE

{

 ePSBearerID [1] EPSBearerID,

 pGWS8UserPlaneFTEID [2] FTEID,

 qCI [3] QCI

}

QCI ::= INTEGER (0..255)

-- ==================

-- 5G UPF definitions

-- ==================

UPFCCPDU ::= OCTET STRING

-- See clause 6.2.3.8 for the details of this structure

ExtendedUPFCCPDU ::= SEQUENCE

{

 payload [1] UPFCCPDUPayload,

 qFI [2] QFI OPTIONAL

}

-- =================

-- 5G UPF parameters

-- =================

UPFCCPDUPayload ::= CHOICE

{

 uPFIPCC [1] OCTET STRING,

 uPFEthernetCC [2] OCTET STRING,

 uPFUnstructuredCC [3] OCTET STRING

}

QFI ::= INTEGER (0..63)

-- ==================

-- 5G UDM definitions

-- ==================

UDMServingSystemMessage ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 gUAMI [4] GUAMI OPTIONAL,

 gUMMEI [5] GUMMEI OPTIONAL,

 pLMNID [6] PLMNID OPTIONAL,

 servingSystemMethod [7] UDMServingSystemMethod,

 serviceID [8] ServiceID OPTIONAL

}

UDMSubscriberRecordChangeMessage ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 oldPEI [4] PEI OPTIONAL,

 oldSUPI [5] SUPI OPTIONAL,

 oldGPSI [6] GPSI OPTIONAL,

 oldserviceID [7] ServiceID OPTIONAL,

 subscriberRecordChangeMethod [8] UDMSubscriberRecordChangeMethod,

 serviceID [9] ServiceID OPTIONAL

}

UDMCancelLocationMessage ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 gUAMI [4] GUAMI OPTIONAL,

 pLMNID [5] PLMNID OPTIONAL,

 cancelLocationMethod [6] UDMCancelLocationMethod

}

UDMLocationInformationResult ::= SEQUENCE

{

 sUPI [1] SUPI,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 locationInfoRequest [4] UDMLocationInfoRequest,

 vPLMNID [5] PLMNID OPTIONAL,

 currentLocationIndicator [6] BOOLEAN OPTIONAL,

 aMFInstanceID [7] NFID OPTIONAL,

 sMSFInstanceID [8] NFID OPTIONAL,

 location [9] Location OPTIONAL,

 rATType [10] RATType OPTIONAL,

 problemDetails [11] UDMProblemDetails OPTIONAL

}

UDMUEInformationResponse ::= SEQUENCE

{

 sUPI [1] SUPI,

 tADSInfo [2] UEContextInfo OPTIONAL,

 fiveGSUserStateInfo [3] FiveGSUserStateInfo OPTIONAL,

 fiveGSRVCCInfo [4] FiveGSRVCCInfo OPTIONAL,

 problemDetails [5] UDMProblemDetails OPTIONAL

}

UDMUEAuthenticationResponse ::= SEQUENCE

{

 sUPI [1] SUPI,

 authenticationInfoRequest [2] UDMAuthenticationInfoRequest,

 aKMAIndicator [3] BOOLEAN OPTIONAL,

 problemDetails [4] UDMProblemDetails OPTIONAL

}

-- =================

-- 5G UDM parameters

-- =================

UDMServingSystemMethod ::= ENUMERATED

{

 amf3GPPAccessRegistration(0),

 amfNon3GPPAccessRegistration(1),

 unknown(2)

}

UDMSubscriberRecordChangeMethod ::= ENUMERATED

{

 pEIChange(1),

 sUPIChange(2),

 gPSIChange(3),

 uEDeprovisioning(4),

 unknown(5),

 serviceIDChange(6)

}

UDMCancelLocationMethod ::= ENUMERATED

{

 aMF3GPPAccessDeregistration(1),

 aMFNon3GPPAccessDeregistration(2),

 uDMDeregistration(3),

 unknown(4)

}

ServiceID ::= SEQUENCE

{

 nSSAI [1] NSSAI OPTIONAL,

 cAGID [2] SEQUENCE OF CAGID OPTIONAL

}

CAGID ::= UTF8String

UDMAuthenticationInfoRequest ::= SEQUENCE

{

 infoRequestType [1] UDMInfoRequestType,

 rGAuthCtx [2] SEQUENCE SIZE(1..MAX) OF SubscriberIdentifier,

 authType [3] PrimaryAuthenticationType,

 servingNetworkName [4] PLMNID,

 aUSFInstanceID [5] NFID OPTIONAL,

 cellCAGInfo [6] CAGID OPTIONAL,

 n5GCIndicator [7] BOOLEAN OPTIONAL

}

UDMLocationInfoRequest ::= SEQUENCE

{

 requested5GSLocation [1] BOOLEAN OPTIONAL,

 requestedCurrentLocation [2] BOOLEAN OPTIONAL,

 requestedRATType [3] BOOLEAN OPTIONAL,

 requestedTimeZone [4] BOOLEAN OPTIONAL,

 requestedServingNode [5] BOOLEAN OPTIONAL

}

UDMProblemDetails ::= SEQUENCE

{

 cause [1] UDMProblemDetailsCause OPTIONAL

}

UDMProblemDetailsCause ::= CHOICE

{

 uDMDefinedCause [1] UDMDefinedCause,

 otherCause [2] UDMProblemDetailsOtherCause

}

UDMDefinedCause ::= ENUMERATED

{

 userNotFound(1),

 dataNotFound(2),

 contextNotFound(3),

 subscriptionNotFound(4),

 other(5)

}

UDMInfoRequestType ::= ENUMERATED

{

 hSS(1),

 aUSF(2),

 other(3)

}

UDMProblemDetailsOtherCause ::= SEQUENCE

{

 problemDetailsType [1] UTF8String OPTIONAL,

 title [2] UTF8String OPTIONAL,

 status [3] INTEGER OPTIONAL,

 detail [4] UTF8String OPTIONAL,

 instance [5] UTF8String OPTIONAL,

 cause [6] UTF8String OPTIONAL,

 uDMInvalidParameters [7] UDMInvalidParameters,

 uDMSupportedFeatures [8] UTF8String

}

UDMInvalidParameters ::= SEQUENCE

{

 parameter [1] UTF8String OPTIONAL,

 reason [2] UTF8String OPTIONAL

}

-- ===================

-- 5G SMSF definitions

-- ===================

-- See clause 6.2.5.3 for details of this structure

SMSMessage ::= SEQUENCE

{

 originatingSMSParty [1] SMSParty,

 terminatingSMSParty [2] SMSParty,

 direction [3] Direction,

 linkTransferStatus [4] SMSTransferStatus,

 otherMessage [5] SMSOtherMessageIndication OPTIONAL,

 location [6] Location OPTIONAL,

 peerNFAddress [7] SMSNFAddress OPTIONAL,

 peerNFType [8] SMSNFType OPTIONAL,

 sMSTPDUData [9] SMSTPDUData OPTIONAL,

 messageType [10] SMSMessageType OPTIONAL,

 rPMessageReference [11] SMSRPMessageReference OPTIONAL

}

SMSReport ::= SEQUENCE

{

 location [1] Location OPTIONAL,

 sMSTPDUData [2] SMSTPDUData,

 messageType [3] SMSMessageType,

 rPMessageReference [4] SMSRPMessageReference

}

-- ==================

-- 5G SMSF parameters

-- ==================

SMSAddress ::= OCTET STRING(SIZE(2..12))

SMSMessageType ::= ENUMERATED

{

 deliver(1),

 deliverReportAck(2),

 deliverReportError(3),

 statusReport(4),

 command(5),

 submit(6),

 submitReportAck(7),

 submitReportError(8),

 reserved(9)

}

SMSParty ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

 pEI [2] PEI OPTIONAL,

 gPSI [3] GPSI OPTIONAL,

 sMSAddress [4] SMSAddress OPTIONAL

}

SMSTransferStatus ::= ENUMERATED

{

 transferSucceeded(1),

 transferFailed(2),

 undefined(3)

}

SMSOtherMessageIndication ::= BOOLEAN

SMSNFAddress ::= CHOICE

{

 iPAddress [1] IPAddress,

 e164Number [2] E164Number

}

SMSNFType ::= ENUMERATED

{

 sMSGMSC(1),

 iWMSC(2),

 sMSRouter(3)

}

SMSRPMessageReference ::= INTEGER (0..255)

SMSTPDUData ::= CHOICE

{

 sMSTPDU [1] SMSTPDU,

 truncatedSMSTPDU [2] TruncatedSMSTPDU

}

SMSTPDU ::= OCTET STRING (SIZE(1..270))

TruncatedSMSTPDU ::= OCTET STRING (SIZE(1..130))

-- ===============

-- MMS definitions

-- ===============

MMSSend ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 dateTime [3] Timestamp,

 originatingMMSParty [4] MMSParty,

 terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

 direction [8] MMSDirection,

 subject [9] MMSSubject OPTIONAL,

 messageClass [10] MMSMessageClass OPTIONAL,

 expiry [11] MMSExpiry,

 desiredDeliveryTime [12] Timestamp OPTIONAL,

 priority [13] MMSPriority OPTIONAL,

 senderVisibility [14] BOOLEAN OPTIONAL,

 deliveryReport [15] BOOLEAN OPTIONAL,

 readReport [16] BOOLEAN OPTIONAL,

 store [17] BOOLEAN OPTIONAL,

 state [18] MMState OPTIONAL,

 flags [19] MMFlags OPTIONAL,

 replyCharging [20] MMSReplyCharging OPTIONAL,

 applicID [21] UTF8String OPTIONAL,

 replyApplicID [22] UTF8String OPTIONAL,

 auxApplicInfo [23] UTF8String OPTIONAL,

 contentClass [24] MMSContentClass OPTIONAL,

 dRMContent [25] BOOLEAN OPTIONAL,

 adaptationAllowed [26] MMSAdaptation OPTIONAL,

 contentType [27] MMSContentType,

 responseStatus [28] MMSResponseStatus,

 responseStatusText [29] UTF8String OPTIONAL,

 messageID [30] UTF8String

}

MMSSendByNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 contentType [7] MMSContentType,

 messageClass [8] MMSMessageClass OPTIONAL,

 dateTime [9] Timestamp,

 expiry [10] MMSExpiry OPTIONAL,

 deliveryReport [11] BOOLEAN OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 senderVisibility [13] BOOLEAN OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 subject [15] MMSSubject OPTIONAL,

 forwardCount [16] INTEGER OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [18] Timestamp OPTIONAL,

 applicID [19] UTF8String OPTIONAL,

 replyApplicID [20] UTF8String OPTIONAL,

 auxApplicInfo [21] UTF8String OPTIONAL,

 contentClass [22] MMSContentClass OPTIONAL,

 dRMContent [23] BOOLEAN OPTIONAL,

 adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotification ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 originatingMMSParty [3] MMSParty OPTIONAL,

 direction [4] MMSDirection,

 subject [5] MMSSubject OPTIONAL,

 deliveryReportRequested [6] BOOLEAN OPTIONAL,

 stored [7] BOOLEAN OPTIONAL,

 messageClass [8] MMSMessageClass,

 priority [9] MMSPriority OPTIONAL,

 messageSize [10] INTEGER,

 expiry [11] MMSExpiry,

 replyCharging [12] MMSReplyCharging OPTIONAL

}

MMSSendToNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 contentType [7] MMSContentType,

 messageClass [8] MMSMessageClass OPTIONAL,

 dateTime [9] Timestamp,

 expiry [10] MMSExpiry OPTIONAL,

 deliveryReport [11] BOOLEAN OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 senderVisibility [13] BOOLEAN OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 subject [15] MMSSubject OPTIONAL,

 forwardCount [16] INTEGER OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [18] Timestamp OPTIONAL,

 applicID [19] UTF8String OPTIONAL,

 replyApplicID [20] UTF8String OPTIONAL,

 auxApplicInfo [21] UTF8String OPTIONAL,

 contentClass [22] MMSContentClass OPTIONAL,

 dRMContent [23] BOOLEAN OPTIONAL,

 adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotificationResponse ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 status [4] MMStatus,

 reportAllowed [5] BOOLEAN OPTIONAL

}

MMSRetrieval ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 messageID [3] UTF8String,

 dateTime [4] Timestamp,

 originatingMMSParty [5] MMSParty OPTIONAL,

 previouslySentBy [6] MMSPreviouslySentBy OPTIONAL,

 prevSentByDateTime [7] Timestamp OPTIONAL,

 terminatingMMSParty [8] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

 direction [10] MMSDirection,

 subject [11] MMSSubject OPTIONAL,

 state [12] MMState OPTIONAL,

 flags [13] MMFlags OPTIONAL,

 messageClass [14] MMSMessageClass OPTIONAL,

 priority [15] MMSPriority,

 deliveryReport [16] BOOLEAN OPTIONAL,

 readReport [17] BOOLEAN OPTIONAL,

 replyCharging [18] MMSReplyCharging OPTIONAL,

 retrieveStatus [19] MMSRetrieveStatus OPTIONAL,

 retrieveStatusText [20] UTF8String OPTIONAL,

 applicID [21] UTF8String OPTIONAL,

 replyApplicID [22] UTF8String OPTIONAL,

 auxApplicInfo [23] UTF8String OPTIONAL,

 contentClass [24] MMSContentClass OPTIONAL,

 dRMContent [25] BOOLEAN OPTIONAL,

 replaceID [26] UTF8String OPTIONAL,

 contentType [27] UTF8String OPTIONAL

}

MMSDeliveryAck ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 reportAllowed [3] BOOLEAN OPTIONAL,

 status [4] MMStatus,

 direction [5] MMSDirection

}

MMSForward ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 dateTime [3] Timestamp OPTIONAL,

 originatingMMSParty [4] MMSParty,

 terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

 direction [8] MMSDirection,

 expiry [9] MMSExpiry OPTIONAL,

 desiredDeliveryTime [10] Timestamp OPTIONAL,

 deliveryReportAllowed [11] BOOLEAN OPTIONAL,

 deliveryReport [12] BOOLEAN OPTIONAL,

 store [13] BOOLEAN OPTIONAL,

 state [14] MMState OPTIONAL,

 flags [15] MMFlags OPTIONAL,

 contentLocationReq [16] UTF8String,

 replyCharging [17] MMSReplyCharging OPTIONAL,

 responseStatus [18] MMSResponseStatus,

 responseStatusText [19] UTF8String OPTIONAL,

 messageID [20] UTF8String OPTIONAL,

 contentLocationConf [21] UTF8String OPTIONAL,

 storeStatus [22] MMSStoreStatus OPTIONAL,

 storeStatusText [23] UTF8String OPTIONAL

}

MMSDeleteFromRelay ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] SEQUENCE OF UTF8String,

 contentLocationConf [5] SEQUENCE OF UTF8String,

 deleteResponseStatus [6] MMSDeleteResponseStatus,

 deleteResponseText [7] SEQUENCE OF UTF8String

}

MMSMBoxStore ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] UTF8String,

 state [5] MMState OPTIONAL,

 flags [6] MMFlags OPTIONAL,

 contentLocationConf [7] UTF8String OPTIONAL,

 storeStatus [8] MMSStoreStatus,

 storeStatusText [9] UTF8String OPTIONAL

}

MMSMBoxUpload ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 state [4] MMState OPTIONAL,

 flags [5] MMFlags OPTIONAL,

 contentType [6] UTF8String,

 contentLocation [7] UTF8String OPTIONAL,

 storeStatus [8] MMSStoreStatus,

 storeStatusText [9] UTF8String OPTIONAL,

 mMessages [10] SEQUENCE OF MMBoxDescription

}

MMSMBoxDelete ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 direction [3] MMSDirection,

 contentLocationReq [4] SEQUENCE OF UTF8String,

 contentLocationConf [5] SEQUENCE OF UTF8String OPTIONAL,

 responseStatus [6] MMSDeleteResponseStatus,

 responseStatusText [7] UTF8String OPTIONAL

}

MMSDeliveryReport ::= SEQUENCE

{

 version [1] MMSVersion,

 messageID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 mMSDateTime [4] Timestamp,

 responseStatus [5] MMSResponseStatus,

 responseStatusText [6] UTF8String OPTIONAL,

 applicID [7] UTF8String OPTIONAL,

 replyApplicID [8] UTF8String OPTIONAL,

 auxApplicInfo [9] UTF8String OPTIONAL

}

MMSDeliveryReportNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 messageID [3] UTF8String,

 terminatingMMSParty [4] SEQUENCE OF MMSParty,

 originatingMMSParty [5] MMSParty,

 direction [6] MMSDirection,

 mMSDateTime [7] Timestamp,

 forwardToOriginator [8] BOOLEAN OPTIONAL,

 status [9] MMStatus,

 statusExtension [10] MMStatusExtension,

 statusText [11] MMStatusText,

 applicID [12] UTF8String OPTIONAL,

 replyApplicID [13] UTF8String OPTIONAL,

 auxApplicInfo [14] UTF8String OPTIONAL

}

MMSReadReport ::= SEQUENCE

{

 version [1] MMSVersion,

 messageID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 originatingMMSParty [4] SEQUENCE OF MMSParty,

 direction [5] MMSDirection,

 mMSDateTime [6] Timestamp,

 readStatus [7] MMSReadStatus,

 applicID [8] UTF8String OPTIONAL,

 replyApplicID [9] UTF8String OPTIONAL,

 auxApplicInfo [10] UTF8String OPTIONAL

}

MMSReadReportNonLocalTarget ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 terminatingMMSParty [3] SEQUENCE OF MMSParty,

 originatingMMSParty [4] SEQUENCE OF MMSParty,

 direction [5] MMSDirection,

 messageID [6] UTF8String,

 mMSDateTime [7] Timestamp,

 readStatus [8] MMSReadStatus,

 readStatusText [9] MMSReadStatusText OPTIONAL,

 applicID [10] UTF8String OPTIONAL,

 replyApplicID [11] UTF8String OPTIONAL,

 auxApplicInfo [12] UTF8String OPTIONAL

}

MMSCancel ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 cancelID [3] UTF8String,

 direction [4] MMSDirection

}

MMSMBoxViewRequest ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 contentLocation [3] UTF8String OPTIONAL,

 state [4] SEQUENCE OF MMState OPTIONAL,

 flags [5] SEQUENCE OF MMFlags OPTIONAL,

 start [6] INTEGER OPTIONAL,

 limit [7] INTEGER OPTIONAL,

 attributes [8] SEQUENCE OF UTF8String OPTIONAL,

 totals [9] INTEGER OPTIONAL,

 quotas [10] MMSQuota OPTIONAL

}

MMSMBoxViewResponse ::= SEQUENCE

{

 transactionID [1] UTF8String,

 version [2] MMSVersion,

 contentLocation [3] UTF8String OPTIONAL,

 state [4] SEQUENCE OF MMState OPTIONAL,

 flags [5] SEQUENCE OF MMFlags OPTIONAL,

 start [6] INTEGER OPTIONAL,

 limit [7] INTEGER OPTIONAL,

 attributes [8] SEQUENCE OF UTF8String OPTIONAL,

 mMSTotals [9] BOOLEAN OPTIONAL,

 mMSQuotas [10] BOOLEAN OPTIONAL,

 mMessages [11] SEQUENCE OF MMBoxDescription

}

MMBoxDescription ::= SEQUENCE

{

 contentLocation [1] UTF8String OPTIONAL,

 messageID [2] UTF8String OPTIONAL,

 state [3] MMState OPTIONAL,

 flags [4] SEQUENCE OF MMFlags OPTIONAL,

 dateTime [5] Timestamp OPTIONAL,

 originatingMMSParty [6] MMSParty OPTIONAL,

 terminatingMMSParty [7] SEQUENCE OF MMSParty OPTIONAL,

 cCRecipients [8] SEQUENCE OF MMSParty OPTIONAL,

 bCCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

 messageClass [10] MMSMessageClass OPTIONAL,

 subject [11] MMSSubject OPTIONAL,

 priority [12] MMSPriority OPTIONAL,

 deliveryTime [13] Timestamp OPTIONAL,

 readReport [14] BOOLEAN OPTIONAL,

 messageSize [15] INTEGER OPTIONAL,

 replyCharging [16] MMSReplyCharging OPTIONAL,

 previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

 previouslySentByDateTime [18] Timestamp OPTIONAL,

 contentType [19] UTF8String OPTIONAL

}

-- =========

-- MMS CCPDU

-- =========

MMSCCPDU ::= SEQUENCE

{

 version [1] MMSVersion,

 transactionID [2] UTF8String,

 mMSContent [3] OCTET STRING

}

-- ==============

-- MMS parameters

-- ==============

MMSAdaptation ::= SEQUENCE

{

 allowed [1] BOOLEAN,

 overriden [2] BOOLEAN

}

MMSCancelStatus ::= ENUMERATED

{

 cancelRequestSuccessfullyReceived(1),

 cancelRequestCorrupted(2)

}

MMSContentClass ::= ENUMERATED

{

 text(1),

 imageBasic(2),

 imageRich(3),

 videoBasic(4),

 videoRich(5),

 megaPixel(6),

 contentBasic(7),

 contentRich(8)

}

MMSContentType ::= UTF8String

MMSDeleteResponseStatus ::= ENUMERATED

{

 ok(1),

 errorUnspecified(2),

 errorServiceDenied(3),

 errorMessageFormatCorrupt(4),

 errorSendingAddressUnresolved(5),

 errorMessageNotFound(6),

 errorNetworkProblem(7),

 errorContentNotAccepted(8),

 errorUnsupportedMessage(9),

 errorTransientFailure(10),

 errorTransientSendingAddressUnresolved(11),

 errorTransientMessageNotFound(12),

 errorTransientNetworkProblem(13),

 errorTransientPartialSuccess(14),

 errorPermanentFailure(15),

 errorPermanentServiceDenied(16),

 errorPermanentMessageFormatCorrupt(17),

 errorPermanentSendingAddressUnresolved(18),

 errorPermanentMessageNotFound(19),

 errorPermanentContentNotAccepted(20),

 errorPermanentReplyChargingLimitationsNotMet(21),

 errorPermanentReplyChargingRequestNotAccepted(22),

 errorPermanentReplyChargingForwardingDenied(23),

 errorPermanentReplyChargingNotSupported(24),

 errorPermanentAddressHidingNotSupported(25),

 errorPermanentLackOfPrepaid(26)

}

MMSDirection ::= ENUMERATED

{

 fromTarget(0),

 toTarget(1)

}

MMSElementDescriptor ::= SEQUENCE

{

 reference [1] UTF8String,

 parameter [2] UTF8String OPTIONAL,

 value [3] UTF8String OPTIONAL

}

MMSExpiry ::= SEQUENCE

{

 expiryPeriod [1] INTEGER,

 periodFormat [2] MMSPeriodFormat

}

MMFlags ::= SEQUENCE

{

 length [1] INTEGER,

 flag [2] MMStateFlag,

 flagString [3] UTF8String

}

MMSMessageClass ::= ENUMERATED

{

 personal(1),

 advertisement(2),

 informational(3),

 auto(4)

}

MMSParty ::= SEQUENCE

{

 mMSPartyIDs [1] SEQUENCE OF MMSPartyID,

 nonLocalID [2] NonLocalID

}

MMSPartyID ::= CHOICE

{

 e164Number [1] E164Number,

 emailAddress [2] EmailAddress,

 iMSI [3] IMSI,

 iMPU [4] IMPU,

 iMPI [5] IMPI,

 sUPI [6] SUPI,

 gPSI [7] GPSI

}

MMSPeriodFormat ::= ENUMERATED

{

 absolute(1),

 relative(2)

}

MMSPreviouslySent ::= SEQUENCE

{

 previouslySentByParty [1] MMSParty,

 sequenceNumber [2] INTEGER,

 previousSendDateTime [3] Timestamp

}

MMSPreviouslySentBy ::= SEQUENCE OF MMSPreviouslySent

MMSPriority ::= ENUMERATED

{

 low(1),

 normal(2),

 high(3)

}

MMSQuota ::= SEQUENCE

{

 quota [1] INTEGER,

 quotaUnit [2] MMSQuotaUnit

}

MMSQuotaUnit ::= ENUMERATED

{

 numMessages(1),

 bytes(2)

}

MMSReadStatus ::= ENUMERATED

{

 read(1),

 deletedWithoutBeingRead(2)

}

MMSReadStatusText ::= UTF8String

MMSReplyCharging ::= ENUMERATED

{

 requested(0),

 requestedTextOnly(1),

 accepted(2),

 acceptedTextOnly(3)

}

MMSResponseStatus ::= ENUMERATED

{

 ok(1),

 errorUnspecified(2),

 errorServiceDenied(3),

 errorMessageFormatCorrupt(4),

 errorSendingAddressUnresolved(5),

 errorMessageNotFound(6),

 errorNetworkProblem(7),

 errorContentNotAccepted(8),

 errorUnsupportedMessage(9),

 errorTransientFailure(10),

 errorTransientSendingAddressUnresolved(11),

 errorTransientMessageNotFound(12),

 errorTransientNetworkProblem(13),

 errorTransientPartialSuccess(14),

 errorPermanentFailure(15),

 errorPermanentServiceDenied(16),

 errorPermanentMessageFormatCorrupt(17),

 errorPermanentSendingAddressUnresolved(18),

 errorPermanentMessageNotFound(19),

 errorPermanentContentNotAccepted(20),

 errorPermanentReplyChargingLimitationsNotMet(21),

 errorPermanentReplyChargingRequestNotAccepted(22),

 errorPermanentReplyChargingForwardingDenied(23),

 errorPermanentReplyChargingNotSupported(24),

 errorPermanentAddressHidingNotSupported(25),

 errorPermanentLackOfPrepaid(26)

}

MMSRetrieveStatus ::= ENUMERATED

{

 success(1),

 errorTransientFailure(2),

 errorTransientMessageNotFound(3),

 errorTransientNetworkProblem(4),

 errorPermanentFailure(5),

 errorPermanentServiceDenied(6),

 errorPermanentMessageNotFound(7),

 errorPermanentContentUnsupported(8)

}

MMSStoreStatus ::= ENUMERATED

{

 success(1),

 errorTransientFailure(2),

 errorTransientNetworkProblem(3),

 errorPermanentFailure(4),

 errorPermanentServiceDenied(5),

 errorPermanentMessageFormatCorrupt(6),

 errorPermanentMessageNotFound(7),

 errorMMBoxFull(8)

}

MMState ::= ENUMERATED

{

 draft(1),

 sent(2),

 new(3),

 retrieved(4),

 forwarded(5)

}

MMStateFlag ::= ENUMERATED

{

 add(1),

 remove(2),

 filter(3)

}

MMStatus ::= ENUMERATED

{

 expired(1),

 retrieved(2),

 rejected(3),

 deferred(4),

 unrecognized(5),

 indeterminate(6),

 forwarded(7),

 unreachable(8)

}

MMStatusExtension ::= ENUMERATED

{

 rejectionByMMSRecipient(0),

 rejectionByOtherRS(1)

}

MMStatusText ::= UTF8String

MMSSubject ::= UTF8String

MMSVersion ::= SEQUENCE

{

 majorVersion [1] INTEGER,

 minorVersion [2] INTEGER

}

-- ==================

-- 5G PTC definitions

-- ==================

PTCRegistration ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCServerURI [2] UTF8String,

 pTCRegistrationRequest [3] PTCRegistrationRequest,

 pTCRegistrationOutcome [4] PTCRegistrationOutcome

}

PTCSessionInitiation ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCOriginatingID [5] PTCTargetInformation,

 pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

 location [8] Location OPTIONAL,

 pTCBearerCapability [9] UTF8String OPTIONAL,

 pTCHost [10] PTCTargetInformation OPTIONAL

}

PTCSessionAbandon ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 location [4] Location OPTIONAL,

 pTCAbandonCause [5] INTEGER

}

PTCSessionStart ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCOriginatingID [5] PTCTargetInformation,

 pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

 location [8] Location OPTIONAL,

 pTCHost [9] PTCTargetInformation OPTIONAL,

 pTCBearerCapability [10] UTF8String OPTIONAL

}

PTCSessionEnd ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCServerURI [3] UTF8String,

 pTCSessionInfo [4] PTCSessionInfo,

 pTCParticipants [5] SEQUENCE OF PTCTargetInformation OPTIONAL,

 location [6] Location OPTIONAL,

 pTCSessionEndCause [7] PTCSessionEndCause

}

PTCStartOfInterception ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 preEstSessionID [3] PTCSessionInfo OPTIONAL,

 pTCOriginatingID [4] PTCTargetInformation,

 pTCSessionInfo [5] PTCSessionInfo OPTIONAL,

 pTCHost [6] PTCTargetInformation OPTIONAL,

 pTCParticipants [7] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCMediaStreamAvail [8] BOOLEAN OPTIONAL,

 pTCBearerCapability [9] UTF8String OPTIONAL

}

PTCPreEstablishedSession ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCServerURI [2] UTF8String,

 rTPSetting [3] RTPSetting,

 pTCMediaCapability [4] UTF8String,

 pTCPreEstSessionID [5] PTCSessionInfo,

 pTCPreEstStatus [6] PTCPreEstStatus,

 pTCMediaStreamAvail [7] BOOLEAN OPTIONAL,

 location [8] Location OPTIONAL,

 pTCFailureCode [9] PTCFailureCode OPTIONAL

}

PTCInstantPersonalAlert ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCIPAPartyID [2] PTCTargetInformation,

 pTCIPADirection [3] Direction

}

PTCPartyJoin ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCParticipantPresenceStatus [5] MultipleParticipantPresenceStatus OPTIONAL,

 pTCMediaStreamAvail [6] BOOLEAN OPTIONAL,

 pTCBearerCapability [7] UTF8String OPTIONAL

}

PTCPartyDrop ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCPartyDrop [4] PTCTargetInformation,

 pTCParticipantPresenceStatus [5] PTCParticipantPresenceStatus OPTIONAL

}

PTCPartyHold ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCHoldID [5] SEQUENCE OF PTCTargetInformation,

 pTCHoldRetrieveInd [6] BOOLEAN

}

PTCMediaModification ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessionInfo [3] PTCSessionInfo,

 pTCMediaStreamAvail [4] BOOLEAN OPTIONAL,

 pTCBearerCapability [5] UTF8String

}

PTCGroupAdvertisement ::=SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCIDList [3] SEQUENCE OF PTCTargetInformation OPTIONAL,

 pTCGroupAuthRule [4] PTCGroupAuthRule OPTIONAL,

 pTCGroupAdSender [5] PTCTargetInformation,

 pTCGroupNickname [6] UTF8String OPTIONAL

}

PTCFloorControl ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCSessioninfo [3] PTCSessionInfo,

 pTCFloorActivity [4] SEQUENCE OF PTCFloorActivity,

 pTCFloorSpeakerID [5] PTCTargetInformation OPTIONAL,

 pTCMaxTBTime [6] INTEGER OPTIONAL,

 pTCQueuedFloorControl [7] BOOLEAN OPTIONAL,

 pTCQueuedPosition [8] INTEGER OPTIONAL,

 pTCTalkBurstPriority [9] PTCTBPriorityLevel OPTIONAL,

 pTCTalkBurstReason [10] PTCTBReasonCode OPTIONAL

}

PTCTargetPresence ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCTargetPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCParticipantPresence ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCParticipantPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCListManagement ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCListManagementType [3] PTCListManagementType OPTIONAL,

 pTCListManagementAction [4] PTCListManagementAction OPTIONAL,

 pTCListManagementFailure [5] PTCListManagementFailure OPTIONAL,

 pTCContactID [6] PTCTargetInformation OPTIONAL,

 pTCIDList [7] SEQUENCE OF PTCIDList OPTIONAL,

 pTCHost [8] PTCTargetInformation OPTIONAL

}

PTCAccessPolicy ::= SEQUENCE

{

 pTCTargetInformation [1] PTCTargetInformation,

 pTCDirection [2] Direction,

 pTCAccessPolicyType [3] PTCAccessPolicyType OPTIONAL,

 pTCUserAccessPolicy [4] PTCUserAccessPolicy OPTIONAL,

 pTCGroupAuthRule [5] PTCGroupAuthRule OPTIONAL,

 pTCContactID [6] PTCTargetInformation OPTIONAL,

 pTCAccessPolicyFailure [7] PTCAccessPolicyFailure OPTIONAL

}

-- =========

-- PTC CCPDU

-- =========

PTCCCPDU ::= OCTET STRING

-- =================

-- 5G PTC parameters

-- =================

PTCRegistrationRequest ::= ENUMERATED

{

 register(1),

 reRegister(2),

 deRegister(3)

}

PTCRegistrationOutcome ::= ENUMERATED

{

 success(1),

 failure(2)

}

PTCSessionEndCause ::= ENUMERATED

{

 initiaterLeavesSession(1),

 definedParticipantLeaves(2),

 numberOfParticipants(3),

 sessionTimerExpired(4),

 pTCSpeechInactive(5),

 allMediaTypesInactive(6)

}

PTCTargetInformation ::= SEQUENCE

{

 identifiers [1] SEQUENCE SIZE(1..MAX) OF PTCIdentifiers

}

PTCIdentifiers ::= CHOICE

{

 mCPTTID [1] UTF8String,

 instanceIdentifierURN [2] UTF8String,

 pTCChatGroupID [3] PTCChatGroupID,

 iMPU [4] IMPU,

 iMPI [5] IMPI

}

PTCSessionInfo ::= SEQUENCE

{

 pTCSessionURI [1] UTF8String,

 pTCSessionType [2] PTCSessionType

}

PTCSessionType ::= ENUMERATED

{

 ondemand(1),

 preEstablished(2),

 adhoc(3),

 prearranged(4),

 groupSession(5)

}

MultipleParticipantPresenceStatus ::= SEQUENCE OF PTCParticipantPresenceStatus

PTCParticipantPresenceStatus ::= SEQUENCE

{

 presenceID [1] PTCTargetInformation,

 presenceType [2] PTCPresenceType,

 presenceStatus [3] BOOLEAN

}

PTCPresenceType ::= ENUMERATED

{

 pTCClient(1),

 pTCGroup(2)

}

PTCPreEstStatus ::= ENUMERATED

{

 established(1),

 modified(2),

 released(3)

}

RTPSetting ::= SEQUENCE

{

 iPAddress [1] IPAddress,

 portNumber [2] PortNumber

}

PTCIDList ::= SEQUENCE

{

 pTCPartyID [1] PTCTargetInformation,

 pTCChatGroupID [2] PTCChatGroupID

}

PTCChatGroupID ::= SEQUENCE

{

 groupIdentity [1] UTF8String

}

PTCFloorActivity ::= ENUMERATED

{

 tBCPRequest(1),

 tBCPGranted(2),

 tBCPDeny(3),

 tBCPIdle(4),

 tBCPTaken(5),

 tBCPRevoke(6),

 tBCPQueued(7),

 tBCPRelease(8)

}

PTCTBPriorityLevel ::= ENUMERATED

{

 preEmptive(1),

 highPriority(2),

 normalPriority(3),

 listenOnly(4)

}

PTCTBReasonCode ::= ENUMERATED

{

 noQueuingAllowed(1),

 oneParticipantSession(2),

 listenOnly(3),

 exceededMaxDuration(4),

 tBPrevented(5)

}

PTCListManagementType ::= ENUMERATED

{

 contactListManagementAttempt(1),

 groupListManagementAttempt(2),

 contactListManagementResult(3),

 groupListManagementResult(4),

 requestUnsuccessful(5)

}

PTCListManagementAction ::= ENUMERATED

{

 create(1),

 modify(2),

 retrieve(3),

 delete(4),

 notify(5)

}

PTCAccessPolicyType ::= ENUMERATED

{

 pTCUserAccessPolicyAttempt(1),

 groupAuthorizationRulesAttempt(2),

 pTCUserAccessPolicyQuery(3),

 groupAuthorizationRulesQuery(4),

 pTCUserAccessPolicyResult(5),

 groupAuthorizationRulesResult(6),

 requestUnsuccessful(7)

}

PTCUserAccessPolicy ::= ENUMERATED

{

 allowIncomingPTCSessionRequest(1),

 blockIncomingPTCSessionRequest(2),

 allowAutoAnswerMode(3),

 allowOverrideManualAnswerMode(4)

}

PTCGroupAuthRule ::= ENUMERATED

{

 allowInitiatingPTCSession(1),

 blockInitiatingPTCSession(2),

 allowJoiningPTCSession(3),

 blockJoiningPTCSession(4),

 allowAddParticipants(5),

 blockAddParticipants(6),

 allowSubscriptionPTCSessionState(7),

 blockSubscriptionPTCSessionState(8),

 allowAnonymity(9),

 forbidAnonymity(10)

}

PTCFailureCode ::= ENUMERATED

{

 sessionCannotBeEstablished(1),

 sessionCannotBeModified(2)

}

PTCListManagementFailure ::= ENUMERATED

{

 requestUnsuccessful(1),

 requestUnknown(2)

}

PTCAccessPolicyFailure ::= ENUMERATED

{

 requestUnsuccessful(1),

 requestUnknown(2)

}

-- ===============

-- IMS definitions

-- ===============

-- See clause 7.12.4.2.1 for details of this structure

IMSMessage ::= SEQUENCE

{

 payload [1] IMSPayload,

 sessionDirection [2] SessionDirection,

 voIPRoamingIndication [3] VoIPRoamingIndication OPTIONAL,

 location [6] Location OPTIONAL

}

-- See clause 7.12.4.2.2 for details of this structure

StartOfInterceptionForActiveIMSSession ::= SEQUENCE

{

 originatingId [1] SEQUENCE OF IMPU,

 terminatingId [2] IMPU,

 sDPState [3] SEQUENCE OF OCTET STRING OPTIONAL,

 diversionIdentity [4] IMPU OPTIONAL,

 voIPRoamingIndication [5] VoIPRoamingIndication OPTIONAL,

 location [7] Location OPTIONAL

}

-- See clause 7.12.4.2.3 for the details.

IMSCCUnavailable ::= SEQUENCE

{

 cCUnavailableReason [1] UTF8String,

 sDPState [2] OCTET STRING OPTIONAL

}

-- ==============

-- IMS parameters

-- ==============

IMSPayload ::= CHOICE

{

 encapsulatedSIPMessage [1] SIPMessage

}

SIPMessage ::= SEQUENCE

{

 iPSourceAddress [1] IPAddress,

 iPDestinationAddress [2] IPAddress,

 sIPContent [3] OCTET STRING

}

VoIPRoamingIndication ::= ENUMERATED

{

 roamingLBO(1),

 roamingS8HR(2),

 roamingN9HR(3)

}

SessionDirection ::= ENUMERATED

{

 fromTarget(1),

 toTarget(2),

 combined(3),

 indeterminate(4)

}

HeaderOnlyIndication ::= BOOLEAN

-- =================================

-- STIR/SHAKEN/RCD/eCNAM definitions

-- =================================

-- See clause 7.11.2.1.2 for details of this structure

STIRSHAKENSignatureGeneration ::= SEQUENCE

{

 pASSporTs [1] SEQUENCE OF PASSporT,

 encapsulatedSIPMessage [2] SIPMessage OPTIONAL

}

-- See clause 7.11.2.1.3 for details of this structure

STIRSHAKENSignatureValidation ::= SEQUENCE

{

 pASSporTs [1] SEQUENCE OF PASSporT OPTIONAL,

 rCDTerminalDisplayInfo [2] RCDDisplayInfo OPTIONAL,

 eCNAMTerminalDisplayInfo [3] ECNAMDisplayInfo OPTIONAL,

 sHAKENValidationResult [4] SHAKENValidationResult,

 sHAKENFailureStatusCode [5] SHAKENFailureStatusCode OPTIONAL,

 encapsulatedSIPMessage [6] SIPMessage OPTIONAL

}

-- ================================

-- STIR/SHAKEN/RCD/eCNAM parameters

-- ================================

PASSporT ::= SEQUENCE

{

 pASSporTHeader [1] PASSporTHeader,

 pASSporTPayload [2] PASSporTPayload,

 pASSporTSignature [3] OCTET STRING

}

PASSporTHeader ::= SEQUENCE

{

 type [1] JWSTokenType,

 algorithm [2] UTF8String,

 ppt [3] UTF8String OPTIONAL,

 x5u [4] UTF8String

}

JWSTokenType ::= ENUMERATED

{

 passport(1)

}

PASSporTPayload ::= SEQUENCE

{

 issuedAtTime [1] GeneralizedTime,

 originator [2] STIRSHAKENOriginator,

 destination [3] STIRSHAKENDestinations,

 attestation [4] Attestation,

 origId [5] UTF8String,

 diversion [6] STIRSHAKENDestination

}

STIRSHAKENOriginator ::= CHOICE

{

 telephoneNumber [1] STIRSHAKENTN,

 sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENDestinations ::= SEQUENCE OF STIRSHAKENDestination

STIRSHAKENDestination ::= CHOICE

{

 telephoneNumber [1] STIRSHAKENTN,

 sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENTN ::= CHOICE

{

 mSISDN [1] MSISDN

}

Attestation ::= ENUMERATED

{

 attestationA(1),

 attestationB(2),

 attestationC(3)

}

SHAKENValidationResult ::= ENUMERATED

{

 tNValidationPassed(1),

 tNValidationFailed(2),

 noTNValidation(3)

}

SHAKENFailureStatusCode ::= INTEGER

ECNAMDisplayInfo ::= SEQUENCE

{

 name [1] UTF8String,

 additionalInfo [2] OCTET STRING OPTIONAL

}

RCDDisplayInfo ::= SEQUENCE

{

 name [1] UTF8String,

 jcd [2] OCTET STRING OPTIONAL,

 jcl [3] OCTET STRING OPTIONAL

}

-- ===================

-- 5G LALS definitions

-- ===================

LALSReport ::= SEQUENCE

{

 sUPI [1] SUPI OPTIONAL,

-- pEI [2] PEI OPTIONAL, deprecated in Release-16, do not re-use this tag number

 gPSI [3] GPSI OPTIONAL,

 location [4] Location OPTIONAL,

 iMPU [5] IMPU OPTIONAL,

 iMSI [7] IMSI OPTIONAL,

 mSISDN [8] MSISDN OPTIONAL

}

-- =====================

-- PDHR/PDSR definitions

-- =====================

PDHeaderReport ::= SEQUENCE

{

 pDUSessionID [1] PDUSessionID,

 sourceIPAddress [2] IPAddress,

 sourcePort [3] PortNumber OPTIONAL,

 destinationIPAddress [4] IPAddress,

 destinationPort [5] PortNumber OPTIONAL,

 nextLayerProtocol [6] NextLayerProtocol,

 iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

 direction [8] Direction,

 packetSize [9] INTEGER

}

PDSummaryReport ::= SEQUENCE

{

 pDUSessionID [1] PDUSessionID,

 sourceIPAddress [2] IPAddress,

 sourcePort [3] PortNumber OPTIONAL,

 destinationIPAddress [4] IPAddress,

 destinationPort [5] PortNumber OPTIONAL,

 nextLayerProtocol [6] NextLayerProtocol,

 iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

 direction [8] Direction,

 pDSRSummaryTrigger [9] PDSRSummaryTrigger,

 firstPacketTimestamp [10] Timestamp,

 lastPacketTimestamp [11] Timestamp,

 packetCount [12] INTEGER,

 byteCount [13] INTEGER

}

-- ====================

-- PDHR/PDSR parameters

-- ====================

PDSRSummaryTrigger ::= ENUMERATED

{

 timerExpiry(1),

 packetCount(2),

 byteCount(3),

 startOfFlow(4),

 endOfFlow(5)

}

-- ==================================

-- Identifier Association definitions

-- ==================================

AMFIdentifierAssociation ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI,

 location [6] Location,

 fiveGSTAIList [7] TAIList OPTIONAL

}

MMEIdentifierAssociation ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 gUTI [4] GUTI,

 location [5] Location,

 tAIList [6] TAIList OPTIONAL

}

-- =================================

-- Identifier Association parameters

-- =================================

MMEGroupID ::= OCTET STRING (SIZE(2))

MMECode ::= OCTET STRING (SIZE(1))

TMSI ::= OCTET STRING (SIZE(4))

-- ===================

-- EPS MME definitions

-- ===================

MMEAttach ::= SEQUENCE

{

 attachType [1] EPSAttachType,

 attachResult [2] EPSAttachResult,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL,

 ePSTAIList [8] TAIList OPTIONAL,

 sMSServiceStatus [9] EPSSMSServiceStatus OPTIONAL,

 oldGUTI [10] GUTI OPTIONAL,

 eMM5GRegStatus [11] EMM5GMMStatus OPTIONAL

}

MMEDetach ::= SEQUENCE

{

 detachDirection [1] MMEDirection,

 detachType [2] EPSDetachType,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 cause [7] EMMCause OPTIONAL,

 location [8] Location OPTIONAL,

 switchOffIndicator [9] SwitchOffIndicator OPTIONAL

}

MMELocationUpdate ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 gUTI [4] GUTI OPTIONAL,

 location [5] Location OPTIONAL,

 oldGUTI [6] GUTI OPTIONAL,

 sMSServiceStatus [7] EPSSMSServiceStatus OPTIONAL

}

MMEStartOfInterceptionWithEPSAttachedUE ::= SEQUENCE

{

 attachType [1] EPSAttachType,

 attachResult [2] EPSAttachResult,

 iMSI [3] IMSI,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL,

 ePSTAIList [9] TAIList OPTIONAL,

 sMSServiceStatus [10] EPSSMSServiceStatus OPTIONAL,

 eMM5GRegStatus [12] EMM5GMMStatus OPTIONAL

}

MMEUnsuccessfulProcedure ::= SEQUENCE

{

 failedProcedureType [1] MMEFailedProcedureType,

 failureCause [2] MMEFailureCause,

 iMSI [3] IMSI OPTIONAL,

 iMEI [4] IMEI OPTIONAL,

 mSISDN [5] MSISDN OPTIONAL,

 gUTI [6] GUTI OPTIONAL,

 location [7] Location OPTIONAL

}

-- See clause 6.3.2.2.8 for details of this structure

MMEPositioningInfoTransfer ::= SEQUENCE

{

 iMSI [1] IMSI,

 iMEI [2] IMEI OPTIONAL,

 mSISDN [3] MSISDN OPTIONAL,

 gUTI [4] GUTI OPTIONAL,

 lPPaMessage [5] OCTET STRING OPTIONAL,

 lPPMessage [6] OCTET STRING OPTIONAL,

 mMELCSCorrelationId [7] OCTET STRING (SIZE(4))

}

-- ==================

-- EPS MME parameters

-- ==================

EMMCause ::= INTEGER (0..255)

ESMCause ::= INTEGER (0..255)

EPSAttachType ::= ENUMERATED

{

 ePSAttach(1),

 combinedEPSIMSIAttach(2),

 ePSRLOSAttach(3),

 ePSEmergencyAttach(4),

 reserved(5)

}

EPSAttachResult ::= ENUMERATED

{

 ePSOnly(1),

 combinedEPSIMSI(2)

}

EPSDetachType ::= ENUMERATED

{

 ePSDetach(1),

 iMSIDetach(2),

 combinedEPSIMSIDetach(3),

 reAttachRequired(4),

 reAttachNotRequired(5),

 reserved(6)

}

EPSSMSServiceStatus ::= ENUMERATED

{

 sMSServicesNotAvailable(1),

 sMSServicesNotAvailableInThisPLMN(2),

 networkFailure(3),

 congestion(4)

}

MMEDirection ::= ENUMERATED

{

 networkInitiated(1),

 uEInitiated(2)

}

MMEFailedProcedureType ::= ENUMERATED

{

 attachReject(1),

 authenticationReject(2),

 securityModeReject(3),

 serviceReject(4),

 trackingAreaUpdateReject(5),

 activateDedicatedEPSBearerContextReject(6),

 activateDefaultEPSBearerContextReject(7),

 bearerResourceAllocationReject(8),

 bearerResourceModificationReject(9),

 modifyEPSBearerContectReject(10),

 pDNConnectivityReject(11),

 pDNDisconnectReject(12)

}

MMEFailureCause ::= CHOICE

{

 eMMCause [1] EMMCause,

 eSMCause [2] ESMCause

}

-- ===========================

-- LI Notification definitions

-- ===========================

LINotification ::= SEQUENCE

{

 notificationType [1] LINotificationType,

 appliedTargetID [2] TargetIdentifier OPTIONAL,

 appliedDeliveryInformation [3] SEQUENCE OF LIAppliedDeliveryInformation OPTIONAL,

 appliedStartTime [4] Timestamp OPTIONAL,

 appliedEndTime [5] Timestamp OPTIONAL

}

-- ==========================

-- LI Notification parameters

-- ==========================

LINotificationType ::= ENUMERATED

{

 activation(1),

 deactivation(2),

 modification(3)

}

LIAppliedDeliveryInformation ::= SEQUENCE

{

 hI2DeliveryIPAddress [1] IPAddress OPTIONAL,

 hI2DeliveryPortNumber [2] PortNumber OPTIONAL,

 hI3DeliveryIPAddress [3] IPAddress OPTIONAL,

 hI3DeliveryPortNumber [4] PortNumber OPTIONAL

}

-- ===============

-- MDF definitions

-- ===============

MDFCellSiteReport ::= SEQUENCE OF CellInformation

-- ==============================

-- 5G EPS Interworking Parameters

-- ==============================

EMM5GMMStatus ::= SEQUENCE

{

 eMMRegStatus [1] EMMRegStatus OPTIONAL,

 fiveGMMStatus [2] FiveGMMStatus OPTIONAL

}

EPS5GGUTI ::= CHOICE

{

 gUTI [1] GUTI,

 fiveGGUTI [2] FiveGGUTI

}

EMMRegStatus ::= ENUMERATED

{

 uEEMMRegistered(1),

 uENotEMMRegistered(2)

}

FiveGMMStatus ::= ENUMERATED

{

 uE5GMMRegistered(1),

 uENot5GMMRegistered(2)

}

-- ========================================

-- Separated Location Reporting definitions

-- ========================================

SeparatedLocationReporting ::= SEQUENCE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI OPTIONAL,

 pEI [3] PEI OPTIONAL,

 gPSI [4] GPSI OPTIONAL,

 gUTI [5] FiveGGUTI OPTIONAL,

 location [6] Location,

 non3GPPAccessEndpoint [7] UEEndpointAddress OPTIONAL,

 rATType [8] RATType OPTIONAL

}

-- =================

-- Common Parameters

-- =================

AccessType ::= ENUMERATED

{

 threeGPPAccess(1),

 nonThreeGPPAccess(2),

 threeGPPandNonThreeGPPAccess(3)

}

AllowedNSSAI ::= SEQUENCE OF NSSAI

AllowedTACs ::= SEQUENCE (SIZE(1..MAX)) OF TAC

AreaOfInterest ::= SEQUENCE

{

 areaOfInterestTAIList [1] AreaOfInterestTAIList OPTIONAL,

 areaOfInterestCellList [2] AreaOfInterestCellList OPTIONAL,

 areaOfInterestRANNodeList [3] AreaOfInterestRANNodeList OPTIONAL

}

AreaOfInterestCellList ::= SEQUENCE (SIZE(1..MAX)) OF NCGI

AreaOfInterestItem ::= SEQUENCE

{

 areaOfInterest [1] AreaOfInterest

}

AreaOfInterestRANNodeList ::= SEQUENCE (SIZE(1..MAX)) OF GlobalRANNodeID

AreaOfInterestTAIList ::= SEQUENCE (SIZE(1..MAX)) OF TAI

BitRate ::= INTEGER

CellCAGList ::= SEQUENCE (SIZE(1..MAX)) OF CAGID

CauseMisc ::= ENUMERATED

{

 controlProcessingOverload(1),

 notEnoughUserPlaneProcessingResources(2),

 hardwareFailure(3),

 oMIntervention(4),

 unknownPLMNOrSNPN(5),

 unspecified(6)

}

CauseNas ::= ENUMERATED

{

 normalRelease(1),

 authenticationFailure(2),

 deregister(3),

 unspecified(4)

}

CauseProtocol ::= ENUMERATED

{

 transferSyntaxError(1),

 abstractSyntaxError-reject(2),

 abstractSyntaxErrorIgnoreAndNotify(3),

 messageNotCompatibleWithReceiverState(4),

 semanticError(5),

 abstractSyntaxErrorFalselyConstructedMessage(6),

 unspecified(7)

}

CauseRadioNetwork ::= ENUMERATED

{

 unspecified(1),

 txnrelocoverallExpiry(2),

 successfulHandover(3),

 releaseDueToNGRANGeneratedReason(4),

 releaseDueTo5gcGeneratedReason(5),

 handoverCancelled(6),

 partialHandover(7),

 hoFailureInTarget5GCNGRANNodeOrTargetSystem(8),

 hoTargetNotAllowed(9),

 tNGRelocOverallExpiry(10),

 tNGRelocPrepExpiry(11),

 cellNotAvailable(12),

 unknownTargetID(13),

 noRadioResourcesAvailableInTargetCell(14),

 unknownLocalUENGAPID(15),

 inconsistentRemoteUENGAPID(16),

 handoverDesirableForRadioReason(17),

 timeCriticalHandover(18),

 resourceOptimisationHandover(19),

 reduceLoadInServingCell(20),

 userInactivity(21),

 radioConnectionWithUELost(22),

 radioResourcesNotAvailable(23),

 invalidQoSCombination(24),

 failureInRadioInterfaceProcedure(25),

 interactionWithOtherProcedure(26),

 unknownPDUSessionID(27),

 multiplePDUSessionIDInstances(29),

 multipleQoSFlowIDInstances(30),

 encryptionAndOrIntegrityProtectionAlgorithmsNotSupported(31),

 nGIntraSystemHandoverTriggered(32),

 nGInterSystemHandoverTriggered(33),

 xNHandoverTriggered(34),

 notSupported5QIValue(35),

 uEContextTransfer(36),

 iMSVoiceeEPSFallbackOrRATFallbackTriggered(37),

 uPIntegrityProtectioNotPossible(38),

 uPConfidentialityProtectionNotPossible(39),

 sliceNotSupported(40),

 uEInRRCInactiveStateNotReachable(41),

 redirection(42),

 resourcesNotAvailableForTheSlice(43),

 uEMaxIntegrityProtectedDataRateReason(44),

 releaseDueToCNDetectedMobility(45),

 n26InterfaceNotAvailable(46),

 releaseDueToPreemption(47),

 multipleLocationReportingReferenceIDInstances(48),

 rSNNotAvailableForTheUP(49),

 nPMAccessDenied(50),

 cAGOnlyAccessDenied(51),

 insufficientUECapabilities(52)

}

CauseTransport ::= ENUMERATED

{

 transportResourceUnavailable(1),

 unspecified(2)

}

Direction ::= ENUMERATED

{

 fromTarget(1),

 toTarget(2)

}

DNN ::= UTF8String

E164Number ::= NumericString (SIZE(1..15))

EmailAddress ::= UTF8String

EquivalentPLMNs ::= SEQUENCE (SIZE(1..MAX)) OF PLMNID

EUI64 ::= OCTET STRING (SIZE(8))

EUTRAEncryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

EUTRAIntegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

FiveGGUTI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 aMFRegionID [3] AMFRegionID,

 aMFSetID [4] AMFSetID,

 aMFPointer [5] AMFPointer,

 fiveGTMSI [6] FiveGTMSI

}

FiveGMMCause ::= INTEGER (0..255)

FiveGSSubscriberID ::= CHOICE

{

 sUPI [1] SUPI,

 sUCI [2] SUCI,

 pEI [3] PEI,

 gPSI [4] GPSI

}

FiveGSSubscriberIDs ::= SEQUENCE

{

 fiveGSSubscriberID [1] SEQUENCE SIZE(1..MAX) OF FiveGSSubscriberID

}

FiveGSMRequestType ::= ENUMERATED

{

 initialRequest(1),

 existingPDUSession(2),

 initialEmergencyRequest(3),

 existingEmergencyPDUSession(4),

 modificationRequest(5),

 reserved(6),

 mAPDURequest(7)

}

FiveGSMCause ::= INTEGER (0..255)

FiveGTMSI ::= INTEGER (0..4294967295)

FiveGSRVCCInfo ::= SEQUENCE

{

 uE5GSRVCCCapability [1] BOOLEAN,

 sessionTransferNumber [2] UTF8String OPTIONAL,

 correlationMSISDN [3] MSISDN OPTIONAL

}

FiveGSUserStateInfo ::= SEQUENCE

{

 fiveGSUserState [1] FiveGSUserState,

 accessType [2] AccessType

}

FiveGSUserState ::= ENUMERATED

{

 deregistered(1),

 registeredNotReachableForPaging(2),

 registeredReachableForPaging(3),

 connectedNotReachableForPaging(4),

 connectedReachableForPaging(5),

 notProvidedFromAMF(6)

}

FiveQI ::= INTEGER (0..255)

ForbiddenAreaInformation ::= SEQUENCE

{

 pLMNIdentity [1] PLMNID,

 forbiddenTACs [2] ForbiddenTACs

}

ForbiddenTACs ::= SEQUENCE (SIZE(1..MAX)) OF TAC

FTEID ::= SEQUENCE

{

 tEID [1] INTEGER (0.. 4294967295),

 iPv4Address [2] IPv4Address OPTIONAL,

 iPv6Address [3] IPv6Address OPTIONAL

}

GPSI ::= CHOICE

{

 mSISDN [1] MSISDN,

 nAI [2] NAI

}

GUAMI ::= SEQUENCE

{

 aMFID [1] AMFID,

 pLMNID [2] PLMNID

}

GUMMEI ::= SEQUENCE

{

 mMEID [1] MMEID,

 mCC [2] MCC,

 mNC [3] MNC

}

GUTI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 mMEGroupID [3] MMEGroupID,

 mMECode [4] MMECode,

 mTMSI [5] TMSI

}

HandoverCause ::= CHOICE

{

 radioNetwork [1] CauseRadioNetwork,

 transport [2] CauseTransport,

 nas [3] CauseNas,

 protocol [4] CauseProtocol,

 misc [5] CauseMisc

}

HandoverType ::= ENUMERATED

{

 intra5GS(1),

 fiveGStoEPS(2),

 ePSto5GS(3),

 fiveGStoUTRA(4)

}

HomeNetworkPublicKeyID ::= OCTET STRING

HSMFURI ::= UTF8String

IABAuthorizedIndicator ::= ENUMERATED

{

 authorized(1),

 notAuthorized(2)

}

IMEI ::= NumericString (SIZE(14))

IMEISV ::= NumericString (SIZE(16))

IMPI ::= NAI

IMPU ::= CHOICE

{

 sIPURI [1] SIPURI,

 tELURI [2] TELURI

}

IMSI ::= NumericString (SIZE(6..15))

Initiator ::= ENUMERATED

{

 uE(1),

 network(2),

 unknown(3)

}

IPAddress ::= CHOICE

{

 iPv4Address [1] IPv4Address,

 iPv6Address [2] IPv6Address

}

IPv4Address ::= OCTET STRING (SIZE(4))

IPv6Address ::= OCTET STRING (SIZE(16))

IPv6FlowLabel ::= INTEGER(0..1048575)

LocationAreaOfInterestList ::= SEQUENCE (SIZE(1..MAX)) OF AreaOfInterestItem

LocationEventType ::= ENUMERATED

{

 direct(1),

 changeOfServeCell(2),

 uEPrescenceInAreaOfInterest(3),

 stopChangeOfServeCell(4),

 stopUEPresenceInAreaOfInterest(5),

 cancelLocationReportingForTheUE(6)

}

LocationReportArea ::= ENUMERATED

{

 cell(1)

}

LocationReportingRequestType ::= SEQUENCE

{

 eventType [1] LocationEventType,

 reportArea [2] LocationReportArea,

 areaOfInterestList [3] LocationAreaOfInterestList

}

LTEV2XAuthorizedIndicator ::= SEQUENCE

{

 vehicleUE [1] VehicleUE,

 pedestrianUE [2] PedestrianUE

}

MACAddress ::= OCTET STRING (SIZE(6))

MACRestrictionIndicator ::= ENUMERATED

{

 noResrictions(1),

 mACAddressNotUseableAsEquipmentIdentifier(2),

 unknown(3)

}

MCC ::= NumericString (SIZE(3))

MNC ::= NumericString (SIZE(2..3))

MMEID ::= SEQUENCE

{

 mMEGI [1] MMEGI,

 mMEC [2] MMEC

}

MMEC ::= NumericString

MMEGI ::= NumericString

MobilityRestrictionList ::= SEQUENCE

{

 servingPLMN [1] PLMNID,

 equivalentPLMNs [2] EquivalentPLMNs OPTIONAL,

 rATRestrictions [3] RATRestrictions OPTIONAL,

 forbiddenAreaInformation [4] ForbiddenAreaInformation OPTIONAL,

 serviceAreaInformation [5] ServiceAreaInformation OPTIONAL

}

MSISDN ::= NumericString (SIZE(1..15))

NAI ::= UTF8String

NextHopChainingCount ::= INTEGER (0..7)

NextLayerProtocol ::= INTEGER(0..255)

NonLocalID ::= ENUMERATED

{

 local(1),

 nonLocal(2)

}

NonIMEISVPEI ::= CHOICE

{

 mACAddress [1] MACAddress

}

NPNAccessInformation ::= CHOICE

{

 pNINPNAccessInformation [1] CellCAGList

}

NREncryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRIntegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRV2XAuthorizedIndicator ::= SEQUENCE

{

 vehicleUE [1] VehicleUE,

 pedestrianUE [2] PedestrianUE

}

NSSAI ::= SEQUENCE OF SNSSAI

PC5QoSFlowItem ::= SEQUENCE

{

 pQI [1] FiveQI,

 pC5QoSFlowBitRate [2] BitRate OPTIONAL

}

PC5QoSFlowList ::= SEQUENCE (SIZE(1..MAX)) OF PC5QoSFlowItem

PC5QoSParameters ::= SEQUENCE

{

 pC5QoSFlowList [1] PC5QoSFlowList,

 pC5LinkAMBR [2] BitRate OPTIONAL

}

PLMNID ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC

}

PLMNList ::= SEQUENCE (SIZE(1..MAX)) OF PLMNID

PDUSessionID ::= INTEGER (0..255)

PDUSessionResourceInformation ::= SEQUENCE

{

 pDUSessionID [1] PDUSessionID

}

PDUSessionType ::= ENUMERATED

{

 iPv4(1),

 iPv6(2),

 iPv4v6(3),

 unstructured(4),

 ethernet(5)

}

PedestrianUE ::= ENUMERATED

{

 authorized(1),

 notAuthorized(2)

}

PEI ::= CHOICE

{

 iMEI [1] IMEI,

 iMEISV [2] IMEISV,

 mACAddress [3] MACAddress,

 eUI64 [4] EUI64

}

PortNumber ::= INTEGER (0..65535)

PrimaryAuthenticationType ::= ENUMERATED

{

 eAPAKAPrime(1),

 fiveGAKA(2),

 eAPTLS(3),

 none(4),

 ePSAKA(5),

 eAPAKA(6),

 iMSAKA(7),

 gBAAKA(8),

 uMTSAKA(9)

}

ProtectionSchemeID ::= INTEGER (0..15)

RANUENGAPID ::= INTEGER (0..4294967295)

-- see Clause 9.3.1.20 of TS 38.413[23] for details

RANSourceToTargetContainer ::= OCTET STRING

-- see Clause 9.3.1.21 of TS 38.413[23] for details

RANTargetToSourceContainer ::= OCTET STRING

RATRestrictions ::= SEQUENCE (SIZE(1..MAX)) OF RATRestrictionItem

RATRestrictionInformation ::= BIT STRING (SIZE(8, ...))

RATRestrictionItem ::= SEQUENCE

{

 pLMNIdentity [1] PLMNID,

 rATRestrictionInformation [2] RATRestrictionInformation

}

RATType ::= ENUMERATED

{

 nR(1),

 eUTRA(2),

 wLAN(3),

 virtual(4),

 nBIOT(5),

 wireline(6),

 wirelineCable(7),

 wirelineBBF(8),

 lTEM(9),

 nRU(10),

 eUTRAU(11),

 trustedN3GA(12),

 trustedWLAN(13),

 uTRA(14),

 gERA(15),

 nRLEO(16),

 nRMEO(17),

 nRGEO(18),

 nROTHERSAT(19),

 nRREDCAP(20)

}

REDCAPIndication ::= ENUMERATED

{

 redcap(1)

}

RejectedNSSAI ::= SEQUENCE OF RejectedSNSSAI

RejectedSNSSAI ::= SEQUENCE

{

 causeValue [1] RejectedSliceCauseValue,

 sNSSAI [2] SNSSAI

}

RejectedSliceCauseValue ::= INTEGER (0..255)

ReRegRequiredIndicator ::= ENUMERATED

{

 reRegistrationRequired(1),

 reRegistrationNotRequired(2)

}

RoutingIndicator ::= INTEGER (0..9999)

SchemeOutput ::= OCTET STRING

SecurityContext ::= SEQUENCE

{

 nextHopChainingCount [1] NextHopChainingCount,

 nextHopNH [2] SecurityKey

}

SecurityKey ::= BIT STRING (SIZE(256))

ServiceAreaInformation ::= SEQUENCE (SIZE(1..MAX)) OF ServiceAreaInfo

ServiceAreaInfo ::= SEQUENCE

{

 pLMNIdentity [1] PLMNID,

 allowedTACs [2] AllowedTACs OPTIONAL,

 notAllowedTACs [3] ForbiddenTACs OPTIONAL

}

SIPURI ::= UTF8String

Slice ::= SEQUENCE

{

 allowedNSSAI [1] NSSAI OPTIONAL,

 configuredNSSAI [2] NSSAI OPTIONAL,

 rejectedNSSAI [3] RejectedNSSAI OPTIONAL

}

SMPDUDNRequest ::= OCTET STRING

-- TS 24.501 [13], clause 9.11.3.6.1

SMSOverNASIndicator ::= ENUMERATED

{

 sMSOverNASNotAllowed(1),

 sMSOverNASAllowed(2)

}

SNSSAI ::= SEQUENCE

{

 sliceServiceType [1] INTEGER (0..255),

 sliceDifferentiator [2] OCTET STRING (SIZE(3)) OPTIONAL

}

SRVCCOperation ::= ENUMERATED

{

 possible(1),

 notPossible(2)

}

SubscriberIdentifier ::= CHOICE

{

 sUCI [1] SUCI,

 sUPI [2] SUPI

}

SUCI ::= SEQUENCE

{

 mCC [1] MCC,

 mNC [2] MNC,

 routingIndicator [3] RoutingIndicator,

 protectionSchemeID [4] ProtectionSchemeID,

 homeNetworkPublicKeyID [5] HomeNetworkPublicKeyID,

 schemeOutput [6] SchemeOutput,

 routingIndicatorLength [7] INTEGER (1..4) OPTIONAL

 -- shall be included if different from the number of meaningful digits given

 -- in routingIndicator

}

SUPI ::= CHOICE

{

 iMSI [1] IMSI,

 nAI [2] NAI

}

SUPIUnauthenticatedIndication ::= BOOLEAN

SwitchOffIndicator ::= ENUMERATED

{

 normalDetach(1),

 switchOff(2)

}

TargetIdentifier ::= CHOICE

{

 sUPI [1] SUPI,

 iMSI [2] IMSI,

 pEI [3] PEI,

 iMEI [4] IMEI,

 gPSI [5] GPSI,

 mSISDN [6] MSISDN,

 nAI [7] NAI,

 iPv4Address [8] IPv4Address,

 iPv6Address [9] IPv6Address,

 ethernetAddress [10] MACAddress

}

TargetIdentifierProvenance ::= ENUMERATED

{

 lEAProvided(1),

 observed(2),

 matchedOn(3),

 other(4)

}

TELURI ::= UTF8String

Timestamp ::= GeneralizedTime

TypeOfError ::= ENUMERATED

{

 notunderstood(1),

 missing(2),

 other(3)

}

TypeOfMessage ::= ENUMERATED

{

 initiatingMessage(1),

 successfulOutcome(2),

 unsuccessfulOutcome(3),

 other(4)

}

UEContextInfo ::= SEQUENCE

{

 supportVoPS [1] BOOLEAN OPTIONAL,

 supportVoPSNon3GPP [2] BOOLEAN OPTIONAL,

 lastActiveTime [3] Timestamp OPTIONAL,

 accessType [4] AccessType OPTIONAL,

 rATType [5] RATType OPTIONAL

}

UEEndpointAddress ::= CHOICE

{

 iPv4Address [1] IPv4Address,

 iPv6Address [2] IPv6Address,

 ethernetAddress [3] MACAddress

}

UERadioCapability ::= OCTET STRING

UESecurityCapabilities ::= SEQUENCE

{

 nREncryptionAlgorithms [1] NREncryptionAlgorithms,

 nRIntegrityProtectionAlgorithms [2] NRIntegrityProtectionAlgorithms,

 eUTRAEncryptionAlgorithms [3] EUTRAEncryptionAlgorithms,

 eUTRAIntegrityProtectionAlgorithms [4] EUTRAIntegrityProtectionAlgorithms

}

UserIdentifiers ::= SEQUENCE

{

 fiveGSSubscriberIDs [1] FiveGSSubscriberIDs OPTIONAL,

 ePSSubscriberIDs [2] EPSSubscriberIDs OPTIONAL,

 targetIdentifiers [3] TargetIdentifier

}

VehicleUE ::= ENUMERATED

{

 authorized(1),

 notAuthorized(2)

}

VoiceEPSFallback ::= ENUMERATED

{

 possible(1),

 notPossible(2)

}

-- ===================

-- Location parameters

-- ===================

Location ::= SEQUENCE

{

 locationInfo [1] LocationInfo OPTIONAL,

 positioningInfo [2] PositioningInfo OPTIONAL,

 locationPresenceReport [3] LocationPresenceReport OPTIONAL,

 ePSLocationInfo [4] EPSLocationInfo OPTIONAL

}

CellSiteInformation ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 azimuth [2] INTEGER (0..359) OPTIONAL,

 operatorSpecificInformation [3] UTF8String OPTIONAL

}

-- TS 29.518 [22], clause 6.4.6.2.6

LocationInfo ::= SEQUENCE

{

 userLocation [1] UserLocation OPTIONAL,

 currentLoc [2] BOOLEAN OPTIONAL,

 geoInfo [3] GeographicArea OPTIONAL,

 rATType [4] RATType OPTIONAL,

 timeZone [5] TimeZone OPTIONAL,

 additionalCellIDs [6] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.7

UserLocation ::= SEQUENCE

{

 eUTRALocation [1] EUTRALocation OPTIONAL,

 nRLocation [2] NRLocation OPTIONAL,

 n3GALocation [3] N3GALocation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.8

EUTRALocation ::= SEQUENCE

{

 tAI [1] TAI,

 eCGI [2] ECGI,

 ageOfLocationInfo [3] INTEGER OPTIONAL,

 uELocationTimestamp [4] Timestamp OPTIONAL,

 geographicalInformation [5] UTF8String OPTIONAL,

 geodeticInformation [6] UTF8String OPTIONAL,

 globalNGENbID [7] GlobalRANNodeID OPTIONAL,

 cellSiteInformation [8] CellSiteInformation OPTIONAL,

 globalENbID [9] GlobalRANNodeID OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.9

NRLocation ::= SEQUENCE

{

 tAI [1] TAI,

 nCGI [2] NCGI,

 ageOfLocationInfo [3] INTEGER OPTIONAL,

 uELocationTimestamp [4] Timestamp OPTIONAL,

 geographicalInformation [5] UTF8String OPTIONAL,

 geodeticInformation [6] UTF8String OPTIONAL,

 globalGNbID [7] GlobalRANNodeID OPTIONAL,

 cellSiteInformation [8] CellSiteInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.10

N3GALocation ::= SEQUENCE

{

 tAI [1] TAI OPTIONAL,

 n3IWFID [2] N3IWFIDNGAP OPTIONAL,

 uEIPAddr [3] IPAddr OPTIONAL,

 portNumber [4] INTEGER OPTIONAL,

 tNAPID [5] TNAPID OPTIONAL,

 tWAPID [6] TWAPID OPTIONAL,

 hFCNodeID [7] HFCNodeID OPTIONAL,

 gLI [8] GLI OPTIONAL,

 w5GBANLineType [9] W5GBANLineType OPTIONAL,

 gCI [10] GCI OPTIONAL,

 ageOfLocationInfo [11] INTEGER OPTIONAL,

 uELocationTimestamp [12] Timestamp OPTIONAL,

 protocol [13] TransportProtocol OPTIONAL

}

-- TS 38.413 [23], clause 9.3.2.4

IPAddr ::= SEQUENCE

{

 iPv4Addr [1] IPv4Address OPTIONAL,

 iPv6Addr [2] IPv6Address OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.28

GlobalRANNodeID ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 aNNodeID [2] ANNodeID,

 nID [3] NID OPTIONAL

}

ANNodeID ::= CHOICE

{

 n3IWFID [1] N3IWFIDSBI,

 gNbID [2] GNbID,

 nGENbID [3] NGENbID,

 eNbID [4] ENbID,

 wAGFID [5] WAGFID,

 tNGFID [6] TNGFID

}

-- TS 38.413 [23], clause 9.3.1.6

GNbID ::= BIT STRING(SIZE(22..32))

-- TS 29.571 [17], clause 5.4.4.4

TAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 tAC [2] TAC,

 nID [3] NID OPTIONAL

}

CGI ::= SEQUENCE

{

 lAI [1] LAI,

 cellID [2] CellID

}

LAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 lAC [2] LAC

}

LAC ::= OCTET STRING (SIZE(2))

CellID ::= OCTET STRING (SIZE(2))

SAI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 lAC [2] LAC,

 sAC [3] SAC

}

SAC ::= OCTET STRING (SIZE(2))

-- TS 29.571 [17], clause 5.4.4.5

ECGI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 eUTRACellID [2] EUTRACellID,

 nID [3] NID OPTIONAL

}

TAIList ::= SEQUENCE OF TAI

-- TS 29.571 [17], clause 5.4.4.6

NCGI ::= SEQUENCE

{

 pLMNID [1] PLMNID,

 nRCellID [2] NRCellID,

 nID [3] NID OPTIONAL

}

RANCGI ::= CHOICE

{

 eCGI [1] ECGI,

 nCGI [2] NCGI

}

CellInformation ::= SEQUENCE

{

 rANCGI [1] RANCGI,

 cellSiteinformation [2] CellSiteInformation OPTIONAL,

 timeOfLocation [3] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.1.57

N3IWFIDNGAP ::= BIT STRING (SIZE(16))

-- TS 29.571 [17], clause 5.4.4.28

N3IWFIDSBI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

TNGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

WAGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62

TNAPID ::= SEQUENCE

{

 sSID [1] SSID OPTIONAL,

 bSSID [2] BSSID OPTIONAL,

 civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.64

TWAPID ::= SEQUENCE

{

 sSID [1] SSID OPTIONAL,

 bSSID [2] BSSID OPTIONAL,

 civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

SSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

BSSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.36 and table 5.4.2-1

HFCNodeID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

GLI ::= OCTET STRING (SIZE(0..150))

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

GCI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.3.38

TransportProtocol ::= ENUMERATED

{

 uDP(1),

 tCP(2)

}

-- TS 29.571 [17], clause 5.4.4.10 and clause 5.4.3.33

W5GBANLineType ::= ENUMERATED

{

 dSL(1),

 pON(2)

}

-- TS 29.571 [17], table 5.4.2-1

TAC ::= OCTET STRING (SIZE(2..3))

-- TS 38.413 [23], clause 9.3.1.9

EUTRACellID ::= BIT STRING (SIZE(28))

-- TS 38.413 [23], clause 9.3.1.7

NRCellID ::= BIT STRING (SIZE(36))

-- TS 38.413 [23], clause 9.3.1.8

NGENbID ::= CHOICE

{

 macroNGENbID [1] BIT STRING (SIZE(20)),

 shortMacroNGENbID [2] BIT STRING (SIZE(18)),

 longMacroNGENbID [3] BIT STRING (SIZE(21))

}

-- TS 23.003 [19], clause 12.7.1 encoded as per TS 29.571 [17], clause 5.4.2

NID ::= UTF8String (SIZE(11))

-- TS 36.413 [38], clause 9.2.1.37

ENbID ::= CHOICE

{

 macroENbID [1] BIT STRING (SIZE(20)),

 homeENbID [2] BIT STRING (SIZE(28)),

 shortMacroENbID [3] BIT STRING (SIZE(18)),

 longMacroENbID [4] BIT STRING (SIZE(21))

}

-- TS 29.518 [22], clause 6.4.6.2.3

PositioningInfo ::= SEQUENCE

{

 positionInfo [1] LocationData OPTIONAL,

 rawMLPResponse [2] RawMLPResponse OPTIONAL

}

RawMLPResponse ::= CHOICE

{

 -- The following parameter contains a copy of unparsed XML code of the

 -- MLP response message, i.e. the entire XML document containing

 -- a <slia> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.2) or

 -- a <slirep> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.3) MLP message.

 mLPPositionData [1] UTF8String,

 -- OMA MLP result id, defined in OMA-TS-MLP-V3\_5-20181211-C [20], Clause 5.4

 mLPErrorCode [2] INTEGER (1..699)

}

-- TS 29.572 [24], clause 6.1.6.2.3

LocationData ::= SEQUENCE

{

 locationEstimate [1] GeographicArea,

 accuracyFulfilmentIndicator [2] AccuracyFulfilmentIndicator OPTIONAL,

 ageOfLocationEstimate [3] AgeOfLocationEstimate OPTIONAL,

 velocityEstimate [4] VelocityEstimate OPTIONAL,

 civicAddress [5] CivicAddress OPTIONAL,

 positioningDataList [6] SET OF PositioningMethodAndUsage OPTIONAL,

 gNSSPositioningDataList [7] SET OF GNSSPositioningMethodAndUsage OPTIONAL,

 eCGI [8] ECGI OPTIONAL,

 nCGI [9] NCGI OPTIONAL,

 altitude [10] Altitude OPTIONAL,

 barometricPressure [11] BarometricPressure OPTIONAL

}

-- TS 29.172 [53], table 6.2.2-2

EPSLocationInfo ::= SEQUENCE

{

 locationData [1] LocationData,

 cGI [2] CGI OPTIONAL,

 sAI [3] SAI OPTIONAL,

 eSMLCCellInfo [4] ESMLCCellInfo OPTIONAL

}

-- TS 29.172 [53], clause 7.4.57

ESMLCCellInfo ::= SEQUENCE

{

 eCGI [1] ECGI,

 cellPortionID [2] CellPortionID

}

-- TS 29.171 [54], clause 7.4.31

CellPortionID ::= INTEGER (0..4095)

-- TS 29.518 [22], clause 6.2.6.2.5

LocationPresenceReport ::= SEQUENCE

{

 type [1] AMFEventType,

 timestamp [2] Timestamp,

 areaList [3] SET OF AMFEventArea OPTIONAL,

 timeZone [4] TimeZone OPTIONAL,

 accessTypes [5] SET OF AccessType OPTIONAL,

 rMInfoList [6] SET OF RMInfo OPTIONAL,

 cMInfoList [7] SET OF CMInfo OPTIONAL,

 reachability [8] UEReachability OPTIONAL,

 location [9] UserLocation OPTIONAL,

 additionalCellIDs [10] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.3.3

AMFEventType ::= ENUMERATED

{

 locationReport(1),

 presenceInAOIReport(2)

}

-- TS 29.518 [22], clause 6.2.6.2.16

AMFEventArea ::= SEQUENCE

{

 presenceInfo [1] PresenceInfo OPTIONAL,

 lADNInfo [2] LADNInfo OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.27

PresenceInfo ::= SEQUENCE

{

 presenceState [1] PresenceState OPTIONAL,

 trackingAreaList [2] SET OF TAI OPTIONAL,

 eCGIList [3] SET OF ECGI OPTIONAL,

 nCGIList [4] SET OF NCGI OPTIONAL,

 globalRANNodeIDList [5] SET OF GlobalRANNodeID OPTIONAL,

 globalENbIDList [6] SET OF GlobalRANNodeID OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.2.17

LADNInfo ::= SEQUENCE

{

 lADN [1] UTF8String,

 presence [2] PresenceState OPTIONAL

}

-- TS 29.571 [17], clause 5.4.3.20

PresenceState ::= ENUMERATED

{

 inArea(1),

 outOfArea(2),

 unknown(3),

 inactive(4)

}

-- TS 29.518 [22], clause 6.2.6.2.8

RMInfo ::= SEQUENCE

{

 rMState [1] RMState,

 accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.2.9

CMInfo ::= SEQUENCE

{

 cMState [1] CMState,

 accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.3.7

UEReachability ::= ENUMERATED

{

 unreachable(1),

 reachable(2),

 regulatoryOnly(3)

}

-- TS 29.518 [22], clause 6.2.6.3.9

RMState ::= ENUMERATED

{

 registered(1),

 deregistered(2)

}

-- TS 29.518 [22], clause 6.2.6.3.10

CMState ::= ENUMERATED

{

 idle(1),

 connected(2)

}

-- TS 29.572 [24], clause 6.1.6.2.5

GeographicArea ::= CHOICE

{

 point [1] Point,

 pointUncertaintyCircle [2] PointUncertaintyCircle,

 pointUncertaintyEllipse [3] PointUncertaintyEllipse,

 polygon [4] Polygon,

 pointAltitude [5] PointAltitude,

 pointAltitudeUncertainty [6] PointAltitudeUncertainty,

 ellipsoidArc [7] EllipsoidArc

}

-- TS 29.572 [24], clause 6.1.6.3.12

AccuracyFulfilmentIndicator ::= ENUMERATED

{

 requestedAccuracyFulfilled(1),

 requestedAccuracyNotFulfilled(2)

}

-- TS 29.572 [24], clause 6.1.6.2.17

VelocityEstimate ::= CHOICE

{

 horVelocity [1] HorizontalVelocity,

 horWithVertVelocity [2] HorizontalWithVerticalVelocity,

 horVelocityWithUncertainty [3] HorizontalVelocityWithUncertainty,

 horWithVertVelocityAndUncertainty [4] HorizontalWithVerticalVelocityAndUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.14

CivicAddress ::= SEQUENCE

{

 country [1] UTF8String,

 a1 [2] UTF8String OPTIONAL,

 a2 [3] UTF8String OPTIONAL,

 a3 [4] UTF8String OPTIONAL,

 a4 [5] UTF8String OPTIONAL,

 a5 [6] UTF8String OPTIONAL,

 a6 [7] UTF8String OPTIONAL,

 prd [8] UTF8String OPTIONAL,

 pod [9] UTF8String OPTIONAL,

 sts [10] UTF8String OPTIONAL,

 hno [11] UTF8String OPTIONAL,

 hns [12] UTF8String OPTIONAL,

 lmk [13] UTF8String OPTIONAL,

 loc [14] UTF8String OPTIONAL,

 nam [15] UTF8String OPTIONAL,

 pc [16] UTF8String OPTIONAL,

 bld [17] UTF8String OPTIONAL,

 unit [18] UTF8String OPTIONAL,

 flr [19] UTF8String OPTIONAL,

 room [20] UTF8String OPTIONAL,

 plc [21] UTF8String OPTIONAL,

 pcn [22] UTF8String OPTIONAL,

 pobox [23] UTF8String OPTIONAL,

 addcode [24] UTF8String OPTIONAL,

 seat [25] UTF8String OPTIONAL,

 rd [26] UTF8String OPTIONAL,

 rdsec [27] UTF8String OPTIONAL,

 rdbr [28] UTF8String OPTIONAL,

 rdsubbr [29] UTF8String OPTIONAL,

 prm [30] UTF8String OPTIONAL,

 pom [31] UTF8String OPTIONAL

}

-- TS 29.571 [17], clauses 5.4.4.62 and 5.4.4.64

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

CivicAddressBytes ::= OCTET STRING

-- TS 29.572 [24], clause 6.1.6.2.15

PositioningMethodAndUsage ::= SEQUENCE

{

 method [1] PositioningMethod,

 mode [2] PositioningMode,

 usage [3] Usage,

 methodCode [4] MethodCode OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.16

GNSSPositioningMethodAndUsage ::= SEQUENCE

{

 mode [1] PositioningMode,

 gNSS [2] GNSSID,

 usage [3] Usage

}

-- TS 29.572 [24], clause 6.1.6.2.6

Point ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.7

PointUncertaintyCircle ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 uncertainty [2] Uncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.8

PointUncertaintyEllipse ::= SEQUENCE

{

 geographicalCoordinates [1] GeographicalCoordinates,

 uncertainty [2] UncertaintyEllipse,

 confidence [3] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.9

Polygon ::= SEQUENCE

{

 pointList [1] SET SIZE (3..15) OF GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.10

PointAltitude ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 altitude [2] Altitude

}

-- TS 29.572 [24], clause 6.1.6.2.11

PointAltitudeUncertainty ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 altitude [2] Altitude,

 uncertaintyEllipse [3] UncertaintyEllipse,

 uncertaintyAltitude [4] Uncertainty,

 confidence [5] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.12

EllipsoidArc ::= SEQUENCE

{

 point [1] GeographicalCoordinates,

 innerRadius [2] InnerRadius,

 uncertaintyRadius [3] Uncertainty,

 offsetAngle [4] Angle,

 includedAngle [5] Angle,

 confidence [6] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.4

GeographicalCoordinates ::= SEQUENCE

{

 latitude [1] UTF8String,

 longitude [2] UTF8String,

 mapDatumInformation [3] OGCURN OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.22

UncertaintyEllipse ::= SEQUENCE

{

 semiMajor [1] Uncertainty,

 semiMinor [2] Uncertainty,

 orientationMajor [3] Orientation

}

-- TS 29.572 [24], clause 6.1.6.2.18

HorizontalVelocity ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle

}

-- TS 29.572 [24], clause 6.1.6.2.19

HorizontalWithVerticalVelocity ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle,

 vSpeed [3] VerticalSpeed,

 vDirection [4] VerticalDirection

}

-- TS 29.572 [24], clause 6.1.6.2.20

HorizontalVelocityWithUncertainty ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle,

 uncertainty [3] SpeedUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.21

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE

{

 hSpeed [1] HorizontalSpeed,

 bearing [2] Angle,

 vSpeed [3] VerticalSpeed,

 vDirection [4] VerticalDirection,

 hUncertainty [5] SpeedUncertainty,

 vUncertainty [6] SpeedUncertainty

}

-- The following types are described in TS 29.572 [24], table 6.1.6.3.2-1

Altitude ::= UTF8String

Angle ::= INTEGER (0..360)

Uncertainty ::= INTEGER (0..127)

Orientation ::= INTEGER (0..180)

Confidence ::= INTEGER (0..100)

InnerRadius ::= INTEGER (0..65535)

AgeOfLocationEstimate ::= INTEGER (0..32767)

HorizontalSpeed ::= UTF8String

VerticalSpeed ::= UTF8String

SpeedUncertainty ::= UTF8String

BarometricPressure ::= INTEGER (30000..155000)

-- TS 29.572 [24], clause 6.1.6.3.13

VerticalDirection ::= ENUMERATED

{

 upward(1),

 downward(2)

}

-- TS 29.572 [24], clause 6.1.6.3.6

PositioningMethod ::= ENUMERATED

{

 cellID(1),

 eCID(2),

 oTDOA(3),

 barometricPressure(4),

 wLAN(5),

 bluetooth(6),

 mBS(7),

 motionSensor(8),

 dLTDOA(9),

 dLAOD(10),

 multiRTT(11),

 nRECID(12),

 uLTDOA(13),

 uLAOA(14),

 networkSpecific(15)

}

-- TS 29.572 [24], clause 6.1.6.3.7

PositioningMode ::= ENUMERATED

{

 uEBased(1),

 uEAssisted(2),

 conventional(3)

}

-- TS 29.572 [24], clause 6.1.6.3.8

GNSSID ::= ENUMERATED

{

 gPS(1),

 galileo(2),

 sBAS(3),

 modernizedGPS(4),

 qZSS(5),

 gLONASS(6),

 bDS(7),

 nAVIC(8)

}

-- TS 29.572 [24], clause 6.1.6.3.9

Usage ::= ENUMERATED

{

 unsuccess(1),

 successResultsNotUsed(2),

 successResultsUsedToVerifyLocation(3),

 successResultsUsedToGenerateLocation(4),

 successMethodNotDetermined(5)

}

-- TS 29.571 [17], table 5.2.2-1

TimeZone ::= UTF8String

-- Open Geospatial Consortium URN [35]

OGCURN ::= UTF8String

-- TS 29.572 [24], clause 6.1.6.2.15

MethodCode ::= INTEGER (16..31)

END

END OF SECOND CHANGE

END OF ALL CHANGES