**3GPP TSG-SA5 Meeting #129-e *S5-201112***

**Online, , 24th Feb 2020 - 4th Mar 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.531** | **CR** | **0041** | **rev** | 1 | **Current version:** | **15.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Rel-15 CR 28.531 Network Slice Identifiction Fix Stage 2 and Stage 3 |
|  |  |
| ***Source to WG:*** | Samsung R&D Institute UK |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | NETSLICE-PRO\_NS |  | ***Date:*** | 2020-02-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Network Slice Instance ID and Network Slice Sub-net Instance ID is misspelled in AllocateNsi and AllocateNssi Operations |
|  |  |
| ***Summary of change:*** | Fixing the misspelled parameters |
|  |  |
| ***Consequences if not approved:*** | The specification remains ambigious making the entire concept worse |
|  |  |
| ***Clauses affected:*** | 6.5.1.3, 6.5.2.3, 6.5.3.2, 6.5.4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

### 6.5.1 AllocateNsi operation

#### 6.5.1.1 Description

This operation is invoked by allocateNsi operation service consumer to request the provider to allocate a network slice instance to satisfy network slice related requirements. The provider may create a new NSI or using existing NSI to satisfy the request.

#### 6.5.1.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| attributeListIn | M | LIST OF SEQUENCE< attribute name, attribute value> | This parameter specifies the network slice related requirements defined in ServiceProfile in Clause 6.3.3 in TS 28.541 [6]. |

#### 6.5.1.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| attributeListOut | M | LIST OF SEQUENCE< attribute name, attribute value> | This list of name/value pairs contains the attributes of the NSI which has been allocated and the actual value assigned to each.  |
| status | M | ENUM (OperationSucceeded, OperationFailed) | An operation may fail because of a specified or unspecified reason. |
| nSIId | M | An attribute uniquely identifies the network slice instance. | It specifies the unifique identifier of the NSI which has been allocated. |

### 6.5.2 AllocateNssi operation

#### 6.5.2.1 Description

This operation is invoked by allocateNssi operation service consumer to request the provider to allocate a network slice subnet instance to satisfy the network slice subnet related requirements. The provider may create a new NSSI or using existing NSSI to satisfy the request.

#### 6.5.2.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| attributeListIn | M | LIST OF SEQUENCE< attribute name, attribute value> | This parameter specifies the network slice subnet related requirements defined in SliceProfile in Clause 6.3.4 in TS 28.541 [6]. |

#### 6.5.2.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| attributeListOut | M | LIST OF SEQUENCE< attribute name, attribute value> | This list of name/value pairs contains the attributes of the NSSI which has been allocated and the actual value assigned to each.  |
| status | M | ENUM (OperationSucceeded, OperationFailed) | An operation may fail because of a specified or unspecified reason. |
| nSSIId | M | An attribute uniquely identifies the network slice subnet instance.  | It specifies the unifique identifier of the NSSI which has been allocated. |

### 6.5.3 DeallocateNsi operation

#### 6.5.3.1 Description

This operation is invoked by deallocateNsi operation service consumer to request the provider to deallocate a network slice instance since the NSI is no longer needed for the consumer. The provider may terminate the requested NSI or modify the requested NSI without termination to satisfy the request.

#### 6.5.3.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| nSIId | M | An attribute uniquely identifies the network slice instance. | It specifies the unifique identifier of the NSI which need to be deallocated. |

#### 6.5.3.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| status | M | ENUM (OperationSucceeded, OperationFailed) | An operation may fail because of a specified or unspecified reason. |

### 6.5.4 DeallocateNssi operation

#### 6.5.4.1 Description

This operation is invoked by deallocateNssi operation service consumer to request the provider to deallocate a network slice subnet instance since the NSSI is no longer needed for the consumer. The provider may terminate the requested NSSI or modify the requested NSSI without termination to satisfy the request.

#### 6.5.4.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| nSSIId | M | An attribute uniquely identifies the network slice subnet instance. | It specifies the unifique identifier of the NSSI which need to be deallocated. |

#### 6.5.4.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| status | M | ENUM (OperationSucceeded, OperationFailed) | An operation may fail because of a specified or unspecified reason. |

|  |
| --- |
| **1st Change End** |