**3GPP TSG-SA5 Meeting #129e *S5-201183rev1***

**e-meeting, 24 February – 4 March 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.552** | **CR** | **0192** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Add measurements related to DL delay between PSA UPF and UE | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Intel, ETRI | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_SLICE\_ePA | | | | |  | ***Date:*** | | | 2020-02-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The end to end UL delay in 5G networks between UE and PSA UPF has direct impact to users’ experience for some types of services (e.g., URLLC). In case the PSA UPF and NG-RAN are time synchronised, the UL delay between PSA UPF and UE can be measured at PSA UPF.  The measurements on the UL delay between PSA UPF and NE can be used to evaluate the user plane delay performance in 5G networks and users’ experience. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Added measurements on UL one way packet delay between PSA UPF and NG-RAN. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UL oacket delay between PSA UPF and NG-RAN cannot be monitored. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.x.y (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Implement the sub-clause 5.4.x.y of this CR to the clause 5.4.x of CR#1xx. | | | | | | | | |

|  |
| --- |
| **1st Modified Section** |

#### 5.4.x.y UL packet delay between PSA UPF and UE

##### 5.4.x.y.1 Average UL packet delay between PSA UPF and UE

a) This measurement provides the average UL packet delay between PSA UPF and UE. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy. For each received GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4]):

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The result of UL packet delay from UE to NG-RAN (including the delay within the NG-RAN and the delay on Uu interface and denoted by in the present document) received in the GTP-U header of the monitoring response packet;

- The 5QI and S-NSSAI associated to the GTP PDU monitoring response packet.

The PSA UPF counts the number (N) of GTP PDU monitoring response packets for each 5QI and each S-NSSAI respectively, and takes the following calculation for each 5QI and each S-NSSAI:

d) Each measurement is a real representing the average delay in microseconds.

e) GTP.DelayUlPsaUpfUeMean.*5QI, where 5QI* identifies the 5QI;   
GTP.DelayUlPsaUpfUeMean.*SNSSAI, where SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

##### 5.4.x.y.2 Distribution of UL packet delay between PSA UPF and UE

a) This measurement provides the distribution of UL packet delay between PSA UPF and UE. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy.

For each received GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4]):

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The result of UL packet delay from UE to NG-RAN (including the delay within the NG-RAN and the delay on Uu interface and denoted by in the present document) received in the GTP-U header of the monitoring response packet;

- The 5QI and S-NSSAI associated to the GTP PDU monitoring response packet.

The PSA UPF 1) takes the following calculation for each GTP PDU monitoring response packet (packet i) for each 5QI and each S-NSSAI respectively, and 2) increment the corresponding bin with the delay range where the result of 1) falls into by 1 for the subcounters per 5QI and subcounters per S-NSSAI.

d) Each measurement is an integer representing the number of GTP PDUs measured with the delay within the range of the bin.

e) GTP.DelayUlPsaUpfUeDist.*5QI.bin,* Where *Bin* indicates a delay range which is vendor specific, and *5QI* identifies the 5QI;   
GTP.DelayUlPsaUpfUeDist.*SNSSAI.bin,* Where *Bin* indicates a delay range which is vendor specific, and *SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

|  |
| --- |
| **End of Modified Sections** |