**3GPP TSG-SA5 Meeting #129e *S5-201218r1***

**e-meeting, 24 February – 4 March 2020**

**Source: Huawei**

**Title: Add message content**

**Document for: Approval**

**Agenda Item: 7.4.3**

# 1 Decision/action requested

***In this box give a very clear / short /concise statement of what is wanted.***

# 2 References

3GPP TS 28.201

# 3 Rationale

This contribution is to provide message content for network slice performance and analytics charging.

# 4 Detailed proposal

|  |
| --- |
| ***First change*** |

### 6.1.1 Message contents

#### 6.1.1.1 General

The Charging Data Request and Charging Data Response are specified in subclause 5.1.2.2.1 of TS 32.290 [57].

Table 6.1.1.1.1 describes the use of these messages for network slice performance and analytics charging.

Table 6.1.1.1.1: network slice performance and analytics charging messages reference table

|  |  |  |
| --- | --- | --- |
| **Message** | **Source** | **Destination** |
| Charging Data Request | CSIF | CHF |
| Charging Data Response | CHF | CSIF |

The following clauses describe the different fields used in the Charging Data messages and the category in the tables is used according to the charging data configuration defined in clause 5.4 of TS 32.240 [1]

|  |
| --- |
| **End of change** |