**3GPP TSG-SA5 Meeting #129-e *S5-201260***

**Online, , 24th Feb 2020 - 4th Mar 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** | **0246** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | SON\_5G |  | ***Date:*** | 2020-02-14 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In order to make the SON function more clear, ANR management policy IOC structure and ANR management control IOC are added.Since some attributes of ANR function belong to the gNB CU-CP, and some attributes belong to the cell. Therefore, two types of policy IOC are introducedIn addition, according to TS 38.300 subclase 15.3.3, ANR Management includes Intra-system ANR function and Inter-system ANR Function. Therefore, intra-system ANR Management Switch and inter-system ANR Management Switch are introduced. |
|  |  |
| ***Summary of change:*** | Add ANR Management policy IOC, ANR Management cell policy IOC and ANR Management control IOC structures.Add ANR Management Switch including intra-system ANR Management Switch and inter-system ANR Management Switch. |
|  |  |
| ***Consequences if not approved:*** | The function of ANR Management is not clear. |
|  |  |
| ***Clauses affected:*** | 4.3.2,4.3.32, 5.4.1, X, D.4.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First of Changes** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System".

[3] 3GPP TS 38.300: "NR; Overall description; Stage-2".

[4] 3GPP TS 38.401: "NG-RAN; Architecture description".

[5] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[6] 3GPP TS 38.420: "NG-RAN; Xn general aspects and principles".

[7] 3GPP TS 38.470: "NG-RAN; F1 general aspects and principles".

[8] 3GPP TS 38.473: "NG-RAN; F1 application protocol (F1AP)".

[9] 3GPP TS 37.340: "NR; Multi-connectivity; Overall description; Stage 2".

[10] 3GPP TS 28.540: "Management and orchestration; 5G Network Resource Model (NRM);Stage 1".

[11] 3GPP TS 28.662: "Telecommunication management; Generic Radio Access Network (RAN) Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS) ".

[12] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception".

[13] 3GPP TS 23.003: "Numbering, Addressing and Identification".

[14] 3GPP TS 36.410: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 general aspects and principles".

[15] 3GPP TS 36.423: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); X2 application protocol".

[16] 3GPP TS 36.425: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); X2 interface user plane protocol".

[17] 3GPP TS 28.625: "State Management Data Definition Integration Reference Point (IRP); Information Service (IS)".

[18] ITU-T Recommendation X.731: "Information technology - Open Systems Interconnection - Systems Management: State management function".

[19] 3GPP TS 28.658: "Telecommunications management; Evolved Universal Terrestrial Radio Access Network (E-UTRAN) Network Resource Model (NRM) Integration Reference Point (IRP): Information Service (IS)".

[20] 3GPP TS 28.702: "Core Network (CN) Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[21] 3GPP TS 28.708: "Telecommunication management; Evolved Packet Core (EPC) Network Resource Model (NRM) Integration Reference Point (IRP): Information Service (IS)".

[22] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[23] 3GPP TS 29.510: "5G system; Network Function Repository Services; Stage 3".

[24] 3GPP TS 29.531: "5G System; Network Slice Selection Services Stage 3".

[25] Void.

[26] 3GPP TS 28.531: "Management and orchestration; Provisioning".

[27] 3GPP TS 28.554: "Management and orchestration; 5G End to end Key Performance Indicators (KPI)".

[28] 3GPP TS 22.261: "Service requirements for next generation new services and markets".

[29] ETSI GS NFV-IFA 013 V2.4.1 (2018-02) "Network Function Virtualisation (NFV); Management and Orchestration; Os-Ma-nfvo Reference Point - Interface and Information Model Specification".

[30] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[31] Void.

[32] 3GPP TS 38.211: "NR; Physical channels and modulation".

[33] 3GPP TS 32.616: "Telecommunication management; Configuration Management (CM); Bulk CM Integration Reference Point (IRP); Solution Set (SS) definitions".

[34] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[35] 3GPP TS 28.532: "Management and orchestration; Management services".

[36] Void.

[37] IETF RFC 791: "Internet Protocol".

[38] IETF RFC 2373: "IP Version 6 Addressing Architecture".

[39] IEEE 802.1Q: "Media Access Control Bridges and Virtual Bridged Local Area Networks".

[40] ETSI GR NFV-IFA 015 (V2.4.1): "Network Function Virtualisation (NFV) Release 2; Management and Orchestration; Report on NFV Information Model".

[41] 3GPP TS 38.213: "NR; Physical layer procedures for control".

[42] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[43] 3GPP TS 32.156: "Telecommunication management; Fixed Mobile Convergence (FMC) model repertoire".

[44] IETF RFC 4122: "A Universally Unique IDentifier (UUID) URN Namespace".

[45] IETF RFC 8528: "YANG Schema Mount".

[46] IETF RFC 8340: "YANG Tree Diagrams".

[47] 3GPP TS 32.160: "Management and orchestration; Management Service Template".

[48] 3GPP TS 38.463: "NG-RAN; E1 application protocol (E1AP)".

[49] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in Idle mode and RRC Inactive state".

[50] GSMA NG.116 - Generic Network Slice Template Version 1.0 (2019-05-23).

[51] 3GPP TS 22.104: "Service requirements for cyber-physical control applications in vertical domains; Stage 1".

[52] 3GPP TS 33.501: " Security architecture and procedures for the 5G System".

[53] 3GPP TS 38.901: "Study on channel model for frequencies from 0.5 to 100 GHz ".

[54] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[55] 3GPP TS 38.215: "NR; Physical layer measurements".

[x] 3GPP TS 28.313: "Self-Organizing Networks (SON) for 5G networks”

|  |
| --- |
| **Second of Changes** |

## 4.2 Class diagram

### 4.2.1 Class diagram for gNB and en-gNB

#### 4.2.1.1 Relationships

This clause depicts the set of classes (e.g. IOCs) that encapsulates the information relevant for this gNB and en-gNB. For the UML semantics, see 3GPP TS 32.156 [43]. Subsequent clauses provide more detailed specification of various aspects of these classes.

The model fragments are for management representation of gNB and en-gNB for all NG-RAN deployment scenario as listed below.

- Non-split NG-RAN deployment senario, represents the gNB defined in TS 38.401[4].

- 2-split NG-RAN deployment scenario, represents the gNB consist of gNB-CU and gNB-DU defined in TS 38.401[4] clause 6.1.1.

- 3-split NG-RAN deployment scenario, represents the gNB consist of gNB-CU-CP, gNB-CU-UP and gNB-DU defined in TS 38.401[4] clause 6.1.2.



Figure 4.2.1.1-1: NRM for all deployment scenarios



Figure 4.2.1.1-2: NRM for EPs for all deployment scenarios



Figure 4.2.1.1-3: NRM for <<IOC>>NRSectorCarrier and <<IOC>>BWP for all deployment scenarios



Figure 4.2.1.1-4: Cell Relation view for all deployment scenarios

NOTE 1: The above NRM fragment uses SubNetwork to hold both NR and LTE external entities and frequencies.



Figure 4.2.1.1-5: Cell Relation view for all deployment scenarios

NOTE 2: The above NRM fragment uses NRNetwork to hold NR external entities and frequency and using EUtraNetwork to hold LTE external entities and frequency. The NRNetwork and EUtraNetwork are subclasses of SubNetwork (defined in TS 28.622 [30]) with no additional attributes. The reason using NRNetwork and EUtraNetwork is for a clean separation of NR external entities and frequency and LTE external entities and frequency.



Figure 4.2.1.1-x: NRM fragment for ANR Management

#### 4.2.1.2 Inheritance







Figure 4.2.1.2-1: Inheritance Hierarchy

|  |
| --- |
| **Second of Changes** |

### 4.3.2 GNBCUCPFunction

#### 4.3.2.1 Definition

For non-split NG-RAN deployment scenario, this IOC together with GNBCUUPFunction IOC and GNBDUFunction IOC provide the management representation of gNB defined in clause 6.1.1 in 3GPP TS 38.401 [4].

For 2-split NG-RAN deployment scenario, this IOC together with GNBCUUPFunction IOC provide management representation of the gNB-CU defined in clause 6.1.1 in 3GPP TS 38.401 [4].

For 3-split NG-RAN deployment scenario, this IOC provides management representation of gNB-CU-CP defined in clause 6.1.2 in 3GPP TS 38.401 [4].

The following table identifies the necessary end points required for the representation of gNB and en-gNB, of all deployment scenarios.

|  |  |  |  |
| --- | --- | --- | --- |
| Req**Role** | End point requirement for 3-split deployment scenario | End point requirement for 2-split deployment scenario | End point requirement for Non-split deployment scenario |
| gNB  | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC, <<IOC>>EP\_F1C, <<IOC>>EP\_E1. | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC, <<IOC>>EP\_F1C<<IOC>>EP\_F1U. | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC. |
| en-gNB | <<IOC>>EP\_X2C, <<IOC>>EP\_F1C, <<IOC>>EP\_E1. | <<IOC>>EP\_X2C, <<IOC>>EP\_F1C. | <<IOC>>EP\_X2C. |

#### 4.3.2.2 Attributes

The GNBCUCPFunction IOC includes attributes inherited from ManagedFunction IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| gNBId | M | T | T | F | T |
| gNBIdLength  | M  | T | T | F | T |
| gNBCUName | O | T | T | F | T |
| pLMNId | M | T | T | T | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### 4.3.2.3 Attribute constraints

None.

#### 4.3.2.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **Third of Changes** |

### 4.3.32 NRCellRelation

#### 4.3.32.1 Definition

This IOC represents a neighbour cell relation from a source cell to a target cell, where the target cell is an NRCellCU or ExternalNRCellCU instance.

The source cell can be a NRCellCU instance. This is the case for an Intra-NR neighbour cell relation.

The source cell can be a EUtranGenericCell instance. This is the case for Inter-LTE-NR neighbour cell relation, from E-UTRAN to NR. See 3GPP TS 28.658 [19].

Neighbour cell relations are unidirectional.

#### 4.3.32.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| nRTCI | O | T | T | F | T |
| cellIndividualOffset | M | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **attribute related to role** |  |  |  |  |  |
| nRFreqRelationRef | M | T | T | F | T |
| adjacentNRCellRef | M | T | T | F | T |

#### 4.3.32.3 Attribute constraints

None.

#### 4.3.32.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **Fourth of Changes** |

### 4.3.x ANRManagementFunction

#### 4.3.x.1 Definition

This <<IOC>> contains attributes to support the D-SON function of ANR Management (See clause 7.1.4 in TS 28.313 [x]).

#### 4.3.x.2 Attributes

The ANRManagementFunction IOC includes the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| x2BlackList | CM | T | T | F | T |
| x2WhiteList | CM | T | T | F | T |
| xnBlackList | M | T | T | F | T |
| xnWhiteList | M | T | T | F | T |
| x2XnHOBlackList | M | T | T | F | T |
| intrasystemANRManagementSwitch | M | T | T | F | T |
| intersystemANRManagementSwitch | M | T | T | F | T |
| aNRManagementCellPolicyList | M | T | T | F | T |

#### 4.3.x.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| x2BlackList | Condition: Multi-Radio Dual Connectivity with the EPC (see TS 37.340 [9] clause 4.1.2) is supported. |
| x2WhiteList | Condition: Multi-Radio Dual Connectivity with the EPC (see TS 37.340 [9] clause 4.1.2) is supported. |

#### 4.3.x.4 Notifications

The common notifications defined in subclause X.1.5 are valid for this IOC, without exceptions or additions.

### 4.3.y ANRManagementCellPolicy <<data type>>

#### 4.3.y.1 Definition

This data type represents the properties of ANRManagementCellPolicy. ANRManagementCellPolicyList is a list and each item of the list has thress attributes. The list of the three attributes is data type of ANRManagementCellPolicy. The attribute isRemoveAllowed indicates if the subject NRCellRelation can be removed (deleted) or not. The attribute isHOAllowed indicates if HO is allowed or prohibited. The attribute NRCellRelationRef indicates the DN of the referenced NRCellRelation.

#### 4.3.y.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| NRCellRelationRef | M | T | T | F | F |
| isRemoveAllowed | M | T | T | F | T |
| isHOAllowed | M | T | T | F | T |

#### 4.3.y.3 Attribute constraints

None.

#### 4.3.y.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Fifth of Changes** |

### 4.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| administrativeState | It indicates the administrative state of the NRCellDU. It describes the permission to use or prohibition against using the cell, imposed through the OAM services.allowedValues: LOCKED, SHUTTING DOWN, UNLOCKED. The meaning of these values is as defined in ITU‑T Recommendation X.731 [18].See Annex A for Relation between the "Pre-operation state of the gNB-DU Cell" and administrative state relevant in case of 2-split and 3-split deployment scenarios. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LOCKEDisNullable: False |
| operationalState | It indicates the operational state of the NRCellDU instance. It describes whether the resource is installed and partially or fully operable (Enabled) or the resource is not installed or not operable (Disabled).allowedValues: ENABLED, DISABLED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| cellState | It indicates the usage state of the NRCellDU instance. It describes whether the cell is not currently in use (Idle), or currently in use but not configured to carry traffic (Inactive) or is currently in use and is configured to carry traffic (Active).The Inactive and Active definitions are in accordance with TS 38.401 [4]:"Inactive: the cell is known by both the gNB-DU and the gNB-CU. The cell shall not serve UEs;Active: the cell is known by both the gNB-DU and the gNB-CU. The cell should be able to serve UEs.""allowedValues: IDLE, INACTIVE, ACTIVE. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnDL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for downlinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for uplinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnSUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for supplementary uplinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| beamAzimuth  | The azimuth of a beam transmission, which means the horizontal beamforming pointing angle (beam peak direction) in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Zero degree implies explicit antenna bearing (boresight). Positive angle implies clockwise from the antenna bearing. allowedValues: [-1800 ..1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamHorizWidth | The Horizontal beamWidth of a beam transmission, which means the horizontal beamforming half-power (3dB down) beamwidth in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53]. allowedValues: [0..3599] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamIndex | Index of the beam.For example, please see subclause 6.6.2 of TS 38.331 [54] where the ssb-Index in the rsIndexResults element of MeasResultNR is defined. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamTilt  | The tilt of a beam transmission, which means the vertical beamforming pointing angle (beam peak direction) in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Positive value implies downtilt.allowedValues: [-900..900] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamType | The type of the beam. allowedValues: "SSB-BEAM" | type: stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamVertWidth | The Vertical beamWidth of a beam transmission, which means the vertical beamforming half-power (3dB down) beamwidth in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53]. allowedValues: [0...1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| bSChannelBwDL  | BS Channel BW in MHz. for downlinkallowedValues: See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bSChannelBwUL  | BS Channel BW in MHz.for uplinkallowedValues:See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bSChannelBwSUL  | BS Channel BW in MHz.for supplementary uplinkallowedValues:See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| configuredMaxTxPower | This is the maximum possible for all downlink channels, used simultaneously in a cell, added together.allowedValues:TBD | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| coverageShape | Identifies the sector carrier coverage shape described by the envelope of the contained SSB beams. The coverage shape is implementation dependent.allowedValues: 0 : 65535 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| digitalTilt | Digitally-controlled tilt through beamforming. It represents the vertical pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical vertical tilt of the selected coverageShape. Positive value gives downwards tilt and negative value gives upwards tilt.allowedValues: [-900..900] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| digitalAzimuth | Digitally-controlled azimuth through beamforming. It represents the horizontal pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical horizontal pan of the selected coverageShape. Positive value gives azimuth to the right and negative value gives an azimuth to the left.allowedValues: [-1800 ..1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cyclicPrefix | Cyclic prefix as defined in TS 38.211 [32], subclause 4.2.allowedValues: NORMAL, EXTENDED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| localAddress  | This parameter specifies the localAddress including IP address and VLAN ID used for initialization of the underlying transport.First string is IP address, IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).Second string is VLAN Id. (See IEEE 802.1Q [39]), | type: Stringmultiplicity: 2isOrdered: TrueisUnique: N/AdefaultValue: NoneisNullable: False |
| remoteAddress | Remote address including IP address used for initialization of the underlying transport.IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBId | It identifies a gNB within a PLMN. The gNB ID is part of the NR Cell Identifier (NCI) of the gNB cells.See "gNB Identifier (gNB ID)" of subclause 8.2 of TS 38.300 [3]). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5]. allowedValues: 0..4294967295 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBIdLength | This indicates the number of bits for encoding the gNB ID. See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].allowedValues: 22 .. 32. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNB­DUId | It uniquely identifies the DU at least within a gNB-CU. See 'gNB-DU ID' in subclause 9.3.1.9 of 3GPP TS 38.473 [8].allowedValues: 0..236-1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNB­CUUPId | It uniquely identifies the gNB-CU-UP at least within a gNB-CU-CP. See 'gNB-CU-UP ID' in subclause 9.3.1.15 of 3GPP TS 38.463 [48].allowedValues: 0..236-1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBCUName | It identifies the Central Entity of a NR node, see subclause 9.2.1.4 of 3GPP TS 38.473 [8].allowedValues: Not applicable | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBDUName | It identifies the Distributed Entity of a NR node, see subclause 9.2.1.5 of 3GPP TS 38.473 [8].allowedValues: Not applicable | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cellLocalId | It identifies a NR cell of a gNB. It, together with the gNB Identifier (using gNBId of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction), identifies a NR cell within a PLMN. This is the NR Cell Identity (NCI). See subclause 8.2 of TS 38.300 [3]), The NCI can be constructed by encoding the gNB Identifier using gNBId (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction) and cellLocalId where the gNB Identifier field is of length specified by gNBIdLength (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].The NR Cell Global identifier (NCGI) is constructed from the PLMN identity the cell belongs to and the NR Cell Identifier (NCI) of the cell.See relation between NCI and NCGI subclause 8.2 of TS 38.300 [3].allowedValues: Not applicable | type: Integermultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| nRPCI | This holds the Physical Cell Identity (PCI) of the NR cell.allowedValues: See 3GPP TS 36.211 subclause 6.11 for legal values of pci. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRTAC | This holds the identity of the common Tracking Area Code for the PLMNs. allowedValues:a) It is the TAC or Extended-TAC. b) A cell can only broadcast one TAC or Extended-TAC. See TS 36.300, subclause 10.1.7 (PLMNID and TAC relation).c) TAC is defined in subclause 19.4.2.3 of 3GPP TS 23.003[13] and Extended-TAC is defined in subclause 9.3.1.29 of 3GPP TS 38.473 [8].d) For a 5G SA (Stand Alone), it has a non-null value. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NULLisNullable: True |
| GNBCUCPFunction.pLMNId | It specifies the PLMN identifier to be used as part of the global RAN node identity.allowedValues: Not applicable. | Type: PLMNId multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| GNBCUUPFunction.pLMNIdList | This is a list of PLMN identifiers. It defines from which set of PLMNs an UE must have as its serving PLMN to be allowed to use the GNB-CU-UP.allowedValues: Not applicable. | type: PLMNId multiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| NRCellCU.pLMNIdList | This is a list of PLMN identifiers. It defines from which set of PLMNs an UE must have as its serving PLMN to be allowed to use the GNB-CU-UP.allowedValues: Not applicable. | type: PLMNIdmultiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| NRCellDU.pLMNIdList | It defines which PLMNs that can be served by the NR cell. The first entry of the list is the PLMN used to construct the nCGI for the NR cell.allowedValues: Not applicable. | type: PLMNIdmultiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| ExternalNRCellCU.pLMNIdList | It defines which PLMNs that are assumed to be served by the NR Cell in another gNB-CU-CP. This list is either updated by the managed element itself (e.g. due to ANR, signalling over Xn etc) or by consumer over the standard interface.allowedValues: Not applicable. | Type: PLMNIdmultiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| sNSSAIList | It represents the list of S-NSSAI the managed object is supporting. The S-NSSAI is defined in 3GPP TS 23.003 [13].allowedValues: See 3GPP TS 23.003 [13] | type: S-NSSAImultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sST | This attribute specifies the Slice/Service type (SST) of the network slice.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sD | This attribute specifies the Slice Differentiator (SD), which is optional information that complements the slice/service type(s) to differentiate amongst multiple Network Slices.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyType | Type of the RRM policy. The value 0 denotes use of the rRMPolicy. The value 1 denotes use of the rRMPolicyNSSIId, rRMPolicyRatioThe value 2 denotes use of the rRMPolicyRatio2.allowedValues: 0 : 65535. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rRMPolicyNSSIId | The list of S-NSSAIs for which a rRMPolicyRatio value is specifiedallowedValues: Not applicable. | type: DNmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyRatio | The RRM policy setting the ratio for the split of the Radio resources between the supported S-NSSAI lists A S-NSSAI list is defined in rRMPolicyNSSIId. rRMPolicyRatio is the list of target percentage values assigned to the corresponding rRMPolicyNSSIId values. Every value specifies the percentage of PRBs to be allocated to the corresponding S-NSSAIs, in average over time. The sum of the values shall be less or equal 100.allowedValues: 0 : 100See NOTE 3 and NOTE 4. | type: Integermultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyRatio2List | The attribute specifies a list of RRMPolicyRatio2 which is defined as a datatype. The attribute is used to set the ratios for the split of the Radio resources between the sNSSAILists for radio resources (e.g. RRC connected users, PDCP resource, etc.) in average time (see NOTE 2 and NOTE 3). The sum of the values included in the item of rRMPolicyRatio2 shall be less or equal 100 (see NOTE 4).allowedValues: Not applicable. | type: RRMPolicyRatio2multiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| groupId | The attribute identifies one sNSSAIList group inside NRCellCU. The rRMPolicyRatio2 is configured for each group. The value of the groupId is unique inside one NRCellCU instance | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| quotaType | The attribute indicates the type of the quota which allows to allocate resources as strictly usable for defined slice(s) ( “strict quota”) or allows that resources to be used by other slice(s) when defined slice(s) do not need them ( “float quota”).allowedValues: STRICT, FLOAT. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rRMPolicyMaxRatio | The RRM policy setting the maximum percentage of radio resources to be allocated to the corresponding S-NSSAIList.This quota can be strict or float quota. Strict quota means resources are not allowed for other sNSSAIs even when they are not used by the defined sNSSAIList. Float quota resources can be used by other sNSSAIs when the defined sNSSAIList do not need them.Value 0 indicates that there is no maximum limit.allowedValues:0 : 100 | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMarginMaxRatio | Maximum quota margin ratio is applicable when maximum quota policy ratio is of type “float quota”. It defines the resource quota within maximum quota to reserve buffers for new resource requirements for the specified S-NSSAIList. With the margin ratio, unused resources of the maximum resource quota can be allocated to other S-NSSAIs when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the specific S-NSSAIList. Value 0 indicates that no margin is used.allowedValues:0 : 100 | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMinRatio | The RRM policy setting the minimum percentage of radio resources to be allocated to the corresponding S-NSSAIList. This quota can be strict or float quota. Strict quota means resources are not allowed for other sNSSAIs even when they are not used by the defined sNSSAIList. Float quota resources can be used by other sNSSAIs when the defined sNSSAIList do not need them.Value 0 indicates that there is no minimum limit.allowedValues: 0 : 100NOTE: The averaging time interval is implementation dependent. | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMarginMinRatio | Minimum quota margin ratio is applicable when minimum quota policy ratio is of type “float quota”. It defines the resource quota within minimum quota to reserve buffers for new resource requirements for the specified S-NSSAIList. With the margin ratio, unused resources of the minimum resource quota can be allocated to other S-NSSAIs when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the specific S-NSSAIList. Value 0 indicates that no margin is used.allowedValues:0 : 100  | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicy | It represents RRM policy which includes guidance for split of radio resources between the S-NSSAIs that the cell supports in case when the rRMPolicyType is absent or equal to 0. The RRM policy is implementation dependent.allowedValues: Not applicable | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| subCarrierSpacing | Subcarrier spacing configuration for a BWP. See subclause 5 in TS 38.104 [12].AllowedValues: [15, 30, 60, 120] depending on the frequency range FR1 or FR2. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| txDirection | Indicates if the transmission direction is downlink (DL), uplink (UL) or both downlink and uplink (DL and UL).allowedValues:  DL, UL, DL and UL | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bwpContext | It identifies whether the object is used for downlink, uplink or supplementary uplink.allowedValues: DL, UL, SUL | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| isInitialBwp | It identifies whether the object is used for initial or other BWP.allowedValues: INITIAL, OTHER | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| startRB | Offset in common resource blocks to common resource block 0 for the applicable subcarrier spacing for a BWP. This corresponds to N\_BWP\_start, see subclause 4.4.5 in TS 38.211 [32]. allowedValues:0 to N\_grid\_size – 1, where N\_grid\_size equals the number of resource blocks for the BS channel bandwidth, given the subcarrier spacing of the BWP. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| numberOfRBs | Number of physical resource blocks for a BWP. This corresponds to N\_BWP\_size, see subclause 4.4.5 in TS 38.211 [32].allowedValues:1 to N\_grid\_size – startRB of the BWP. Se startRB for definition of N\_grid\_size. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRTCI | This is the Target NR Cell Identifier. It consists of NR Cell Identifier (NCI) and Physical Cell Identifier of the target NR cell (nRPCI).The NRRelation.nRTCI identifies the target cell from the perspective of the NRCell, the name-containing instance of the subject NRCellCU instance.allowedValues: Not applicable. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| adjacentCellRef | This attribute contains the DN of an adjacentNRCell (NRCellCU or ExternalNRCellCU) allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| ssbFrequency | Indicates cell defining SSB frequency domain positionFrequency of the cell defining SSB transmission. The frequency provided in this attribute identifies the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block. The frequency must be positioned on the NR global frequency raster, as defined in TS 38.101 [42] subclause 5.4.2. and within bSChannelBwDL.allowedValues: 0..3279165 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRFrequencyRef | This attribute contains the DN of the referenced NRFrequency.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| nRSectorCarrierRef | This attribute contains the DN of the referenced NRSectorCarrier.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| bWPRef | This attribute contains the DN of the referenced BWP.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| sectorEquipmentFunctionRef | This attribute contains the DN of the referenced NSectorEquipmentFunction.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| offsetMO | It is a list of offset values applicable to all measured cells with reference signal(s) indicated in this *MeasObjectNR*. See offsetMO of subclause 5.5.4 of TS 38.331 [31].allowedValues: Not applicable. | type: QOffsetRangeListmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: False |
| cellIndividualOffset | It is a list of offset values for the neighbour cell. Used when UE is in connected mode. The unit is 1dB. It is defined for rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, rsrqOffsetCSI-RS and sinrOffsetCSI-RS. See TS 38.331 [31].  allowedValues: Not applicable. | type: Integermultiplicity: 6isOrdered: TrueisUnique: N/AdefaultValue: 0isNullable: False |
| blackListEntry | It specifies a list of PCI (physical cell identity) that are blacklisted in EUTRAN measurements as described in 3GPP TS 38.331 [31].allowedValues: { 0…1007 } | type: Integermultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| blackListEntryIdleMode | It specifies a list of PCI (physical cell identity) that are blacklisted in SIB4 and SIB5.allowedValues: { 0…1007 } | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cellReselectionPriority | It is the absolute priority of the carrier frequency used by the cell reselection procedure. See *CellReselectionPriority* IE in TS 38.331 [31].It corresponds to the parameter priority in 3GPP TS 38.304 [49].Value 0 means lowest priority. The UE behaviour when no value is entered is specified in subclause 5.2.4.1 of 3GPP TS 38.304 [49]. The value must not already used by other RAT, i.e. equal priorities between RATs are not supported.allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0NoneisNullable: False |
| cellReselectionSubPriority | It indicates a fractional value to be added to the value of cellReselectionPriority to obtain the absolute priority of the concerned carrier frequency for E-UTRA and NR. See *CellReselectionSubPriority* IE in TS 38.331 [31].allowedValues: { 0.2, 0.4, 0.6, 0.8 }. | type: Shortmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| pMax | It calculates the parameter Pcompensation (defined in 3GPP TS 38.304 [49]), at cell reselection to an Cell. Its unit is 1 dBm. It corresponds to parameter PEMAX in 3GPP TS 38.101 [??]. allowedValues: { -30..33 }.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| qOffsetFreq | It is the frequency specific offset applied when evaluating candidates for cell reselection. See TS 38.331 [49]. Its unit is 1 dB.allowedValues:{ -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 20, 22, 24 } | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0isNullable: False |
| qOffsetRangeList | It is used to indicate a cell, beam or measurement object specific offset to be applied when evaluating candidates for cell re-selection or when evaluating triggering conditions for measurement reporting. The value in dB. Value dB-24 corresponds to -24 dB, dB-22 corresponds to -22 dB and so on.This is a list of enum values representing, in sequence: rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, srqOffsetCSI-RS, sinrOffsetCSI-RS. See Q-OffsetRangeList in subclause of subclause 6.3.1 of TS 38.311 [31].allowedValues: { -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 18, 20, 22, 24 }  | type: ENUMmultiplicity: 6isOrdered: TrueisUnique: N/AdefaultValue: 0isNullable: False |
| qQualMin | It indicates the minimum required quality level in the cell (dB). See qQualMin in TS 38.304 [49]. Unit is 1 dB.Value 0 means that it is not sent and UE applies in such case the (default) value of negative infinity for Qqualmin. Sent in SIB3 or SIB5.allowedValues: { -34..-3, 0 }  | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| qRxLevMin | It indicates the required minimum received Reference Symbol Received Power (RSRP) level in the (E-UTRA) frequency for cell reselection. It corresponds to Qrxlevmin defined in 3GPP TS 38.304 [49]. It is broadcast in SIB3 or SIB5, depending on whether the related frequency is intra- or inter-frequency. Its unit is 1 dBm and resolution is 2.allowedValues: { -140..-44 }. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXHighP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighPin 3GPP TS 38.304 [49]. Its unit is 1 dB and resolution is 2**.**allowedValues: { 0..62 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXHighQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighQ in TS 38.304 [49]. Its unit is 1 dB.allowedValues: { 0..31 } | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXLowP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,LowP in 3GPP TS 38.304 [49]. Its unit is 1 dB. Its resolution is 2.allowedValues: { 0..62 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXLowQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,Low in TS 38.304 [49]. Its unit is 1 dB.allowedValues: {0..31}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNr | It is the cell reselection timer and corresponds to parameter TreselectionRAT for NR defined in 38.331 [4]. Its unit is in seconds. allowedValues: {0..7}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNRSfHigh | The attribute t-ReselectionNr (a parameter TreselectionNR in TS 38.304 [49]) is multiplied with this factor if the UE is in high mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium high state in 3GPP TS 38.304 [49]. The unit is one %.Value mapping:25 = 0.2550 = 0.575 = 0.75100 = 1.0 allowedValues: {25, 50, 75, 100}.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNRSfMedium | The attribute t-ReselectionNR (a parameter "TreselectionNR in TS 38.304 [49]”) is multiplied with this factor if the UE is in medium mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium mobility state in 3GPP TS 38.304 [49]. Its unit is one %.Value mapping:25 = 0.2550 = 0.575 = 0.75100 = 1.0 allowedValues: {25, 50, 75, 100}.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| absoluteFrequencySSB | The absolute frequency applicable for a downlink NR carrier frequency associated with the SSB.allowedValues: {0.. 3279165}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| sSBSubCarrierSpacing | This SSB is used for for synchronization. See subclause 5 in TS 38.104 [12]. Its units are in kHz.allowedValues: {15, 30, 120, 240}.Note that the allowed values of SSB used for representing data, by e.g. a BWP, are: 15, 30, 60 and 120 in units of kHz. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| multiFrequencyBandListNR | It is a list of additional frequency bands the frequency belongs to. The list is automatically set by the gNB.allowedValues: {1..256 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbPeriodicity | Indicates cell defined SSB periodicity in number of subframes (ms).The SSB periodicity in msec is used for the rate matching purpose. allowedValues: 5, 10, 20, 40, 80, 160. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbOffset

|  |
| --- |
|  |

 | Indicates cell defining SSB time domain position. Defined as the offset of the measurement window, in number of subframes (ms), in which to receive SS/PBCH blocks, where allowed values depend on the ssbPeriodicity.allowedValues: ssbPeriodicity5 ms 0..4,ssbPeriodicity10 ms 0..9,ssbPeriodicity20 ms 0..19,ssbPeriodicity40 ms 0..39,ssbPeriodicity80 ms 0..79,ssbPeriodicity160 ms 0..159. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbDuration

|  |
| --- |
|  |

 | Duration of the measurement window in which to receive SS/PBCH blocks. It is given in number of subframes (ms) (see 38.213 [41], subclause 4.1.allowedValues: 1, 2, 3, 4, 5. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rimRSMonitoringStartTime | This field configures the UTC time when the gNB attempts to start RIM-RS monitoring.allowedValues: containing the information same with xsd: dateTime. | type: String multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rimRSMonitoringStopTime | This field configures the UTC time when the gNB stops RIM-RS monitoring.allowedValues: containing the information same with xsd: dateTime. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| isRemoveAllowed | This indicates if the subject NRCellRelation can be removed (deleted) or not. If YES, the subject NRCellRelation instance can be removed (deleted). If NO, the subject NRCellRelation instance shall not be removed (deleted) by any entity but an MnS consumer.allowedValues: YES, NO | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| isHOAllowed | This indicates if HO is allowed or prohibited.If YES, handover is allowed from source cell to target cell. The source cell is identified by the name-containing NRCellCU of the NRCellRelation that contains the isHOAllowed. The target cell is referenced by the NRCellRelation that contains this isHOAllowed. If NO, handover shall not be allowed.allowedValues: YES, NO | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| x2BlackList | This is a list of DNs of NRCellCU and ExternalNRCellCU. If the target node DN is a member of the source node’s NRCellCU.x2BlackList, the source node is: 1) Prohibited from sending X2 connection request to target node;2) Forced to tear down established X2 connection to target node 3) Not allowed to accept incoming X2 connection request from target node.The same DN may appear here and in NRCellCU.x2WhiteList. In such case, the DN in x2WhiteList shall be treated as if it is absent. | type: DNmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| xnBlackList | This is a list of DNs of NRCellCU and ExternalNRCellCU. If the target node DN is a member of the source node’s NRCellCU.xnBlackList, the source node is: 1) Prohibited from sending Xn connection request to target node;2) Forced to tear down established Xn connection to target node 3) Not allowed to accept incoming Xn connection request from target node.The same DN may appear here and in NRCellCU.xnWhiteList. In such case, the DN in xnWhiteList shall be treated as if it is absent. | type: DNmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| x2WhiteList | This is a list of DNs of NRCellCU and ExternalNRCellCU. If the target node DN is a member of the source node’s NRCellCU.x2WhiteList, the source node:- is allowed to request the establishment of X2 connection with the target node;- is not allowed to initiate the tear down of established X2 connection to target nodeThe same DN may appear here and in NRCellCU.x2BlackList. In such case, the DN here shall be treated as if it is absent. | type: Stringmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| xnWhiteList | This is a list of DNs of NRCellCU and ExternalNRCellCU. If the target node DN is a member of the source node’s NRCellCU.xnWhiteList, the source node:- is allowed to request the establishment of Xn connection with the target node;- is not allowed to initiate the tear down of established Xn connection to target nodeThe same DN may appear here and in NRCellCU.xnBlackList. In such case, the DN here shall be treated as if it is absent. | type: Stringmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| x2XnHOBlackList | This is a list of DNs of any number and combination of cells represented by the following IoCs:NRCellCUExternalNRCellCU. ExternalEUtranCellTDDExternalEUtranCellFDDEUtranCellTDDEUtranCellFDDFor all the entries in NRCellCU.x2XnHOBlackList, the subject NRCellCU is prohibited to use the X2 or Xn interface for HOs even if an X2 or Xn interface exists to the target cell. | type: DNmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| intrasystemANRManagementSwitch | This attribute determines whether the intra-system ANR function is activated or deactivated.If “on”, the intra-system ANR function may add or remove intra NG-RAN Neighbour Relations, i.e. add or remove NRCellRelation instances from NRCellCU of this GNBCUCPFunction.If “off”, the intra-system ANR Function must not add or remove Neighbour Relations, i.e. add or remove NRCellRelation instances from NRCellCU of this GNBCUCPFunction.allowedValues: On, Off | type: enumerationmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| intersystemANRManagementSwitch | This attribute determines whether the inter-system ANR function is activated or deactivated.If “on”, the inter-system ANR function may add or remove inter-system Neighbour Relations, i.e. add or remove EUtranRelation instances from NRCellCU of this GNBCUCPFunction.If “off”, the inter-system ANR Function must not add or remove inter-system Neighbour Relations, i.e. add or remove EUtranRelation instances from NRCellCU of this GNBCUCPFunction.allowedValues: On, Off | type: enumerationmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| aNRManagementCellPolicyList | This attribute specifies the cell policy information of ANR management. | type: aNRManagementCellPolicymultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| NRCellRelationRef | This attribute contains the DN of the referenced NRCellRelation for which the attributes (i.e. isRemovedAllowed, isHOAllowed) of the same<<dateType>> is applicable.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| NOTE 1: VoidNOTE 2: The radio resource can be signaling resources (e.g. RRC connected users) or user plane resources (e.g. PDCP). The detail resource and how to map the ratio to exact number of resources is implementation dependant.NOTE 3: The averaging time interval is implementation dependent.NOTE 4: How to calculate the sum of the ratio is implementation dependent. |

|  |
| --- |
| **Sixth of Changes** |

### 5.4.1 Attribute properties

The following table defines the attributes that are present in several Information Object Classes (IOCs) of the present document.

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| aMFIdentifier | The AMFI is constructed from an AMF Region ID, an AMF Set ID and an AMF Pointer. The AMF Region ID identifies the region, the AMF Set ID uniquely identifies the AMF Set within the AMF Region, and the AMF Pointer uniquely identifies the AMF within the AMF Set. (Ref. 3GPP TS 23.003 [13]) | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| aMFSetId | It represents the AMF Set ID, which is uniquely identifies the AMF Set within the AMF Region.allowedValues: defined in subclause 2.10.1 of 3GPP TS 23.003 [13]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| aMFSetMemberList | It is the list of DNs of AMFFunction instances of the AMFSet. allowedValues: N/A | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| aMFRegionId | It represents the AMF Region ID, which identifies the region.allowedValues: defined in subclause 2.10.1 of 3GPP TS 23.003 [13]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| localAddress  | This parameter specifies the localAddress including IP address and VLAN ID used for initialization of the underlying transport.First string is IP address, IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).Second string is VLAN Id (See IEEE 802.1Q [39]). | type: Stringmultiplicity: 2isOrdered: TrueisUnique: N/AdefaultValue: NoneisNullable: False |
| remoteAddress | Remote address including IP address used for initialization of the underlying transport.IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nfProfileList | It is a set of NFProfile(s) to be registered in the NRF instance. NFProfile is defined in 3GPP TS 29.510 [23]. | type: <<dataType>>multiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| nSIIdList | It is a set of NSI Id. The NSI ID is defined in subclause 6.1.6.2.8 of 3GPP TS 29.531 [24].  | type: Stringmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sNSSAIList | See subclause 4.4.1. |  |
| sBIFQDN | It is used to indicate the FQDN of the registered NF instance in service-based interface, for example, NF instance FQDN structure is:nftype<nfnum>.slicetype<sliceid>.mnc<MNC>.mcc<MCC>.3gppnetwork.org | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sBIServiceList | It is used to indicate the all supported NF services registered on service-based interface. | type: Stringmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| nRTACList | It is the list of Tracking Area Codes (either legacy TAC or extended TAC). allowedValues:Legacy TAC and Extended TAC are defined in clause 9.3.3.10 of TS 38.413 [5]. | type: Integermultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| supportedBMOList | It is used to indicate the list of supported BMOs (Bridge Managed Objects) required for integration with TSN system. | type: Stringmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| managedNFProfile | This parameter defines profile for managed NF (See TS 23.501 [22]). allowedValues: N/A | type: ManagedNFProfilemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| nfInstanceID | This parameter defines unique identity of the NF Instance. The format of the NF Instance ID shall be a Universally Unique Identifier (UUID) version 4, as described in IETF RFC 4122 [44]allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| nfType | This parameter defines type of Network FunctionallowedValues: See TS 23.501[22] for NF types | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fqdn | This parameter defines FQDN of the Network Function (See TS 23.003 [5])allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| ipAddress | This parameter defines IP Address of the Network Function. It can be IPv4 address (See RFC 791 [24]) or IPv6 address (See RFC 2373 [25]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| authzInfo | This parameter defines NF Specific Service authorization information. It shall include the NF type (s) and NF realms/origins allowed to consume NF Service(s) of NF Service Producer (See TS 23.501[22]). allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: True |
| locality | The parameter defines information about the location of the NF instance (e.g. geographic location, data center) defined by operator (See TS 29.510[23]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: True |
| capacity | This parameter defines static capacity information in the range of 0-65535, expressed as a weight relative to other NF instances of the same type; if capacity is also present in the nfServiceList parameters, those will have precedence over this value (See TS 29.510[23])allowedValues: 0-65535 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| nFInfo | This parameter includes NF specific data in Managed NF profileallowedValues: N/A | type: NFInfomultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| hostAddr | This parameter defines host address of a NFallowedValues: N/A | type: HostAddrmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| priority | This parameter defines Priority (relative to other NFs of the same type) in the range of 0-65535, to be used for NF selection; lower values indicate a higher priority. If priority is also present in the nfServiceList parameters, those will have precedence over this value (See TS 29.510[23]).allowedValues: 0-65535 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| supportedDataSetIds | This parameter defines list of supported data sets in the UDR instance (See TS 29.510[23]).allowedValues: "SUBSCRIPTION", "POLICY", EXPOSURE", "APPLICATION" | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: FalsedefaultValue: NoneisNullable: False |
| nFSrvGroupId | This parameter defines identity of the group that is served by the NF instance (See TS 29.510[23]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| smfServingAreas | This parameter defines the SMF service area(s) the UPF can serve (See TS 29.510[23]).allowedValues: N/A | type: Stringmultiplicity: 1..\*isOrdered: FisUnique: TruedefaultValue: NoneisNullable: False |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| groupId | This parameter identiies a list of target NF services on which the same communication model is applied to. allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: FalsedefaultValue: NoneisNullable: False |
| commModelType | This parameter defines communication model used by a NF to interact with NF service(s) (See TS 23.501 [2]). allowedValues:”DIRECT\_COMMUNICATION\_WO\_NRF”, “DIRECT\_COMMUNICATION\_WITH\_NRF”, “INDIRECT\_COMMUNICATION\_WO\_DEDICATED\_DISCOVERY”, “INDIRECT\_COMMUNICATION\_WITH\_DEDICATED\_DISCOVERY” | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| targetNFServiceList | This parameter lists target NF services sharing same communication model and configuration.allowedValues: N/A | type: DNmultiplicity: 1..\*isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| commModelConfiguration | This parameter defines configuration parameters for specific communication model for a group of NF Services.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| supportedFuncList | This parameter lists functionalities supported by a SCP. Refer to TS 23.501 [2]. | type: SupportedFunctionmultiplicity: 1..\*isOrdered: N/AisUnique: FalsedefaultValue: NoneisNullable: False |
| address | This parameter defines address of a SCP instance, it can be IP address (either IPv4 address (See RFC 791 [24]) or IPv6 address (See RFC 2373 [25])) or FQDN (See TS 23.003 [5]).  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| function | This parameter defines name of a functionality supported by a SCP. | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| policy | This parameter defines configuration policies of a functionality supported by a SCP. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| capabilityList | This parameter lists capabilities supported by a NEF. Refer to TS 23.501 [2].allowedValues: N/A | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: FalsedefaultValue: NoneisNullable: False |
| isINEF | This parameter defines if the NEF is an Intermediate NEF. allowedValues: TRUE, FALSE | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| isCAPIFSup | This parameter defines if the NEF support Common API Framework.allowedValues: TRUE, FALSE | type: Booleanmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| sEPPType | This parameter defines the type of a SEPP entity. Refer to TS 33.501 [52].allowedValues: “CSEPP”, “PSEPP” | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: FalsedefaultValue: NoneisNullable: False |
| sEPPId | This parameter is identifier of a SEPP, it is unique inside a PLMN. allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| remotePlmnId | This parameter defines PLMNId of the remote SEPP.allowedValues: N/A | Type: PLMNId multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| remoteSeppAddress | This parameter defines address of the remote SEPP. It can be IP address (either IPv4 address (See RFC 791 [24]) or IPv6 address (See RFC 2373 [25])) or FQDN(See TS 23.003 [5]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| remoteSeppId | This parameter defines identifier of the remote SEPP. it is unique inside a PLMN.allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| n32cParas | This attribute is used to configure parameters to establish security link between two SEPPs. allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| n32fPolicy | This attribute is used to configure policies to protect the messages exchanged between SEPPs.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FisUnique: N/AdefaultValue: NoneisNullable: False |
| withIPX | This attribute defines if there’s an IPX interconnected between two SEPPs.allowedValues: TRUE, FALSE | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |

|  |
| --- |
| **Fourth of Changes** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |

|  |
| --- |
|  |

## C.4.3 XML schema "nRNrm.xsd"

<?xml version="1.0" encoding="UTF-8"?>

<!--

 3GPP TS 28.541 NR Network Resource Model

 XML schema definition

 nrNrm.xsd

-->

<schema xmlns="http://www.w3.org/2001/XMLSchema"

xmlns:xn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"

xmlns:nn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#nrNrm"

xmlns:en="http://www.3gpp.org/ftp/specs/archive/28\_series/28.659#eutranNrm"

xmlns:epc="http://www.3gpp.org/ftp/specs/archive/28\_series/28.709#epcNrm"

xmlns:sm="http://www.3gpp.org/ftp/specs/archive/28\_series/28.626#stateManagementIRP"

xmlns:ngc="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#ngcNrm"

xmlns:sp="http://www.3gpp.org/ftp/specs/archive/28\_series/28.629#sonPolicyNrm"

targetNamespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#nrNrm" elementFormDefault="qualified">

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.709#epcNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.626#stateManagementIRP"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#ngcNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.629#sonPolicyNrm"/>

<simpleType name="GnbId">

 <restriction base="unsignedLong">

 <maxInclusive value="4294967295"/>

 </restriction>

</simpleType>

<simpleType name="GnbIdLength">

 <restriction base="integer">

 <minLength value="22"/>

 <maxLength value="32"/>

 </restriction>

</simpleType>

<simpleType name="Nci">

 <restriction base="unsignedLong">

 <maxInclusive value="68719476735"/>

 </restriction>

</simpleType>

<simpleType name="Pci">

 <restriction base="unsignedShort">

 <maxInclusive value="503"/>

 <!-- Minimum value is 0, maximum value is 3x167+2=503 -->

 </restriction>

</simpleType>

<simpleType name="NrTac">

 <restriction base="unsignedLong">

 <maxInclusive value="16777215"/>

 <!--5G TAC is 3-octets length -->

 </restriction>

</simpleType>

<simpleType name="GnbDuId">

 <restriction base="unsignedLong">

 <maxInclusive value="68719476735"/>

 <!-- Minimum value is 0, maximum value is 2^36-1=68719476735 -->

 </restriction>

</simpleType>

<simpleType name="GnbCuupId">

 <restriction base="unsignedLong">

 <maxInclusive value="68719476735"/>

 <!-- Minimum value is 0, maximum value is 2^36-1=68719476735 -->

 </restriction>

</simpleType>

<simpleType name="GnbName">

 <restriction base="string">

 <minLength value="1"/>

 <maxLength value="150"/>

 </restriction>

</simpleType>

<simpleType name="CyclicPrefix">

 <restriction base="integer">

 <enumeration value="15"/>

 <enumeration value="30"/>

 <enumeration value="60"/>

 <enumeration value="120"/>

 </restriction>

</simpleType>

<simpleType name="QuotaType">

 <restriction base="string">

 <enumeration value="STRICT"/>

 <enumeration value="FLOAT"/>

 </restriction>

</simpleType>

<simpleType name="CellState">

 <restriction base="string">

 <enumeration value="IDLE"/>

 <enumeration value="INACTIVE"/>

 <enumeration value="ACTIVE"/>

 </restriction>

</simpleType>

<simpleType name="BwpContext">

 <restriction base="string">

 <enumeration value="DL"/>

 <enumeration value="UL"/>

 <enumeration value="SUL"/>

 </restriction>

</simpleType>

<simpleType name="IsInitialBwp">

 <restriction base="string">

 <enumeration value="INITIAL"/>

 <enumeration value="OTHER"/>

 </restriction>

</simpleType>

<simpleType name="qOffsetRangeList">

 <restriction base="string">

 <enumeration value="dB-24"/>

 <enumeration value="dB-22"/>

 <enumeration value="dB-20"/>

 <enumeration value="dB-18"/>

 <enumeration value="dB-16"/>

 <enumeration value="dB-14"/>

 <enumeration value="dB-12"/>

 <enumeration value="dB-10"/>

 <enumeration value="dB-8"/>

 <enumeration value="dB-6"/>

 <enumeration value="dB-5"/>

 <enumeration value="dB-4"/>

 <enumeration value="dB-3"/>

 <enumeration value="dB-2"/>

 <enumeration value="dB-1"/>

 <enumeration value="dB0"/>

 <enumeration value="dB1"/>

 <enumeration value="dB2"/>

 <enumeration value="dB3"/>

 <enumeration value="dB4"/>

 <enumeration value="dB5"/>

 <enumeration value="dB6"/>

 <enumeration value="dB8"/>

 <enumeration value="dB10"/>

 <enumeration value="dB12"/>

 <enumeration value="dB14"/>

 <enumeration value="dB16"/>

 <enumeration value="dB18"/>

 <enumeration value="dB20"/>

 <enumeration value="dB22"/>

 <enumeration value="dB24"/>

 </restriction>

</simpleType>

<simpleType name="cellReselectionPriority">

 <restriction base="unsignedLong">

 <minInclusive value="0"/>

 <maxInclusive value="16"/>

 <!--Value 0 means lowest priority-->

 </restriction>

</simpleType>

<simpleType name="cellReselectionSubPriority">

 <restriction base="unsignedLong">

 <minInclusive value="0"/>

 <maxInclusive value="16"/>

 <!--Value 0 means lowest priority-->

 </restriction>

</simpleType>

<simpleType name="PMaxRangeType">

 <restriction base="short">

 <minInclusive value="-30"/>

 <maxInclusive value="33"/>

 </restriction>

</simpleType>

<simpleType name="qOffsetFreq">

 <restriction base="short">

 <minInclusive value="-24"/>

 <maxInclusive value="24"/>

 </restriction>

</simpleType>

<simpleType name="qQualMin">

 <restriction base="integer">

 <minInclusive value="-34"/>

 <maxInclusive value="0"/>

 </restriction>

</simpleType>

<simpleType name="qRxLevMin">

 <restriction base="integer">

 <minInclusive value="-140"/>

 <maxInclusive value="-44"/>

 </restriction>

</simpleType>

<simpleType name="Thresxhighp">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="62"/>

 </restriction>

</simpleType>

<simpleType name="Threshxhighq">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="31"/>

 </restriction>

</simpleType>

<simpleType name="Threshxlowp">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="62"/>

 </restriction>

</simpleType>

<simpleType name="Threshxlowq">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="62"/>

 </restriction>

</simpleType>

<simpleType name="Treselectionnr">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="7"/>

 </restriction>

</simpleType>

<simpleType name="Treselectionnrsfhigh">

 <restriction base="string">

 <enumeration value="25"/>

 <enumeration value="50"/>

 <enumeration value="75"/>

 <enumeration value="100"/>

 </restriction>

</simpleType>

<simpleType name="Treselectionnrsfmedium">

 <restriction base="string">

 <enumeration value="25"/>

 <enumeration value="50"/>

 <enumeration value="75"/>

 <enumeration value="100"/>

 </restriction>

</simpleType>

<simpleType name="Absolutefrequencyssb">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="3279165"/>

 </restriction>

</simpleType>

<simpleType name="Ssbsubcarrierspacing">

 <restriction base="string">

 <enumeration value="15"/>

 <enumeration value="30"/>

 <enumeration value="120"/>

 <enumeration value="240"/>

 </restriction>

</simpleType>

<simpleType name="Multifrequencybandlistnr">

 <restriction base="integer">

 <minInclusive value="1"/>

 <maxInclusive value="256"/>

 </restriction>

</simpleType>

<simpleType name="beamType">

 <restriction base="string">

 <enumeration value="SSB-BEAM"/>

 </restriction>

</simpleType>

<simpleType name="beamAzimuth">

 <restriction base="integer">

 <minInclusive value="-1800"/>

 <maxInclusive value="1800"/>

 </restriction>

</simpleType>

<simpleType name="beamTilt">

 <restriction base="integer">

 <minInclusive value="-900"/>

 <maxInclusive value="900"/>

 </restriction>

</simpleType>

<simpleType name="beamHorizWidth">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="3599"/>

 </restriction>

</simpleType>

<simpleType name="beamVertWidth">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="1800"/>

 </restriction>

</simpleType>

<simpleType name="coverageShapeType">

 <restriction base="integer">

 <minInclusive value="0"/>

 <maxInclusive value="65535"/>

 </restriction>

</simpleType>

<complexType name="LocalEndPoint">

 <sequence>

 <element name="ipv4Address" type="string"/>

 <element name="ipv6Address" type="string"/>

 <element name="ipv6Prefix" type="string"/>

 <element name="vlanId" type="integer"/>

 </sequence>

</complexType>

<complexType name="RemoteEndPoint">

 <sequence>

 <element name="ipv4Address" type="string"/>

 <element name="ipv6Address" type="string"/>

 <element name="ipv6Prefix" type="string"/>

 </sequence>

</complexType>

<complexType name="blackListEntry">

 <sequence minOccurs="0" maxOccurs="1007" >

 <element name="pci" type="en:Pci" maxOccurs="504"/>

 </sequence>

</complexType>

<complexType name="blackListEntryIdleMode">

 <sequence minOccurs="0" maxOccurs="1007" >

 <element name="pci" type="en:Pci" maxOccurs="504"/>

 </sequence>

</complexType>

<complexType name="RRMPolicyRation2">

 <sequence>

 <element name="groupId" type="integer"/>

 <element name="sNSSAIList" type="ngc:SnssaiList"/>

 <element name="quotaType" type="QuotaType"/>

 <element name="rRMPolicyMaxRation" type="integer"/>

 <element name="rRMPolicyMarginMaxRation" type="integer"/>

 <element name="rRMPolicyMinRation" type="integer"/>

 <element name="rRMPolicyMarginMinRation" type="integer"/>

 </sequence>

</complexType>

<complexType name="PLMNIdList">

 <sequence>

 <element name="pLMNId" type="en:PLMNId" maxOccurs="6"/>

 <!-- The first pLMNId of the pLMNIdList is primary PLMN id -->

 </sequence>

</complexType>

<complexType name="cellIndividualOffset">

 <sequence>

 <element name="rsrpOffsetSSB" type="qOffsetRangeList"/>

 <element name="rsrqOffsetSSB" type="qOffsetRangeList"/>

 <element name="sinrOffsetSSB" type="qOffsetRangeList"/>

 <element name="rsrpOffsetCSI-RS" type="qOffsetRangeList"/>

 <element name="rsrqOffsetCSI-RS" type="qOffsetRangeList"/>

 <element name="sinrOffsetCSI-RS" type="qOffsetRangeList"/>

 </sequence>

 </complexType>

<element name="GNBDUFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="gnbId" type="nn:GnbId"/>

 <element name="gnbIdLength" type="nn:GnbIdLength"/>

 <element name="gnbDUId" type="nn:GnbDuId"/>

 <element name="gnbDuName" type="nn:GnbName" minOccurs="0"/>

 <element name="x2Blacklist" type="xn:dnList" minOccurs="0"/>

 <element name="x2Whitelist" type="xn:dnList" minOccurs="0"/>

 <element name="xnBlacklist" type="xn:dnList" minOccurs="0"/>

 <element name="xnWhitelist" type="xn:dnList" minOccurs="0"/>

 <element name="x2XnHOBlackList" type="xn:dnList" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="nn:NRCellDU"/>

 <element ref="nn:BWP"/>

 <element ref="nn:NRSectorCarrier"/>

 <element ref="nn:EP\_F1C"/>

 <element ref="nn:EP\_F1U"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="GNBCUCPFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="gnbId" type="nn:GnbId" />

 <element name="gnbIdLength" type="nn:GnbIdLength"/>

 <element name="gnbCuName" type=" nn:GnbName" minOccurs="0"/>

 <element name="pLMNId" type="en:PLMNId" />

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="nn:NRCellCU"/>

 <element ref="nn:EP\_F1C"/>

 <element ref="nn:EP\_E1"/>

 <element ref="nn:EP\_XnC"/>

 <element ref="nn:EP\_X2C"/>

 <element ref="nn:EP\_NgC"/>

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="GNBCUUPFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="gNBCUUPId" type="nn:GnbCuupId "/>

 <element name="pLMNIdList" type="en:PLMNIdList"/>

 <element name="gNBId" type="nn:GnbId"/>

 <element name="gnbIdLength" type="nn:GnbIdLength"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="nn:EP\_E1"/>

 <element ref="nn:EP\_F1U"/>

 <element ref="nn:EP\_XnU"/>

 <element ref="nn:EP\_NgU"/>

 <element ref="nn:EP\_X2U"/>

 <element ref="nn:EP\_S1U"/>

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRCellCU">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="nCGI" type="nn:Ncgi"/>

 <element name="pLMNIdList" type="en:PLMNIdList"/>

 <element name="sNSSAIList" type="ngc:SnssaiList" minOccurs="0"/>

 <element name="rRMPolicyType" type="integer" minOccurs="0"/>

 <element name="rRMPolicyNSSIId" type="xn:dn" minOccurs="0"/>

 <element name="rRMPolicyRatio" type="integer" minOccurs="0"/>

 <element name="rRMPolicy" type="string" minOccurs="0"/>

 <element name="rRMPolicyRatio2" type="RRMPolicyRation2" minOccurs="0"/>

 <element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 <element ref="nRCellRelation"/>

 <element ref="nRFreqRelation"/>

 <element ref="eUtranCellRelation"/>

 <element ref="eUtranFreqRelation"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRCellDU">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="nCGI" type="nn:Ncgi" minOccurs="0"/>

 <element name="operationalState" type="sm:operationalStateType" minOccurs="0"/>

 <element name="administrativeState" type="sm:administrativeStateType" minOccurs="0"/>

 <element name="cellState" type="nn:CellState"/>

 <element name="pLMNIdList" type="en:PLMNIdList"/>

 <element name="sNSSAIList" type="ngc:SnssaiList" minOccurs="0"/>

 <element name="nRpci" type="nn:Pci" />

 <element name="nRTac" type="nn:NrTac" />

 <element name="arfcnDL" type="integer"/>

 <element name="arfcnUL" type="integer" minOccurs="0"/>

 <element name="arfcnSUL" type="integer" minOccurs="0"/>

 <element name="bSChannelBwDL" type="integer"/>

 <element name="bSChannelBwUL" type="integer" minOccurs="0"/>

 <element name="bSChannelBwSUL" type="integer" minOccurs="0"/>

 <element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

 <element name="nRSectorCarrierRef" type="xn:dn" minOccurs="0"/>

 <element name="bWPRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRSectorCarrier">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="txDirection" type="nn:TxDirection"/>

 <element name="configuredMaxTxPower" type="integer"/>

 <element name="arfcnDL" type="integer" minOccurs="0"/>

 <element name="arfcnUL" type="integer" minOccurs="0"/>

 <element name="bSChannelBwDL" type="integer" minOccurs="0"/>

 <element name="bSChannelBwUL" type="integer" minOccurs="0"/>

 <element name="sectorEquipmentFunctionRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="BWP">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction-->

 <element name="bwpContext" type="nn:BwpContext"/>

 <element name="isInitialBwp" type="nn:IsInitialBwp"/>

 <element name="subCarrierSpacing" type="integer"/>

 <element name="cyclicPrefix" type="nn:CyclicPrefix"/>

 <element name="startRB" type="integer"/>

 <element name="numberOfRBs" type="integer"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="CommonBeamformingFunction">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <element name="coverageShape" type="coverageShapeType" minOccurs="0"/>

 <element name="digitalTilt" type="beamTilt" minOccurs="0"/>

 <element name="digitalAzimuth" type="beamAzimuth" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="Beam">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <element name="beamIndex" type="integer" minOccurs="0"/>

 <element name="beamType" type="beamType" minOccurs="0"/>

 <element name="beamAzimuth" type="beamAzimuth" minOccurs="0"/>

 <element name="beamTilt" type="beamTilt" minOccurs="0"/>

 <element name="beamHorizWidth" type="beamHorizWidth" minOccurs="0"/>

 <element name="beamVertWidth" type="beamVertWidth" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_E1">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_XnC">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_XnU">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

 </element>

<element name="EP\_NgC">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LoacalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_NgU">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_F1C">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_F1U">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_S1U">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_X2C">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="EP\_X2U">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes" minOccurs="0">

 <complexType>

 <all>

 <!-- Inherited attributes from EP\_RP -->

 <element name="farEndEntity" type="xn:dn" minOccurs="0"/>

 <element name="userLabel" type="string" minOccurs="0"/>

 <!-- End of inherited attributes from EP\_RP -->

 <element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

 <element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRCellRelation">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction -->

 <element name="nRTCI" type="nn:Nrtci"/>

 <element name="cellIndividualOffset" type="en:CellIndividualOffset"/>

 <element name="nRFreqRelationRef" type="xn:dn" minOccurs="0"/>

 <element name="adjacentNRCellRef" type="xn:dn" minOccurs="0"/>

 <element name="isRemoveAllowed" type="boolean" minOccurs="0"/>

 <element name="isHOAllowed" type="boolean" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRFreqRelation">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction -->

 <element name="offsetMO" type="en:qOffsetRangeList"/>

 <element name="blackListEntry" type="en:blackListEntry" minOccurs="0"/>

 <element name="blackListEntryIdleMode" type="en:blackListEntryIdleMode" minOccurs="0"/>

 <element name="cellReselectionPriority" type="en:cellReselectionPriority"/>

 <element name="cellReselectionSubPriority" type="en:cellReselectionSubPriority"/>

 <element name="pMax" type="en:PMaxRangeType" minOccurs="0"/>

 <element name="qOffserFreq" type="nn:qOffserFreq" minOccurs="0"/>

 <element name="qQualMin" type="en:qQualMin" minOccurs="0"/>

 <element name="qRxLevMin" type="en:qRxLevMin" minOccurs="0"/>

 <element name="threshXHighP" type="en:threshxhighp" minOccurs="0"/>

 <element name="threshXHighQ" type="en:threshxhighq" minOccurs="0"/>

 <element name="threshXLowP" type="en:threshxlowp" minOccurs="0"/>

 <element name="threshXLowQ" type="en:threshxlowp" minOccurs="0"/>

 <element name="tReselectionNr" type="nn:Treselectionnr" minOccurs="0"/>

 <element name="tReselectionNRSfHigh" type="nn:Treselectionnrsfhigh" minOccurs="0"/>

 <element name="tReselectionNRSfMedium" type="nn:Treselectionnrsfmedium" minOccurs="0"/>

 <element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="ExternalNRCellCU">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction -->

 <element name="nCGI" type="nn:Ncgi"/>

 <element name="pLMNIdList" type="en:PLMNIdList"/>

 <element name="nRPCI" type="nn:Nrpci" minOccurs="0"/>

 <element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="ExternalGNBCUCPFunction" substitutionGroup="xn:SubNetworkOptionallyContainedNrmClass ">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction -->

 <element name="gnbId" type="nn:GnbId" />

 <element name="gnbIdLength" type="nn:GnbIdLength"/>

 <element name="pLMNId" type="en:PLMNIdList" />

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="RRMPolicyRatio2">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <element name="userLabel" type="string"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="groupId" type="integer"/>

 <element name="sNSSAIList" type="ngc:SnssaiList" minOccurs="0"/>

 <element name="quotaType" type="nn:quotaType"/>

 <element name="rRMPolicyMaxRatio" type="integer" minOccurs="0"/>

 <element name="rRMPolicyMarginMaxRatio" type="integer" minOccurs="0"/>

 <element name="rRMPolicyMinRatio" type="integer" minOccurs="0"/>

 <element name="rRMPolicyMarginMinRatio" type="integer" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="NRFrequency" substitutionGroup="xn:SubNetworkOptionallyContainedNrmClass">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <!-- Inherited attributes from ManagedFunction -->

 <element name="userLabel" type="string" minOccurs="0"/>

 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

 <element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

 <element name="priority" type="integer" minOccurs="0"/>

 <element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

 <!--End of inherited attributes from ManagedFunction -->

 <element name="absoluteFrequencySSB" type="nn:Absolutefrequencyssb" minOccurs="0"/>

 <element name="sSBSubCarrierSpacing" type="nn:Ssbsubcarrierspacing" minOccurs="0"/>

 <element name="multiFrequencyBandListNR" type="nn:MultifrequencyBandlistnr" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:VsDataContainer"/>

 </choice>

 <choice minOccurs="0" maxOccurs="1">

 <element ref="sp:EnergySavingProperties"/>

 <element ref="sp:ESPolicies"/>

 </choice>

 <choice minOccurs="0" maxOccurs="unbounded">

 <element ref="xn:MeasurementControl"/>

 </choice>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="ANRManagementFunction">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <element name="x2Blacklist" type="xn:dnList" minOccurs="0"/>

 <element name="x2Whitelist" type="xn:dnList" minOccurs="0"/>

 <element name="xnBlacklist" type="xn:dnList" minOccurs="0"/>

 <element name="xnWhitelist" type="xn:dnList" minOccurs="0"/>

 <element name="x2XnHOBlackList" type="xn:dnList" minOccurs="0"/>

 <element name="intrasystemANRManagementSwitch" type="boolean" minOccurs="0"/>

 <element name="intersystemANRManagementSwitch" type="boolean" minOccurs="0"/>

 <element name="aNRManagementCellPolicy" type="ANRManagementCellPolicy" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element>

<element name="ANRManagementCellPolicy">

 <complexType>

 <complexContent>

 <extension base="xn:NrmClass">

 <sequence>

 <element name="attributes">

 <complexType>

 <all>

 <element name="isRemoveAllowed" type="boolean" minOccurs="0"/>

 <element name="isHOAllowed" type="boolean" minOccurs="0"/>

 <element name="NRCellRelationRef" type="xn:dn" minOccurs="0"/>

 </all>

 </complexType>

 </element>

 </sequence>

 </extension>

 </complexContent>

 </complexType>

</element></schema>

## D.4.3 JSON schema "nrNrm.json"

{

 "openapi": "3.0.1",

 "info": {

 "title": "3GPP NR NRM",

 "version": "16.1.0",

 "description": "OAS 3.0.1 specification compatible schema for 3GPP NR NRM"

 },

 "paths": {},

 "components": {

 "schemas": {

 "GnbId": {

 "type": "string"

 },

 "GnbIdLength": {

 "type": "integer",

 "minimum": 22,

 "maximum": 32

 },

 "GnbName": {

 "type": "string",

 "maxLength": 150

 },

 "GnbDuId": {

 "type": "number",

 "minimum": 0,

 "maximum": 68719476735

 },

 "GnbCuUpId": {

 "type": "number",

 "minimum": 0,

 "maximum": 68719476735

 },

 "NCi": {

 "type": "object",

 "properties": {

 "plmnId": {

 "$ref": "#/components/schemas/PlmnId"

 },

 "nCI": {

 "$ref": "#/components/schemas/NrCellId"

 }

 }

 },

 "SnssaiList": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/Snssai"

 }

 },

 "RrmPolicy": {

 "type": "string"

 },

 "NrPci": {

 "type": "integer",

 "maximum": 503

 },

 "NrTac": {

 "type": "integer",

 "maximum": 16777215

 },

 "NrCellId": {

 "type": "integer",

 "maximum": 68719476735

 },

 "Sst": {

 "type": "integer",

 "maximum": 255

 },

 "Snssai": {

 "type": "object",

 "properties": {

 "sst": {

 "$ref": "#/components/schemas/Sst"

 },

 "sd": {

 "type": "string"

 }

 }

 },

 "CellState": {

 "type": "string",

 "enum": [

 "IDLE",

 "INACTIVE",

 "ACTIVE"

 ]

 },

 "CyclicPrefix": {

 "type": "string",

 "enum": [

 "15",

 "30",

 "60",

 "120"

 ]

 },

 "TxDirection": {

 "type": "string",

 "enum": [

 "DL",

 "UL",

 "DL and UL"

 ]

 },

 "BwpContext": {

 "type": "string",

 "enum": [

 "DL",

 "UL",

 "SUL"

 ]

 },

 "IsInitialBwp": {

 "type": "string",

 "enum": [

 "INITIAL",

 "OTHER",

 "SUL"

 ]

 },

 "QuotaType": {

 "type": "string",

 "enum": [

 "STRICT",

 "FLOAT"

 ]

 },

 "RrmPolicyRatio2": {

 "type": "object",

 "properties": {

 "groupId": {

 "type": "integer"

 },

 "sNSSAIList": {

 "$ref": "#/components/schemas/SnssaiList"

 },

 "quotaType": {

 "$ref": "#/components/schemas/QuotaType"

 },

 "rRMPolicyMaxRation": {

 "type": "integer"

 },

 "rRMPolicyMarginMaxRation": {

 "type": "integer"

 },

 "rRMPolicyMinRation": {

 "type": "integer"

 },

 "rRMPolicyMarginMinRation": {

 "type": "integer"

 }

 }

 },

 "Mnc": {

 "type": "string",

 "pattern": "[0-9]{3}|[0-9]{2}"

 },

 "PlmnId": {

 "type": "object",

 "properties": {

 "mcc": {

 "$ref": "genericNrm.json#/components/schemas/Mcc"

 },

 "mnc": {

 "$ref": "#/components/schemas/Mnc"

 }

 }

 },

 "PlmnIdList": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/PlmnId"

 }

 },

 "LocalAddress": {

 "type": "object",

 "properties": {

 "ipv4Address": {

 "$ref": "genericNrm.json#/components/schemas/Ipv4Addr"

 },

 "ipv6Address": {

 "$ref": "genericNrm.json#/components/schemas/Ipv6Addr"

 },

 "vlanId": {

 "type": "integer",

 "minimum": 0,

 "maximum": 4096

 },

 "port": {

 "type": "integer",

 "minimum": 0,

 "maximum": 65535

 }

 }

 },

 "RemoteAddress": {

 "type": "object",

 "properties": {

 "ipv4Address": {

 "$ref": "genericNrm.json#/components/schemas/Ipv4Addr"

 },

 "ipv6Address": {

 "$ref": "genericNrm.json#/components/schemas/Ipv6Addr"

 }

 }

 },

 "CellIndividualOffset": {

 "type": "object",

 "properties": {

 "rsrpOffsetSSB": {

 "type": "integer"

 },

 "rsrqOffsetSSB": {

 "type": "integer"

 },

 "sinrOffsetSSB": {

 "type": "integer"

 },

 "rsrpOffsetCSI-RS": {

 "type": "integer"

 },

 "rsrqOffsetCSI-RS": {

 "type": "integer"

 },

 "sinrOffsetCSI-RS": {

 "type": "integer"

 }

 }

 },

 "QOffsetRange": {

 "type": "integer",

 "enum": [

 -24,

 -22,

 -20,

 -18,

 -16,

 -14,

 -12,

 -10,

 -8,

 -6,

 -5,

 -4,

 -3,

 -2,

 -1,

 0,

 24,

 22,

 20,

 18,

 16,

 14,

 12,

 10,

 8,

 6,

 5,

 4,

 3,

 2,

 1

 ]

 },

 "QOffsetRangeList": {

 "type": "object",

 "properties": {

 "rsrpOffsetSSB": {

 "$ref": "#/components/schemas/QOffsetRange"

 },

 "rsrqOffsetSSB": {

 "$ref": "#/components/schemas/QOffsetRange"

 },

 "sinrOffsetSSB": {

 "$ref": "#/components/schemas/QOffsetRange"

 },

 "rsrpOffsetCSI-RS": {

 "$ref": "#/components/schemas/QOffsetRange"

 },

 "rsrqOffsetCSI-RS": {

 "$ref": "#/components/schemas/QOffsetRange"

 },

 "sinrOffsetCSI-RS": {

 "$ref": "#/components/schemas/QOffsetRange"

 }

 }

 },

 "QOffsetFreq": {

 "type": "number"

 },

 "TReselectionNRSf": {

 "type": "integer",

 "enum": [

 25,

 50,

 75,

 100

 ]

 },

 "SsbPeriodicity": {

 "type": "integer",

 "enum": [

 5,

 10,

 20,

 40,

 80,

 160

 ]

 },

 "SsbDuration": {

 "type": "integer",

 "enum": [

 1,

 2,

 3,

 4,

 5

 ]

 },

 "SsbSubCarrierSpacing": {

 "type": "integer",

 "enum": [

 15,

 30,

 120,

 240

 ]

 },

 "coverageShape": {

 "type": "integer",

 "maximum": 65535

 },

 "digitalTilt": {

 "type": "integer",

 "minimum": -900,

 "maximum": 900

 },

 "digitalAzimuth": {

 "type": "integer",

 "minimum": -1800,

 "maximum": 1800

 },

 "ANRManagementCellPolicy": {

 "type": "object",

 "properties": {

 "isRemoveAllowed": {

 "type": "boolean"

 },

 "isHOAllowed": {

 "type": "boolean"

 }

 "NRCellRelationRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 },

 "GnbDuFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbDuId": {

 "$ref": "#/components/schemas/GnbDuId"

 },

 "gnbDuName": {

 "$ref": "#/components/schemas/GnbName"

 },

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_F1C": {

 "$ref": "#/components/schemas/EP\_F1C"

 },

 "EP\_F1U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1U"

 }

 },

 "NrCellDu": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NrCellDu"

 }

 },

 "NrSectorCarrier": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NrSectorCarrier"

 }

 },

 "Bwp": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/Bwp"

 }

 },

 "CommonBeamformingFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/CommonBeamformingFunction"

 }

 },

 "Beam": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/Beam"

 }

 }

 }

 }

 ]

 },

 "GnbCuCpFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 },

 "gnbCuName": {

 "$ref": "#/components/schemas/GnbName"

 },

 "plmnId": {

 "$ref": "#/components/schemas/PlmnId"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_F1C": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1C"

 }

 },

 "EP\_E1": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_E1"

 }

 },

 "EP\_XnC": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_XnC"

 }

 },

 "EP\_X2C": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_X2C"

 }

 },

 "EP\_NgC": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_NgC"

 }

 },

 "NrCellCu": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NrCellCu"

 }

 },

 "ANRManagementFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ANRManagementFunction"

 }

 }

 }

 }

 ]

 },

 "GnbCuUpFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 },

 "gnbCuUpId": {

 "$ref": "#/components/schemas/GnbCuUpId"

 },

 "plmnIdList": {

 "$ref": "#/components/schemas/PlmnIdList"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_E1": {

 "$ref": "#/components/schemas/EP\_E1"

 },

 "EP\_F1U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1U"

 }

 },

 "EP\_XnU": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_XnU"

 }

 },

 "EP\_NgU": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_NgU"

 }

 },

 "EP\_X2U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_X2U"

 }

 },

 "EP\_S1U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_S1U"

 }

 }

 }

 }

 ]

 },

 "NrCellCu": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "cellLocalId": {

 "type": "integer"

 },

 "plmnIdList": {

 "$ref": "#/components/schemas/PlmnIdList"

 },

 "snssaiList": {

 "$ref": "#/components/schemas/SnssaiList"

 },

 "rrmPolicyType": {

 "type": "integer"

 },

 "rrmPolicyNSSIId": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 },

 "rrmPolicyRatio": {

 "type": "integer"

 },

 "rrmPolicy": {

 "$ref": "#/components/schemas/RrmPolicy"

 },

 "rrmPolicyRatio2": {

 "$ref": "#/components/schemas/RrmPolicyRatio2"

 },

 "nRFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "NRCellRelation": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NRCellRelation"

 }

 },

 "NRFreqRelation": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NRFreqRelation"

 }

 },

 "EUtranCellRelation": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EUtranCellRelation"

 }

 },

 "EUtranFreqRelation": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EUtranFreqRelation"

 }

 }

 }

 }

 ]

 },

 "NrCellDu": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "administrativeState": {

 "$ref": "genericNrm.json#/components/schemas/AdministrativeState"

 },

 "operationalState": {

 "$ref": "genericNrm.json#/components/schemas/OperationalState"

 },

 "cellLocalId": {

 "type": "integer"

 },

 "cellState": {

 "$ref": "#/components/schemas/CellState"

 },

 "plmnIdList": {

 "$ref": "#/components/schemas/PlmnIdList"

 },

 "snssaiList": {

 "$ref": "#/components/schemas/SnssaiList"

 },

 "nrPci": {

 "$ref": "#/components/schemas/NrPci"

 },

 "nrTac": {

 "$ref": "#/components/schemas/NrTac"

 },

 "arfcnDL": {

 "type": "integer"

 },

 "arfcnUL": {

 "type": "integer"

 },

 "arfcnSUL": {

 "type": "integer"

 },

 "bSChannelBwDL": {

 "type": "integer"

 },

 "bSChannelBwUL": {

 "type": "integer"

 },

 "bSChannelBwSUL": {

 "type": "integer"

 },

 "ssbFrequency": {

 "type": "integer",

 "minimum": 0,

 "maximum": 3279165

 },

 "ssbPeriodicity": {

 "$ref": "#/components/schemas/SsbPeriodicity"

 },

 "ssbSubCarrierSpacing": {

 "$ref": "#/components/schemas/SsbSubCarrierSpacing"

 },

 "ssbOffset": {

 "type": "integer",

 "minimum": 0,

 "maximum": 159

 },

 "ssbDuration": {

 "$ref": "#/components/schemas/SsbDuration"

 },

 "nrSectorCarrierRef": {

 "type": "array",

 "items": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 },

 "bwpRef": {

 "type": "array",

 "items": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 },

 "nRFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "NrSectorCarrier": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "txDirection": {

 "$ref": "#/components/schemas/TxDirection"

 },

 "configuredMaxTxPower": {

 "type": "integer"

 },

 "arfcnDL": {

 "type": "integer"

 },

 "arfcnUL": {

 "type": "integer"

 },

 "bSChannelBwDL": {

 "type": "integer"

 },

 "bSChannelBwUL": {

 "type": "integer"

 },

 "sectorEquipmentFunctionRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "Bwp": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "bwpContext": {

 "$ref": "#/components/schemas/BwpContext"

 },

 "isInitialBwp": {

 "$ref": "#/components/schemas/IsInitialBwp"

 },

 "subCarrierSpacing": {

 "type": "integer"

 },

 "cyclicPrefix": {

 "$ref": "#/components/schemas/CyclicPrefix"

 },

 "startRB": {

 "type": "integer"

 },

 "numberOfRBs": {

 "type": "integer"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "CommonBeamformingFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "type": "object",

 "properties": {

 "coverageShape": {

 "type": "#/components/schemas/coverageShape"

 },

 "digitalAzimuth": {

 "type": "#/components/schemas/digitalAzimuth"

 },

 "digitalTilt": {

 "type": "#/components/schemas/digitalTilt"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "Beam": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "type": "object",

 "properties": {

 "beamIndex": {

 "type": "integer"

 },

 "beamType": {

 "type": "string",

 "enum": [

 "SSB-BEAM"

 ]

 },

 "beamAzimuth": {

 "type": "integer",

 "minimum": -1800,

 "maximum": 1800

 },

 "beamTilt": {

 "type": "integer",

 "minimum": -900,

 "maximum": 900

 },

 "beamHorizWidth": {

 "type": "integer",

 "minimum": 0,

 "maximum": 3599

 },

 "beamVertWidth": {

 "type": "integer",

 "minimum": 0,

 "maximum": 1800

 }

 }

 }

 ]

 }

 }

 }

 ]

 },

 "ExternalGnbDuFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_F1C": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1C"

 }

 },

 "EP\_F1U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1U"

 }

 }

 }

 }

 ]

 },

 "ExternalGnbCuCpFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 },

 "plmnId": {

 "$ref": "#/components/schemas/PlmnId"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "ExternalNrCellCu": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ExternalNrCellCu"

 }

 },

 "EP\_F1C": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1C"

 }

 },

 "EP\_E1": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_E1"

 }

 },

 "EP\_XnC": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_XnC"

 }

 }

 }

 }

 ]

 },

 "ExternalGnbCuUpFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "gnbId": {

 "$ref": "#/components/schemas/GnbId"

 },

 "gnbIdLength": {

 "$ref": "#/components/schemas/GnbIdLength"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_E1": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_E1"

 }

 },

 "EP\_F1U": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_F1U"

 }

 },

 "EP\_XnU": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_XnU"

 }

 }

 }

 }

 ]

 },

 "ExternalAmfFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_NgC": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_NgC"

 }

 }

 }

 }

 ]

 },

 "ExternalUpfFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "EP\_NgU": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EP\_NgU"

 }

 }

 }

 }

 ]

 },

 "ExternalNrCellCu": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "cellLocalId": {

 "type": "integer"

 },

 "nrPci": {

 "$ref": "#/components/schemas/NrPci"

 },

 "plmnIdList": {

 "$ref": "#/components/schemas/PlmnIdList"

 },

 "nRFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "NRCellRelation": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "nRTCI": {

 "type": "integer"

 },

 "cellIndividualOffset": {

 "$ref": "#/components/schemas/CellIndividualOffset"

 },

 "adjacentNRCellRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 },

 "nRFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "NRFreqRelation": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "offsetMO": {

 "$ref": "#/components/schemas/QOffsetRangeList"

 },

 "blackListEntry": {

 "type": "array",

 "items": {

 "type": "integer",

 "minimum": 0,

 "maximum": 1007

 }

 },

 "blackListEntryIdleMode": {

 "type": "integer"

 },

 "cellReselectionPriority": {

 "type": "integer"

 },

 "cellReselectionSubPriority": {

 "type": "number",

 "minimum": 0.2,

 "maximum": 0.8,

 "multipleOf": 0.2

 },

 "pMax": {

 "type": "integer",

 "minimum": -30,

 "maximum": 33

 },

 "qOffsetFreq": {

 "$ref": "#/components/schemas/QOffsetFreq"

 },

 "qQualMin": {

 "type": "number"

 },

 "qRxLevMin": {

 "type": "integer",

 "minimum": -140,

 "maximum": -44

 },

 "threshXHighP": {

 "type": "integer",

 "minimum": 0,

 "maximum": 62

 },

 "threshXHighQ": {

 "type": "integer",

 "minimum": 0,

 "maximum": 31

 },

 "threshXLowP": {

 "type": "integer",

 "minimum": 0,

 "maximum": 62

 },

 "threshXLowQ": {

 "type": "integer",

 "minimum": 0,

 "maximum": 31

 },

 "tReselectionNr": {

 "type": "integer",

 "minimum": 0,

 "maximum": 7

 },

 "tReselectionNRSfHigh": {

 "$ref": "#/components/schemas/TReselectionNRSf"

 },

 "tReselectionNRSfMedium": {

 "$ref": "#/components/schemas/TReselectionNRSf"

 },

 "nRFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "NRFrequency": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "absoluteFrequencySSB": {

 "type": "integer",

 "minimum": 0,

 "maximum": 3279165

 },

 "ssbSubCarrierSpacing": {

 "$ref": "#/components/schemas/SsbSubCarrierSpacing"

 },

 "multiFrequencyBandListNR": {

 "type": "integer",

 "minimum": 1,

 "maximum": 256

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "ExternalENBFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "eNBId": {

 "type": "integer"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "ExternalEUTranCell": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ExternalEUTranCell"

 }

 }

 }

 }

 ]

 },

 "ExternalEUTranCell": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "EUtranFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "EUtranCellRelation": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "adjacentEUtranCellRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "EUtranFreqRelation": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "eUTranFrequencyRef": {

 "$ref": "genericNrm.json#/components/schemas/Dn"

 }

 }

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "EUtranFrequency": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

 },

 {

 "type": "object",

 "properties": {}

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

 }

 ]

 },

 "ManagedElement-Single": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedElement-Attributes"

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/ManagedElement-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "GnbDuFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/GnbDuFunction"

 }

 },

 "GnbCuCpFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/GnbCuCpFunction"

 }

 },

 "GnbCuUpFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/GnbCuUpFunction"

 }

 }

 }

 }

 ]

 },

 "ManagedElement-Multiple": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ManagedElement-Single"

 }

 },

 "SubNetwork-Single": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/SubNetwork-Attributes"

 }

 ]

 }

 }

 },

 {

 "$ref": "genericNrm.json#/components/schemas/SubNetwork-ContainingObjects"

 },

 {

 "type": "object",

 "properties": {

 "SubNetwork": {

 "$ref": "#/components/schemas/SubNetwork-Multiple"

 },

 "ManagedElement": {

 "$ref": "#/components/schemas/ManagedElement-Multiple"

 },

 "ExternalGnbCuCpFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ExternalGnbCuCpFunction"

 }

 },

 "ExternalENBFunction": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/ExternalENBFunction"

 }

 },

 "NRFrequency": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/NRFrequency"

 }

 },

 "EUtranFrequency": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/EUtranFrequency"

 }

 }

 }

 }

 ]

 },

 "SubNetwork-Multiple": {

 "type": "array",

 "items": {

 "$ref": "#/components/schemas/SubNetwork-Single"

 }

 },

 "EP\_RP": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "type": "object",

 "properties": {

 "userLabel": {

 "type": "string"

 },

 "farEndEntity": {

 "type": "string"

 },

 "localAddress": {

 "$ref": "#/components/schemas/LocalAddress"

 },

 "remoteAddress": {

 "$ref": "#/components/schemas/RemoteAddress"

 }

 }

 }

 }

 }

 ]

 },

 "EP\_E1": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_XnC": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_XnU": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_NgC": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_NgU": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_F1C": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_F1U": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_S1U": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_X2C": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "EP\_X2U": {

 "$ref": "#/components/schemas/EP\_RP"

 },

 "ANRManagementFunction": {

 "allOf": [

 {

 "$ref": "genericNrm.json#/components/schemas/Top-Attributes"

 },

 {

 "type": "object",

 "properties": {

 "attributes": {

 "allOf": [

 {

 "type": "object",

 "properties": {

 "x2BlackList": {

 "$ref": "genericNrm.json#/components/schemas/DnList"

 },

 "x2WhiteList": {

 "$ref": "genericNrm.json#/components/schemas/DnList"

 },

 "xnBlackList": {

 "$ref": "genericNrm.json#/components/schemas/DnList"

 },

 "xnWhiteList": {

 "$ref": "genericNrm.json#/components/schemas/DnList"

 },

 "x2XnHOBlackList": {

 "$ref": "genericNrm.json#/components/schemas/DnList"

 },

 "intrasystemANRManagementSwitch": {

 "type": "boolean"

 },

 "intersystemANRManagementSwitch": {

 "type": "boolean"

 },

 "aNRManagementCellPolicy": {

 "$ref": "#/components/schemas/ANRManagementCellPolicy"

 }

 }

 }

 ]

 }

 }

 }

 ]

 }

 }

 }

}

|  |
| --- |
| **End of Changes** |