|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **3GPP TSG-SA5 Meeting #130-e *S5-202116*****Online, , 20th Apr 2020 - 28th Apr 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** | **0263** | **rev** | **1** | **Current version:** | **16.4.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |

 |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | CATT |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Implementation of CR after SA#86 need correction |
|  |  |
| ***Summary of change:*** | Replaced [??] with correct [42], and [x] with [50] in text. Correct reference to TS 38.331. |
|  |  |
| ***Consequences if not approved:*** | References to TS 38.101-1 and GST in text are missingReferences to TS 38.331 in text are wrong. |
|  |  |
| ***Clauses affected:*** | 4.4.1, L1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Editorial |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

### 4.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| administrativeState | It indicates the administrative state of the NRCellDU. It describes the permission to use or prohibition against using the cell, imposed through the OAM services.allowedValues: LOCKED, SHUTTING DOWN, UNLOCKED. The meaning of these values is as defined in ITU‑T Recommendation X.731 [18].See Annex A for Relation between the "Pre-operation state of the gNB-DU Cell" and administrative state relevant in case of 2-split and 3-split deployment scenarios. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LOCKEDisNullable: False |
| operationalState | It indicates the operational state of the NRCellDU instance. It describes whether the resource is installed and partially or fully operable (Enabled) or the resource is not installed or not operable (Disabled).allowedValues: ENABLED, DISABLED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| cellState | It indicates the usage state of the NRCellDU instance. It describes whether the cell is not currently in use (Idle), or currently in use but not configured to carry traffic (Inactive) or is currently in use and is configured to carry traffic (Active).The Inactive and Active definitions are in accordance with TS 38.401 [4]:"Inactive: the cell is known by both the gNB-DU and the gNB-CU. The cell shall not serve UEs;Active: the cell is known by both the gNB-DU and the gNB-CU. The cell should be able to serve UEs.""allowedValues: IDLE, INACTIVE, ACTIVE. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnDL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for downlinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for uplinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcnSUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for supplementary uplinkallowedValues: See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| beamAzimuth  | The azimuth of a beam transmission, which means the horizontal beamforming pointing angle (beam peak direction) in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Zero degree implies explicit antenna bearing (boresight). Positive angle implies clockwise from the antenna bearing. allowedValues: [-1800 ..1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamHorizWidth | The Horizontal beamWidth of a beam transmission, which means the horizontal beamforming half-power (3dB down) beamwidth in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53]. allowedValues: [0..3599] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamIndex | Index of the beam.For example, please see subclause 6.6.2 of TS 38.331 [54] where the ssb-Index in the rsIndexResults element of MeasResultNR is defined. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamTilt  | The tilt of a beam transmission, which means the vertical beamforming pointing angle (beam peak direction) in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Positive value implies downtilt.allowedValues: [-900..900] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamType | The type of the beam. allowedValues: "SSB-BEAM" | type: stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| beamVertWidth | The Vertical beamWidth of a beam transmission, which means the vertical beamforming half-power (3dB down) beamwidth in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53]. allowedValues: [0...1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NullisNullable: True |
| bSChannelBwDL  | BS Channel BW in MHz. for downlinkallowedValues: See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bSChannelBwUL  | BS Channel BW in MHz.for uplinkallowedValues:See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bSChannelBwSUL  | BS Channel BW in MHz.for supplementary uplinkallowedValues:See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| configuredMaxTxPower | This is the maximum possible for all downlink channels, used simultaneously in a cell, added together.allowedValues:TBD | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| coverageShape | Identifies the sector carrier coverage shape described by the envelope of the contained SSB beams. The coverage shape is implementation dependent.allowedValues: 0 : 65535 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| digitalTilt | Digitally-controlled tilt through beamforming. It represents the vertical pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical vertical tilt of the selected coverageShape. Positive value gives downwards tilt and negative value gives upwards tilt.allowedValues: [-900..900] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| digitalAzimuth | Digitally-controlled azimuth through beamforming. It represents the horizontal pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical horizontal pan of the selected coverageShape. Positive value gives azimuth to the right and negative value gives an azimuth to the left.allowedValues: [-1800 ..1800] 0.1 degree | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cyclicPrefix | Cyclic prefix as defined in TS 38.211 [32], subclause 4.2.allowedValues: NORMAL, EXTENDED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| localAddress  | This parameter specifies the localAddress including IP address and VLAN ID used for initialization of the underlying transport.First string is IP address, IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).Second string is VLAN Id. (See IEEE 802.1Q [39]), | type: Stringmultiplicity: 2isOrdered: TrueisUnique: N/AdefaultValue: NoneisNullable: False |
| remoteAddress | Remote address including IP address used for initialization of the underlying transport.IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBId | It identifies a gNB within a PLMN. The gNB ID is part of the NR Cell Identifier (NCI) of the gNB cells.See "gNB Identifier (gNB ID)" of subclause 8.2 of TS 38.300 [3]). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5]. allowedValues: 0..4294967295 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBIdLength | This indicates the number of bits for encoding the gNB ID. See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].allowedValues: 22 .. 32. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNB­DUId | It uniquely identifies the DU at least within a gNB-CU. See 'gNB-DU ID' in subclause 9.3.1.9 of 3GPP TS 38.473 [8].allowedValues: 0..236-1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNB­CUUPId | It uniquely identifies the gNB-CU-UP at least within a gNB-CU-CP. See 'gNB-CU-UP ID' in subclause 9.3.1.15 of 3GPP TS 38.463 [48].allowedValues: 0..236-1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBCUName | It identifies the Central Entity of a NR node, see subclause 9.2.1.4 of 3GPP TS 38.473 [8].allowedValues: Not applicable | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| gNBDUName | It identifies the Distributed Entity of a NR node, see subclause 9.2.1.5 of 3GPP TS 38.473 [8].allowedValues: Not applicable | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cellLocalId | It identifies a NR cell of a gNB. It, together with the gNB Identifier (using gNBId of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction), identifies a NR cell within a PLMN. This is the NR Cell Identity (NCI). See subclause 8.2 of TS 38.300 [3]), The NCI can be constructed by encoding the gNB Identifier using gNBId (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction) and cellLocalId where the gNB Identifier field is of length specified by gNBIdLength (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].The NR Cell Global identifier (NCGI) is constructed from the PLMN identity the cell belongs to and the NR Cell Identifier (NCI) of the cell.See relation between NCI and NCGI subclause 8.2 of TS 38.300 [3].allowedValues: Not applicable | type: Integermultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| nRPCI | This holds the Physical Cell Identity (PCI) of the NR cell.allowedValues: See 3GPP TS 36.211 subclause 6.11 for legal values of pci. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRTAC | This holds the identity of the common Tracking Area Code for the PLMNs. allowedValues:a) It is the TAC or Extended-TAC. b) A cell can only broadcast one TAC or Extended-TAC. See TS 36.300, subclause 10.1.7 (PLMNID and TAC relation).c) TAC is defined in subclause 19.4.2.3 of 3GPP TS 23.003[13] and Extended-TAC is defined in subclause 9.3.1.29 of 3GPP TS 38.473 [8].d) For a 5G SA (Stand Alone), it has a non-null value. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NULLisNullable: True |
| GNBCUCPFunction.pLMNId | It specifies the PLMN identifier to be used as part of the global RAN node identity.allowedValues: Not applicable. | Type: PLMNId multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| GNBCUUPFunction.pLMNIdList | This is a list of PLMN identifiers. It defines from which set of PLMNs an UE must have as its serving PLMN to be allowed to use the GNB-CU-UP.allowedValues: Not applicable. | type: PLMNId multiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| NRCellCU.pLMNInfoList | It defines which PLMNs that can be served by the NR cell,and which S-NSSAIs can be supported by the NR cell for corresponding PLMN in case of network slicing feature is supportedallowedValues: Not applicable. | type: PLMNInfomultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| NRCellDU.pLMNInfoList | It defines which PLMNs that can be served by the NR cell, and which S-NSSAs can be supported by the NR cell for corresponding PLMN in case of network slicing feature is supported. The pLMNId of the first entry of the list is the PLMNId used to construct the nCGI for the NR cell.allowedValues: Not applicable. | type: PLMNInfomultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| ExternalNRCellCU.pLMNIdList | It defines which PLMNs that are assumed to be served by the NR Cell in another gNB-CU-CP. This list is either updated by the managed element itself (e.g. due to ANR, signalling over Xn etc) or by consumer over the standard interface.allowedValues: Not applicable. | Type: PLMNIdmultiplicity: 1..12isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| rRMPolicyMemberList | It represents the list of RRMPolicyMember (s) that the managed object is supporting. A RRMPolicyMember <<dataType>> include the PLMNId <<dataType>> and S-NSSAI <<dataType>>.allowedValues: N/A | type: RRMPolicyMembermultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| resourceType | The resource type of interest for an RRM Policy. allowedValues:PRB (for NRCellDU)RRC connected users (for NRCellCU)DRB (for GNBCUUPFunction)See NOTE 2, NOTE 3 and NOTE 4 | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| sNSSAIList | It represents the list of S-NSSAI the managed object is supporting. The S-NSSAI is defined in 3GPP TS 23.003 [13].allowedValues: See 3GPP TS 23.003 [13] | type: S-NSSAImultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sST | This attribute specifies the Slice/Service type (SST) of the network slice.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sD | This attribute specifies the Slice Differentiator (SD), which is optional information that complements the slice/service type(s) to differentiate amongst multiple Network Slices.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| quotaType | The attribute indicates the type of the quota which allows to allocate resource as strictly usable for defined rRMPolicyMemberList (“strict quota”) or allows that resource to be used by other rRMPolicyMemberList(s) when defined rRMPolicyMemberList do not need them ( “float quota”).allowedValues: STRICT, FLOAT. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rRMPolicyMaxRatio | The RRM policy setting the maximum percentage of radio resources to be allocated to the corresponding rRMPolicyMemberList.This quota can be strict or float quota : - Strict quota means the defined rRMPolicyMemberList cannot be allocated resource if its used resource reached maxRatio. - Float quota means the defined rRMPolicyMemberList can use quota from other rRMPolicyMemberList(s) even if its resource has reached maxRatio, if there’s free quota from other rRMPolicyMemberList. In addition, resource of the defined rRMPolicyMemberList can be used by other rRMPolicyMemberList(s) when the defined rRMPolicyMemberList do not need them.Value 0 indicates that there is no maximum limit.allowedValues:0 : 100 | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMarginMaxRatio | Maximum quota margin ratio is applicable when maximum quota policy ratio is of type “float quota”. It defines the resource quota within maximum quota to reserve buffers for new resource requirements for the defined rRMPolicyMemberList. With the margin ratio, unused resources of the maximum resource quota can be allocated to other rRMPolicyMemberList(s) when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the defined rRMPolicyMemberList.. Value 0 indicates that no margin is used.allowedValues:0 : 100 | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMinRatio | The RRM policy setting the minimum percentage of radio resources to be allocated to the corresponding rRMPolicyMemberList, especially in congestion situation. This quota can be strict or float quota: - Strict quota means resources are not allowed for other rRMPolicyMemberList(s) even when they are not used by the defined rRMPolicyMemberList. -Float quota resources can be used by other rRMPolicyMemberList(s) when the defined rRMPolicyMemberList do not need them.Value 0 indicates that there is no minimum limit.allowedValues: 0 : 100NOTE: The averaging time interval is implementation dependent. | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| rRMPolicyMarginMinRatio | Minimum quota margin ratio is applicable when minimum quota policy ratio is of type “float quota”. It defines the resource quota within minimum quota to reserve buffers for new resource requirements for the defined rRMPolicyMemberList. With the margin ratio, unused resources of the minimum resource quota can be allocated to other rRMPolicyMemberList(s) when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the defined rRMPolicyMemberList. Value 0 indicates that no margin is used.allowedValues:0 : 100  | type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| subCarrierSpacing | Subcarrier spacing configuration for a BWP. See subclause 5 in TS 38.104 [12].AllowedValues: [15, 30, 60, 120] depending on the frequency range FR1 or FR2. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| txDirection | Indicates if the transmission direction is downlink (DL), uplink (UL) or both downlink and uplink (DL and UL).allowedValues:  DL, UL, DL and UL | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| bwpContext | It identifies whether the object is used for downlink, uplink or supplementary uplink.allowedValues: DL, UL, SUL | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| isInitialBwp | It identifies whether the object is used for initial or other BWP.allowedValues: INITIAL, OTHER | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| startRB | Offset in common resource blocks to common resource block 0 for the applicable subcarrier spacing for a BWP. This corresponds to N\_BWP\_start, see subclause 4.4.5 in TS 38.211 [32]. allowedValues:0 to N\_grid\_size – 1, where N\_grid\_size equals the number of resource blocks for the BS channel bandwidth, given the subcarrier spacing of the BWP. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| numberOfRBs | Number of physical resource blocks for a BWP. This corresponds to N\_BWP\_size, see subclause 4.4.5 in TS 38.211 [32].allowedValues:1 to N\_grid\_size – startRB of the BWP. Se startRB for definition of N\_grid\_size. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRTCI | This is the Target NR Cell Identifier. It consists of NR Cell Identifier (NCI) and Physical Cell Identifier of the target NR cell (nRPCI).The NRRelation.nRTCI identifies the target cell from the perspective of the NRCell, the name-containing instance of the subject NRCellCU instance.allowedValues: Not applicable. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| adjacentCellRef | This attribute contains the DN of an adjacentNRCell (NRCellCU or ExternalNRCellCU) allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| ssbFrequency | Indicates cell defining SSB frequency domain positionFrequency of the cell defining SSB transmission. The frequency provided in this attribute identifies the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block. The frequency must be positioned on the NR global frequency raster, as defined in TS 38.101-1 [42] subclause 5.4.2. and within bSChannelBwDL.allowedValues: 0..3279165 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nRFrequencyRef | This attribute contains the DN of the referenced NRFrequency.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| nRSectorCarrierRef | This attribute contains the DN of the referenced NRSectorCarrier.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| bWPRef | This attribute contains the DN of the referenced BWP.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| sectorEquipmentFunctionRef | This attribute contains the DN of the referenced NSectorEquipmentFunction.allowedValues: Not applicable. | type: DNmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| offsetMO | It is a list of offset values applicable to all measured cells with reference signal(s) indicated in this *MeasObjectNR*. See offsetMO of subclause 5.5.4 of TS 38.331 [54].allowedValues: Not applicable. | type: QOffsetRangeListmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: False |
| cellIndividualOffset | It is a list of offset values for the neighbour cell. Used when UE is in connected mode. The unit is 1dB. It is defined for rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, rsrqOffsetCSI-RS and sinrOffsetCSI-RS. See TS 38.331 [54].  allowedValues: Not applicable. | type: Integermultiplicity: 6isOrdered: TrueisUnique: N/AdefaultValue: 0isNullable: False |
| blackListEntry | It specifies a list of PCI (physical cell identity) that are blacklisted in EUTRAN measurements as described in 3GPP TS 38.331 [54].allowedValues: { 0…1007 } | type: Integermultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| blackListEntryIdleMode | It specifies a list of PCI (physical cell identity) that are blacklisted in SIB4 and SIB5.allowedValues: { 0…1007 } | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cellReselectionPriority | It is the absolute priority of the carrier frequency used by the cell reselection procedure. See *CellReselectionPriority* IE in TS 38.331 [54].It corresponds to the parameter priority in 3GPP TS 38.304 [49].Value 0 means lowest priority. The UE behaviour when no value is entered is specified in subclause 5.2.4.1 of 3GPP TS 38.304 [49]. The value must not already used by other RAT, i.e. equal priorities between RATs are not supported.allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0NoneisNullable: False |
| cellReselectionSubPriority | It indicates a fractional value to be added to the value of cellReselectionPriority to obtain the absolute priority of the concerned carrier frequency for E-UTRA and NR. See *CellReselectionSubPriority* IE in TS 38.331 [54].allowedValues: { 0.2, 0.4, 0.6, 0.8 }. | type: Shortmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| pMax | It calculates the parameter Pcompensation (defined in 3GPP TS 38.304 [49]), at cell reselection to an Cell. Its unit is 1 dBm. It corresponds to parameter PEMAX in 3GPP TS 38.101-1 [42]. allowedValues: { -30..33 }.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| qOffsetFreq | It is the frequency specific offset applied when evaluating candidates for cell reselection. See TS 38.331 [49]. Its unit is 1 dB.allowedValues:{ -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 20, 22, 24 } | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0isNullable: False |
| qOffsetRangeList | It is used to indicate a cell, beam or measurement object specific offset to be applied when evaluating candidates for cell re-selection or when evaluating triggering conditions for measurement reporting. The value in dB. Value dB-24 corresponds to -24 dB, dB-22 corresponds to -22 dB and so on.This is a list of enum values representing, in sequence: rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, srqOffsetCSI-RS, sinrOffsetCSI-RS. See Q-OffsetRangeList in subclause of subclause 6.3.1 of TS 38.311 [31].allowedValues: { -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 18, 20, 22, 24 }  | type: ENUMmultiplicity: 6isOrdered: TrueisUnique: N/AdefaultValue: 0isNullable: False |
| qQualMin | It indicates the minimum required quality level in the cell (dB). See qQualMin in TS 38.304 [49]. Unit is 1 dB.Value 0 means that it is not sent and UE applies in such case the (default) value of negative infinity for Qqualmin. Sent in SIB3 or SIB5.allowedValues: { -34..-3, 0 }  | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| qRxLevMin | It indicates the required minimum received Reference Symbol Received Power (RSRP) level in the (E-UTRA) frequency for cell reselection. It corresponds to Qrxlevmin defined in 3GPP TS 38.304 [49]. It is broadcast in SIB3 or SIB5, depending on whether the related frequency is intra- or inter-frequency. Its unit is 1 dBm and resolution is 2.allowedValues: { -140..-44 }. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXHighP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighPin 3GPP TS 38.304 [49]. Its unit is 1 dB and resolution is 2**.**allowedValues: { 0..62 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXHighQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighQ in TS 38.304 [49]. Its unit is 1 dB.allowedValues: { 0..31 } | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXLowP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,LowP in 3GPP TS 38.304 [49]. Its unit is 1 dB. Its resolution is 2.allowedValues: { 0..62 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| threshXLowQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,Low in TS 38.304 [49]. Its unit is 1 dB.allowedValues: {0..31}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNr | It is the cell reselection timer and corresponds to parameter TreselectionRAT for NR defined in 38.331 [54]. Its unit is in seconds. allowedValues: {0..7}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNRSfHigh | The attribute t-ReselectionNr (a parameter TreselectionNR in TS 38.304 [49]) is multiplied with this factor if the UE is in high mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium high state in 3GPP TS 38.304 [49]. The unit is one %.Value mapping:25 = 0.2550 = 0.575 = 0.75100 = 1.0 allowedValues: {25, 50, 75, 100}.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tReselectionNRSfMedium | The attribute t-ReselectionNR (a parameter "TreselectionNR in TS 38.304 [49]”) is multiplied with this factor if the UE is in medium mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium mobility state in 3GPP TS 38.304 [49]. Its unit is one %.Value mapping:25 = 0.2550 = 0.575 = 0.75100 = 1.0 allowedValues: {25, 50, 75, 100}.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| absoluteFrequencySSB | The absolute frequency applicable for a downlink NR carrier frequency associated with the SSB.allowedValues: {0.. 3279165}. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| sSBSubCarrierSpacing | This SSB is used for for synchronization. See subclause 5 in TS 38.104 [12]. Its units are in kHz.allowedValues: {15, 30, 120, 240}.Note that the allowed values of SSB used for representing data, by e.g. a BWP, are: 15, 30, 60 and 120 in units of kHz. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| multiFrequencyBandListNR | It is a list of additional frequency bands the frequency belongs to. The list is automatically set by the gNB.allowedValues: {1..256 }  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbPeriodicity | Indicates cell defined SSB periodicity in number of subframes (ms).The SSB periodicity in msec is used for the rate matching purpose. allowedValues: 5, 10, 20, 40, 80, 160. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbOffset

|  |
| --- |
|  |

 | Indicates cell defining SSB time domain position. Defined as the offset of the measurement window, in number of subframes (ms), in which to receive SS/PBCH blocks, where allowed values depend on the ssbPeriodicity.allowedValues: ssbPeriodicity5 ms 0..4,ssbPeriodicity10 ms 0..9,ssbPeriodicity20 ms 0..19,ssbPeriodicity40 ms 0..39,ssbPeriodicity80 ms 0..79,ssbPeriodicity160 ms 0..159. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ssbDuration

|  |
| --- |
|  |

 | Duration of the measurement window in which to receive SS/PBCH blocks. It is given in number of subframes (ms) (see 38.213 [41], subclause 4.1.allowedValues: 1, 2, 3, 4, 5. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rimRSMonitoringStartTime | This field configures the UTC time when the gNB attempts to start RIM-RS monitoring.allowedValues: containing the information same with xsd: dateTime. | type: String multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| rimRSMonitoringStopTime | This field configures the UTC time when the gNB stops RIM-RS monitoring.allowedValues: containing the information same with xsd: dateTime. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| aggressorSetID | This attributer indicates the associated aggressor gNB Set ID of the cell. (See subclause 7.4.1.6 in TS 38.211 [32]). Editor's Note: The definition of aggressorSetID needs further clarification with RAN1.allowedValues:The bit length of the set ID is maximum 22bit. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| victimSetID | This attributer indicates the associated Victim gNB Set ID of the cell. (See subclause 7.4.1.6 in TS 38.211 [32]). Editor's Note: The definition of victimSetID needs further clarification with RAN1.allowedValues:The bit length of the set ID is maximum 22bit. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mappingSetIDBackhaulAddressList | The attribute specifies a list of mappingSetIDBackhaulAddress which is defined as a datatype (see clause 4.3.47). Which is used to retrieve the backhaul address of the victim set.allowedValues: Not applicable | type: MappingSetIDBackhaulAddressmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| backhaulAddress | The attribute specifies backhaulAddress which is defined as a datatype (see clause 4.3.48). allowedValues: Not applicable | type: BackhaulAddressmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| setID | This specifies the set ID. (See subclause 7.4.1.6 in TS 38.211 [32]). allowedValues:The bit length of the set ID is maximum 22bit. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tAI | Indicates the TAI (see subclause 9.3.3.11 in TS 38.413[5]), including PpLMNId ID and nRTAC. allowedValues: Not applicable  | type: TAImultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| NOTE 1: VoidNOTE 2: The radio resource can be signaling resources (e.g. RRC connected users) or user plane resources (e.g. PRB, DRB). NOTE 3: The averaging time interval is implementation dependent.NOTE 4: A RRM Policy can make use of the defined policy RRMPolicyRatio or a vendor specific RRM Policy. |

|  |
| --- |
| **Next change** |

# L.1 General

This annex describes the relation between GSMA GST[50] and information model ServiceProfile and SliceProfile.

|  |
| --- |
| **End of Change** |