**3GPP TSG-SA5 Meeting #130-e *S5-202160***

**Online, , 20th Apr 2020 - 28th Apr 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.550** | **CR** | **0052** | **rev** | **-** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Clarify performance measurement for a tenant |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | MEMTANE |  | ***Date:*** | 2020-04-10 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | This contribution clarifies what performance measurement can be exposed to a tenant. |
|  |  |
| ***Summary of change:*** | Tenant as a consumer of CSI may associate with S-NSSAI or sNSSAIList. When performance management services are exposed to tenants, 3GPP management system may provide tenant with performance measurements related to S-NSSAI.  |
|  |  |
| ***Consequences if not approved:*** | The performance measurements for tenant are not clear in TS 28.550. |
|  |  |
| ***Clauses affected:*** | 2, 4.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| ***First change*** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[3] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[4] ITU-T Recommendation X.721 (1992): "Information technology - Open Systems Interconnection - Structure of management information: Definition of management information".

[5] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[6] ISO 8601:2000(E) Data elements and interchange formats – Information interchange – Representation of dates and times".

[7] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[8] Void

[9] Void

[10] Void

[11] Void

[12] Void

[13] 3GPP TS 28.628: "Telecommunication management; Self-Organizing Networks (SON) Policy Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[14] 3GPP TS 32.158: "Management and orchestration; Design rules for Representational State Transfer (REST) Solution Sets (SS)".

[15] ITU-T Recommendation X.680 (08/2015) "Information Technology - Abstract Syntax Notation One (ASN.1): Specification of basic notation" (Same as the ISO/IEC International Standard 8824-1).

[16] ITU-T Recommendation X.681 (08/2015) "Information Technology - Abstract Syntax Notation One (ASN.1): Information object specification" (Same as the ISO/IEC International Standard 8824-2).

[17] ITU-T Recommendation X.691 (08/2015) "Information technology - ASN.1 encoding rules: Specification of Packed Encoding Rules (PER)" (Same as the ISO/IEC International Standard 8825-2).

[18] IETF RFC 6455: "The WebSocket Protocol".

[19] IETF RFC 793: "TRANSMISSION CONTROL PROTOCOL".

[20] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[21] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[22] 3GPP TS 23.288: " Technical Specification Group Services and System Aspects; Architecture enhancements for 5G System (5GS) to support network data analytics services".

 [xx] 3GPP TS 28.530: “Technical Specification Group Services and System Aspects; Management and orchestration; Concepts, use cases and requirements”.

|  |
| --- |
| ***Second change*** |

## 4.4 PM services for multiple tenant support

The MnS consumer, acting on behalf of a tenant, may get the performance measurements of a network slice.. Performance measurements specified in TS 28.552 [1] can be split into sub-counters per S-NSSAI. 3GPP management system can use these sub-counters to distinguish performance measurements for different tenants, which might be required when performance measurements are exposed as part of Network Slice as a Service (NSaaS) offer specified in TS 28.530 [xx].

|  |
| --- |
| **End of changes** |