**3GPP TSG-SA5 Meeting #130e *S5-202162rev***

**e-meeting, 20 April– 24 April 2020** Revision of S5-20xxxx

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **32.254** | **CR** | **0011** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add the Retransmission Indicator |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | NAPS-CH |  | ***Date:*** | 2020-04-23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | To keep alignment with TS 32.290, the Retransmission Indicator and One-time Event Type in charging data request should be added.  |
|  |  |
| ***Summary of change:*** | Add the Retransmission indicator and One-time Event Type. |
|  |  |
| ***Consequences if not approved:*** | Can not be aligned with other specifications.  |
|  |  |
| ***Clauses affected:*** | 6.2a.1.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |
| --- |
| **First change** |

##### 6.2a.1.2.1 Charging Data Request message

Table 6.2a.1.2.1.1 illustrates the basic structure of a Charging Data Request message as used for NEF converged charging.

Table 6.2a.1.2.1.1: Charging Data Request message contents

|  |  |  |
| --- | --- | --- |
| **Information Element** | **Category** | **Description** |
| Session Identifier | OC | Described in TS 32.290 [57] |
| Subscriber Identifier | OM | Described in TS 32.290 [57], and holds the identifier of the AF |
| NF Consumer Identification | M | Described in TS 32.290 [57] |
| Invocation Timestamp | M | Described in TS 32.290 [57] |
| Invocation Sequence Number | M | Described in TS 32.290 [57] |
| Retransmission Indicator | - | This field is not applicable. |
| One-time Event | OC | This field indicates, if included, that this is a one-time event and that there will be no update or termination. |
| One-time Event Type | OC | Described in TS 32.290 [57]. |
| Notify URI | OC | This field contains URI to which notifications are sent by the CHF. The latest received value shall always be used at notifications. |
| Triggers | OC | This field is described in TS 32.290 [57] and holds the NEF specific triggers described in clause 5.x |
| Multiple Unit Usage | OC | This field contains the parameters for the quota management request and/or usage reporting. |
| NEF API Charging Information | OM | This field holds the NEF API specific information described in clause 6.3.1.x |

Editor's note: The Multiple Unit Usage is FFS.

|  |
| --- |
| **End of change** |