**3GPP TSG-SA5 Meeting #132e *S5-204229rev1***

**e-meeting 17th 28th August 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **32.255** | **CR** | **0244** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Add support of stateless SMF |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI16, 5GS\_Ph1-DCH |  | ***Date:*** | 2020-08-07 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Notify URI is already included in charging data request message in case of intiate and update. This contribution is to add description of noticiation URI update to CHF when SMF as NF is changed. |
|  |  |
| ***Summary of change:*** | Add description that “the SMF should be able update the Notification when the SMF is changed.” |
|  |  |
| ***Consequences if not approved:*** | The notify URI in charging data request [update] is only allowed in TS 32.255, but the use of it for stateless SMF is not clean. |
|  |  |
| ***Clauses affected:*** | 6.1.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

#### 6.1.1.2 Charging Data Request message

Table 6.1.1.2.1 illustrates the basic structure of a Charging Data Request message from the SMF as used for 5G data connectivity converged charging.

Table 6.1.1.2.1: Charging Data Request message contents

| **Information Element** | **Category for converged charging** | **Category for offline only charging** | **Description** |
| --- | --- | --- | --- |
| Session Identifier | OC | OC | Described in TS 32.290 [57] |
| Subscriber Identifier | OM | M | Described in TS 32.290 [57]In case SUPI is not present (for emergency service), the User Equipment Info in table 6.2.1.2.1. shall be present for identifying the user. |
| NF Consumer Identification | M | M | Described in TS 32.290 [57] |
| NF Functionality | M | OC | Described in TS 32.290 [57] |
| NF Name | OC | OC | Described in TS 32.290 [57] |
| NF Address | OC | OC | Described in TS 32.290 [57] |
| NF PLMN ID | OC | OC | Described in TS 32.290 [57] |
| Invocation Timestamp | M | M | Described in TS 32.290 [57] |
| Invocation Sequence Number | M | M | Described in TS 32.290 [57] |
| Notify URI | OC | OC | Described in TS 32.290 [57] and the new SMF instance can update the Notify URI when a SMF is deployed as a stateless NF and the SMF is changed. |
| Service Specification Information | OC | OC | Described in TS 32.290 [57] |
| Triggers | OC | OC | This field is described in TS 32.290 [57] and holds the 5G data connectivity specific triggers described in clause 5.2.1. |
| Multiple Unit Usage  | OC | OC | Described in TS 32.290 [57]This field is not applicable to QBC. |
| Rating Group | M | M | Described in TS 32.290 [57] |
| Requested Unit | OC | - | Described in TS 32.290 [57] |
| Used Unit Container | OC | OC | Described in TS 32.290 [57] |
| Triggers | OC | OC | This field is described in TS 32.290 [57] and holds the 5G data connectivity specific triggers described in clause 5.2.1.  |
| PDU Container Information  | OC | OC | This field holds the 5G data connectivity PDU session container specific information described in clause 6.2. |
| UPF ID | OC | OC | This field holds the UPF identifier used to identify the UPF.These fields shall only be included when either quota is requested per UPF, or used units are reported per UPF |
| PDU Session Charging Information | OM | OM | This field holds the 5G data connectivity specific information described in clause 6.2. |
| Roaming QBC information | OM | OM | This field holds the roaming QBC specific information defined in clause 6.2.1.4This field is not applicable to FBC. |

|  |
| --- |
| **End of change** |