**3GPP TSG-SA5 Meeting #132e *S5-204371rev2***

**e-meeting 17th 28th August 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** | **0264** | **rev** | **1** | **Current version:** | **15.6.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction on Converged Charging and Requested Unit handling |
|  |  |
| ***Source to WG:*** | Matrixx |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 5GS\_Ph1-SBI\_CH  |  | ***Date:*** | 2020-08-26 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The current Nchf interface description does not contains the clarification on presence of Requested Unit Information element in the Charging Data Request message, which could be either missing or empty for the selection of charging service support without (offline) or with (online) quota management as well as how Unit determination and Rating (centralized /decentralized) will be done based on the presence of parameter in the RequestedUnit parameter.Only possible to send an empty RequestedUnit but it’s stated that “If none is included the category and amount is determined by CHF.” |
|  |  |
| ***Summary of change:*** | Refinement on the presence of Requested Unit in the table for the usage of centralized unite determination and rating in absence . |
|  |  |
| ***Consequences if not approved:*** | Charging errors on Nchf interface due too different Requested Unit handling  |
|  |  |
| ***Clauses affected:*** | 6.1.6.2.1.9 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | TS 32.290 CR 0129 |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

######

###### 6.1.6.2.1.9 Type RequestedUnit

Table 6.1.6.2.1.9-1: Definition of type RequestedUnit

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| time | Uint32 | OC | 0..1 | This field holds the amount of requested time. |  |
| totalVolume | Uint64 | OC | 0..1 | This field holds the amount of requested volume in both uplink and downlink directions. |  |
| uplinkVolume | Uint64 | OC | 0..1 | This field holds the amount of requested volume in uplink direction. |  |
| downlinkVolume | Uint64 | OC | 0..1 | This field holds the amount of requested volume in downlink direction. |  |
| serviceSpecificUnits | Uint64 | OC | 0..1 | This field holds the amount of requested service specific units. |  |
| NOTE 1: If none of them is included, "RequestedUnit": {}, the category and amount is determined by CHF for online charging scenario with centralized unit determination and rating scenario.  |

|  |
| --- |
|  |

|  |
| --- |
| **End of changes** |