**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0265** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | X | Core Network | X |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_SLICE\_ePA-KPI | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Section 5.4.6.1 says “This measurement provides the average round-trip GTP packet delay between PSA UPF and UE (\*\*including UE processing time\*\*”. The calculation depend on the avaliability of QFI, TEID, sequence number and QMP indicator at UE.  The measurement of “Round-trip packet delay between PSA UPF and UE” is not doable because TEID, sequence number and QMP indicator are not transmitted to the UE | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Deleting measurements “Round-trip packet delay between PSA UPF and UE”. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not implementable measurement definition. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.6.1, 6.4.6.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | X | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | X | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | X | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

### 

### 

|  |
| --- |
| **Start of 1st modification** |

### 5.4.6 Void

### 5.4.7 One way packet delay between NG-RAN and PSA UPF

#### 5.4.7.1 UL packet delay between NG-RAN and PSA UPF

##### 5.4.7.1.1 Average UL GTP packet delay between PSA UPF and NG-RAN

a) This measurement provides the average UL GTP packet delay between PSA UPF and NG-RAN. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy.

For each GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The 5QI and S-NSSAI associated to the GTP PDU.

The PSA UPF counts the number (N) of GTP PDU monitoring response packets for each 5QI and each S-NSSAI respectively, and takes the following calculation for each 5QI and each S-NSSAI:

d) Each measurement is a real representing the average delay in microseconds.

e) GTP.DelayUlPsaUpfNgranMean.*5QI, where 5QI* identifies the 5QI;   
GTP.DelayUlPsaUpfNgranMean.*SNSSAI, where SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

##### 5.4.7.1.2 Distribution of UL GTP packet delay between PSA UPF and NG-RAN

a) This measurement provides the distribution of UL GTP packet delay between PSA UPF and NG-RAN. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy.

For each GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T3 received in the GTP-U header indicating the local time that the NG-RAN sent out the monitoring response packet to the UPF;

- T4 that the monitoring response packet received by the PSA UPF;

- The 5QI and S-NSSAI associated to the DL GTP PDU.

The PSA UPF 1) takes the following calculation for each GTP PDU monitoring response packets for each 5QI and each S-NSSAI respectively, and 2) increment the corresponding bin with the delay range where the result of 1) falls into by 1 for the subcounters per 5QI and subcounters per S-NSSAI.

d) Each measurement is an integer representing the number of GTP PDUs measured with the delay within the range of the bin.

e) GTP.DelayUlPsaUpfNgranDist.*5QI*.*Bin,* Where *Bin* indicates a delay range which is vendor specific, and *5QI* identifies the 5QI;   
GTP.DelayUlPsaUpfNgranDist.*SNSSAI.bin,* Where *Bin* indicates a delay range which is vendor specific, and *SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

### 5.4.8 Round-trip packet delay between PSA UPF and NG-RAN

#### 5.4.8.1 Average round-trip packet delay between PSA UPF and NG-RAN

a) This measurement provides the average round-trip GTP packet delay between PSA UPF and NG-RAN. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are not time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy.

For each received GTP PDU monitoring response packet (packet i) encapsulated with QFI, TEID, and QMP indicator for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T1 received in the GTP-U header of the monitoring response packet indicating the local time that the DL GTP PDU was sent by the PSA UPF;

- T2 received in the GTP-U header of the monitoring response packet indicating the local time that the DL GTP PDU was received by NG-RAN;

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The 5QI and S-NSSAI associated to the DL GTP PDU.

The PSA UPF counts the number (N) of received GTP PDU monitoring response packets for each 5QI and each S-NSSAI respectively, and takes the following calculation for each 5QI and each S-NSSAI:

d) Each measurement is a real representing the average delay in microseconds.

e) GTP.RttDelayPsaUpfNgranMean.*5QI, where 5QI* identifies the 5QI;   
GTP.RttDelayPsaUpfNgranMean.*SNSSAI, where SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

#### 5.4.8.2 Distribution of round-trip packet delay between PSA UPF and NG-RAN

a) This measurement provides the distribution of round-trip GTP packet delay between PSA UPF and NG-RAN. This measurement is split into subcounters per 5QI and subcounters per S-NSSAI. This measurement is only applicable to the case the PSA UPF and NG-RAN are not time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

The UPF samples the GTP packets for QoS monitoring based on the policy provided by OAM or SMF.

NOTE: The sampling rate may vary for different S-NSSAI and different 5QIs, and the specific sampling rate is up to implementation unless given by the QoS monitoring policy.

For each received GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T1 received in the GTP-U header of the monitoring response packet indicating the local time that the DL GTP PDU was sent by the PSA UPF;

- T2 received in the GTP-U header of the monitoring response packet indicating the local time that the DL GTP PDU was received by NG-RAN;

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The 5QI and S-NSSAI associated to the DL GTP PDU.

The PSA UPF 1) takes the following calculation for each received GTP PDU monitoring response packet (packet i) for each 5QI and each S-NSSAI respectively, and 2) increment the corresponding bin with the delay range where the result of 1) falls into by 1 for the subcounters per 5QI and subcounters per S-NSSAI.

d) Each measurement is an integer representing the number of DL GTP PDUs measured with the delay within the range of the bin.

e) GTP.RttDelayPsaUpfNgranDist.*5QI*.*Bin,* Where *Bin* indicates a delay range which is vendor specific, and *5QI* identifies the 5QI;   
GTP.RttDelayPsaUpfNgranDist.*SNSSAI.bin,* Where *Bin* indicates a delay range which is vendor specific, and *SNSSAI* identifies the S-NSSAI.

f) EP\_N3 (contained by UPFFunction);   
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.