**3GPP TSG-SA5 Meeting #133e *S5-205047rev2***

**e-meeting 12th - 21st October 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.554** | **CR** | **0059** | **rev** | **1** | **Current version:** | **15.4.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correct UDM e2e KPI | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NETSLICE-ADPM5G | | | | |  | ***Date:*** | | | 2020-09-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The 28.552 CR0038r2 and the 28.554 CR0005r2 removed subcounters per network slice, therefore it is impossible to calculate the number of registered subscribers through UDM per network slice. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The KPI for UDM is changed from the number of subscribers that are registered to a network slice to the number of subscribers that are registered to a network. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Current desciption on UDM KPI is incorrect. KPI cannot be supported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

|  |
| --- |
| **First Modified Sections** |

## 6.2.2 Registered Subscribers of Network through UDM

a) Registered Subscribers of Network through UDM

b) This KPI describes the total number of subscribers that are registered to a network through UDM.

c) This KPI is corresponding to the measurement RM.RegisteredSubUDMNbrMean that counts subscribers registered in UDM..

d) 

e) RegisteredSubUDMNbrMean

f) 5GS

g) Accessibility

h) Integer

i) CUM

|  |
| --- |
| **End of Modified Sections** |