**3GPP TSG-SA5 Meeting #133-e *S5-205095***

**Online, , 12th Oct 2020 - 21st Oct 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.313** | **CR** | **0001** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | R16 CR TS 28.313 add subclause reference for ranges of handover parameters |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | SON\_5G |  | ***Date:*** | 2020-10-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | MRO function in TS 38.300 and TS 38.423 are available, subclause reference for MRO parameters should be added. |
|  |  |
| ***Summary of change:*** | Add subclause of TS 38.300 and TS 38.423 for MRO function. |
|  |  |
| ***Consequences if not approved:*** | The MRO Function would not be clear. |
|  |  |
| ***Clauses affected:*** | 7.1.2.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st modified section** |

7.1.2.2.3 Parameters to be updated

**Table 7.1.2.2.3-1. Ranges of handover parameters**

| **Control parameters** | **Definition** | **Legal Values** |
| --- | --- | --- |
| Maximum deviation of Handover Trigger | This parameter defines the maximum allowed absolute deviation of the Handover Trigger, from the default point of operation (see subclause 15.5.2.5 in TS 38.300 [7] and subclause 9.2.2.61 in TS 38.423 [17]). | [-20..20] in unit 0.5 dB |
| Minimum time between Handover Trigger changes | This parameter defines the minimum allowed time interval between two Handover Trigger change performed by MRO. This is used to control the stability and convergence of the algorithm (see subclause 15.5.2.5 in TS 38.300 [7]). | [0.. 604800] in unit Seconds |
| Tstore\_UE\_cntxt | The timer used for detection of too early HO, too late HO and HO to wrong cell. Corresponds to Tstore\_UE\_cntxt timer described in subclause 15.5.2.5 in TS 38.300 [7]. | [0..1023] in unit 100 milliseconds |

|  |
| --- |
| **End of modified section** |