**3GPP TSG-SA5 Meeting #133-e *S5-205283***

**Online, , 12th Oct 2020 - 21st Oct 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** |  | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **×** |

|  |
| --- |
|  |
| ***Title:***  | CR Rel-17 ServiceProfle to SliceProfile Translation Stage 3 |
|  |  |
| ***Source to WG:*** | Samsung Research America, Telefonica, China Mobile, Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | EMA5SLA |  | ***Date:*** | 2020-10-01 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Stage 3 for 205039 |
|  |  |
| ***Summary of change:*** | YAML definition for 205039 |
|  |  |
| ***Consequences if not approved:*** | Missing Stage 3 |
|  |  |
| ***Clauses affected:*** | 6.3.4.2, 6.3.x(new), 6.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **×** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **×** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **×** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This is input to the Rel-17 28.541 DraftCR for ServiceProfile to SliceProfile translationForge Branch: https://forge.3gpp.org/rep/sa5/MnS/raw/S5-205283\_ServiceProfle\_to\_SliceProfile\_Translation\_Stage\_3.docx/OpenAPI/sliceNrm.yaml |
|  |  |
| ***This CR's revision history:*** |  |

## J.4.3 OpenAPI document "sliceNrm.yaml"

openapi: 3.0.1

info:

 title: Slice NRM

 version: 16.5.0

 description: >-

 OAS 3.0.1 specification of the Slice NRM

 @ 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.541 V16.4.0; 5G NRM, Slice NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

 schemas:

#------------ Type definitions ---------------------------------------------------

 Float:

 type: number

 format: float

 MobilityLevel:

 type: string

 enum:

 - STATIONARY

 - NOMADIC

 - RESTRICTED MOBILITY

 - FULLY MOBILITY

 SharingLevel:

 type: string

 enum:

 - SHARED

 - NON-SHARED

 ServiceType:

 type: string

 enum:

 - eMBB

 - RLLC

 - MIoT

 - V2X

 PerfReqEmbb:

 type: object

 properties:

 expDataRateDL:

 type: number

 expDataRateUL:

 type: number

 areaTrafficCapDL:

 type: number

 areaTrafficCapUL:

 type: number

 userDensity:

 type: number

 activityFactor:

 type: number

 PerfReqEmbbList:

 type: array

 items:

 $ref: '#/components/schemas/PerfReqEmbb'

 PerfReqUrllc:

 type: object

 properties:

 cSAvailabilityTarget:

 type: number

 cSReliabilityMeanTime:

 type: string

 expDataRate:

 type: number

 msgSizeByte:

 type: string

 transferIntervalTarget:

 type: string

 survivalTime:

 type: string

 PerfReqUrllcList:

 type: array

 items:

 $ref: '#/components/schemas/PerfReqUrllc'

 PerfReq:

 oneOf:

 - $ref: '#/components/schemas/PerfReqEmbbList'

 - $ref: '#/components/schemas/PerfReqUrllcList'

 Category:

 type: string

 enum:

 - CHARACTER

 - SCALABILITY

 Tagging:

 type: string

 enum:

 - PERFORMANCE

 - FUNCTION

 - OPERATION

 Exposure:

 type: string

 enum:

 - API

 - KPI

 ServAttrCom:

 type: object

 properties:

 category:

 $ref: '#/components/schemas/Category'

 tagging:

 $ref: '#/components/schemas/Tagging'

 exposure:

 $ref: '#/components/schemas/Exposure'

 Support:

 type: string

 enum:

 - NOT SUPPORTED

 - SUPPORTED

 DelayTolerance:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 DeterministicComm:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 availability:

 $ref: '#/components/schemas/Support'

 periodicityList:

 type: string

 DLThptPerSlice:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 DLThptPerUE:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerSlice:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerUE:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 MaxPktSize:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 maxsize:

 type: integer

 MaxNumberofPDUSessions:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 nOofPDUSessions:

 type: integer

 KPIMonitoring:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 kPIList:

 type: string

 NBIoT:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 UserMgmtOpen:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 V2XCommModels:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 v2XMode:

 $ref: '#/components/schemas/Support'

 TermDensity:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 density:

 type: integer

 NsInfo:

 type: object

 properties:

 nsInstanceId:

 type: string

 nsName:

 type: string

 CNSliceSubnetProfile:

 type: object

 properties:

 maxNumberofUEs:

 type: Integer

 latency:

 type: Integer

 dLThptPerSlice:

 type: '#/components/schemas/DLThpt'

 dLThptPerUE:

 type: '#/components/schemas/DLThpt'

 uLThptPerSlice:

 type: '#/components/schemas/ULThpt'

 uLThptPerUE:

 type: '#/components/schemas/ULThpt'

 maxNumberOfPDUSessions:

 type: Integer

 RANSliceSubnetProfile:

 type: object

 properties:

 coverageAreaGeoPolygon:

 type: String

 coverageAreaTAList:

 type: Integer

 MobilityLevel:

 $ref: '#/components/schemas/MobilityLevel'

 resourceSharingLevel:

 $ref: '#/components/schemas/SharingLevel'

 maxNumberofUEs:

 type: Integer

 activityFactor:

 type: Float

 dLThptPerUE:

 $ref: '#/components/schemas/ULThpt'

 uLThptPerUE:

 $ref: '#/components/schemas/ULThpt'

 uESpeed:

 type: Integer

 reliability:

 type: String

 serviceType:

 $ref: '#/components/schemas/ServiceType'

 TopSliceSubnetProfile:

 type: object

 properties:

 coverageArea:

 type: String

 latency:

 type: Integer

 maxNumberofUEs:

 type: Integer

 dLThptPerSlice:

 type: '#/components/schemas/DLThpt'

 dLThptPerUE:

 type: '#/components/schemas/DLThpt'

 uLThptPerSlice:

 type: '#/components/schemas/ULThpt'

 uLThptPerUE:

 type: '#/components/schemas/ULThpt'

 maxPktSize:

 $ref: '#/components/schemas/MaxPktSize'

 maxNumberofConns:

 type: Integer ServiceProfileList:

 type: object

 additionalProperties:

 type: object

 properties:

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 maxNumberofUEs:

 type: number

 latency:

 type: number

 uEMobilityLevel:

 $ref: '#/components/schemas/MobilityLevel'

 sst:

 $ref: 'nrNrm.yaml#/components/schemas/Sst'

 resourceSharingLevel:

 $ref: '#/components/schemas/SharingLevel'

 availability:

 type: number

 delayTolerance:

 $ref: '#/components/schemas/DelayTolerance'

 deterministicComm:

 $ref: '#/components/schemas/DeterministicComm'

 dLThptPerSlice:

 $ref: '#/components/schemas/DLThptPerSlice'

 dLThptPerUE:

 $ref: '#/components/schemas/DLThptPerUE'

 uLThptPerSlice:

 $ref: '#/components/schemas/ULThptPerSlice'

 uLThptPerUE:

 $ref: '#/components/schemas/ULThptPerUE'

 maxPktSize:

 $ref: '#/components/schemas/MaxPktSize'

 maxNumberofPDUSessions:

 $ref: '#/components/schemas/MaxNumberofPDUSessions'

 kPIMonitoring:

 $ref: '#/components/schemas/KPIMonitoring'

 nBIoT:

 $ref: '#/components/schemas/NBIoT'

 userMgmtOpen:

 $ref: '#/components/schemas/UserMgmtOpen'

 v2XModels:

 $ref: '#/components/schemas/V2XCommModels'

 coverageArea:

 type: string

 termDensity:

 $ref: '#/components/schemas/TermDensity'

 activityFactor:

 $ref: '#/components/schemas/Float'

 uESpeed:

 type: integer

 jitter:

 type: integer

 survivalTime:

 type: string

 reliability:

 type: string

maxDLDataVolume:

 type: string

maxULDataVolume:

 type: string

 SliceProfileList:

 type: object

 additionalProperties:

 type: object

 properties:

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 perfReq:

 $ref: '#/components/schemas/PerfReq'

 CNSliceSubnetProfile:

 $ref: '#/components/schemas/CNSliceSubnetProfile'

 RANSliceSubnetProfile:

 $ref: '#/components/schemas/RANSliceSubnetProfile'

 tOPSliceSubnetProfile:

 $ref: '#/components/schemas/ tOPSliceSubnetProfile'

 IpAddress:

 oneOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

 - $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

#------------ Definition of concrete IOCs ----------------------------------------

 NetworkSlice:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - type: object

 properties:

 networkSliceSubnetRef:

 $ref: 'genericNrm.yaml#/components/schemas/Dn'

 operationalState:

 $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 serviceProfileList:

 $ref: '#/components/schemas/ServiceProfileList'

 NetworkSliceSubnet:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - type: object

 properties:

 managedFunctionRefList:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 networkSliceSubnetRefList:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 operationalState:

 $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 nsInfo:

 $ref: '#/components/schemas/NsInfo'

 sliceProfileList:

 $ref: '#/components/schemas/SliceProfileList'

 EPTransport:

 $ref: '#/components/schemas/EP\_Transport-Multiple'

 EP\_Transport-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 ipAddress:

 $ref: '#/components/schemas/IpAddress'

 logicInterfaceId:

 type: string

 nextHopInfo:

 type: string

 qosProfile:

 type: string

 epApplicationRefs:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 EP\_Transport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Transport-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

 resources-sliceNrm:

 oneOf:

 - $ref: '#/components/schemas/NetworkSlice'

 - $ref: '#/components/schemas/NetworkSliceSubnet'

 - $ref: '#/components/schemas/EP\_Transport-Single'

Annex K (normative):
Void