**3GPP TSG-SA5 Meeting #133e *S5-206310rev1***

**e-meeting 12th – 21st October 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **2** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Move Distributed PCI control IOC from DU to CU | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SON\_5G | | | | |  | ***Date:*** | | | 2020-10-02 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The IOC for control attributes for PCI optimization is incorrectly placed on a DU instead of a CU IOC.  The PCI reconfiguration is controlled by the CU, as evident from TS 38.473 clause 9.2.1.10, Information Element *NR PCI* | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Move IOC with control attributes for PCI optimization from DU to CU. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | TS 28.541 will not be aligned with RAN3 specification 38.473.  Interoperability of configuration of PCI optimization in the CU-DU split scenario will not be possible. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.1.1, C.4.3, D.4.3, E.5.19, E.5.20, E.5.32 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | | **X** |  | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | *https://forge.3gpp.org/rep/sa5/MnS/tree/S5-206067\_Rel-16\_CR\_28.541\_Move\_Distributed\_PCI\_control\_IOC\_from\_DU\_to\_CU* | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S5-205142 | | | | | | | | |

**First change**

### 4.2.1 Class diagram for gNB and en-gNB

#### 4.2.1.1 Relationships

This clause depicts the set of classes (e.g. IOCs) that encapsulates the information relevant for this gNB and en-gNB. For the UML semantics, see 3GPP TS 32.156 [43]. Subsequent clauses provide more detailed specification of various aspects of these classes.

The model fragments are for management representation of gNB and en-gNB for all NG-RAN deployment scenario as listed below.

- Non-split NG-RAN deployment scenario, represents the gNB defined in TS 38.401[4]. In this scenario, a gNB is represented by a combination of a GNBCUCPFunction, one or more GNBCUUPFunctions and one or more GNBDUFunctions.

- 2-split NG-RAN deployment scenario, represents the gNB consist of gNB-CU and gNB-DU defined in TS 38.401[4] clause 6.1.1. In this scenario, a gNB-CU is represented by a combination of a GNBCUCPFunction and one or more GNBCUUPFunctions, whereas a gNB-DU is represented by a GNBDUFunction.

- 3-split NG-RAN deployment scenario, represents the gNB consist of gNB-CU-CP, gNB-CU-UP and gNB-DU defined in TS 38.401[4] clause 6.1.2. In this scenario, a gNB-CU-CP is represented by a GNBCUCPFunction, a gNB-CU-UP is represented by a GNBCUUPFunction, and a gNB-DU is represented by a GNBDUFunction.



Figure 4.2.1.1-1: NRM for all deployment scenarios




Figure 4.2.1.1-2: NRM for EPs for all deployment scenarios



Figure 4.2.1.1-3: NRM for <<IOC>>NRSectorCarrier and <<IOC>>BWP for all deployment scenarios



Figure 4.2.1.1-4: Cell Relation view for all deployment scenarios

NOTE 1: The above NRM fragment uses SubNetwork to hold both NR and LTE external entities and frequencies.



Figure 4.2.1.1-5: Cell Relation view for all deployment scenarios

NOTE 2: The above NRM fragment uses NRNetwork to hold NR external entities and frequency and using EUtraNetwork to hold LTE external entities and frequency. The NRNetwork and EUtraNetwork are subclasses of SubNetwork (defined in TS 28.622 [30]) with no additional attributes. The reason using NRNetwork and EUtraNetwork is for a clean separation of NR external entities and frequency and LTE external entities and frequency.



Figure 4.2.1.1-6: NRM fragment for RRM Policies




Figure 4.2.1.1-7: NRM fragment to support RIM

The Figure 4.2.1.1-8 shows the NRM fragment for configurable 5QIs in NG-RAN.



Figure 4.2.1.1-8: NRM fragment for configurable 5QIs in NG-RAN



Figure 4.2.1.1-9: NRM fragment for DANR Management



**Figure 4.2.1.1-10: NRM fragment for DES Management**



**Figure 4.2.1.1-11: NRM fragment for DRACH Management**



Figure 4.2.1.1-12: NRM fragment for DMRO Management




Figure 4.2.1.1-13: NRM fragment for DPCI Management



Figure 4.2.1.1-14: NRM fragment for CES Management




Figure 4.2.1.1-15: NRM fragment for CPCI Management

The Figure 4.2.1.1-16 shows the NRM fragment for dynamic 5QIs in NG-RAN.




Figure 4.2.1.1-16: NRM fragment for dynamic 5QIs in NG-RAN

#### 4.2.1.2 Inheritance












Figure 4.2.1.2-1: Inheritance Hierarchy




Figure 4.2.1.2-2: Inheritance Hierarchy

**Next change**

## C.4.3 XML schema "nRNrm.xsd"

<?xml version="1.0" encoding="UTF-8"?>

<!--

3GPP TS 28.541 NR Network Resource Model

XML schema definition

nrNrm.xsd

-->

<schema xmlns="http://www.w3.org/2001/XMLSchema"

xmlns:xn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"

xmlns:nn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#nrNrm"

xmlns:en="http://www.3gpp.org/ftp/specs/archive/28\_series/28.659#eutranNrm"

xmlns:epc="http://www.3gpp.org/ftp/specs/archive/28\_series/28.709#epcNrm"

xmlns:sm="http://www.3gpp.org/ftp/specs/archive/28\_series/28.626#stateManagementIRP"

xmlns:ngc="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#ngcNrm"

xmlns:sp="http://www.3gpp.org/ftp/specs/archive/28\_series/28.629#sonPolicyNrm"

targetNamespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#nrNrm" elementFormDefault="qualified">

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.709#epcNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.626#stateManagementIRP"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.541#ngcNrm"/>

<import namespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.629#sonPolicyNrm"/>

<simpleType name="GnbId">

<restriction base="unsignedLong">

<maxInclusive value="4294967295"/>

</restriction>

</simpleType>

<simpleType name="GnbIdLength">

<restriction base="integer">

<minLength value="22"/>

<maxLength value="32"/>

</restriction>

</simpleType>

<simpleType name="Nci">

<restriction base="unsignedLong">

<maxInclusive value="68719476735"/>

</restriction>

</simpleType>

<simpleType name="Pci">

<restriction base="unsignedShort">

<maxInclusive value="503"/>

<!-- Minimum value is 0, maximum value is 3x167+2=503 -->

</restriction>

</simpleType>

<simpleType name="NrTac">

<restriction base="unsignedLong">

<maxInclusive value="16777215"/>

<!--5G TAC is 3-octets length -->

</restriction>

</simpleType>

<simpleType name="GnbDuId">

<restriction base="unsignedLong">

<maxInclusive value="68719476735"/>

<!-- Minimum value is 0, maximum value is 2^36-1=68719476735 -->

</restriction>

</simpleType>

<simpleType name="GnbCuupId">

<restriction base="unsignedLong">

<maxInclusive value="68719476735"/>

<!-- Minimum value is 0, maximum value is 2^36-1=68719476735 -->

</restriction>

</simpleType>

<simpleType name="GnbName">

<restriction base="string">

<minLength value="1"/>

<maxLength value="150"/>

</restriction>

</simpleType>

<simpleType name="CyclicPrefix">

<restriction base="integer">

<enumeration value="15"/>

<enumeration value="30"/>

<enumeration value="60"/>

<enumeration value="120"/>

</restriction>

</simpleType>

<simpleType name="QuotaType">

<restriction base="string">

<enumeration value="STRICT"/>

<enumeration value="FLOAT"/>

</restriction>

</simpleType>

<simpleType name="CellState">

<restriction base="string">

<enumeration value="IDLE"/>

<enumeration value="INACTIVE"/>

<enumeration value="ACTIVE"/>

</restriction>

</simpleType>

<simpleType name="BwpContext">

<restriction base="string">

<enumeration value="DL"/>

<enumeration value="UL"/>

<enumeration value="SUL"/>

</restriction>

</simpleType>

<simpleType name="IsInitialBwp">

<restriction base="string">

<enumeration value="INITIAL"/>

<enumeration value="OTHER"/>

</restriction>

</simpleType>

<simpleType name="qOffsetRangeList">

<restriction base="string">

<enumeration value="dB-24"/>

<enumeration value="dB-22"/>

<enumeration value="dB-20"/>

<enumeration value="dB-18"/>

<enumeration value="dB-16"/>

<enumeration value="dB-14"/>

<enumeration value="dB-12"/>

<enumeration value="dB-10"/>

<enumeration value="dB-8"/>

<enumeration value="dB-6"/>

<enumeration value="dB-5"/>

<enumeration value="dB-4"/>

<enumeration value="dB-3"/>

<enumeration value="dB-2"/>

<enumeration value="dB-1"/>

<enumeration value="dB0"/>

<enumeration value="dB1"/>

<enumeration value="dB2"/>

<enumeration value="dB3"/>

<enumeration value="dB4"/>

<enumeration value="dB5"/>

<enumeration value="dB6"/>

<enumeration value="dB8"/>

<enumeration value="dB10"/>

<enumeration value="dB12"/>

<enumeration value="dB14"/>

<enumeration value="dB16"/>

<enumeration value="dB18"/>

<enumeration value="dB20"/>

<enumeration value="dB22"/>

<enumeration value="dB24"/>

</restriction>

</simpleType>

<simpleType name="isESCoveredBy">

<restriction base="string">

<enumeration value="NO"/>

<enumeration value="PARTIAL"/>

<enumeration value="FULL"/>

</restriction>

</simpleType>

<simpleType name="cellReselectionPriority">

<restriction base="unsignedLong">

<minInclusive value="0"/>

<maxInclusive value="16"/>

<!--Value 0 means lowest priority-->

</restriction>

</simpleType>

<simpleType name="cellReselectionSubPriority">

<restriction base="unsignedLong">

<minInclusive value="0"/>

<maxInclusive value="16"/>

<!--Value 0 means lowest priority-->

</restriction>

</simpleType>

<simpleType name="PMaxRangeType">

<restriction base="short">

<minInclusive value="-30"/>

<maxInclusive value="33"/>

</restriction>

</simpleType>

<simpleType name="qOffsetFreq">

<restriction base="short">

<minInclusive value="-24"/>

<maxInclusive value="24"/>

</restriction>

</simpleType>

<simpleType name="qQualMin">

<restriction base="integer">

<minInclusive value="-34"/>

<maxInclusive value="0"/>

</restriction>

</simpleType>

<simpleType name="qRxLevMin">

<restriction base="integer">

<minInclusive value="-140"/>

<maxInclusive value="-44"/>

</restriction>

</simpleType>

<simpleType name="Thresxhighp">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="62"/>

</restriction>

</simpleType>

<simpleType name="Threshxhighq">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="31"/>

</restriction>

</simpleType>

<simpleType name="Threshxlowp">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="62"/>

</restriction>

</simpleType>

<simpleType name="Threshxlowq">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="62"/>

</restriction>

</simpleType>

<simpleType name="Treselectionnr">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="7"/>

</restriction>

</simpleType>

<simpleType name="Treselectionnrsfhigh">

<restriction base="string">

<enumeration value="25"/>

<enumeration value="50"/>

<enumeration value="75"/>

<enumeration value="100"/>

</restriction>

</simpleType>

<simpleType name="Treselectionnrsfmedium">

<restriction base="string">

<enumeration value="25"/>

<enumeration value="50"/>

<enumeration value="75"/>

<enumeration value="100"/>

</restriction>

</simpleType>

<simpleType name="Absolutefrequencyssb">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="3279165"/>

</restriction>

</simpleType>

<simpleType name="Ssbsubcarrierspacing">

<restriction base="string">

<enumeration value="15"/>

<enumeration value="30"/>

<enumeration value="120"/>

<enumeration value="240"/>

</restriction>

</simpleType>

<simpleType name="Multifrequencybandlistnr">

<restriction base="integer">

<minInclusive value="1"/>

<maxInclusive value="256"/>

</restriction>

</simpleType>

<simpleType name="beamType">

<restriction base="string">

<enumeration value="SSB-BEAM"/>

</restriction>

</simpleType>

<simpleType name="beamAzimuth">

<restriction base="integer">

<minInclusive value="-1800"/>

<maxInclusive value="1800"/>

</restriction>

</simpleType>

<simpleType name="beamTilt">

<restriction base="integer">

<minInclusive value="-900"/>

<maxInclusive value="900"/>

</restriction>

</simpleType>

<simpleType name="beamHorizWidth">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="3599"/>

</restriction>

</simpleType>

<simpleType name="beamVertWidth">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="1800"/>

</restriction>

</simpleType>

<simpleType name="coverageShapeType">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="65535"/>

</restriction>

</simpleType>

<simpleType name="resourceType">

<restriction base="string">

<enumeration value="PRB"/>

<enumeration value="RRC"/>

<enumeration value="DRB"/>

</restriction>

</simpleType>

<complexType name="LocalEndPoint">

<sequence>

<element name="ipv4Address" type="string"/>

<element name="ipv6Address" type="string"/>

<element name="ipv6Prefix" type="string"/>

<element name="vlanId" type="integer"/>

</sequence>

</complexType>

<complexType name="RemoteEndPoint">

<sequence>

<element name="ipv4Address" type="string"/>

<element name="ipv6Address" type="string"/>

<element name="ipv6Prefix" type="string"/>

</sequence>

</complexType>

<complexType name="blackListEntry">

<sequence minOccurs="0" maxOccurs="1007">

<element name="pci" type="en:Pci" maxOccurs="504"/>

</sequence>

</complexType>

<complexType name="blackListEntryIdleMode">

<sequence minOccurs="0" maxOccurs="1007">

<element name="pci" type="en:Pci" maxOccurs="504"/>

</sequence>

</complexType>

<complexType name="PLMNIdList">

<sequence>

<element name="pLMNId" type="en:PLMNId" maxOccurs="6"/>

<!-- The first pLMNId of the pLMNIdList is primary PLMN id -->

</sequence>

</complexType>

<complexType name="cellIndividualOffset">

<sequence>

<element name="rsrpOffsetSSB" type="qOffsetRangeList"/>

<element name="rsrqOffsetSSB" type="qOffsetRangeList"/>

<element name="sinrOffsetSSB" type="qOffsetRangeList"/>

<element name="rsrpOffsetCSI-RS" type="qOffsetRangeList"/>

<element name="rsrqOffsetCSI-RS" type="qOffsetRangeList"/>

<element name="sinrOffsetCSI-RS" type="qOffsetRangeList"/>

</sequence>

</complexType>

<complexType name="PLMNInfoType">

<sequence>

<element name="pLMNId" type="en:PLMNId"/>

<element name="sNSSAI" type="ngc:SNssai" minOccurs="0"/>

</sequence>

</complexType>

<complexType name="PLMNInfoListType">

<sequence>

<element name="pLMNInfo" type="PLMNInfoType" minOccurs="1"/>

</sequence>

</complexType>

<simpleType name="maximumDeviationHoTrigger">

<restriction base="integer">

<minInclusive value="-20"/>

<maxInclusive value="20"/>

</restriction>

</simpleType>

<simpleType name="minimumTimeBetweenHoTriggerChange">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="604800"/>

</restriction>

</simpleType>

<simpleType name="tstoreUEcntxt">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="1023"/>

</restriction>

</simpleType>

<simpleType name="loadThreshold">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="100"/>

</restriction>

</simpleType>

<simpleType name="timeDuration">

<restriction base="integer">

<minInclusive value="0"/>

<maxInclusive value="900"/>

</restriction>

</simpleType>

<simpleType name="energySavingControl">

<restriction base="string">

<enumeration value="toBeEnergySaving"/>

<enumeration value="toBeNotEnergySaving"/>

</restriction>

</simpleType>

<simpleType name="energySavingState">

<restriction base="string">

<enumeration value="isNotEnergySaving"/>

<enumeration value="isEnergySaving"/>

</restriction>

</simpleType>

<simpleType name="isProbingCapable">

<restriction base="string">

<enumeration value="yes"/>

<enumeration value="no"/>

</restriction>

</simpleType>

<simpleType name="AccessDelayRange">

<restriction base="unsignedShort">

<minInclusive value="10"/>

<maxInclusive value="560"/>

</restriction>

</simpleType>

<simpleType name="NumberOfPreambleRange">

<restriction base="unsignedShort">

<minInclusive value="1"/>

<maxInclusive value="200"/>

</restriction>

</simpleType>

<simpleType name="RachProbability">

<restriction base="unsignedShort">

<enumeration value="25"/>

<enumeration value="50"/>

<enumeration value="75"/>

<enumeration value="90"/>

</restriction>

</simpleType>

<complexType name="UeAccDelayProbilityDistPerSSB">

<sequence>

<element name="Probability" type="sp:RachProbability"/>

<element name="AccessDelay" type="sp:AccessDelayRange"/>

</sequence>

</complexType>

<complexType name="UeAccDelayProbilityDistPerSSBlist">

<sequence>

<element name="ueAccDelayProbilityDistPerSSB" type="sp:UeAccDelayProbilityDistPerSSB" maxOccurs="4"/>

</sequence>

</complexType>

<complexType name="UeAccProbilityDistPerSSB">

<sequence>

<element name="Probability" type="sp:RachProbability"/>

<element name="NumberOfPreamble" type="sp:NumberOfPreambleRange"/>

</sequence>

</complexType>

<complexType name="UeAccProbilityDistPerSSBlist">

<sequence>

<element name="ueAccProbilityDistPerSSB" type="sp:UeAccProbilityDistPerSSB" maxOccurs="4"/>

</sequence>

</complexType>

<simpleType name="NRPci">

<restriction base="unsignedShort">

<maxInclusive value="1007"/>

</restriction>

</simpleType>

<complexType name="NRPciList">

<sequence>

<element name="nRPci" type="en:NRPci" maxOccurs="1008"/>

</sequence>

</complexType>

<simpleType name="NRPci">

<restriction base="unsignedShort">

<maxInclusive value="1007"/>

</restriction>

</simpleType>

<complexType name="CSonPciList">

<sequence>

<element name="nRPci" type="en:NRPci" maxOccurs="1008"/>

</sequence>

</complexType>

<element name="GNBDUFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="gnbId" type="nn:GnbId"/>

<element name="gnbIdLength" type="nn:GnbIdLength"/>

<element name="gnbDUId" type="nn:GnbDuId"/>

<element name="gnbDuName" type="nn:GnbName" minOccurs="0"/>

<element name="x2Blacklist" type="string" minOccurs="0"/>

<element name="x2Whitelist" type="string" minOccurs="0"/>

<element name="xnBlacklist" type="string" minOccurs="0"/>

<element name="xnWhitelist" type="string" minOccurs="0"/>

<element name="xnHOBlackList" type="string" minOccurs="0"/>

<element name="x2HOBlackList" type="string" minOccurs="0"/>

<element name="aggressorSetID" type="nn:AggressorSetID"/>

<element name="victimSetID" type="nn:VictimSetID"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="nn:NRCellDU"/>

<element ref="nn:BWP"/>

<element ref="nn:NRSectorCarrier"/>

<element ref="nn:EP\_F1C"/>

<element ref="nn:EP\_F1U"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="GNBCUCPFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="gnbId" type="nn:GnbId" />

<element name="gnbIdLength" type="nn:GnbIdLength"/>

<element name="gnbCuName" type=" nn:GnbName" minOccurs="0"/>

<element name="pLMNId" type="en:PLMNId" />

<element name="x2Blacklist" type="string" minOccurs="0"/>

<element name="x2Whitelist" type="string" minOccurs="0"/>

<element name="xnBlacklist" type="string" minOccurs="0"/>

<element name="xnWhitelist" type="string" minOccurs="0"/>

<element name="xnHOBlackList" type="string" minOccurs="0"/>

<element name="x2HOBlackList" type="string" minOccurs="0"/>

<element name="mappingSetIDBackhaulAddress" type="MappingSetIDBackhaulAddress" minOccurs="0"/>

<element name="configurable5QISetRef" type="xn:dn"/>

<element name="dynamic5QISetRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="nn:NRCellCU"/>

<element ref="nn:EP\_F1C"/>

<element ref="nn:EP\_E1"/>

<element ref="nn:EP\_XnC"/>

<element ref="nn:EP\_X2C"/>

<element ref="nn:EP\_NgC"/>

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="DESManagementFunction"/>

<element ref="DRACHOptimizationFunction"/>

<element ref="DMROFunction"/>

<element ref="DANRManagementFunction"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="GNBCUUPFunction" substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="gNBCUUPId" type="nn:GnbCuupId "/>

<element name="pLMNInfoList" type="PLMNInfoListType"/>

<element name="gNBId" type="nn:GnbId"/>

<element name="gnbIdLength" type="nn:GnbIdLength"/>

<element name="configurable5QISetRef" type="xn:dn"/>

<element name="dynamic5QISetRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="nn:EP\_E1"/>

<element ref="nn:EP\_F1U"/>

<element ref="nn:EP\_XnU"/>

<element ref="nn:EP\_NgU"/>

<element ref="nn:EP\_X2U"/>

<element ref="nn:EP\_S1U"/>

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRCellCU">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="nCGI" type="nn:Ncgi"/>

<element name="pLMNIdList" type="en:PLMNIdList"/>

<element name="sNSSAIList" type="ngc:SnssaiList" minOccurs="0"/>

<element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

<element ref="nRCellRelation"/>

<element ref="nRFreqRelation"/>

<element ref="eUtranCellRelation"/>

<element ref="eUtranFreqRelation"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref= "RRMPolicyRatio"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="DESManagementFunction"/>

<element ref="DRACHOptimizationFunction"/>

<element ref="DMROFunction"/>

<element ref="CESManagementFunction"/>

<element ref="DPCIConfigurationFunction"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRCellDU">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="nCGI" type="nn:Ncgi" minOccurs="0"/>

<element name="operationalState" type="sm:operationalStateType" minOccurs="0"/>

<element name="administrativeState" type="sm:administrativeStateType" minOccurs="0"/>

<element name="cellState" type="nn:CellState"/>

<element name="pLMNIdList" type="en:PLMNIdList"/>

<element name="sNSSAIList" type="ngc:SnssaiList" minOccurs="0"/>

<element name="nRpci" type="nn:Pci" />

<element name="nRTac" type="nn:NrTac" />

<element name="arfcnDL" type="integer"/>

<element name="arfcnUL" type="integer" minOccurs="0"/>

<element name="arfcnSUL" type="integer" minOccurs="0"/>

<element name="bSChannelBwDL" type="integer"/>

<element name="bSChannelBwUL" type="integer" minOccurs="0"/>

<element name="bSChannelBwSUL" type="integer" minOccurs="0"/>

<element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

<element name="nRSectorCarrierRef" type="xn:dn" minOccurs="0"/>

<element name="bWPRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="RRMPolicyRatio"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="CPCIConfigurationFunction"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRSectorCarrier">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="txDirection" type="nn:TxDirection"/>

<element name="configuredMaxTxPower" type="integer"/>

<element name="arfcnDL" type="integer" minOccurs="0"/>

<element name="arfcnUL" type="integer" minOccurs="0"/>

<element name="bSChannelBwDL" type="integer" minOccurs="0"/>

<element name="bSChannelBwUL" type="integer" minOccurs="0"/>

<element name="sectorEquipmentFunctionRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="BWP">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction-->

<element name="bwpContext" type="nn:BwpContext"/>

<element name="isInitialBwp" type="nn:IsInitialBwp"/>

<element name="subCarrierSpacing" type="integer"/>

<element name="cyclicPrefix" type="nn:CyclicPrefix"/>

<element name="startRB" type="integer"/>

<element name="numberOfRBs" type="integer"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="CommonBeamformingFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="coverageShape" type="coverageShapeType" minOccurs="0"/>

<element name="digitalTilt" type="beamTilt" minOccurs="0"/>

<element name="digitalAzimuth" type="beamAzimuth" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="Beam">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="beamIndex" type="integer" minOccurs="0"/>

<element name="beamType" type="beamType" minOccurs="0"/>

<element name="beamAzimuth" type="beamAzimuth" minOccurs="0"/>

<element name="beamTilt" type="beamTilt" minOccurs="0"/>

<element name="beamHorizWidth" type="beamHorizWidth" minOccurs="0"/>

<element name="beamVertWidth" type="beamVertWidth" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_E1">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_XnC">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_XnU">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_NgC">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LoacalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_NgU">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_F1C">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_F1U">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_S1U">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_X2C">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EP\_X2U">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes" minOccurs="0">

<complexType>

<all>

<!-- Inherited attributes from EP\_RP -->

<element name="farEndEntity" type="xn:dn" minOccurs="0"/>

<element name="userLabel" type="string" minOccurs="0"/>

<!-- End of inherited attributes from EP\_RP -->

<element name="localAddress" type="nn:LocalEndPoint" minOccurs="0"/>

<element name="remoteAddress" type="nn:RemoteEndPoint" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRCellRelation">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from Top\_ -->

<element name="id" type="string" />

<!--End of inherited attributes from Top\_ -->

<element name="nRTCI" type="nn:Nrtci"/>

<element name="cellIndividualOffset" type="en:CellIndividualOffset"/>

<element name="nRFreqRelationRef" type="xn:dn" minOccurs="0"/>

<element name="adjacentNRCellRef" type="xn:dn" minOccurs="0"/>

<element name="isRemoveAllowed" type="boolean" minOccurs="0"/>

<element name="isHOAllowed" type="boolean" minOccurs="0"/>

<element name="isESCoveredBy" type="nn:isESCoveredBy" minOccurs="0"/>

<element name="isENDCAllowed" type="boolean" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRFreqRelation">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from Top\_ -->

<element name="id" type="string" />

<!--End of inherited attributes from Top\_ -->

<element name="offsetMO" type="en:qOffsetRangeList"/>

<element name="blackListEntry" type="en:blackListEntry" minOccurs="0"/>

<element name="blackListEntryIdleMode" type="en:blackListEntryIdleMode" minOccurs="0"/>

<element name="cellReselectionPriority" type="en:cellReselectionPriority"/>

<element name="cellReselectionSubPriority" type="en:cellReselectionSubPriority"/>

<element name="pMax" type="en:PMaxRangeType" minOccurs="0"/>

<element name="qOffserFreq" type="nn:qOffserFreq" minOccurs="0"/>

<element name="qQualMin" type="en:qQualMin" minOccurs="0"/>

<element name="qRxLevMin" type="en:qRxLevMin" minOccurs="0"/>

<element name="threshXHighP" type="en:threshxhighp" minOccurs="0"/>

<element name="threshXHighQ" type="en:threshxhighq" minOccurs="0"/>

<element name="threshXLowP" type="en:threshxlowp" minOccurs="0"/>

<element name="threshXLowQ" type="en:threshxlowp" minOccurs="0"/>

<element name="tReselectionNr" type="nn:Treselectionnr" minOccurs="0"/>

<element name="tReselectionNRSfHigh" type="nn:Treselectionnrsfhigh" minOccurs="0"/>

<element name="tReselectionNRSfMedium" type="nn:Treselectionnrsfmedium" minOccurs="0"/>

<element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="ExternalNRCellCU">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction -->

<element name="nCGI" type="nn:Ncgi"/>

<element name="pLMNIdList" type="en:PLMNIdList"/>

<element name="nRPCI" type="nn:Nrpci" minOccurs="0"/>

<element name="nRFrequencyRef" type="xn:dn" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="ExternalGNBCUCPFunction" substitutionGroup="xn:SubNetworkOptionallyContainedNrmClass ">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction -->

<element name="gnbId" type="nn:GnbId" />

<element name="gnbIdLength" type="nn:GnbIdLength"/>

<element name="pLMNId" type="en:PLMNId" />

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="RRMPolicy\_">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="resourceType" type="ResourceType" />

<element name="rRMPolicyMemberList" type="PLMNInfoListType"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="RRMPolicyRatio">

<complexType>

<complexContent>

<extension base="RRMPolicy\_">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="rRMPolicyMaxRatio" type="integer" minOccurs="1"/>

<element name="rRMPolicyMinRatio" type="integer" minOccurs="1"/>

<element name="rRMPolicyDedicatedRatio" type="integer" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="NRFrequency" substitutionGroup="xn:SubNetworkOptionallyContainedNrmClass">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<!-- Inherited attributes from ManagedFunction -->

<element name="userLabel" type="string" minOccurs="0"/>

<element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element name="peeParametersList" type="xn:peeParametersListType" minOccurs="0"/>

<element name="priority" type="integer" minOccurs="0"/>

<element name="measurements" type="xn:MeasurementTypesAndGPsList" minOccurs="0"/>

<!--End of inherited attributes from ManagedFunction -->

<element name="absoluteFrequencySSB" type="nn:Absolutefrequencyssb" minOccurs="0"/>

<element name="sSBSubCarrierSpacing" type="nn:Ssbsubcarrierspacing" minOccurs="0"/>

<element name="multiFrequencyBandListNR" type="nn:MultifrequencyBandlistnr" minOccurs="0"/>

</all>

</complexType>

</element>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:VsDataContainer"/>

</choice>

<choice minOccurs="0" maxOccurs="1">

<element ref="sp:EnergySavingProperties"/>

<element ref="sp:ESPolicies"/>

</choice>

<choice minOccurs="0" maxOccurs="unbounded">

<element ref="xn:MeasurementControl"/>

</choice>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="MappingSetIDBackhaulAddress">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="setID" type="nn:SetId" />

<element name="backhaulAdress" type="BackhaulAddress" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="BackhaulAddress">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="gNBID" type="nn:GnbId" />

<element name="tAI" type="TAI" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="TAI">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="nRTac" type="nn:NrTac" />

<element name="pLMNId" type="en:PLMNId" />

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="DANRManagementFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="intrasystemANRManagementSwitch" type="boolean" minOccurs="0"/>

<element name="intrasystemANRManagementSwitch" type="beamType" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="DESManagementFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="desSwitch" type="boolean" minOccurs="0"/>

<element name="intraRatEsActivationOriginalCellLoadParameters" type="IntraRatEsActivationOriginalCellLoadParameters " minOccurs="0"/>

<element name="intraRatEsActivationCandidateCellsLoadParameters" type="IntraRatEsActivationCandidateCellsLoadParameters" minOccurs="0"/>

<element name="intraRatEsDeactivationCandidateCellsLoadParameters" type="IntraRatEsDeactivationCandidateCellsLoadParameters" minOccurs="0"/>

<element name="esNotAllowedTimePeriod" type="EsNotAllowedTimePeriod" minOccurs="0"/>

<element name="interRatEsActivationOriginalCellParameters" type="InterRatEsActivationOriginalCellParameters" minOccurs="0"/>

<element name="interRatEsActivationCandidateCellParameters" type="InterRatEsActivationCandidateCellParameters" minOccurs="0"/>

<element name="interRatEsDeactivationCandidateCellParameters" type="InterRatEsDeactivationCandidateCellParameters" minOccurs="0"/>

<element name="energySavingState" type="energySavingState" minOccurs="0"/>

<element name="isProbingCapable" type="isProbingCapable" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="IntraRatEsActivationOriginalCellLoadParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="IntraRatEsActivationCandidateCellsLoadParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="IntraRatEsDeactivationCandidateCellsLoadParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="EsNotAllowedTimePeriod">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="startTimeandendTime" type="nn:startTimeandendTime" />

<element name="periodOfDay" type="nn:startTimeandendTime" />

<element name="daysOfWeekList" type="en:daysOfWeekList" />

<element name="listoftimeperiods" type="en:listoftimeperiods" />

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="InterRatEsActivationOriginalCellParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="InterRatEsActivationCandidateCellParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="InterRatEsDeactivationCandidateCellParameters">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="loadThreshold" type="loadThreshold" minOccurs="0"/>

<element name="timeDuration" type="timeDuration" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="DRACHOptimizationFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="ueAccProbilityDistPerSSBlist" type="UeAccProbilityDistPerSSBlist" minOccurs="0"/>

<element name="ueAccDelayProbilityDistPerSSBlist" type="UeAccDelayProbilityDistPerSSBlist" minOccurs="0"/>

<element name="drachOptimizationControl" type="boolean" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="DMROFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="dmroControl" type=" boolean" minOccurs="0"/>

<element name="maximumDeviationHoTrigger" type="maximumDeviationHoTrigger" minOccurs="0"/>

<element name="minimumTimeBetweenHoTriggerChange" type="minimumTimeBetweenHoTriggerChange" minOccurs="0"/>

<element name="tstoreUEcntxt" type="tstoreUEcntxt" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="DPCIConfigurationFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="nRPciList" type="NRPciList" minOccurs="0"/>

<element name="dPciConfigurationControl" type="boolean" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="CPCIConfigurationFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="cSonPciList" type="CSonPciList" minOccurs="0"/>

<element name="cPciConfigurationControl" type="boolean" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

<element name="CESManagementFunction">

<complexType>

<complexContent>

<extension base="xn:NrmClass">

<sequence>

<element name="attributes">

<complexType>

<all>

<element name="cesSwitch" type="boolean" minOccurs="0"/>

<element name="energySavingState" type="energySavingState" minOccurs="0"/>

<element name="energySavingControl" type="energySavingControl" minOccurs="0"/>

</all>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

</element>

</schema>

**Next change**

## D.4.3 OpenAPI document "nrNrm.yaml"

openapi: 3.0.1

info:

title: NR NRM

version: 16.6.0

description: >-

OAS 3.0.1 specification of the NR NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541 V16.6.0; 5G NRM, NR NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

GnbId:

type: string

GnbIdLength:

type: integer

minimum: 22

maximum: 32

GnbName:

type: string

maxLength: 150

GnbDuId:

type: number

minimum: 0

maximum: 68719476735

GnbCuUpId:

type: number

minimum: 0

maximum: 68719476735

Sst:

type: integer

maximum: 255

Snssai:

type: object

properties:

sst:

$ref: '#/components/schemas/Sst'

sd:

type: string

SnssaiList:

type: array

items:

$ref: '#/components/schemas/Snssai'

Mnc:

type: string

pattern: '[0-9]{3}|[0-9]{2}'

PlmnId:

type: object

properties:

mcc:

$ref: 'genericNrm.yaml#/components/schemas/Mcc'

mnc:

$ref: '#/components/schemas/Mnc'

PlmnIdList:

type: array

items:

$ref: '#/components/schemas/PlmnId'

PlmnInfo:

type: object

properties:

plmnId":

$ref: '#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

PlmnInfoList:

type: array

items:

$ref: '#/components/schemas/PlmnInfo'

GGnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(22|23|24|25|26|27|28|29|30|31|32)-[0-9]{1,10}'

GEnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(18|20|21|22)-[0-9]{1,7}'

GGnbIdList:

type: array

items:   
 $ref: '#/components/schemas/GGnbId'

GEnbIdList:

type: array

items:   
 $ref: '#/components/schemas/GEnbId'

NrPci:

type: integer

maximum: 503

NrTac:

type: integer

maximum: 16777215

Tai:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

nrTac:

$ref: '#/components/schemas/NrTac'

BackhaulAddress:

type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

tai:

$ref: "#/components/schemas/Tai"

MappingSetIDBackhaulAddress:

type: object

properties:

setID:

type: integer

backhaulAddress:

$ref: '#/components/schemas/BackhaulAddress'

IntraRatEsActivationOriginalCellLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsActivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsDeactivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

EsNotAllowedTimePeriod:

type: object

properties:

startTimeandendTime:

type: string

periodOfDay:

type: string

daysOfWeekList:

type: string

listoftimeperiods:

type: string

InterRatEsActivationOriginalCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsActivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsDeactivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

UeAccProbilityDistPerSSB:

type: object

properties:

targetProbability:

type: integer

numberofpreamblessent:

type: integer

UeAccDelayProbilityDistPerSSB:

type: object

properties:

targetProbability:

type: integer

accessdelay:

type: integer

NRPciList:

type: object

properties:

NRPci:

type: integer

CSonPciList:

type: object

properties:

NRPci:

type: integer

MaximumDeviationHoTrigger:

type: integer

minimum: -20

maximum: 20

MinimumTimeBetweenHoTriggerChange:

type: integer

minimum: 0

maximum: 604800

TstoreUEcntxt:

type: integer

minimum: 0

maximum: 1023

CellState:

type: string

enum:

- IDLE

- INACTIVE

- ACTIVE

CyclicPrefix:

type: string

enum:

- '15'

- '30'

- '60'

- '120'

TxDirection:

type: string

enum:

- DL

- UL

- DL and UL

BwpContext:

type: string

enum:

- DL

- UL

- SUL

IsInitialBwp:

type: string

enum:

- INITIAL

- OTHER

- SUL

QuotaType:

type: string

enum:

- STRICT

- FLOAT

IsESCoveredBy:

type: string

enum:

- NO

- PARTIAL

- FULL

RrmPolicyMember:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

RrmPolicyMemberList:

type: array

items:

$ref: '#/components/schemas/RrmPolicyMember'

AddressWithVlan:

type: object

properties:

ipv4Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

vlanId:

type: integer

minimum: 0

maximum: 4096

LocalAddress:

type: object

properties:

addressWithVlan:

$ref: '#/components/schemas/AddressWithVlan'

port:

type: integer

minimum: 0

maximum: 65535

RemoteAddress:

type: object

properties:

ipv4Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

CellIndividualOffset:

type: object

properties:

rsrpOffsetSSB:

type: integer

rsrqOffsetSSB:

type: integer

sinrOffsetSSB:

type: integer

rsrpOffsetCSI-RS:

type: integer

rsrqOffsetCSI-RS:

type: integer

sinrOffsetCSI-RS:

type: integer

QOffsetRange:

type: integer

enum:

- -24

- -22

- -20

- -18

- -16

- -14

- -12

- -10

- -8

- -6

- -5

- -4

- -3

- -2

- -1

- 0

- 24

- 22

- 20

- 18

- 16

- 14

- 12

- 10

- 8

- 6

- 5

- 4

- 3

- 2

- 1

QOffsetRangeList:

type: object

properties:

rsrpOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrpOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

QOffsetFreq:

type: number

TReselectionNRSf:

type: integer

enum:

- 25

- 50

- 75

- 100

SsbPeriodicity:

type: integer

enum:

- 5

- 10

- 20

- 40

- 80

- 160

SsbDuration:

type: integer

enum:

- 1

- 2

- 3

- 4

- 5

SsbSubCarrierSpacing:

type: integer

enum:

- 15

- 30

- 120

- 240

CoverageShape:

type: integer

maximum: 65535

DigitalTilt:

type: integer

minimum: -900

maximum: 900

DigitalAzimuth:

type: integer

minimum: -1800

maximum: 1800

RSSetId:

type: integer

maximum: 4194303

RSSetType:

type: string

enum:

- RS1

- RS2

FrequencyDomainPara:

type: object

properties:

rimRSSubcarrierSpacing:

type: integer

rIMRSBandwidth:

type: integer

nrofGlobalRIMRSFrequencyCandidates:

type: integer

rimRSCommonCarrierReferencePoint:

type: integer

rimRSStartingFrequencyOffsetIdList:

type: array

items:

type: integer

SequenceDomainPara:

type: object

properties:

nrofRIMRSSequenceCandidatesofRS1:

type: integer

rimRSScrambleIdListofRS1:

type: array

items:

type: integer

nrofRIMRSSequenceCandidatesofRS2:

type: integer

rimRSScrambleIdListofRS2:

type: array

items:

type: integer

enableEnoughNotEnoughIndication:

type: string

enum:

- ENABLE

- DISABLE

RIMRSScrambleTimerMultiplier:

type: integer

RIMRSScrambleTimerOffset:

type: integer

TimeDomainPara:

type: object

properties:

dlULSwitchingPeriod1:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint1:

type: integer

dlULSwitchingPeriod2:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint2:

type: integer

totalnrofSetIdofRS1:

type: integer

totalnrofSetIdofRS2:

type: integer

nrofConsecutiveRIMRS1:

type: integer

nrofConsecutiveRIMRS2:

type: integer

consecutiveRIMRS1List:

type: array

items:

type: integer

consecutiveRIMRS2List:

type: array

items:

type: integer

enablenearfarIndicationRS1:

type: string

enum:

- ENABLE

- DISABLE

enablenearfarIndicationRS2:

type: string

enum:

- ENABLE

- DISABLE

RimRSReportInfo:

type: object

properties:

detectedSetID:

type: integer

propagationDelay:

type: integer

functionalityOfRIMRS:

type: string

enum:

- RS1

- RS2

- RS1forEnoughMitigation

- RS1forNotEnoughMitigation

RimRSReportConf:

type: object

properties:

reportIndicator:

type: string

enum:

- ENABLE

- DISABLE

reportInterval:

type: integer

nrofRIMRSReportInfo:

type: integer

maxPropagationDelay:

type: integer

rimRSReportInfoList:

type: array

items:

$ref: '#/components/schemas/RimRSReportInfo'

TceMappingInfo:

type: object

properties:

TceIPAddress:

oneOf:

- $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

- $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

TceID:

type: integer

PlmnTarget:

$ref: '#/components/schemas/PlmnId'

TceMappingInfoList:

type: array

items:

$ref: '#/components/schemas/TceMappingInfo'

#-------- Definition of abstract IOCs --------------------------------------------

RrmPolicy\_-Attr:

type: object

properties:

resourceType:

type: string

rRMPolicyMemberList:

$ref: '#/components/schemas/RrmPolicyMemberList'

#-------- Definition of concrete IOCs --------------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

$ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

SubNetwork:

$ref: '#/components/schemas/SubNetwork-Multiple'

ManagedElement:

$ref: '#/components/schemas/ManagedElement-Multiple'

NRFrequency:

$ref: '#/components/schemas/NRFrequency-Multiple'

ExternalGnbCuCpFunction:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Multiple'

ExternalENBFunction:

$ref: '#/components/schemas/ExternalENBFunction-Multiple'

EUtranFrequency:

$ref: '#/components/schemas/EUtranFrequency-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

RimRSGlobal:

$ref: '#/components/schemas/RimRSGlobal-Single'

Dynamic5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

ManagedElement-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

$ref: 'genericNRM.yaml#/components/schemas/ManagedElement-Attr'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedElement-ncO'

- type: object

properties:

GnbDuFunction:

$ref: '#/components/schemas/GnbDuFunction-Multiple'

GnbCuUpFunction:

$ref: '#/components/schemas/GnbCuUpFunction-Multiple'

GnbCuCpFunction:

$ref: '#/components/schemas/GnbCuCpFunction-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

GnbDuFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbDuId:

$ref: '#/components/schemas/GnbDuId'

gnbDuName:

$ref: '#/components/schemas/GnbName'

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

rimRSReportConf:

$ref: '#/components/schemas/RimRSReportConf'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellDu:

$ref: '#/components/schemas/NrCellDu-Multiple'

Bwp-Multiple:

$ref: '#/components/schemas/Bwp-Multiple'

NrSectorCarrier-Multiple:

$ref: '#/components/schemas/NrSectorCarrier-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

GnbCuUpFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuUpId:

$ref: '#/components/schemas/GnbCuUpId'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

configurable5QISetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_NgU:

$ref: '#/components/schemas/EP\_NgU-Multiple'

EP\_X2U:

$ref: '#/components/schemas/EP\_X2U-Multiple'

EP\_S1U:

$ref: '#/components/schemas/EP\_S1U-Multiple'

GnbCuCpFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuName:

$ref: '#/components/schemas/GnbName'

plmnId:

$ref: '#/components/schemas/PlmnId'

x2BlackList:

$ref: '#/components/schemas/GGnbIdList'

xnBlackList:

$ref: '#/components/schemas/GGnbIdList'

x2WhiteList:

$ref: '#/components/schemas/GGnbIdList'

xnWhiteList:

$ref: '#/components/schemas/GGnbIdList'

xnHOBlackList:

$ref: '#/components/schemas/GGnbIdList'

x2HOBlackList:

$ref: '#/components/schemas/GEnbIdList'

mappingSetIDBackhaulAddress:

$ref: '#/components/schemas/MappingSetIDBackhaulAddress'

tceMappingInfoList:

$ref: '#/components/schemas/TceMappingInfoList'

configurable5QISetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellCu:

$ref: '#/components/schemas/NrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_NgC:

$ref: '#/components/schemas/EP\_NgC-Multiple'

EP\_X2C:

$ref: '#/components/schemas/EP\_X2C-Multiple'

DANRManagementFunction:

$ref: '#/components/schemas/DANRManagementFunction-Single'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

NrCellCu-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nRFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NRCellRelation:

$ref: '#/components/schemas/NRCellRelation-Multiple'

EUtranCellRelation:

$ref: '#/components/schemas/EUtranCellRelation-Multiple'

NRFreqRelation:

$ref: '#/components/schemas/NRFreqRelation-Multiple'

EUtranFreqRelation:

$ref: '#/components/schemas/EUtranFreqRelation-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

NrCellDu-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

administrativeState:

$ref: 'genericNRM.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'genericNRM.yaml#/components/schemas/OperationalState'

cellLocalId:

type: integer

cellState:

$ref: '#/components/schemas/CellState'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nrPci:

$ref: '#/components/schemas/NrPci'

nrTac:

$ref: '#/components/schemas/NrTac'

arfcnDL:

type: integer

arfcnUL:

type: integer

arfcnSUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

bSChannelBwSUL:

type: integer

ssbFrequency:

type: integer

minimum: 0

maximum: 3279165

ssbPeriodicity:

$ref: '#/components/schemas/SsbPeriodicity'

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

ssbOffset:

type: integer

minimum: 0

maximum: 159

ssbDuration:

$ref: '#/components/schemas/SsbDuration'

nrSectorCarrierRef:

type: array

items:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

bwpRef:

type: array

items:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

nRFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

victimSetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

aggressorSetRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

NRFrequency-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

absoluteFrequencySSB:

type: integer

minimum: 0

maximum: 3279165

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

multiFrequencyBandListNR:

type: integer

minimum: 1

maximum: 256

EUtranFrequency-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

earfcnDL:

type: integer

minimum: 0

maximum: 262143

multiBandInfoListEutra:

type: integer

minimum: 1

maximum: 256

NrSectorCarrier-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

txDirection:

$ref: '#/components/schemas/TxDirection'

configuredMaxTxPower:

type: integer

arfcnDL:

type: integer

arfcnUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

sectorEquipmentFunctionRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

CommonBeamformingFunction:

$ref: '#/components/schemas/CommonBeamformingFunction-Single'

Bwp-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

bwpContext:

$ref: '#/components/schemas/BwpContext'

isInitialBwp:

$ref: '#/components/schemas/IsInitialBwp'

subCarrierSpacing:

type: integer

cyclicPrefix:

$ref: '#/components/schemas/CyclicPrefix'

startRB:

type: integer

numberOfRBs:

type: integer

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

CommonBeamformingFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

coverageShape:

$ref: '#/components/schemas/CoverageShape'

digitalAzimuth:

$ref: '#/components/schemas/DigitalAzimuth'

digitalTilt:

$ref: '#/components/schemas/DigitalTilt'

- type: object

properties:

Beam:

$ref: '#/components/schemas/Beam-Multiple'

Beam-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

beamIndex:

type: integer

beamType:

type: string

enum:

- SSB-BEAM

beamAzimuth:

type: integer

minimum: -1800

maximum: 1800

beamTilt:

type: integer

minimum: -900

maximum: 900

beamHorizWidth:

type: integer

minimum: 0

maximum: 3599

beamVertWidth:

type: integer

minimum: 0

maximum: 1800

RRMPolicyRatio-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: '#/components/schemas/RrmPolicy\_-Attr'

- type: object

properties:

rRMPolicyMaxRatio:

type: integer

rRMPolicyMinRatio:

type: integer

rRMPolicyDedicatedRatio:

type: integer

NRCellRelation-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

nRTCI:

type: integer

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

adjacentNRCellRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

nRFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

isRemoveAllowed:

type: boolean

isHOAllowed:

type: boolean

isESCoveredBy:

$ref: '#/components/schemas/IsESCoveredBy'

isENDCAllowed:

type: boolean

EUtranCellRelation-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

adjacentEUtranCellRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

NRFreqRelation-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

offsetMO:

$ref: '#/components/schemas/QOffsetRangeList'

blackListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blackListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionNr:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

nRFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

EUtranFreqRelation-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

blackListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blackListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionEutran:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

eUTranFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

DANRManagementFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

intrasystemANRManagementSwitch:

type: boolean

intersystemANRManagementSwitch:

type: boolean

DESManagementFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

desSwitch:

type: boolean

intraRatEsActivationOriginalCellLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

intraRatEsActivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationCandidateCellsLoadParameters"

intraRatEsDeactivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsDeactivationCandidateCellsLoadParameters"

esNotAllowedTimePeriod:

$ref: "#/components/schemas/EsNotAllowedTimePeriod"

interRatEsActivationOriginalCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsActivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsDeactivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

isProbingCapable:

type: string

enum:

- yes

- no

energySavingState:

type: string

enum:

- isNotEnergySaving

- isEnergySaving

DRACHOptimizationFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

drachOptimizationControl:

type: boolean

ueAccProbilityDistPerSSB:

$ref: "#/components/schemas/UeAccProbilityDistPerSSB"

ueAccDelayProbilityDistPerSSB:

$ref: "#/components/schemas/UeAccDelayProbilityDistPerSSB"

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

DMROFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

dmroControl:

type: boolean

maximumDeviationHoTrigger:

$ref: '#/components/schemas/MaximumDeviationHoTrigger'

minimumTimeBetweenHoTriggerChange:

$ref: '#/components/schemas/MinimumTimeBetweenHoTriggerChange'

tstoreUEcntxt:

$ref: '#/components/schemas/TstoreUEcntxt'

DPCIConfigurationFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

dPciConfigurationControl:

type: boolean

nRPciList:

$ref: "#/components/schemas/NRPciList"

CPCIConfigurationFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

cPciConfigurationControl:

type: boolean

cSonPciList:

$ref: "#/components/schemas/CSonPciList"

CESManagementFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

cesSwitch:

type: boolean

energySavingControl:

type: string

enum:

- toBeEnergySaving

- toBeNotEnergySaving

energySavingState:

type: string

enum:

- isNotEnergySaving

- isEnergySaving

RimRSGlobal-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

frequencyDomainPara:

$ref: '#/components/schemas/FrequencyDomainPara'

sequenceDomainPara:

$ref: '#/components/schemas/SequenceDomainPara'

timeDomainPara:

$ref: '#/components/schemas/TimeDomainPara'

RimRSSet:

$ref: '#/components/schemas/RimRSSet-Multiple'

RimRSSet-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

setId:

$ref: '#/components/schemas/RSSetId'

setType:

$ref: '#/components/schemas/RSSetType'

rimRSMonitoringStartTime:

type: string

rimRSMonitoringStopTime:

type: string

rimRSMonitoringWindowDuration:

type: integer

rimRSMonitoringWindowStartingOffset:

type: integer

rimRSMonitoringWindowPeriodicity:

type: integer

rimRSMonitoringOccasionInterval:

type: integer

rimRSMonitoringOccasionStartingOffset:

type: integer

nRCellDURefs:

$ref: 'genericNRM.yaml#/components/schemas/DnList'

ExternalGnbDuFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

ExternalGnbCuUpFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

ExternalGnbCuCpFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: >-

genericNRM.yaml#/components/schemas/ManagedFunction-Attr

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

plmnId:

$ref: '#/components/schemas/PlmnId'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalNrCellCu:

$ref: '#/components/schemas/ExternalNrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

ExternalNrCellCu-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

nrPci:

$ref: '#/components/schemas/NrPci'

plmnIdList:

$ref: '#/components/schemas/PlmnIdList'

nRFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

ExternalENBFunction-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

eNBId:

type: integer

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalEUTranCell:

$ref: '#/components/schemas/ExternalEUTranCell-Multiple'

ExternalEUTranCell-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

EUtranFrequencyRef:

$ref: 'genericNRM.yaml#/components/schemas/Dn'

- $ref: 'genericNRM.yaml#/components/schemas/ManagedFunction-ncO'

EP\_XnC-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_E1-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1C-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_NgC-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_X2C-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_XnU-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1U-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_NgU-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

EP\_X2U-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_S1U-Single:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNRM.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

SubNetwork-Multiple:

type: array

items:

$ref: '#/components/schemas/SubNetwork-Single'

ManagedElement-Multiple:

type: array

items:

$ref: '#/components/schemas/ManagedElement-Single'

GnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbDuFunction-Single'

GnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuUpFunction-Single'

GnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuCpFunction-Single'

NrCellDu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellDu-Single'

NrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellCu-Single'

NRFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/NRFrequency-Single'

EUtranFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/EUtranFrequency-Single'

NrSectorCarrier-Multiple:

type: array

items:

$ref: '#/components/schemas/NrSectorCarrier-Single'

Bwp-Multiple:

type: array

items:

$ref: '#/components/schemas/Bwp-Single'

Beam-Multiple:

type: array

items:

$ref: '#/components/schemas/Beam-Single'

RRMPolicyRatio-Multiple:

type: array

items:

$ref: '#/components/schemas/RRMPolicyRatio-Single'

NRCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRCellRelation-Single'

EUtranCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranCellRelation-Single'

NRFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRFreqRelation-Single'

EUtranFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranFreqRelation-Single'

RimRSSet-Multiple:

type: array

items:

$ref: '#/components/schemas/RimRSSet-Single'

ExternalGnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbDuFunction-Single'

ExternalGnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

ExternalGnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

ExternalNrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalNrCellCu-Single'

ExternalENBFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalENBFunction-Single'

ExternalEUTranCell-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalEUTranCell-Single'

EP\_E1-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnC-Single'

EP\_F1C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_NgC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgC-Single'

EP\_X2C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2C-Single'

EP\_XnU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnU-Single'

EP\_F1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1U-Single'

EP\_NgU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgU-Single'

EP\_X2U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2U-Single'

EP\_S1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_S1U-Single'

#-------- Definitions in TS 28.541 for TS 28.532 ---------------------------------

resources-nrNrm:

oneOf:

- $ref: '#/components/schemas/SubNetwork-Single'

- $ref: '#/components/schemas/ManagedElement-Single'

- $ref: '#/components/schemas/GnbDuFunction-Single'

- $ref: '#/components/schemas/GnbCuUpFunction-Single'

- $ref: '#/components/schemas/GnbCuCpFunction-Single'

- $ref: '#/components/schemas/NrCellCu-Single'

- $ref: '#/components/schemas/NrCellDu-Single'

- $ref: '#/components/schemas/NRFrequency-Single'

- $ref: '#/components/schemas/EUtranFrequency-Single'

- $ref: '#/components/schemas/NrSectorCarrier-Single'

- $ref: '#/components/schemas/Bwp-Single'

- $ref: '#/components/schemas/CommonBeamformingFunction-Single'

- $ref: '#/components/schemas/Beam-Single'

- $ref: '#/components/schemas/RRMPolicyRatio-Single'

- $ref: '#/components/schemas/NRCellRelation-Single'

- $ref: '#/components/schemas/EUtranCellRelation-Single'

- $ref: '#/components/schemas/NRFreqRelation-Single'

- $ref: '#/components/schemas/EUtranFreqRelation-Single'

- $ref: '#/components/schemas/DANRManagementFunction-Single'

- $ref: '#/components/schemas/DESManagementFunction-Single'

- $ref: '#/components/schemas/DRACHOptimizationFunction-Single'

- $ref: '#/components/schemas/DMROFunction-Single'

- $ref: '#/components/schemas/DPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CESManagementFunction-Single'

- $ref: '#/components/schemas/RimRSGlobal-Single'

- $ref: '#/components/schemas/RimRSSet-Single'

- $ref: '#/components/schemas/ExternalGnbDuFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

- $ref: '#/components/schemas/ExternalNrCellCu-Single'

- $ref: '#/components/schemas/ExternalENBFunction-Single'

- $ref: '#/components/schemas/ExternalEUTranCell-Single'

- $ref: '#/components/schemas/EP\_XnC-Single'

- $ref: '#/components/schemas/EP\_E1-Single'

- $ref: '#/components/schemas/EP\_F1C-Single'

- $ref: '#/components/schemas/EP\_NgC-Single'

- $ref: '#/components/schemas/EP\_X2C-Single'

- $ref: '#/components/schemas/EP\_XnU-Single'

- $ref: '#/components/schemas/EP\_F1U-Single'

- $ref: '#/components/schemas/EP\_NgU-Single'

- $ref: '#/components/schemas/EP\_X2U-Single'

- $ref: '#/components/schemas/EP\_S1U-Single'

**Next change**

## E.5.19 module \_3gpp-nr-nrm-nrcellcu.yang

module \_3gpp-nr-nrm-nrcellcu {

yang-version 1.1;

namespace "urn:3gpp:sa5:\_3gpp-nr-nrm-nrcellcu";

prefix "nrcellcu3gpp";

import \_3gpp-common-yang-types { prefix types3gpp; }

import \_3gpp-common-managed-function { prefix mf3gpp; }

import \_3gpp-common-managed-element { prefix me3gpp; }

import \_3gpp-nr-nrm-gnbcucpfunction { prefix gnbcucp3gpp; }

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-nr-nrm-common { prefix nrcommon3gpp; }

organization "3GPP SA5";

contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

description "Defines the YANG mapping of the NRCellCU Information Object

Class (IOC) that is part of the NR Network Resource Model (NRM).";

reference "3GPP TS 28.541 5G Network Resource Model (NRM)";

revision 2020-11-25 { reference CR-0385 ; }

revision 2020-05-08 { reference S5-203316 ; }

revision 2020-02-14 { reference S5-20XXXX ; }

revision 2019-10-28 { reference S5-193518 ; }

revision 2019-06-17 {

description "Initial revision";

}

feature DPCIConfigurationFunction {

description "Classs representing Distributed SON or Domain-Centralized SON

function of PCI configuration feature";

}

feature DESManagementFunction {

description "Classs representing Distributed SON or Domain-Centralized SON Energy Saving feature";

}

feature DRACHOptimizationFunction {

description "Classs representing D-SON function of RACH optimization feature";

}

feature DMROFunction {

description "Classs representing D-SON function of MRO feature";

}

feature CESManagementFunction {

description "Classs representing Cross Domain-Centralized SON Energy Saving feature";

}

grouping NRCellCUGrp {

description "Represents the NRCellCU IOC.";

reference "3GPP TS 28.541";

uses mf3gpp:ManagedFunctionGrp;

leaf cellLocalId {

description "Identifies an NR cell of a gNB. Together with corresponding

gNB ID it forms the NR Cell Identifier (NCI).";

mandatory true;

type int32 { range "0..16383"; }

}

list pLMNInfoList {

description "The PLMNInfoList is a list of PLMNInfo data type. It defines which PLMNs

that can be served by the NR cell, and which S-NSSAIs that can be supported by the

NR cell for corresponding PLMN in case of network slicing feature is supported.";

// Note: Whether the attribute pLMNId in the pLMNInfo can be writable depends on the implementation.

key "mcc mnc";

min-elements 1;

uses nrcommon3gpp:PLMNInfo;

}

leaf nRFrequencyRef {

description "Reference to corresponding NRFrequency instance.";

config false;

type types3gpp:DistinguishedName;

}

}

augment "/me3gpp:ManagedElement/gnbcucp3gpp:GNBCUCPFunction" {

list NRCellCU {

description "Represents the information required by CU that is

responsible for the management of inter-cell mobility and neighbour

relations via ANR.";

reference "3GPP TS 28.541";

key id;

uses top3gpp:Top\_Grp;

container attributes {

uses NRCellCUGrp;

}

uses mf3gpp:ManagedFunctionContainedClasses;

}

}

}

**Next change**

## E.5.20 module \_3gpp-nr-nrm-nrcelldu.yang

module \_3gpp-nr-nrm-nrcelldu {

yang-version 1.1;

namespace "urn:3gpp:sa5:\_3gpp-nr-nrm-nrcelldu";

prefix "nrcelldu3gpp";

import \_3gpp-common-yang-types { prefix types3gpp; }

import \_3gpp-common-managed-function { prefix mf3gpp; }

import \_3gpp-common-managed-element { prefix me3gpp; }

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-nr-nrm-gnbdufunction { prefix gnbdu3gpp; }

import \_3gpp-nr-nrm-rrmpolicy { prefix nrrrmpolicy3gpp; }

import \_3gpp-nr-nrm-common { prefix nrcommon3gpp; }

organization "3GPP SA5";

contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

description "Defines the YANG mapping of the NRCellDU Information Object

Class (IOC) that is part of the NR Network Resource Model (NRM).";

reference "3GPP TS 28.541 5G Network Resource Model (NRM)";

revision 2020-11-25 { reference CR-0385 ; }

revision 2020-05-08 { reference S5-203316 ; }

revision 2020-02-14 { reference S5-20XXXX ; }

revision 2019-10-28 { reference S5-193518 ; }

revision 2019-09-03 {

description "Initial revision";

}

feature CPCIConfigurationFunction {

description "Classs representing Cross Domain-Centralized SON function of PCI configuration feature";

}

grouping NRCellDUGrp {

description "Represents the NRCellDU IOC.";

reference "3GPP TS 28.541";

uses mf3gpp:ManagedFunctionGrp;

uses nrrrmpolicy3gpp:RRMPolicy\_Grp;

leaf cellLocalId {

description "Identifies an NR cell of a gNB. Together with the

corresponding gNB identifier in forms the NR Cell Identity (NCI).";

reference "NCI in 3GPP TS 38.300";

mandatory true;

type int32 { range "0..16383"; }

}

leaf operationalState {

description "Operational state of the NRCellDU instance. Indicates

whether the resource is installed and partially or fully operable

(ENABLED) or the resource is not installed or not operable

(DISABLED).";

config false;

type types3gpp:OperationalState;

}

leaf administrativeState {

description "Administrative state of the NRCellDU. Indicates the

permission to use or prohibition against using the cell, imposed

through the OAM services.";

type types3gpp:AdministrativeState;

default LOCKED;

}

leaf cellState {

description "Cell state of the NRCellDU instance. Indicates whether the

cell is not currently in use (IDLE), or currently in use but not

configured to carry traffic (INACTIVE), or currently in use and is

configured to carry traffic (ACTIVE).";

config false;

type types3gpp:CellState;

}

list pLMNInfoList {

description "The PLMNInfoList is a list of PLMNInfo data type. It defines which PLMNs that

can be served by the NR cell, and which S-NSSAIs that can be supported by the NR cell for

corresponding PLMN in case of network slicing feature is supported. The plMNId of the first

entry of the list is the PLMNId used to construct the nCGI for the NR cell.";

key "mcc mnc";

min-elements 1;

uses nrcommon3gpp:PLMNInfo;

}

leaf nRPCI {

description "The Physical Cell Identity (PCI) of the NR cell.";

reference "3GPP TS 36.211";

mandatory true;

type int32 { range "0..1007"; }

}

leaf nRTAC {

description "The common 5GS Tracking Area Code for the PLMNs.";

reference "3GPP TS 23.003, 3GPP TS 38.473";

type types3gpp:Tac;

}

leaf arfcnDL {

description "NR Absolute Radio Frequency Channel Number (NR-ARFCN) for

downlink.";

reference "3GPP TS 38.104";

mandatory true;

type int32;

}

leaf arfcnUL {

description "NR Absolute Radio Frequency Channel Number (NR-ARFCN) for

uplink.";

reference "3GPP TS 38.104";

type int32;

}

leaf arfcnSUL {

description "NR Absolute Radio Frequency Channel Number (NR-ARFCN) for

supplementary uplink.";

reference "3GPP TS 38.104";

type int32;

}

leaf bSChannelBwDL {

description "Base station channel bandwidth for downlink.";

reference "3GPP TS 38.104";

type int32;

units MHz;

}

leaf bSChannelBwUL {

description "Base station channel bandwidth for uplink.";

reference "3GPP TS 38.104";

type int32;

units MHz;

}

leaf bSChannelBwSUL {

description "Base station channel bandwidth for supplementary uplink.";

reference "3GPP TS 38.104";

mandatory false;

type int32;

units MHz;

}

leaf ssbFrequency {

description "Indicates cell defining SSB frequency domain position.

Frequency (in terms of NR-ARFCN) of the cell defining SSB transmission.

The frequency identifies the position of resource element RE=#0

(subcarrier #0) of resource block RB#10 of the SS block. The frequency

must be positioned on the NR global frequency raster, as defined in

3GPP TS 38.101-1, and within bSChannelBwDL.";

mandatory true;

type int32 { range "0..3279165"; }

}

leaf ssbPeriodicity {

description "Indicates cell defined SSB periodicity. The SSB periodicity

is used for the rate matching purpose.";

mandatory true;

type int32 { range "5 | 10 | 20 | 40 | 80 | 160"; }

units "subframes (ms)";

}

leaf ssbSubCarrierSpacing {

description "Subcarrier spacing of SSB. Only the values 15 kHz or 30 kHz

(< 6 GHz), 120 kHz or 240 kHz (> 6 GHz) are applicable.";

reference "3GPP TS 38.211";

mandatory true;

type int32 { range "15 | 30 | 120 | 240"; }

units kHz;

}

leaf ssbOffset {

description "Indicates cell defining SSB time domain position. Defined

as the offset of the measurement window, in which to receive SS/PBCH

blocks, where allowed values depend on the ssbPeriodicity

(ssbOffset < ssbPeriodicity).";

mandatory true;

type int32 { range "0..159"; }

units "subframes (ms)";

}

leaf ssbDuration {

description "Duration of the measurement window in which to receive

SS/PBCH blocks.";

reference "3GPP TS 38.213";

mandatory true;

type int32 { range "1..5"; }

units "subframes (ms)";

}

leaf-list nRSectorCarrierRef {

description "Reference to corresponding NRSectorCarrier instance.";

min-elements 1;

type types3gpp:DistinguishedName;

}

leaf-list bWPRef {

description "Reference to corresponding BWP instance.";

min-elements 0;

type types3gpp:DistinguishedName;

}

leaf-list nRFrequencyRef {

description "Reference to corresponding NRFrequency instance.";

min-elements 0;

type types3gpp:DistinguishedName;

}

}

augment "/me3gpp:ManagedElement/gnbdu3gpp:GNBDUFunction" {

list NRCellDU {

description "Represents the information of a cell known by DU.";

reference "3GPP TS 28.541";

key id;

uses top3gpp:Top\_Grp;

container attributes {

uses NRCellDUGrp;

}

uses mf3gpp:ManagedFunctionContainedClasses;

}

}

}

**Next change**

## E.5.32 module [\_3gpp-nr-nrm-dpciconfigurationfunction.yang](mailto:_3gpp-nr-nrm-dmrofunction.yang@2020-04-28.yang)

module \_3gpp-nr-nrm-dpciconfigurationfunction {

yang-version 1.1;

namespace "urn:3gpp:sa5:\_3gpp-nr-nrm-dpciconfigurationfunction";

prefix "dpciconfigurationfunction3gpp";

import \_3gpp-common-subnetwork { prefix subnet3gpp; }

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-nr-nrm-nrcellcu { prefix nrcellcu3gpp; }

import \_3gpp-nr-nrm-gnbcucpfunction { prefix gnbcucp3gpp; }

import \_3gpp-common-managed-element { prefix me3gpp; }

organization "3GPP SA5";

contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

description "Defines the YANG mapping of the DPCIConfigurationFunction Information Object Class

(IOC) that is part of the NR Network Resource Model (NRM).";

reference "3GPP TS 28.541 5G Network Resource Model (NRM)";

revision 2020-11-25 { reference CR-0385 ; }

revision 2020-05-08 { reference S5-203316; }

grouping DPCIConfigurationFunctionGrp {

description "Represents the DPCICONFIGURATIONFunction IOC.";

reference "3GPP TS 28.541";

uses top3gpp:Top\_Grp;

list nRPciList {

key NRPci;

description "This holds a list of physical cell identities that can be assigned to the NR cells. This attribute shall be supported if D-SON PCI configuration or domain Centralized SON PCI configuration function is supported.";

leaf NRPci {type int32;}

container attributes {

uses NRPciListGrp;

}

}

leaf dPciConfigurationControl {

description " This attribute determines whether the Distributed SON or Domain-Centralized SON PCI configuration Function is enabled or disabled.";

type boolean;

}

}

grouping NRPciListGrp {

description "Represents the NR PCI list for the PCI configuration function.";

leaf NRPci {

description "This attribute determines the NR PCI.";

type int32 { range "0..1007"; }

units "1";

}

}

augment "/me3gpp:ManagedElement/gnbcucp3gpp:GNBCUCPFunction/nrcellcu3gpp:NRCellCU" {

if-feature nrcellcu3gpp:DPCIConfigurationFunction;

uses DPCIConfigurationFunctionGrp;

}

augment "/me3gpp:ManagedElement" {

if-feature me3gpp:DPCIConfigurationFunction;

uses DPCIConfigurationFunctionGrp;

}

augment "/subnet3gpp:SubNetwork" {

if-feature subnet3gpp:DPCIConfigurationFunction;

uses DPCIConfigurationFunctionGrp;

}

}

**End of changes**