**3GPP TSG-SA5 Meeting #135e *S5-211190***

**e-meeting 25th January - 3rd February 2021**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.535** | **CR** | **0025** | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Relation between Communication service LCM, Control loop LCM and NetworkSlice LCM |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | eCOSLA |  | ***Date:*** | 2021-01-08 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The relation of Communication service LCM, Control loop LCM and NetworkSlice LCMs need to be clear described in 28.535 |
|  |  |
| ***Summary of change:*** | Add description about the relation of Communication service LCM, Control loop LCM and NetworkSlice LCMs |
|  |  |
| ***Consequences if not approved:*** | The relation of Communication service LCM, Control loop LCM and NetworkSlice LCMs are not clear described in 28.535 |
|  |  |
| ***Clauses affected:*** | 4.2.x |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st of changes** |

4.2.x

Relation of Communication service LCM, Control loop LCM and NetworkSlice LCM

The control loop will be initialized with the assurance goal from the Communication service and the mornitored resource information from the allocated NetworkSlice.The control loop lifecycle is dependent on the communincation service lifecycle and the allocated NetworkSlice lifecycle.

* The commissioning phase of the control loop need to be after the commissioning phase of corresponding communication service and NetworkSlice.
* The decommissioning phase of the control loop need to be before the decommissioning phase of corresponding communication service and NetworkSlice.
* The control loop could not exist without the corresponding communication service and NetworkSlice.

|  |
| --- |
| **End of changes** |