**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Correction of incorrect YANG mapping from stage 2 to stage3 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Only Stage 3 YANG changes:  Correcting pyang –strict validation errors  Correcting items that don’t match the stage 2 definitions  Refactored vnfParametersList and peeParametersList into lists following stage 2 and 32.160 clause 6.2.12 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Invalid YANG code, mismatch between stage 2 and 3, mismatch between model mapping guidelines and YANG code. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | D.2.3, D.2.10 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | <https://forge.3gpp.org/rep/sa5/MnS/tree/Rel17_YANG_extracted_from_28623-g60_and_28541-h10_corrected_by_balazs>  <https://forge.3gpp.org/rep/sa5/MnS/tree/Rel16_YANG_extracted_from_28623-g60_and_28541-g70_corrected_by_balazs> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

***First change***

D.2.3 module \_3gpp-common-managed-function.yang

module \_3gpp-common-managed-function {

yang-version 1.1;

namespace urn:3gpp:sa5:\_3gpp-common-managed-function;

prefix mf3gpp;

import \_3gpp-common-yang-types { prefix types3gpp; }

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-common-measurements { prefix meas3gpp; }

import \_3gpp-common-trace { prefix trace3gpp; }

organization "3GPP SA5";

contact "<https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464>";

description "The module defines a base class/grouping for major 3GPP

functions.";

reference

"3GPP TS 28.622

Generic Network Resource Model (NRM)

Integration Reference Point (IRP);

Information Service (IS)

3GPP TS 28.620

Umbrella Information Model (UIM)";

revision 2021-01-25 { reference "CR-0122"; }

revision 2020-09-30 { reference "CR-bbbb"; }

revision 2020-08-06 { reference "CR-0102"; }

revision 2020-08-03 { reference "CR-0095"; }

revision 2020-06-23 { reference "CR-085"; }

revision 2020-06-08 { reference "CR-0092"; }

revision 2019-11-21 { reference "S5-197275, S5-197735"; }

revision 2019-10-28 { reference S5-193518 ; }

revision 2019-06-18 { reference "Initial revision"; }

feature MeasurementsUnderManagedFunction {

description "The MeasurementSubtree shall be contained under ManageElement";

}

feature TraceUnderManagedFunction {

description "The TraceSubtree shall be contained under ManagedFunction";

}

grouping Operation {

description "This data type represents an Operation.";

reference "3gpp TS 28.622";

leaf name {

type string;

mandatory true;

}

leaf-list allowedNFTypes {

type string;

min-elements 1;

description "The type of the managed NF service instance

The specifc values allowed are described in TS 23.501";

}

leaf operationSemantics {

type enumeration {

enum REQUEST\_RESPONSE;

enum SUBSCRIBE\_NOTIFY;

}

config false;

mandatory true;

description "Semantics type of the operation.";

reference "3GPP TS 23.502";

}

}

grouping ManagedNFServiceGrp {

description "A ManagedNFService represents a Network Function (NF) service.";

reference "Clause 7 of 3GPP TS 23.501.";

leaf userLabel {

type string;

description "A user-friendly (and user assignable) name of this object.";

}

leaf nFServiceType {

config false;

mandatory true;

type string;

description "The type of the managed NF service instance

The specifc values allowed are described in clause 7.2 of TS 23.501";

}

list sAP {

key "host port";

min-elements 1;

max-elements 1;

description "The service access point of the managed NF service instance";

uses types3gpp:SAP;

}

list operations {

key name;

min-elements 1;

uses Operation ;

description "Set of operations supported by the managed NF

service instance";

}

leaf administrativeState {

type types3gpp:AdministrativeState;

mandatory true;

description "Permission to use or prohibition against using the instance";

}

leaf operationalState {

type types3gpp:OperationalState;

config false;

mandatory true;

description "Describes whether the resource is installed and working";

}

leaf usageState {

type types3gpp:usageState ;

config false;

mandatory true;

description "Describes whether the resource is actively in use at a

specific instant, and if so, whether or not it has spare

capacity for additional users.";

}

leaf registrationState {

type enumeration {

enum REGISTERED;

enum DEREGISTERED;

}

config false;

}

}

grouping Function\_Grp {

description "A base grouping for 3GPP functions.";

leaf userLabel {

type string;

description "A user-friendly (and user assignable) name of this object.";

}

}

grouping ManagedFunctionGrp {

description "Abstract root class to be inherited/reused by classes

representing 3GPP functions.

Anywhere this grouping is used by classes inheriting from ManagedFunction

the list representing the inheriting class needs to include all

contained classes of ManagedFunction too. Contained classes are

either

- augmented into the Function class or

- shall be included in the list representing the inheriting class

using the grouping ManagedFunctionContainedClasses:

1) EP\_RP solved using augment

2) uses mf3gpp:ManagedFunctionContainedClasses;

";

uses Function\_Grp;

list vnfParametersList {

key vnfInstanceId;

description "Contains the parameter set of the VNF

instance(s) corresponding to an NE.

The presence of this list indicates that the ManagedFunction

represented is realized by one or more VNF instance(s). Otherwise it

shall be absent.

The presence of a vnfParametersList entry, whose vnfInstanceId with a

string length of zero, in createMO operation can trigger the

instantiation of the related VNF/VNFC instances.";

leaf vnfInstanceId {

type string ;

description "VNF instance identifier";

reference "ETSI GS NFV-IFA 008 v2.1.1:

Network Functions Virtualisation (NFV); Management and Orchestration;

Ve-Vnfm reference point - Interface and Information Model Specification

section 9.4.2

ETSI GS NFV-IFA 015 v2.1.2: Network Functions Virtualisation (NFV);

Management and Orchestration; Report on NFV Information Model

section B2.4.2.1.2.3";

}

leaf vnfdId {

type string ;

description "Identifier of the VNFD on which the VNF instance is based.

The absence of the leaf or a string length of zero for vnfInstanceId

means the VNF instance(s) does not exist (e.g. has not been

instantiated yet, has already been terminated).";

reference "ETSI GS NFV-IFA 008 v2.1.1:

Network Functions Virtualisation (NFV); Management and Orchestration;

Ve-Vnfm reference point - Interface and Information Model Specification

section 9.4.2";

}

leaf flavourId {

type string ;

description "Identifier of the VNF Deployment Flavour applied to this

VNF instance.";

reference "ETSI GS NFV-IFA 008 v2.1.1:

Network Functions Virtualisation (NFV) Management and Orchestration";

}

leaf autoScalable {

type boolean ;

mandatory true;

description "Indicator of whether the auto-scaling of this

VNF instance is enabled or disabled.";

}

}

list peeParametersList {

key idx;

description "Contains the parameter set for the control

and monitoring of power, energy and environmental parameters of

ManagedFunction instance(s).";

leaf idx { type uint32; }

leaf siteIdentification {

type string;

mandatory true;

description "The identification of the site where the

ManagedFunction resides.";

}

leaf siteLatitude {

type decimal64 {

fraction-digits 4;

range "-90.0000..+90.0000";

}

description "The latitude of the site where the ManagedFunction

instance resides, based on World Geodetic System (1984 version)

global reference frame (WGS 84). Positive values correspond to

the northern hemisphere. This attribute is optional in case of

BTSFunction and RNCFunction instance(s).";

}

leaf siteLongitude {

type decimal64 {

fraction-digits 4;

range "-180.0000..+180.0000";

}

description "The longitude of the site where the ManagedFunction

instance resides, based on World Geodetic System (1984 version)

global reference frame (WGS 84). Positive values correspond to

degrees east of 0 degrees longitude. This attribute is optional in

case of BTSFunction and RNCFunction instance(s).";

}

leaf siteDescription {

type string;

mandatory true;

description "An operator defined description of the site where

the ManagedFunction instance resides.";

}

leaf equipmentType {

type string;

mandatory true;

description "The type of equipment where the managedFunction

instance resides.";

reference "clause 4.4.1 of ETSI ES 202 336-12";

}

leaf environmentType {

type string;

mandatory true;

description "The type of environment where the managedFunction

instance resides.";

reference "clause 4.4.1 of ETSI ES 202 336-12";

}

leaf powerInterface {

type string;

mandatory true;

description "The type of power.";

reference "clause 4.4.1 of ETSI ES 202 336-12";

}

}

leaf priorityLabel {

mandatory true;

type uint32;

}

uses meas3gpp:SupportedPerfMetricGroupGrp;

}

grouping ManagedFunctionContainedClasses {

description "A grouping used to containe classes (lists) contained by

the abstract IOC ManagedFunction";

list ManagedNFService {

description "Represents a Network Function (NF)";

reference "3GPP TS 23.501";

key id;

uses top3gpp:Top\_Grp;

container attributes {

uses ManagedNFServiceGrp;

}

}

uses meas3gpp:MeasurementSubtree {

if-feature MeasurementsUnderManagedFunction ;

}

uses trace3gpp:TraceSubtree {

if-feature TraceUnderManagedFunction ;

}

}

}

***Next change***

D.2.10 module \_3gpp-common-trace.yang

module \_3gpp-common-trace {

yang-version 1.1;

namespace "urn:3gpp:sa5:\_3gpp-common-trace";

prefix "trace3gpp";

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-common-yang-types {prefix types3gpp; }

import ietf-inet-types { prefix inet; }

organization "3GPP SA5";

contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

description "Trace handling";

reference "3GPP TS 28.623

Generic Network Resource Model (NRM)

Integration Reference Point (IRP);

Solution Set (SS) definitions

3GPP TS 28.622

Generic Network Resource Model (NRM)

Integration Reference Point (IRP);

Information Service (IS)";

revision 2021-01-25 { reference "CR-0122"; }

revision 2020-11-16 { reference "CR-0117"; }

revision 2020-08-06 { reference "CR-0102"; }

grouping TraceJobGrp {

leaf tjJobType {

type enumeration {

enum IMMEDIATE\_MDT\_ONLY;

enum LOGGED\_MDT\_ONLY;

enum TRACE\_ONLY;

enum IMMEDIATE\_MDT\_AND\_TRACE;

enum RLF\_REPORT\_ONLY;

enum RCEF\_REPORT\_ONLY;

enum LOGGED\_MBSFN\_MDT;

}

default TRACE\_ONLY;

description "Specifies the MDT mode and it specifies also whether the

TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined

Trace and MDT job. The attribute is applicable for Trace, MDT, RCEF and

RLF reporting.";

reference "Clause 5.9a of 3GPP TS 32.422 for additional details on the

allowed values.";

}

list tjListOfInterfaces {

key idx;

must 'count(MSCServerInterfaces)+count(MGWInterfaces)+count(RNCInterfaces)'

+'+count(SGSNInterfaces)+count(GGSNInterfaces)+count(S-CSCFInterfaces)'

+'+count(P-CSCFInterfaces)+count(I-CSCFInterfaces)+count(MRFCInterfaces)'

+'+count(MGCFInterfaces)+count(IBCFInterfaces)+count(E-CSCFInterfaces)'

+'+count(BGCFInterfaces)+count(ASInterfaces)+count(HSSInterfaces)'

+'+count(EIRInterfaces)+count(BM-SCInterfaces)+count(MMEInterfaces)'

+'+count(SGWInterfaces)+count(PDN\_GWInterfaces)+count(eNBInterfaces)'

+'+count(en-gNBInterfaces)+count(AMFInterfaces)+count(AUSFInterfaces)'

+'+count(NEFInterfaces)+count(NRFInterfaces)+count(NSSFInterfaces)'

+'+count(PCFInterfaces)+count(SMFInterfaces)+count(SMSFInterfaces)'

+'+count(UDMInterfaces)+count(UPFInterfaces)+count(ng-eNBInterfaces)'

+'+count(gNB-CU-CPInterfaces)+count(gNB-CU-UPInterfaces)+count(gNB-DUInterfaces)';

description "Specifies the interfaces that need to be traced in the given

ManagedEntityFunction.The attribute is applicable only for Trace. In

case this attribute is not used, it carries a null semantic.";

reference "Clause 5.5 of 3GPP TS 32.422 for additional details on the

allowed values.";

leaf idx { type uint32 ; }

leaf-list MSCServerInterfaces {

type enumeration {

enum A ;

enum Iu-CS ;

enum Mc ;

enum MAP-G ;

enum MAP-B ;

enum MAP-E ;

enum MAP-F ;

enum MAP-D ;

enum MAP-C ;

enum CAP ;

}

}

leaf-list MGWInterfaces {

type enumeration {

enum Mc ;

enum Nb-UP ;

enum Iu-UP ;

}

}

leaf-list RNCInterfaces {

type enumeration {

enum Iu-CS ;

enum Iu-PS ;

enum Iur ;

enum Iub ;

enum Uu ;

}

}

leaf-list SGSNInterfaces {

type enumeration {

enum Gb ;

enum Iu-PS ;

enum Gn ;

enum MAP-Gr ;

enum MAP-Gd ;

enum MAP-Gf ;

enum Ge ;

enum Gs ;

enum S6d ;

enum S4 ;

enum S3 ;

enum S13 ;

}

}

leaf-list GGSNInterfaces {

type enumeration {

enum Gn ;

enum Gi ;

enum Gmb ;

}

}

leaf-list S-CSCFInterfaces {

type enumeration {

enum Mw ;

enum Mg ;

enum Mr ;

enum Mi ;

}

}

leaf-list P-CSCFInterfaces {

type enumeration {

enum Gm ;

enum Mw ;

}

}

leaf-list I-CSCFInterfaces {

type enumeration {

enum Cx ;

enum Dx ;

enum Mg ;

enum Mw ;

}

}

leaf-list MRFCInterfaces {

type enumeration {

enum Mp ;

enum Mr ;

}

}

leaf-list MGCFInterfaces {

type enumeration {

enum Mg ;

enum Mj ;

enum Mn ;

}

}

leaf-list IBCFInterfaces {

type enumeration {

enum Ix ;

enum Mx ;

}

}

leaf-list E-CSCFInterfaces {

type enumeration {

enum Mw ;

enum Ml ;

enum Mm ;

enum Mi-Mg ;

}

}

leaf-list BGCFInterfaces {

type enumeration {

enum Mi ;

enum Mj ;

enum Mk ;

}

}

leaf-list ASInterfaces {

type enumeration {

enum Dh ;

enum Sh ;

enum ISC ;

enum Ut ;

}

}

leaf-list HSSInterfaces {

type enumeration {

enum MAP-C ;

enum MAP-D ;

enum Gc ;

enum Gr ;

enum Cx ;

enum S6d ;

enum S6a ;

enum Sh ;

}

}

leaf-list EIRInterfaces {

type enumeration {

enum MAP-F ;

enum S13 ;

enum MAP-Gf ;

}

}

leaf-list BM-SCInterfaces {

type enumeration {

enum Gmb ;

}

}

leaf-list MMEInterfaces {

type enumeration {

enum S1-MME ;

enum S3 ;

enum S6a ;

enum S10 ;

enum S11 ;

enum S13 ;

}

}

leaf-list SGWInterfaces {

type enumeration {

enum S4 ;

enum S5 ;

enum S8 ;

enum S11 ;

enum Gxc ;

}

}

leaf-list PDN\_GWInterfaces {

type enumeration {

enum S2a ;

enum S2b ;

enum S2c ;

enum S5 ;

enum S6b ;

enum Gx ;

enum S8 ;

enum SGi ;

}

}

leaf-list eNBInterfaces {

type enumeration {

enum S1-MME ;

enum X2 ;

}

}

leaf-list en-gNBInterfaces {

type enumeration {

enum S1-MME ;

enum X2 ;

enum Uu ;

enum F1-C ;

enum E1 ;

}

}

leaf-list AMFInterfaces {

type enumeration {

enum N1 ;

enum N2 ;

enum N8 ;

enum N11 ;

enum N12 ;

enum N14 ;

enum N15 ;

enum N20 ;

enum N22 ;

enum N26 ;

}

}

leaf-list AUSFInterfaces {

type enumeration {

enum N12 ;

enum N13 ;

}

}

leaf-list NEFInterfaces {

type enumeration {

enum N29 ;

enum N30 ;

enum N33 ;

}

}

leaf-list NRFInterfaces {

type enumeration {

enum N27 ;

}

}

leaf-list NSSFInterfaces {

type enumeration {

enum N22 ;

enum N31 ;

}

}

leaf-list PCFInterfaces {

type enumeration {

enum N5 ;

enum N7 ;

enum N15 ;

}

}

leaf-list SMFInterfaces {

type enumeration {

enum N4 ;

enum N7 ;

enum N10 ;

enum N11 ;

enum S5-C ;

}

}

leaf-list SMSFInterfaces {

type enumeration {

enum N20 ;

enum N21 ;

}

}

leaf-list UDMInterfaces {

type enumeration {

enum N8 ;

enum N10 ;

enum N13 ;

enum N21 ;

}

}

leaf-list UPFInterfaces {

type enumeration {

enum N4 ;

}

}

leaf-list ng-eNBInterfaces {

type enumeration {

enum NG-C ;

enum Xn-C ;

enum Uu ;

}

}

leaf-list gNB-CU-CPInterfaces {

type enumeration {

enum NG-C ;

enum Xn-C ;

enum Uu ;

enum F1-C ;

enum E1 ;

enum X2-C ;

}

}

leaf-list gNB-CU-UPInterfaces {

type enumeration {

enum E1 ;

}

}

leaf-list gNB-DUInterfaces {

type enumeration {

enum F1-C ;

}

}

}

leaf-list tjListOfNeTypes {

type enumeration {

enum MSC\_SERVER;

enum SGSN;

enum MGW;

enum GGSN;

enum RNC;

enum BM\_SC;

enum MME;

enum SGW;

enum PGW;

enum ENB;

enum EN\_GNB;

enum GNB\_CU\_CP;

enum GNB\_CU\_UP;

enum GNB\_DU;

}

description "Specifies in which type of ManagedFunction the trace should

be activated. The attribute is applicable only for Trace with

Signalling Based Trace activation. In case this attribute is not used,

it carries a null semantic";

reference "Clause 5.4 of 3GPP TS 32.422 for additional details on the

allowed values";

}

leaf tjPLMNTarget {

type string;

mandatory true;

description "Specifies which PLMN that the subscriber of the session to

be recorded uses as selected PLMN. PLMN Target might differ from the

PLMN specified in the Trace Reference";

reference "Clause 5.9b of 3GPP TS 32.422";

}

leaf tjStreamingTraceConsumerURI {

when './tjTraceReportingFormat = "STREAMING"';

type inet:uri;

mandatory true;

description "URI of the Streaming Trace data reporting MnS consumer

(a.k.a. streaming target).

This attribute shall be present if file based trace data reporting is

supported and tjTraceReportingFormat set to 'file based' or when

tjJobType is set to Logged MDT or Logged MBSFN MDT.";

reference "Clause 5.9 of 3GPP TS 32.422";

}

leaf tjTraceCollectionEntityAddress {

when './tjTraceReportingFormat = "FILE\_BASED" or '

+'./tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type union {

type inet:uri;

type inet:ip-address;

}

mandatory true;

description "Specifies the address of the Trace Collection Entity when

the attribute tjTraceReportingFormat is configured for the file-based

reporting. The attribute is applicable for both Trace and MDT.";

reference "Clause 5.9 of 3GPP TS 32.422";

}

leaf tjTraceDepth {

when './tjJobType = "TRACE\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type enumeration {

enum MINIMUM;

enum MEDIUM;

enum MAXIMUM;

enum VENDORMINIMUM;

enum VENDORMEDIUM;

enum VENDORMAXIMUM;

}

default MAXIMUM;

description "Specifies how detailed information should be recorded in the

Network Element. The Trace Depth is a paremeter for Trace Session level,

i.e., the Trace Depth is the same for all of the NEs to be traced in

the same Trace Session.

The attribute is applicable only for Trace, otherwise it carries a null

semantic.";

reference "Clause 5.3 of 3GPP TS 32.422";

}

leaf tjTraceReference {

type uint64;

mandatory true;

description "A globally unique identifier, which uniquely identifies the

Trace Session that is created by the TraceJob.

In case of shared network, it is the MCC and MNC of the Participating

Operator that request the trace session that shall be provided.

The attribute is applicable for both Trace and MDT.";

}

leaf tjTraceReportingFormat {

type enumeration {

enum FILE\_BASED;

enum STREAMING;

}

default FILE\_BASED;

description "Specifies the trace reporting format - streaming trace

reporting or file-based trace reporting";

reference "3GPP TS 32.422 clause 5.11";

}

list tjTraceTarget {

key "targetIdType targetIdValue";

max-elements 1;

leaf targetIdType {

type enumeration {

enum IMSI;

enum IMEI;

enum IMEISV;

enum PUBLIC\_ID;

enum UTRAN\_CELL;

enum E\_UTRAN\_CELL;

enum NG\_RAN\_CELL;

enum ENB;

enum RNC;

enum GNB;

enum SUPI;

}

}

leaf targetIdValue {

type string;

}

description "Specifies the target object of the Trace and MDT. The

attribute is applicable for both Trace and MDT. This attribute

includes the ID type of the target as an enumeration and the ID value.

The tjTraceTarget shall be public ID in case of a Management Based

Activation is done to an ScscfFunction. The tjTraceTarget shall be

cell only in case of the UTRAN cell traffic trace function.

The tjTraceTarget shall be E-UtranCell only in case of E-UTRAN cell

traffic trace function.The tjTraceTarget shall be either IMSI or

IMEI(SV) if the Trace Session is activated to any of the following

ManagedEntity(ies):

- HssFunction

- MscServerFunction

- SgsnFunction

- GgsnFunction

- BmscFunction

- RncFunction

- MmeFunction

The tjTraceTarget shall be IMSI if the Trace Session is activated to a

ManagedEntity playing a role of ServinGWFunction.

In case of signaling based Trace/MDT, the tjTraceTarget attribute shall be

able to carry (IMSI or IMEI(SV)or SUPI), the tjMDTAreaScope attribute shall be

able to carry a list of (cell or E-UtranCell or NRCellDU or TA/LA/RA).

In case of management based Immediate MDT, the tjTraceTarget attribute

shall be null value, the tjMDTAreaScope attribute shall carry a list of

(Utrancell or E-UtranCell or NRCellDU).

In case of management based Logged MDT, the tjTraceTarget attribute

shall carry an eBs or a RNC or gNBs. The Logged MDT should be initiated on

the specified eNB or RNC or gNB in tjTraceTarget. The tjMDTAreaScope attribute

shall carry a list of (Utrancell or E-UtranCell or NRCellDU or TA/LA/RA).

In case of RLF reporting, or RCEF reporting, the tjTraceTarget attribute

shall be null value, the tjMDTAreaScope attribute shall carry one or

list of eNBs/gNBs";

reference "3GPP TS 32.422";

}

leaf tjTriggeringEvent {

when './tjJobType = "TRACE" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type string ;

mandatory true;

description "Specifies the triggering event parameter of the trace session.

The attribute is applicable only for Trace. In case this attribute is

not used, it carries a null semantic.";

reference "Clause 5.1 of 3GPP TS 32.422";

}

leaf tjMDTAnonymizationOfData {

when ./tjMDTAreaScope ;

type enumeration {

enum NO\_IDENTITY;

enum TAC\_OF\_IMEI;

}

default NO\_IDENTITY;

description "Specifies level of MDT anonymization.";

reference "3GPP TS 32.422 clause 5.10.12.";

}

list tjMDTAreaConfigurationForNeighCell {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

key "idx";

min-elements 1;

leaf idx { type uint32 ; }

description "It specifies the area for which UE is requested to perform

measurement logging for neighbour cells which have list of frequencies.

If it is not configured, the UE shall perform measurement logging for

all the neighbour cells.

Applicable only to NR Logged MDT.";

reference "3GPP TS 32.422 clause 5.10.26.";

leaf frequency {

type string;

}

leaf cell {

type string;

}

}

leaf-list tjMDTAreaScope {

type string;

description "specifies MDT area scope when activates an MDT job.

For RLF and RCEF reporting it specifies the eNB or list of eNBs where the

RLF or RCEF reports should be collected.

List of cells/TA/LA/RA for signaling based MDT or management based Logged

MDT.

List of cells for management based Immediate MDT.

Cell, TA, LA, RA are mutually exclusive.

One or list of eNBs for RLF and RCEFreporting";

reference "Clause 5.10.2 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodRrmLte {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

+"24000|28000|32000|64000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM configured

measurement samples for M2, M3 in LTE. The attribute is applicable only

for Immediate MDT. In case this attribute is not used, it carries a

null semantic.";

reference "Clause 5.10.20 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodRrmUmts {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|1280|2048|2560|5120|"

+"10240|60000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM configured

measurement samples for M3, M4, M5 in UMTS. The attribute is applicable

only for Immediate MDT. In case this attribute is not used, it carries

a null semantic";

reference "Clause 5.10.21 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodRrmNR {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|2048|5120|10240|60000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM configured

measurement samples for M4, M5 in NR. The attribute is applicable only

for Immediate MDT. In case this attribute is not used, it carries a

null semantic.";

reference "Clause 5.10.30 of 3GPP TS 32.422";

}

leaf tjMDTEventListForTriggeredMeasurement {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

type enumeration {

enum OUT\_OF\_COVERAGE ;

enum A2\_EVENT ;

}

mandatory true;

description "Specifies event types for event triggered measurement in the

case of logged NR MDT. Each trace session may configure at most one

event. The UE shall perform logging of measurements only upon certain

condition being fulfilled:

- Out of coverage.

- A2 event.";

reference "Clause 5.10.28 of 3GPP TS 32.422";

}

leaf tjMDTEventThreshold {

type int64;

description "Specifies the threshold which should trigger the reporting

in case A2 event reporting in LTE or 1F/1l event in UMTS. The attribute

is applicable only for Immediate MDT and when reportingTrigger is

configured for A2 event in LTE or 1F event or 1l event in UMTS. In

case this attribute is not used, it carries a null semantic.";

reference "Clauses 5.10.7 and 5.10.7a of 3GPP TS 32.422";

}

leaf tjMDTListOfMeasurements {

when './tjJobType = "IMMEDIATE\_MDT"';

type int64;

mandatory true;

description "It specifies the UE measurements that shall be collected in

an Immediate MDT job. The attribute is applicable only for Immediate MDT.

In case this attribute is not used, it carries a null semantic.";

reference "3GPP TS 32.422 clause 5.10.3";

}

leaf tjMDTLoggingDuration {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "600|1200|2400|3600|5400|7200";

}

units seconds;

mandatory true;

description "Specifies how long the MDT configuration is valid at the

UE in case of Logged MDT. The attribute is applicable only for

Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it

carries a null semantic.";

reference "5.10.9 of 3GPP TS 32.422";

}

leaf tjMDTLoggingInterval {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "1280|2560|5120|10240|20480|"

+"30720|40960|61440";

}

units milliseconds;

mandatory true;

description "Specifies the periodicty for Logged MDT. The attribute is

applicable only for Logged MDT and Logged MBSFN MDT. In case this

attribute is not used, it carries a null semantic";

reference "5.10.8 of 3GPP TS 32.422";

}

leaf-list tjMDTMBSFNAreaList {

when './tjJobType = "LOGGED\_MBSFN\_MDT"';

type string;

min-elements 1;

max-elements 8;

description "The MBSFN Area consists of a MBSFN Area ID and Carrier

Frequency (EARFCN). The target MBSFN area List can have up to 8 entries.

This parameter is applicable only if the job type is Logged MBSFN MDT.";

reference "5.10.25 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementPeriodLTE {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|1280|2048|2560|5120|"

+"10240|60000";

}

units milliseconds;

mandatory true;

description "It specifies the measurement period for the Data Volume and

Scheduled IP throughput measurements for MDT taken by the eNB.

The attribute is applicable only for Immediate MDT. In case this

attribute is not used, it carries a null semantic.";

reference "Clause 5.10.23 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementPeriodUMTS {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

+"24000|28000|32000|64000";

}

units milliseconds;

mandatory true;

description "It specifies the measurement period for the Data Volume and

Throughput measurements for MDT taken by RNC.

The attribute is applicable only for Immediate MDT. In case this

attribute is not used, it carries a null semantic.";

reference "Clause 5.10.22 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementQuantity {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint64 ;

mandatory true;

description "It specifies the measurements that are collected in an MDT

job for a UMTS MDT configured for event triggered reporting.";

reference "Clause 5.10.15 of 3GPP TS 32.422";

}

list tjMDTPLMList {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

key "mcc mnc";

uses types3gpp:PLMNId;

min-elements 1;

max-elements 16;

description "It indicates the PLMNs where measurement collection, status

indication and log reporting is allowed.";

reference "Clause 5.10.24 of 3GPP TS 32.422";

}

leaf tjMDTPositioningMethod {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type enumeration {

enum GNSS;

enum E\_CELL\_ID;

}

mandatory true;

description "It specifies what positioning method should be used in the

MDT job.";

reference "Clause 5.10.19 of 3GPP TS 32.422";

}

leaf tjMDTReportAmount {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" and ./tjMDTReportingTrigger = "PERIODICAL"';

type union {

type uint32 {

range "1|4|8|16|32|64" ;

}

type enumeration {

enum INFINITY;

}

}

mandatory true;

description "It specifies the number of measurement reports that shall be

taken for periodic reporting while the UE is in connected.

The attribute is applicable only for Immediate MDT and when

tjMDTReportingTrigger is configured for periodical measurements. In

case this attribute is not used, it carries a null semantic.";

reference "Clause 5.10.6 of 3GPP TS 32.422";

}

leaf tjMDTReportingTrigger {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"';

type enumeration {

enum PERIODICAL;

enum A2\_FOR\_LTE;

enum 1F\_FOR\_UMTS;

enum 1I\_FOR\_UMTS\_MCPS\_TDD;

enum A2\_TRIGGERED\_PERIODIC\_FOR\_LTE;

enum ALL\_CONFIGURED\_RRM\_FOR\_LTE;

enum ALL\_CONFIGURED\_RRM\_FOR\_UMTS;

}

description "It specifies whether periodic or event based measurements

should be collected.

The attribute is applicable only for Immediate MDT and when the

tjMDTListOfMeasurements is configured for M1 (for both UMTS and LTE)

or M2 (only for UMTS). In case this attribute is not used, it carries

a null semantic.";

reference "Clause 5.10.4 of 3GPP TS 32.422";

}

leaf tjMDTReportInterval {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY" and ./tjMDTReportingTrigger = "PERIODICAL"';

type uint32 {

range "120|240|250|480|500|640|1000|1024|2000|2048|3000|4000|"

+"5120|6000|8000|10240|12000|16000|20000|"

+"24000|28000|32000|60000|64000|"

+"360000|720000|1800000|3600000";

}

units milliseconds;

mandatory true;

description "It specifies the interval between the periodical measurements

that shall be taken when the UE is in connected mode.

The attribute is applicable only for Immediate MDT and when

tjMDTReportingTrigger is configured for periodical measurements. In case

this attribute is not used, it carries a null semantic.";

reference "5.10.5 of 3GPP TS 32.422";

}

leaf tjMDTReportType {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

type enumeration {

enum PERIODICAL;

enum EVENT\_TRIGGERED;

}

mandatory true;

description "It specifies report type for logged NR MDT";

reference "Clause 5.10.27 of 3GPP TS 32.422";

}

leaf tjMDTSensorInformation {

type bits {

bit BAROMETRIC\_PRESSURE;

bit UE\_SPEED;

bit UE\_ORIENTATION;

}

default "";

description "It specifies which sensor information shall be included in

logged NR MDT and immediate NR MDT measurement if they are available.

The following sensor measurement can be included or excluded for the UE.";

reference "Clause 5.10.29 of 3GPP TS 32.422";

}

leaf tjMDTTraceCollectionEntityID {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint8;

mandatory true;

description "It specifies the TCE Id which is sent to the UE in Logged MDT.";

reference "Clause 5.10.11 of 3GPP TS 32.422";

}

}

grouping TraceSubtree {

description "Contains classes that manage Tracing.

Should be used in all classes (or classes inheriting from)

- SubNnetwork

- ManagedElement

- ManagedFunction

If a YANG module wants to augment these classes/list/groupings they must

augment all user classes!";

list TraceJob {

description "Represents the Trace Control and Configuration parameters of a

particular Trace Job (see TS 32.421 and TS 32.422 for details).

To activate Trace Jobs, a MnS consumer has to create TraceJob object

instances on the MnS producer. A MnS consumer can activate a Trace Job

for another MnS consumer since it is not required the value of

tjTraceCollectionEntityAddress or tjStreamingTraceConsumerUri to be his

own.

When a MnS consumer wishes to deactivate a Trace Job, the MnS consumer

shall delete the corresponding TraceJob instance.

For details of management Trace Job activation/deactivation see clause

4.1.1.1.2 of TS 32.422.

Creation and deletion of TraceJob instances by MnS consumers is optional;

when not supported, the TraceJob instances may be created and deleted by

the system or be pre-installed.";

key id;

uses top3gpp:Top\_Grp ;

container attributes {

uses TraceJobGrp ;

}

}

}

}

***End of changes***