**3GPP TSG-SA5 Meeting #141-e *S5-221045***

**Online, , 17th Jan 2022 - 26th Jan 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **0647** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Enhance 5G Core managed NF Profile NRM fragment (Stage 3) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia Germany | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | adNRM | | | | |  | ***Date:*** | | | 2022-01-05 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Currently NRM is missing the lcHsupportInd and oclHsupportInd to support fully the configuration of 5GC NFs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add lcHsupportInd and oclHsupportInd in managedNFprofile. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Lack of support for configuring 5G Core NFs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | Annex G | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | 2 | | | | | | | | |

Annex G (normative):  
OpenAPI definition of the 5GC NRM

# G.1 General

This annex contains the OpenAPI definition of the NR NRM in YAML format.

The Information Service (IS) of the NR NRM is defined in clause 4.

Mapping rules to produce the OpenAPI definition based on the IS are defined in TS 32.160 [47].

# G.2 Void

# G.3 Void

# G.4 Solution Set (SS) definitions

## G.4.1 Void

## G.4.2 Void

## G.4.3 OpenAPI document "5gcNrm.yaml"

openapi: 3.0.1

info:

title: 3GPP 5GC NRM

version: 17.4.0

description: >-

OAS 3.0.1 specification of the 5GC NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541; 5G NRM, 5GC NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

AmfIdentifier:

type: object

description: 'AmfIdentifier comprise of amfRegionId, amfSetId and amfPointer'

properties:

amfRegionId:

$ref: '#/components/schemas/AmfRegionId'

amfSetId:

$ref: '#/components/schemas/AmfSetId'

amfPointer:

$ref: '#/components/schemas/AmfPointer'

AmfRegionId:

type: integer

description: AmfRegionId is defined in TS 23.003

maximum: 255

AmfSetId:

type: string

description: AmfSetId is defined in TS 23.003

maximum: 1023

AmfPointer:

type: integer

description: AmfPointer is defined in TS 23.003

maximum: 63

IpEndPoint:

type: object

properties:

ipv4Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

ipv6Prefix:

$ref: 'genericNrm.yaml#/components/schemas/Ipv6Prefix'

transport:

$ref: 'genericNrm.yaml#/components/schemas/TransportProtocol'

port:

type: integer

NFProfileList:

type: array

description: List of NF profile

items:

$ref: '#/components/schemas/NFProfile'

NFProfile:

type: object

description: 'NF profile stored in NRF, defined in TS 29.510'

properties:

nFInstanceId:

type: string

description: uuid of NF instance

nFType:

$ref: 'genericNrm.yaml#/components/schemas/NFType'

nFStatus:

$ref: '#/components/schemas/NFStatus'

plmn:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

sNssais:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

fqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

interPlmnFqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

nfServices:

type: array

items:

$ref: '#/components/schemas/NFService'

NFService:

type: object

description: NF Service is defined in TS 29.510

properties:

serviceInstanceId:

type: string

serviceName:

type: string

version:

type: string

schema:

type: string

fqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

interPlmnFqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

ipEndPoints:

type: array

items:

$ref: '#/components/schemas/IpEndPoint'

apiPrfix:

type: string

allowedPlmns:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

allowedNfTypes:

type: array

items:

$ref: 'genericNrm.yaml#/components/schemas/NFType'

allowedNssais:

type: array

items:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

NFStatus:

type: string

description: any of enumrated value

enum:

- REGISTERED

- SUSPENDED

CNSIIdList:

type: array

items:

$ref: '#/components/schemas/CNSIId'

CNSIId:

type: string

description: CNSI Id is defined in TS 29.531, only for Core Network

TACList:

type: array

items:

$ref: 'nrNrm.yaml#/components/schemas/NrTac'

WeightFactor:

type: integer

UdmInfo:

type: object

properties:

nFSrvGroupId:

type: string

AusfInfo:

type: object

properties:

nFSrvGroupId:

type: string

UpfInfo:

type: object

properties:

smfServingAreas:

type: string

AmfInfo:

type: object

properties:

priority:

type: integer

SupportedDataSetId:

type: string

description: any of enumrated value

enum:

- SUBSCRIPTION

- POLICY

- EXPOSURE

- APPLICATION

Udrinfo:

type: object

properties:

supportedDataSetIds:

type: array

items:

$ref: '#/components/schemas/SupportedDataSetId'

nFSrvGroupId:

type: string

NFInfo:

oneOf:

- $ref: '#/components/schemas/UdmInfo'

- $ref: '#/components/schemas/AusfInfo'

- $ref: '#/components/schemas/UpfInfo'

- $ref: '#/components/schemas/AmfInfo'

- $ref: '#/components/schemas/Udrinfo'

NotificationType:

type: string

enum:

- N1\_MESSAGES

- N2\_INFORMATION

- LOCATION\_NOTIFICATION

- DATA\_REMOVAL\_NOTIFICATION

- DATA\_CHANGE\_NOTIFICATION

- LOCATION\_UPDATE\_NOTIFICATION

- NSSAA\_REAUTH\_NOTIFICATION

- NSSAA\_REVOC\_NOTIFICATION

DefaultNotificationSubscription:

type: object

properties:

notificationType:

$ref: '#/components/schemas/NotificationType'

callbackURI:

type: string

n1MessageClass:

type: boolean

n2InfroamtionClass:

type: boolean

versions:

type: string

binding:

type: string

ManagedNFProfile:

type: object

properties:

nfInstanceID:

type: string

nfType:

$ref: 'genericNrm.yaml#/components/schemas/NFType'

heartbeatTimer:

type: integer

authzInfo:

type: string

hostAddr:

$ref: 'genericNrm.yaml#/components/schemas/HostAddr'

allowedPLMNs:

type: array

item:

$ref: 'comDefs.yaml#/components/schemas/PlmnId''

allowedSNPNs:

type: array

item:

$ref: 'nrNrm.yaml#/components/schemas/SnpnInfo'

allowedNfTypes:

type: array

item:

$ref: 'genericNrm.yaml#/components/schemas/NFType'

allowedNfDomains:

type: array

item: string

allowedNSSAIs:

type: array

item:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

locality:

type: string

nFInfo:

$ref: '#/components/schemas/NFInfo'

capacity:

type: integer

recoveryTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

nfServicePersistence:

type: boolean

nfSetIdList:

type: array

item: string

nfProfileChangesSupportInd:

type: boolean

defaultNotificationSubscriptions:

type: array

item:

$ref: '#/components/schemas/DefaultNotificationSubscription'

servingScope:

type: array

item: string

lcHSupportInd:

type: boolean

olcHSupportInd:

type: boolean

nfSetRecoveryTimeList:

type: array

item:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

scpDomains:

type: array

item: string

vendorId:

type: string

SEPPType:

type: string

description: any of enumrated value

enum:

- CSEPP

- PSEPP

SupportedFunc:

type: object

properties:

function:

type: string

policy:

type: string

SupportedFuncList:

type: array

items:

$ref: '#/components/schemas/SupportedFunc'

CommModelType:

type: string

description: any of enumrated value

enum:

- DIRECT\_COMMUNICATION\_WO\_NRF

- DIRECT\_COMMUNICATION\_WITH\_NRF

- INDIRECT\_COMMUNICATION\_WO\_DEDICATED\_DISCOVERY

- INDIRECT\_COMMUNICATION\_WITH\_DEDICATED\_DISCOVERY

CommModel:

type: object

properties:

groupId:

type: integer

commModelType:

$ref: '#/components/schemas/CommModelType'

targetNFServiceList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

commModelConfiguration:

type: string

CommModelList:

type: array

items:

$ref: '#/components/schemas/CommModel'

CapabilityList:

type: array

items:

type: string

FiveQiDscpMapping:

type: object

properties:

fiveQIValues:

type: array

items:

type: integer

dscp:

type: integer

NetworkSliceInfo:

type: object

properties:

sNSSAI:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

cNSIId:

$ref: '#/components/schemas/CNSIId'

networkSliceRef:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

NetworkSliceInfoList:

type: array

items:

$ref: '#/components/schemas/NetworkSliceInfo'

PacketErrorRate:

type: object

properties:

scalar:

type: integer

exponent:

type: integer

GtpUPathDelayThresholdsType:

type: object

properties:

n3AveragePacketDelayThreshold:

type: integer

n3MinPacketDelayThreshold:

type: integer

n3MaxPacketDelayThreshold:

type: integer

n9AveragePacketDelayThreshold:

type: integer

n9MinPacketDelayThreshold:

type: integer

n9MaxPacketDelayThreshold:

type: integer

QFPacketDelayThresholdsType:

type: object

properties:

thresholdDl:

type: integer

thresholdUl:

type: integer

thresholdRtt:

type: integer

QosData:

type: object

properties:

qosId:

type: string

fiveQIValue:

type: integer

maxbrUl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxbrDl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrUl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrDl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

arp:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Arp'

qosNotificationControl:

type: boolean

reflectiveQos:

type: boolean

sharingKeyDl:

type: string

sharingKeyUl:

type: string

maxPacketLossRateDl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxPacketLossRateUl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

extMaxDataBurstVol:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

QosDataList:

type: array

items:

$ref: '#/components/schemas/QosData'

SteeringMode:

type: object

properties:

steerModeValue:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteerModeValue'

active:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessType'

standby:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessTypeRm'

threeGLoad:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Uinteger'

prioAcc:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessType'

TrafficControlData:

type: object

properties:

tcId:

type: string

flowStatus:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowStatus'

redirectInfo:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RedirectInformation'

addRedirectInfo:

type: array

items:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RedirectInformation'

minItems: 1

muteNotif:

type: boolean

trafficSteeringPolIdDl:

type: string

nullable: true

trafficSteeringPolIdUl:

type: string

nullable: true

routeToLocs:

type: array

items:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

traffCorreInd:

type: boolean

upPathChgEvent:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

steerFun:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

steerModeDl:

$ref: '#/components/schemas/SteeringMode'

steerModeUl:

$ref: '#/components/schemas/SteeringMode'

mulAccCtrl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MulticastAccessControl'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

TrafficControlDataList:

type: array

items:

$ref: '#/components/schemas/TrafficControlData'

PccRule:

type: object

properties:

pccRuleId:

type: string

description: Univocally identifies the PCC rule within a PDU session.

flowInfoList:

type: array

items:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowInformation'

applicationId:

type: string

appDescriptor:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ApplicationDescriptor'

contentVersion:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

precedence:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Uinteger'

afSigProtocol:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

isAppRelocatable:

type: boolean

isUeAddrPreserved:

type: boolean

qosData:

type: array

items:

$ref: '#/components/schemas/QosDataList'

altQosParams:

type: array

items:

$ref: '#/components/schemas/QosDataList'

trafficControlData:

type: array

items:

$ref: '#/components/schemas/TrafficControlDataList'

conditionData:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ConditionData'

tscaiInputDl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

SnssaiInfo:

type: object

properties:

plmnInfo:

$ref: 'nrNrm.yaml#/components/schemas/PlmnInfo'

administrativeState:

$ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

NsacfInfoSnssai:

type: object

properties:

SnssaiInfo:

$ref: '#/components/schemas/SnssaiInfo'

isSubjectToNsac:

type: boolean

maxNumberofUEs:

type: integer

eACMode:

type: string

enum:

- INACTIVE

- ACTIVE

activeEacThreshhold:

type: integer

deactiveEacThreshhold:

type: integer

numberofUEs:

type: integer

uEIdList:

type: array

items:

type: string

SupportedBMOList:

type: array

items:

type: string

ECSAddrConfigInfo:

type: array

items:

type: string

maxNumberofPDUSessions:

type: integer

NrTACRange:

type: object

properties:

nRTACstart:

type: string

nRTACend:

type: string

nRTACpattern:

type: string

TaiRange:

type: object

properties:

plmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

nrTACRangelist:

type: array

items:

$ref: '#/components/schemas/NrTACRange'

#-------- Definition of concrete IOCs --------------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

SubNetwork:

$ref: '#/components/schemas/SubNetwork-Multiple'

ManagedElement:

$ref: '#/components/schemas/ManagedElement-Multiple'

ExternalAmfFunction:

$ref: '#/components/schemas/ExternalAmfFunction-Multiple'

ExternalNrfFunction:

$ref: '#/components/schemas/ExternalNrfFunction-Multiple'

ExternalNssfFunction:

$ref: '#/components/schemas/ExternalNssfFunction-Multiple'

AmfSet:

$ref: '#/components/schemas/AmfSet-Multiple'

AmfRegion:

$ref: '#/components/schemas/AmfRegion-Multiple'

Configurable5QISet:

$ref: '#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: '#/components/schemas/Dynamic5QISet-Multiple'

ManagedElement-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-ncO'

- type: object

properties:

AmfFunction:

$ref: '#/components/schemas/AmfFunction-Multiple'

SmfFunction:

$ref: '#/components/schemas/SmfFunction-Multiple'

UpfFunction:

$ref: '#/components/schemas/UpfFunction-Multiple'

N3iwfFunction:

$ref: '#/components/schemas/N3iwfFunction-Multiple'

PcfFunction:

$ref: '#/components/schemas/PcfFunction-Multiple'

AusfFunction:

$ref: '#/components/schemas/AusfFunction-Multiple'

UdmFunction:

$ref: '#/components/schemas/UdmFunction-Multiple'

UdrFunction:

$ref: '#/components/schemas/UdrFunction-Multiple'

UdsfFunction:

$ref: '#/components/schemas/UdsfFunction-Multiple'

NrfFunction:

$ref: '#/components/schemas/NrfFunction-Multiple'

NssfFunction:

$ref: '#/components/schemas/NssfFunction-Multiple'

SmsfFunction:

$ref: '#/components/schemas/SmsfFunction-Multiple'

LmfFunction:

$ref: '#/components/schemas/LmfFunction-Multiple'

NgeirFunction:

$ref: '#/components/schemas/NgeirFunction-Multiple'

SeppFunction:

$ref: '#/components/schemas/SeppFunction-Multiple'

NwdafFunction:

$ref: '#/components/schemas/NwdafFunction-Multiple'

ScpFunction:

$ref: '#/components/schemas/ScpFunction-Multiple'

NefFunction:

$ref: '#/components/schemas/NefFunction-Multiple'

Configurable5QISet:

$ref: '#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: '#/components/schemas/Dynamic5QISet-Multiple'

GUAMInfo:

type: object

properties:

pLMNId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

aMFIdentifier:

type: integer

AmfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

amfIdentifier:

$ref: '#/components/schemas/AmfIdentifier'

sBIFqdn:

type: string

interPlmnFQDN:

type: string

taiList:

$ref: 'nrNrm.yaml#/components/schemas/Tai'

taiRangeList:

$ref: 'nrNrm.yaml#/components/schemas/TaiRange'

weightFactor:

$ref: '#/components/schemas/WeightFactor'

cNSIIdList:

$ref: '#/components/schemas/CNSIIdList'

gUAMIdList:

$ref: '#/components/schemas/GUAMInfo'

backupInfoAmfFailure:

$ref: '#/components/schemas/GUAMInfo'

backupInfoAmfRemoval:

$ref: '#/components/schemas/GUAMInfo'

amfSetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N2:

$ref: '#/components/schemas/EP\_N2-Multiple'

EP\_N8:

$ref: '#/components/schemas/EP\_N8-Multiple'

EP\_N11:

$ref: '#/components/schemas/EP\_N11-Multiple'

EP\_N12:

$ref: '#/components/schemas/EP\_N12-Multiple'

EP\_N14:

$ref: '#/components/schemas/EP\_N14-Multiple'

EP\_N15:

$ref: '#/components/schemas/EP\_N15-Multiple'

EP\_N17:

$ref: '#/components/schemas/EP\_N17-Multiple'

EP\_N20:

$ref: '#/components/schemas/EP\_N20-Multiple'

EP\_N22:

$ref: '#/components/schemas/EP\_N22-Multiple'

EP\_N26:

$ref: '#/components/schemas/EP\_N26-Multiple'

EP\_NLS:

$ref: '#/components/schemas/EP\_NLS-Multiple'

EP\_NLG:

$ref: '#/components/schemas/EP\_NLG-Multiple'

AmfSet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

nRTACList:

$ref: '#/components/schemas/TACList'

amfSetId:

$ref: '#/components/schemas/AmfSetId'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

aMFRegionRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

aMFSetMemberList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

AmfRegion-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

nRTACList:

$ref: '#/components/schemas/TACList'

amfRegionId:

$ref: '#/components/schemas/AmfRegionId'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

aMFSetListRef:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

SmfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

nRTACList:

$ref: '#/components/schemas/TACList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

configurable5QISetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N4:

$ref: '#/components/schemas/EP\_N4-Multiple'

EP\_N7:

$ref: '#/components/schemas/EP\_N7-Multiple'

EP\_N10:

$ref: '#/components/schemas/EP\_N10-Multiple'

EP\_N11:

$ref: '#/components/schemas/EP\_N11-Multiple'

EP\_N16:

$ref: '#/components/schemas/EP\_N16-Multiple'

EP\_S5C:

$ref: '#/components/schemas/EP\_S5C-Multiple'

FiveQiDscpMappingSet:

$ref: '#/components/schemas/FiveQiDscpMappingSet-Single'

GtpUPathQoSMonitoringControl:

$ref: '#/components/schemas/GtpUPathQoSMonitoringControl-Single'

QFQoSMonitoringControl:

$ref: '#/components/schemas/QFQoSMonitoringControl-Single'

PredefinedPccRuleSet:

$ref: '#/components/schemas/PredefinedPccRuleSet-Single'

UpfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

nRTACList:

$ref: '#/components/schemas/TACList'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

supportedBMOList:

$ref: '#/components/schemas/SupportedBMOList’

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N3:

$ref: '#/components/schemas/EP\_N3-Multiple'

EP\_N4:

$ref: '#/components/schemas/EP\_N4-Multiple'

EP\_N6:

$ref: '#/components/schemas/EP\_N6-Multiple'

EP\_N9:

$ref: '#/components/schemas/EP\_N9-Multiple'

EP\_S5U:

$ref: '#/components/schemas/EP\_S5U-Multiple'

N3iwfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N3:

$ref: '#/components/schemas/EP\_N3-Multiple'

EP\_N4:

$ref: '#/components/schemas/EP\_N4-Multiple'

PcfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

supportedBMOList:

$ref: '#/components/schemas/SupportedBMOList’ '

configurable5QISetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N5:

$ref: '#/components/schemas/EP\_N5-Multiple'

EP\_N7:

$ref: '#/components/schemas/EP\_N7-Multiple'

EP\_N15:

$ref: '#/components/schemas/EP\_N15-Multiple'

EP\_N16:

$ref: '#/components/schemas/EP\_N16-Multiple'

EP\_Rx:

$ref: '#/components/schemas/EP\_Rx-Multiple'

PredefinedPccRuleSet:

$ref: '#/components/schemas/PredefinedPccRuleSet-Single'

AusfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N12:

$ref: '#/components/schemas/EP\_N12-Multiple'

EP\_N13:

$ref: '#/components/schemas/EP\_N13-Multiple'

UdmFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N8:

$ref: '#/components/schemas/EP\_N8-Multiple'

EP\_N10:

$ref: '#/components/schemas/EP\_N10-Multiple'

EP\_N13:

$ref: '#/components/schemas/EP\_N13-Multiple'

UdrFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

UdsfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

NrfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

cNSIIdList:

$ref: '#/components/schemas/CNSIIdList'

nFProfileList:

$ref: '#/components/schemas/NFProfileList'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N27:

$ref: '#/components/schemas/EP\_N27-Multiple'

NssfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

cNSIIdList:

$ref: '#/components/schemas/CNSIIdList'

nFProfileList:

$ref: '#/components/schemas/NFProfileList'

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

commModelList:

$ref: '#/components/schemas/CommModelList'

eCSAddrConfigInfo:

$ref: '#/components/schemas/ECSAddrConfigInfo'$ref: '#/components/schemas/ECSAddrConfigInfo'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N22:

$ref: '#/components/schemas/EP\_N22-Multiple'

EP\_N31:

$ref: '#/components/schemas/EP\_N31-Multiple'

SmsfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N20:

$ref: '#/components/schemas/EP\_N20-Multiple'

EP\_N21:

$ref: '#/components/schemas/EP\_N21-Multiple'

EP\_MAP\_SMSC:

$ref: '#/components/schemas/EP\_MAP\_SMSC-Multiple'

LmfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_NLS:

$ref: '#/components/schemas/EP\_NLS-Multiple'

NgeirFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N17:

$ref: '#/components/schemas/EP\_N17-Multiple'

SeppFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

sEPPType:

$ref: '#/components/schemas/SEPPType'

sEPPId:

type: integer

fqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N32:

$ref: '#/components/schemas/EP\_N32-Multiple'

NwdafFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

networkSliceInfoList:

$ref: '#/components/schemas/NetworkSliceInfoList'

ScpFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

supportedFuncList:

$ref: '#/components/schemas/SupportedFuncList'

address:

$ref: 'genericNrm.yaml#/components/schemas/HostAddr'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

NefFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

sBIFqdn:

type: string

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

capabilityList:

$ref: '#/components/schemas/CapabilityList'

isCAPIFSup:

type: boolean

taiList:

items:

$ref: 'nrNrm.yaml#/components/schemas/TaiList'

taiRangeList:

type: array

items:

$ref: '#/components/schemas/TaiRange’

dnai：

type：string

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N33:

$ref: '#/components/schemas/EP\_N33-Multiple'

NsacfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

nsacfInfoSnssai:

type: array

items:

$ref: '#/components/schemas/NsacfInfoSnssai'

taiList:

type: array

items:

$ref: 'nrNrm.yaml#/components/schemas/TaiList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_N60:

$ref: '#/components/schemas/EP\_N60-Multiple'

DDNMFFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

sBIFqdn:

type: string

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

commModelList:

$ref: '#/components/schemas/CommModelList'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_Npc464:

$ref: '#/components/schemas/EP\_Npc464-Multiple'

EP\_Npc665:

$ref: '#/components/schemas/EP\_Npc665-Multiple'

EP\_Npc766:

$ref: '#/components/schemas/EP\_Npc766-Multiple'

EP\_Npc8:

$ref: '#/components/schemas/EP\_Npc8-Multiple'

EASDFFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

sBIFqdn:

type: string

managedNFProfile:

$ref: '#/components/schemas/ManagedNFProfile'

serverAddr:

type: string

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_Nxx:

$ref: '#/components/schemas/EP\_Nxx-Multiple'

ExternalAmfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

amfIdentifier:

$ref: '#/components/schemas/AmfIdentifier'

ExternalNrfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

ExternalNssfFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnIdList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

ExternalSeppFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

plmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

sEPPId:

type: integer

fqdn:

$ref: 'genericNrm.yaml#/components/schemas/Fqdn'

EP\_N2-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N3-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

EP\_N4-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N5-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N6-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N7-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N8-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N9-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N10-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N11-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N12-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N13-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N14-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N15-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N16-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N17-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N20-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N21-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N22-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N26-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N27-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N31-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N32-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

remotePlmnId:

$ref: 'nrNrm.yaml#/components/schemas/PlmnId'

remoteSeppAddress:

$ref: 'genericNrm.yaml#/components/schemas/HostAddr'

remoteSeppId:

type: integer

n32cParas:

type: string

n32fPolicy:

type: string

withIPX:

type: boolean

EP\_N33-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_S5C-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_S5U-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Rx-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_MAP\_SMSC-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_NLS-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_NLG-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_N60-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Npc464-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Npc665-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Npc766-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Npc8-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

EP\_Nxx-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

remoteAddress:

$ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

FiveQiDscpMappingSet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

FiveQiDscpMappingList:

type: array

items:

$ref: '#/components/schemas/FiveQiDscpMapping'

FiveQICharacteristics-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

fiveQIValue:

type: integer

resourceType:

type: string

enum:

- GBR

- NonGBR

priorityLevel:

type: integer

packetDelayBudget:

type: integer

packetErrorRate:

$ref: '#/components/schemas/PacketErrorRate'

averagingWindow:

type: integer

maximumDataBurstVolume:

type: integer

FiveQICharacteristics-Multiple:

type: array

items:

$ref: '#/components/schemas/FiveQICharacteristics-Single'

Configurable5QISet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

configurable5QIs:

type: array

items:

$ref: '#/components/schemas/FiveQICharacteristics-Multiple'

Dynamic5QISet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

dynamic5QIs:

type: array

items:

$ref: '#/components/schemas/FiveQICharacteristics-Multiple'

GtpUPathQoSMonitoringControl-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

gtpUPathQoSMonitoringState:

type: string

enum:

- ENABLED

- DISABLED

gtpUPathMonitoredSNSSAIs:

type: array

items:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

monitoredDSCPs:

type: array

items:

type: integer

minimum: 0

maximum: 255

isEventTriggeredGtpUPathMonitoringSupported:

type: boolean

isPeriodicGtpUMonitoringSupported:

type: boolean

isImmediateGtpUMonitoringSupported:

type: boolean

gtpUPathDelayThresholds:

$ref: '#/components/schemas/GtpUPathDelayThresholdsType'

gtpUPathMinimumWaitTime:

type: integer

gtpUPathMeasurementPeriod:

type: integer

QFQoSMonitoringControl-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

qFQoSMonitoringState:

type: string

enum:

- ENABLED

- DISABLED

qFMonitoredSNSSAIs:

type: array

items:

$ref: 'nrNrm.yaml#/components/schemas/Snssai'

qFMonitored5QIs:

type: array

items:

type: integer

minimum: 0

maximum: 255

isEventTriggeredQFMonitoringSupported:

type: boolean

isPeriodicQFMonitoringSupported:

type: boolean

isSessionReleasedQFMonitoringSupported:

type: boolean

qFPacketDelayThresholds:

$ref: '#/components/schemas/QFPacketDelayThresholdsType'

qFMinimumWaitTime:

type: integer

qFMeasurementPeriod:

type: integer

PredefinedPccRuleSet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

predefinedPccRules:

type: array

items:

$ref: '#/components/schemas/PccRule'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

SubNetwork-Multiple:

type: array

items:

$ref: '#/components/schemas/SubNetwork-Single'

ManagedElement-Multiple:

type: array

items:

$ref: '#/components/schemas/ManagedElement-Single'

AmfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/AmfFunction-Single'

SmfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/SmfFunction-Single'

UpfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/UpfFunction-Single'

N3iwfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/N3iwfFunction-Single'

PcfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/PcfFunction-Single'

AusfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/AusfFunction-Single'

UdmFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/UdmFunction-Single'

UdrFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/UdrFunction-Single'

UdsfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/UdsfFunction-Single'

NrfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NrfFunction-Single'

NssfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NssfFunction-Single'

SmsfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/SmsfFunction-Single'

LmfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/LmfFunction-Single'

NgeirFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NgeirFunction-Single'

SeppFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/SeppFunction-Single'

NwdafFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NwdafFunction-Single'

ScpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ScpFunction-Single'

NefFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NefFunction-Single'

NsacfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/NsacfFunction-Single'

ExternalAmfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalAmfFunction-Single'

ExternalNrfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalNrfFunction-Single'

ExternalNssfFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalNssfFunction-Single'

ExternalSeppFunction-Nultiple:

type: array

items:

$ref: '#/components/schemas/ExternalSeppFunction-Single'

AmfSet-Multiple:

type: array

items:

$ref: '#/components/schemas/AmfSet-Single'

AmfRegion-Multiple:

type: array

items:

$ref: '#/components/schemas/AmfRegion-Single'

EP\_N2-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N2-Single'

EP\_N3-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N3-Single'

EP\_N4-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N4-Single'

EP\_N5-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N5-Single'

EP\_N6-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N6-Single'

EP\_N7-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N7-Single'

EP\_N8-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N8-Single'

EP\_N9-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N9-Single'

EP\_N10-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N10-Single'

EP\_N11-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N11-Single'

EP\_N12-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N12-Single'

EP\_N13-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N13-Single'

EP\_N14-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N14-Single'

EP\_N15-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N15-Single'

EP\_N16-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N16-Single'

EP\_N17-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N17-Single'

EP\_N20-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N20-Single'

EP\_N21-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N21-Single'

EP\_N22-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N22-Single'

EP\_N26-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N26-Single'

EP\_N27-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N27-Single'

EP\_N31-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N31-Single'

EP\_N32-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N32-Single'

EP\_N33-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N33-Single'

EP\_S5C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_S5C-Single'

EP\_S5U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_S5U-Single'

EP\_Rx-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Rx-Single'

EP\_MAP\_SMSC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_MAP\_SMSC-Single'

EP\_NLS-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NLS-Single'

EP\_NLG-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NLG-Single'

EP\_N60-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_N60-Single'

EP\_Npc464-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Npc464-Single'

EP\_Npc665-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Npc665-Single'

EP\_Npc766-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Npc766-Single'

EP\_Npc8-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Npc8-Single'

EP\_Nxx-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Nxx-Single'

Configurable5QISet-Multiple:

type: array

items:

$ref: '#/components/schemas/Configurable5QISet-Single'

Dynamic5QISet-Multiple:

type: array

items:

$ref: '#/components/schemas/Dynamic5QISet-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

resources-5gcNrm:

oneOf:

- $ref: '#/components/schemas/SubNetwork-Single'

- $ref: '#/components/schemas/ManagedElement-Single'

- $ref: '#/components/schemas/AmfFunction-Single'

- $ref: '#/components/schemas/SmfFunction-Single'

- $ref: '#/components/schemas/UpfFunction-Single'

- $ref: '#/components/schemas/N3iwfFunction-Single'

- $ref: '#/components/schemas/PcfFunction-Single'

- $ref: '#/components/schemas/AusfFunction-Single'

- $ref: '#/components/schemas/UdmFunction-Single'

- $ref: '#/components/schemas/UdrFunction-Single'

- $ref: '#/components/schemas/UdsfFunction-Single'

- $ref: '#/components/schemas/NrfFunction-Single'

- $ref: '#/components/schemas/NssfFunction-Single'

- $ref: '#/components/schemas/SmsfFunction-Single'

- $ref: '#/components/schemas/LmfFunction-Single'

- $ref: '#/components/schemas/NgeirFunction-Single'

- $ref: '#/components/schemas/SeppFunction-Single'

- $ref: '#/components/schemas/NwdafFunction-Single'

- $ref: '#/components/schemas/ScpFunction-Single'

- $ref: '#/components/schemas/NefFunction-Single'

- $ref: '#/components/schemas/NsacfFunction-Single'

- $ref: '#/components/schemas/ExternalAmfFunction-Single'

- $ref: '#/components/schemas/ExternalNrfFunction-Single'

- $ref: '#/components/schemas/ExternalNssfFunction-Single'

- $ref: '#/components/schemas/ExternalSeppFunction-Single'

- $ref: '#/components/schemas/AmfSet-Single'

- $ref: '#/components/schemas/AmfRegion-Single'

- $ref: '#/components/schemas/QFQoSMonitoringControl-Single'

- $ref: '#/components/schemas/GtpUPathQoSMonitoringControl-Single'

- $ref: '#/components/schemas/EP\_N2-Single'

- $ref: '#/components/schemas/EP\_N3-Single'

- $ref: '#/components/schemas/EP\_N4-Single'

- $ref: '#/components/schemas/EP\_N5-Single'

- $ref: '#/components/schemas/EP\_N6-Single'

- $ref: '#/components/schemas/EP\_N7-Single'

- $ref: '#/components/schemas/EP\_N8-Single'

- $ref: '#/components/schemas/EP\_N9-Single'

- $ref: '#/components/schemas/EP\_N10-Single'

- $ref: '#/components/schemas/EP\_N11-Single'

- $ref: '#/components/schemas/EP\_N12-Single'

- $ref: '#/components/schemas/EP\_N13-Single'

- $ref: '#/components/schemas/EP\_N14-Single'

- $ref: '#/components/schemas/EP\_N15-Single'

- $ref: '#/components/schemas/EP\_N16-Single'

- $ref: '#/components/schemas/EP\_N17-Single'

- $ref: '#/components/schemas/EP\_N20-Single'

- $ref: '#/components/schemas/EP\_N21-Single'

- $ref: '#/components/schemas/EP\_N22-Single'

- $ref: '#/components/schemas/EP\_N26-Single'

- $ref: '#/components/schemas/EP\_N27-Single'

- $ref: '#/components/schemas/EP\_N31-Single'

- $ref: '#/components/schemas/EP\_N32-Single'

- $ref: '#/components/schemas/EP\_N33-Single'

- $ref: '#/components/schemas/EP\_N60-Single'

- $ref: '#/components/schemas/EP\_S5C-Single'

- $ref: '#/components/schemas/EP\_S5U-Single'

- $ref: '#/components/schemas/EP\_Rx-Single'

- $ref: '#/components/schemas/EP\_MAP\_SMSC-Single'

- $ref: '#/components/schemas/EP\_NLS-Single'

- $ref: '#/components/schemas/EP\_NLG-Single'

- $ref: '#/components/schemas/Configurable5QISet-Single'

- $ref: '#/components/schemas/FiveQiDscpMappingSet-Single'

- $ref: '#/components/schemas/PredefinedPccRuleSet-Single'

- $ref: '#/components/schemas/Dynamic5QISet-Single'