**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.536** | **CR** | **0037** | **rev** | **-** | **Current version:** | **17.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Editorial on the definition of AssuranceClosedControlLoop |
|  |  |
| ***Source to WG:*** | Nokia Germany |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | eCOSLA |  | ***Date:*** | 2022-01-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The current text includes some wording that needs improvement.  |
|  |  |
| ***Summary of change:*** | Improve readability of the text.  |
|  |  |
| ***Consequences if not approved:*** | The text would be more hard to read.  |
|  |  |
| ***Clauses affected:*** | 4.1.2.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

##### 4.1.2.3.1 AssuranceClosedControlLoop

4.1.2.3.1.1 Definition

This class represents the information for controlling and monitoring an assurance closed control loop associated with a NetworkSlice or NetworkSliceSubnet. It can be name-contained by SubNetwork or ManagedElement.

To express the assurance closed control loop goals, the MnS consumer needs to request the MnS producer to create an AssuranceClosedControlLoop on the MnS producer. The MnS producer may trigger to create the AssuranceClosedControlLoop as well, for example, when an instance of NetworkSlice or NetworkSliceSubnet is created, MnS producer may create an instance of AssuranceClosedControlLoop associated to the instance of NetworkSlice or NetworkSliceSubnet to assure the target described in ServiceProfile or SliceProfile. For the deletion of the assurance closed control loop, the MnS consumer needs to request the MnS producer to delete the AssuranceClosedControlLoop to free up resources on the MnS producer. MnS producer also can trigger to delete AssuranceClosedControlLoop to free up resources by itself.

For temporary deactivation of the assurance closed control loop, the MnS consumer can modify the value of the administrative state attribute to “LOCKED”. The MnS producer may disable the assurance closed control loop, for example in conflict situations, by setting the operational state attribute to “disabled”. When a closed control loop is enabled by the MnS producer, the operational state is set again to “enabled”. For the activation of an assurance closed control loop, the MnS consumer can modify the value of the administrative state attribute to “UNLOCKED”.

An AssuranceClosedControlLoop can name-contain multiple instances of AssuranceGoal which represents the assurance goal and corresponding observed or predicted goal fulfilment information (see clause 4.1.2.3.2). The AssuranceGoal may optionally include an assurance scope in terms of location (see clause 4.1.2.3.2).

The attribute “controlLoopLifeCyclePhase” is used to keep track of the lifecycle of an AssuranceClosedControlLoop

4.1.2.3.1.2 Attributes

The AssuranceClosedControlLoop IOC includes attributes inherited from Top IOC (defined TS 28.622[5]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| operationalState | M | T | F | F | T |
| administrativeState | M | T | T | F | T |
| controlLoopLifeCyclePhase | M | T | T | F | T |

4.1.2.3.1.3 Constraints

No constraints have been defined for this document.

4.1.2.3.1.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for this IOC, without exceptions or additions.