**3GPP TSG-SA5 Meeting #141-e *S5-221161***

**e-meeting, 17 - 24 January 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **0538** | **rev** | **2** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Add tenant IOC to support multiple tenant environment | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eMEMTANE | | | | |  | ***Date:*** | | | 2021-11-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | It was endorsed to enhance NRM with a tenant IOC associated to S-NSSAI list to support multiple tenant environment in 3GPP management system in last meeting (S5-203134). But the definition of tenant IOC is missing in 3GPP specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add a tenant IOC for description of tenant information in TS 28.541. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The definition of tenant IOC is missing in 3GPP specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 6.2, 6.3.X(new), 6.4.1, J.4.3,Annex X(new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR … CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge link: <https://forge.3gpp.org/rep/sa5/MnS/tree/28.541_Rel17_CR0538_Add_tenant_IOC_to_support_multiple_tenant_environment> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S5-215089 is the revision of S5-214218.  S5-216228 is the revision of S5-215089.  S5-22xxxx is the revision of S5-216228. | | | | | | | | |

|  |
| --- |
| **1st Change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System".

[3] 3GPP TS 38.300: "NR; Overall description; Stage-2".

[4] 3GPP TS 38.401: "NG-RAN; Architecture description".

[5] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[6] 3GPP TS 38.420: "NG-RAN; Xn general aspects and principles".

[7] 3GPP TS 38.470: "NG-RAN; F1 general aspects and principles".

[8] 3GPP TS 38.473: "NG-RAN; F1 application protocol (F1AP)".

[9] 3GPP TS 37.340: "NR; Multi-connectivity; Overall description; Stage 2".

[10] 3GPP TS 28.540: "Management and orchestration; 5G Network Resource Model (NRM);Stage 1".

[11] 3GPP TS 28.662: "Telecommunication management; Generic Radio Access Network (RAN) Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS) ".

[12] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception".

[13] 3GPP TS 23.003: "Numbering, Addressing and Identification".

[14] 3GPP TS 36.410: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 general aspects and principles".

[15] 3GPP TS 36.423: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); X2 application protocol".

[16] 3GPP TS 36.425: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); X2 interface user plane protocol".

[17] 3GPP TS 28.625: "State Management Data Definition Integration Reference Point (IRP); Information Service (IS)".

[18] ITU-T Recommendation X.731: "Information technology - Open Systems Interconnection - Systems Management: State management function".

[19] 3GPP TS 28.658: "Telecommunications management; Evolved Universal Terrestrial Radio Access Network (E-UTRAN) Network Resource Model (NRM) Integration Reference Point (IRP): Information Service (IS)".

[20] 3GPP TS 28.702: "Core Network (CN) Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[21] 3GPP TS 28.708: "Telecommunication management; Evolved Packet Core (EPC) Network Resource Model (NRM) Integration Reference Point (IRP): Information Service (IS)".

[22] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[23] 3GPP TS 29.510: "5G system; Network Function Repository Services; Stage 3".

[24] 3GPP TS 29.531: "5G System; Network Slice Selection Services Stage 3".

[25] Void.

[26] 3GPP TS 28.531: "Management and orchestration; Provisioning".

[27] 3GPP TS 28.554: "Management and orchestration; 5G End to end Key Performance Indicators (KPI)".

[28] 3GPP TS 22.261: "Service requirements for next generation new services and markets".

[29] ETSI GS NFV-IFA 013 V2.4.1 (2018-02) "Network Function Virtualisation (NFV); Management and Orchestration; Os-Ma-nfvo Reference Point - Interface and Information Model Specification".

[30] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[31] Void.

[32] 3GPP TS 38.211: "NR; Physical channels and modulation".

[33] 3GPP TS 32.616: "Telecommunication management; Configuration Management (CM); Bulk CM Integration Reference Point (IRP); Solution Set (SS) definitions".

[34] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[35] 3GPP TS 28.532: "Management and orchestration; Management services".

[36] Void.

[37] IETF RFC 791: "Internet Protocol".

[38] IETF RFC 2373: "IP Version 6 Addressing Architecture".

[39] IEEE 802.1Q: "Media Access Control Bridges and Virtual Bridged Local Area Networks".

[40] ETSI GR NFV-IFA 015 (V2.4.1): "Network Function Virtualisation (NFV) Release 2; Management and Orchestration; Report on NFV Information Model".

[41] 3GPP TS 38.213: "NR; Physical layer procedures for control".

[42] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[43] 3GPP TS 32.156: "Telecommunication management; Fixed Mobile Convergence (FMC) model repertoire".

[44] IETF RFC 4122: "A Universally Unique IDentifier (UUID) URN Namespace".

[45] IETF RFC 8528: "YANG Schema Mount".

[46] Void

[47] 3GPP TS 32.160: "Management and orchestration; Management Service Template".

[48] 3GPP TS 38.463: "NG-RAN; E1 application protocol (E1AP)".

[49] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in Idle mode and RRC Inactive state".

[50] GSMA NG.116 - Generic Network Slice Template Version 3.0 (2020-05-22).

[51] 3GPP TS 22.104: "Service requirements for cyber-physical control applications in vertical domains; Stage 1".

[52] 3GPP TS 33.501: "Security architecture and procedures for the 5G System".

[53] 3GPP TS 38.901: "Study on channel model for frequencies from 0.5 to 100 GHz ".

[54] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[55] 3GPP TS 38.215: "NR; Physical layer measurements".

[56] 3GPP TS 29.244: "Technical Specification Group Core Network and Terminals; Interface between the Control Plane and the User Plane Nodes; Stage 3".

[57] 3GPP TS 28.313: "Self-Organizing Networks (SON) for 5G networks".

[58] 3GPP TS 38.423: "NR; Xn application protocol (XnAP)".

[59] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System; Stage 2".

[60] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[61] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[62] 3GPP TS 29.214: "Policy and Charging Control over Rx reference point".

[63] IETF RFC 7042: "IANA Considerations and IETF Protocol and Documentation Usage for IEEE 802 Parameters".

[64] IEEE 802.3-2015: "IEEE Standard for Ethernet".

[65] IEEE 802.1Q-2014: "Bridges and Bridged Networks".

[66] IETF RFC 4301: "Security Architecture for the Internet Protocol".

[67] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[68] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[69] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[70] 3GPP TS 28.530: "Management and orchestration; Concepts, use cases and requirements".

[71] 3GPP TS 28.310: "Management and orchestration; Energy efficiency of 5G".

[xx] 3GPP TS 28.533: "Management and orchestration; Architecture framework".

|  |
| --- |
| **2nd Change** |

## 6.2 Class diagram

### 6.2.1 Relationships

Figure 6.2.1-1: Network slice NRM fragment relationship

NOTE 1: The <<OpenModelClass>> NetworkService and <<OpenModelClass>> VNF are defined in [40].

NOTE 2: The target Network Service (NS) instance represents a group of VNFs and PNFs that are supporting the source network slice subnet instance.

NOTE 3: The instance tree of this NRM fragment would not contain the instances of NetworkService and VNF. However, the NetworkSliceSubNet instances would have an attribute holding the identifiers of NetworkService instances and the ManagedFunction instance would have an attribute holding identifiers of VNF instances.



Figure 6.2.1-2: Transport EP NRM fragment relationship

Figure 6.2.1-3: containment relationship for network slice fragment




Figure 6.2.1-x: Tenant NRM fragment relationship

### 6.2.2 Inheritance



Figure 6.2.2-1: Network slice inheritance relationship




Figure 6.2.2-x: Tenant inheritance relationship

|  |
| --- |
| **3rd Change** |

### 6.3.x Tenant

#### 6.3.x.1 Definition

This IOC represents the information of a tenant, related management capability and information related to a particular communication service consumer (e.g. an enterprise user) in 3GPP management system. The tenant IOC in 3GPP management system allows management capability exposure governance to governance management services to a tenant. For more information on the management capability exposure governance, see 3GPP TS 28.533 [xx].

#### 6.3.x.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| tenantId | M | T | F | F | F |
| administrativeState | M | T | F | F | F |
| sNSSAIList | M | T | F | F | F |
| serviceProfileInfoList | M | T | F | F | F |
| ManagementServiceExposedList | M | T | F | F | F |

#### 6.3.x.3 Notifications

The common notifications defined in subclause 6.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **4th Change** |

### 6.3.y serviceProfileInfo <<dataType>>

#### 6.3.y.1 Definition

This <<data type>> represents the service profile information assosiated to network slice for the tenant supported by the tenant IOC in clause 6.3.x.

#### 6.3.y.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| networkSliceRef | M | T | F | F | T |
| serviceProfileId | M | T | F | F | F |

#### 6.3.y.3 Attribute constraints

None.

#### 6.3.y.4 Notifications

The clause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

## 6.4 Attribute definitions

### 6.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| availability | This parameter specifies the communication service availability requirement, expressed as a percentage. The communication service availability is defined in clause 3.1 of TS 22.261 [28]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: True |
| serviceProfileId | A unique identifier of property of network slice related requirement should be supported by the network slice. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| sliceProfileId | A unique identifier of the property of network slice subnet related requirement should be supported by the network slice subnet. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| operationalState | It indicates the operational state of the network slice or the network slice subnet. It describes whether or not the resource is physically installed and working.  allowedValues: "ENABLED", "DISABLED".  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| administrativeState | It indicates the administrative state of the network slice or the network slice subnet. It describes the permission to use or prohibition against using the managed object instance, imposed through the OAM services.  allowedValues: “LOCKED”, “UNLOCKED”, SHUTTINGDOWN”  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: LOCKED  allowedValues: N/A  isNullable: False |
| nsInfo | This attribute contains the NsInfo of the NS instance corresponding to the network slice subnet instance. The NsInfo is described in clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: NsInfo  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: No default value  isNullable: True |
| nSInstanceId | This attribute specifies the identifier of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: No default value  isNullable: True |
| nsName | This attribute specifies the name of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: No default value  isNullable: True |
| description | This attribute specifies the description of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: No default value  isNullable: True |
| category | This attribute specifies the category of a service requirement/attribute of GST (see GSMA NG.116 [50]).  allowedValues: character, scalability | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| tagging | This attribute specifies the tagging of a service requirement/attribute of GST in character category (see GSMA NG.116 [50]).  allowedValues: performance, function, operation | type: ENUM  multiplicity: 1…3  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| exposure | This attribute specifies exposure mode of a service requirement/attribute of GST (see GSMA NG.116 [50]).  allowedValues: API, KPI | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sNSSAIList | This parameter specifies the S-NSSAI list to be supported by the network slice new to be created or the existing network slice to be re-used.  sNSSAList is defined in subclause 4.4.1 |  |
| maxNumberofUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice or network slice subnet instance. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| coverageAreaTAList | An attribute specifies a list of Tracking Areas for the network slice .  allowedValues:  Legacy TAC and Extended TAC are defined in clause 9.3.3.10 of TS 38.413 [5]. | type: Integer  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| latency | An attribute specifies the packet transmission latency (millisecond) through the RAN, CN, and TN part of 5G network and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| topSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| CNSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through CN domain of the network slice and is used to evaluate the delay in CN domain, e.g. time between received UL/DL packet on N3/N6 interface of UPF and successfully sent out the packet on N6/N3 interface. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| RANSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through RAN domain of the network slice and is used to evaluate the delay in RAN domain, e.g. time between received UL/DL packet on air interface/NgU of gNB and successfully sent out the packet on NgU/air interface of the gNB. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uEMobilityLevel | An attribute specifies the mobility level of UE accessing the network slice. See 6.2.1 of TS 22.261 [28].  allowedValues: stationary, nomadic, restricted mobility, fully mobility. | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: True |
| serviceProfilenetworkSlice.SharingIndicator | The attribute specifies whether a service, defined by the ServiceProfile, can share a NetworkSlice instance with other services or not. If “non-shared” the service needs a dedicated NetworkSlice instance. If “shared” the service may share a NetworkSlice instance with other service(s).  allowedValues: shared, non-shared. | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| serviceProfile.pLMNInfoList | It defines which PLMN and S-NSSAI combinations that are assigned for the service to satisfy service requirements represented by the ServiceProfile in case of network slicing feature is supported.  allowedValues: Not applicable. | type: PLMNInfo  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| sliceProfile.pLMNInfoList | It defines which PLMN and S-NSSAI combinations that are served by the SliceProfile in case of network slicing feature is supported.  allowedValues: Not applicable. | type: PLMNInfo  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| sliceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice subnet may be shared with another network slice subnet(s).  allowedValues: shared, non-shared. | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: Yes  isNullable: True |
| serviceProfileList | An attribute specifies a list of ServiceProfile (see clause 6.3.3) supported by the network slice | type: ServiceProfile  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sliceProfileList | An attribute specifies a list of SliceProfile (see clause 6.3.4) supported by the network slice subnet | type: SliceProfile  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sST | This parameter specifies the slice/service type in a ServiceProfile to be supported by a network slice.  See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| delayTolerance | An attribute specifies the properties of service delivery flexibility, especially for the vertical services that are not chasing a high system performance. See clause 4.3 of TS 22.104 [51]. | type: DelayTolerance  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DelayTolerance.support | An attribute specifies whether or not the network slice supports service delivery flexibility, especially for the vertical services that are not chasing a high system performance.  allowedValues:  "NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| deterministicComm | An attribute specifies the properties of the deterministic communication for periodic user traffic, see clause 4.3 of TS 22.104 [51]. | type: DeterministicComm  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DeterministicComm.availability | An attribute specifies whether or not the network slice supports deterministic communication for period user traffic.  allowedValues:  "NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DeterministicComm.periodicityList | An attribute specifies a list of periodicities supported by the network slice for deterministic communication. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| dLThptPerSlice | This attribute defines achievable data rate of the network slice in downlink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in downlink that is available ubiquitously across the coverage area of the slice. | type: XDLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| guaThpt | This attribute describes the guaranteed data rate. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| maxThpt | This attribute describes the maximum data rate. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| uLThptPerSlice | This attribute defines achievable data rate of the network slice in uplink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in uplink that is available ubiquitously across the coverage area of the slice. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxPktSize | This parameter specifies the maximum packet size supported by the network slice or the network slice subnet, refer NG.116 [50]. | type: MaxPktSize  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxPktSize.maxsize | This parameter specifies the maximum packet size supported by the network slice, refer NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxNumberofPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice, refer NG.116 [50]. | type: MaxNumberofPDUSessions  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxNumberofPDUSessions.nOofPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice, refer NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| kPIMonitoring | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: KPIMonitoring  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| KPIMonitoring. kPIList | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| nBIoT | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50]. | type: NBIoT  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NBIoT.support | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50].  allowedValues:  "NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| synchronicity | An attribute specifies whether synchronicity of communication devices is supported, Two cases are most important in this context, see clause 3.4.29 of NG.116 [50]:  - Synchronicity between a base station and a mobile device and  - Synchronicity between mobile devices. | type: Synchronicity  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Synchronicity.availability | An attribute specifies whether synchronicity of communication devices is supported, see NG.116 [50].  allowedValues:  "NOT SUPPORTED", "BETWEEN BS AND UE", "BETWEEN BS AND UE & UE AND UE". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Synchronicity.accuracy | An attribute specifies the accuracy of the synchronicity, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.synchronicity | An attribute specifies whether synchronicity of communication devices is supported in the RAN domain, Two cases are most important in this context, see clause 3.4.29 of NG.116 [50]:  - Synchronicity between a base station and a mobile device and  - Synchronicity between mobile devices. | type: SynchronicityRANSubnet  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| SynchronicityRANSubnet.availability | An attribute specifies whether synchronicity of communication devices is supported in the RAN domain, see NG.116 [50].  allowedValues:  "NOT SUPPORTED", "BETWEEN BS AND UE", "BETWEEN BS AND UE & UE AND UE". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| SynchronicityRANSubnet.accuracy | An attribute specifies the accuracy of the synchronicity in the RAN domain, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| userMgmtOpen | An attribute specifies whether or not the network slice supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements. | type: UserMgmtOpen  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| UserMgmtOpen.support | An attribute specifies whether or not the network slice supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements.  allowedValues:  "NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| v2XCommModels | An attribute specifies whether or not the V2X communication mode is supported by the network slice. | type: V2XCommMode  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| V2XCommMode.v2XMode | An attribute specifies whether or not the V2X communication mode is supported by the network slice.  allowedValues:  "NOT SUPPORTED", "SUPPORTED BY NR". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| coverageArea | An attribute specifies the coverage area of the network slice, i.e. the geographic region where a 3GPP communication service is accessible, see Table 7.1-1 of TS 22.261 [28]) and NG.116 [50]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| termDensity | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: TermDensity  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| TermDensity.density | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| positioning | An attribute specifies whether the network slice provides geo-localization methods or supporting methods, see clause 3.4.20 of NG.116 [50]. | type: Positioning  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Positioning.availability | An attribute specifies if this attribute is provided by the network slice and contains a list of positioning methods provided by the slice. If the list is empty this attribute is not available in the network slice and the other parameters might be ignored, see NG.116 [50]. Comma separated multiple values are allowed:  CIDE-CID (LTE and NR), OTDOA (LTE and NR), RF fingerprinting, AECID, Hybrid positioning, NET-RTK. | type: ENUM  multiplicity: 1..6  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Positioning.predictionfrequency | An attribute specifies how often location information is provided. This parameter simply defines how often the customer is allowed to request location information. This is not related to the time it takes to determine the location, which is a characteristic of the positioning method, see NG.116 [50].  allowedValues:  "PERSEC", "PERMIN", "PERHOUR". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Positioning.accuracy | An attribute specifies the accuracy of the location information. Accuracy depends on the respective positioning solution applied in the network slice, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.positioning | An attribute specifies whether the RAN domain of the network slice provides geo-localization methods or supporting methods, see clause 3.4.20 of NG.116 [50]. | type: PositioningRANSubnet  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| PositioningRANSubnet.availability | An attribute specifies if this attribute is provided by the RAN domain of the network slice and contains a list of positioning methods provided by the RAN domain. If the list is empty this attribute is not available in the RAN domain and the other parameters might be ignored, see NG.116 [50]. Comma separated multiple values are allowed:  CIDE-CID (LTE and NR), OTDOA (LTE and NR), RF fingerprinting, AECID, Hybrid positioning, NET-RTK. | type: ENUM  multiplicity: 1..6  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| PositioningRANSubnet.predictionfrequency | An attribute specifies how often location information is provided. This parameter simply defines how often the customer is allowed to request location information. This is not related to the time it takes to determine the location, which is a characteristic of the positioning method, see NG.116 [50].  allowedValues:  "PERSEC", "PERMIN", "PERHOUR". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| PositioningRANSubnet.accuracy | An attribute specifies the accuracy of the location information. Accuracy depends on the respective positioning solution applied in the RAN domain of the network slice, measurement unit is meter, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| activityFactor | An attribute specifies the percentage value of the amount of simultaneous active UEs to the total number of UEs where active means the UEs are exchanging data with the network. See Table 7.1-1 of TS 22.261 [28]). | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| uESpeed | An attribute specifies the maximum speed (in km/hour) supported by the network slice or network slice subnet at which a defined QoS can be achieved. See Table 7.1-1 of TS 22.261 [28]). | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| jitter | An attribute specifies the deviation from the desired value to the actual value when assessing time parameters, see clause C.4.1 of TS 22.104 [51]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| survivalTime | An attribute specifies the time that an application consuming a communication service may continue without an anticipated message. See clause 5 of TS 22.104 [51]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| reliability | An attribute specifies in the context of network layer packet transmissions, percentage value of the amount of sent network layer packets successfully delivered to a given system entity within the time constraint required by the targeted service, divided by the total number of sent network layer packets, see TS 22.261 [28] and TS 22.104 [51]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| NetworkSlice.networkSliceSubnetRef | This holds a DN of NetworkSliceSubnet relating to the NetworkSlice instance. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnet.networkSliceSubnetRef | This holds a list of DN of constituent NetworkSliceSubnet supporting NetworkSliceSubnet instance | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| managedFunctionRef | This holds a list of DN of ManagedFunction instances supporting the NetworkSliceSubnet instance. | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| ipAddress | This parameter specifies the IP address assigned to a logical transport interface/endpoint.  It can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).  See note 1 | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| logicInterfaceId | This parameter specifies the identify of a logical transport interface. It could be VLAN ID (See IEEE 802.1Q [39]), MPLS Tag or Segment ID. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nextHopInfoList | This parameter is used to identify ingress transport node. Each node can be identified by any of combination of IP address of next-hop router of transport network, system name, port name, IP management address of transport nodes. | type: String  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| qosProfileRefList | This parameter specifies reference to QoS Profile for a logical transport interface. A QoS profile includes a set of parameters which are locally provisioned on both sides of a logical transport interface. | type: String  multiplicity: \*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: True |
| maxDLDataVolume | An attribute specifies the maximum DL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxULDataVolume | An attribute specifies the maximum UL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| serviceType | An attribute specifies the standardized network slice type.  allowedValues: eMBB, URLLC, MIoT, V2X. | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: True |
| epApplicationRef | This parameter specifies a list of application level EPs (i.e. EP\_N3 or EP\_NgU) associated with the logical transport interface. | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| epTransportRef | This parameter specifies a list of transport level EPs associated with the application level EP (i.e. EP\_N3 or EP\_NgU) or network slice subnet. | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: True |
| sliceSimultaneousUse | This attribute describes whether a network slice can be simultaneously used by a device together with other network slices and if so, with which other classes of network slices.  allowedValues: “0”, “1”, “2”, “3”, “4”.  “0”: Can be used with any network slice  “1”: Can be used with network slices with same SST value  “2”: Can be used with any network slice with same SD value  “3”: Cannot be used with another network slice  “4”: Cannot be used by a UE in a specific location | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| energyEfficiency | An attribute which describes the energy efficiency, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: EnergyEfficiency  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| EnergyEfficiency.performance | Depending on the sST value, EnergyEfficiency.performance will be  - eMBBEEPerfReq  or  - uRLLCEEPerfReq  or  - mIoTEEPerfReq  allowedValues:  - eMBBEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule, where performance can take the following forms:  - number of bits (Integer) (see TS 28.554 [27] clause 6.7.2.2).  - uRLLCEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule, where performance can take the following forms:  - latency in 0.1ms (Integer) (see TS 28.554 [27] clause 6.7.2.3).  - mIoTEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule, where performance can take the following forms:  - maximum number of registered subscribers (Integer) (see TS 28.554 [27] clause 6.7.2.4.1),  - mean number of active UEs (Integer) (see TS 28.554 [27] clause 6.7.2.4.2).  See NOTE 3. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| topSliceSubnetProfile.energyEfficiency | An attribute which describes the energy efficiency through all domains of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| CNSliceSubnetProfile. energyEfficiency | An attribute which describes the energy efficiency through CN domain of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| RANSliceSubnetProfile. energyEfficiency | An attribute which describes the energy efficiency through RAN domain of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| Tenant.tenantId | It is identifier which is allocated by network operator to identify a tenant. | type: string  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| Tenant.administrativeState | It indicates the administrative state of the network slice or the network slice subnet offered to the tenant. It describes the permission to use or prohibition against using the managed object instance, imposed through the OAM services.  allowedValues: “LOCKED”, “UNLOCKED”, SHUTTINGDOWN”  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: LOCKED  allowedValues: N/A  isNullable: False |
| Tenant.ManagementServiceExposedList | The managementServiceExposed indicates the management services exposed to the tenant (identified by tenantId). The precise semantics of this attribute is not specified in the present document. | type: string  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| Tenant.sNSSAIList | This parameter specifies the S-NSSAI list associated to the network slice(s) offered to the tenant by network slice provider. | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| Tenant.serviceProfileId | A unique identifier of property of network slice related requirement should be supported by the network slice associated to the tenant. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| Tenant.networkSliceRef | This parameter specifies the network slice(s) offered to the tenant by network slice provider. | type: DN  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| NOTE 1: There is no direct relationship between localAddress/remoteAddress in EP\_RP and ipAddress in EP\_transport. While the localAddress/remoteAddress in EP\_RP could be exchanged as part of signalling between GTP-u tunnel end points, ipAddress in EP\_transport is used for transport routing.  NOTE 2: void  NOTE 3: energy efficiency requirement for V2X is not part of the current document. | | |

|  |
| --- |
| **5th Change** |

## J.4.3 OpenAPI document "sliceNrm.yaml"

openapi: 3.0.1

info:

title: Slice NRM

version: 17.3.0

description: >-

OAS 3.0.1 specification of the Slice NRM

@ 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541; 5G NRM, Slice NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#------------ Type definitions ---------------------------------------------------

Float:

type: number

format: float

MobilityLevel:

type: string

enum:

- STATIONARY

- NOMADIC

- RESTRICTED MOBILITY

- FULLY MOBILITY

SynAvailability:

type: string

enum:

- NOT SUPPORTED

- BETWEEN BS AND UE

- BETWEEN BS AND UE & UE AND UE

PositioningAvailability:

type: array

items:

type: string

enum:

- CIDE-CID

- OTDOA

- RF FINGERPRINTING

- AECID

- HYBRID POSITIONING

- NET-RTK

Predictionfrequency:

type: string

enum:

- PERSEC

- PERMIN

- PERHOUR

SharingLevel:

type: string

enum:

- SHARED

- NON-SHARED

NetworkSliceSharingIndicator:

type: string

enum:

- SHARED

- NON-SHARED

ServiceType:

type: string

enum:

- eMBB

- RLLC

- MIoT

- V2X

SliceSimultaneousUse:

type: string

enum:

- ZERO

- ONE

- TWO

- THREE

- FOUR

Category:

type: string

enum:

- CHARACTER

- SCALABILITY

Tagging:

type: array

items:

type: string

enum:

- PERFORMANCE

- FUNCTION

- OPERATION

Exposure:

type: string

enum:

- API

- KPI

ServAttrCom:

type: object

properties:

category:

$ref: '#/components/schemas/Category'

tagging:

$ref: '#/components/schemas/Tagging'

exposure:

$ref: '#/components/schemas/Exposure'

Support:

type: string

enum:

- NOT SUPPORTED

- SUPPORTED

DelayTolerance:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

DeterministicComm:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/Support'

periodicityList:

type: string

XLThpt:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

MaxPktSize:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

maxsize:

type: integer

MaxNumberofPDUSessions:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

nOofPDUSessions:

type: integer

KPIMonitoring:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

kPIList:

type: string

NBIoT:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

Synchronicity:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/SynAvailability'

accuracy:

$ref: '#/components/schemas/Float'

SynchronicityRANSubnet:

type: object

properties:

availability:

$ref: '#/components/schemas/SynAvailability'

accuracy:

$ref: '#/components/schemas/Float'

Positioning:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/PositioningAvailability'

predictionfrequency:

$ref: '#/components/schemas/Predictionfrequency'

accuracy:

$ref: '#/components/schemas/Float'

PositioningRANSubnet:

type: object

properties:

availability:

$ref: '#/components/schemas/PositioningAvailability'

predictionfrequency:

$ref: '#/components/schemas/Predictionfrequency'

accuracy:

$ref: '#/components/schemas/Float'

UserMgmtOpen:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

V2XCommModels:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

v2XMode:

$ref: '#/components/schemas/Support'

TermDensity:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

density:

type: integer

NsInfo:

type: object

properties:

nsInstanceId:

type: string

nsName:

type: string

EmbbEEPerfReq:

type: integer

UrllcEEPerfReq:

type: integer

MIoTEEPerfReq:

type: object

properties:

KpiType:

type: string

enum:

- MAXREGSUBS

- MEANACTIVEUES

Req:

type: integer

EEPerfReq:

oneOf:

- $ref: '#/components/schemas/EmbbEEPerfReq'

- $ref: '#/components/schemas/UrllcEEPerfReq'

- $ref: '#/components/schemas/MIoTEEPerfReq'

EnergyEfficiency:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

performance:

$ref: '#/components/schemas/EEPerfReq'

CNSliceSubnetProfile:

type: object

properties:

maxNumberofUEs:

type: integer

latency:

type: integer

dLThptPerSliceSubnet:

$ref: '#/components/schemas/XLThpt'

dLThptPerUE:

$ref: '#/components/schemas/XLThpt'

uLThptPerSliceSubnet:

$ref: '#/components/schemas/XLThpt'

uLThptPerUE:

$ref: '#/components/schemas/XLThpt'

maxNumberOfPDUSessions:

type: integer

coverageAreaTAList:

type: integer

resourceSharingLevel:

$ref: '#/components/schemas/SharingLevel'

maxPktSize:

type: integer

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

synchronicity:

$ref: '#/components/schemas/SynchronicityRANSubnet'

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

reliability:

type: string

energyEfficiency:

type: integer

deterministicComm:

$ref: '#/components/schemas/DeterministicComm'

RANSliceSubnetProfile:

type: object

properties:

coverageAreaTAList:

type: integer

uEMobilityLevel:

$ref: '#/components/schemas/MobilityLevel'

resourceSharingLevel:

$ref: '#/components/schemas/SharingLevel'

maxNumberofUEs:

type: integer

activityFactor:

type: integer

dLThptPerUE:

$ref: '#/components/schemas/XLThpt'

uLThptPerUE:

$ref: '#/components/schemas/XLThpt'

uESpeed:

type: integer

reliability:

type: string

serviceType:

$ref: '#/components/schemas/ServiceType'

maxPktSize:

type: integer

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

positioning:

$ref: '#/components/schemas/PositioningRANSubnet'

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

energyEfficiency:

type: integer

termDensity:

$ref: '#/components/schemas/TermDensity'

survivalTime:

type: string

synchronicity:

$ref: '#/components/schemas/SynchronicityRANSubnet'

deterministicComm:

$ref: '#/components/schemas/DeterministicComm'

TopSliceSubnetProfile:

type: object

properties:

coverageArea:

type: string

latency:

type: integer

maxNumberofUEs:

type: integer

dLThptPerSliceSubnet:

$ref: '#/components/schemas/XLThpt'

dLThptPerUE:

$ref: '#/components/schemas/XLThpt'

uLThptPerSliceSubnet:

$ref: '#/components/schemas/XLThpt'

uLThptPerUE:

$ref: '#/components/schemas/XLThpt'

maxPktSize:

type: integer

maxNumberOfPDUSessions:

type: integer

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

energyEfficiency:

type: integer

synchronicity:

$ref: '#/components/schemas/Synchronicity'

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

positioning:

$ref: '#/components/schemas/Positioning'

termDensity:

$ref: '#/components/schemas/TermDensity'

activityFactor:

type: integer

coverageAreaTAList:

type: integer

resourceSharingLevel:

$ref: '#/components/schemas/SharingLevel'

uEMobilityLevel:

$ref: '#/components/schemas/MobilityLevel'

uESpeed:

type: integer

reliability:

type: string

serviceType:

$ref: '#/components/schemas/ServiceType'

deterministicComm:

$ref: '#/components/schemas/DeterministicComm'

survivalTime:

type: string

ServiceProfile:

type: object

properties:

serviceProfileId:

type: string

plmnInfoList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnInfoList'

maxNumberofUEs:

type: number

latency:

type: number

uEMobilityLevel:

$ref: '#/components/schemas/MobilityLevel'

sst:

$ref: 'nrNrm.yaml#/components/schemas/Sst'

networkSliceSharingIndicator:

$ref: '#/components/schemas/NetworkSliceSharingIndicator'

availability:

type: number

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

deterministicComm:

$ref: '#/components/schemas/DeterministicComm'

dLThptPerSlice:

$ref: '#/components/schemas/XLThpt'

dLThptPerUE:

$ref: '#/components/schemas/XLThpt'

uLThptPerSlice:

$ref: '#/components/schemas/XLThpt'

uLThptPerUE:

$ref: '#/components/schemas/XLThpt'

maxPktSize:

$ref: '#/components/schemas/MaxPktSize'

maxNumberofPDUSessions:

$ref: '#/components/schemas/MaxNumberofPDUSessions'

kPIMonitoring:

$ref: '#/components/schemas/KPIMonitoring'

nBIoT:

$ref: '#/components/schemas/NBIoT'

synchronicity:

$ref: '#/components/schemas/Synchronicity'

positioning:

$ref: '#/components/schemas/Positioning'

userMgmtOpen:

$ref: '#/components/schemas/UserMgmtOpen'

v2XModels:

$ref: '#/components/schemas/V2XCommModels'

coverageArea:

type: string

termDensity:

$ref: '#/components/schemas/TermDensity'

activityFactor:

$ref: '#/components/schemas/Float'

uESpeed:

type: integer

jitter:

type: integer

survivalTime:

type: string

reliability:

type: string

maxDLDataVolume:

type: string

maxULDataVolume:

type: string

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

energyEfficiency:

$ref: '#/components/schemas/EnergyEfficiency'

SliceProfile:

type: object

properties:

serviceProfileId:

type: string

plmnInfoList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnInfoList'

cNSliceSubnetProfile:

$ref: '#/components/schemas/CNSliceSubnetProfile'

rANSliceSubnetProfile:

$ref: '#/components/schemas/RANSliceSubnetProfile'

topSliceSubnetProfile:

$ref: '#/components/schemas/TopSliceSubnetProfile'

IpAddress:

oneOf:

- $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

- $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

ServiceProfileList:

type: array

items:

$ref: '#/components/schemas/ServiceProfile'

SliceProfileList:

type: array

items:

$ref: '#/components/schemas/SliceProfile'

ManagementServiceExposedList:

type: array

items:

$ref: '#/components/schemas/ManagementServiceExposured'

ManagementServiceExposed:

type: string

#------------ Definition of concrete IOCs ----------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

SubNetwork:

$ref: '#/components/schemas/SubNetwork-Multiple'

NetworkSlice:

$ref: '#/components/schemas/NetworkSlice-Multiple'

NetworkSliceSubnet:

$ref: '#/components/schemas/NetworkSliceSubnet-Multiple'

EP\_Transport:

$ref: '#/components/schemas/EP\_Transport-Multiple'

tenant:

$ref: '#/components/schemas/tenant-Multiple'

NetworkSlice-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

networkSliceSubnetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

operationalState:

$ref: 'genericNrm.yaml#/components/schemas/OperationalState'

administrativeState:

$ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

serviceProfileList:

$ref: '#/components/schemas/ServiceProfileList'

NetworkSliceSubnet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

managedFunctionRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

networkSliceSubnetRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

operationalState:

$ref: 'genericNrm.yaml#/components/schemas/OperationalState'

administrativeState:

$ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

nsInfo:

$ref: '#/components/schemas/NsInfo'

sliceProfileList:

$ref: '#/components/schemas/SliceProfileList'

epTransportRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

EP\_Transport-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

ipAddress:

$ref: '#/components/schemas/IpAddress'

logicInterfaceId:

type: string

nextHopInfo:

type: string

qosProfile:

type: string

epApplicationRefs:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

tenant-Single:

allOf:

- $ref: genericNrm.yaml#/components/schemas/Top

- type: object

properties:

attributes:

type: object

properties:

tenantId:

type: string

administrativeState:

$ref: genericNrm.yaml#/components/schemas/AdministrativeState

snssaiList:

$ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

ManagementServiceExposedList:

type: string

serviceProfileInfo:

type: object

properties:

serviceProfileID:

type: string

networkSliceRef:

$ref: genericNrm.yaml#/components/schemas/DnList

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

SubNetwork-Multiple:

type: array

items:

$ref: '#/components/schemas/SubNetwork-Single'

NetworkSlice-Multiple:

type: array

items:

$ref: '#/components/schemas/NetworkSlice-Single'

NetworkSliceSubnet-Multiple:

type: array

items:

$ref: '#/components/schemas/NetworkSliceSubnet-Single'

EP\_Transport-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Transport-Single'

tenant-Multiple:

type: array

items:

$ref: '#/components/schemas/tenant-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

resources-sliceNrm:

oneOf:

- $ref: '#/components/schemas/SubNetwork-Single'

- $ref: '#/components/schemas/NetworkSlice-Single'

- $ref: '#/components/schemas/NetworkSliceSubnet-Single'

- $ref: '#/components/schemas/EP\_Transport-Single'

- $ref: '#/components/schemas/tenant-Single'

|  |
| --- |
| **6th Change** |

# Annex X: Information model definition for Tenant(informative)

## X.1 Relationship UML diagram for Tenant(Figure 6.2.1-x)

@startuml

hide circle

hide methods

hide members

skinparam class {

AttributeIconSize 0

BackgroundColor white

BorderColor black

ArrowColor black

}

skinparam Shadowing false

skinparam Monochrome true

skinparam ClassBackgroundColor White

class “<<InformationObjectClass>> \n SubNetwork ” as SubNetwork{}

class “<<InformationObjectClass>>\n Tenant ” as Tenant {}

class “<<InformationObjectClass>>\n NetworkSlice” as NetworkSlice{}

SubNetwork "1" \*-- "\*" Tenant

Tenant "\*"--> "\*" NetworkSlice

@enduml

## X.2 Inheritance relationship UML diagram for Tenant(Figure 6.2.2-x)

@startuml

hide circle

hide methods

hide members

skinparam class {

AttributeIconSize 0

BackgroundColor white

BorderColor black

ArrowColor black

}

skinparam Shadowing false

skinparam Monochrome true

skinparam ClassBackgroundColor White

class “<<InformationObjectClass>> \n Top ” as Top{}

class “<<InformationObjectClass>>\n Tenant ” as Tenant {}

Top <|-- Tenant

@enduml

|  |
| --- |
| **End of Change** |