**3GPP TSG SA WG5 Meeting #141e S5-221565**

**Online, , 17 Jan 2021- 26 Jan 2021**

**Source: Samsung**

**Title: pCR 28.538 Edge NRM Stage-3**

**Document for: Approval**

**Agenda Item: 6.4.18**

# 1 Decision/action requested

***The group is asked to discuss and approve the proposals.***

# 2 References

None

# 3 Rationale

This contribution provides stage 3 for edge NRM.

# 4 Detailed proposal

|  |
| --- |
| **First modification** |

# P.1 General

This annex contains the OpenAPI definition of the Edge NRM in YAML format.

The Information Service (IS) of the Edge NRM is defined in clause 6.

Mapping rules to produce the OpenAPI definition based on the IS are defined in TS 32.160 [10].

# P.2 Solution Set (SS) definitions

## P.2.1 OpenAPI document "edgeNrm.yml"

openapi: 3.0.1

info:

title: 3GPP Edge NRM

version: 17.1.0

description: >-

OAS 3.0.1 specification of the Edge NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.538; Edge NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.538/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

EASRequirements:

type: object

properties:

requiredEASservingLocation:

$ref: '#/components/schemas/ServingLocation'

ServingLocation:

type: object

properties:

geographicalLocation:

$ref: '#/components/schemas/GeoLoc'

tAi:

$ref: 'genericNrm.yaml#/components/schemas/TAI '

GeoLoc:

type: object

properties:

civicAddress:

Type: String

lat:

type: float

long:

type: float

EDNConnectionInfo:

type: object

properties:

dNN:

Type: String

eDNServiceArea:

$ref: '#/components/schemas/ServingLocation'

#-------- Definition of concrete IOCs --------------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

DNFunction:

$ref: '5GCNrm.yaml#/components/schemas/DNFunction'

EASFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

eASIdentifier:

Type: string

eASRequirements:

$ref: '#/components/schemas/EASRequirements'

ECSFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

eCSAddress:

Type: string

providerIdentifier:

Type: string

eDNConnectionInfo:

$ref: '#/components/schemas/EASRequirements'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

EASFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/EASFunction-Single'

ECSFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ECSFunction-Single'