**3GPP TSG-SA5 Meeting #141-e *S5-221566***

**e-meeting, 17 -26 January 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **0679** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correct NR YAML in TS document | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | S5 | | | | | | | | | |
| ***Source to TSG:*** | Huawei | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | adNRM | | | | |  | ***Date:*** | | | 2022-01-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The yaml definition for several attributes (including IPv4address, IPv6address, DN, DNlist,administrativeState,operationalState) are moved to comDefs.yaml from genericNrm.yaml. However, in NrNRM.yaml, these attributes still refers to the genericNrm.yaml. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Update the reference of above attributes to comDefs.yaml | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | In Correct references for above attributes. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | D.4.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge link: <https://forge.3gpp.org/rep/sa5/MnS/-/tree/code_moderator_testing_branch_rel17_init> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **1st Change** |

## D.4.3 OpenAPI document "nrNrm.yaml"

openapi: 3.0.1

info:

title: NR NRM

version: 17.4.0

description: >-

OAS 3.0.1 specification of the NR NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541; 5G NRM, NR NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

GnbId:

type: string

GnbIdLength:

type: integer

minimum: 22

maximum: 32

GnbName:

type: string

maxLength: 150

GnbDuId:

type: number

minimum: 0

maximum: 68719476735

GnbCuUpId:

type: number

minimum: 0

maximum: 68719476735

Sst:

type: integer

maximum: 255

Snssai:

type: object

properties:

sst:

$ref: '#/components/schemas/Sst'

sd:

type: string

SnssaiList:

type: array

items:

$ref: '#/components/schemas/Snssai'

Mnc:

type: string

pattern: '[0-9]{3}|[0-9]{2}'

PlmnId:

type: object

properties:

mcc:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

mnc:

$ref: '#/components/schemas/Mnc'

PlmnIdList:

type: array

items:

$ref: '#/components/schemas/PlmnId'

PlmnInfo:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

PlmnInfoList:

type: array

items:

$ref: '#/components/schemas/PlmnInfo'

SnpnId:

type: object

properties:

mcc:

$ref: 'genericNrm.yaml#/components/schemas/Mcc'

mnc:

$ref: '#/components/schemas/Mnc'

nid:

type: string

SnpnInfo:

type: object

properties:

snpnId:

$ref: '#/components/schemas/SnpnId'

snssai:

$ref: '#/components/schemas/Snssai'

cagId:

type: string

nid:

type: string

NpnIdentity:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

cagidList:

$ref: '#/components/schemas/cagId'

nidList:

$ref: '#/components/schemas/nid'

NpnIdentityList:

type: array

items:

$ref: '#/components/schemas/NpnIdentity'

GGnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(22|23|24|25|26|27|28|29|30|31|32)-[0-9]{1,10}'

GEnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(18|20|21|22)-[0-9]{1,7}'

GGnbIdList:

type: array

items:

$ref: '#/components/schemas/GGnbId'

GEnbIdList:

type: array

items:

$ref: '#/components/schemas/GEnbId'

NrPci:

type: integer

maximum: 503

NrTac:

type: integer

maximum: 16777215

Tai:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

nrTac:

$ref: '#/components/schemas/NrTac'

NrtacRange:

type: object

properties:

nRTACstart:

type: string

nRTACend:

type: string

nRTACpattern:

type: string

TaiRange:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

nRTACRangeList:

type: array

items:

$ref: '#/components/schemas/NrtacRange'

TaiList:

type: array

items:

$ref: '#/components/schemas/Tai'

BackhaulAddress:

type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

tai:

$ref: "#/components/schemas/Tai"

MappingSetIDBackhaulAddress:

type: object

properties:

setID:

type: integer

backhaulAddress:

$ref: '#/components/schemas/BackhaulAddress'

IntraRatEsActivationOriginalCellLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsActivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsDeactivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

EsNotAllowedTimePeriod:

type: object

properties:

startTimeandendTime:

type: string

periodOfDay:

type: string

daysOfWeekList:

type: string

listoftimeperiods:

type: string

InterRatEsActivationOriginalCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsActivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsDeactivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

UeAccProbilityDist:

type: object

properties:

targetProbability:

type: integer

numberofpreamblessent:

type: integer

UeAccDelayProbilityDist:

type: object

properties:

targetProbability:

type: integer

accessdelay:

type: integer

NRPciList:

type: object

properties:

NRPci:

type: integer

CSonPciList:

type: object

properties:

NRPci:

type: integer

MaximumDeviationHoTrigger:

type: integer

minimum: -20

maximum: 20

MinimumTimeBetweenHoTriggerChange:

type: integer

minimum: 0

maximum: 604800

TstoreUEcntxt:

type: integer

minimum: 0

maximum: 1023

CellState:

type: string

enum:

- IDLE

- INACTIVE

- ACTIVE

CyclicPrefix:

type: string

enum:

- '15'

- '30'

- '60'

- '120'

TxDirection:

type: string

enum:

- DL

- UL

- DL and UL

BwpContext:

type: string

enum:

- DL

- UL

- SUL

IsInitialBwp:

type: string

enum:

- INITIAL

- OTHER

- SUL

QuotaType:

type: string

enum:

- STRICT

- FLOAT

IsESCoveredBy:

type: string

enum:

- NO

- PARTIAL

- FULL

RrmPolicyMember:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

RrmPolicyMemberList:

type: array

items:

$ref: '#/components/schemas/RrmPolicyMember'

AddressWithVlan:

type: object

properties:

ipv4Address:

$ref: 'comDefs.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'comDefs.yaml#/components/schemas/Ipv6Addr'

vlanId:

type: integer

minimum: 0

maximum: 4096

LocalAddress:

type: object

properties:

addressWithVlan:

$ref: '#/components/schemas/AddressWithVlan'

port:

type: integer

minimum: 0

maximum: 65535

RemoteAddress:

type: object

properties:

ipv4Address:

$ref: 'comDefs.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'comDefs.yaml#/components/schemas/Ipv6Addr'

CellIndividualOffset:

type: object

properties:

rsrpOffsetSSB:

type: integer

rsrqOffsetSSB:

type: integer

sinrOffsetSSB:

type: integer

rsrpOffsetCSI-RS:

type: integer

rsrqOffsetCSI-RS:

type: integer

sinrOffsetCSI-RS:

type: integer

QOffsetRange:

type: integer

enum:

- -24

- -22

- -20

- -18

- -16

- -14

- -12

- -10

- -8

- -6

- -5

- -4

- -3

- -2

- -1

- 0

- 24

- 22

- 20

- 18

- 16

- 14

- 12

- 10

- 8

- 6

- 5

- 4

- 3

- 2

- 1

QOffsetRangeList:

type: object

properties:

rsrpOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrpOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

QOffsetFreq:

type: number

TReselectionNRSf:

type: integer

enum:

- 25

- 50

- 75

- 100

SsbPeriodicity:

type: integer

enum:

- 5

- 10

- 20

- 40

- 80

- 160

SsbDuration:

type: integer

enum:

- 1

- 2

- 3

- 4

- 5

SsbSubCarrierSpacing:

type: integer

enum:

- 15

- 30

- 120

- 240

CoverageShape:

type: integer

maximum: 65535

DigitalTilt:

type: integer

minimum: -900

maximum: 900

DigitalAzimuth:

type: integer

minimum: -1800

maximum: 1800

RSSetId:

type: integer

maximum: 4194303

RSSetType:

type: string

enum:

- RS1

- RS2

FrequencyDomainPara:

type: object

properties:

rimRSSubcarrierSpacing:

type: integer

rIMRSBandwidth:

type: integer

nrofGlobalRIMRSFrequencyCandidates:

type: integer

rimRSCommonCarrierReferencePoint:

type: integer

rimRSStartingFrequencyOffsetIdList:

type: array

items:

type: integer

SequenceDomainPara:

type: object

properties:

nrofRIMRSSequenceCandidatesofRS1:

type: integer

rimRSScrambleIdListofRS1:

type: array

items:

type: integer

nrofRIMRSSequenceCandidatesofRS2:

type: integer

rimRSScrambleIdListofRS2:

type: array

items:

type: integer

enableEnoughNotEnoughIndication:

type: string

enum:

- ENABLE

- DISABLE

RIMRSScrambleTimerMultiplier:

type: integer

RIMRSScrambleTimerOffset:

type: integer

TimeDomainPara:

type: object

properties:

dlULSwitchingPeriod1:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint1:

type: integer

dlULSwitchingPeriod2:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint2:

type: integer

totalnrofSetIdofRS1:

type: integer

totalnrofSetIdofRS2:

type: integer

nrofConsecutiveRIMRS1:

type: integer

nrofConsecutiveRIMRS2:

type: integer

consecutiveRIMRS1List:

type: array

items:

type: integer

consecutiveRIMRS2List:

type: array

items:

type: integer

enablenearfarIndicationRS1:

type: string

enum:

- ENABLE

- DISABLE

enablenearfarIndicationRS2:

type: string

enum:

- ENABLE

- DISABLE

RimRSReportInfo:

type: object

properties:

detectedSetID:

type: integer

propagationDelay:

type: integer

functionalityOfRIMRS:

type: string

enum:

- RS1

- RS2

- RS1forEnoughMitigation

- RS1forNotEnoughMitigation

RimRSReportConf:

type: object

properties:

reportIndicator:

type: string

enum:

- ENABLE

- DISABLE

reportInterval:

type: integer

nrofRIMRSReportInfo:

type: integer

maxPropagationDelay:

type: integer

rimRSReportInfoList:

type: array

items:

$ref: '#/components/schemas/RimRSReportInfo'

TceMappingInfo:

type: object

properties:

TceIPAddress:

oneOf:

- $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

- $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

TceID:

type: integer

PlmnTarget:

$ref: '#/components/schemas/PlmnId'

TceMappingInfoList:

type: array

items:

$ref: '#/components/schemas/TceMappingInfo'

ResourceType:

type: string

enum:

- PRB

- PRB\_UL

- PRB\_DL

- RRC

- DRB

#-------- Definition of abstract IOCs --------------------------------------------

RrmPolicy\_-Attr:

type: object

properties:

resourceType:

$ref: '#/components/schemas/ResourceType'

rRMPolicyMemberList:

$ref: '#/components/schemas/RrmPolicyMemberList'

#-------- Definition of concrete IOCs --------------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

$ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

SubNetwork:

$ref: '#/components/schemas/SubNetwork-Multiple'

ManagedElement:

$ref: '#/components/schemas/ManagedElement-Multiple'

NRFrequency:

$ref: '#/components/schemas/NRFrequency-Multiple'

ExternalGnbCuCpFunction:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Multiple'

ExternalENBFunction:

$ref: '#/components/schemas/ExternalENBFunction-Multiple'

EUtranFrequency:

$ref: '#/components/schemas/EUtranFrequency-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

RimRSGlobal:

$ref: '#/components/schemas/RimRSGlobal-Single'

Dynamic5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

ManagedElement-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

$ref: 'genericNrm.yaml#/components/schemas/ManagedElement-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-ncO'

- type: object

properties:

GnbDuFunction:

$ref: '#/components/schemas/GnbDuFunction-Multiple'

GnbCuUpFunction:

$ref: '#/components/schemas/GnbCuUpFunction-Multiple'

GnbCuCpFunction:

$ref: '#/components/schemas/GnbCuCpFunction-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: '5gcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

GnbDuFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbDuId:

$ref: '#/components/schemas/GnbDuId'

gnbDuName:

$ref: '#/components/schemas/GnbName'

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

rimRSReportConf:

$ref: '#/components/schemas/RimRSReportConf'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellDu:

$ref: '#/components/schemas/NrCellDu-Multiple'

Bwp-Multiple:

$ref: '#/components/schemas/Bwp-Multiple'

NrSectorCarrier-Multiple:

$ref: '#/components/schemas/NrSectorCarrier-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

OperatorDu-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- type: object

properties:

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

GnbCuUpFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuUpId:

$ref: '#/components/schemas/GnbCuUpId'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

configurable5QISetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_NgU:

$ref: '#/components/schemas/EP\_NgU-Multiple'

EP\_X2U:

$ref: '#/components/schemas/EP\_X2U-Multiple'

EP\_S1U:

$ref: '#/components/schemas/EP\_S1U-Multiple'

GnbCuCpFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuName:

$ref: '#/components/schemas/GnbName'

plmnId:

$ref: '#/components/schemas/PlmnId'

x2BlackList:

$ref: '#/components/schemas/GGnbIdList'

xnBlackList:

$ref: '#/components/schemas/GGnbIdList'

x2WhiteList:

$ref: '#/components/schemas/GGnbIdList'

xnWhiteList:

$ref: '#/components/schemas/GGnbIdList'

x2XnHOBlackList:

$ref: '#/components/schemas/GEnbIdList'

mappingSetIDBackhaulAddress:

$ref: '#/components/schemas/MappingSetIDBackhaulAddress'

tceMappingInfoList:

$ref: '#/components/schemas/TceMappingInfoList'

configurable5QISetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

dDAPSHOControl:

type: boolean

dCHOControl:

type: boolean

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellCu:

$ref: '#/components/schemas/NrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_NgC:

$ref: '#/components/schemas/EP\_NgC-Multiple'

EP\_X2C:

$ref: '#/components/schemas/EP\_X2C-Multiple'

DANRManagementFunction:

$ref: '#/components/schemas/DANRManagementFunction-Single'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

NrCellCu-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nRFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NRCellRelation:

$ref: '#/components/schemas/NRCellRelation-Multiple'

EUtranCellRelation:

$ref: '#/components/schemas/EUtranCellRelation-Multiple'

NRFreqRelation:

$ref: '#/components/schemas/NRFreqRelation-Multiple'

EUtranFreqRelation:

$ref: '#/components/schemas/EUtranFreqRelation-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

NrCellDu-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

administrativeState:

$ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'comDefs.yaml#/components/schemas/OperationalState'

cellLocalId:

type: integer

cellState:

$ref: '#/components/schemas/CellState'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

npnIdentityList:

$ref: '#/components/schemas/NpnIdentityList'

nrPci:

$ref: '#/components/schemas/NrPci'

nrTac:

$ref: '#/components/schemas/NrTac'

arfcnDL:

type: integer

arfcnUL:

type: integer

arfcnSUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

bSChannelBwSUL:

type: integer

ssbFrequency:

type: integer

minimum: 0

maximum: 3279165

ssbPeriodicity:

$ref: '#/components/schemas/SsbPeriodicity'

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

ssbOffset:

type: integer

minimum: 0

maximum: 159

ssbDuration:

$ref: '#/components/schemas/SsbDuration'

nrSectorCarrierRef:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/Dn'

bwpRef:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/Dn'

rimRSMonitoringStartTime:

type: string

rimRSMonitoringStopTime:

type: string

rimRSMonitoringWindowDuration:

type: integer

rimRSMonitoringWindowStartingOffset:

type: integer

rimRSMonitoringWindowPeriodicity:

type: integer

rimRSMonitoringOccasionInterval:

type: integer

rimRSMonitoringOccasionStartingOffset:

type: integer

nRFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

victimSetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

aggressorSetRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

NrOperatorCellDu-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

cellLocalId:

type: integer

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nrTac:

$ref: '#/components/schemas/NrTac'

NRFrequency-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

absoluteFrequencySSB:

type: integer

minimum: 0

maximum: 3279165

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

multiFrequencyBandListNR:

type: integer

minimum: 1

maximum: 256

EUtranFrequency-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

earfcnDL:

type: integer

minimum: 0

maximum: 262143

multiBandInfoListEutra:

type: integer

minimum: 1

maximum: 256

NrSectorCarrier-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

txDirection:

$ref: '#/components/schemas/TxDirection'

configuredMaxTxPower:

type: integer

arfcnDL:

type: integer

arfcnUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

sectorEquipmentFunctionRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

CommonBeamformingFunction:

$ref: '#/components/schemas/CommonBeamformingFunction-Single'

Bwp-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

bwpContext:

$ref: '#/components/schemas/BwpContext'

isInitialBwp:

$ref: '#/components/schemas/IsInitialBwp'

subCarrierSpacing:

type: integer

cyclicPrefix:

$ref: '#/components/schemas/CyclicPrefix'

startRB:

type: integer

numberOfRBs:

type: integer

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

CommonBeamformingFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

coverageShape:

$ref: '#/components/schemas/CoverageShape'

digitalAzimuth:

$ref: '#/components/schemas/DigitalAzimuth'

digitalTilt:

$ref: '#/components/schemas/DigitalTilt'

- type: object

properties:

Beam:

$ref: '#/components/schemas/Beam-Multiple'

Beam-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

beamIndex:

type: integer

beamType:

type: string

enum:

- SSB-BEAM

beamAzimuth:

type: integer

minimum: -1800

maximum: 1800

beamTilt:

type: integer

minimum: -900

maximum: 900

beamHorizWidth:

type: integer

minimum: 0

maximum: 3599

beamVertWidth:

type: integer

minimum: 0

maximum: 1800

RRMPolicyRatio-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: '#/components/schemas/RrmPolicy\_-Attr'

- type: object

properties:

rRMPolicyMaxRatio:

type: integer

rRMPolicyMinRatio:

type: integer

rRMPolicyDedicatedRatio:

type: integer

NRCellRelation-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

nRTCI:

type: integer

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

adjacentNRCellRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

nRFreqRelationRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

isRemoveAllowed:

type: boolean

isHOAllowed:

type: boolean

isESCoveredBy:

$ref: '#/components/schemas/IsESCoveredBy'

isENDCAllowed:

type: boolean

isMLBAllowed:

type: boolean

EUtranCellRelation-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

adjacentEUtranCellRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

NRFreqRelation-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

offsetMO:

$ref: '#/components/schemas/QOffsetRangeList'

blockListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blockListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionNr:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

nRFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

EUtranFreqRelation-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

blackListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blackListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionEutran:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

eUTranFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

DANRManagementFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

intrasystemANRManagementSwitch:

type: boolean

intersystemANRManagementSwitch:

type: boolean

DESManagementFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

desSwitch:

type: boolean

intraRatEsActivationOriginalCellLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

intraRatEsActivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationCandidateCellsLoadParameters"

intraRatEsDeactivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsDeactivationCandidateCellsLoadParameters"

esNotAllowedTimePeriod:

$ref: "#/components/schemas/EsNotAllowedTimePeriod"

interRatEsActivationOriginalCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsActivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsDeactivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

isProbingCapable:

type: string

enum:

- yes

- no

energySavingState:

type: string

enum:

- isNotEnergySaving

- isEnergySaving

DRACHOptimizationFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

drachOptimizationControl:

type: boolean

ueAccProbilityDist:

$ref: "#/components/schemas/UeAccProbilityDist"

ueAccDelayProbilityDist:

$ref: "#/components/schemas/UeAccDelayProbilityDist"

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

DMROFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dmroControl:

type: boolean

maximumDeviationHoTrigger:

$ref: '#/components/schemas/MaximumDeviationHoTrigger'

minimumTimeBetweenHoTriggerChange:

$ref: '#/components/schemas/MinimumTimeBetweenHoTriggerChange'

tstoreUEcntxt:

$ref: '#/components/schemas/TstoreUEcntxt'

DLBOFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dlboControl:

type: boolean

maximumDeviationHoTrigger:

$ref: '#/components/schemas/MaximumDeviationHoTrigger'

minimumTimeBetweenHoTriggerChange:

$ref: '#/components/schemas/MinimumTimeBetweenHoTriggerChange'

DPCIConfigurationFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dPciConfigurationControl:

type: boolean

nRPciList:

$ref: "#/components/schemas/NRPciList"

CPCIConfigurationFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cPciConfigurationControl:

type: boolean

cSonPciList:

$ref: "#/components/schemas/CSonPciList"

CESManagementFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cesSwitch:

type: boolean

intraRatEsActivationOriginalCellLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

intraRatEsActivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationCandidateCellsLoadParameters"

intraRatEsDeactivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsDeactivationCandidateCellsLoadParameters"

esNotAllowedTimePeriod:

$ref: "#/components/schemas/EsNotAllowedTimePeriod"

interRatEsActivationOriginalCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsActivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsDeactivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

energySavingControl:

type: string

enum:

- toBeEnergySaving

- toBeNotEnergySaving

energySavingState:

type: string

enum:

- isNotEnergySaving

- isEnergySaving

RimRSGlobal-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

frequencyDomainPara:

$ref: '#/components/schemas/FrequencyDomainPara'

sequenceDomainPara:

$ref: '#/components/schemas/SequenceDomainPara'

timeDomainPara:

$ref: '#/components/schemas/TimeDomainPara'

RimRSSet:

$ref: '#/components/schemas/RimRSSet-Multiple'

RimRSSet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

setId:

$ref: '#/components/schemas/RSSetId'

setType:

$ref: '#/components/schemas/RSSetType'

nRCellDURefs:

$ref: 'comDefs.yaml#/components/schemas/DnList'

ExternalGnbDuFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

ExternalGnbCuUpFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

ExternalGnbCuCpFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: >-

genericNrm.yaml#/components/schemas/ManagedFunction-Attr

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

plmnId:

$ref: '#/components/schemas/PlmnId'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalNrCellCu:

$ref: '#/components/schemas/ExternalNrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

ExternalNrCellCu-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

nrPci:

$ref: '#/components/schemas/NrPci'

plmnIdList:

$ref: '#/components/schemas/PlmnIdList'

nRFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

ExternalENBFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

eNBId:

type: integer

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalEUTranCell:

$ref: '#/components/schemas/ExternalEUTranCell-Multiple'

ExternalEUTranCell-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

EUtranFrequencyRef:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

EP\_XnC-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_E1-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1C-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_NgC-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_X2C-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_XnU-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1U-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'comDefs.yaml#/components/schemas/DnList'

EP\_NgU-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'comDefs.yaml#/components/schemas/DnList'

EP\_X2U-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_S1U-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

SubNetwork-Multiple:

type: array

items:

$ref: '#/components/schemas/SubNetwork-Single'

ManagedElement-Multiple:

type: array

items:

$ref: '#/components/schemas/ManagedElement-Single'

GnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbDuFunction-Single'

OperatorDu-Multiple:

type: array

items:

$ref: '#/components/schemas/OperatorDu-Single'

GnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuUpFunction-Single'

GnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuCpFunction-Single'

NrCellDu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellDu-Single'

NrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellCu-Single'

NRFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/NRFrequency-Single'

EUtranFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/EUtranFrequency-Single'

NrSectorCarrier-Multiple:

type: array

items:

$ref: '#/components/schemas/NrSectorCarrier-Single'

Bwp-Multiple:

type: array

items:

$ref: '#/components/schemas/Bwp-Single'

Beam-Multiple:

type: array

items:

$ref: '#/components/schemas/Beam-Single'

RRMPolicyRatio-Multiple:

type: array

items:

$ref: '#/components/schemas/RRMPolicyRatio-Single'

NRCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRCellRelation-Single'

EUtranCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranCellRelation-Single'

NRFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRFreqRelation-Single'

EUtranFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranFreqRelation-Single'

RimRSSet-Multiple:

type: array

items:

$ref: '#/components/schemas/RimRSSet-Single'

ExternalGnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbDuFunction-Single'

ExternalGnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

ExternalGnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

ExternalNrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalNrCellCu-Single'

ExternalENBFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalENBFunction-Single'

ExternalEUTranCell-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalEUTranCell-Single'

EP\_E1-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnC-Single'

EP\_F1C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_NgC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgC-Single'

EP\_X2C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2C-Single'

EP\_XnU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnU-Single'

EP\_F1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1U-Single'

EP\_NgU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgU-Single'

EP\_X2U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2U-Single'

EP\_S1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_S1U-Single'

#-------- Definitions in TS 28.541 for TS 28.532 ---------------------------------

resources-nrNrm:

oneOf:

- $ref: '#/components/schemas/SubNetwork-Single'

- $ref: '#/components/schemas/ManagedElement-Single'

- $ref: '#/components/schemas/GnbDuFunction-Single'

- $ref: '#/components/schemas/GnbCuUpFunction-Single'

- $ref: '#/components/schemas/GnbCuCpFunction-Single'

- $ref: '#/components/schemas/OperatorDu-Single'

- $ref: '#/components/schemas/NrCellCu-Single'

- $ref: '#/components/schemas/NrCellDu-Single'

- $ref: '#/components/schemas/NrOperatorCellDu-Single'

- $ref: '#/components/schemas/NRFrequency-Single'

- $ref: '#/components/schemas/EUtranFrequency-Single'

- $ref: '#/components/schemas/NrSectorCarrier-Single'

- $ref: '#/components/schemas/Bwp-Single'

- $ref: '#/components/schemas/CommonBeamformingFunction-Single'

- $ref: '#/components/schemas/Beam-Single'

- $ref: '#/components/schemas/RRMPolicyRatio-Single'

- $ref: '#/components/schemas/NRCellRelation-Single'

- $ref: '#/components/schemas/EUtranCellRelation-Single'

- $ref: '#/components/schemas/NRFreqRelation-Single'

- $ref: '#/components/schemas/EUtranFreqRelation-Single'

- $ref: '#/components/schemas/DANRManagementFunction-Single'

- $ref: '#/components/schemas/DESManagementFunction-Single'

- $ref: '#/components/schemas/DRACHOptimizationFunction-Single'

- $ref: '#/components/schemas/DMROFunction-Single'

- $ref: '#/components/schemas/DLBOFunction-Single'

- $ref: '#/components/schemas/DPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CESManagementFunction-Single'

- $ref: '#/components/schemas/RimRSGlobal-Single'

- $ref: '#/components/schemas/RimRSSet-Single'

- $ref: '#/components/schemas/ExternalGnbDuFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

- $ref: '#/components/schemas/ExternalNrCellCu-Single'

- $ref: '#/components/schemas/ExternalENBFunction-Single'

- $ref: '#/components/schemas/ExternalEUTranCell-Single'

- $ref: '#/components/schemas/EP\_XnC-Single'

- $ref: '#/components/schemas/EP\_E1-Single'

- $ref: '#/components/schemas/EP\_F1C-Single'

- $ref: '#/components/schemas/EP\_NgC-Single'

- $ref: '#/components/schemas/EP\_X2C-Single'

- $ref: '#/components/schemas/EP\_XnU-Single'

- $ref: '#/components/schemas/EP\_F1U-Single'

- $ref: '#/components/schemas/EP\_NgU-Single'

- $ref: '#/components/schemas/EP\_X2U-Single'

- $ref: '#/components/schemas/EP\_S1U-Single'

|  |
| --- |
| **End of Change** |