**3GPP TSG-SA5 Meeting #141-e *S5-221567***

**e-meeting, 17 -26 January 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** | **0680** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correct 5GC YAML in TS document |
|  |  |
| ***Source to WG:*** | S5 |
| ***Source to TSG:*** | Huawei |
|  |  |
| ***Work item code:*** | adNRM |  | ***Date:*** | 2022-01-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The yaml definition for several attributes (including IPv4address, IPv6address, DN, DNlist,administrativeState,operationalState) are moved to comDefs.yaml from genericNrm.yaml. However, in 5GCNRM.yaml, these attributes still refers to the genericNrm.yaml. |
|  |  |
| ***Summary of change:*** | Update the reference of above attributes to comDefs.yaml |
|  |  |
| ***Consequences if not approved:*** | In Correct references for above attributes. |
|  |  |
| ***Clauses affected:*** | G.4.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Forge link: <https://forge.3gpp.org/rep/sa5/MnS/-/tree/code_moderator_testing_branch_rel17_init> |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

## G.4.3 OpenAPI document "5gcNrm.yaml"

openapi: 3.0.1

info:

 title: 3GPP 5GC NRM

 version: 17.4.0

 description: >-

 OAS 3.0.1 specification of the 5GC NRM

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.541; 5G NRM, 5GC NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

 schemas:

#-------- Definition of types-----------------------------------------------------

 AmfIdentifier:

 type: object

 description: 'AmfIdentifier comprise of amfRegionId, amfSetId and amfPointer'

 properties:

 amfRegionId:

 $ref: '#/components/schemas/AmfRegionId'

 amfSetId:

 $ref: '#/components/schemas/AmfSetId'

 amfPointer:

 $ref: '#/components/schemas/AmfPointer'

 AmfRegionId:

 type: integer

 description: AmfRegionId is defined in TS 23.003

 maximum: 255

 AmfSetId:

 type: string

 description: AmfSetId is defined in TS 23.003

 maximum: 1023

 AmfPointer:

 type: integer

 description: AmfPointer is defined in TS 23.003

 maximum: 63

 IpEndPoint:

 type: object

 properties:

 ipv4Address:

 $ref: 'comDefs.yaml#/components/schemas/Ipv4Addr'

 ipv6Address:

 $ref: 'comDefs.yaml#/components/schemas/Ipv6Addr'

 ipv6Prefix:

 $ref: 'comDefs.yaml#/components/schemas/Ipv6Prefix'

 transport:

 $ref: 'genericNrm.yaml#/components/schemas/TransportProtocol'

 port:

 type: integer

 NFProfileList:

 type: array

 description: List of NF profile

 items:

 $ref: '#/components/schemas/NFProfile'

 NFProfile:

 type: object

 description: 'NF profile stored in NRF, defined in TS 29.510'

 properties:

 nFInstanceId:

 type: string

 description: uuid of NF instance

 nFType:

 $ref: 'genericNrm.yaml#/components/schemas/NFType'

 nFStatus:

 $ref: '#/components/schemas/NFStatus'

 plmn:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 sNssais:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 fqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 interPlmnFqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 nfServices:

 type: array

 items:

 $ref: '#/components/schemas/NFService'

 NFService:

 type: object

 description: NF Service is defined in TS 29.510

 properties:

 serviceInstanceId:

 type: string

 serviceName:

 type: string

 version:

 type: string

 schema:

 type: string

 fqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 interPlmnFqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 ipEndPoints:

 type: array

 items:

 $ref: '#/components/schemas/IpEndPoint'

 apiPrfix:

 type: string

 allowedPlmns:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 allowedNfTypes:

 type: array

 items:

 $ref: 'genericNrm.yaml#/components/schemas/NFType'

 allowedNssais:

 type: array

 items:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 NFStatus:

 type: string

 description: any of enumrated value

 enum:

 - REGISTERED

 - SUSPENDED

 CNSIIdList:

 type: array

 items:

 $ref: '#/components/schemas/CNSIId'

 CNSIId:

 type: string

 description: CNSI Id is defined in TS 29.531, only for Core Network

 TACList:

 type: array

 items:

 $ref: 'nrNrm.yaml#/components/schemas/NrTac'

 WeightFactor:

 type: integer

 UdmInfo:

 type: object

 properties:

 nFSrvGroupId:

 type: string

 AusfInfo:

 type: object

 properties:

 nFSrvGroupId:

 type: string

 UpfInfo:

 type: object

 properties:

 smfServingAreas:

 type: string

 AmfInfo:

 type: object

 properties:

 priority:

 type: integer

 SupportedDataSetId:

 type: string

 description: any of enumrated value

 enum:

 - SUBSCRIPTION

 - POLICY

 - EXPOSURE

 - APPLICATION

 Udrinfo:

 type: object

 properties:

 supportedDataSetIds:

 type: array

 items:

 $ref: '#/components/schemas/SupportedDataSetId'

 nFSrvGroupId:

 type: string

 NFInfo:

 oneOf:

 - $ref: '#/components/schemas/UdmInfo'

 - $ref: '#/components/schemas/AusfInfo'

 - $ref: '#/components/schemas/UpfInfo'

 - $ref: '#/components/schemas/Udrinfo'

 NotificationType:

 type: string

 enum:

 - N1\_MESSAGES

 - N2\_INFORMATION

 - LOCATION\_NOTIFICATION

 - DATA\_REMOVAL\_NOTIFICATION

 - DATA\_CHANGE\_NOTIFICATION

 - LOCATION\_UPDATE\_NOTIFICATION

 - NSSAA\_REAUTH\_NOTIFICATION

 - NSSAA\_REVOC\_NOTIFICATION

 DefaultNotificationSubscription:

 type: object

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 callbackURI:

 type: string

 n1MessageClass:

 type: boolean

 n2InfroamtionClass:

 type: boolean

 versions:

 type: string

 binding:

 type: string

 ManagedNFProfile:

 type: object

 properties:

 nfInstanceID:

 type: string

 nfType:

 $ref: 'genericNrm.yaml#/components/schemas/NFType'

 heartbeatTimer:

 type: integer

 authzInfo:

 type: string

 hostAddr:

 $ref: 'genericNrm.yaml#/components/schemas/HostAddr'

 allowedPLMNs:

 type: array

 item:

 $ref: 'comDefs.yaml#/components/schemas/PlmnId''

 allowedSNPNs:

 type: array

 item:

 $ref: 'nrNrm.yaml#/components/schemas/SnpnInfo'

 allowedNfTypes:

 type: array

 item:

 $ref: 'genericNrm.yaml#/components/schemas/NFType'

 allowedNfDomains:

 type: array

 item: string

 allowedNSSAIs:

 type: array

 item:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 locality:

 type: string

 nFInfo:

 $ref: '#/components/schemas/NFInfo'

 capacity:

 type: integer recoveryTime:

 $ref: 'comDefs.yaml#/components/schemas/DateTime'

 nfServicePersistence:

 type: boolean

 nfSetIdList:

 type: array

 item: string

 nfProfileChangesSupportInd:

 type: boolean

 defaultNotificationSubscriptions:

 type: array

 item:

 $ref: '#/components/schemas/DefaultNotificationSubscription'

 servingScope:

 type: array

 item: string

 nfSetRecoveryTimeList:

 type: array

 item:

 $ref: 'comDefs.yaml#/components/schemas/DateTime'

 scpDomains:

 type: array

 item: string

 vendorId:

 type: string

 SEPPType:

 type: string

 description: any of enumrated value

 enum:

 - CSEPP

 - PSEPP

 SupportedFunc:

 type: object

 properties:

 function:

 type: string

 policy:

 type: string

 SupportedFuncList:

 type: array

 items:

 $ref: '#/components/schemas/SupportedFunc'

 CommModelType:

 type: string

 description: any of enumrated value

 enum:

 - DIRECT\_COMMUNICATION\_WO\_NRF

 - DIRECT\_COMMUNICATION\_WITH\_NRF

 - INDIRECT\_COMMUNICATION\_WO\_DEDICATED\_DISCOVERY

 - INDIRECT\_COMMUNICATION\_WITH\_DEDICATED\_DISCOVERY

 CommModel:

 type: object

 properties:

 groupId:

 type: integer

 commModelType:

 $ref: '#/components/schemas/CommModelType'

 targetNFServiceList:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 commModelConfiguration:

 type: string

 CommModelList:

 type: array

 items:

 $ref: '#/components/schemas/CommModel'

 CapabilityList:

 type: array

 items:

 type: string

 FiveQiDscpMapping:

 type: object

 properties:

 fiveQIValues:

 type: array

 items:

 type: integer

 dscp:

 type: integer

 NetworkSliceInfo:

 type: object

 properties:

 sNSSAI:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 cNSIId:

 $ref: '#/components/schemas/CNSIId'

 networkSliceRef:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 NetworkSliceInfoList:

 type: array

 items:

 $ref: '#/components/schemas/NetworkSliceInfo'

 PacketErrorRate:

 type: object

 properties:

 scalar:

 type: integer

 exponent:

 type: integer

 GtpUPathDelayThresholdsType:

 type: object

 properties:

 n3AveragePacketDelayThreshold:

 type: integer

 n3MinPacketDelayThreshold:

 type: integer

 n3MaxPacketDelayThreshold:

 type: integer

 n9AveragePacketDelayThreshold:

 type: integer

 n9MinPacketDelayThreshold:

 type: integer

 n9MaxPacketDelayThreshold:

 type: integer

 QFPacketDelayThresholdsType:

 type: object

 properties:

 thresholdDl:

 type: integer

 thresholdUl:

 type: integer

 thresholdRtt:

 type: integer

 QosData:

 type: object

 properties:

 qosId:

 type: string

 fiveQIValue:

 type: integer

 maxbrUl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxbrDl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrUl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrDl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 arp:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Arp'

 qosNotificationControl:

 type: boolean

 reflectiveQos:

 type: boolean

 sharingKeyDl:

 type: string

 sharingKeyUl:

 type: string

 maxPacketLossRateDl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 extMaxDataBurstVol:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

 QosDataList:

 type: array

 items:

 $ref: '#/components/schemas/QosData'

 SteeringMode:

 type: object

 properties:

 steerModeValue:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteerModeValue'

 active:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessType'

 standby:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessTypeRm'

 threeGLoad:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 prioAcc:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/AccessType'

 TrafficControlData:

 type: object

 properties:

 tcId:

 type: string

 flowStatus:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowStatus'

 redirectInfo:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RedirectInformation'

 addRedirectInfo:

 type: array

 items:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RedirectInformation'

 minItems: 1

 muteNotif:

 type: boolean

 trafficSteeringPolIdDl:

 type: string

 nullable: true

 trafficSteeringPolIdUl:

 type: string

 nullable: true

 routeToLocs:

 type: array

 items:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 traffCorreInd:

 type: boolean

 upPathChgEvent:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

 steerFun:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

 steerModeDl:

 $ref: '#/components/schemas/SteeringMode'

 steerModeUl:

 $ref: '#/components/schemas/SteeringMode'

 mulAccCtrl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MulticastAccessControl'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 TrafficControlDataList:

 type: array

 items:

 $ref: '#/components/schemas/TrafficControlData'

 PccRule:

 type: object

 properties:

 pccRuleId:

 type: string

 description: Univocally identifies the PCC rule within a PDU session.

 flowInfoList:

 type: array

 items:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowInformation'

 applicationId:

 type: string

 appDescriptor:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ApplicationDescriptor'

 contentVersion:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

 precedence:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 afSigProtocol:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

 isAppRelocatable:

 type: boolean

 isUeAddrPreserved:

 type: boolean

 qosData:

 type: array

 items:

 $ref: '#/components/schemas/QosDataList'

 altQosParams:

 type: array

 items:

 $ref: '#/components/schemas/QosDataList'

 trafficControlData:

 type: array

 items:

 $ref: '#/components/schemas/TrafficControlDataList'

 conditionData:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ConditionData'

 tscaiInputDl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: 'https://forge.3gpp.org/rep/all/5G\_APIs/raw/REL-16/TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

 SnssaiInfo:

 type: object

 properties:

 plmnInfo:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnInfo'

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 NsacfInfoSnssai:

 type: object

 properties:

 SnssaiInfo:

 $ref: '#/components/schemas/SnssaiInfo'

 isSubjectToNsac:

 type: boolean

 maxNumberofUEs:

 type: integer

 eACMode:

 type: string

 enum:

 - INACTIVE

 - ACTIVE

 activeEacThreshhold:

 type: integer

 deactiveEacThreshhold:

 type: integer

 numberofUEs:

 type: integer

 uEIdList:

 type: array

 items:

 type: string

 SupportedBMOList:

 type: array

 items:

 type: string

 ECSAddrConfigInfo:

 type: array

 items:

 type: string

 maxNumberofPDUSessions:

 type: integer

NrTACRange:

 type: object

 properties:

 nRTACstart:

 type: string

 nRTACend:

 type: string

 nRTACpattern:

 type: string

 TaiRange:

 type: object

 properties:

 plmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 nrTACRangelist:

 type: array

 items:

 $ref: '#/components/schemas/NrTACRange'

#-------- Definition of concrete IOCs --------------------------------------------

 SubNetwork-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

 - type: object

 properties:

 SubNetwork:

 $ref: '#/components/schemas/SubNetwork-Multiple'

 ManagedElement:

 $ref: '#/components/schemas/ManagedElement-Multiple'

 ExternalAmfFunction:

 $ref: '#/components/schemas/ExternalAmfFunction-Multiple'

 ExternalNrfFunction:

 $ref: '#/components/schemas/ExternalNrfFunction-Multiple'

 ExternalNssfFunction:

 $ref: '#/components/schemas/ExternalNssfFunction-Multiple'

 AmfSet:

 $ref: '#/components/schemas/AmfSet-Multiple'

 AmfRegion:

 $ref: '#/components/schemas/AmfRegion-Multiple'

 Configurable5QISet:

 $ref: '#/components/schemas/Configurable5QISet-Multiple'

 Dynamic5QISet:

 $ref: '#/components/schemas/Dynamic5QISet-Multiple'

 ManagedElement-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-ncO'

 - type: object

 properties:

 AmfFunction:

 $ref: '#/components/schemas/AmfFunction-Multiple'

 SmfFunction:

 $ref: '#/components/schemas/SmfFunction-Multiple'

 UpfFunction:

 $ref: '#/components/schemas/UpfFunction-Multiple'

 N3iwfFunction:

 $ref: '#/components/schemas/N3iwfFunction-Multiple'

 PcfFunction:

 $ref: '#/components/schemas/PcfFunction-Multiple'

 AusfFunction:

 $ref: '#/components/schemas/AusfFunction-Multiple'

 UdmFunction:

 $ref: '#/components/schemas/UdmFunction-Multiple'

 UdrFunction:

 $ref: '#/components/schemas/UdrFunction-Multiple'

 UdsfFunction:

 $ref: '#/components/schemas/UdsfFunction-Multiple'

 NrfFunction:

 $ref: '#/components/schemas/NrfFunction-Multiple'

 NssfFunction:

 $ref: '#/components/schemas/NssfFunction-Multiple'

 SmsfFunction:

 $ref: '#/components/schemas/SmsfFunction-Multiple'

 LmfFunction:

 $ref: '#/components/schemas/LmfFunction-Multiple'

 NgeirFunction:

 $ref: '#/components/schemas/NgeirFunction-Multiple'

 SeppFunction:

 $ref: '#/components/schemas/SeppFunction-Multiple'

 NwdafFunction:

 $ref: '#/components/schemas/NwdafFunction-Multiple'

 ScpFunction:

 $ref: '#/components/schemas/ScpFunction-Multiple'

 NefFunction:

 $ref: '#/components/schemas/NefFunction-Multiple'

 Configurable5QISet:

 $ref: '#/components/schemas/Configurable5QISet-Multiple'

 Dynamic5QISet:

 $ref: '#/components/schemas/Dynamic5QISet-Multiple'

 GUAMInfo:

 type: object

 properties:

 pLMNId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 aMFIdentifier:

 type: integer

 AmfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 amfIdentifier:

 $ref: '#/components/schemas/AmfIdentifier'

 sBIFqdn:

 type: string

 interPlmnFQDN:

 type: string

 taiList:

 $ref: 'nrNrm.yaml#/components/schemas/Tai'

 taiRangeList:

 $ref: 'nrNrm.yaml#/components/schemas/TaiRange'

 weightFactor:

 $ref: '#/components/schemas/WeightFactor'

 cNSIIdList:

 $ref: '#/components/schemas/CNSIIdList'

 gUAMIdList:

 $ref: '#/components/schemas/GUAMInfo'

 backupInfoAmfFailure:

 $ref: '#/components/schemas/GUAMInfo'

 backupInfoAmfRemoval:

 $ref: '#/components/schemas/GUAMInfo'

 amfSetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N2:

 $ref: '#/components/schemas/EP\_N2-Multiple'

 EP\_N8:

 $ref: '#/components/schemas/EP\_N8-Multiple'

 EP\_N11:

 $ref: '#/components/schemas/EP\_N11-Multiple'

 EP\_N12:

 $ref: '#/components/schemas/EP\_N12-Multiple'

 EP\_N14:

 $ref: '#/components/schemas/EP\_N14-Multiple'

 EP\_N15:

 $ref: '#/components/schemas/EP\_N15-Multiple'

 EP\_N17:

 $ref: '#/components/schemas/EP\_N17-Multiple'

 EP\_N20:

 $ref: '#/components/schemas/EP\_N20-Multiple'

 EP\_N22:

 $ref: '#/components/schemas/EP\_N22-Multiple'

 EP\_N26:

 $ref: '#/components/schemas/EP\_N26-Multiple'

 EP\_NLS:

 $ref: '#/components/schemas/EP\_NLS-Multiple'

 EP\_NLG:

 $ref: '#/components/schemas/EP\_NLG-Multiple'

 AmfSet-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 nRTACList:

 $ref: '#/components/schemas/TACList'

 amfSetId:

 $ref: '#/components/schemas/AmfSetId'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 aMFRegionRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 aMFSetMemberList:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 AmfRegion-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 nRTACList:

 $ref: '#/components/schemas/TACList'

 amfRegionId:

 $ref: '#/components/schemas/AmfRegionId'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 aMFSetListRef:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 SmfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 nRTACList:

 $ref: '#/components/schemas/TACList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 configurable5QISetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 dynamic5QISetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N4:

 $ref: '#/components/schemas/EP\_N4-Multiple'

 EP\_N7:

 $ref: '#/components/schemas/EP\_N7-Multiple'

 EP\_N10:

 $ref: '#/components/schemas/EP\_N10-Multiple'

 EP\_N11:

 $ref: '#/components/schemas/EP\_N11-Multiple'

 EP\_N16:

 $ref: '#/components/schemas/EP\_N16-Multiple'

 EP\_S5C:

 $ref: '#/components/schemas/EP\_S5C-Multiple'

 FiveQiDscpMappingSet:

 $ref: '#/components/schemas/FiveQiDscpMappingSet-Single'

 GtpUPathQoSMonitoringControl:

 $ref: '#/components/schemas/GtpUPathQoSMonitoringControl-Single'

 QFQoSMonitoringControl:

 $ref: '#/components/schemas/QFQoSMonitoringControl-Single'

 PredefinedPccRuleSet:

 $ref: '#/components/schemas/PredefinedPccRuleSet-Single'

 UpfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 nRTACList:

 $ref: '#/components/schemas/TACList'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

supportedBMOList:

 $ref: '#/components/schemas/SupportedBMOList’

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N3:

 $ref: '#/components/schemas/EP\_N3-Multiple'

 EP\_N4:

 $ref: '#/components/schemas/EP\_N4-Multiple'

 EP\_N6:

 $ref: '#/components/schemas/EP\_N6-Multiple'

 EP\_N9:

 $ref: '#/components/schemas/EP\_N9-Multiple'

 EP\_S5U:

 $ref: '#/components/schemas/EP\_S5U-Multiple'

 N3iwfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N3:

 $ref: '#/components/schemas/EP\_N3-Multiple'

 EP\_N4:

 $ref: '#/components/schemas/EP\_N4-Multiple'

 PcfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

supportedBMOList:

 $ref: '#/components/schemas/SupportedBMOList’ '

 configurable5QISetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 dynamic5QISetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N5:

 $ref: '#/components/schemas/EP\_N5-Multiple'

 EP\_N7:

 $ref: '#/components/schemas/EP\_N7-Multiple'

 EP\_N15:

 $ref: '#/components/schemas/EP\_N15-Multiple'

 EP\_N16:

 $ref: '#/components/schemas/EP\_N16-Multiple'

 EP\_Rx:

 $ref: '#/components/schemas/EP\_Rx-Multiple'

 PredefinedPccRuleSet:

 $ref: '#/components/schemas/PredefinedPccRuleSet-Single'

 AusfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N12:

 $ref: '#/components/schemas/EP\_N12-Multiple'

 EP\_N13:

 $ref: '#/components/schemas/EP\_N13-Multiple'

 UdmFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N8:

 $ref: '#/components/schemas/EP\_N8-Multiple'

 EP\_N10:

 $ref: '#/components/schemas/EP\_N10-Multiple'

 EP\_N13:

 $ref: '#/components/schemas/EP\_N13-Multiple'

 UdrFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 UdsfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 NrfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 cNSIIdList:

 $ref: '#/components/schemas/CNSIIdList'

 nFProfileList:

 $ref: '#/components/schemas/NFProfileList'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N27:

 $ref: '#/components/schemas/EP\_N27-Multiple'

 NssfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 cNSIIdList:

 $ref: '#/components/schemas/CNSIIdList'

 nFProfileList:

 $ref: '#/components/schemas/NFProfileList'

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

eCSAddrConfigInfo:

$ref: '#/components/schemas/ECSAddrConfigInfo'$ref: '#/components/schemas/ECSAddrConfigInfo'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N22:

 $ref: '#/components/schemas/EP\_N22-Multiple'

 EP\_N31:

 $ref: '#/components/schemas/EP\_N31-Multiple'

 SmsfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N20:

 $ref: '#/components/schemas/EP\_N20-Multiple'

 EP\_N21:

 $ref: '#/components/schemas/EP\_N21-Multiple'

 EP\_MAP\_SMSC:

 $ref: '#/components/schemas/EP\_MAP\_SMSC-Multiple'

 LmfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_NLS:

 $ref: '#/components/schemas/EP\_NLS-Multiple'

 NgeirFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N17:

 $ref: '#/components/schemas/EP\_N17-Multiple'

 SeppFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 sEPPType:

 $ref: '#/components/schemas/SEPPType'

 sEPPId:

 type: integer

 fqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N32:

 $ref: '#/components/schemas/EP\_N32-Multiple'

 NwdafFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 networkSliceInfoList:

 $ref: '#/components/schemas/NetworkSliceInfoList'

 ScpFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 supportedFuncList:

 $ref: '#/components/schemas/SupportedFuncList'

 address:

 $ref: 'genericNrm.yaml#/components/schemas/HostAddr'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 NefFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 sBIFqdn:

 type: string

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 capabilityList:

 $ref: '#/components/schemas/CapabilityList'

 isCAPIFSup:

 type: boolean

taiList:

 items:

 $ref: 'nrNrm.yaml#/components/schemas/TaiList'

 taiRangeList:

 type: array

 items:

 $ref: '#/components/schemas/TaiRange’

 dnai：

 type：string

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N33:

 $ref: '#/components/schemas/EP\_N33-Multiple'

 NsacfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 nsacfInfoSnssai:

 type: array

 items:

 $ref: '#/components/schemas/NsacfInfoSnssai'

taiList:

 items:

 $ref: 'nrNrm.yaml#/components/schemas/TaiList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_N60:

 $ref: '#/components/schemas/EP\_N60-Multiple'

 DDNMFFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 sBIFqdn:

 type: string

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 commModelList:

 $ref: '#/components/schemas/CommModelList'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_Npc4:

 $ref: '#/components/schemas/EP\_Npc4-Multiple'

 EP\_Npc6:

 $ref: '#/components/schemas/EP\_Npc6-Multiple'

 EP\_Npc7:

 $ref: '#/components/schemas/EP\_Npc7-Multiple'

 EP\_Npc8:

 $ref: '#/components/schemas/EP\_Npc8-Multiple'

 EASDFFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 sBIFqdn:

 type: string

 managedNFProfile:

 $ref: '#/components/schemas/ManagedNFProfile'

 serverAddr:

 type: string

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 EP\_Nxx:

 $ref: '#/components/schemas/EP\_Nxx-Multiple'

 ExternalAmfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 amfIdentifier:

 $ref: '#/components/schemas/AmfIdentifier'

 ExternalNrfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 ExternalNssfFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 ExternalSeppFunction-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 plmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 sEPPId:

 type: integer

 fqdn:

 $ref: 'genericNrm.yaml#/components/schemas/Fqdn'

 EP\_N2-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N3-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 epTransportRefs:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 EP\_N4-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N5-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N6-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N7-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N8-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N9-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N10-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N11-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N12-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N13-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N14-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N15-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N16-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N17-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N20-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N21-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N22-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N26-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N27-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N31-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N32-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 remotePlmnId:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnId'

 remoteSeppAddress:

 $ref: 'genericNrm.yaml#/components/schemas/HostAddr'

 remoteSeppId:

 type: integer

 n32cParas:

 type: string

 n32fPolicy:

 type: string

 withIPX:

 type: boolean

 EP\_N33-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_S5C-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_S5U-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Rx-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_MAP\_SMSC-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_NLS-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_NLG-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_N60-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Npc4-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Npc6-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Npc7-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Npc8-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 EP\_Nxx-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/EP\_RP-Attr'

 - type: object

 properties:

 localAddress:

 $ref: 'nrNrm.yaml#/components/schemas/LocalAddress'

 remoteAddress:

 $ref: 'nrNrm.yaml#/components/schemas/RemoteAddress'

 FiveQiDscpMappingSet-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 FiveQiDscpMappingList:

 type: array

 items:

 $ref: '#/components/schemas/FiveQiDscpMapping'

 FiveQICharacteristics-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 fiveQIValue:

 type: integer

 resourceType:

 type: string

 enum:

 - GBR

 - NonGBR

 priorityLevel:

 type: integer

 packetDelayBudget:

 type: integer

 packetErrorRate:

 $ref: '#/components/schemas/PacketErrorRate'

 averagingWindow:

 type: integer

 maximumDataBurstVolume:

 type: integer

 FiveQICharacteristics-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/FiveQICharacteristics-Single'

 Configurable5QISet-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 configurable5QIs:

 type: array

 items:

 $ref: '#/components/schemas/FiveQICharacteristics-Multiple'

 Dynamic5QISet-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 dynamic5QIs:

 type: array

 items:

 $ref: '#/components/schemas/FiveQICharacteristics-Multiple'

 GtpUPathQoSMonitoringControl-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 gtpUPathQoSMonitoringState:

 type: string

 enum:

 - ENABLED

 - DISABLED

 gtpUPathMonitoredSNSSAIs:

 type: array

 items:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 monitoredDSCPs:

 type: array

 items:

 type: integer

 minimum: 0

 maximum: 255

 isEventTriggeredGtpUPathMonitoringSupported:

 type: boolean

 isPeriodicGtpUMonitoringSupported:

 type: boolean

 isImmediateGtpUMonitoringSupported:

 type: boolean

 gtpUPathDelayThresholds:

 $ref: '#/components/schemas/GtpUPathDelayThresholdsType'

 gtpUPathMinimumWaitTime:

 type: integer

 gtpUPathMeasurementPeriod:

 type: integer

 QFQoSMonitoringControl-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 qFQoSMonitoringState:

 type: string

 enum:

 - ENABLED

 - DISABLED

 qFMonitoredSNSSAIs:

 type: array

 items:

 $ref: 'nrNrm.yaml#/components/schemas/Snssai'

 qFMonitored5QIs:

 type: array

 items:

 type: integer

 minimum: 0

 maximum: 255

 isEventTriggeredQFMonitoringSupported:

 type: boolean

 isPeriodicQFMonitoringSupported:

 type: boolean

 isSessionReleasedQFMonitoringSupported:

 type: boolean

 qFPacketDelayThresholds:

 $ref: '#/components/schemas/QFPacketDelayThresholdsType'

 qFMinimumWaitTime:

 type: integer

 qFMeasurementPeriod:

 type: integer

 PredefinedPccRuleSet-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 predefinedPccRules:

 type: array

 items:

 $ref: '#/components/schemas/PccRule'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

 SubNetwork-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/SubNetwork-Single'

 ManagedElement-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagedElement-Single'

 AmfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AmfFunction-Single'

 SmfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/SmfFunction-Single'

 UpfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/UpfFunction-Single'

 N3iwfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/N3iwfFunction-Single'

 PcfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/PcfFunction-Single'

 AusfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AusfFunction-Single'

 UdmFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/UdmFunction-Single'

 UdrFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/UdrFunction-Single'

 UdsfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/UdsfFunction-Single'

 NrfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NrfFunction-Single'

 NssfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NssfFunction-Single'

 SmsfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/SmsfFunction-Single'

 LmfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/LmfFunction-Single'

 NgeirFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NgeirFunction-Single'

 SeppFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/SeppFunction-Single'

 NwdafFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NwdafFunction-Single'

 ScpFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ScpFunction-Single'

 NefFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NefFunction-Single'

 NsacfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NsacfFunction-Single'

 ExternalAmfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ExternalAmfFunction-Single'

 ExternalNrfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ExternalNrfFunction-Single'

 ExternalNssfFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ExternalNssfFunction-Single'

 ExternalSeppFunction-Nultiple:

 type: array

 items:

 $ref: '#/components/schemas/ExternalSeppFunction-Single'

 AmfSet-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AmfSet-Single'

 AmfRegion-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AmfRegion-Single'

 EP\_N2-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N2-Single'

 EP\_N3-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N3-Single'

 EP\_N4-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N4-Single'

 EP\_N5-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N5-Single'

 EP\_N6-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N6-Single'

 EP\_N7-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N7-Single'

 EP\_N8-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N8-Single'

 EP\_N9-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N9-Single'

 EP\_N10-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N10-Single'

 EP\_N11-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N11-Single'

 EP\_N12-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N12-Single'

 EP\_N13-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N13-Single'

 EP\_N14-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N14-Single'

 EP\_N15-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N15-Single'

 EP\_N16-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N16-Single'

 EP\_N17-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N17-Single'

 EP\_N20-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N20-Single'

 EP\_N21-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N21-Single'

 EP\_N22-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N22-Single'

 EP\_N26-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N26-Single'

 EP\_N27-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N27-Single'

 EP\_N31-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N31-Single'

 EP\_N32-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N32-Single'

 EP\_N33-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N33-Single'

 EP\_S5C-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_S5C-Single'

 EP\_S5U-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_S5U-Single'

 EP\_Rx-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Rx-Single'

 EP\_MAP\_SMSC-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_MAP\_SMSC-Single'

 EP\_NLS-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_NLS-Single'

 EP\_NLG-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_NLG-Single'

 EP\_N60-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_N60-Single'

 EP\_Npc4-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Npc4-Single'

 EP\_Npc6-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Npc6-Single'

 EP\_Npc7-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Npc7-Single'

 EP\_Npc8-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Npc8-Single'

 EP\_Nxx-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Nxx-Single'

 Configurable5QISet-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/Configurable5QISet-Single'

 Dynamic5QISet-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/Dynamic5QISet-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

 resources-5gcNrm:

 oneOf:

 - $ref: '#/components/schemas/SubNetwork-Single'

 - $ref: '#/components/schemas/ManagedElement-Single'

 - $ref: '#/components/schemas/AmfFunction-Single'

 - $ref: '#/components/schemas/SmfFunction-Single'

 - $ref: '#/components/schemas/UpfFunction-Single'

 - $ref: '#/components/schemas/N3iwfFunction-Single'

 - $ref: '#/components/schemas/PcfFunction-Single'

 - $ref: '#/components/schemas/AusfFunction-Single'

 - $ref: '#/components/schemas/UdmFunction-Single'

 - $ref: '#/components/schemas/UdrFunction-Single'

 - $ref: '#/components/schemas/UdsfFunction-Single'

 - $ref: '#/components/schemas/NrfFunction-Single'

 - $ref: '#/components/schemas/NssfFunction-Single'

 - $ref: '#/components/schemas/SmsfFunction-Single'

 - $ref: '#/components/schemas/LmfFunction-Single'

 - $ref: '#/components/schemas/NgeirFunction-Single'

 - $ref: '#/components/schemas/SeppFunction-Single'

 - $ref: '#/components/schemas/NwdafFunction-Single'

 - $ref: '#/components/schemas/ScpFunction-Single'

 - $ref: '#/components/schemas/NefFunction-Single'

 - $ref: '#/components/schemas/NsacfFunction-Single'

 - $ref: '#/components/schemas/ExternalAmfFunction-Single'

 - $ref: '#/components/schemas/ExternalNrfFunction-Single'

 - $ref: '#/components/schemas/ExternalNssfFunction-Single'

 - $ref: '#/components/schemas/ExternalSeppFunction-Single'

 - $ref: '#/components/schemas/AmfSet-Single'

 - $ref: '#/components/schemas/AmfRegion-Single'

 - $ref: '#/components/schemas/QFQoSMonitoringControl-Single'

 - $ref: '#/components/schemas/GtpUPathQoSMonitoringControl-Single'

 - $ref: '#/components/schemas/EP\_N2-Single'

 - $ref: '#/components/schemas/EP\_N3-Single'

 - $ref: '#/components/schemas/EP\_N4-Single'

 - $ref: '#/components/schemas/EP\_N5-Single'

 - $ref: '#/components/schemas/EP\_N6-Single'

 - $ref: '#/components/schemas/EP\_N7-Single'

 - $ref: '#/components/schemas/EP\_N8-Single'

 - $ref: '#/components/schemas/EP\_N9-Single'

 - $ref: '#/components/schemas/EP\_N10-Single'

 - $ref: '#/components/schemas/EP\_N11-Single'

 - $ref: '#/components/schemas/EP\_N12-Single'

 - $ref: '#/components/schemas/EP\_N13-Single'

 - $ref: '#/components/schemas/EP\_N14-Single'

 - $ref: '#/components/schemas/EP\_N15-Single'

 - $ref: '#/components/schemas/EP\_N16-Single'

 - $ref: '#/components/schemas/EP\_N17-Single'

 - $ref: '#/components/schemas/EP\_N20-Single'

 - $ref: '#/components/schemas/EP\_N21-Single'

 - $ref: '#/components/schemas/EP\_N22-Single'

 - $ref: '#/components/schemas/EP\_N26-Single'

 - $ref: '#/components/schemas/EP\_N27-Single'

 - $ref: '#/components/schemas/EP\_N31-Single'

 - $ref: '#/components/schemas/EP\_N32-Single'

 - $ref: '#/components/schemas/EP\_N33-Single'

 - $ref: '#/components/schemas/EP\_N60-Single'

 - $ref: '#/components/schemas/EP\_S5C-Single'

 - $ref: '#/components/schemas/EP\_S5U-Single'

 - $ref: '#/components/schemas/EP\_Rx-Single'

 - $ref: '#/components/schemas/EP\_MAP\_SMSC-Single'

 - $ref: '#/components/schemas/EP\_NLS-Single'

 - $ref: '#/components/schemas/EP\_NLG-Single'

 - $ref: '#/components/schemas/Configurable5QISet-Single'

 - $ref: '#/components/schemas/FiveQiDscpMappingSet-Single'

 - $ref: '#/components/schemas/PredefinedPccRuleSet-Single'

 - $ref: '#/components/schemas/Dynamic5QISet-Single'

|  |
| --- |
| **End of Change** |