**3GPP TSG-SA5 Meeting #141-eS5-221588**

**e-meeting, 17 - 24 January 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.536** | **CR** | **0041** | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Input to draftCR clean up stage 2 descriptions |
|  |  |
| ***Source to WG:*** | Ericsson, Deutsche Telekom, Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | eCOSLA |  | ***Date:*** | 2021-09-26 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | With the development of the stage 2 specification for eCosla Rel-17 many changes have been implemented and due to the many changes, the descriptions of classes, data types and attributes could be improved to make them more useable. |
|  |  |
| ***Summary of change:*** | 1. Change the association between AR class and ACCL class to AR is name contained by ACCL.
2. The references to NSI and NSSI are moved from AG to ACCL, same for associated constraints.
3. Update text in clause 4.1.2.2.1 according TS 32.160
4. Fix name of NetworkSLice to NetworkSlice and fix formatting in clause 4.1.2.3.1/2/3/4/5 from Justified to Align Right
5. Update properties of AssuranceTargetList to Writeable.
6. Update properties of AssuranceTarget to Writeable
7. Update description of AssuranceGoal 4.1.2.3.2 and fix formattting of heading
8. Update description of AssuranceGoalStatus 4.1.2.3.1, table heading and make AssuranceGoalStatusId of datatype Userlabel and writeable
9. Update description of AssuranceReport
10. Add missing notification “notifyMOIChanges” from TS 28.532 to table in clause 4.1.2.5.2
 |
|  |  |
| ***Consequences if not approved:*** | If not approved the specifications may lead to incompatible implementations |
|  |  |
| ***Clauses affected:*** | 2, 4.1.2.2.1, 4.1.2.2.2, 4.1.2.3.1.1, 4.1.2.3.2.2, 4.1.2.3.l (new), 4.1.2.3.m (new), 4.1.2.3.x (new), 4.1.2.3.x.2, 4.1.2.3.x.34.1.2.4.1B.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This is input to the Rel-17 28.536 DraftCR for eCOSLA[Files · 28.536\_Rel17\_CR0041\_Input\_to\_draftCR\_TS\_28.536\_clean\_up\_stage\_2\_descriptions · SA5 – Management & Orchestration and Charging / Management and Orchestration APIs · GitLab (3gpp.org)](https://forge.3gpp.org/rep/sa5/MnS/-/tree/28.536_Rel17_CR0041_Input_to_draftCR_TS_28.536_clean_up_stage_2_descriptions)[178515f1](https://forge.3gpp.org/rep/sa5/MnS/-/commit/178515f16910c04f8f694b855bc24f02c5b5b656) |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 22.261: "Service requirements for the 5G system".

[3] 3GPP TS 28.550: "Management and orchestration; Performance assurance".

[4] 3GPP TS 28.531: "Management and orchestration; Provisioning".

[5] ETSI GS ZSM 002 (V1.1.1) (2019-08): "Zero-touch network and Service Management (ZSM); Reference Architecture".

[6] 3GPP TS 28.545: "Management and orchestration; Fault Supervision (FS)".

[7] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[8] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[9] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[x] 3GPP TS 28.535: "Management and orchestration; Management services for communication service assurance; Requirements".

|  |
| --- |
| **2nd change** |

### 4.1.2 Model

#### 4.1.2.1 Imported and associated information entities

##### 4.1.2.1.1 Imported information entities and local labels

|  |  |
| --- | --- |
| Label reference | Local label  |
| TS 28.622 [5], IOC, Top | Top |

##### 4.1.2.1.2 Associated information entities and local labels

|  |  |
| --- | --- |
| Label reference | Local label  |
| TS 28.622 [5], IOC, SubNetwork | SubNetwork |
| TS 28.541 [6], IOC, NetWorkSlice | NetworkSlice |
| TS 28.541 [6], IOC, NetWorkSliceSubnet | NetworkSliceSubnet |
| TS 28.622 [5], IOC, ManagedElement | ManagedElement |
| TS 28.541 [6], attribute, serviceProfileId | serviceProfileId |
| TS 28.541 [6], attribute, sliceProfileId | sliceProfileId |

#### 4.1.2.2 Class diagram

#### 4.1.2.2.1 Relationships

This clause depicts the set of classes that encapsulates the information relevant for this MnS. This clause provides an overview of the relationships between relevant classes in UML. This clause provides an overview of the relationships between relevant classes in UML. Subsequent clauses provide more detailed specification of various aspects of these classes.



Figure 4.1.2.2.1.1: Assurance management NRM fragment

#### 4.1.2.2.2 Inheritance



Figure 4.1.2.2.2.1: Assurance management inheritance relationships

#### 4.1.2.3 Class definitions

##### 4.1.2.3.1 AssuranceClosedControlLoop

4.1.2.3.1.1 Definition

This class represents the information for controlling and monitoring an assurance closed control loop associated with a NetworkSlice or NetworkSliceSubnet. It can be name-contained by SubNetwork or ManagedElement.

To express the assurance closed control loop requirements, the MnS consumer needs to request MnS producer to create an AssuranceClosedControlLoop on the MnS producer. The MnS producer may trigger to create the AssuranceClosedControlLoop as well, for example, when an instance of NetworkSlice or NetworkSliceSubnet is created, MnS producer may create an instance of AssuranceClosedControlLoop associated to the instance of NetworkSlice or NetworkSliceSubnet to assure the target described in ServiceProfile or SliceProfile. For ultimate deletion of assurance closed control loop, the MnS consumer needs to request the MnS producer to delete the AssuranceClosedControlLoop to free up resources on the MnS producer. MnS producer also can trigger to delete AssuranceClosedControlLoop to free up resources by itself.

For temporary deactivation of assurance closed control loop, the MnS consumer can manipulate the value of the administrative state attribute to “LOCKED”. The MnS producer may disable assurance closed control loop as well, for example in conflict situations. This situation is indicated by the MnS producer with setting the operational state attribute to “disabled”. When closed control loop is enabled by the MnS producer the operational state is set again to “enabled”. For activation of assurance closed control loop, the MnS consumer can manipulate the value of the administrative state attribute to “UNLOCKED”.

An AssuranceClosedControlLoop can name-contain multiple instances of AssuranceGoal which represents the assurance goal and corresponding observed or predicted goal fulfilment information (see clause 4.1.2.3.2).

The attribute “controlLoopLifeCyclePhase” is used to keep track of the lifecycle of an AssuranceClosedControlLoop

4.1.2.3.1.2 Attributes

The AssuranceClosedControlLoop IOC includes attributes inherited from Top IOC (defined TS 28.622[5]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| operationalState | M | T | F | F | T |
| administrativeState | M | T | T | F | T |
| controlLoopLifeCyclePhase | M | T | T | F | T |
| **Attributes related to role** |  |  |  |  |  |
| networkSliceRef | CM | T | T | F | T |
| networkSliceSubnetRef | CM | T | T | F | T |

4.1.2.3.1.3 Constraints

|  |  |
| --- | --- |
| Name | Definition |
| networkSliceSubnetRef | Condition: the AssuranceGoal applies to a NetworkSliceSubNet |
| networkSliceRef | Condition: the AssuranceGoal applies to a NetworkSlice |

4.1.2.3.1.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for this IOC, without exceptions or additions.

##### 4.1.2.3.2 AssuranceGoal

4.1.2.3.2.1 Definition

This IOC represents assurance goal.

To express a new assurance goal for the assurance closed control loop, the MnS consumer needs to request the MnS producer to create an instance of AssuranceGoal. MnS producer can also trigger the creation of an instance of AssuranceGoal. For example, when a new instance NetworkSlice or NetworkSliceSubnet is created on the MnS producer and the corresponding SLS needs to be assured, a new instance of AssuranceGoal needs to be created and associated to the new instance NetworkSlice or NetworkSliceSubnet by configuring the attributes “networkSliceRef” or “networkSliceSubnetRef” and corresponding attributes “serviceProfileId” and “sliceProfileId”.

The attribute “assuranceTargetList” defines a list of assurance targets (the subset of attributes from an SLS, i.e. a ServiceProfile or a SliceProfile, that are subject to assurance requirements.) that should be assured by the AssuranceClosedControlLoop. The attribute “assuranceTargetList” is configured by MnS producer based on the specified ServiceProfile or SliceProfile.

NOTE: Multiple instances of AssuranceGoal can be created for a single instance of NetworkSlice or NetworkSliceSubnet.

4.1.2.3.2.2 Attributes

The AssuranceGoal IOC includes attributes inherited from Top IOC (defined TS 28.622[5]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
|  |  |  |  |  |  |
| assuranceTargetList | M | T | F | F | T |
| sliceProfileId | CM | T | T | F | T |
| serviceProfileId | CM | T | T | F | T |
| observationTime | M | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

.

4.1.2.3.2.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| sliceProfileId | Condition: the AssuranceGoal applies to a NetworkSliceSubNet |
| serviceProfileId | Condition: the AssuranceGoal applies to a NetworkSlice |
|  |  |
|  |  |

4.1.2.3.2.4 Notifications

The common notifications defined in subclause 4.1.2.5 are valid for this IOC, without exceptions or additions.

##### 4.1.2.3.3 Void

##### 4.1.2.3.4 Void

##### 4.1.2.3.5 AssuranceTarget <<dataType>>

4.1.2.3.5.1 Definition

This data type represents a single attribute name-value-pair of which one or more are included in an AssuranceGoal.

4.1.2.3.5.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceTargetName | M | T | T | F | T |
| assuranceTargetValue | M | T | F | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

4.1.2.3.5.3 Attribute constraints

No constraints have been defined for this document.

4.1.2.3.5.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

##### 4.1.2.3.l AssuranceGoalStatus <<dataType>>

4.1.2.3.l.1 Definition

This data type represents the observed and/or predicted AssuranceGoal fulfilment status.

To obtain the observed predicted status of the the goal fulfilment information, the MnS consumer can query the attributes “AssuranceGoalStatusObserved” and “AssuranceGoalStatusPredicted”from MnS producer. The attributes “AssuranceGoalStatusObserved” and “AssuranceGoalStatusPredicted” are configured by MnS producer at the end of an observation period. The observation period is assigned by MnS consumer through requesting the MnS producer to set attribute “observationTime”. The status of the goal fuilfilment is considered FULFILLED if all the constituent targets are FULFILLED.

4.1.2.3.m.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceGoalStatusId | M | T | F | F | T |
| assuranceGoalId | O | T | F | F | T |
| assuranceGoalStatusObserved | O | T | F | F | T |
| assuranceGoalStatusPredicted | O | T | F | F | T |
| assuranceTargetStatusList | O | T | F | F | T |

4.1.2.3.l.3 Attribute constraints

No constraints have been defined for this document.

4.1.2.3.l.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for this <<IOC>> , without exceptions or additions.

##### 4.1.2.3.m AssuranceTargetStatus <<dataType>>

4.1.2.3.m.1 Definition

This data type represents the observed and/or predicted target fulfilment status.

To obtain the observed predicted status of the the target fulfilment information, the MnS consumer can query the attributes “AssuranceTargetStatusObserved” and “AssuranceTargetPredicted” from MnS producer. The attributes“AssuranceTargetStatusObserved” and “AssuranceTargetStatusPredicted” are configured by MnS producer at the end of an observation period. The observation period is assigned by MnS consumer through requesting the MnS producer to set attribute “observationTime”. The status of the target fuilfilment is considered FULFILLED if all the constituent target are FULFILLED.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceTargetStatusId | M | T | F | F | T |
| assuranceTargetName | O | T | F | F | T |
| assuranceTargetStatusObserved | O | T | F | F | T |
| assuranceTargetStatusPredicted | O | T | F | F | T |

4.1.2.3.m.3 Attribute constraints

No constraints have been defined for this document.

4.1.2.3.m.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

##### 4.1.2.3.x AssuranceReport <<IOC>>

4.1.2.3.x.1 Definition

This class represents the attributes of assurance report, e.g, the information about one or multiple AssuranceGoalStatus and one or multiple AssuranceTargetStatus.

The attribute “assuranceGoalStatusList” defines a list of AssuranceGoalStatus..

AssuranceReport represents the monitoring information of an assurance closed control loop. An AssuranceReport is contained by an AssuranceClosedControlLoop. There is one AssuranceReport per assurance closed control loop for an observation time. The content of the AssuranceReport may be different for different observation time. According to the AssuranceGoal and the AssuranceReport, the consumer performs closed control loop governance as described in clause "4.2.5 Closed control loop governance and monitoring" in TS 28.535 [x].

4.1.2.3.x.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceGoalStatusList | O | T | F | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **Attributes related to role**  |  |  |  |  |  |
| assuranceGoalRef | O | T | F | F | T |

4.1.2.3.x.3 Attribute constraints

No constraints have been defined for this document

|  |  |
| --- | --- |
|  |  |
|  |  |

4.1.2.3.x.4 Notifications

The common notifications defined in subclause 4.1.2.5 are valid for this IOC, without exceptions or additions.

#### 4.1.2.4 Attribute definitions

##### 4.1.2.4.1 Attribute properties

The following table defines the properties of attributes that are specified in the present document.

Table 4.1.2.4.1.1

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| controlLoopLifeCyclePhase | It indicates the lifecycle phase of the AssuranceClosedControlLoop instance. AllowedValues: Preparation, Commissioning, Operation and Decommissioning.  | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NULL isNullable: False |
| assuranceTargetName | The name of the attribute which is part of AssuranceTarget and AssuranceTargetStatus. The assuranceTargetName uniquely identifies the name of an AssuranceTarget instance in corresponding AssuranceTargetStatus instance. The assuranceTargetName shall be equal to the name of an attribute in the relevant ServiceProfile or SliceProfile. The relevant ServiceProfile or SliceProfile is identified by the attribute serviceProfileId or sliceProfileId in the AssuranceGoal. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetValue | The value of the attribute which is part of AssuranceTarget | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetList | This is an attribute containing a list of AssuranceTarget(s) that are part of an AssuranceGoal | type: AssuranceTargetmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| observationTime | It indicates the time duration over which an AssuranceGoal is observed. The observation time is expressed in seconds. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceGoalStatusObserved | It holds the status of the observed goal fulfilment to the assuranceGoal. The value is FULFILLED only if all the constituent assuranceTargetStatusObserved are FULFILLED. During the initial operation of a closed control loop no fulfilment information may be available to report, the value NO\_REPORT will be used.allowedValues: "NO\_REPORT,”FULFILLED", “NOT\_FULFILLED Editor’s Note: Whether a more suiteable phrase for NO\_REPLY is needed is FFS | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceGoalStatusPredicted | It holds the status of the predicted future goal fulfilment to the assuranceGoal . The value is FULFILLED only if all the constituent assuranceTargetStatusPredicted are FULFILLED.During the initial operation of a closed control loop no fulfilment information may be available to report, the value NO\_REPORT will be used.allowedValues: "NO\_REPORT", "FULFILLED", “NOT\_FULFILLED"Editor’s Note: Whether a more suiteable phrase for NO\_REPLY is needed is FFS | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceTargetStatusObserved | It holds the status of the observed target fulfilment to the assuranceGoal. allowedValues: "FULFILLED", “NOT\_FULFILLED  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceTargetStatusPredicted | It holds the status of the predicted future target fulfilment to the assuranceGoal allowedValues: "FULFILLED", “NOT\_FULFILLED" | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| networkSliceRef | It holds the reference to the NetworkSlice instance subject to assurance requirements | type: Dnmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| networkSliceSubnetRef | It holds the reference to the NetworkSliceSubnet instance subject to assurance requirements | type: Dnmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| operationalState | It indicates the operational state of the AssuranceClosedControlLoop instance. It describes whether the resource is installed and partially or fully operable (Enabled) or the resource is not installed or not operable (Disabled).Allowed values; Enabled/DisabledallowedValues: "ENABLED", "DISABLED".The meaning of these values is as defined in 3GPP TS 28.625 [14] and ITU-T X.731 [15]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DisabledallowedValues: Enabled, DisabledisNullable: False |
| administrativeState | It indicates the administrative state of the AssuranceClosedControlLoop instance. It describes the permission to use or the prohibition against using the AssuranceClosedControlLoop instance. The administrative state is set by the MnS consumer. Allowed values; Locked/UnlockedallowedValues: "LOCKED", "UNLOCKED".The meaning of these values is as defined in 3GPP TS 28.625 [14] and ITU-T X.731 [15]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LockedallowedValues: Locked, UnlockedisNullable: False |
| assuranceGoalStatusId | The indication of the AssuranceGoalStatus | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetStatusId | The indication of the AssuranceTargetStatus. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceGoalStatusList | This is an attribute containing a list of assuranceGoalStatus | type: AssuranceGoalStatusmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetStatusList | This is an attribute containing a list of assuranceTargetStatus | type: AssuranceTargetStatusmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
|  |  |  |
| assuranceGoalId | It holds the identity in AssuranceGoalStatus that uniquely identifies the corresponding AssuranceGoal instance  | type: Dnmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| NOTE 1: VoidNOTE 2: Void |

##### 4.1.2.4.2 Constraints

No constraints have been identified for this document.

##### 4.1.2.4.3 Notifications

This subclause presents a list of notifications, defined in [7], that provisioning management service consumer can receive. The notification parameter objectClass/objectInstance, defined in [10], would capture the DN of an instance of an IOC defined in the present document.

#### 4.1.2.5 Common notifications

##### 4.1.2.5.1 Alarm notifications

This clause presents a list of notifications, defined in TS 28.532 [7], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance, defined in TS 32.302 [8], shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyNewAlarm | M | -- |
| notifyClearedAlarm | M | -- |
| notifyAckStateChanged | M | -- |
| notifyAlarmListRebuilt | M | -- |
| notifyChangedAlarm | O | -- |
| notifyCorrelatedNotificationChanged | O | -- |
| notifyChangedAlarmGeneral | O | -- |
| notifyComments | O | -- |
| notifyPotentialFaultyAlarmList | O | -- |

##### 4.1.2.5.2 Configuration notifications

This clause presents a list of notifications, defined in TS 28.532 [7], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance, defined in TS 32.302 [8], shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyMOICreation | O | -- |
| notifyMOIDeletion | O | -- |
| notifyMOIAttributeValueChanges | O | -- |
| notifyMOIChanges | O | -- |
| notifyEvent | O | -- |

|  |
| --- |
| **3rd change** |

# B.2 Solution Set (SS) definitions

## B.2.1 OpenAPI document "coslaNrm.yml"

openapi: 3.0.2

info:

 title: coslaNrm

 version: 17.1.0

 description:

 OAS 3.0.1 specification of the Cosla NRM

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.536 V17.1.0; Cosla NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.536/

paths: {}

components:

 schemas:

#------------ Type definitions ---------------------------------------------------

 ControlLoopLifeCyclePhase:

 type: string

 enum:

 - PREPARATION

 - COMMISSIONING

 - OPERATION

 - DECOMMISSIONING

 ObservationTime:

 type: integer

 AssuranceGoalStatusObserved:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceGoalStatusPredicted:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTargetStatusObserved:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTargetStatusPredicted:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTargetName:

 Type: string

 AssuranceTarget:

 type: object

 properties:

 assuranceTargetName:

 $ref: '#/components/schemas/AssuranceTargetName'

 assuranceTargetValue:

 type: string

 AssuranceTargetList:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceTarget'

 AssuranceGoalStatus:

 type: object

 properties:

 assuranceGoalStatusId:

 type: string

 assuranceGoalId:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 assuranceGoalStatusObserved:

 $ref: '#/components/schemas/AssuranceGoalStatusObserved'

 assuranceGoalStatusPredicted:

 $ref: '#/components/schemas/AssuranceGoalStatusPredicted'

 assuranceGoalRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 AssuranceGoalStatusList:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceGoalStatus'

 AssuranceTargetStatus:

 type: object

 properties:

 assuranceTargetStatusId:

 type: string

 assuranceTargetName:

 $ref: '#/components/schemas/AssuranceTargetName'

 assuranceTargetStatusObserved:

 $ref: '#/components/schemas/AssuranceTargetStatusObserved'

 assuranceTargetStatusPredicted:

 $ref: '#/components/schemas/AssuranceTargetStatusPredicted'

 AssuranceTargetStatusList:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceTargetStatus'

#-------- Definition of concrete IOCs --------------------------------------------

 SubNetwork-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

 - type: object

 properties:

 AssuranceClosedControlLoop:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Multiple'

 ManagedElement-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-ncO'

 - type: object

 properties:

 AssuranceClosedControlLoop:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Multiple'

 AssuranceClosedControlLoop-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 controlLoopLifeCyclePhase:

 $ref: '#/components/schemas/ControlLoopLifeCyclePhase'

 AssuranceGoal:

 $ref: '#/components/schemas/AssuranceGoal-Multiple'

 networkSliceRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 networkSliceSubnetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 AssuranceGoal-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 observationTime:

 $ref: '#/components/schemas/ObservationTime'

 assuranceTargetList:

 $ref: '#/components/schemas/AssuranceTargetList'

 serviceProfileId:

 type: string

 sliceProfileId:

 type: string

 AssuranceReport-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 assuranceGoalStatusList:

 $ref: '#/components/schemas/AssuranceGoalStatusList'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

 AssuranceClosedControlLoop-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Single'

 AssuranceGoal-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceGoal-Single'

#------------ Definitions in TS 28.536 for TS 28.623 -----------------------------

 resources-coslaNrm:

 oneOf:

 - $ref: '#/components/schemas/AssuranceClosedControlLoop-Single'

 - $ref: '#/components/schemas/AssuranceGoal-Single'

 - $ref: '#/components/schemas/AssuranceReport-Single'

 - $ref: '#/components/schemas/SubNetwork-Single'

 - $ref: '#/components/schemas/ManagedElement-Single'

|  |
| --- |
| **End of changes** |