**3GPP TSG-SA5 Meeting #145-e *S5-225601***

e-meeting, 15 - 24 Aug 2022

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.622** | **CR** | **0176** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 CR 28.622 Correcting Support Qualifier for jobId attribute |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | FIMA |  | ***Date:*** | 2022-08-04 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Incorrect Support Qualifier for attribute |
|  |  |
| ***Summary of change:*** | Support Qualifier for attribute jobId is corrected |
|  |  |
| ***Consequences if not approved:*** | Use of not defined support qualifier for attribute jobId |
|  |  |
| ***Clauses affected:*** | 4.3.30.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

***Start of first change***

#### 4.3.30.2 Attributes

The TraceJob IOC includes attributes inherited from Top IOC (defined in clause 4.3.29) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | S | isReadable | isWritable | isInvariant | isNotifyable |
| jobType | M | T | T | F | T |
| listOfInterfaces | CO | T | T | F | T |
| listOfNeTypes | CM | T | T | F | T |
| plmnTarget | CM | T | T | F | T |
| traceReportingConsumerUri | CM | T | T | F | T |
| traceCollectionEntityIpAddress | CM | T | T | F | T |
| traceDepth | CM | T | T | F | T |
| traceReference | M | T | T | F | T |
| traceRecordingSessionReference | M | T | T | F | T |
| jobId | O | T | T | T | T |
| traceReportingFormat | M | T | T | F | T |
| traceTarget | M | T | T | F | T |
| triggeringEvents | CM | T | T | F | T |
| anonymizationOfMdtData | CM | T | T | F | T |
| areaConfigurationForNeighCell | CO | T | T | F | T |
| areaScope | CO | T | T | F | T |
| collectionPeriodRrmLte | CM | T | T | F | T |
| collectionPeriodM6Lte | CM | T | T | F | T |
| collectionPeriodM7Lte | CM | T | T | F | T |
| collectionPeriodRrmUmts | CM | T | T | F | T |
| collectionPeriodRrmNr | CM | T | T | F | T |
| collectionPeriodM6Nr | CM | T | T | F | T |
| collectionPeriodM7Nr | CM | T | T | F | T |
| beamLevelMeasurement | CM | T | T | F | T |
| eventListForEventTriggeredMeasurement | CM | T | T | F | T |
| eventThreshold | CM | T | T | F | T |
| listOfMeasurements | CM | T | T | F | T |
| loggingDuration | CM | T | T | F | T |
| loggingInterval | CM | T | T | F | T |
| eventThresholdL1 | CM | T | T | F | T |
| hysteresisL1 | CM | T | T | F | T |
| timeToTriggerL1 | CM | T | T | F | T |
| mbsfnAreaList | CM | T | T | F | T |
| measurementPeriodLte | CM | T | T | F | T |
| measurementPeriodUmts | CM | T | T | F | T |
| measurementQuantity | CM | T | T | F | T |
| eventThresholdUphUmts | CO | T | T | F | T |
| plmnList | CO | T | T | F | T |
| positioningMethod | CO | T | T | F | T |
| reportAmount | CM | T | T | F | T |
| reportingTrigger | CM | T | T | F | T |
| reportInterval | CM | T | T | F | T |
| reportType | CM | T | T | F | T |
| sensorInformation | CO | T | T | F | T |
| traceCollectionEntityId | CM | T | T | F | T |

***End of changes***